{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["pricelist"],"not_rendered":{"external_links":12,"defined_names":571},"read":"whole","date_system":"1900"}

{"sheet":"pricelist","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"merged":[[1,1,1,3]]}
[]
[]
[null,"Description","Unit","Estimated hours","Rate","Total","Contract duration (5yrs)","Amount"]
[]
[null,"Fixed Preliminaries and General ( Breakdown required)"]
[]
[1,"Site establishment","sum",1,null,null,5]
[{"$f":"A7+1","v":2},"PPE - Provide annually","sum",1,null,null,5]
[{"$f":"A8+1","v":3},"Medicals - Entry, enterim and exit","sum",1,null,null,5]
[4,"Safety file - Once off","Item",1,null,null,1]
[]
[null,"Time Related Preliminaries and Generals"]
[]
[{"$f":"A10+1","v":5},"Transport ","per km",23850,null,null,5]
[{"$f":"A14+1","v":6},"Accommodation","per day",160,null,null,5]
[{"$f":"A15+1","v":7},"Site establishment","sum",1,null,null,5]
[null,"Sub Total"]
[]
[null,"Description","Unit","Quantity","Rate","Total","Contract duration (5yrs)","Amount"]
[null,"Full Correlation Test"]
[1,"Full Correlation Test for dust monitors (Dust Meter)","Per Unit",6,null,null,5]
[]
[null,"Full Parallel Tests"]
[{"$f":"A21+1","v":2},"Verification of the gaseous monitors (QAL2/3)","Per Unit",6,null,null,5]
[]
[null,"Spot Measurements"]
[{"$f":"A24+1","v":3},"Particulate Emission Monitors Correlation Spot Check to 6 units smoke stack","Per Unit",6,null,null,5]
[]
[null,"Spot Measurements"]
[{"$f":"A27+1","v":4},"Gaseous Emission Monitors  Parallel Verification Check to 6 units smoke stack","Per Unit",6,null,null,5]
[]
[null,"Emissions Measurements - To Boilers"]
[{"$f":"A30+1","v":5},"Traversing for velocity, gas volume, pressure, temperature, moisture, particulate matter, CO, SO2, NO, O2","Per Boiler",3,null,null,5]
[]
[null,"Sub Total"]
[]
[null,"TOTAL OF PRICES"]