{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Schedule 1","Sheet1"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Schedule 1","index":0,"n_rows":1312,"n_cols":8,"rows_kept":1312,"merged":[[0,1,0,7],[43,1,43,7],[82,1,82,7]]}
[]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[199,"A0",null,"PRELIMINARY AND GENERAL"]
[]
[200,null,"8.3","FIXED-CHARGE ITEMS"]
[]
[201,"A0.1","8,3,1","Contractual Requirements","Sum","1.0"]
[]
[203,null,"8.3.2","Establish Facilities on the Site :"]
[]
[205,null,"8.3.2.1 ","a) Facilities for Engineer"]
[]
[207,"A0.2","PSA 4.3","Furnished Office (1 No.)","Sum","1.0"]
[]
[209,"A0.3",null,"Name boards as per eThekwini municipality Water Design Branch plan No. 9","No.","2.0"]
[]
[211,null,"8.3.2.2","b) Facilities for Contractor"]
[]
[213,"A0.4",null,"Offices and storage sheds","Sum","1.0"]
[]
[215,"A0.5",null,"Workshops","Sum","1.0"]
[]
[217,"A0.6",null,"Ablution and latrine facilities","Sum","1.0"]
[]
[219,"A0.7",null,"Tools and equipment","Sum","1.0"]
[]
[221,"A0.8",null,"Water supplies, electric power and communications","Sum","1.0"]
[]
[223,"A0.9",null,"Dealing with water (Sub-clause 5.5)","Sum","1.0"]
[]
[225,"A0.10",null,"Access (Sub-clause 5.8)","Sum","1.0"]
[]
[227,"A0.11","PSA 8.9","Security (unarmed) on site for the duration of the contract ","Sum","1.0"]
[]
[229,"A0.12","PSA 8.10","Security (armed) on site for the duration of the contract","Sum","1.0"]
[]
[231,"A0.13","PSA 8.11","Daily photographing of Works and Traffic Accommodation, including record keeping.","Sum","1.0"]
[]
[233,"A0.14","PSA 8.12","Provision of \"As-Built\" information by professional surveyor","Sum","1.0"]
[]
[235,"A0.15","8.3.3","Other fixed-charge obligations","Sum","1.0"]
[]
[null," Total Carried Forward"]
[]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[237,"A0.16","8.3.4","Remove Engineer's and Contractor's Site establishment on completion","Sum","1.0"]
[]
[239,"A0.17","AH 14.1","Contractor's initial obligations in respect of the Occupational Health and Safety Act and Construction Regulations (Regulations (Contractor to provide full breakdown for this pricing item in accordance with H&S Specification and Construction Regulations requirements at time of submission of Detailed Health & Safety Plan)","Sum","1.0"]
[]
[241,"A0.18","AH 14.3","Prepare and submit Health and Safety file for Employer's approval","Sum","1.0"]
[]
[243,null,"8.4","TIME-RELATED ITEMS"]
[]
[245,"A0.19","8.4.1","Contractual Requirements","Days",{"v":560,"d":"560.00"}]
[]
[247,"A0.20","PSA 8.14","Provision of Mentorship by main contractor to CPG contractors","Days",{"v":560,"d":"560.00"}]
[]
[249,null,"8.4.2","Operate and maintain facilities on the Site:"]
[251,null,null,"a) Facilities for Engineer"]
[]
[253,"A0.21","PSA 4.3","Furnished Office (1 No.)","Days",{"v":560,"d":"560.00"}]
[]
[255,"A0.22",null,"Name boards (up to a maximum of 4)","Days",{"v":560,"d":"560.00"}]
[]
[257,null,"8.4.2.2","b) Facilities for Contractor for duration of construction, except where otherwise stated"]
[]
[259,"A0.23",null,"Offices and storage sheds","Days",{"v":560,"d":"560.00"}]
[]
[261,"A0.24",null,"Workshops","Days",{"v":560,"d":"560.00"}]
[]
[263,"A0.25",null,"Ablution and latrine facilities","Days",{"v":560,"d":"560.00"}]
[]
[265,"A0.26",null,"Tools and equipment","Days",{"v":560,"d":"560.00"}]
[]
[267,"A0.27",null,"Water supplies, electric power and communications","Days",{"v":560,"d":"560.00"}]
[]
[269,"A0.28","PSA 8.9","Security (unarmed) on site for the duration of the contract ","Days",{"v":560,"d":"560.00"}]
[]
[271,"A0.29","PSA 8.10","Security (armed) on site for the duration of the contract","Days",{"v":560,"d":"560.00"}]
[]
[null," Total Carried Forward"]
[null,"PRELIMINARY AND GENERAL"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[273,"A0.30","PSA 8.11","Daily photographing of works and Traffic Accommodation, including record keeping.","Days",{"v":560,"d":"560.00"}]
[]
[275,"A0.31","PSA 8.12","Provision of \"As-Built\" information by professional surveyor","Days",{"v":560,"d":"560.00"}]
[]
[277,"A0,32","8,4,3","Supervision for the duration of the contract","Days",{"v":560,"d":"560.00"}]
[]
[279,"A0.33","8.4.4","Company and head office overhead costs","Days",{"v":560,"d":"560.00"}]
[]
[281,"A0.34","8.4.5","Other time-related obligations","Days",{"v":560,"d":"560.00"}]
[]
[282]
[]
[283,"A0.35","AH 14.2","Contractor's time related obligations in respect of the Occupational Health and Safety Act and Construction Regulations (Contractor to provide full breakdown for this pricing item in accordance with H&S Specification and Construction Regulations requirements at time of submission of Detailed Health & Safety Plan)","Days",{"v":560,"d":"560.00"}]
[]
[284,"A0.36","PSA 8.21","Management of CPG Contractors (a maximum of 10 sub-contractors) during the course of the construction period.  The contractor will be paid pro-rate for the number of days that the specific sub-contractors is managed."]
[]
[null,"A0.36.1",null,"CPG Sub Contractor 1","Days",{"v":560,"d":"560.00"}]
[]
[null,"A0.36.2",null,"CPG Sub Contractor 2","Days",{"v":560,"d":"560.00"}]
[]
[null,"A0.36.3",null,"CPG Sub Contractor 3","Days",{"v":560,"d":"560.00"}]
[]
[null,"A0.36.4",null,"CPG Sub Contractor 4","Days",{"v":560,"d":"560.00"}]
[]
[null,"A0.36.5",null,"CPG Sub Contractor 5","Days",{"v":560,"d":"560.00"}]
[]
[null,"A0.36.6",null,"CPG Sub Contractor 6","Days",{"v":560,"d":"560.00"}]
[]
[null,"A0.36.7",null,"CPG Sub Contractor 7","Days",{"v":560,"d":"560.00"}]
[]
[null,"A0.36.8",null,"CPG Sub Contractor 8","Days",{"v":560,"d":"560.00"}]
[]
[null,"A0.36.9",null,"CPG Sub Contractor 9","Days",{"v":560,"d":"560.00"}]
[]
[null,"A0.36.10",null,"CPG Sub Contractor 10","Days",{"v":560,"d":"560.00"}]
[null," Total Carried Forward"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[]
[285,"A0.37",null,"Provision of traffic safety officer","Days",{"v":560,"d":"560.00"}]
[]
[287,null,"8.8","TEMPORARY WORKS"]
[]
[289,"A0.38","PSA 8.15","Provide temporary access to properties over open trench excavation","No.",{"v":1150,"d":"1150.00"}]
[]
[291,null,"8.8.4","Existing services"]
[]
[293,"A0,39","8,8,4 c)","Excavate by hand in soft material to expose existing services as instructed by the Engineer","m³",{"v":2690,"d":"2690.00"}]
[]
[295,"A0.40","8.8.4 d)","Temporary protection of Electricity service","Sum","1.0"]
[]
[297,"A0.41","8.8.4 d)","Temporary protection of all Telecommunication & Fibre Services","Sum","1.0"]
[]
[408,"A0.42","8.8.4 d)","Temporary protection of Sewer service","Sum","1.0"]
[]
[401,"A0.43","8.8.4 d)","Temporary protection of Stormwater service","Sum","1.0"]
[]
[403,"A0.44","8.8.4 d)","Temporary protection of Petrochemical/Gas services","Sum","1.0"]
[]
[409,"A0.45","8.8.4 d)","Temporary protection of any water mains not being replaced under the Project Scope, typically trunk mains.","Sum","1.0"]
[]
[null,"A0.46",null,"All-inclusive rate for supervision, lighting, attending to health and safety requirements for tie-ins / water connections of size up to 250mm diameter of any configuration -  undertaken by the contractor on behalf of eThekwini Water and Sanitation / Operations.  The duration of the tie-in would be a maximum of 48 hours.  The cost of labour, plant and consumables required in preparing and undertaking the tie-in work is measured under Dayworks and the respective extra-over items for dayworks performed after normal hours including night work.","No.",{"v":5,"d":"5.00"}]
[]
[]
[null," Total Carried Forward To Summary"]
[]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[299,"A1",null,"SUMS STATED PROVISIONALLY "]
[]
[301,"A1.1","PSA 8.18","Material and other tests ordered by the Employer or his representative","P Sum",{"v":1,"d":"1.00"},{"v":336000,"d":"R336,000.00"},{"$f":"F155*G155","v":{"v":336000,"d":"R336,000.00"}}]
[]
[302,"A1.1.1","8.5 b) 2","Overheads, charges and profits on item above","%",{"v":336000,"d":"R336,000.00"}]
[]
[303,"A1.2","PSA 8.13","Community Liaison Officer (CLO)","P Sum",{"v":1,"d":"1.00"},{"v":360000,"d":"R360,000.00"},{"$f":"F159*G159","v":{"v":360000,"d":"R360,000.00"}}]
[]
[304,"A1.2.1","8.5 b) 2","Overheads, charges and profits on item above","%",{"v":360000,"d":"R360,000.00"}]
[]
[305,"A1.3","PSA 8.16","Supply use (or hire) of specialist equipment for the detection of underground services (Prov)","P Sum",{"v":1,"d":"1.00"},{"v":75000,"d":"R75,000.00"},{"$f":"F163*G163","v":{"v":75000,"d":"R75,000.00"}}]
[]
[306,"A1.3.1","8.5 b) 2","Overheads, charges and profits on item above","%",{"v":75000,"d":"R75,000.00"}]
[]
[307,"A1.4","PSA 8.19","Leak detection on existing pipes by an approved specialist","P Sum",{"v":1,"d":"1.00"},{"v":75000,"d":"R75,000.00"},{"$f":"F167*G167","v":{"v":75000,"d":"R75,000.00"}}]
[]
[308,"A1.4.1","8.5 b) 2","Overheads, charges and profits on item above","%",{"v":75000,"d":"R75,000.00"}]
[]
[309,"A1.5","PSA 8.20","Institutional and Social Facilitator rendered by sub-contractor as per clause 4.4.4 of the General Conditions of Contract","P Sum",{"v":1,"d":"1.00"},{"v":420000,"d":"R420,000.00"},{"$f":"F171*G171","v":{"v":420000,"d":"R420,000.00"}}]
[]
[310,"A1.5.1","8.5 b) 2","Overheads, charges and profits on item above","%",{"v":420000,"d":"R420,000.00"}]
[]
[311,"A1.6","PSA 8.17","As-built/GIS field work and verification","P Sum",{"v":1,"d":"1.00"},{"v":25000,"d":"R25,000.00"},{"$f":"F175*G175","v":{"v":25000,"d":"R25,000.00"}}]
[]
[312,"A1.6.1","8.5 b) 2","Overheads, charges and profits on item above","%",{"v":25000,"d":"R25,000.00"}]
[]
[313,"A1.7",null,"Inspection, structural design, supply, test, comission steel pipe supports and fixing brackets for bridge crossings","P Sum",{"v":1,"d":"1.00"},{"v":112000,"d":"R112,000.00"},{"$f":"F179*G179","v":{"v":112000,"d":"R112,000.00"}}]
[]
[314,"A1.7.1","8.5 b) 2","Overheads, charges and profits on item above","%",{"v":112000,"d":"R112,000.00"}]
[]
[315,"A1.8",null,"Provisional sum for Computer equipment (Software and Hardware) for the Engineer and Employer","P Sum",{"v":1,"d":"1.00"},{"v":120000,"d":"R120,000.00"},{"$f":"F183*G183","v":{"v":120000,"d":"R120,000.00"}}]
[]
[316,"A1.8.1","8.5 b) 2","Overheads, charges and profits on item above","%",{"v":120000,"d":"R120,000.00"}]
[null," Total Carried Forward To Summary"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[]
[317,"A1.9",null,"Provisional sum for Allowance for mentorship of 2 student technician resources for the duration of the Contract Period","P Sum",{"v":1,"d":"1.00"},{"v":200000,"d":"R200,000.00"},{"$f":"F190*G190","v":{"v":200000,"d":"R200,000.00"}}]
[]
[318,"A1.9.1","8.5 b) 2","Overheads, charges and profits on item above","%",{"v":200000,"d":"R200,000.00"}]
[]
[413,"A1.10",null,"Provisional sum for Additional lateral support where ordered by the Engineer","P Sum",{"v":1,"d":"1.00"},{"v":200000,"d":"R200,000.00"},{"$f":"F194*G194","v":{"v":200000,"d":"R200,000.00"}}]
[]
[410,"A1.10.1","8.5 b) 2","Overheads, charges and profits on item above","%",{"v":200000,"d":"R200,000.00"}]
[]
[414,"A1.11",null,"Provisional sum for Additional Quality Control Equipment for use by the Engineer","P Sum",{"v":1,"d":"1.00"},{"v":50000,"d":"R50,000.00"},{"$f":"F198*G198","v":{"v":50000,"d":"R50,000.00"}}]
[]
[]
[412,"A1.11.1",null,"Overheads, charges and profits on item above","%",{"v":50000,"d":"R50,000.00"}]
[]
[319,"A1.12",null,"Construction of new and Rehabilitation of Existing PRV Chambers ","P Sum",{"v":1,"d":"1.00"},{"v":200000,"d":"R200,000.00"},{"$f":"F203*G203","v":{"v":200000,"d":"R200,000.00"}}]
[]
[1453,"A1.12.1","8.5 b) 2","Overheads, charges and profits on item above","%",{"v":200000,"d":"R200,000.00"}]
[]
[null,"A1.13","PSA 8.22","Provisional Sum for Adhoc Watermain repair or replacement as and when requested by the Client ","P Sum",{"v":1,"d":"1.00"},{"v":5000000,"d":"R5,000,000.00"},{"v":5000000,"d":"R5,000,000.00"}]
[1455,null,null,"replacement as and when requested by the Client "]
[]
[null,"A1.14","8.5 b) 2","Overheads, charges and profits on item A1.13","%",{"v":5000000,"d":"R5,000,000.00"}]
[]
[null," Total Carried Forward To Summary"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[417,"A2","SANS 1921-2","TRAFFIC ACCOMMODATION"]
[]
[419,"A2.4.1","PSA 8.8.2","Accommodation of traffic and re-use or removal of temporary traffic control facilities","m",{"v":19500,"d":"19500.00"}]
[]
[421,"A2,4,2",null,"Flagmen (including equipment) - including all CPG sub-contractor flagmen requirements, assuming a maximum of 10 CPG sub-contractors","man-day",{"v":2480,"d":"2480.00"}]
[]
[423,"A2,4,3",null,"Portable STOP and GO signs","No.",{"v":40,"d":"40.00"}]
[]
[425,"A2,4,4",null,"Amber flicker lights","No.",{"v":25,"d":"25.00"}]
[]
[427,null,null,"Road signs, R- and TR-series,"]
[]
[429,"A2,4,5",null,"900mm diameter","No.",{"v":30,"d":"30.00"}]
[]
[431,null,null,"Road signs, TW-TWA series, "]
[]
[433,"A2,4,6",null,"1200mm sides","No.",{"v":30,"d":"30.00"}]
[]
[435,null,null,"Road signs, TGP series,"]
[]
[437,"A2,4,7",null,"900mm x 675mm TGP1","No.",{"v":30,"d":"30.00"}]
[]
[439,"A2,4,8",null,"900mm x 675mm TGP3","No.",{"v":30,"d":"30.00"}]
[]
[441,"A2,4,9",null,"900mm x 675mm TGP4","No.",{"v":30,"d":"30.00"}]
[]
[443,"A2,4,10",null,"900mm x 675mm TGP9","No.",{"v":50,"d":"50.00"}]
[]
[445,"A2,4,11",null,"Traffic cones (750mm high with high visibility reflectorized jackets)","No.",{"v":200,"d":"200.00"}]
[]
[447,null,null,"Delineators (TW401/402) including stands and supports"]
[]
[449,"A2,4,12",null,"Single sided (250mm x 1000mm)","No.",{"v":450,"d":"450.00"}]
[]
[451,"A2,4,13","PSDA 5,1,1,1","Plastic Mesh Safety Fencing","m",{"v":3950,"d":"3950.00"}]
[]
[null," Total Carried Forward to Summary"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[453,"A3.4","SANS 1200 A 8.","DAYWORKS (Quantities are only indicative and shall only be used upon instruction by Engineer)"]
[]
[455,null,null,"Labour"]
[]
[457,"A3,4,1",null,"Artisan","h",{"v":150,"d":"150.00"}]
[]
[458,"A3,4,2",null,"Extra over Item A3,4,1 for work undertaken after hours including night work.","h",{"v":75,"d":"75.00"}]
[]
[459,"A3,4,3",null,"Construction hand","h",{"v":150,"d":"150.00"}]
[]
[460,"A3,4,4",null,"Extra over Item A3,4,3 for work undertaken after hours including night work.","h",{"v":75,"d":"75.00"}]
[]
[461,"A3,4,5",null,"Unskilled Labourer","h",{"v":250,"d":"250.00"}]
[]
[462,"A3,4,6",null,"Extra over Item A3,4,5 for work undertaken after hours including night work.","h",{"v":75,"d":"75.00"}]
[]
[463,"A3,4,7",null,"Semi-skilled labourer","h",{"v":250,"d":"250.00"}]
[]
[464,"A3,4,8",null,"Extra over Item A3,4,7 for work undertaken after hours including night work.","h",{"v":75,"d":"75.00"}]
[]
[465,"A3.4.9",null,"Flagmen","h",{"v":250,"d":"250.00"}]
[]
[466,"A3,4,10",null,"Extra over Item A3,4,9 for work undertaken after hours including night work.","h",{"v":75,"d":"75.00"}]
[]
[467,null,null,"Equipment"]
[]
[469,"A3,4,11",null,"Air compressor of at least 7 m³/min (includes breakers and hose)","h",{"v":100,"d":"100.00"}]
[]
[470,"A3,4,12",null,"Extra over Item A3,4,11 for work undertaken after hours including night work.","h",{"v":50,"d":"50.00"}]
[]
[471,"A3,4,13",null,"Generator or Alternator set of at least 10 kW capacity","h",{"v":100,"d":"100.00"}]
[]
[472,"A3,4,14",null,"Extra over Item A3,4,13 for work undertaken after hours including night work.","h",{"v":50,"d":"50.00"}]
[]
[473,"A3,4,15",null,"Vibrating plate compactor","h",{"v":100,"d":"100.00"}]
[]
[474,"A3,4,16",null,"Extra over Item A3,4,15 for work undertaken after hours including night work.","h",{"v":50,"d":"50.00"}]
[]
[475,"A3,4,17",null,"Rammer","h",{"v":100,"d":"100.00"}]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[476,"A3,4,18",null,"Extra over Item A3,4,17 for work undertaken after hours including night work.","h",{"v":50,"d":"50.00"}]
[]
[477,"A3,4,19",null,"Tractor/Loader/Backhoe, power approximately 55kW","h",{"v":200,"d":"200.00"}]
[]
[478,"A3,4,20",null,"Extra over Item A3,4,19 for work undertaken after hours including night work.","h",{"v":100,"d":"100.00"}]
[]
[479,"A3,4,21",null,"Tippers (5m³)","h",{"v":200,"d":"200.00"}]
[]
[480,"A3,4,22",null,"Extra over Item A3,4,21 for work undertaken after hours including night work.","h",{"v":100,"d":"100.00"}]
[]
[481,"A3,4,23",null,"Tippers (10m³)","h",{"v":200,"d":"200.00"}]
[]
[482,"A3,4,24",null,"Extra over Item A3,4,23 for work undertaken after hours including night work.","h",{"v":100,"d":"100.00"}]
[]
[483,"A3,4,25",null,"Hand propelled vibratory roller, 0,5t","h",{"v":200,"d":"200.00"}]
[]
[484,"A3,4,26",null,"Extra over Item A3,4,25 for work undertaken after hours including night work.","h",{"v":100,"d":"100.00"}]
[]
[485,"A3,4,27",null,"Water Tanker (6 kℓ)","h",{"v":250,"d":"250.00"}]
[]
[486,"A3,4,28",null,"Extra over Item A3,4,27 for work undertaken after hours including night work.","h",{"v":100,"d":"100.00"}]
[]
[487,"A3,4,29",null,"Excavator (130 kW)","h",{"v":250,"d":"250.00"}]
[]
[488,"A3,4,30",null,"Extra over Item A3,4,29 for work undertaken after hours including night work.","h",{"v":100,"d":"100.00"}]
[]
[489,"A3,4,31",null,"Hydraulic Breaker (Pecker), 22t","h",{"v":250,"d":"250.00"}]
[]
[490,"A3,4,32",null,"Extra over Item A3,4,31 for work undertaken after hours including night work.","h",{"v":100,"d":"100.00"}]
[]
[491,"A3,4,33",null,"Small concrete mixer, ± 200 ℓ","h",{"v":250,"d":"250.00"}]
[]
[492,"A3,4,34",null,"Extra over Item A3,4,33 for work undertaken after hours including night work.","h",{"v":100,"d":"100.00"}]
[]
[493,"A3,4,35",null,"Industrial drill","h",{"v":250,"d":"250.00"}]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[494,"A3,4,36",null,"Extra over Item A3,4,35 for work undertaken after hours including night work.","h",{"v":100,"d":"100.00"}]
[]
[495,null,null,"Transport"]
[]
[497,"A3,4,37",null,"LDV","km",{"v":2500,"d":"2500.00"}]
[]
[498,"A3,4,38",null,"Extra over Item A3,4,37 for work undertaken after hours including night work.","km",{"v":1000,"d":"1000.00"}]
[]
[499,"A3,4,39",null,"Flatbed truck (incl 5t crane)","km",{"v":4500,"d":"4500.00"}]
[]
[500,"A3,4,40",null,"Extra over Item A3,4,39 for work undertaken after hours including night work.","km",{"v":2000,"d":"2000.00"}]
[]
[501,"A3,4,41",null,"Low bed trailer with mechanical horse","km",{"v":1500,"d":"1500.00"}]
[]
[null,"A3,4,42",null,"Extra over Item A3,4,41 for work undertaken after hours including night work.","km",{"v":800,"d":"800.00"}]
[]
[null,"A3,4,43","PSA 8.7","Materials"]
[]
[null,"A3,4,43,1",null,"Sand (Building)","m3",{"v":15,"d":"15.00"}]
[]
[null,"A3,4,43,2",null,"Sand (river)","m3",{"v":10,"d":"10.00"}]
[]
[null,"A3,4,43,3",null,"50 kg pocket of Cement","No.",{"v":80,"d":"80.00"}]
[]
[null,"A3,4,43,4",null,"Hard burnt red Face Brick (satin red)","m2",{"v":150,"d":"150.00"}]
[]
[{"$nulls":3},"Dayworks Provisional Sum"]
[]
[null,"A3,4,44","PSA 8.7","Allowance for Dayworks activities not covered under the Daworks section / quantities allowed for in the BOQ.","P Sum",{"v":1,"d":"1.00"},{"v":500000,"d":"R500,000.00"},{"$f":"F362*G362","v":{"v":500000,"d":"R500,000.00"}}]
[]
[]
[]
[]
[null," Total Carried Forward To Summary"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[503,"A4.4","\"SANS1200 C\"","SECTION : SITE CLEARANCE"]
[]
[505,null,null,"CLEAR SITE"]
[]
[507,"A4.4.1","8.2.1 & PSC 5.3","Clear and grub Site (excluding items listed below)","m²",{"v":11500,"d":"11500.00"}]
[]
[509,"A4,4,2","8,2,1 & PSC 5,3","Roadways","m²",{"v":18850,"d":"18850.00"}]
[]
[511,"A4,4,3","8,2,1 & PSC 5,3","Side walks and other paved areas","m²",{"v":8750,"d":"8750.00"}]
[]
[513,"A4,4,4","8,2,1 & PSC 5,3","Removal of fire hydrants and associated material","No,",{"v":160,"d":"160.00"}]
[]
[515,"A4,4,5","8,2,1 & PSC 5,3","Removal of guard rails and posts","m",{"v":400,"d":"400.00"}]
[]
[517,"A4,4,6","8,2,1 & PSC 5,3","Removal of traffic signs, bollards and posts","No,",{"v":300,"d":"300.00"}]
[]
[519,"A4,4,7","8,2,1 & PSC 5,3","Removal of brick walls","m²",{"v":870,"d":"870.00"}]
[]
[521,null,"8.2.2","Remove and grub large trees and tree stumps of girth:"]
[]
[604,"A4,4,8",null,"Under 1 m","No,",{"v":15,"d":"15.00"}]
[{"$nulls":5}," "]
[523,"A4,4,9",null,"Over 1 m and up to 2 m","No,",{"v":8,"d":"8.00"}]
[]
[525,"A4,4,10","8,2,5","Take down existing fences, and stockpile on site","m²",{"v":2350,"d":"2350.00"}]
[]
[527,"A4,4,11","PSC 8,2,20","Take down existing pre-cast walling, and stockpile on site","m²",{"v":1500,"d":"1500.00"}]
[]
[529,"A4,4,12","PSC 8,2,17","Reinstate existing fences","m²",{"v":2350,"d":"2350.00"}]
[]
[531,"A4,4,13","PSC 8,2,21","Reinstate pre-cast walling","m²",{"v":1500,"d":"1500.00"}]
[]
[533,"A4,4,14","PSL 8,2,22","Construct new pre-cast walling","m²",{"v":150,"d":"150.00"}]
[]
[535,"A4,4,15","PSC 8,2,23","Construct new double leaf  brick wall","m²",{"v":100,"d":"100.00"}]
[]
[537,"A4,4,16","PSC 8,2,18","Reinstate guard rails and guard rail posts","m",{"v":400,"d":"400.00"}]
[]
[539,"A4,4,17","PSC 8,2,19","Reinstate traffic and street signs, bollards and posts","No,",{"v":300,"d":"300.00"}]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[541,"A4.4.18","PSC 8.2.14","Landscape preservation and conservation of Flora","m²",{"v":2710,"d":"2710.00"}]
[]
[543,"A4,4,19","8,2,7","Dismantle and remove pipelines encased in concrete","m",{"v":301,"d":"301.00"}]
[]
[545,"A4,4,20","8,2,7","Dismantle and remove pipelines (not encased in concrete), including valves and fittings","m",{"v":2350,"d":"2350.00"}]
[]
[547,"A4,4,21","PSC 8,2,11","Extra over item A4,4,20 for dismantling, removal and disposal of Asbestos Cement (AC) pipelines (not encased in concrete), including valves and fittings","m",{"v":3800,"d":"3800.00"}]
[]
[549,"A4.4.22","PSC 8.2.12","Recovering and stockpiling of re-usable material from clearing operation","t",{"v":9.5,"d":"9.50"}]
[]
[551,"A4.4.23","PSC 8.2.13","Loading, transporting and offloading of Re-usable Material to EWS store or Municipal Depot","t",{"v":9.5,"d":"9.50"}]
[]
[553,"A4.4.24","PSC 8.2.10","Remove topsoil along pipeline route to nominal depth of 150mm and stockpile on site","m³",{"v":1938,"d":"1938.00"}]
[]
[555,"A4,4,25","PSC 8,2,15","Reinstate topsoil from stockpile","m³",{"v":1938,"d":"1938.00"}]
[]
[556]
[]
[557,"A4,4,26","PSC 8,2,16","Reinstate topsoil by importation from commercial sources","m³",{"v":300,"d":"300.00"}]
[]
[559,"A4,4,27","PSDB 8,3,6,2","Grassing","m²",{"v":12250,"d":"12250.00"}]
[]
[null," Total Carried Forward to Summary"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[606,"A5.4","\"SANS1200 DB\"","SECTION : PIPE TRENCHES"]
[]
[608,null,null,"EXCAVATION"]
[]
[610,null,"8.3.2(a)","Excavate in all materials for trenches backfill, compact, and dispose of surplus/unsuitable material, for all pipes up to 110 mm diam. for total trench depth:"]
[]
[612,"A5,4,1",null,"Exceeding 0,0 m but not exceeding 1,0 m","m",{"v":400,"d":"400.00"}]
[]
[614,"A5,4,2",null,"Exceeding 1,0 m but not exceeding 2,0 m","m",{"v":800,"d":"800.00"}]
[]
[616,"A5,4,3",null,"Exceeding 2,0 m but not exceeding 3,0 m","m",{"v":100,"d":"100.00"}]
[]
[618,null,null,"Over 110 up to 300 mm diam. for total trench depth:"]
[]
[620,"A5,4,4",null,"Exceeding 0,0 m but not exceeding 1,0 m","m",{"v":250,"d":"250.00"}]
[]
[622,"A5,4,5",null,"Exceeding 1,0 m but not exceeding 2,0 m","m",{"v":500,"d":"500.00"}]
[]
[624,"A5,4,6",null,"Exceeding 2,0 m but not exceeding 3,0 m","m",{"v":75,"d":"75.00"}]
[]
[626,null,null,"Over 300 up to 400 mm diam. for total trench depth:"]
[]
[628,"A5,4,7",null,"Exceeding 0,0 m but not exceeding 1,0 m","m",{"v":10,"d":"10.00"}]
[]
[630,"A5,4,8",null,"Exceeding 1,0 m but not exceeding 2,0 m","m",{"v":100,"d":"100.00"}]
[]
[632,"A5,4,9",null,"Exceeding 2,0 m but not exceeding 3,0 m","m",{"v":50,"d":"50.00"}]
[]
[634,null,"8.3.2(b)","Extra-over items A5.4.1 to A5.4.9  incl. for (prov):"]
[]
[636,"A5.4.10",null,"Intermediate excavation","m³",{"v":150,"d":"150.00"}]
[]
[638,"A5.4.11",null,"Hard rock excavation","m³",{"v":50,"d":"50.00"}]
[]
[640,"A5.4.12",null,"Boulder excavation Class A","m³",{"v":15,"d":"15.00"}]
[]
[642,"A5.4.13",null,"Boulder excavation Class B","m³",{"v":10,"d":"10.00"}]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[644,"A5.4.14","8.3.2(c)","Excavate and dispose of unsuitable material from trench bottom (Provisional)","m³",{"v":200,"d":"200.00"}]
[]
[646,null,"SANS 1200 PSDA 8.3.2 (a)","Excavate in all materials for trenches backfill, compact, and dispose of surplus/unsuitable material, in RESTRICTED AREAS for pipes: 110 mm diam, at depth ranges:"]
[]
[648,"A5,4,15",null,"Exceeding 0,0 m but not exceeding 1,0 m","m",{"v":1250,"d":"1250.00"}]
[]
[650,"A5,4,16",null,"Exceeding 1,0 m but not exceeding 2,0 m","m",{"v":17950,"d":"17950.00"}]
[]
[652,"A5,4,17",null,"Exceeding 2,0 m but not exceeding 3,0 m","m",{"v":100,"d":"100.00"}]
[]
[654,null,null,"Over 110 up to 300 mm diam. for total trench depth:"]
[]
[656,"A5,4,18",null,"Exceeding 0,0 m but not exceeding 1,0 m","m",{"v":500,"d":"500.00"}]
[]
[658,"A5,4,19",null,"Exceeding 1,0 m but not exceeding 2,0 m","m",{"v":3750,"d":"3750.00"}]
[]
[660,"A5,4,20",null,"Exceeding 2,0 m but not exceeding 3,0 m","m",{"v":50,"d":"50.00"}]
[]
[662,null,null,"Over 300 up to 400 mm diam. for total trench depth:"]
[]
[664,"A5,4,21",null,"Exceeding 0,0 m but not exceeding 1,0 m","m",{"v":25,"d":"25.00"}]
[]
[666,"A5,4,22",null,"Exceeding 1,0 m but not exceeding 2,0 m","m",{"v":100,"d":"100.00"}]
[]
[668,"A5,4,23",null,"Exceeding 2,0 m but not exceeding 3,0 m","m",{"v":50,"d":"50.00"}]
[]
[670,null,"SANS 1200 PSDA 8.3.2(b)","Extra-over items A5.4.15 to A5.4.23 incl. for (prov):"]
[]
[672,"A5.4.24",null,"Intermediate excavation","m³",{"v":4915,"d":"4915.00"}]
[]
[674,"A5,4,25",null,"Hard rock excavation","m³",{"v":1620,"d":"1620.00"}]
[]
[676,"A5.4.26",null,"Boulder excavation Class A","m³",{"v":100,"d":"100.00"}]
[]
[678,"A5.4.27",null,"Boulder excavation Class B","m³",{"v":50,"d":"50.00"}]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[680,null,null,"EXCAVATION ANCILLARIES Make up deficiency in backfill material (Provisional)"]
[]
[682,"A5.4.28","8.3.3.1 (a)","from other necessary excavations on site","m³",{"v":2650,"d":"2650.00"}]
[]
[684,"A5.4.29","8.3.3.1 (c)","by importation from commercial sources","m³",{"v":1300,"d":"1300.00"}]
[]
[686,null,"8.3.4 (a)","Shore trench opposite structure or service or as instructed by Engineer, for total trench depth:"]
[]
[688,"A5.4.30",null,"Exceeding 0,0 m but not exceeding 1,0 m","m",{"v":500,"d":"500.00"}]
[]
[690,"A5.4.31",null,"Exceeding 1,0 m but not exceeding 2,0 m","m",{"v":2250,"d":"2250.00"}]
[]
[692,"A5.4.32",null,"Exceeding 2,0 m but not exceeding 3,0 m","m",{"v":125,"d":"125.00"}]
[]
[694,null,null,"EXISTING SERVICES"]
[]
[696,"A5,4,33","PSDB 8,3,5(a)","Services that intersect a trench","No,",{"v":500,"d":"500.00"}]
[]
[698,"A5,4,34","PSDB 8,3,5(b)","Services that adjoin a trench","m",{"v":8500,"d":"8500.00"}]
[]
[null," Total Carried Forward to Summary"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[]
[707,"A6.4","SASTT-TS-TT3: 2016","HORIZONTAL DIRECTIONAL DRILLING"]
[]
[709,null,null,"Horizontal Directional Drilling (HDD) as directed by the Engineer"]
[]
[711,"A6,4,1","Annex C 1,2,1","HDD establishment on site","Sum",{"v":1,"d":"1.00"}]
[]
[713,"A6,4,2","Annex C 1,2,2","HDD installation setup","No,",{"v":100,"d":"100.00"}]
[]
[715,"A6,4,3","Annex C 1,2,3","Excavation of drilling Pits","No,",{"v":200,"d":"200.00"}]
[]
[717,"A6,4,4","Annex C 1,2,4","Hand excavation of pits","m³",{"v":500,"d":"500.00"}]
[]
[719,null,"Annex C 1.2.5","HDD installation of HDPE sleeves (SDR 11, PE 100, PN 16),see Standard eThekwini Drawing #118 \"\"Typical Watermain Pipe Duct for Road Crossings\"\""]
[]
[721,"A6,4,5",null,"75 mm diam, ","m",{"v":56,"d":"56.00"}]
[]
[723,"A6,4,6",null,"110 mm diam,","m",{"v":125,"d":"125.00"}]
[]
[725,"A6,4,7",null,"160 mm diam, ","m",{"v":80,"d":"80.00"}]
[]
[727,"A6,4,8",null,"200 mm diam, ","m",{"v":29,"d":"29.00"}]
[]
[729,"A6,4,9",null,"250 mm diam, ","m",{"v":15,"d":"15.00"}]
[]
[731,"A6,4,10",null,"315 mm diam,","m",{"v":25,"d":"25.00"}]
[]
[733,"A6,4,11",null,"355 mm diam,","m",{"v":10,"d":"10.00"}]
[]
[735,null,"Annex C 1.2.5","Supply, install, test and commission under the HDD installation the following HDPE pipes (SDR 11, PE 100, PN 16) inside HDPE sleeves (items A6,4,5 to A6,4,11) complete with stainless steel Table 1600 puddle flange but-welded to one end,  Item includes stainless steel Table 1600 flanged to both ends of pipes"]
[]
[737,"A6,4,12",null,"110mm diam,","m",{"v":90,"d":"90.00"}]
[]
[739,"A6,4,13",null,"160mm diam,","m",{"v":50,"d":"50.00"}]
[]
[]
[null," Total Carried Forward To Summary"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[808,"A7,4","\"SANS1200 LB\"","SECTION : BEDDING AND SUB-SOIL DRAINS"]
[]
[810,null,null,"PROVISION OF BEDDING"]
[]
[812,null,null,"Available from trench excavations (All haul regarded as free haul)"]
[]
[814,"A7,4,1","8,2,1","Selected granular material","m³",{"v":750,"d":"750.00"}]
[]
[816,"A7,4,2",null,"Selected fill material","m³",{"v":4915,"d":"4915.00"}]
[]
[818,null,"PSLB 8,2,2,3","Provision of bedding from commercial sources"]
[]
[820,"A7,4,3",null,"Selected granular material","m³",{"v":7400,"d":"7400.00"}]
[]
[822,"A7,4,4",null,"Selected fill blanket","m³",{"v":2850,"d":"2850.00"}]
[]
[824,"A7,4,5",null,"Rock fill","m³",{"v":150,"d":"150.00"}]
[]
[826,"A7,4,6",null,"Stone bedding","m³",{"v":300,"d":"300.00"}]
[]
[827,"A7,4,7",null,"Supply, place and compact 5% soilcrete using material on site.","m³",{"v":100,"d":"100.00"}]
[]
[828,"A7,4,8",null,"Supply, install and join Bidim (Grade A4) around stone bedding,","m²",{"v":750,"d":"750.00"}]
[]
[830,null,"SANS 1200 LE & PSLB 5,2,5","SUB-SOIL DRAINS"]
[]
[832,null,null,"Supply and lay slotted HDPE subsoil drainage pipe complete with couplings in stone bedding"]
[]
[834,"A7,4,8",null,"110 mm","m",{"v":435,"d":"435.00"}]
[]
[836,"A7,4,9",null,"160 mm","m",{"v":205,"d":"205.00"}]
[]
[838,null,null,"Supply and lay uPVC bends, junctions and stops in stone bedding"]
[]
[840,"A7,4,10",null,"110 mm Bend","No.",{"v":10,"d":"10.00"}]
[]
[842,"A7,4,11",null,"160 mm Bend","No.",{"v":10,"d":"10.00"}]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[844,"A7,4,12",null,"110 mm Junction","No.",{"v":25,"d":"25.00"}]
[]
[846,"A7,4,13",null,"160 mm Junction","No.",{"v":25,"d":"25.00"}]
[]
[848,"A7,4,14",null,"110 mm Stop End","No.",{"v":10,"d":"10.00"}]
[]
[850,"A7,4,15",null,"160 mm Stop End","No.",{"v":10,"d":"10.00"}]
[]
[852,null,null,"Geofabric"]
[]
[854,"A7,4,16",null,"Supply, install and  join Bidim (Grade A4) around slotted pipes, bedding and fittings,","m²",{"v":210,"d":"210.00"}]
[]
[856,null,null,"Crushed Stone for Subsoil drains"]
[]
[858,"A7,4,17",null,"Supply and lay 13 mm stone","m³",{"v":80,"d":"80.00"}]
[]
[860,null,null,"Outlet/Join to existing"]
[]
[862,"A7,4,18","PSLE 8,2,14","Join subsoil drains to existing stormwater manholes and repair","No.",{"v":50,"d":"50.00"}]
[]
[864,"A7,4,19","SANS 1200 GA 8,4,3","Concrete V-drain (Class 20/19), including formwork (see SANRAL drawing TD-D-RD-1001-V1 Type E ) ","m³",{"v":25,"d":"25.00"}]
[]
[]
[null," Total Carried Forward To Summary"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[909,"A8.4","\"SANS1200 L\"","SECTION : WATER MAINS"]
[]
[911,null,"PSL 8.2.1","Supply, lay and bed pipes complete with Couplings. Rate includes disinfection and pressure testing."]
[]
[913,null,"PSL 8.2.1","HDPE pipes (SDR 11, PE 100, PN 16)"]
[]
[915,"A8.4.1",null,"25mm diam,","m",{"v":500,"d":"500.00"}]
[]
[917,"A8.4.2",null,"50 mm diam, ","m",{"v":6700,"d":"6700.00"}]
[]
[919,null,"PSL 8,2,1","mPVC pipes (Class 12)"]
[]
[921,"A8.4.3",null,"75mm diam,","m",{"v":1370,"d":"1370.00"}]
[]
[923,"A8.4.4",null,"110 mm diam, ","m",{"v":9900,"d":"9900.00"}]
[]
[925,"A8.4.5",null,"160 mm diam, ","m",{"v":3715,"d":"3715.00"}]
[]
[927,"A8.4.6",null,"200 mm diam, (Provisional)","m",{"v":50,"d":"50.00"}]
[]
[929,"A8.4.7",null,"250 mm diam, (Provisional)","m",{"v":20,"d":"20.00"}]
[]
[931,"A8.4.8",null,"315 mm diam, (Provisional)","m",{"v":15,"d":"15.00"}]
[]
[933,"A8.4.9",null,"355 mm diam, (Provisional)","m",{"v":10,"d":"10.00"}]
[]
[1440,null,"PSL 3,4 & PSL 8,2,1","Steel flanged pipes for road crossings, all flanges Table 16, pipe diameters and wall thicknesses, pipe coating and corrosion protection as per project specification, All pipe lengths to be 12m unless otherwise instructured by Engineer, Pipe fully flanged both sides and welded to meet required length for road crossing,"]
[]
[1442,"A8.4.10",null,"80mm diameter - 10m long pipe flanged both sides","No.",{"v":75,"d":"75.00"}]
[]
[1444,"A8.4.11",null,"100 mm diameter - 10m long pipe flanged both sides","No.",{"v":20,"d":"20.00"}]
[]
[1446,"A8.4.12",null,"150 mm diameter - 10m long pipe flanged both sides","No.",{"v":25,"d":"25.00"}]
[]
[1448,"A8.4.13",null,"200 mm diameter - 10m long pipe flanged both sides","No.",{"v":3,"d":"3.00"}]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[]
[1450,"A8.4.14",null,"250 mm diameter - 10m long pipe flanged both sides","No.",{"v":1,"d":"1.00"}]
[]
[1456,null,"PSL 3,4 & PSL 8,2,1","Extra over flanged steel pipes for road crossings where lengths are to be adjusted to meet specific road width requirements."]
[]
[1458,"A8.4.15",null,"Item A8.4.10 - 80mm diameter","m",{"v":220,"d":"220.00"}]
[]
[1460,"A8.4.16",null,"Item A8.4.11 - 100 mm diameter","m",{"v":100,"d":"100.00"}]
[]
[1462,"A8.4.17",null,"Item A8.4.12 - 150 mm diameter","m",{"v":50,"d":"50.00"}]
[]
[1464,"A8.4.18",null,"Item A8.4.13 - 200 mm diameter","m",{"v":5,"d":"5.00"}]
[]
[1466,"A8.4.19",null,"Item A8.4.14 - 250 mm diameter","m",{"v":16,"d":"16.00"}]
[]
[935,null,"PSL 8,2,1","uPVC Class 34 solid wall (heavy duty) sleeves at road crossings"]
[]
[937,"A8.4.20",null,"160 mm diam, ","m",{"v":200,"d":"200.00"}]
[]
[939,"A8.4.21",null,"200 mm diam, ","m",{"v":250,"d":"250.00"}]
[]
[941,"A8.4.22",null,"250 mm diam, ","m",{"v":50,"d":"50.00"}]
[]
[943,"A8.4.23",null,"315 mm diam,","m",{"v":25,"d":"25.00"}]
[]
[945,"A8.4.24",null,"355 mm diam,","m",{"v":25,"d":"25.00"}]
[]
[947,"A8.4.25",null,"400mm diam,","m",{"v":25,"d":"25.00"}]
[]
[949,"A8.4.26",null,"450mm diam,","m",{"v":25,"d":"25.00"}]
[]
[951,null,"PSL 8,2,1","HDPE (SDR 11, PE 100, PN 16), sleeves at road crossings"]
[]
[953,"A8.4.27",null,"200mm diam,","m",{"v":50,"d":"50.00"}]
[]
[955,"A8.4.28",null,"250mm diam,","m",{"v":460,"d":"460.00"}]
[]
[957,"A8.4.29",null,"315mm diam,","m",{"v":30,"d":"30.00"}]
[]
[959,"A8.4.30",null,"355mm diam,","m",{"v":10,"d":"10.00"}]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[961,"A8.4.31",null,"400mm diam,","m",{"v":10,"d":"10.00"}]
[]
[963,"A8.4.32",null,"450mm diam,","m",{"v":10,"d":"10.00"}]
[]
[965,null,"PSL 8,2,18","Extra-over item A8,4,2 to A8,4,9 for laying pipes through uPVC pipes Class 34 solid wall (heavy duty) pipe sleeves at road crossings"]
[]
[967,"A8.4.33",null,"50mm diam,","m",{"v":20,"d":"20.00"}]
[]
[969,"A8.4.34",null,"75mm diam,","m",{"v":100,"d":"100.00"}]
[]
[971,"A8.4.35",null,"110mm diam,","m",{"v":200,"d":"200.00"}]
[]
[973,"A8.4.36",null,"160mm diam,","m",{"v":250,"d":"250.00"}]
[]
[975,"A8.4.37",null,"200mm diam,","m",{"v":25,"d":"25.00"}]
[]
[977,"A8.4.38",null,"250mm diam,","m",{"v":25,"d":"25.00"}]
[]
[979,"A8.4.39",null,"315mm diam,","m",{"v":25,"d":"25.00"}]
[]
[981,"A8.4.40",null,"355mm diam,","m",{"v":25,"d":"25.00"}]
[]
[983,"A8.4.41","PSL 8,2,22","Pressure testing and disinfection of existing pipe (in-situ)","m",{"v":3000,"d":"3000.00"}]
[]
[985,null,"PSL 8,2,23","CCTV inspection of pipes"]
[]
[987,"A8.4.42",null,"300 mm up to 450 mm diam,","m",{"v":2000,"d":"2000.00"}]
[]
[989,"A8.4.43",null,"450 mm up to 900 mm diam,","m",{"v":500,"d":"500.00"}]
[]
[993,null,null,"BENDS AND FITTINGS"]
[]
[995,null,"8.2.2","90 deg mPVC Bend (Class 16) as per eThekwini Municipality Water Design branch Plan No. 69"]
[]
[997,"A8.4.44",null,"75 mm diam, ","No.",{"v":35,"d":"35.00"}]
[]
[999,"A8.4.45",null,"110 mm diam, ","No.",{"v":52,"d":"52.00"}]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[1001,"A8.4.46",null,"160 mm diam, ","No.",{"v":11,"d":"11.00"}]
[]
[1003,"A8.4.47",null,"200 mm diam,","No.",{"v":2,"d":"2.00"}]
[]
[1005,null,"8,2,2","45 deg mPVC Bend (Class 16) as per eThekwini Municipality Water Design branch Plan No, 68"]
[]
[]
[1007,"A8.4.48",null,"75 mm diam, ","No.",{"v":28,"d":"28.00"}]
[]
[1009,"A8.4.49",null,"110 mm diam, ","No.",{"v":76,"d":"76.00"}]
[]
[1011,"A8.4.50",null,"160 mm diam, ","No.",{"v":36,"d":"36.00"}]
[]
[1013,"A8.4.51",null,"200 mm diam, ","No.",{"v":2,"d":"2.00"}]
[]
[1015,null,"8,2,2","22,5 deg mPVC Bend (Class 16) as per eThekwini Municipality Water Design branch Plan No, 67"]
[]
[1017,"A8.4.52",null,"75 mm diam, ","No.",{"v":65,"d":"65.00"}]
[]
[1019,"A8.4.53",null,"110 mm diam, ","No.",{"v":90,"d":"90.00"}]
[]
[1021,"A8.4.54",null,"160 mm diam, ","No.",{"v":48,"d":"48.00"}]
[]
[1023,"A8.4.55",null,"200 mm diam, ","No.",{"v":2,"d":"2.00"}]
[]
[1025,null,"8,2,2","11,25 deg mPVC Bend (Class 16)"]
[]
[1027,"A8.4.56",null,"75 mm diam, ","No.",{"v":20,"d":"20.00"}]
[]
[1029,"A8.4.57",null,"110 mm diam, ","No.",{"v":50,"d":"50.00"}]
[]
[1031,"A8.4.58",null,"160 mm diam, ","No.",{"v":30,"d":"30.00"}]
[]
[1033,"A8.4.59",null,"200 mm diam, ","No.",{"v":2,"d":"2.00"}]
[]
[1035,null,"8,2,2","90 degree \"AQUALOCK\" socketed bend as per eThekwini Municipality Water Design branch Plan No, 72"]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[1037,"A8.4.60",null,"250 mm diam, ","No.",{"v":2,"d":"2.00"}]
[]
[1039,null,"8,2,2","45 degree \"AQUALOCK\" socketed bend as per eThekwini Municipality Water Design branch Plan No, 71"]
[1041,"A8.4.61",null,"250 mm diam, ","No.",{"v":4,"d":"4.00"}]
[]
[1043,null,"8,2,2","22,5 degree \"AQUALOCK\" socketed bend as per eThekwini Municipality Water Design branch Plan No, 70"]
[]
[1045,"A8.4.62",null,"250 mm diam, ","No.",{"v":3,"d":"3.00"}]
[]
[1047,null,"8,2,2","11,25 degree \"AQUALOCK\" socketed bend as per eThekwini Municipality Water Design branch Plan No, 70"]
[]
[1049,"A8.4.63",null,"250 mm diam, ","No.",{"v":5,"d":"5.00"}]
[]
[1051,"A8.4.64",null,"315 mm diam, ","No.",{"v":1,"d":"1.00"}]
[]
[1053,null,"8,2,2","STEEL FLANGED EQUAL TEE as per eThekwini Municipality Water Design branch Plan No, 73 Rev A"]
[]
[1055,"A8.4.65",null,"80 mm diam,","No.",{"v":22,"d":"22.00"}]
[]
[1057,"A8.4.66",null,"100 mm diam, ","No.",{"v":118,"d":"118.00"}]
[]
[1059,"A8.4.67",null,"150 mm diam,","No.",{"v":58,"d":"58.00"}]
[]
[1061,"A8.4.68",null,"200 mm diam,","No.",{"v":2,"d":"2.00"}]
[]
[1063,"A8.4.69",null,"250 mm diam,","No.",{"v":2,"d":"2.00"}]
[]
[1065,"A8.4.70",null,"300mm diam","No.",{"v":2,"d":"2.00"}]
[]
[1067,"A8.4.71",null,"400mm diam","No.",{"v":1,"d":"1.00"}]
[]
[1069,null,"8,2,2","90 degree HDPE compression BEND (PN16)"]
[]
[1071,"A8.4.72",null,"25 mm","No.",{"v":10,"d":"10.00"}]
[]
[1073,"A8.4.73",null,"50 mm","No.",{"v":75,"d":"75.00"}]
[]
[1075,"A8.4.74",null,"110 mm","No.",{"v":5,"d":"5.00"}]
[]
[1077,null,"8,2,2","Ductile Iron socketed/flanged TEE (for Hydrants)"]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[1079,"A8.4.75",null,"80mm (socketed) x 80mm (socketed) x 80mm (flanged)","No.",{"v":20,"d":"20.00"}]
[]
[1081,"A8.4.76",null,"110 mm (socketed) x 110 mm (socketed) x 80mm (flanged) ","No.",{"v":30,"d":"30.00"}]
[]
[1083,"A8.4.77",null,"160 mm (socketed) x 160 mm (socketed) x 80mm (flanged) ","No.",{"v":20,"d":"20.00"}]
[]
[1085,"A8.4.78",null,"200 mm (socketed) x 200 mm (socketed) x 80mm (flanged) ","No.",{"v":4,"d":"4.00"}]
[]
[1087,"A8.4.79",null,"250 mm (socketed) x 250 mm (socketed) x 80mm (flanged) ","No.",{"v":4,"d":"4.00"}]
[]
[1089,"A8.4.80",null,"315 mm (socketed) x 315 mm (socketed) x 80mm (flanged) ","No.",{"v":1,"d":"1.00"}]
[]
[1091,null,"8,2,2","STEEL TAPER FLANGED as per eThekwini municipality water design branch plan No, 80"]
[]
[1093,"A8.4.81",null,"80/50mm","No.",{"v":215,"d":"215.00"}]
[]
[1095,"A8.4.82",null,"100/80mm","No.",{"v":25,"d":"25.00"}]
[]
[1097,"A8.4.83",null,"150/80mm","No.",{"v":10,"d":"10.00"}]
[]
[1099,"A8.4.84",null,"150/100 mm","No.",{"v":10,"d":"10.00"}]
[]
[1101,"A8.4.85",null,"200/80 mm","No.",{"v":1,"d":"1.00"}]
[]
[1103,"A8.4.86",null,"200/100 mm","No.",{"v":1,"d":"1.00"}]
[]
[1105,"A8.4.87",null,"200/150 mm","No.",{"v":1,"d":"1.00"}]
[]
[1107,"A8.4.88",null,"250/80 mm","No.",{"v":1,"d":"1.00"}]
[]
[1109,"A8.4.89",null,"250/100 mm","No.",{"v":1,"d":"1.00"}]
[]
[1111,"A8.4.90",null,"250/150 mm","No.",{"v":2,"d":"2.00"}]
[]
[1113,"A8.4.91",null,"250/200 mm","No.",{"v":1,"d":"1.00"}]
[]
[1115,"A8.4.92",null,"300/80 mm","No.",{"v":1,"d":"1.00"}]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[1117,"A8.4.93",null,"300/100 mm","No.",{"v":5,"d":"5.00"}]
[]
[1119,"A8.4.94",null,"300/150 mm","No.",{"v":2,"d":"2.00"}]
[]
[1121,"A8.4.95",null,"300/200 mm","No.",{"v":1,"d":"1.00"}]
[]
[1123,"A8.4.96",null,"300/250 mm","No.",{"v":1,"d":"1.00"}]
[]
[1125,"A8.4.97",null,"400/80 mm","No.",{"v":1,"d":"1.00"}]
[]
[1127,"A8.4.98",null,"400/100 mm","No.",{"v":1,"d":"1.00"}]
[]
[1129,"A8.4.99",null,"400/150 mm","No.",{"v":1,"d":"1.00"}]
[]
[1131,null,"8,2,2","END CAP as per eThekwini municipality water design branch plan No, 74"]
[]
[1133,"A8.4.100",null,"50 mm diam, ","No.",{"v":75,"d":"75.00"}]
[]
[1135,"A8.4.101",null,"75 mm diam, ","No.",{"v":15,"d":"15.00"}]
[]
[1137,"A8.4.102",null,"110 mm diam,","No.",{"v":5,"d":"5.00"}]
[]
[1139,"A8.4.103",null,"160 mm diam,","No.",{"v":5,"d":"5.00"}]
[]
[1141,"A8.4.104",null,"200 mm diam,","No.",{"v":1,"d":"1.00"}]
[]
[1143,"A8.4.105",null,"250 mm diam,","No.",{"v":1,"d":"1.00"}]
[]
[1145,"A8.4.106",null,"315 mm diam,","No.",{"v":1,"d":"1.00"}]
[]
[1147,null,"8,2,2","FLANGE ADAPTOR as per eThekwini municipality water design branch plan No, 77"]
[]
[1149,"A8.4.107",null,"75 mm diam, ","No.",{"v":450,"d":"450.00"}]
[]
[1151,"A8.4.108",null,"110 mm diam,","No.",{"v":270,"d":"270.00"}]
[]
[1153,"A8.4.109",null,"160 mm diam,","No.",{"v":156,"d":"156.00"}]
[]
[1155,"A8.4.110",null,"200 mm diam,","No.",{"v":1,"d":"1.00"}]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[1157,"A8.4.111",null,"250 mm diam,","No.",{"v":1,"d":"1.00"}]
[]
[1159,"A8.4.112",null,"315 mm diam,","No.",{"v":42,"d":"42.00"}]
[]
[1161,null,"8,2,2","UNIVERSAL FLANGE ADAPTOR as per eThekwini municipality Water Design Branch Plan No, 78 Rev B"]
[]
[1163,"A8.4.113",null,"75 mm diam, ","No.",{"v":25,"d":"25.00"}]
[]
[1165,"A8.4.114",null,"110 mm diam,","No.",{"v":10,"d":"10.00"}]
[]
[1167,"A8.4.115",null,"160 mm diam,","No.",{"v":5,"d":"5.00"}]
[]
[1169,"A8.4.116",null,"200 mm diam,","No.",{"v":5,"d":"5.00"}]
[]
[1171,"A8.4.117",null,"250 mm diam,","No.",{"v":4,"d":"4.00"}]
[]
[1173,"A8.4.118",null,"315 mm diam,","No.",{"v":2,"d":"2.00"}]
[]
[1175,null,"8.2.2","UNIVERSAL COUPLING as per eThekwini municipality Water Design Branch Plan No. 81 Rev A"]
[]
[1177,"A8.4.119",null,"75 mm diam, ","No.",{"v":10,"d":"10.00"}]
[]
[1179,"A8.4.120",null,"110 mm diam,","No.",{"v":2,"d":"2.00"}]
[]
[1181,"A8.4.121",null,"160 mm diam,","No.",{"v":2,"d":"2.00"}]
[]
[1183,"A8.4.122",null,"200 mm diam,","No.",{"v":2,"d":"2.00"}]
[]
[1185,"A8.4.123",null,"250 mm diam,","No.",{"v":2,"d":"2.00"}]
[]
[1187,"A8.4.124",null,"315 mm diam,","No.",{"v":4,"d":"4.00"}]
[]
[1189,null,"8,2,2","\"AQUALOK\" STEPFIT COUPLING, including saddle, as per eThekwini municipality Water Design Branch Plan No, 79 Rev A"]
[]
[1191,"A8.4.125",null,"200-232 mm diam, (mPVC to AC)","No.",{"v":4,"d":"4.00"}]
[]
[1193,"A8.4.126",null,"250-286 mm diam, (mPVC to AC)","No.",{"v":4,"d":"4.00"}]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[1195,"A8.4.127",null,"315-345 mm diam, (mPVC to AC) including 315 x 100 mm saddle","No.",{"v":4,"d":"4.00"}]
[]
[1197,null,"PSL 8,2,21","RECOVERED FITTINGS FROM CLEARING OPERATION"]
[]
[1199,"A8.4.128",null,"All diameters and types","No.",{"v":453,"d":"453.00"}]
[]
[1201,null,"8.2.3","Supplying, Laying, bedding and installation of Valves"]
[]
[1203,null,null,"Flanged Gate valves as per EWS Technical specification - PART B"]
[]
[1205,"A8.4.129",null,"300 mm diam,","No.",{"v":4,"d":"4.00"}]
[]
[1207,"A8.4.130",null,"400 mm diam,","No.",{"v":4,"d":"4.00"}]
[]
[1209,null,null,"Flanged RSV valves as per EWS Technical specification - PART B"]
[]
[1211,"A8.4.131",null,"50mm diam,","No.",{"v":31,"d":"31.00"}]
[]
[1213,"A8.4.132",null,"80 mm diam, ","No.",{"v":10,"d":"10.00"}]
[]
[1215,"A8.4.133",null,"100 mm diam,","No.",{"v":47,"d":"47.00"}]
[]
[1217,"A8.4.134",null,"150 mm diam,","No.",{"v":16,"d":"16.00"}]
[]
[1219,"A8.4.135",null,"200 mm diam,","No.",{"v":1,"d":"1.00"}]
[]
[1221,"A8.4.136",null,"250 mm diam,","No.",{"v":1,"d":"1.00"}]
[]
[1223,"A8.4.137",null,"315 mm diam,","No.",{"v":4,"d":"4.00"}]
[]
[1225,null,"PSL 8,2,","AIR VALVES,Standard eThekwini Water & Sanitation Drawing No 40306, Sheet 2"]
[]
[1227,"A8.4.138",null,"75mm diam","No.",{"v":25,"d":"25.00"}]
[]
[1229,null,"PSL 8,2,21","RECOVERED VALVES FROM CLEARING OPERATION"]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[1231,"A8.4.139",null,"All diameters and types","No.",{"v":250,"d":"250.00"}]
[]
[1233,null,null,"TEMPORARY CONNECTION"]
[]
[1235,null,"PSL 8.2.19","Temporary house and property water connections, including supply, commissioning, maintenance, design of rider main, connection to existing mains and removal on completion of customer connection. "]
[]
[1237,"A8.4.140",null,"25 mm dia,","No.",{"v":982,"d":"982.00"}]
[]
[1239,"A8.4.141",null,"50 mm dia,","No.",{"v":80,"d":"80.00"}]
[]
[1241,"A8.4.142",null,"80 mm dia,","No.",{"v":20,"d":"20.00"}]
[]
[1243,"A8.4.143",null,"100 mm dia,","No.",{"v":10,"d":"10.00"}]
[]
[1245,null,null,"PERMANENT CONNECTIONS"]
[]
[1247,null,"PSL 8,2,20","House Connection, complete with saddle (Plan 75 REV A), ball valve and pipework inclusive of 5m HDPE (SDR 11, PE 100, PN 16) pipe of size 25mm or 50mm to match connection size"]
[]
[1249,"A8.4.144",null,"25 mm dia, (Plan 56 B of the eThekwini Design Branch)","No.",{"v":982,"d":"982.00"}]
[]
[1251,"A8.4.145",null,"50 mm dia, (Plan 56C of the eThekwini Design Branch)","No.",{"v":80,"d":"80.00"}]
[]
[1253,"A8.4.146",null,"Extra-over item A8,4,131 to A8,4,132 to re-locate existing house connection to position as instructed by the Engineer,","No.",{"v":20,"d":"20.00"}]
[]
[1255,"A8.4.147",null,"Extra-over item A8,4,131  includes removal of existing saddle, supply, install and test new saddle over existing ferrule and blanking off","No.",{"v":10,"d":"10.00"}]
[]
[1257,"A8.4.148",null,"Extra-over item A8,4,132  includes removal of existing saddle, supply, install and test new saddle over existing ferrule and blanking off","No.",{"v":10,"d":"10.00"}]
[]
[1259,null,"PSL 8.2.1","Supply, lay and bed steel pipes (flanged) for consumer meter connections (Refer to EWS standard drawing 72056) "]
[]
[1261,"A8.4.149",null,"50 mm dia,","m",{"v":25,"d":"25.00"}]
[]
[1263,"A8.4.150",null,"80mm  dia,","m",{"v":25,"d":"25.00"}]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[1265,"A8.4.151",null,"100mm dia","m",{"v":25,"d":"25.00"}]
[]
[1267,"A8.4.152",null,"150mm dia","m",{"v":25,"d":"25.00"}]
[]
[1269,null,"8,2,2","HDPE COMPRESSION COUPLING (PN 16)"]
[]
[1271,"A8.4.153",null,"25 mm","No.",{"v":982,"d":"982.00"}]
[]
[1273,"A8.4.154",null,"50 mm","No.",{"v":80,"d":"80.00"}]
[]
[1275,"A8.4.155",null,"90 mm","No.",{"v":5,"d":"5.00"}]
[]
[1277,null,"8,2,2","HDPE COMPRESSION T- PIECE (PN 16)"]
[]
[1279,"A8.4.156",null,"50 mm","No.",{"v":20,"d":"20.00"}]
[]
[1281,"A8.4.157",null,"110 mm","No.",{"v":4,"d":"4.00"}]
[]
[1283,"A8.4.158","PSL 8,2,16","Extra over for cutting of pipe","No.",{"v":500,"d":"500.00"}]
[]
[1285,null,"8,2,2","Supply, handle and install 90 deg steel BEND (flanged) for consumer meter connections (Refer to EWS standard drawing 72056): "]
[]
[1287,"A8.4.159",null,"50 mm dia,","No.",{"v":1500,"d":"1500.00"}]
[]
[1289,"A8.4.160",null,"80 mm dia,","No.",{"v":255,"d":"255.00"}]
[]
[1291,"A8.4.161",null,"100 mm dia,","No.",{"v":0,"d":"0.00"}]
[]
[1293,"A8.4.162",null,"150 mm dia,","No.",{"v":0,"d":"0.00"}]
[]
[1295,null,"PSL 8,2,17","Connecting to Existing Pipeline"]
[]
[1297,"A8.4.163",null,"75 mm diam, ","No.",{"v":2,"d":"2.00"}]
[]
[1299,"A8.4.164",null,"110 mm diam, ","No.",{"v":5,"d":"5.00"}]
[]
[1301,"A8.4.165",null,"160 mm diam, ","No.",{"v":5,"d":"5.00"}]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[1303,"A8.4.166",null,"200 mm diam, ","No.",{"v":3,"d":"3.00"}]
[]
[1305,"A8.4.167",null,"250 mm diam, ","No.",{"v":2,"d":"2.00"}]
[]
[1307,"A8.4.168",null,"315 mm diam,","No.",{"v":1,"d":"1.00"}]
[]
[1309,"A8.4.169",null,"355mm diam,","No.",{"v":1,"d":"1.00"}]
[]
[1311,"A8.4.170",null,"400mm diam,","No.","0.00"]
[]
[1313,null,null,"FIRE HYDRANTS"]
[]
[1315,"A8.4.171",null,"Supply and install Standard Hydrant as per eThekwini Water Design Branch Plan No, 26B including 100mm dia, gate valve with valve cover, spacer rings, 110mm dia, ''Plasson''  flange adaptors, 110mm dia, ''Plasson'' 90deg elbow, 110mm dia, HDPE pipe, concrete anchor blocks (T-piece measured elsewhere),","No.",{"v":61,"d":"61.00"}]
[]
[1317,"A8.4.172",null,"Supply and install Double Standard Hydrant as per eThekwini Water Design Branch Plan No, 20B including 100mm dia, gate valves with valve covers, spacer rings, 110mm dia, ''Plasson''  flange adaptors, 110mm dia, ''Plasson'' 90deg elbow, 110mm dia, HDPE pipe, concrete anchor blocks,","No.",{"v":5,"d":"5.00"}]
[]
[1319,"A8.4.173","PSL 8,2,11","ANCHOR/THRUST BLOCKS AND PEDESTALS as per eThekwini municipality Water Design Branch Plan No, 39 (Grade 20/19), Final thrust block dimensions to be confirmed on site with the Engineer,","No.",{"v":455,"d":"455.00"}]
[]
[1321,null,"8,2,13","VALVE CHAMBERS AND MANHOLES:"]
[]
[1322]
[]
[1323,"A8.4.174",null,"Air valve chamber as per eThekwini municipality Water Design Branch Drawing No, 40306","No.",{"v":8,"d":"8.00"}]
[]
[1325,"A8.4.175",null,"Pressure Reducing Valve Chamber as per eThekwini municipality Water Design Branch Drawing No, 43718 & 43719","No.","2.00"]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[]
[1327,"A8.4.176",null,"Valve chamber constructed from precast concrete valve spacer rings ( eThekwini municipality Water Design Branch, Plan No, 6) complete with Valve Cap ( eThekwini municipality Water Design Branch, Plan Number 28, Valve Cover 5B),","No.",{"v":145,"d":"145.00"}]
[]
[1329,null,null,"MARKER BLOCKS"]
[]
[1331,"A8.4.177",null,"Valve Marker as per eThekwini water and Sanitation Plan No, 27","No.",{"v":212,"d":"212.00"}]
[]
[1333,null,"PSL 8,2,15","CORROSION PROTECTION for Buried Fittings or valves (DENSO or similar approved)"]
[]
[1335,null,"PSL 8,2,15","Flanged Joints for diameters:"]
[]
[1337,"A8.4.178",null,"80 mm diam, ","No.",{"v":220,"d":"220.00"}]
[]
[1339,"A8.4.179",null,"100 mm diam,","No.",{"v":260,"d":"260.00"}]
[]
[1341,"A8.4.180",null,"150 mm diam,","No.",{"v":110,"d":"110.00"}]
[]
[1343,"A8.4.181",null,"200 mm diam,","No.",{"v":60,"d":"60.00"}]
[]
[1345,"A8.4.182",null,"250 mm diam,","No.",{"v":20,"d":"20.00"}]
[]
[1347,"A8.4.183",null,"300  mm diam,","No.",{"v":10,"d":"10.00"}]
[]
[1349,"A8.4.184",null,"400 mm diam,","No.",{"v":1,"d":"1.00"}]
[]
[null," Total Carried Forward To Summary"]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[]
[1351,"A9.4","COD PART S","SECTION : REINSTATEMENT"]
[]
[1353,null,"S.8.2","Roads and Hardened Areas"]
[]
[1355,"A9,4,1",null,"Temporary Reinstatement of Road","m²",{"v":18850,"d":"18850.00"}]
[]
[1357,null,null,"Permanent Reinstatement of Road for (including additional compaction of backfill as specified): "]
[]
[1359,"A9,4,2",null,"Road Category A","m²",{"v":100,"d":"100.00"}]
[]
[1361,"A9,4,3",null,"Road Category B","m²",{"v":2500,"d":"2500.00"}]
[]
[1363,"A9,4,4",null,"Road Category C","m²",{"v":5000,"d":"5000.00"}]
[]
[1365,"A9,4,5",null,"Road Category D","m²",{"v":13350,"d":"13350.00"}]
[]
[1367,null,null,"Permanent Reinstatement of Side walks, Footpaths and Median Areas complying to Part EG of City of Durban Standard Engineering Specification:"]
[]
[1369,"A9,4,6",null,"Reinstatement of paved side walks (Pre-cast Concrete slabs) ","m²",{"v":20,"d":"20.00"}]
[]
[1371,"A9,4,7",null,"Reinstatement of paved side walks (Brick paving blocks) ","m²",{"v":500,"d":"500.00"}]
[]
[1373,"A9,4,8",null,"Reinstatement of paved side walks (Asphalt) ","m³",{"v":950,"d":"950.00"}]
[]
[1375,"A9,4,9",null,"Reinstatement of Asphalt Access Hardening and Scoops for property entrances/accesses","m²",{"v":1500,"d":"1500.00"}]
[]
[1377,"A9,4,10",null,"Reinstatement of Concrete Access Hardening and Scoops property entrances/accesses ","m²",{"v":750,"d":"750.00"}]
[]
[1379,null,"S.8.3","Kerbing and Haunching"]
[]
[1381,"A9,4,11",null,"Type A Barrier Kerb and Channel, complete as per eThekwini Standard drawing 38577","m",{"v":15,"d":"15.00"}]
[]
[1383,"A9,4,12",null,"Type B Barrier Kerb and Channel, complete as per eThekwini Standard drawing 38577","m",{"v":15,"d":"15.00"}]
[]
[1385,"A9,4,13",null,"Type C Mountable Kerb and Channel, complete as per eThekwini Standard drawing 38577","m",{"v":15,"d":"15.00"}]
[]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[1387,"A9,4,14",null,"Type D Barrier Kerb and Channel, complete as per eThekwini Standard drawing 38577","m",{"v":5650,"d":"5650.00"}]
[]
[1389,"A9,4,15",null,"Type E Semi Mountable Kerb and Channel, complete as per eThekwini Standard drawing 38577","m",{"v":3560,"d":"3560.00"}]
[]
[1391,"A9,4,16",null,"Type F Mountable Kerb and Fillet, complete as per eThekwini Standard drawing 38577","m",{"v":9620,"d":"9620.00"}]
[]
[1393,"A9,4,17",null,"Type G Extruded Barrier Kerb and Channel, complete as per eThekwini Standard drawing 38577","m",{"v":400,"d":"400.00"}]
[]
[1395,"A9,4,18",null,"Type H Extruded Mountable Kerb and Channel, complete as per eThekwini Standard drawing 38577","m",{"v":60,"d":"60.00"}]
[]
[1397,null,"\"SANS 1200 MM\"","SECTION: ROAD MARKINGS"]
[]
[1399,null,"8.4.1","Road Markings (5.3)"]
[]
[1401,null,null,"a) White lines "]
[]
[1403,"A9,4,19",null,"i) 100 mm wide, broken","m",{"v":2000,"d":"2000.00"}]
[]
[1405,"A9,4,20",null,"ii) 200 mm wide, broken","m",{"v":2750,"d":"2750.00"}]
[1406]
[]
[1407,"A9,4,21",null,"iii)150 mm wide, continuous","m",{"v":3500,"d":"3500.00"}]
[]
[1409,"A9,4,22",null,"iv) 200 mm wide, continuous","m",{"v":500,"d":"500.00"}]
[]
[1411,null,null,"b) Yellow lines"]
[]
[1413,"A9,4,23",null,"i) 100 mm wide, continuous","m",{"v":1000,"d":"1000.00"}]
[]
[1415,"A9,4,24",null,"ii) 150 mm wide, continuous","m",{"v":500,"d":"500.00"}]
[]
[1417,null,null,"c) Red  lines"]
[]
[1419,"A9,4,25",null,"i) 100 mm wide, continuous","m",{"v":200,"d":"200.00"}]
[]
[1421,"A9,4,26",null,"ii) 150 mm wide, continuous","m",{"v":200,"d":"200.00"}]
[]
[1423,null,null,"d) Symbols or characters"]
[null,"`"]
[null," Total Carried Forward "]
[null,"ITEM\nNO","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT R"]
[null," Brought Forward"]
[1425,"A9,4,27",null,"i) White symbols or characters","m²",{"v":200,"d":"200.00"}]
[]
[1427,"A9,4,28",null,"ii) Yellow symbols or characters","m²",{"v":200,"d":"200.00"}]
[]
[1429,null,"8,4,2","Variation in Rate of Application"]
[]
[1431,"A9,4,29",null,"White paint","ℓ",{"v":250,"d":"250.00"}]
[]
[1433,"A9,4,30",null,"Yellow paint","ℓ",{"v":100,"d":"100.00"}]
[]
[1435,"A9,4,31",null,"Red paint","ℓ",{"v":25,"d":"25.00"}]
[]
[1437,"A9,4,32",null,"Glass beads","kg",{"v":55,"d":"55.00"}]
[]
[null," Total Carried Forward To Summary"]
[{"$nulls":3},"SUMMARY OF SECTIONS"]
[null," ","SECTION","DESCRIPTION",{"$nulls":3},"AMOUNT R"]
[null,null,"A0","Preliminary And General"]
[]
[null,null,"A1","Sums Stated Provisionally"]
[]
[null,null,"A2","Traffic Accommodation"]
[]
[null,null,"A3.4","Dayworks"]
[]
[null,null,"A4.4","Site Clearance"]
[]
[null,null,"A5.4","Pipe Trenches"]
[]
[null,null,"A6.4","HDD And Trenchless Technology"]
[]
[null,null,"A7.4","Bedding & Sub-Soil Drains"]
[]
[null,null,"A8.4","Water Mains"]
[]
[null,null,"A9.4","Reinstatement Of Road Reserve"]
[]
[{"$nulls":3},"   SUBTOTAL"]
[]
[{"$nulls":3},"Add 15% VAT"]
[null,null," Total Carried Forward To Summary Of Schedules"]
{"$rows_empty":43}
[{"$nulls":3},"42"]

{"sheet":"Sheet1","index":1,"n_rows":52,"n_cols":8,"rows_kept":52,"merged":[[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,0,7],[51,0,51,5]]}
["ITEM","PAYMENT","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["NO",{"$nulls":5},"R","c"]
["A1",null,"PRELIMINARY & GENERAL "]
[]
["A1.1",8.3,"FIXED-CHARGE ITEMS"]
[]
["A1.1.1","8.3.1","Contractual Requirements","Sum",1]
[]
[null,"8.3.2","Establish Facilities on the Site :"]
[]
[null,"8.3.2.1 ","a) Facilities for Engineer"]
[]
["A1.1.2","PSA 4.3","Furnished Office (1 No.)","Sum",1]
[]
["A1.1.3",null,"Name boards as per eThekwini Municipality WDNRW Branch plan No. 9","No.",2]
[]
[null,"8.3.2.2","b) Facilities for Contractor"]
[]
["A1.1.4",null,"Offices and storage sheds","Sum",1]
[]
["A1.1.5",null,"Workshops","Sum",1]
[]
["A1.1.6",null,"Ablution and latrine facilities","Sum",1]
[]
["A1.1.7",null,"Tools and equipment","Sum",1]
[]
["A1.1.8",null,"Water supplies, electric power and communications","Sum",1]
[]
["A1.1.9",null,"Dealing with water (Sub-clause 5.5)","Sum",1]
[]
["A1.1.10",null,"Access (Sub-clause 5.8)","Sum",1]
[]
["A1.1.11","PSA 8.9","Security (unarmed) on site for the duration of the contract ","Sum",1]
[]
["A1.1.12","PSA 8.10","Security (armed) on site for the duration of the contract","Sum",1]
[]
["A1.1.13","PSA 8.11","Daily photographing of Works and Traffic Accommodation, including record keeping.","Sum",1]
[]
["A1.1.14","PSA 8.12","Provision of \"As-Built\" information by professional surveyor","Sum",1]
[]
["A1.1.15","8.3.3","Other fixed-charge obligations","Sum",1]
[]
["A1.1.16","8.3.4","Remove Engineer's and Contractor's Site establishment on completion","Sum",1]
{"$rows_empty":8}
[" Total Carried Forward"]