{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["Dell Requirements ","Dell Summary","VMware","HP Requirement"],"read":"whole","date_system":"1900"}

{"sheet":"Dell Requirements ","index":0,"n_rows":78,"n_cols":4,"rows_kept":78,"merged":[[39,0,39,2],[40,0,40,2],[41,0,41,2],[42,0,42,2],[46,0,46,2],[57,0,57,2],[58,0,58,2],[59,0,59,2],[60,0,60,2],[62,0,62,2],[63,0,63,2],[64,0,64,2],[65,0,65,2],[66,0,66,2],[67,0,67,2],[72,0,77,0],[72,1,77,1],[72,3,77,3]]}
[null,"Production","High Availability","DR "]
["Sites","AZ1","AZ2","DR (CPT)"]
["Management Clusters","4 x VxRail E660F","4 x VxRail E660F","4 x VxRail E660F"]
[null," 2 x Intel® Xeon® Gold 5320 2.2G, 26C CPUs"," 2 x Intel® Xeon® Gold 5320 2.2G, 26C CPUs"," 2 x Intel® Xeon® Gold 5320 2.2G, 26C CPUs"]
[null,"16 x 32GB RDIMM, Memory","16 x 32GB RDIMM, Memory","16 x 32GB RDIMM, Memory"]
[null,"5 x 3.84TB SSD SATA Read Intensive 6Gbps SSDs","5 x 3.84TB SSD SATA Read Intensive 6Gbps SSDs","5 x 3.84TB SSD SATA Read Intensive 6Gbps SSDs"]
[null,"Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0"]
[null,"ProdePloy Plus Services","ProdePloy Plus Services","ProdePloy Plus Services"]
[null,"5 Yrs Prosupport Plus Services","5 Yrs Prosupport Plus Services","5Yrs Prosupport Plus Services"]
[null,"VxRail VMware, vSAN Enterprise, 5 Years","VxRail VMware, vSAN Enterprise, 5 Years","VxRail VMware, vSAN Enterprise, 5 Years"]
[]
["Production Cluster ","5 x VxRail P670F","5 x VxRail P670F","5 x VxRail P670F"]
[null," 2 x Intel® Xeon® Platinum 8358 2.6G, 32C CPUs"," 2 x Intel® Xeon® Platinum 8358 2.6G, 32C CPUs"," 2 x Intel® Xeon® Platinum 8358 2.6G, 32C CPUs"]
[null,"16 x 32GB RDIMM, Memory","16 x 32GB RDIMM, Memory","16 x 32GB RDIMM, Memory"]
[null,"16 x 64GB RDIMM, Memory","16 x 64GB RDIMM, Memory","16 x 64GB RDIMM, Memory"]
[null,"Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0"]
[null,"Emulex LPE 35002 Dual Port 32Gb Fibre Channel HBA, PCIe Low Profile","Emulex LPE 35002 Dual Port 32Gb Fibre Channel HBA, PCIe Low Profile","Emulex LPE 35002 Dual Port 32Gb Fibre Channel HBA, PCIe Low Profile"]
[null,"ProdePloy Plus Services","ProdePloy Plus Services","ProdePloy Plus Services"]
[null,"5 Yrs Prosupport Plus Services","5 Yrs Prosupport Plus Services","5 YrsProsupport Plus Services"]
[]
["Storage ","Dell Powerstore 1200T","Dell Powerstore 1200T","Dell Powerstore 1200T"]
[null,"384GB Appliance DIMM 192GB Per Node","384GB Appliance DIMM 192GB Per Node","384GB Appliance DIMM 192GB Per Node"]
[null,"25GBE OPTICAL 4 PORT CARD PAIR","25GBE OPTICAL 4 PORT CARD PAIR","25GBE OPTICAL 4 PORT CARD PAIR"]
[null,"14 x 25X2.5 NVME SED SSD 15.36TB ","14 x 25X2.5 NVME SED SSD 15.36TB ","14 x 25X2.5 NVME SED SSD 15.36TB "]
[null,"3M PASSIVE 25G TWINAX CABLE QTY 2","3M PASSIVE 25G TWINAX CABLE QTY 2","3M PASSIVE 25G TWINAX CABLE QTY 2"]
[null,"32GB FC 4 PORT IO MODULE PAIR","32GB FC 4 PORT IO MODULE PAIR","32GB FC 4 PORT IO MODULE PAIR"]
[null,"ProDeploy Plus for PowerStore 1xxx T","ProDeploy Plus for PowerStore 1xxx T","ProDeploy Plus for PowerStore 1xxx T"]
[null,"ProDeploy Plus Add-On for PowerStore Remote Replication","ProDeploy Plus Add-On for PowerStore Remote Replication","ProDeploy Plus Add-On for PowerStore Remote Replication"]
[null,"ProDeploy Plus Add-On for PowerStore Local Replication","ProDeploy Plus Add-On for PowerStore Local Replication","ProDeploy Plus Add-On for PowerStore Local Replication"]
[null,"Data Migration Services: Remote Virtual V2V Migration 101 Plus VMs","Data Migration Services: Remote Virtual V2V Migration 101 Plus VMs","Data Migration Services: Remote Virtual V2V Migration 101 Plus VMs"]
[null,"5 Yrs ProSupport Plus and 4Hr Mission Critical ","5 Yrs ProSupport Plus and 4Hr Mission Critical ","5 Yrs ProSupport Plus and 4Hr Mission Critical "]
[]
[]
["IP Networking Switches","2 x S5248F","2 x S5248F","2 x S5248F"]
["SAN Switches","2 x DS6620","2 x DS6620 ","2 x DS6620"]
["Mgmt Switches","1 x S3048","1 x S3048","1 x S3048"]
["Rack","1 x 42U Dell NetShelter Rack","1 x 42U Dell NetShelter Rack","1 x 42U Dell NetShelter Rack"]
["Rack PDUs","2 x Rack PDU 32A, 230V, (36) C13 & (6) C19 ","2 x Rack PDU 32A, 230V, (36) C13 & (6) C19 ","2 x Rack PDU 32A, 230V, (36) C13 & (6) C19 "]
[]
["Physical Servers"]
[]
["Domain Controllers - 3  x PowerEdge R660xs"]
["Metro -Witness Server - 1 x PowerEdge R450 Server"]
[]
[]
[]
["Dell Software (Transactional License Agreement )"]
["Quantity","License Model","Licensed SW"]
[5,"147-BCVE","PowerStore 1200 Base License TLA=IC "]
[742,"147-BBKO","PowerStore Capacity SW TLA=CB "]
[35,"147-BCSW","VxRail HCI15G AF/Hybrid ProcrGold TLA=IG "]
[44,"147-BCTG","VxRail 15G DynNode Processor Plat TLA=IG "]
[70,"147-BCTM","VxRail HCI Sys SW (CAP3.84 SATA)TLA=CF "]
[633,"147-BCSY","VxRail HCI Sys Memory 32GB TLA=CG "]
[352,"147-BCSP","VxRail HCI Sys Memory 64GB TLA=CG "]
[]
[]
["Year1 Professional Services"]
["5yrs - Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price"]
["Deployment of VCF Components & SRM (Once Off)                                   "]
[]
[]
["Year2 to Year 5 Services"]
["Year 2 Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price"]
["Year 3 Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price"]
["Year 3 Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price"]
["Year 5 Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price"]
[]
[]
["Cable Cleanup"]
[]
[null,"Vmware SaaS"]
["Virtualisation /VMware Licenses to cover all hosts",2,"·        VMware Virtual Private Cloud Platform including:"]
[null,null,"o   vSphere Enterprise Plus"]
[null,null,"o   vCenter Standard per site"]
[null,null,"o   NSX Professional"]
[null,null,"o   vRealise Operations Manager Adv"]
[null,null,"o   Site Recovery Manager for ~ 300 VMs"]

{"sheet":"Dell Summary","index":1,"n_rows":78,"n_cols":4,"rows_kept":78,"merged":[[39,0,39,2],[40,0,40,2],[41,0,41,2],[42,0,42,2],[43,0,43,2],[46,0,46,2],[57,0,57,2],[58,0,58,2],[59,0,59,2],[60,0,60,2],[62,0,62,2],[63,0,63,2],[64,0,64,2],[65,0,65,2],[66,0,66,2],[67,0,67,2],[72,0,77,0],[72,1,77,1],[72,3,77,3]]}
[null,"Production","High Availability","DR "]
["Sites","AZ1","AZ2","DR (CPT)"]
["Management Clusters","4 x VxRail E660F","4 x VxRail E660F","4 x VxRail E660F"]
[null," 2 x Intel® Xeon® Gold 5320 2.2G, 26C CPUs"," 2 x Intel® Xeon® Gold 5320 2.2G, 26C CPUs"," 2 x Intel® Xeon® Gold 5320 2.2G, 26C CPUs"]
[null,"16 x 32GB RDIMM, Memory","16 x 32GB RDIMM, Memory","16 x 32GB RDIMM, Memory"]
[null,"5 x 3.84TB SSD SATA Read Intensive 6Gbps SSDs","5 x 3.84TB SSD SATA Read Intensive 6Gbps SSDs","5 x 3.84TB SSD SATA Read Intensive 6Gbps SSDs"]
[null,"Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0"]
[null,"ProdePloy Plus Services","ProdePloy Plus Services","ProdePloy Plus Services"]
[null,"5 Yrs Prosupport Plus Services","5 Yrs Prosupport Plus Services","5Yrs Prosupport Plus Services"]
[null,"VxRail VMware, vSAN Enterprise, 5 Years","VxRail VMware, vSAN Enterprise, 5 Years","VxRail VMware, vSAN Enterprise, 5 Years"]
[]
["Production Cluster ","5 x VxRail P670F","5 x VxRail P670F","5 x VxRail P670F"]
[null," 2 x Intel® Xeon® Platinum 8358 2.6G, 32C CPUs"," 2 x Intel® Xeon® Platinum 8358 2.6G, 32C CPUs"," 2 x Intel® Xeon® Platinum 8358 2.6G, 32C CPUs"]
[null,"16 x 32GB RDIMM, Memory","16 x 32GB RDIMM, Memory","16 x 32GB RDIMM, Memory"]
[null,"16 x 64GB RDIMM, Memory","16 x 64GB RDIMM, Memory","16 x 64GB RDIMM, Memory"]
[null,"Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0","Broadcom 57504 Quad Port 10/25GbE,SFP28, OCP NIC 3.0"]
[null,"Emulex LPE 35002 Dual Port 32Gb Fibre Channel HBA, PCIe Low Profile","Emulex LPE 35002 Dual Port 32Gb Fibre Channel HBA, PCIe Low Profile","Emulex LPE 35002 Dual Port 32Gb Fibre Channel HBA, PCIe Low Profile"]
[null,"ProdePloy Plus Services","ProdePloy Plus Services","ProdePloy Plus Services"]
[null,"5 Yrs Prosupport Plus Services","5 Yrs Prosupport Plus Services","5 YrsProsupport Plus Services"]
[]
["Storage ","Dell Powerstore 1200T","Dell Powerstore 1200T","Dell Powerstore 1200T"]
[null,"384GB Appliance DIMM 192GB Per Node","384GB Appliance DIMM 192GB Per Node","384GB Appliance DIMM 192GB Per Node"]
[null,"25GBE OPTICAL 4 PORT CARD PAIR","25GBE OPTICAL 4 PORT CARD PAIR","25GBE OPTICAL 4 PORT CARD PAIR"]
[null,"14 x 25X2.5 NVME SED SSD 15.36TB ","14 x 25X2.5 NVME SED SSD 15.36TB ","14 x 25X2.5 NVME SED SSD 15.36TB "]
[null,"3M PASSIVE 25G TWINAX CABLE QTY 2","3M PASSIVE 25G TWINAX CABLE QTY 2","3M PASSIVE 25G TWINAX CABLE QTY 2"]
[null,"32GB FC 4 PORT IO MODULE PAIR","32GB FC 4 PORT IO MODULE PAIR","32GB FC 4 PORT IO MODULE PAIR"]
[null,"ProDeploy Plus for PowerStore 1xxx T","ProDeploy Plus for PowerStore 1xxx T","ProDeploy Plus for PowerStore 1xxx T"]
[null,"ProDeploy Plus Add-On for PowerStore Remote Replication","ProDeploy Plus Add-On for PowerStore Remote Replication","ProDeploy Plus Add-On for PowerStore Remote Replication"]
[null,"ProDeploy Plus Add-On for PowerStore Local Replication","ProDeploy Plus Add-On for PowerStore Local Replication","ProDeploy Plus Add-On for PowerStore Local Replication"]
[null,"Data Migration Services: Remote Virtual V2V Migration 101 Plus VMs","Data Migration Services: Remote Virtual V2V Migration 101 Plus VMs","Data Migration Services: Remote Virtual V2V Migration 101 Plus VMs"]
[null,"5 Yrs ProSupport Plus and 4Hr Mission Critical ","5 Yrs ProSupport Plus and 4Hr Mission Critical ","5 Yrs ProSupport Plus and 4Hr Mission Critical "]
[]
[]
["IP Networking Switches","2 x S5248F","2 x S5248F","2 x S5248F"]
["SAN Switches","2 x DS6620","2 x DS6620 ","2 x DS6620"]
["Mgmt Switches","1 x S3048","1 x S3048","1 x S3048"]
["Rack","1 x 42U Dell NetShelter Rack","1 x 42U Dell NetShelter Rack","1 x 42U Dell NetShelter Rack"]
["Rack PDUs","2 x Rack PDU 32A, 230V, (36) C13 & (6) C19 ","2 x Rack PDU 32A, 230V, (36) C13 & (6) C19 ","2 x Rack PDU 32A, 230V, (36) C13 & (6) C19 "]
[]
["Physical Servers"]
[]
["Domain Controllers - 3  x PowerEdge R660xs"]
["Metro -Witness Server - 1 x PowerEdge R450 Server"]
["Cable Cleanup"]
[]
[]
["Dell Software (Transactional License Agreement )"]
["Quantity","License Model","Licensed SW"]
[5,"147-BCVE","PowerStore 1200 Base License TLA=IC "]
[742,"147-BBKO","PowerStore Capacity SW TLA=CB "]
[35,"147-BCSW","VxRail HCI15G AF/Hybrid ProcrGold TLA=IG "]
[44,"147-BCTG","VxRail 15G DynNode Processor Plat TLA=IG "]
[70,"147-BCTM","VxRail HCI Sys SW (CAP3.84 SATA)TLA=CF "]
[633,"147-BCSY","VxRail HCI Sys Memory 32GB TLA=CG "]
[352,"147-BCSP","VxRail HCI Sys Memory 64GB TLA=CG "]
[]
[]
["Year1 Professional Services"]
["5yrs - Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price"]
["Deployment of VCF Components & SRM (Once Off)                                   "]
[]
[]
["Year2 to Year 5 Services"]
["Year 2 Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price"]
["Year 3 Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price"]
["Year 3 Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price"]
["Year 5 Managed Services -  24x7 Hybrid : (Onsite Resources during business hrs & Remote after hrs) - Yearly Price"]
[]
[]
[]
[]
[null,"Vmware SaaS"]
["Virtualisation /VMware Licenses to cover all hosts",2,"·        VMware Virtual Private Cloud Platform including:"]
[null,null,"o   vSphere Enterprise Plus"]
[null,null,"o   vCenter Standard per site"]
[null,null,"o   NSX Professional"]
[null,null,"o   vRealise Operations Manager Adv"]
[null,null,"o   Site Recovery Manager for ~ 300 VMs"]

{"sheet":"VMware","index":2,"n_rows":15,"n_cols":3,"rows_kept":15,"merged":[[1,2,6,2],[7,0,11,0],[7,2,11,2],[12,2,14,2]]}
["Item","Description","Estimate Cost"]
[null,"Based on the consumption model, the solution includes the below."]
["VMware Private Cloud Platform","1.       vSphere Enterprise Plus"]
[null,"2.       vCenter standard"]
[null,"3.       NSX Prof"]
[null,"4.       vRealize Operations Manager adv"]
[null,"5.       Site Recovery Manager"]
["Value Added Services","The below services are included:"]
[null,"1.       Install, Manage & Operate VMware Software delivered to the customer as a Service."]
[null,"2.       Metering and reporting of VMware Product Usage and monthly billing to end customers. "]
[null,"3.       First-level support to customers & Log Support Calls to VMware."]
[]
["Deployment: ","These are services to stabilize and bring to a supported state the VMware environment for National Treasury. ","."]
["(Including Migrations and Upgrades)"]
[null,"Note: The previous scope can be used for this, based on the previous RFP"]

{"sheet":"HP Requirement","index":3,"n_rows":86,"n_cols":6,"rows_kept":86,"merged":[[1,1,1,5],[2,1,3,1],[2,2,3,2],[2,3,2,5],[3,3,3,5],[4,3,4,5],[5,1,9,1],[5,2,9,2],[5,3,5,5],[6,3,6,5],[7,3,7,5],[8,3,8,5],[9,3,9,5],[10,1,14,1],[10,2,14,2],[10,3,10,5],[11,3,11,5],[12,3,12,5],[13,3,13,5],[14,3,14,5],[15,1,19,1],[15,2,19,2],[15,3,15,5],[16,3,16,5],[17,3,17,5],[18,3,18,5],[19,3,19,5],[20,1,24,1],[20,2,24,2],[20,3,20,5],[21,3,21,5],[22,3,22,5],[23,3,23,5],[24,3,24,5],[25,1,29,1],[25,2,29,2],[25,3,25,5],[26,3,26,5],[27,3,27,5],[28,3,28,5],[29,3,29,5],[30,1,32,1],[30,2,32,2],[30,3,30,5],[31,3,31,5],[32,3,32,5],[33,1,44,1],[33,2,44,2],[33,3,33,5],[34,3,34,5],[46,1,57,1],[46,2,57,2],[46,4,57,4],[58,1,75,1],[58,2,75,2],[58,4,75,4],[76,1,78,1],[76,2,78,2],[76,4,78,4],[79,1,84,1],[79,2,84,2],[79,4,84,4],[85,1,87,1],[85,2,87,2],[85,4,87,4]]}
[]
[null,"Converged Solution with Software, Services and Support, with the following minimum specification:HP"]
[null,"Rack Infrastructure","·        2","·        2 x HPE 42U 600x1200mm Racks each with   4 x 7.3kVA/60309 3-wire 32A/230V Outlets (36) C13 (6) C19/Vertical INTL PDU "]
[{"$nulls":3},"·        KVM switch, Mouse, Monitor and LCD"]
[null,null,"·        3","·        2 x H PESynergy 12000 Blade enclosure provided with relevant redundant 100GB Interconnect Modules providing 100GB uplinks and 50GB downlinks with relevant 32GB FC connectivity and Ethernet Connectivity and all cables and transceivers for connectivity."]
[null,"General Purpose Workloads - Virtualisation Servers","·        3","·        10 x HPE Synergy Blade servers, each configured with: "]
[{"$nulls":3},"-        2x Processors: 4th Gen Gold Xeon® 24-core Scalable processors "]
[{"$nulls":3},"-        Memory: 1024TB (64GB (1x64GB) Dual Rank x4 DDR5-4800 CAS-40-39-39 EC8 Registered Smart Memory Kit)."]
[{"$nulls":3},"-        Internal HDD: 2 x 240GB SSDs. "]
[{"$nulls":3},"-        Mezzanine: Converged Network Adapter or equivalent with 25GB Ethernet and 32GB FC).."]
[null,"ALM Virtualisation Nodes","·        3","·        3 x HPE Synergy Blade servers, each configured with: "]
[{"$nulls":3},"-        2x Processors: 4th Gen Gold Xeon® 24-core Scalable processor."]
[{"$nulls":3},"-        Memory: 1024TB (64GB (1x64GB) Dual Rank x4 DDR5-4800 CAS-40-39-39 EC8 Registered Smart Memory Kit)."]
[{"$nulls":3},"-        Internal HDD: 2 x 240GB SSDs. "]
[{"$nulls":3},"·        Mezzanine: Converged Network Adapter or equivalent with 25GB Ethernet and 32GB FC).."]
[null,"Management nodes","·        3","·        3 x HPE Synergy Blade servers, each configured with: "]
[{"$nulls":3},"-        2x Processors: 4th Gen Gold Xeon® 24-core Scalable processor."]
[{"$nulls":3},"-        Memory: 1024TB (64GB (1x64GB) Dual Rank x4 DDR5-4800 CAS-40-39-39 EC8 Registered Smart Memory Kit)."]
[{"$nulls":3},"-        Internal HDD: 2 x 240GB SSDs. "]
[{"$nulls":3},"·        Mezzanine: Converged Network Adapter or equivalent with 25GB Ethernet and 32GB FC)."]
[]
[]
[]
[]
[]
[null,"Domain Controllers","·        3","·        HPE DL20 servers, each configured with: "]
[{"$nulls":3},"-        1 x Processors: Intel Xeon E-2314 2.8GHz 4-core processor "]
[{"$nulls":3},"-        Memory: 128GB "]
[{"$nulls":3},"-        Internal HDD: 2 x 1.2TB SAS 12G. "]
[{"$nulls":3},"-        NIC: 10Gb 2-port SFP+ Adapter"]
[null,"Networking","·        3","·        2 x Redundant Aruba 48 Port 25G SFP+/28, with 8 x 100G QSFP+/28 uplink ports"]
[{"$nulls":3},"·        2 x redundant Aruba 48 Port 1 or 10 GB base-T Management switches  with 4 x 40G/100GB QSFP+QSFP28  uplink ports"]
[{"$nulls":3},"-        ALL cables and the necessary transceivers  for connectivity"]
[null,"Storage Array ","·        3","·         Storage Array with 372TB useable capacity and 481TB Raw capacity and 929TB Effective useable capacity on a ratio of  2.5:1 with the following minimum specification."]
[]
[{"$nulls":3},"Qty","Part","Description"]
[{"$nulls":3},1,"R0N93A","HPE Alletra 9000 4-way NVMe Storage Base"]
[{"$nulls":3},1,"R0N99A","HPE Alletra 9060 2N Controller"]
[{"$nulls":3},2,"R4W00A","HPE 1700W PS Battery Kit"]
[{"$nulls":3},2,"R3B28A","HPE Alletra 9000 16/32Gb 4p FC HBA"]
[{"$nulls":3},8,"Q2P62A","HPE 32Gb SFP28 Short Wave 1-pack Pull Tab Optical Transceiver"]
[{"$nulls":3},1,"R3B13A","HPE Alletra 2240 2U SFF FIO Drive Enclosure"]
[{"$nulls":3},32,"R0Q10B","HPE ALLETRA 9000 15.36TB NVMe FE SSD"]
[{"$nulls":3},1,"R1P29A","HPE Data Encryption LTU"]
[{"$nulls":3},0,"R7N52AAE#CTF","HPE Alletra Software and Support SaaS 3-year Subscription"]
[]
[null,"Consulting and Deployment Services","·        3","·        Project Management with Complete documentation of the solution (Test, sign-off and handover)"]
[{"$nulls":3},"·        Solution design."]
[{"$nulls":3},"-        Hardware design (Server, Network, Storage, Backup and DR  Solution)."]
[{"$nulls":3},"-        Vmware Design."]
[{"$nulls":3},"·        Solution Installation and Configuration"]
[{"$nulls":3},"-        Onsite Installation and start up services for Server, Network, Storage, backup solution as per the design."]
[{"$nulls":3},"-        Vmware installation and configuration as per the design."]
[{"$nulls":3},"-        Data migration (about ~213TB), from  current environment to new infrastructure"]
[{"$nulls":3},"-        V2V migrations to new environment (About 300 VMs)"]
[{"$nulls":3},"-        Disaster Recovery setup and configuration with automated failover and failback."]
[{"$nulls":3},"-        Disater Recovery testing "]
[]
[null,"Managed Services (HW, OS and vMware Excl Applications)","·        3","Managed Services (HO, SITA and DR) with Onsite Resource during business hrs & Remote after hrs."]
[{"$nulls":3},"·        Hardware Management"]
[{"$nulls":3},"·        System administration and operation"]
[{"$nulls":3},"·        Operating System (OS) Management"]
[{"$nulls":3},"·        Database Support and Management"]
[{"$nulls":3},"·        Bare Metal Management"]
[{"$nulls":3},"·        On Premise Cloud support and management"]
[{"$nulls":3},"·        Hypervisor support and management "]
[{"$nulls":3},"·        Virtual Machine Management ~ 300 "]
[{"$nulls":3},"·        Resource monitoring and alerting"]
[{"$nulls":3},"·        Resource administration and operation"]
[{"$nulls":3},"·        Aggregated log monitoring"]
[{"$nulls":3},"·        OS imaging and patch management"]
[{"$nulls":3},"·        Backup Management"]
[{"$nulls":3},"·        Resource Backup, Archival and Recovery"]
[{"$nulls":3},"·        Resource optimization"]
[{"$nulls":3},"·        Capacity and utilisation Dashboards"]
[]
[null,"Support and Maintenance","·        3","·        Hardware – 5 year 24x7 Complete Care (Semi-annual operating-system environment patch analysis, firmware analysis, Annual System Health Check)"]
[{"$nulls":3},"·        Software – 5 year 24x7 telephonic support standard"]
[{"$nulls":3},"o    "]
[null,"Support Credits  and Training","·        1","·        300 OEM Credits to provide for any additional services required by the department."]
[{"$nulls":3},"·        Training for 5 x Resources on the following"]
[{"$nulls":3},"o   Compute"]
[{"$nulls":3},"o   Storage"]
[{"$nulls":3},"o   vMware vSphere"]
[]
[null,"Cable Cleanup"]