{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Schedule - Fittings","Deviation Schedule","Test Schedule"],"not_rendered":{"defined_names":7},"read":"whole","date_system":"1900"}

{"sheet":"Schedule - Fittings","index":0,"n_rows":52,"n_cols":7,"rows_kept":52,"merged":[[0,0,0,7],[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,1,4,6],[5,1,5,6],[8,2,8,3],[9,2,9,3],[26,2,26,3],[27,2,27,3],[40,1,40,3],[41,0,41,7]]}
["ESKOM TENDER E2719DXLIMOU"]
[null,"Technical Schedules A and B for"]
[null,"COACH SCREW,GALV 75x6 HEX HD  D3090"]
[null,"SAP No.0163803"]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No",null,{"v":163803,"d":"0163803"},"xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer Name",null,"xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Product Code",null,"xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's Drawing number & Revision number",null,"xxxxxxxxxx"]
[null,"1.1.6",null,"Physical identification mark on product",null,"xxxxxxxxxx"]
[null,"1.1.7",null,"Compliance to critial dimensions on Buyer's Guide","Eskom's D-DT 3090","YES"]
[null,"1.1.8",null,"Item sample required, upon request from Eskom. (As per the Technical Criteria Document)",null,"YES"]
[null,1.2,"·","Mechanical Properties"]
[null,"1.2.2",null,"Material Grade",null,"SAE 1008"]
[null,1.3,"·","Coupling interfaces (where applicalbe)"]
[null,"1.3.1",null,"Diameter Thread","mm",12]
[null,"1.3.2",null,"Length","mm",75]
[null,"1.3.3",null,"Thread type",null,"Wood Screw"]
[null,1.4,"·","Galvanising (where applicalbe)"]
[null,"1.4.1",null,"Average minimum galvanising thickness on product body to SANS 121","YES/NO","YES"]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to be provided in electronic format."]
[null,2.1,"·","General"]
[null,"2.1.1",null,"Outline drawings of item","Sets",1]
[null,"2.1.2",null,"Material grade certification",null,"YES"]
[null,2.2,"·","Test Reports (where applicable)","Test","Specification","Report Number"]
[null,"2.2.1",null,"Visual inspection and dimensions verification","Type Test","SANS 1171 "]
[null,"2.2.5",null,"Depth gauging of cross recesses","Type Test","SANS 1171 "]
[null,"2.2.6",null,"Tensile Test ","Type Test","SANS 1171 "]
[null,"2.2.7",null,"Tilt of screw Heads ","Type Test","SANS 1171 "]
[null,3,null,"Packaging information"]
[null,3.1,"·","General"]
[{"$nulls":3},"Mass of coach screws package ","kg",25]
[]
[]
["ESKOM TENDER E2719DXLIMOU"]
[null,"SIGNATURES"]
[]
[null,"Supplier"]
[{"$nulls":3},"Name (Print)",null,"Sign","Date"]
[]
[null,"Manufacturer"]
[{"$nulls":3},"Name (Print)",null,"Sign","Date"]
[]
[null,"Eskom"]
[{"$nulls":3},"Name (Print)",null,"Sign","Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":43,"n_cols":8,"rows_kept":43,"merged":[[0,0,0,8],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,1,4,7],[6,1,6,7],[7,3,7,7],[8,3,8,7],[9,3,9,7],[10,3,10,7],[11,3,11,7],[12,3,12,7],[13,3,13,7],[14,3,14,7],[15,3,15,7],[16,3,16,7],[17,3,17,7],[18,3,18,7],[19,3,19,7],[20,3,20,7],[21,3,21,7],[22,3,22,7],[23,3,23,7],[24,3,24,7],[25,3,25,7],[26,3,26,7],[27,3,27,7],[28,3,28,7],[29,3,29,7],[30,3,30,7],[32,0,32,8],[35,1,35,2],[36,1,36,2],[38,1,38,2],[39,1,39,2],[41,1,41,2],[42,1,42,2]]}
["ESKOM TENDER E2719DXLIMOU"]
[null,"Deviation Schedule"]
[null,"Technical Schedules A and B for"]
[null,"COACH SCREW,GALV 75x12 HEX HD  D3090"]
[null,"SAP No.0163803"]
[]
[null,"Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
[null,"Item","Clause","Description of Deviation"]
{"$rows_empty":24}
["ESKOM TENDER E2719DXLIMOU"]
[null,"SIGNATURES"]
[]
[null,"Supplier",null,"         "]
[{"$nulls":3},"Name (Print)",null,"Sign",null,"Date"]
[]
[null,"Manufacturer",null,"         "]
[{"$nulls":3},"Name (Print)",null,"Sign",null,"Date"]
[]
[null,"Eskom",null,"         "]
[{"$nulls":3},"Name (Print)",null,"Sign",null,"Date"]

{"sheet":"Test Schedule","index":2,"n_rows":21,"n_cols":5,"rows_kept":21,"merged":[[0,0,0,5],[1,1,1,4],[2,1,2,4],[3,1,3,4],[10,1,10,2],[13,0,13,5],[16,0,16,2],[16,4,16,5],[20,0,20,2],[20,4,20,5]]}
["ESKOM TENDER E2719DXLIMOU"]
[null,"Test Report Schedule"]
[null,"COACH SCREW,GALV 75x12 HEX HD  D3090"]
[null,"SAP No. 0163803"]
[null,1,2,3,4]
[null,"Item ","Description","Specification","Report No."]
[null,"2.2.1","Visual inspection and dimensions verification","SANS 1171"]
[null,"2.2.2","Depth gauging of cross recesses","SANS 1171"]
[null,"2.2.3","Tensile Test ","SANS 1171"]
[null,"2.2.4","Tilt of screw Heads ","SANS 1171"]
[]
[]
[]
["SIGNATURES"]
[]
["         "]
["Name (Print)",{"$nulls":3},"Company Name"]
[]
[]
[]
["Sign",{"$nulls":3},"Date"]