{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Available"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Available","index":0,"n_rows":2254,"n_cols":12,"rows_kept":2254,"merged":[[0,0,0,5],[81,0,81,1],[82,0,82,1],[83,0,83,5],[84,0,84,5],[164,0,164,1],[165,0,165,1],[166,0,166,1],[168,0,168,5],[251,0,251,4],[264,0,264,4],[330,0,330,1],[331,0,331,1],[332,0,332,1],[333,0,333,5],[417,0,417,3],[430,0,430,3],[490,0,490,1],[491,0,491,1],[492,0,492,1],[574,0,574,1],[575,0,575,1],[576,0,576,1],[578,0,578,5],[659,0,659,1],[660,0,660,1],[661,0,661,1],[663,0,663,5],[674,0,674,1],[675,0,675,1],[676,0,676,1],[743,0,743,1],[744,0,744,1],[745,0,745,1],[747,0,747,5],[838,0,838,4],[851,0,851,4],[920,0,920,1],[921,0,921,1],[922,0,922,1],[924,0,924,5],[999,0,999,1],[1000,0,1000,1],[1001,0,1001,1],[1003,0,1003,5],[1080,0,1080,1],[1081,0,1081,1],[1082,0,1082,1],[1084,0,1084,5],[1161,0,1161,1],[1162,0,1162,1],[1163,0,1163,1],[1165,0,1165,5],[1250,0,1250,1],[1251,0,1251,1],[1252,0,1252,1],[1254,0,1254,5],[1334,0,1334,1],[1335,0,1335,1],[1336,0,1336,1],[1337,0,1337,5],[1415,0,1415,1],[1416,0,1416,1],[1417,0,1417,1],[1418,0,1418,5],[1487,0,1487,1],[1488,0,1488,1],[1489,0,1489,1],[1490,0,1490,5],[1571,0,1571,1],[1572,0,1572,1],[1573,0,1573,1],[1574,0,1574,5],[1583,1,1583,4],[1712,0,1712,1],[1713,0,1713,1],[1714,0,1714,1],[1715,0,1715,5],[1794,0,1794,1],[1795,0,1795,1],[1796,0,1796,1],[1798,0,1798,5],[1876,0,1876,1],[1877,0,1877,1],[1878,0,1878,1],[1880,0,1880,5],[1960,0,1960,1],[1961,0,1961,1],[1962,0,1962,1],[1963,0,1963,5],[2043,0,2043,1],[2044,0,2044,1],[2045,0,2045,1],[2123,0,2123,1],[2124,0,2124,1],[2125,0,2125,1],[2127,0,2127,5],[2135,3,2136,5],[2194,1,2194,2],[2197,0,2198,0],[2197,1,2198,2],[2199,1,2200,2],[2199,3,2200,3],[2199,5,2200,5],[2201,1,2202,2],[2201,3,2202,3],[2201,5,2202,5],[2203,0,2204,2],[2203,3,2204,3],[2203,5,2204,5],[2217,0,2217,5]],"flags":["formulas_cached_only"]}
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control",{"$nulls":8},"DURATION"]
["  ROADWORKS",{"$nulls":6},5.275,null,16]
["SECTION 1200",{"$nulls":6},"INTERSECTION"]
[{"$nulls":7},0.7]
[{"$nulls":7},"BELL-MOUTHS"]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT",null,0.1]
[{"$nulls":5},"R"]
[]
[12,"GENERAL REQUIREMENTS AND",{"$nulls":4},"TOTAL",6.075]
[null,"PROVISIONS"]
[{"$nulls":7},6075]
["B12.30","Excavation for existing services:"]
[]
[null,"(a) Excavation in search of existing"]
[null,"      services in soft material situated in"]
[null,"      the following depth ranges:"]
[]
[null,"      (i) 0 m to 2 m","m³",{"v":400,"d":"400.00"}]
[null,"      (ii) 2 m to 3 m","m³",{"v":240,"d":"240.00"}]
[]
[null,"(b) Extra over B12.01(a) for excavation"]
[null,"      in hard material in close vicinity of"]
[null,"      services using picks, jackhammers,"]
[null,"      powertools etc. where no blasting or"]
[null,"      machine excavation is permitted","m³",{"v":320,"d":"320.00"}]
[]
["B12.31","Relocating of services:"]
[]
[null,"(a) Allow a provisional sum for the repair"]
[null,"      and / or relocation of existing"]
[null,"      services which is not allowed for in"]
[null,"      the schedule of quantities","Prov. Sum",{"v":1,"d":"1.00"},{"v":300000,"d":"R 300,000.00"},{"v":300000,"d":"300,000.00"}]
[]
[null,"(b) Handling costs and profit in respect"]
[null,"     of sub-item B12.31 (a)","%",{"v":300000,"d":"300000.00"}]
[]
["B12.32","Backfilling"]
[]
[null,"(a) Using the excavated material","m³",{"v":320,"d":"320.00"}]
[]
[null,"(b) Using imported selected material","m³",{"v":64,"d":"64.00"}]
[]
["B12.33","Provision of training:"]
[]
[null,"(a) General skills training "]
[null,"(technical and entrepeneurial skills)","Prov. Sum",{"v":1,"d":"1.00"},{"v":200000,"d":"R 200,000.00"},{"v":200000,"d":"200,000.00"}]
[]
[null,"(b) Handing cost and Profit with respect to "]
[null,"sub-item B13.33","%",{"v":200000,"d":"200000.00"}]
[]
["B12.34","Provision for the implementation and monitoring"]
[null,"of Enviromental Management Plan","Prov Sum",{"v":1,"d":"1.00"},{"v":320000,"d":"R320,000.00"},{"v":320000,"d":"320,000.00"}]
[]
[null,"(a) Handing cost and profit with respect to "]
[null,"sub-item B13.34","%",{"v":320000,"d":"320000.00"}]
[]
["B12.35","Public Participation"]
[]
[null,"(a) Allow a provisional sum for payment"]
[null,"    of salary for CLO including cellphone allowance","Prov. Sum",{"v":1,"d":"1.00"},{"v":96000,"d":"R 96,000.00"},{"v":96000,"d":"96,000.00"}]
[]
[null,"(b) Allow a provisional sum for payment","Prov. Sum",{"v":1,"d":"1.00"},{"v":192000,"d":"R 192,000.00"},{"v":192000,"d":"192,000.00"}]
[null,"      of salary for 2 students"]
[]
[null,"(c) Provisional Sum for PSC (R200/member/sitting)","Prov. Sum",{"v":1,"d":"1.00"},{"v":19200,"d":"R 19,200.00"},{"v":19200,"d":"19,200.00"}]
[]
[null,"(d) Provisional sum for payment of royalties","Prov Sum",{"v":1,"d":"1.00"},{"v":20000,"d":"R 20,000.00"},{"v":20000,"d":"20,000.00"}]
[]
[null,"(e) Allow a provisional sum for payment",null,{"v":1,"d":"1.00"},{"v":72000,"d":"R 72,000.00"},{"v":72000,"d":"72,000.00"}]
[null,"      of SHE Rep"]
[]
[null,"(e ) Social Facilitation","Prov. Sum",{"v":1,"d":"1.00"},{"v":320000,"d":"R320,000.00"},{"v":320000,"d":"320,000.00"}]
[]
[null,"(d) Occupational Health and Safety obligations","Prov. Sum",{"v":1,"d":"1.00"},{"v":560000,"d":"R 560,000.00"},{"v":560000,"d":"560,000.00"}]
[null,"(items covered are included in the specifications)"]
[]
[null,"(f) Handling cost and profit"]
[null,"    in respect of sub-item B12.35","%",{"v":1279200,"d":"R1,279,200.00"}]
[]
[]
[" Total Carried Forward to Summary "]
[]
[1]
[]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 1300"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[13,"CONTRACTOR'S ESTABLISHMENT"]
[null,"ON SITE AND GENERAL"]
[null,"OBLIGATIONS"]
[]
["13.01","Contractor's general obligations"]
[]
[null,"(a) Fixed obligations","Lump Sum",{"v":1,"d":"1.00"}]
[]
[null,"(b) Value-related obligations","Lump Sum",{"v":1,"d":"1.00"}]
[]
[null,"(c) Time-related obligations","Month",{"v":16,"d":"16.00"}]
[]
[]
[null,"Note:"]
[null,"Should the combined total tendered sub-items (a), "]
[null,"(b) and (c) exceeds 15% of the tender sum"]
[null,"(excluding VAT), the tenderer shall state their"]
[null,"reasons in writing a letter attached to Form"]
{"$rows_empty":51}
[" Total Carried Forward to Summary"]
[]
[" ",null,2]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 1400"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[14,"HOUSING, OFFICES AND LABORATORIES "]
[null,"FOR THE ENGINEERS SITE PERSONNEL"]
[]
["14.01","Office and laboratory accommodation:"]
[]
[null,"(a) Offices (interior floor space only)","m²",{"v":40,"d":"40.00"}]
[]
[null,"(b) Laboratories (interior floor space only)","m²",null,null,"Rate Only"]
[]
[null,"(c) Open concrete working floors (150 mm thick)","m²",{"v":15,"d":"15.00"}]
[]
[null,"(d) Roofs over open concrete working floors","m²",{"v":15,"d":"15.00"}]
[]
[null,"(e) Ablution units","m²",{"v":15,"d":"15.00"}]
[]
[null,"(f) Stores","m²",{"v":20,"d":"20.00"}]
[]
["14.02","Office and laboratory furniture:"]
[]
[null,"(a) Chairs","No",{"v":15,"d":"15.00"}]
[]
[null,"(b) Draughtsman's stools ","No",null,null,"Rate Only"]
[]
[null,"(c) High chairs for laboratory","No",null,null,"Rate Only"]
[]
[null,"(d) Desks, complete with drawers and locks"," No ",{"v":2,"d":"2.00"}]
[]
[null,"(e) Drawing tables","No"]
[]
[null,"(f)  Conference tables","No",{"v":2,"d":"2.00"}]
[]
["14.03","Office and  laboratory fittings,"]
[null,"Installations and equipment:"]
[]
[null,"(a) Items measured by number"]
[]
[null,"    (i) 220/250 volt power points","No",{"v":1,"d":"1.00"}]
[]
[null,"    (ii) 400/231 volt 3-phase power points ","No",{"v":1,"d":"1.00"}]
[]
[null,"    (iii) Double 80 watt fluorescent light fittings"]
[null,"          complete with ballast and tubes","No",{"v":2,"d":"2.00"}]
[]
[null,"    (iv) Double 55 watt fluorescent-light fittings"]
[null,"          complete with ballast and tubes","No",{"v":2,"d":"2.00"}]
[]
[null,"    (v) Single incandescent-light fittings "]
[null,"         complete with 100 watt globes","No",{"v":1,"d":"1.00"}]
[]
[null,"    (vi) Wash-hand basins complete"]
[null,"        with taps and drains","No",{"v":2,"d":"2.00"}]
[]
[null,"    (x) Fire extinguishers, 9 kg,all purpose dry"]
[null,"        powder type, complete, mounted on wall"]
[null,"        with brackets","No",{"v":2,"d":"2.00"}]
[]
[null,"    (xi) Air-conditioning unit with, 2,2kW minimum"]
[null,"         capacity, mounted and with own power "]
[null,"         connection","No",{"v":1,"d":"1.00"}]
[]
[null,"    (xii) Heater, space-heating type, minimum "]
[null,"           capacity 1,5 kW","No",{"v":1,"d":"1.00"}]
[]
[null,"    (xiv) General-purpose steel cupboards "]
[null,"          with shelves","No",{"v":2,"d":"2.00"}]
[]
[null,"    (xvi) Refrigerators ","No",{"v":1,"d":"1.00"}]
[]
[]
[]
[]
[]
["Total Carried Forward "]
[]
[null,null,3]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 1400"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[{"$nulls":5},"R"]
[]
["Brought Forward"]
[]
[]
["14.03","Office and  laboratory fittings,"]
[null,"Installations and equipment:"]
[]
[null,"(b) Prime-cost items and items paid for in a "]
[null,"lump sum:"]
[]
[null,"(i) The provision of telephone service, including "]
[null,"the cost of cells in connection with contract "]
[null,"administration and telephone rental","PC Sum",{"v":1,"d":"1.00"},{"v":40000,"d":"R 40,000.00"},{"v":40000,"d":"40,000.00"}]
[]
[null,"(ii) Handling costs and profit in respect of"]
[null,"sub-sub-item 14.03(b)(i)","%",{"v":40000,"d":"40000.00"}]
[]
[null,"(iii) The provision of a direct independent "]
[null,"telephone line for the engineer, including"]
[null,"the cost of cells in connection with contract"]
[null,"administration and telephone rental","PC Sum",{"v":1,"d":"1.00"},{"v":70000,"d":"R 70,000.00"},{"v":70000,"d":"70,000.00"}]
[]
[null,"(iv) Handling costs and profit in respect to"]
[null,"sub-subitem (b)(iii)","%",{"v":70000,"d":"70000.00"}]
[]
[null,"(vii) The provision of 400/231 volt 3-phase"]
[null,"electrical power installation, including all wiring,"]
[null,"switchboards, mains connections, etc","Lump Sum",{"v":1,"d":"1.00"}]
[]
[]
[null,"    (viii) Notice boards (contract name board)","No",{"v":1,"d":"1.00"}]
[]
["14.04","Car Ports"]
[]
[null,"Car ports as specified at offices and","No",{"v":3,"d":"3.00"}]
[null,"laboratory buildings"]
[]
["14.07","Rental, hotel and other accommodation:"]
[]
[null,"(a) Provisional sum for providing rented housing,"]
[null,"hotel or ther accommodation as described in"]
[null,"sub-subclause 1403(c)(ii)","Prov Sum",{"v":1,"d":"1.00"},{"v":350000,"d":"R 350,000.00"},{"v":350000,"d":"350,000.00"}]
[]
[null,"(b) Handlingg cost and profit iin respect to"]
[null,"sub-item 14.07(a)","%",{"v":350000,"d":"350000.00"}]
[]
["14.08","Services"]
[]
[null,"The provision of water, electricity, low pressure"]
[null,"gas, sewerage, septic tanks, sewage and rubbish"]
[null,"removal, cleaning services, ,maintenance and"]
[null,"repairs including the construction and"]
[null,"maintenance of the access roads, footpaths etc"]
[]
[null,"(a) Services at offices and laboratories"]
[]
[null,"         (i) Fixed Costs","Lump Sum",{"v":1,"d":"1.00"}]
[]
[null,"         (ii) Running Costs","Month",{"v":16,"d":"16.00"}]
[]
[null,"(c)  Services for rented houses","Month",{"v":16,"d":"16.00"}]
[]
["B14.11","Provision of photostat facilities","Prov Sum",{"v":1,"d":"1.00"},{"v":10000,"d":"R 10,000.00"},{"v":10000,"d":"10,000.00"}]
[]
[null,"Handling cost and profit in respect ","%",{"v":10000,"d":"10000.00"}]
[null,"of sub-item B14.11"]
[]
[]
[" Total Carried Forward to Summary"]
[]
[4]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 1500"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[15,"ACCOMODATION OF TRAFFIC"]
[]
["15.01","Accommodating traffic and maintaining"]
[null,"temporary deviations","km",{"v":7,"d":"7.00"}]
[]
["15.02","Earthworks for temporary deviations:"]
[]
[null,"(a) Shaping of temporary deviations","km",{"v":7,"d":"7.00"}]
[]
[null,"(b) Cut and borrow to fill","m3",{"v":7000,"d":"7000.00"}]
[]
[null,"(c) Cut to spoil ","m3",{"v":2600,"d":"2600.00"}]
[]
["15.03","Temporary traffic-control facilities:"]
[]
[null,"(a) Flagmen ","Man-day ",1408]
[]
[null,"(b) Portable STOP (R1.5A) and"]
[null,"     GO-RY (R1.5B) sgins","No",{"v":2,"d":"2.00"}]
[]
[null,"(c) Temporary traffic-control signals as specified  "]
[null,"      or shown on the drawing ","No",{"v":2,"d":"2.00"},null,"Rate Only"]
[]
[null,"(e) Road sgins, R- and TR-series (1200x1600mm)","No",{"v":30,"d":"30.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"     i. TR103/104 (Keep left/right)","No ",{"v":4,"d":"4.00"}]
[null,"    ii. TR214 (Overtaking prohibited)","No ",{"v":2,"d":"2.00"}]
[null,"   iii. TR201 - 80 (speed limit)","No ",{"v":2,"d":"2.00"}]
[null,"   iv. TR201 - 60 (speed limit)","No ",{"v":2,"d":"2.00"}]
[null,"    v. TR201 - 40 (speed limit)","No ",{"v":6,"d":"6.00"}]
[null,"   vi. TR218 (Pedestrians prohibited)","No",{"v":2,"d":"2.00"}]
[]
[null,"(f) Road signs. TW-series (1200x1600 mm)"]
[null,"     i. TW336 (Road work ahead)","No",{"v":5,"d":"5.00"}]
[null,"    ii. TW343.TIN11.3 (Stop/Ry-Go control ahead)","No",{"v":2,"d":"2.00"}]
[null,"   iii. TW411 (Temporary barricade)","No",{"v":5,"d":"5.00"}]
[null,"   iv. TW304 (Traffic control ahead)","No",{"v":2,"d":"2.00"}]
[null,"    v. TW305 (Scholar patrol ahead)","No",{"v":5,"d":"5.00"}]
[null,"    vi. TW308 (Children)","No",{"v":10,"d":"10.00"}]
[null,"    vii. TW"]
[]
[null,"(g) Road signs, STW-, DTG-, TGS-, and TG-series"]
[null,"     (excluding delineators and barricades)","No",{"v":10,"d":"10.00"},{"v":1000,"d":"R 1,000.00"},"Rate Only"]
[]
[null,"(h) Delineators (DTG50J) 250x1000 mm:"]
[null,"        (i) Single","No",{"v":25,"d":"25.00"}]
[null,"        (ii) Mounted back to back","No",{"v":50,"d":"50.00"}]
[]
[null,"(i) Movable barricades/road sgin "]
[null,"    combination (2400x1500 mm)","No",{"v":4,"d":"4.00"}]
[]
[null,"(j) Traffic cones (750 mm high)","No",{"v":250,"d":"250.00"}]
[]
[null,"(l) Movable barriers (steel or hard plastic)","No",{"v":15,"d":"15.00"},null,"Rate Only"]
[]
[null,"(m) Two-way communication devices","No",{"v":2,"d":"2.00"}]
[]
["15.04 ","Relocation of traffic-control facilities ","Lump Sum",{"v":1,"d":"1.00"}]
[]
["15.05","Gravelling and repair of temporary deviations "]
[null,"and existing gravel shoulders used as temporary "]
[null,"deviations:"]
[]
[null,"(a) Temporary deviations","m3",{"v":6300,"d":"6300.00"}]
[]
[null,"(b) Existing gravel shoulders","m3",{"v":45,"d":"45.00"}]
[]
["15.06","Watering of temporary deviations","kℓ",{"v":500,"d":"500.00"}]
[]
[]
[]
[]
["Total Carried Forward"]
[]
[null,null,5]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 1500"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT "]
[{"$nulls":5},"R"]
[]
["Brought Forward"]
[]
[]
[]
["15.07","Blading by road grader of:"]
[]
[null,"(a) Temporary deviations","km-pass",null,null,"Rate Only"]
[]
[null,"(b) Existing roads used as temporary deviations","km-pass",null,null,"Rate Only"]
[]
[null,"(c) Existing gravel shoulders used as "]
[null,"emporary deviations","km-pass",null,null,"Rate Only"]
[]
["B15.14","Provision of traffic safety equipment for"]
[null,"the Engineer"]
[]
[null,"(a) 'Construction' sticker for vehicles with "]
[null,"100 mm high lettering ","No",{"v":3,"d":"3.00"}]
[]
[null,"(b) Safety jackets","No",{"v":3,"d":"3.00"}]
[]
[null,"(c) Amber flicker lights ","No",{"v":3,"d":"3.00"}]
{"$rows_empty":39}
[" Total Carried Forward To Summary"]
[]
[null,null,6]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 1700"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[17,"CLEARING AND GRUBBING"]
[]
["17.01","Clearing and Grubbing","ha",{"v":5,"d":"5.00"}]
[]
["17.02","Removal and grubbing of large trees and tree"]
[null,"stumps"]
[]
[null,"(a) Girth exceeding 1m up to and including 2m","No",{"v":30,"d":"30.00"}]
[]
[null,"(b) Girth exceeding 2m up to and including 3m","No",{"v":20,"d":"20.00"}]
[]
["17.04","Clearing and grubbing at inlets and outlets of "]
[null,"hydraulic structures","m³",{"v":15,"d":"15.00"}]
[]
["17.05","Cleaning out of hydraulic structures:"]
[]
[null,"(a) Pipes with an internal diameter","m³",null,null,"Rate Only"]
[null,"up to and including 750mm"]
[]
[null,"(b) Pipes with an internal diameter","m³",null,null,"Rate only "]
[null,"exceeding 750mm"]
[]
[null,"(c)  Box culverts up to and including 1,5 m "]
[null,"vertical dimension","m³",{"v":15,"d":"15.00"}]
[]
[null,"(d) Box culverts exceeding 1,5 m vertical"]
[null,"dimension","m³",{"v":15,"d":"15.00"}]
{"$rows_empty":43}
[" Total Carried Forward To Summary"]
[]
[null,null,7]
[]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 2100"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[21,"DRAINS"]
[]
["21.01","Excavation for open drains:"]
[]
[null,"(a) Excavating soft material situated"]
[null,"      within the following depth ranges"]
[null,"      below the surface level:"]
[]
[null,"      (i) 0 m up to 1,5 m","m³",{"v":1666.875,"d":"1666.88"}]
[]
[null,"      (ii) Exceeding 1,5 m up to 3 m","m³",{"v":600,"d":"600.00"}]
[]
[null,"(b) Extra over subitem 21.01(a) for"]
[null,"      excavation in hard material,"]
[null,"      irrespective of depth","m³",{"v":1333.5,"d":"1333.50"},null,null,5200]
[]
["21.02","Clearing and shaping existing open drains","m³",null,null,"Rate Only"]
[]
["21.03","Excavation for subsoil drainage systems:"]
[]
[null,"(a)  Excavating soft material situated within the"]
[null,"     following depth ranges below the surface level:"]
[null,"                    (i) 0m up to 1,0m","m³",{"v":9112.5,"d":"9112.50"}]
[]
[null,"(b)  Extra over subitem 21.03(a) for excavation in"]
[null,"          hard material irrespective of depth","m³",{"v":1822.5,"d":"1822.50"}]
[]
["21.04","Impermeable backfilling to subsoil drainage"]
[null,"systems","m³",{"v":150,"d":"150.00"}]
[]
["21.05","Banks and dykes","m³",null,null,"Rate Only"]
[]
["21.06","Natural permeable material in subsoil"]
[null,"drainage systems (crushed-stone):"]
[]
[null,"(a) Crushed-stone obtained from approved"]
[null,"     sources (no-overhaul):"]
[]
[null,"        (i) Fine grade stone (13,2mm nominal size","m³",{"v":150,"d":"150.00"}]
[null,"            aggregate)"]
[null,"        (ii) Coarse grade stone (19mm nominal size "]
[null,"            aggregate)","m³",{"v":150,"d":"150.00"}]
[]
["21.07","Natural permeable material in subsoil"]
[null,"drainage systems (sand):",{"$nulls":5},200,"Length"]
[]
[null,"(b) Sand from commercial sources (no-overhaul)","m³",{"v":150,"d":"150.00"},{"$nulls":3},0.2,"depth (iii)"]
[]
["21.08","Pipes in subsurface drainage systems:",{"$nulls":5},0.5,"Width"]
[]
[null,"(b) Unplasticized PVC pipes and fittings, normal",{"$nulls":5},0.3,"depth (ii)"]
[null,"      duty, complete with couplings:"]
[]
[null,"            (i) 160mm diameter, perforated","m",{"v":200,"d":"200.00"},{"$nulls":3},0.8,"depth (i)"]
[]
["21.10","Synthetic-fibre filter fabric:"]
[]
[null,"(a) Non-woven needle punched type:"]
[]
[null,"     (i) \"Bidim Grade A4\" or approved  equivalent","m²",{"v":600,"d":"600.00"}]
{"$rows_empty":10}
[" Total Carried Forward "]
[]
[null,null,8]
[]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 2100"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[" Brought Forward"]
[]
[]
[]
["21.12","Concrete outlet structures, manhole boxes,"]
[null,"junction boxes and cleaning eyes for "]
[null,"subsoil drainage systems:"]
[]
[null,"(a)    Outlet structures","No",{"v":1,"d":"1.00"}]
[]
[null,"(d)     Cleaning eyes","No",{"v":1,"d":"1.00"}]
[]
[]
["21.13","Concrete caps for subsoil drain pipes","No",{"v":2,"d":"2.00"}]
[]
["21.15","Overhaul for material hauled in excess"]
[null,"of 1,0 km free-haul (normal overhaul)","m³-km",{"v":3600,"d":"3600.00"}]
[]
["21.17","Test flushing of pipe subsoil drains","No",{"v":1,"d":"1.00"}]
[]
[]
["B21.20","Subsoil drainage markers ","No",{"v":2,"d":"2.00"}]
[]
["B21.21","Cast In-situ reinforced Energy Breakers ","m³",{"v":10.756800000000002,"d":"10.76"}]
{"$rows_empty":45}
[" Total Carried Forward To Summary"]
[]
[null,null,9]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 2200"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[22,"PREFABRICATED CULVERTS"]
[]
["22.01","Excavation"]
[]
[null,"(a) Excavating soft material situated within the"]
[null,"     following depth ranges below the surface level:"]
[null,"       "]
[null,"      (i) 0 m up to 1.5 m","m³",{"v":504,"d":"504.00"}]
[]
[null,"      (ii) Exceeding 1,5 m and up to 3,0 m","m³",{"v":151.2,"d":"151.20"}]
[]
[null,"(b) Extra over subitem 22.01(a) for excavation","m³",{"v":100.80000000000001,"d":"100.80"}]
[null,"in hard material, irrespective of depth"]
[]
["22.02","Backfilling:"]
[]
[null,"(a) Using the excavated material","m³",{"v":504,"d":"504.00"}]
[]
[null,"(b) Using imported selected material","m³",{"v":100.80000000000001,"d":"100.80"}]
[]
[null,"(c) Extra over subitems 22.02(a) and (b)"]
[null,"for soil cement backfilling with 4% cement","m³",13.97]
[]
["22.05","Portal and rectangular culverts"]
[]
[null,"a) Complete with prefabricated floor slabs:"]
[]
[null,"      (i) 1200mm x 600mm box culverts","m",null,null,"Rate Only"]
[]
[null,"b) Without prefabricated floor slabs:"]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[null,"      (i) 750mm x 750mm box culverts","m",18]
[]
[null,"      (ii) 900mm x 600mm box culverts","m",10]
[]
[null,"      (iii) 900mm x 750mm box culverts","m",18]
[]
[null,"      (iv) 900mm x 900mm box culverts","m",18]
[]
[null,"      (v) 1500mm x 900mm box culverts","m",18]
[]
[null,"      (vi) 2000mm x 1500mm box culverts","m",18]
[]
["22.07","Cast in in-situ concrete and formwork"]
[]
[null,"(b) In floor slabs for portal or rectangular culverts,"]
[null,"including formwork, joints and class U2 surface "]
[null,"finish:"]
[null,"                   (i) Class 25/19","m³",{"v":120,"d":"120.00"}]
[]
[null,"(c) In inlet and outlet structures, skewed"]
[null,"ends, catchpits, manholes, thrust and anchor"]
[null,"blocks, excluding formwork but including class U2"]
[null,"surface finish:"]
[null,"                   (i) Class 25/19","m³",{"v":120,"d":"120.00"}]
[]
[null,"(d) Formwork of concrete under subitem 22.07(a) "]
[null,"and (c)  above:"]
[]
[null,"      (i) Vertical formwork for F1 surface finish","m²",{"v":11.6765,"d":"11.68"}]
[]
[null,"      (ii) Vertical formwork for F2 surface finish","m²",{"v":6.6979,"d":"6.70"}]
[]
["22.08","Concrete backfill for culverts:"]
[null,"                  (i) Class 15/19","m³",{"v":72,"d":"72.00"}]
[]
["22.10","Steel reinforcement:"]
[]
[null,"     (b) High steel bars:"]
[]
[null,"             (i) Y12 steel bar","t",{"v":3,"d":"3.00"}]
[]
[null,"            (ii) Y16 steel bar ","t",{"v":3,"d":"3.00"}]
[]
[null,"     (c) Welded steel fabric (mesh-Ref 395)","kg",100]
[]
[]
[]
[]
[]
["Total Carried Forward"]
[]
[null,null,10]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 2200"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[{"$nulls":5},"R"]
[]
["Brought Forward"]
[]
[]
[]
["22.12","Removing existing concrete"]
[]
[null,"     (a) Plain concrete","m³",{"v":50,"d":"50.00"}]
[]
[null,"     (b) Reinforced concrete","m³",{"v":80,"d":"80.00"}]
[]
["22.14","Removing and stacking existing prefabricated"]
[null,"culverts"]
[]
[null,"(a) 450mm box culverts","m",{"v":40,"d":"40.00"}]
{"$rows_empty":56}
[" Total Carried Forward To Summary"]
[]
[null,null,11]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 2300"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[23,"CONCRETE KERBING, CONCRETE"]
[null,"CHANNELLING, CHUTES AND"]
[null,"DOWNPIPES, AND CONCRETE"]
[null,"LININGS FOR OPEN DRAINS"]
[]
["23.01","Concrete kerbing"]
[]
[null," (a) Pre-cast mountable kerb (Fig 8C) complete"]
[null,"with excavations, trimming, bedding and haunching","m",7500]
[]
[null," (b) Pre-cast mountable kerb (Fig 7 ) ","m",null,null,"Rate Only"]
[]
["23.07","Trimming of Excavations for concrete-lined"]
[null,"open drains:"]
[]
[null,"     (a) In soft material","m²",{"v":1687.5,"d":"1687.50"}]
[]
[null,"     (b) In hard material","m²",{"v":337.5,"d":"337.50"}]
[]
["23.08","Concrete lining for open drains"]
[]
[null,"     (a) Cast in situ concrete lining class 30/19:"]
[null,"               (i) Type F1","m³",null,null,"Rate Only"]
[null,"               (ii) Type F2 (1,5 m wide)","m³",{"v":1687.5,"d":"1687.50"},null,null,{"v":1313550,"d":"1,313,550.00"},5620]
[null,"               (iii) Type F3","m³",null,null,"Rate Only"]
[null,"               (iv) Type F4","m³",null,null,"Rate Only"]
[]
[null,"     (b) Class U2 surface finish to cast in situ"]
[null,"      concrete for type F3 open drain","m²",{"v":9112.5,"d":"9112.50"}]
[]
["23.09","Formwork to cast in situ concrete lining"]
[null,"for open drains (Class F1 surface finish):"]
[]
[null,"     (a) To sides with formwork on the"]
[null,"      internal face only","m²",null,null,"Rate Only"]
[]
[null,"     (b) To sides with formwork on both"]
[null,"      internal and external faces (each"]
[null,"      face measured)","m²",{"v":2278.125,"d":"2278.13"}]
[]
["23.10","Sealed joints in concrete linings of open "]
[null,"drains and concrete kerbing:"]
[]
[null,"     (a) Silicone joint sealant (Bostic 22DS100"]
[null,"         highway sealant or approved equivalent) "]
[null,"         in expansion joints, 15mm wide and ","m",{"v":1125,"d":"1125.00"}]
[null,"         10mm deep"]
[]
["23.12","Steel reinforcement:"]
[]
[null,"    (c) Welded steel fabric:"]
[null,"               (i) Ref 193","kg",{"v":21712.5,"d":"21712.50"}]
{"$rows_empty":13}
[" Total Carried Forward To Summary"]
[]
[null,null,12]
[]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 3100"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[31,"BORROW MATERIALS"]
[]
["31.01","Excess overburden","m³",{"v":4500,"d":"4500.00"}]
[]
["31.03","Rehabilitation of Borrowpit ","Prov Sum",{"v":1,"d":"1.00"},{"v":500000,"d":"R 500,000.00"},{"v":500000,"d":"500,000.00"}]
[]
[null,"(f) Handling cost and profit"]
[null,"    in respect of sub-item 31.03","%",{"v":500000,"d":"500000.00"}]
{"$rows_empty":58}
[" Total Carried Forward To Summary"]
[]
[null,null,13]
[]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 3300"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[33,"MASS EARTHWORKS"]
[]
["33.04","Cut to spoil, including free-haul up to 0,5"]
[null,"km. Material obtained from:"]
[{"$nulls":7},"ROAD",26586]
[null,"(a) Soft excavation","m³",{"v":1458,"d":"1458.00"},{"$nulls":3},"INTERSECTION",6120]
[{"$nulls":7},"BELL MOUTHS",831.6]
[null,"(b) Intermediate excavation","m³",{"v":7290,"d":"7290.00"}]
[]
[null,"(c) Hard excavation","m³",{"v":18225,"d":"18225.00"}]
[]
[null,"(d) Boulder Excavation Class A","m³",{"v":4374,"d":"4374.00"}]
[]
[null,"(e) Boulder Excavation Class B","m³",{"v":874.8000000000001,"d":"874.80"}]
[]
["33.10","Roadbed preparation and the"]
[null,"compaction of material"]
[]
[null,"(b) Compaction to 93% of modified"]
[null,"      AASHTO density","m³",{"v":9112.5,"d":"9112.50"}]
[]
["33.12","In situ treatment of roadbed"]
[]
[null,"(a) In situ treatment by ripping","m³",null,null,"Rate Only"]
[null,"(b) In situ treatment by blasting","m³",{"v":4374,"d":"4374.00"}]
[]
["B33.20","Overhaul on material hauled in excess"]
[null,"of a freehaul distance of 0.5km, for haul"]
[null,"up to or through 0,5km (restricted)","m³",20667.15]
[]
["B33.21","Overhaul on material hauled in excess"]
[null,"of 1.0km (ordinary overhaul)","m³-km",{"v":206671.5,"d":"206671.50"}]
[]
["B33.22","Rock fill","Prov Sum",{"v":1,"d":"1.00"},{"v":850000,"d":"R 850,000.00"},{"v":850000,"d":"850,000.00"},935000]
[]
[null,"(a) Handling cost and profit ","%",{"v":850000,"d":"850000.00"}]
{"$rows_empty":30}
[" Total Carried Forward To Summary"]
[]
[null,null,14]
[]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 3400"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[34,"PAVEMENT LAYERS OF GRAVEL"]
[null,"MATERIAL"]
[]
["34.01","Pavement layers constructed from",{"$nulls":5},2550000]
[null,"gravel taken from cut or borrow,"]
[null,"including free-haul up to 1,0 km (Including bus stops):"]
[]
[null,"    (a) Gravel selected layer compacted to:"]
[]
[null,"            (ii) 95% of Modified AASHTO density"]
[null,"                 (upper selected layer)","m³",{"v":9112.5,"d":"9112.50"}]
[]
[null,"            (iii) 95% of modified AASHTO density"]
[null,"                  (lower selected layer)","m³",null,null,"Rate Only"]
[]
[]
[null,"    (c) Gravel subbase layer (unstabilised)"]
[null,"     compacted to:"]
[]
[null,"      (iii) 97 % of modified AASHTO density (Including bus stops)","m³",8201.25]
[]
[null,"     (f) Gravel base (chemically stabilised material)"]
[null,"      compacted to:"]
[]
[null,"             (ii) 98 % of modified AASHTO density (Including bus stops)","m³",{"v":7290,"d":"7290.00"}]
[]
[]
[null,"     ( c) Construct a pioneer layer","Prov Sum",{"v":1,"d":"1.00"},{"v":3200000,"d":"R 3,200,000.00"},{"v":3200000,"d":"3,200,000.00"}]
[]
[null,"(d) Handling cost and profit","%",{"v":3200000,"d":"3200000.00"}]
[]
["B34.15","Overhaul on material hauled in excess"]
[null,"of 1.0km (ordinary overhaul)","m³-km",{"v":9112.5,"d":"9112.50"}]
{"$rows_empty":41}
[" Total Carried Forward To Summary"]
[]
[null,null,15]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 3500"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[{"$nulls":7},297.525825]
[35,"STABILISATION",{"$nulls":5},272.73200625000004]
[{"$nulls":7},52.6428]
["35.02","Chemical Stabilisation Agent",{"$nulls":5},47.0025]
[{"$nulls":7},9.306495]
[null,"(a) Ordinary portland cement","ton",{"v":380.72025,"d":"380.72"},{"$nulls":3},8.530953749999998]
[{"$nulls":7},687.7405799999999]
{"$rows_empty":63}
[" Total Carried Forward To Summary"]
[]
[16]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 4100"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[41,"PRIME COAT"]
[]
["B41.01","Prime coat:"]
[]
[null,"MSP1 at an application rate of 0,75 l/m²","litre",null,null,"Rate Only"]
[]
["41.03","Extra over item B41.01 for applying the"]
[null,"prime coat in areas accessible only to"]
[null,"hand held equipment","litre",null,null,"Rate Only"]
{"$rows_empty":59}
[" Total Carried Forward To Summary"]
[]
[17]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 4200"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[42,"ASPHALT BASE AND SURFACING"]
[]
["42.02","Asphalt surfacing "]
[]
[null,"(a) Continuously graded"]
[]
[null,"     (i) 30mm nominal thickness","m²",null,null,"Rate Only"]
[]
["42.04","Tack coat of 30% stable-grade emulsion "]
[null,"at an application rate of 0,6 l/m²","litre",null,null,"Rate Only"]
[]
["42.08","100 mm cores in asphalt paving","No",null,null,"Rate Only"]
[]
["B42.21","Construction of speed humps using asphalt","No",null,null,"Rate Only"]
[]
["B42.22","Road crossing to install culverts","PC Sum",null,null,"Rate Only"]
[]
["B42.23","Handling cost and profit in respect to sub-item B42.22","%",null,null,"Rate Only"]
{"$rows_empty":40}
[" Total Carried Forward To Summary"]
[]
[18]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 5100"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[51,"PITCHING, STONEWORK AND"]
[null,"PROTECTION AGAINST EROSION"]
[]
["51.01","Stone pitching (complete with excavations"]
[null,"trimming and compaction)"]
[]
[null,"      (b) Grouted stone pitching","m²",{"v":400,"d":"400.00"}]
[]
["51.05","Concrete edge beams"]
[]
[null,"      (a) Class 30/19","m³",{"v":300,"d":"300.00"}]
{"$rows_empty":59}
[" Total Carried Forward To Summary"]
[]
[19]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["5200"]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT","PREV.","PRES.","TOTAL","AMOUNT"]
[{"$nulls":5},"R","(Qty)","(Qty)","(Qty)","(Rand)"]
[]
[]
["5200","GABIONS"]
[]
["B52.01","Foundation trench excavation and backfilling:"]
[]
[null,"(a) In solid rock (material which requires blasting)","m³",67.5,null,0,100,0,100,0]
[]
[null,"(b) In all other classes of materials","m³",50,null,0,50,0,50,0]
[]
["B52.02","Surface preparation for bedding the gabions","m²",15,null,0,15,0,15,0]
[]
["B52.03","Gabions:"]
[]
[null,"(a) Galvanized gabion boxes"]
[]
[null,"(1) 1,0 m wide by 0,3 m deep"]
[]
[null,"(i) by 1,0 m long mesh ........","m³",67.5,null,0,50,0,50,0]
[]
[null,"(ii) by 2,0 m long mesh ........","m³",null,null,"Rate Only"]
[]
[null,"(iii) by 3,0 m long mesh ........","m³",null,null,"Rate Only"]
[]
[null,"(iv) by 4,0 m long mesh ........","m³",null,null,"Rate Only"]
[]
[null,"(b) PVC-coated gabion boxes (2000mm x 1000mm x 500mm with hexagon woven mesh wire)","m³",10,null,0,30,0,30,0]
[]
[null,"(c) PVC-coated gabion mattresses (2000mm x 1000mm x 500mm with hexagon woven mesh wire) ","m³",10,null,0,30,0,30,0]
{"$rows_empty":20}
[" TOTAL CARRIED FORWARD TO SUMMARY",{"$nulls":8},0]
[]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 5500"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[55,"FENCING"]
[]
["55.01","Clearing the fence line, 2 m wide strip","Prov sum",{"v":1,"d":"1.00"},{"v":50000,"d":"R 50,000.00"},{"v":50000,"d":"50,000.00"}]
[]
["55.02","Supply and erect new fencing material for new"]
[null,"fences and for supplementing material in existing","Prov Sum",{"v":1,"d":"1.00"},{"v":350000,"d":"R 350,000.00"},{"v":350000,"d":"350,000.00"}]
[null,"fences which are being repaired or removed:"]
[]
[null,"(i) Handling cost and profit in respect to "]
[null,"items 55.01 and 55.02","%",{"v":400000,"d":"400000.00"}]
{"$rows_empty":59}
[" Total Carried Forward To Summary"]
[]
[20]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 5600"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[56,"ROAD SIGNS"]
[]
["56.01","Road sign boards with painted or"]
[null,"coloured semi-matt background."]
[null,"Symbols, lettering and borders in semi-"]
[null,"matt black or in Class 1 retro-reflective"]
[null,"material, where the sign board is"]
[null,"constructed from:"]
[]
[null,"(c) Prepainted galvanized steel plate"]
[null,"      (chromadek 1,6 mm thick or"]
[null,"      approved equivalent):"]
[]
[null,"            (i) Area not exceeding 2 m²","m²",77.19]
[]
[null,"(d) Prepainted galvanized steel profiles"]
[null,"      (200 mm high chromadek or"]
[null,"      approved equivalent):"]
[]
[null,"            (i) Area not exceeding 2 m²","m²",{"v":16,"d":"16.00"}]
[]
[null,"            (ii) Area exceeding 2 m² but not 10 m²","m²",{"v":16,"d":"16.00"}]
[]
["56.02","Extra over item 56.01 for using:"]
[]
[null,"(a) Background of retro-reflective"]
[null,"      material of:"]
[]
[null,"             (ii) Class III","m²",77.19]
[]
[null,"(b) Lettering, symbols, numbers, arrows,"]
[null,"      emblems and borders of retro-"]
[null,"      reflective material:"]
[]
[null,"             (ii) Class III","m²",{"v":46.314,"d":"46.31"}]
[]
["56.03","Road sign supports  (overhead road"]
[null,"sign structures excluded):"]
[]
[null,"(a) Steel tubing (75mm diameter galvanised)","t",{"v":2.61633719424,"d":"2.62"},null,{"v":0,"d":"0.00"}]
[]
["56.05","Excavation and backfilling for road sign"]
[null,"supports (not applicable to kilometre"]
[null,"posts)","m³",{"v":2.8486079999999996,"d":"2.85"},null,{"v":0,"d":"0.00"}]
[]
["56.06","Extra over item 56.05 for cement-"]
[null,"treated soil backfill","m³",{"v":1.0173599999999998,"d":"1.02"},null,{"v":0,"d":"0.00"}]
[]
["B56.10","Danger plates:"]
[]
[null,"(a)    Type A (at bridges):  1200mm X 300mm","No.",null,null,"Rate Only"]
[]
[null,"(b)    Type B (at culverts):  600mm x 150mm","No.",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"}]
{"$rows_empty":15}
[" Total Carried Forward To Summary"]
[]
[null,null,21]
[]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 5700"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[57,"ROAD MARKINGS"]
[]
["57.02","Retro-reflective road marking paint:"]
[]
[null,"(a) White lines (broken or unbroken):"]
[]
[null,"      (i) 150 mm wide","km",{"v":6.37875,"d":"6.38"}]
[]
[null,"      (ii) 200 mm wide","km",{"v":6.98625,"d":"6.99"}]
[]
[null,"      (iii) 300 mm wide","m²",{"v":270,"d":"270.00"}]
[]
[null,"(b) Yellow lines (broken or unbroken):"]
[]
[null,"      (i) 100 mm wide","km",{"v":12.7575,"d":"12.76"}]
[]
[null,"      (ii) 300 mm wide","m²",{"v":270,"d":"270.00"}]
[]
[null,"(d) White lettering and symbols","m²",{"v":258.885,"d":"258.89"}]
[null,"    "]
[null,"(e) Yellow lettering and symbols","m²",{"v":12.629999999999999,"d":"12.63"}]
[]
[null,"(f) Transverse lines, painted island and arrestor "]
[null,"bed markings (yellow)","m²",1.08]
[]
["57.06","Setting out and premarking the lines"]
[null,"(Excluding traffic-island markings,"]
[null,"lettering and symbols)","km",{"v":6.682500000000001,"d":"6.68"}]
[]
["57.07","Re-establishing the painting unit at the"]
[null,"end of the maintenance period","Lump Sum",{"v":1,"d":"1.00"}]
{"$rows_empty":36}
[" Total Carried Forward To Summary"]
[]
[null,null,22]
[]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 5900"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[59,"FINISHING THE ROAD AND ROAD"]
[null,"RESERVE AND TREATING OLD"]
[null,"ROADS"]
[]
["59.01","Finishing the road and road reserve:"]
[]
[null,"(b) Single carriageway road","km",{"v":6.075,"d":"6.08"}]
{"$rows_empty":62}
[" Total Carried Forward To Summary"]
[]
[23]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 7300"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
["73 LI","CONCRETE PAVING FOR ROADS"]
[]
["73,01 LI","80mm interlocking concrete block paving "]
[null,"complate with bedding sand, laying, filling sand,"]
[null,"compaction and cleaning (Including bus stops)","m²",42600]
[]
[null,"Bedding sand to receive block paving","m³",852]
[]
[null,"Jointing sand for sealing joints","m³",{"v":340.8,"d":"341"}]
[]
["73,03 LI","Provision of approved herbicide and ant poison"]
[]
[null,"(a) Provision of materials","PC Sum",{"v":1,"d":"1.00"},{"v":20000,"d":"R 20,000.00"},{"v":20000,"d":"R 20,000.00"}]
[]
[null,"(b) Contractor's charges and profit added to the prime cost sum","%",{"v":20000,"d":"20000.00"}]
[]
["B73,04","Construction of speed humps","No",{"v":8,"d":"8.00"}]
{"$rows_empty":52}
[" Total Carried Forward To Summary"]
[]
[]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["  ROADWORKS"]
["SECTION 8100"]
[]
[]
["ITEM","DESCRIPTION","UNIT","QTY","RATE","   AMOUNT"]
[{"$nulls":5},"R"]
[]
[]
[81,"TESTING MATERIALS AND"]
[null,"WORKMANSHIP"]
[]
["B81.04","Testing of materials"]
[]
[null,"(a) Testing as required by the engineer","Prov. Sum",{"v":1,"d":"1.00"},{"v":400000,"d":"R 400,000.00"},{"v":400000,"d":"400,000.00"}]
[]
[null,"(b) Handling cost and profit","%",{"v":400000,"d":"400000.00"}]
{"$rows_empty":58}
[" Total Carried Forward To Summary"]
[]
[null,null,24]
[]
[]
[]
["Elias Motsoaledi Local Municipality"]
["CONTRACT: EMLM 04/2024 Upgrading of Mokumong Access road to Marateng Taxi Rank and Stormwater Control"]
["ROADWORKS"]
["SUMMARY OF SECTIONS        "]
[]
["SECTION","DESCRIPTION",null,"AMOUNT (RAND)"]
[]
[]
["PART A","SCHEDULE A: ROADWORKS"]
[]
[1200,"GENERAL REQUIREMENTS AND PROVISIONS"]
[]
[]
[1300,"CONTRACTOR'S ESTABLISHMENT ON SITE AND GENERAL"]
[null,"OBLIGATIONS"]
[]
[1400,"HOUSING, OFFICES AND LABORATORY FOR THE"]
[null,"ENGINEER'S SITE PERSONNEL"]
[]
[1500,"ACCOMODATION OF TRAFFIC"]
[]
[1700,"CLEARING AND GRUBBING"]
[]
[2100,"DRAINS"]
[]
[2200,"PREFABRICATED CULVERTS"]
[]
[2300,"CONCRETE KERBING, CONCRETE CHANNELLING,  CHUTES"]
[null,"AND DOWNPIPES, AND CONCRETE LINNING FOR OPEN DRAINS"]
[]
[3100,"BORROW MATERIALS"]
[]
[3300,"MASS EARTHWORKS"]
[]
[3400,"PAVEMENT LAYERS OF GRAVEL MATERIAL"]
[]
[3600,"STABILISATION"]
[]
[4100,"PRIME COAT"]
[]
[4200,"ASPHALT BASE AND SURFACING"]
[]
[5100,"PITCHING, STONEWORK AND PROTECTION AGAINST EROSION"]
[]
[5200,"GABIONS"]
[]
[5500,"FENCING"]
[]
[5600,"ROAD SIGNS"]
[]
[5700,"ROAD MARKINGS"]
[]
[5900,"FINISHING THE ROAD AND ROAD RESERVE AND TREATING OLD"]
[null,"ROADS"]
[]
[7300,"CONCRETE PAVING FOR ROADS"]
[]
[8100,"TESTING MATERIALS AND WORKMANSHIP"]
[]
[{"$nulls":8},46368452.05810521]
[]
[]
[]
[]
[null,"SUBTOTAL 1"]
[null,null,"ADD  3% CPA"]
[null,null,"SUBTOTAL 2"]
[null,"ADD 5% CONTIGENCIES"]
[]
[null,"SUBTOTAL 3"]
[{"$nulls":6},0]
[null,"ADD 15% VAT",{"$nulls":6},{"v":10000000,"d":"10,000,000.00"}]
[]
["TOTAL CONSTRUCTION COST "]
{"$rows_empty":8}
[{"$nulls":11}," "]
[]
[]
[]
[]
[25]
{"$rows_empty":35}
[150]