{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["A&B Schedules","Deviation Schedule","Test Schedule"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"A&B Schedules","index":0,"n_rows":65,"n_cols":26,"rows_kept":65,"merged":[[0,0,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,0,4,6],[5,2,5,4],[5,5,5,6],[6,2,6,4],[6,5,8,6],[7,2,7,4],[8,2,8,4],[9,1,9,6],[11,1,11,6],[12,1,12,6],[15,2,15,3],[16,2,16,3],[17,3,17,4],[24,3,24,4],[34,3,34,4],[37,2,37,4],[38,2,38,5],[39,3,39,4],[41,3,41,4],[45,3,45,4],[53,0,53,6],[54,1,55,6],[57,0,57,6],[59,0,59,1],[64,2,64,3]]}
["ESKOM TENDER E2719DXLIMOU"]
[null,"Technical Schedules A and B for"]
[null," D-DT-3163 -BI Metal Lug"]
[null,"NB. UNIQUE SCHEDULES ARE TO BE COMPLETED PER SAP NUMBER LISTED BELOW "]
["NB. SUPPLIERS TO CONFIRM ADHERENCE TO THE LATEST PUBLISHED REVISION OF ALL APPLICABLE ESKOM DRAWINGS"]
[null,"Sap Number","Description",null,null,"SANS Specification"]
[null,554113,"CONNECTOR,LUG:AL/CU FOX/35 M12 0 DEG",null,null,"SANS 61284"]
[null,554114,"CONNECTOR,LUG:AL/CU MINK/PINE M12 0 DEG"]
[null,554115,"CONNECTOR,LUG:AL/CU OAK/HARE M12 0 DEG"]
[{"$nulls":21},3116,6,215200,"LUG,CRIMP PRE-INSUL 54.6 SQ ABC D3116","CABLE ACCESSORIES - LUGS AND FERRULES"]
[{"$nulls":21},3116,6,165667,"LUG,CRIMP PRE-INSUL 70 SQ ABC D3116"]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,"Requirements","Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No (Select from the drop down)",554115,"xxxxxxxxxx"]
[null,"1.1.2",null,"Description",{"$f":"IF(E19=B7,C7,IF(E19=B8,C8, IF(E19=B9,C9)))","v":"CONNECTOR,LUG:AL/CU OAK/HARE M12 0 DEG"},"xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer","Manufacturer name","xxxxxxxxxx"]
[null,"1.1.3",null,"Manufacturer's Product Code","Specify Code","xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Drawing number & Revision number","Specify No and Rev","xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's physical unique identifier and knurl marks indelibly marked on product body","Specify markings","xxxxxxxxxx"]
[null,"1.2","·","Compliance to Eskom Buyer's Guide Drawings"]
[null,"1.2.1",null,"Terminal Lug , Compression, Pre-Insulated and Bi-Metal (Aluminium to Cupper)"," Eskom D DT-3163","YES"]
[null,"1.2.2",null,"Bimetal","Aluminium To Copper"]
[null,"1.2.3",null,"Conductor Connection: ","Crimp Compression Circumferential"]
[null,"1.2.4",null,"Palm Hole","Fitted With A Copper Insert"]
[null,"1.2.5",null,"Conductor",{"$f":"IF(E19=B7,\"Fox 8.37mm OR (35) 8.31mm\",IF(E19=B8,\"Mink10.98mm or Pine 10.83mm\", IF(E19=B9,\"Oak 13.95mm or Hare 14.16mm\")))","v":"Oak 13.95mm or Hare 14.16mm"}]
[null,"1.2.6",null,"Palm Hole Bolt Clearance  ","M12","YES"]
[null,"1.2.7",null,"Lug angle",0,"YES"]
[null,"1.2.8",null,"Filled with jointing compound and capped "," Eskom DDT-3163","YES"]
[null,"1.2.9",null,"For use with hydraulic crimping tool and Die size",{"$f":"IF(E25=B14,\"699\",IF(E25=B13,558,IF(E25=B15,554)))","v":"699"},"YES"]
[null,"1.3","·","Mechanical Properties",{"$nulls":14},"(add this as a requirement for compliance with DDT3116)"]
[null,"1.3.1",null,"Material ( Aluminium and copper) - Bi-metal fitting as per buyers guide drawing"," Eskom DDT-3163","YES"]
[null,"1.3.2",null,"Material compound -  Electrical jointing compound as per buyers guide drawing"," Eskom DDT-3163","YES"]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to also be provided in electronic format."]
[null,"2.1","·","General"]
[null,"2.1.1",null,"Approved Manufacturer Drawings showing markings and dimensions","1 Set submitted","YES"]
[null,"2.2","·","Test Reports (Iin accordance with SANS 50483- 4,5 and 6)",null,"Required"]
[null,"2.2.1",null,"Has the relevant signed mandatory test schedule been submitted.","Signed Test Schedule Submitted ","YES"]
[null,"2.2.2",null,"Are all non-metallic components to satisfy the glow-wire test requirements."," As per  IEC 695-2-1/1","YES/NO"]
[null,"2.2.3",null,"Type test at min failing load and certificate valid sample test certificate to be provided for the production run associated with each delivery","Signed Test Report Submitted ","YES/NO"]
[null,3,null,"Packaging"]
[null,"3.1",null,"Individually sealed ","each","Individually sealed "]
[null,"3.2",null,"Corrosion and mechanical damage protection",null,"Yes/No"]
[null,"3.3",null,"Information to appear on a bulk package\n• the name of the manufacturer;\n• the fitting reference and size;\n• the number of fittings per package;\n• the purchaser's order number; and\n• The date of manufacture.\n",null,"Yes"]
[null,"3.4",null,"Packaging material, method and maximum quantity, not exceeding 30kg.",null,"Supplier to provide details"]
[null,"3.5",null,"Markings to be stipulated.",null,"Supplier to provide details"]
[null,"3.6",null,"Installation instructions provided in packaging.",null,"YES"]
[]
["ESKOM TENDER E2719DXLIMOU"]
[null,"Deviations to any of the stated requirements are to be captured on the Deviation Schedule."]
[]
[]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":46,"n_cols":6,"rows_kept":46,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[2,7,2,13],[2,14,2,20],[2,21,2,27],[2,28,2,34],[2,35,2,41],[2,42,2,48],[2,49,2,55],[2,56,2,62],[2,63,2,69],[2,70,2,76],[2,77,2,83],[2,84,2,90],[2,91,2,97],[2,98,2,104],[2,105,2,111],[2,112,2,118],[2,119,2,125],[2,126,2,132],[2,133,2,139],[2,140,2,146],[2,147,2,153],[2,154,2,160],[2,161,2,167],[2,168,2,174],[2,175,2,181],[2,182,2,188],[2,189,2,195],[2,196,2,202],[2,203,2,209],[2,210,2,216],[2,217,2,223],[2,224,2,230],[2,231,2,237],[2,238,2,244],[2,245,2,251],[2,252,2,255],[3,0,3,6],[3,7,3,13],[3,14,3,20],[3,21,3,27],[3,28,3,34],[3,35,3,41],[3,42,3,48],[3,49,3,55],[3,56,3,62],[3,63,3,69],[3,70,3,76],[3,77,3,83],[3,84,3,90],[3,91,3,97],[3,98,3,104],[3,105,3,111],[3,112,3,118],[3,119,3,125],[3,126,3,132],[3,133,3,139],[3,140,3,146],[3,147,3,153],[3,154,3,160],[3,161,3,167],[3,168,3,174],[3,175,3,181],[3,182,3,188],[3,189,3,195],[3,196,3,202],[3,203,3,209],[3,210,3,216],[3,217,3,223],[3,224,3,230],[3,231,3,237],[3,238,3,244],[3,245,3,251],[3,252,3,255],[4,0,4,6],[5,2,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[34,2,34,6],[35,2,35,6],[37,0,37,6],[38,0,38,6],[40,0,40,1],[41,2,41,3],[45,2,45,3]]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation schedule"]
[{"$f":"'A&B Schedules'!B3","v":" D-DT-3163 -BI Metal Lug"}]
["SAP No: 0554115"]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":31}
["ESKOM TENDER E2719DXLIMOU"]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[null,null,"Name (Print)",null,null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Test Schedule","index":2,"n_rows":23,"n_cols":6,"rows_kept":23,"merged":[[1,0,1,7],[2,0,2,7],[3,1,3,5],[4,0,4,7],[14,1,14,8],[15,1,15,8],[18,1,18,2],[22,1,22,2]]}
[null,null,"ESKOM TENDER E2719DXLIMOU"]
["Test Report Schedule"]
[{"$f":"'A&B Schedules'!B3","v":" D-DT-3163 -BI Metal Lug"}]
[null,"The test reports are required for the selected SAP number listed on this sheet."]
["SAP No:  0554115"]
[]
[null,1,2,3,4,5]
[null,"Item ","Description","Standard","Clause ","Report No."]
[null,1,"Dimension and Material verification","SANS 61284",8]
[null,2,"Damage and Failure load test","SANS 61284","11.3.1"]
[null,3,"Tensile test","SANS 61284","11.5.1"]
[null,4,"Heat cycle test","SANS 61284",13]
[null,5,"Short-circuit test","SANS 61284","13.2.2"]
[null,6,"Corrosion test","SANS 61284"]
[]
[null,"SUPPLIER SIGNATURES"]
[]
[]
[null,"Name (Print)",{"$nulls":3},"Company name"]
[]
[]
[]
[null,"Sign",{"$nulls":3},"Date"]