{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":274,"n_cols":7,"rows_kept":274}
["Item","Description (refer to Works Specification for works details)","Quantity","Unit of measure ","Contract Scope of Work","Rate","ToTal"]
[1,"Panel Decommissioning"]
["1.1","Automatic Relay Panel 1800(H) x 2700(W) x 900(D)",2,"items","Remove"]
["1.2","Turbine Gauge Board 1800(H) x 2400(W) x 600(D)",2,"items","Remove"]
["1.3","Digital Governor 1395(H) x 900(W) x 550(D) ",2,"items","Remove"]
["1.4","Supervisory Relay Panel 1800(H) x 600(W) x 600(D)",2,"items","Remove"]
["1.5","Maxi flex 1395(H) x 900(W) x 550(D) ",2,"items","Remove"]
["1.6","Interbud 1395(H) x 900(W) x 550(D) ",2,"items","Remove"]
["1.7","Unit Control Console",2,"items","Remove"]
["1.8","Station Control Console",1,"items","Remove"]
["1.9","Solenoid Drives 1800(H) x 900(W) x 600(D)",2,"items","Remove"]
[2,"Cable Decommissioning"]
["2.1","BVS4BCV",6000,"meters","Remove"]
["2.2","BVS12BCV",5000,"meters","Remove"]
["2.3","BVS20BCV",4000,"meters","Remove"]
["2.4","BVX2DCV",400,"meters","Remove"]
["2.5","BVX7DCV",200,"meters","Remove"]
["2.6","BVX12DCV",400,"meters","Remove"]
["2.7","BVX2ECV",3000,"meters","Remove"]
["2.8","BVX3ECV",300,"meters","Remove"]
["2.9","BVX4ECV",100,"meters","Remove"]
["2.10","BVX2HCV",1000,"meters","Remove"]
["2.11","BVX4HCV",200,"meters","Remove"]
["2.12","TVH10BV",2000,"meters","Remove"]
[3,"Instrumentation Decommissioning"]
["3.1","Pressure transmitter",26,"items","Remove"]
["3.2","Pressure switch",30,"items","Remove"]
["3.3","Level instrument",34,"items","Remove"]
["3.4","Flowmeter",20,"items","Remove"]
["3.5","Temperature switch",12,"items","Remove"]
["3.6","Copper pipe tubing ",5000,"meters","Remove"]
["3.7","Junction Boxes",10,"items","Remove"]
[4,"Cable Trays"]
["4.1","Welded (HDG) galvanised Wire mesh trays 50X50mm comes with joiner sets",2000,"meters","Supply and install"]
["4.2","Welded (HDG) galvanised Wire mesh trays 114X50mm comes with joiner sets",2000,"meters","Supply and install"]
["4.3","Medium duty (HDG) galvanised perforated tray (MCT75) 114x38x1.6mm",1000,"meters","Supply and install"]
["4.4","Medium duty (HDG) galvanised perforated tray (MCT300) 305x76x1.6mm",1000,"meters","Supply and install"]
["4.5","Heavy duty (HDG) galvanised perforated tray (MCT75) 76x38x1.6mm",500,"meters","Supply and install"]
["4.6","Heavy duty (HDG) galvanised perforated tray (MCT450) 457x76x1.6mm ",1000,"meters","Supply and install"]
["4.7","Bosal Conduit - 20mm",200,"meters","Supply and install"]
["4.8","Raised Hospital Saddles – 20mm",500,"each","Supply and install"]
[5,"Earthing"]
["5.1","Twisted bare copper earthing wire 16 mm sq.",4000,"meters","Supply and install"]
["5.2","Copper bar 25x2.5mm",100,"meters","Supply and install"]
[6,"Cabling"]
["6.1","BVV2DCM",2000,"meters","Supply and install"]
["6.2","BVV3ECM",500,"meters","Supply and install"]
["6.3","BVV4DCM",500,"meters","Supply and install"]
["6.4","BVX4DCM",500,"meters","Supply and install"]
["6.5","BVV4ECM",500,"meters","Supply and install"]
["6.6","BVX4ECM",500,"meters","Supply and install"]
["6.7","UVG2ACM",10000,"meters","Supply and install"]
["6.8","UVG02BCM",2000,"meters","Supply and install"]
["6.9","UVG02CCM",1000,"meters","Supply and install"]
["6.10","UVG04ACM",1000,"meters","Supply and install"]
["6.11","UVG04BCM",500,"meters ","Supply and install"]
["6.12","UVG08ACM",4000,"meters","Supply and install"]
["6.13","UVG12ACM",4000,"meters","Supply and install"]
["6.14","UVG20ACM",500,"meters","Supply and install"]
["6.15","UVH02BCM",500,"meters","Supply and install"]
["6.16","UVK01BCM",4000,"meters","Supply and install"]
["6.17","UVM12BCM",1000,"meters","Supply and install"]
["6.18","Heavy Duty Duct Multi-Mode F/O 8core",2000,"meters","Supply and install"]
["6.19","RG58 co-axial cable, outdoor GPS antenna cable",200,"meters","Supply and install"]
["6.20","Ruggedised MM F/O 25m Patch lead (2 core, ST-LC) ",10,"each","Supply and install"]
["6.21","Ruggedised MM F/O 25m Patch lead (2 core, ST-ST)",6,"each","Supply and install"]
[7,"Control Panels and Junction Boxes Installation"]
["7.1","Unit 1 and 2 Main Unit Controller Local",4,"items","Install"]
["7.2","Unit 1 and 2 Main Unit Controller Remote IO Generator",2,"items","Install"]
["7.3","Unit 1 and 2 Main Unit Controller Remote IO Turbine",2,"items","Install"]
["7.4","Unit 1 and 2 Main Unit Controller Remote IO Common",2,"items","Install"]
["7.5","Unit 1 and 2 Digital Governor ",2,"items","Install"]
["7.6","Unit 1 and 2 Temperature and Speed Monitoring",4,"items","Install"]
["7.7","Unit 1 and 2 Control Console",2,"items","Install"]
["7.8","Station Control Console",1,"items","Install"]
["7.9","National Control Centre interface",1,"items","Install"]
["7.1","Station Controller",1,"items","Install"]
["7.11","Station Remote IO",1,"items","Install"]
["7.12","Unit 1 and 2 Gen Terminal Junction Box Enclosure (1000(H) x 800(W) x 250mm(D))",2,"items","Supply and install"]
["7.13","Unit 1 and 2 Turbine Pit Junction Box Enclosure (600(H) x 600(W) x 250mm(D))",2,"items","Supply and install"]
[8,"Control Panel and Junction Boxes Cable Wiring Terminations"]
["8.1","Unit 1 and 2 Main Unit Controller Local",600,"items","Install"]
["8.2","Unit 1 and 2 Main Unit Controller Remote IO Generator",600,"items","Install"]
["8.3","Unit 1 and 2 Main Unit Controller Remote IO Turbine",700,"items","Install"]
["8.4","Unit 1 and 2 Main Unit Controller Remote IO Common",400,"items","Install"]
["8.5","Unit 1 and 2 Digital Governor ",200,"items","Install"]
["8.6","Unit 1 and 2 Temperature and Speed Monitoring",600,"items","Install"]
["8.7","Unit 1 and 2 Control Console",300,"items","Install"]
["8.8","Station Control Console",100,"items","Install"]
["8.9","National Control Centre interface",50,"items","Install"]
["8.10","Station Controller",200,"items","Install"]
["8.11","Station Remote IO",200,"items","Install"]
["8.12","Unit 1 and 2 Gen Terminal Junction Box (1000(H) x 800(W) x 250mm(D))",500,"items","Install"]
["8.13","Unit 1 and 2 Turbine Pit Junction Box (600(H) x 600(W) x 250mm(D))",200,"items","Install"]
[9,"Network Communication Cabinets"]
["9.1","Cabinet for FO patch panels, 8U wall mounted, 19\" network cabinet",6,"items","Supply and install"]
[10,"Pressure Instruments"]
["10.1","Pressure transmitter  EJX530A-JBS8N-019EF",10,"each","Supply and install"]
["10.2","Pressure transmitter  EJX530A-JCS8N-019EF",10,"each","Supply and install"]
["10.3","Pressure transmitter EJX530A-JDS8N-019EF",5,"each","Supply and install"]
["10.4","Differential Pressure transmitter EJX110A-JHS4G-919EB",10,"each","Supply and install"]
["10.5","Bourdon Tube Pressure Gauge",22,"each","Supply and install"]
["10.6","2 Way Valve-Manifold",25,"each","Supply and install"]
["10.7","3 Way Valve-Manifold",6,"each","Supply and install"]
["10.8","Stainless Steel Instrumentation Quick Connect Body, SS-QC4-B-4PM, 316 Stainless Steel",25,"each","Supply and install"]
["10.9","Stainless Steel braided flexible tube with quick connectors - SS-810-1-8",10,"each","Supply and install"]
["10.10","Field Mate Versatile Device Management Software",1,"each","Supply"]
["10.11","USB Field Mate Modem: BRAIN / HART",2,"each","Supply"]
["10.12","Installation mechanical bracket for single pressure transmitter ",12,"each","Manufacture and install"]
["10.13","Installation mechanical bracket for redundant pressure transmitter ","16 ","each","Manufacture and install"]
[11,"Level instruments"]
["11.1","Reed Level Transmitter MPJ5-M280 with PR5343A transmitter",4,"each","Supply and install"]
["11.2","Reed Level Transmitter MPJ5-M505 with PR5343A transmitter",8,"each","Supply and install"]
["11.3","Reed Level Transmitter MPJ5-M350 with PR5343A transmitter",4,"each","Supply and install"]
["11.4","Reed Sensor for Bypass Level Indicators MPJ5-M1500  with PR5343A transmitter",8,"each","Supply and install"]
["11.5","Loop link 5909 communication interface",2,"each","Supply"]
["11.6","11.6PReset software (configuration software)",2,"each","Supply"]
["11.7","BMD-SA Magnetic Display for Bypass Level Indicator ",4,"each","Supply and install"]
["11.8","BGU Magnetic Switch for Bypass Level Indicator ",6,"each","Supply and install"]
["11.9","Flange for BMD-SA Magnetic Display for Bypass Level Indicator",8,"each","Supply and install"]
["11.10","Decommission, Fabrication and Installation",8,"each","Decommission, supply and install"]
["11.11","Level chamber with sight glass",5,"each","Supply and install"]
["11.11.1","Decommission, Fabrication (pipe work) and Installation",4,"each","Decommission, supply and install"]
[12,"Flow instruments"]
["12.1","DWM2000 Electromagnetic Flow Meter",12,"each","Supply and install"]
["12.2","Flow switch – Flowphant T_DTT32-A1111AEX1AB, with connecting plug 51006327",6,"each","Supply and install"]
["12.2.1","Removal, Fabrication and Installation",4,"each","Removal, supply and install"]
["12.3","Brach/Stub/Nozzle weld for spool pieces",40,"each","Supply and install"]
["12.4","200B3DASSR2MXI Electromagnetic Flow Meter",3,"each","Supply and install"]
["12.4.1","Removal, Fabrication and Installation",2,"each"]
["12.5","DWM2000 Spool pieces for DN40 pipe with welding socket",4,"each","Supply and install"]
["12.6","200NB SA312 SS316 pipe",6,"each","Supply, manufacture and install"]
["12.7","100NB SA312 SS316 pipe",2,"each","Supply, manufacture and install"]
["12.8","200NB to JIS B2220 K (ASTM A240 GR316) Flange",8,"each","Supply, manufacture and install"]
["12.9","100NB to JIS B2220 10K (ASTM A240 GR316) Flange",4,"each","Supply, manufacture and install"]
["12.10","200NB to JIS B2220 10K Carbon Steel Flange",2,"each","Supply, manufacture and install"]
["12.11","100NB to JIS B2220 10K Carbon Steel Flange",2,"each","Supply, manufacture and install"]
["12.12","40NB to JIS B2220 10K Carbon Steel Flange",4,"each","Supply, manufacture and install"]
[13,"Position and Detector Instruments"]
["13.1","Limit switches",40,"each","Supply and install"]
["13.2","Point level detector 11375Z",6,"each","Supply and install"]
["13.3","FTW325 Transmitter",6,"each","Supply and install"]
[14,"Temperature instruments"]
["14.1","Temperature probes TR10-H (Pt100, 600mm probe length for Turbine Bearing systems)",4,"each","Supply and install"]
["14.2","Temperature probes TR10-H (Pt100, 675mm probe length with 150mm flexible rod for Thrust Guide Bearing systems)",8,"each","Supply and install"]
["14.3","Temperature probes (Pt100, 100mm probe length with embedded steel braided cable)",10,"each","Supply and install"]
["14.4","Temperature probes (Pt100, 130mm probe length with embedded steel braided cable)",4,"each","Supply and install"]
["14.5","Temperature probes (Pt100, 240mm probe length with embedded steel braided cable)",4,"each","Supply and install"]
["14.6","Pt100 RTD with Terminal Head (50mm probe length) ",100,"each","Supply and install"]
["14.7","Pt100 RTD with Terminal Head (100mm probe length) ",20,"each","Supply and install"]
["14.8","Pt100 RTD with Terminal Head (200mm probe length) ",4,"each","Supply and install"]
["14.9","Temperature probes (Pt100 white ceramic terminal block)",200,"each","Supply and install"]
["14.10","Stub Weld, (thermowell)",40,"each","Supply and install"]
[15,"Instrument accessories"]
["15.1","Seamless Instrumentation Grade 316 Austenitic stainless-steel tubing 12 mm OD x 2.0 mm wall thickness, in length of 6 meters",400,"meters","Supply and install"]
["15.2","1/2’’ Flexible hose pipe (Parker 301SN-6) - Nitrile (NBR) Inner Tube, Two High-Tensile Steel Wire Braid Reinforcement & Synthetic Rubber Cover pipe with length of 330 mm end to end. Both sides of end fittings to be a straight female 12 mm swivel nuts type 316 SS, both end fittings to be ASME standard. Maximum working pressure 330 bar. ",100,"each","Supply and install"]
["15.3","1/4’’ Flexible hose pipe single wire braided (with max pressure of 18Mpa) hose pipe with length of 330 mm end to end. One side of end fitting to be a straight female 12 mm swivel type 316 SS and the other end to be a 90° female 12 mm swivel type 316 SS, both end fittings to be ASME standard. To be pressure tested to 8Mpa. ",20,"each","Supply and install"]
["15.4","12 mm hydraulic pipe clamp with polyproline support body, carbon steel weld base plate, top plate and M6 bolts.",600,"each","Supply and install"]
["15.5","90-degree elbow fittings for 12 mm tubing. Material Grade 316 stainless-steel with 12L nut and ferrule both sides, fittings to be according to ASME standard.",200,"each","Supply and install"]
["15.6","T-piece for 12 mm tubing.  Grade 316 stainless-steel with 12L nut and ferrule all three sides fittings. Fittings to be according to ASME standard",200,"each","Supply and install"]
["15.7","Union fittings Grade 316 stainless-steel with 12L nut and ferrule for 12 mm tubing both sides. Fittings to be according to ASME standard.",200,"each","Supply and install"]
["15.8","½’’ Female BSPP to 12L male. Material Grade 316 stainless-steel with nut and ferrule on the 12L side. Fittings to be according to ASME standard.",200,"each","Supply and install"]
["15.9","3/8’’ Male BSPP to 12L male Grade 316 stainless-steel with nut and ferrule on the 12L side. Fittings to be according to ASME standard.",200,"each","Supply and install"]
["15.10","3/8” Male BSPP to 12L male ASTM SA-105N carbon steel with nut and ferrule on the 12L side. Fittings to be according to ASME standard.",100,"each","Supply and install"]
["15.11","½’’ Male BSPP to 12L male Grade 316 stainless-steel with nut and ferrule on the 12L side. Fittings to be according to ASME standard.",400,"each","Supply and install"]
["15.12","½’’ Male BSPP to 12L male ASTM SA-105N carbon steel with nut and ferrule on the 12L side. Fittings to be according to ASME standard.",100,"each","Supply and install"]
["15.13","1/4’’ Male BSPP to 12L male Grade 316 stainless-steel with nut and ferrule on the 12L side. Fittings to be according to ASME standard.",200,"each","Supply and install"]
["15.14","1/4” Male BSPP to 12L male ASTM SA-105N carbon steel with nut and ferrule on the 12L side. Fittings to be according to ASME standard.",100,"each","Supply and install"]
["15.15","1/2’’ Male NPT to 12L male Grade 316 stainless-steel with nut and ferrule on the 12L side. Fittings to be according to ASME standard.",50,"each","Supply and install"]
["15.16","1/4’’ Male NPT to 12L male Grade 316 stainless-steel with nut and ferrule on the 12L side. Fittings to be according to ASME standard.",50,"each","Supply and install"]
["15.17","3/8’’ Male NPT to 12L male Grade 316 stainless-steel with nut and ferrule on the 12L side. Fittings to be according to ASME standard.",50,"each","Supply and install"]
["15.18"," ½’’ Male BSPP to 1/2’’ male BSPP grade 316 stainless steel. Fittings to be according to ASME standard ",50,"each","Supply and install"]
["15.19","½’’ Male BSPP to 1/4’’ male BSPP grade 316 stainless steel. Fittings to be according to ASME standard ",50,"each","Supply and install"]
["15.20","½’’ Male BSPP to 3/8’’ male BSPP grade 316 stainless steel. Fittings to be according to ASME standard ",50,"each","Supply and install"]
["15.21","½’’ Male BSPP to 1/2’’ male NPT grade 316 stainless steel. Fittings to be according to ASME standard ",50,"each","Supply and install"]
["15.22","½’’ Male BSPP to 1/4’’ male NPT grade 316 stainless steel. Fittings to be according to ASME standard ",50,"each","Supply and install"]
["15.23"," ½’’ Male BSPP to 3/8’’ male NPT grade 316 stainless steel. Fittings to be according to ASME standard ",50,"each","Supply and install"]
["15.24","1/2’’ Male NPT to ½’’ male NPT grade 316 stainless steel. Fittings to be according to ASME standard ",50,"each","Supply and install"]
["15.25","1/2’’ Male NPT to ¼’’ male NPT grade 316 stainless steel. Fittings to be according to ASME standard ",50,"each","Supply and install"]
["15.26"," 1/2’’ Male NPT to 3/8’’ male NPT grade 316 stainless steel. Fittings to be according to ASME standard ",50,"each","Supply and install"]
["15.27","½’’ Female BSPP T-piece grade 316 stainless-steel fittings on all three sides. Fittings to be according to ASME standard ",25,"each","Supply and install"]
["15.28","½’’ male BSPP grade 316 stainless steel blank stud. Fittings to be according to ASME standard",100,"each","Supply and install"]
["15.29","¼’’ male BSPP grade 316 stainless steel blank stud. Fittings to be according to ASME standard",100,"each","Supply and install"]
["15.30","3/8’’ male BSPP grade 316 stainless steel blank stud. Fittings to be according to ASME standard",100,"each","Supply and install"]
["15.31","¼’’ Male BSPP to 1/4’’ male BSPP grade 316 stainless steel. Fittings to be according to ASME standard  ",50,"each","Supply and install"]
["15.32","1/2\" Forged Elbow. EN16Mo3 As per BS EN 10253-Forged Carbon Steel",100,"each","Supply and install"]
["15.33","1/2’’ Teflon seal to fit 1/2” BSPP male fittings.",400,"each","Supply and install"]
["15.34","1/2’’ Seal Bonded Washer (Dowty gasket seal plated carbon steel with buna O-ring).",400,"each","Supply and install"]
["15.35"," 1/4’’ Seal Bonded Washer (Dowty gasket seal plated carbon steel with buna O-ring)",100,"each","Supply and install"]
["15.36","3/8’’ Seal Bonded Washer (Dowty gasket seal plated carbon steel with buna O-ring)",200,"each","Supply and install"]
["15.37","BALL VALVE WITH FEMALE BSPP ENDS: 1/2\" BSPP Grade 316 Stainless Steel Ball Valve with lockable handle. Max. allowable (Working) Pressure of 69 bar.",50,"each","Supply and install"]
["15.38","ISOLATION VALVE WITH FEMALE NPT ENDS: 3/8\" NPT Stainless Steel Ball Valve with lockable handle. Max. allowable (Working) Pressure of 69 bar. Part Number: 521561 ",25,"each","Supply and install"]
["15.39","ISOLATION VALVE FEMALE BSPP ENDS: 1/2\" both sides, mild steel",100,"each","Supply and install"]
["15.40","ISOLATION VALVE WITH BLEED VALVE: Pressure gauge Shut-off valve with vent screw (bleed valve). PN400 with ½” BSPP male inlet and ½” female outlet union nut, Carbon Steel",100,"each","Supply and install"]
["15.41","NEEDLE SHUT-OFF VALVES: Type S350 High Pressure Needle Valve ½” BSPP female both sides. PN400, 1.0460 Carbon Steel. Part number S350.03.104.",50,"each","Supply and install"]
["15.42","NEEDLE SHUT-OFF VALVES: Type S350 High Pressure Needle Valve ½” BSPP female both sides. PN400, 1.4571 Stainless Steel. Part number S350.03.204",50,"each","Supply and install"]
["15.43","3-Piece Ball Valve (PEKOS FIG.K 809 SGSGV CL800 1/2\" BSPP) Description: 3-piece, full bore, soft seat ball valve with ½” BSPP female flanges on both ends. Material: ASTM SA-105N (Flanges and Body); Grade 316 stainless steel (ball)",10,"each","Supply and install"]
["15.44","3-Piece Ball Valve (FIG.K 809 SGSGV CL800 1/2\" BW). Description: 3-piece, full bore, soft seat ball valve with flanges prepared for butt welding a ½” pipe on both ends. Material: ASTM SA-105N (Flanges and Body); Grade 316 stainless steel (ball)",10,"each","Supply and install"]
[16,"Consumables"]
["16.1","20mm Gland Hole blanks plug",200,"each","Supply "]
["16.2","25mm Gland Hole Blanks plug",200,"each","Supply "]
["16.3","Labelling Type: 15mm Sleeves (Clear). Size: 1-2mm",20,"BX","Supply"]
["16.4","Labelling Type: 23mm Sleeves (Clear). Size: 1-2mm",20,"BX","Supply"]
["16.5","Labelling Type: PVC tags (yellow). Size: 15mm",20,"BX","Supply "]
["16.6","Labelling Type: PVC tags (yellow). Size: 23mm",20,"BX","Supply"]
["16.7","70X10 Cable Sleeves ",20,"BX","Supply"]
["16.8","70X10 Yellow Cable Labels ",20,"BX","Supply "]
["16.9","Black Cable Ties T120R ",200,"100/PKT","Supply "]
["16.10","Black Cable Ties T50R ",200,"100/PKT","Supply"]
["16.11","Black Cable Ties T30R ",200,"100/PKT","Supply"]
["16.12","Black Cable Ties T18R ",200,"100/PKT","Supply"]
["16.13","Black Cable Ties T16R ",200,"100/PKT","Supply"]
["16.14","Black Heat shrink (Shrink ratio 2:1) Size 12.7/6.4mm",4000,"meters","Supply "]
["16.15","Black Heat shrink (Shrink ratio 2:1) Size 19.1/9.5mm",4000,"meters","Supply"]
["16.16","Black Heat shrink (Shrink ratio 2:1) Size 9.5/4.7mm",500,"meters","Supply"]
["16.17","Black Screen Heat shrink (Shrink ratio 3:1) Size 1.5/0.5mm",4000,"meters","Supply"]
["16.18","Clear Cable Spiral Wrapping (Bind) Ty-Rap ",500,"meters","Supply "]
["16.19","Earth (Green/ Yellow) Single Core Multi Stranded Panel Wire 1.5mm ",400,"meters","Supply"]
["16.20","Size 0 Black Shrouds ",1000,"each","Supply"]
["16.21","Size 0 Glands ",1000,"each","Supply"]
["16.22","Size 00 Black Shrouds ",1000,"each","Supply "]
["16.23","Size 00 Glands ",1000,"each","Supply "]
["16.24","Size 1 Black Shrouds ",1000,"each","Supply"]
["16.25","Size 1 Glands ",1000,"each","Supply"]
["16.26","Size 2 Black Shrouds ",500,"each","Supply "]
["16.27","Size 2 Glands ",500,"each","Supply"]
["16.28","Size 3 Black Shrouds ",50,"each","Supply"]
["16.29","Size 3 Glands ",50,"each","Supply"]
["16.30","Size 4 Black Shrouds ",50,"each","Supply "]
["16.31","Size 4 Glands ",50,"each","Supply"]
["16.32","WTR 4SL Spring Loaded Terminal",500,"each","Supply "]
["16.33","Terminal numbers for WTR 4SL Spring Loaded Terminal",null,"each","Supply"]
["16.34","Terminal Strip Marker ",100,"each","Supply"]
["16.35","PVC Coated Galvanised Steel, Black, 25 meters, 20mm Flexible Conduit TSP20/BL/25M",500,"meters","Supply "]
["16.36","PVC Coated Galvanised Steel, Black, 25 meters, 32mm Flexible Conduit TSP32/BL/25M",500,"meters","Supply"]
["16.37","Straight Fitting 20mm T/SP20/M20/A M20 ",100,"each","Supply "]
["16.38","Straight Fitting 32mm T/SP32/M32/A M32 ",100,"each","Supply "]
["16.39","Smooth Entry Bush 20mm T/SP20/20/C",100,"each","Supply"]
["16.40","Smooth Entry Bush 32mm T/SP32/32/C",100,"each","Supply"]
["16.41","Conduit Terminator 20mm T/SP20/E",100,"each","Supply"]
["16.42","Conduit Terminator 32mm T/SP32/E",100,"each","Supply"]
["16.43","Brass Female Couplers Metric Thread 20mm T/B/M20/C",100,"each","Supply "]
["16.44","Brass Female Couplers Metric Thread 32mm T/B/M32/C ",100,"each","Supply"]
["16.45","Straight Fitting Swivel External Male Thread 20mm T/SP20/M20/B",100,"each","Supply"]
["16.46","Straight Fitting Swivel External Male Thread 32mm T/SP32/M32/B",100,"each","Supply "]
["16.47","Nickel Plated Brass - 45° Elbow T/SPL20/M20/C45",100,"each","Supply "]
["16.48","Nickel Plated Brass - 90° Elbow T/SPL20/M20/C90",100,"each","Supply"]
["16.49","Nickel Plated Brass - 90° Elbow T/SPL32/M32/C90",100,"each","Supply"]
["16.50","2-piece P1000 Clamp (with bolt and nylock nut) for TSP20 (Unistrut Channel Clamps 20mm) T15/20",1500,"each","Supply "]
["16.51","2-piece P1000 Clamp (with bolt and nylock nut) for TSP20 (Unistrut Channel Clamps 32mm) T25/30",1500,"each","Supply"]
["16.52","EX Thread Convertors 25mm to 20mm T/EXN/M25-M20/R",100,"each","Supply "]
["16.53","Pre-insulated Ring Lugs (Red).  Size: 0.25-1.65mm². Product ID: 1R3",200,"100/PKT","Supply "]
["16.54","Pre-insulated Ring Lugs (Blue).  Size: 1.04-2.63mm² Product ID: 2R35",200,"100/PKT","Supply"]
["16.55","Pre-insulated Hook Blade Lugs (Red).  Size: 0.25-1.65mm².  Product ID: 1HB3",200,"100/PKT","Supply"]
["16.56","Pre-insulated Hook Blade Lugs (Blue). Size: 1.04-2.63mm².  Product ID: 2HB3",200,"100/PKT","Supply"]
["16.57","Insulated Bootlace Ferrules (Red). Size: 1.00mm². Product ID:  E1010RD",200,"100/PKT","Supply "]
["16.58","Insulated Bootlace Ferrules (Black). Size: 1.50mm². Product ID:  E1010BK",200,"100/PKT","Supply"]
["16.59","Insulated Bootlace Ferrules (Grey). Size: 2.50mm². Product ID:  E1010GY",40,"100/PKT","Supply "]
["16.60","Harting plugs: Han A Hood Coupler 1 Lever M20, Category: Hoods/Housing, Series: Han A, Type: Housing, Part number 19 20 003 1750",200,"each","Supply"]
["16.61","Harting plugs: Han A Hood Top Entry 2 Pegs M20, Category: Hoods/Housing, Series: Han A, Type: Hood, Part number 19 20 003 1440",200,"each","Supply"]
["16.62","Harting plugs: Han 4A-STI-S, Category: Inserts, Series: Han A, Termination method: Screw termination, Number of contacts: 4, Part number 09 20 004 2611",200,"each","Supply "]
["16.63","Harting plugs: Han A 04 Pos. F Insert Screw, Category: Inserts, Series: Han A, Termination method: Screw termination, Number of contacts: 4, Part number 09 20 004 2711",200,"each","Supply "]
["16.64","Harting plugs: Han CGM-M M20x1,5 D.5-9mm, Category: Accessories, Series: Han CGM-M, Type: Cable Gland, Part number 19 00 000 5080",200,"each","Supply "]
["16.65","Harting plugs: Screw teethed M3x6 (PU 100pcs), Category: Accessories, Series: Han 3 A, Type: Fixing screws, Part number 09 20 000 9995",200,"each","Supply "]
[17,"Transportation"]
["17.1","Phase 1 Control Panels from Cape Town (Acacia Power Station) to Vanderkloof Power Station  ",826,"km","Transport"]
["17.2","Phase 2 Control Panels from Cape Town (Acacia Power Station) to Vanderkloof Power Station  ",826,"km","Transport"]
[18,"Sample of Labour Activities to be considered"]
["18.1","Wiring and fitting of harting plugs",null,"each"]
["18.2","Configuration and Bench Testing of instruments (Pre-Outage)",null,"each"]
["18.3","Cold commissioning (loop checks)",null,"each"]
["18.4","Hot Commissioning (Instrument Function Checks)",null,"each"]
["18.5","Provide support during commissioning",null,"each"]
[null,"TOTAL OF PRICES"]