{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":46,"n_cols":7,"rows_kept":46,"merged":[[42,2,42,3],[44,2,44,3]]}
{"$rows_empty":10}
[null,"Price Schedule"]
[]
[null,"Smart Classtooms and Smart Boards"]
[]
[null,"Item","Description ",null,"QTY","Unit Price (incl. VAT)","Total Price (incl. VAT)"]
[null,1,null,"Models","Quantity"]
[null,2,"Interactive Screen","DS-D5C86RB/B",4,"R","R"]
[null,3,"Windows OPS","DS-D5AC12T5-8S2",4,"R","R"]
[null,4,"Classroom Recording Devices","DS-9604LNI-V/B12",1,"R","R"]
[null,5,"Teacher Tracking Camera","IDS-2CD7186G0-IZS/TEA",8,"R","R"]
[null,6,"Student Attendance Camera","iDS-EGD0288-H/FR(C4F0)(O-STD)",4,"R","R"]
[null,7,"Microphone","DS-UAC-M1P",4,"R","R"]
[null,8,"Networking Video Recorder","DS-7732NXI-I4/S(STD)",1,"R","R"]
[null,9,"20m HDMI Cable","HDMI-20M",1,"R","R"]
[null,10,"43 inch Monitor","DS-D5043QE",1,"R","R"]
[null,11,"HDD","ST10000VE0001",4,"R","R"]
[null,12,"POE Switch","DS-3E1526P-SI",1,"R","R"]
[null,13,"Facial Enrollment","DS-K1F600U-D6E-F",1,"R","R"]
[null,14,"Single-door Magnetic Lock, 280kg Linear Thrust, 12 VDC, 340mA.","DS-K4H258S",4,"R","R"]
[null,15,"LZ-Bracket of Magnetic Lock, for DS-K4H258S","DS-K4H258-LZ",4,"R","R"]
[null,16,"Door Closer,for door weight 60 85Kg","DS-K4DC104",4,"R","R"]
[null,17,"No Touch Exit Sensor","DS-K7P04",4,"R","R"]
[null,18,"Emergency Break glass, green color.","DS-K7PEB",4,"R","R"]
[null,19,"Face Recognition Terminal","DS-K1T342MFWX-E1",4,"R","R"]
[null,20,"HikCentral Class Sharing Tool License","hikCentral-E-ClassIn-Remote",4,"R","R"]
[null,21,"HikCentral Rackmount VMS Server with 64CH","HikCentral-P-VER/HW1D/64",1,"R","R"]
[null,22,"HikCentral access control base package 16 door","HikCentral-P-ACS-16Door/Base/Promo",1,"R","R"]
[null,23,"HikCentral facial recognition channel license","HikCentral-P-Facial&Body-1Ch",4,"R","R"]
[null,24,"Time and Attendance Module Expansion package","HikCentral-P-Attendance-Module",1,"R","R"]
[null,25,"Analogue mixing console","DS-QAPMCR8-A",4,"R","R"]
[null,26,"8\" Speaker 200w","DS-QAP1R20-8",4,"R","R"]
[null,27,"PROFESSIONAL AMPLIFIER","DS-QAPAR50-2",4,"R","R"]
[null,28,"Training, 2 type of training to be conducted,Smart class room and interactive board utilization",null,2,"R","R"]
[null,29,"SmartBoard Device Support and Maintenance",null,"36 Months","R","R"]
[null,null,"TOTAL BID PRICE (Including Supply, Delivery, Commissiong, Support and Maintanance)",{"$nulls":3},"R"]
[null,null,"NB: See detailed  specification attached seperately."]