{"text_format":"3","workbook":"xlsx","n_sheets":6,"sheets":["Cover","Cover ","Instructions ","Summary","P&Gs","Security Upgrade"],"not_rendered":{"images":1,"external_links":1,"defined_names":40},"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"hidden":true,"merged":[[0,5,6,8],[7,0,7,8],[8,0,8,8],[9,0,9,8],[10,0,10,8],[12,0,12,8]]}
[{"$nulls":5},"BILL OF QUANTITIES"]
{"$rows_empty":7}
["ESKOM REAL ESTATE PROJECT DELIVERY"]
["ESKOM MEGAWATT PARK"]
["REPLACEMENT OF ELECTRIC FENCE AT MWP"]
[]
[]
[]
[]
["Use this page as a cover page for the Bill of Quantities:"]
["1. Tenderers must ensure that adequate provision is made in the Bill of Quantities for the health and safety measures "]
["required by Eskom"]
["2. The original format Bill of Quantities must be populated by hand in black ink and will be the document used for"]
["evaluation purposes."]
["3. Tenderers are also required to electronically populate the Excel format and add to the required Flash Drive with your"]
["submission. This will be used to support verification of pricing errors."]
["4. The pricing instructions shall be read prior to pricing this Bill"]
["5. The PDF submission of the BOQ (all pages) shall be signed by the supplier prior to submission of this tender"]
[]
[]
["PRICING INFORMATION"]
[]
[]
["ENQUIRY NUMBER:"]
[]
[]
[]
["TENDERERS NAME:"]
[]
[]
["THE PRICE IN RAND (excluding Vat):"]
[]
[]
[]
[]
["DATE:"]
[]
[]
[]
["Signed By:"]
[]
[]
[]
["DESIGNATION: "]

{"sheet":"Cover ","index":1,"n_rows":48,"n_cols":6,"rows_kept":48,"merged":[[0,5,6,8],[7,0,7,8],[8,0,8,8],[9,0,9,8],[10,0,10,8]]}
[{"$nulls":5},"BILL OF QUANTITIES"]
[]
[]
[]
[]
[]
[]
["ESKOM REAL ESTATE PROJECT DELIVERY"]
["ESKOM ACADEMY OF LEARNING"]
["MWP PERIMETER UPGRADE PROJECT"]
[]
[]
[]
[]
["Use this page as a cover page for the Bill of Quantities:"]
["1. Tenderers must ensure that adequate provision is made in the Bill of Quantities for the health and safety measures "]
["required by Eskom"]
["2. The original format Bill of Quantities must be populated by hand in black ink and will be the document used for"]
["evaluation purposes."]
["3. Tenderers are also required to electronically populate the Excel format and add to the required Flash Drive with your"]
["submission. This will be used to support verification of pricing errors."]
["4. The pricing instructions shall be read prior to pricing this Bill"]
["5. The PDF submission of the BOQ (all pages) shall be signed by the supplier prior to submission of this tender"]
[]
["PRICING INFORMATION"]
[]
[]
["ENQUIRY NUMBER:"]
[]
[]
[]
["TENDERERS NAME:"]
[]
[]
["THE PRICE IN RAND (excluding Vat):"]
[]
[]
[]
[]
["DATE:"]
[]
[]
[]
["Signed By:"]
[]
[]
[]
["DESIGNATION: "]

{"sheet":"Instructions ","index":2,"n_rows":109,"n_cols":2,"rows_kept":109,"merged":[[1,0,1,9],[2,0,2,9],[3,0,3,9],[4,0,4,9],[5,1,5,8]]}
[]
["           ESKOM REAL ESTATE PROJECT DELIVERY \nESKOM ACADEMY OF LEARNING \nKENDAL ROOF REPLACEMENT PROJECT\nPHASE 2"]
["PRICING INSTRUCTIONS"]
["ESKOM ACADEMY OF LEARNING "]
["MWP PERIMETER SECURITY UPGRADE PROJECT"]
[]
[]
["NB: Please read these pricing instructions before pricing this Bill."]
[]
["PRICING INSTRUCTIONS"]
[]
["The units of measurement described in the Pricing Schedule are metric units. Abbreviations used"]
["in the Pricing Schedule are as follows:"]
[]
[]
["%","percent"]
["h","hour"]
["ha","hectare"]
["kg","kilogram"]
["kl","kilolitre"]
["km","kilometre"]
["km-pass","kilometre-pass"]
["kPa","kilopascal"]
["kW","kilowatt"]
["","litre"]
["m","metre"]
["mm","millimetre"]
["m²","square metre"]
["m²-pass","squaremetre-pass"]
["m³","cubic metre"]
["m³-km","cubicmetre-kilometre"]
["MN","mega newton"]
["MN.m","meganewton-metre"]
["MPa","megapascal"]
["No.","number"]
["Prov sum","Provisional sum"]
["PC sum","Prime cost sum"]
["R/only","Rate only"]
["sum","lump sum"]
["t","ton (1000kg)"]
["W/day","Work day"]
[]
["For the purposes of this Pricing Schedule, the following shall have the meanings assigned to them:"]
[]
["Unit: ","The unit of measurement for each item of work"]
[]
["Quantity:","The number of units of work for each item"]
[]
["Rate:","The payment per unit of work for which the Service Provider tenders to do the work"]
[]
["Amount:","The product of the quantity and the rate tendered for an item."]
[]
["Item:","An amount tendered for an item, the extent of which is described in the Pricing Schedule, "]
[null,"the Scope of work or eslewhere, but of which the quantity of work is not measured in units."]
[]
[]
["THE BILL OF QUANTITIES"]
[]
["The Bill of quantities shall be priced in alignment with the works information as stated in the NEC contract."]
["The Bill of quantities shall not be used as the Works Information. The Works Information as stated under "]
["Clause 55.1 of the NEC contract. Any items that the contractor does not fully understand, the contractor "]
["shall obtain clarity on such items prior to pricing as indicated by the Eskom conditions of Tender."]
["The contractors final submitted offer shall be binding for duration of the project for provision of the full"]
["scope of works as noted in the works information."]
[]
["PRICING"]
[]
["The prices and rates in the Pricing Schedule are fully inclusive prices for the work described"]
["under the items. Such prices and rates cover all costs and expenses that may be required in and for"]
["the execution of the work described in accordance with the provisions of the Scope of Work,"]
["and shall cover the cost of all general risks, liabilities and obligations set forth or implied in the "]
["in the Contract Data and profit as deemed necessary."]
[]
["Where the Scope of Work requires detailed drawings and designs or other information to be"]
["provided, all costs associated therewith are deemed to have been provided for and included in"]
["the unit rates and sum amount tendered such items."]
[]
["NO RATE OR PRICE"]
[]
["An item against which no price is entered will be considered to be covered by the other "]
["prices or rates in the Pricing Schedule. A single lump sum will apply should a number of items"]
["be grouped together for pricing purposes."]
[]
["QUANTITIES"]
[]
["The quantities set out in the Pricing Schedule are approximate and do not necessarily represent the actual  "]
["amount of work to be done. The quantities of work accepted shall be verified by the contractor and all discrepancies"]
["shall be noted. Huge variations from the BOQ quantities shall be reported prior to pricing the BOQ."]
[]
["Should there be a discrepancy between the items in the bill of quantities and works information"]
["the contractor is liable to indicate such discrapancies to the Employer prior to pricing these bill of quantities."]
[]
["ADDITIONS"]
[]
["Reasonable compensation will be received where no payment item appears in the Pricing"]
["Schedule in respect of work required in terms of the Contract and which is not covered in any"]
["other payment item. This shall constitute a compensation event which shall be approved by Eskom "]
["prior to work being completed on site."]
[]
["The short descriptions of the items of payment given in the Pricing Schedule are only for the"]
["purposes of identifying the items. More details regarding the extent of the work entailed under"]
["each item appear in the Technical Specification."]
[]
["CONTRACT PRICE ADJUSTMENT"]
[]
["The contractors offer shall not be changed during the contruction period of the project. Adjustment "]
["is only applicable if the contract continues beyond the anniversary of the tender date."]
["The contractor is therefore liable to providing a price which factors all adjustments that may take place within "]
["the industry prior to that time."]

{"sheet":"Summary","index":3,"n_rows":18,"n_cols":5,"rows_kept":18,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,4],[3,0,3,4],[4,0,4,4],[17,0,17,3]]}
["ESKOM REAL ESTATE PROJECT DELIVERY"]
["ESKOM MEGAWATT PARK"]
["MWP PERIMETER SECURITY UPGRADE"]
["PRICING SCHEDULE"]
[]
["Item no","Description",null,null,"Amount"]
[]
[1.1,"Preliminaries and General"]
[]
[1.2,"Alterations"]
[]
[1.3,"Brickwork"]
[]
[1.4,"Electrical works"]
[]
[1.5,"External work"]
[]
["TOTAL COST OF PROJECT (Excl. Vat)"]

{"sheet":"P&Gs","index":4,"n_rows":137,"n_cols":7,"rows_kept":137,"merged":[[1,0,1,6],[2,0,2,6],[3,0,3,6],[4,0,4,6],[5,0,5,6]]}
[]
["ESKOM REAL ESTATE PROJECT DELIVERY"]
["ESKOM MEGAWATT PARK"]
["MWP PERIMETER SECURITY UPGRADE"]
["PRICING SCHEDULE"]
[]
["Item no","SABS 1200","Description","Unit","Quantity","Rate","Amount"]
[]
[null,null,"BILL 1: PRELIMINARIES AND GENERAL"]
[]
[null,null,"Pricing instructions and the works information shall be read prior to pricing of the Bill of Quantities"]
[]
[null,"A","PRELIMINARY AND GENERAL"]
[null,"A.8.3","FIXED CHARGE ITEMS"]
[]
[null,null,"The Model Preambles for Trades (2008 Edition) as published by the Association of South African Quantity Surveyors shall be deemed to be incorporated in these bills of quantities and no claim arising from brevity of description of items fully described in the said Model Preambles will be entertained"]
[]
[null,null,"Where Model Preambles for Trades and Supplementary Preambles are in conflict, the Supplementary Preamble shall take precedence."]
[]
[null,null,"Supplementary preambles are incorporated in these bills of quantities to satisfy the requirements of this project. Such supplementary preambles shall take precedence over the provisions of the said Model Preambles"]
[]
[null,null,"This bill of quantities must be read in conjunction with the works information which is in the Contract Works information -Section 3. "]
[]
[null,null,"The contractor's prices for all items throughout these bills of quantities must take account of and include for all of the obligations, requirements and specifications given in the Works Information."]
[]
[null,null,"PRICING OF PRELIMINARIES"]
[]
[null,null,"The value for Preliminaries and General will fully take into account all the items required to carry out the works but cannot be attributed to the items under the scope of works."]
[]
[null,null,"A detailed breakdown of the Preliminaries and General may be requested during the evaluation period."]
[]
[null,null,"The sums stated for items under this heading shall cover the cost of providing, establishing and commissioning on the site the facilities adequately equipped to enable all the work to commence and to proceed to completion as required in terms of the contract.The sums shall also cover ( where appropriate) the cost of demolition of and the removal from the site of all items established and shall include for making good and restoring the site to the satisfaction of the Engineer."]
[]
[]
[null,"A.8.3.2","Establishment of Facilities on the Site"]
[null,null," for Contractor "]
[]
[null,"A.8.3.2.2","Facilities for Contractor "]
[]
[1.1,null,"Name boards","Item",1]
[]
[1.2,"A.8.3.2.2a","Offices and Storage sheds","Item",1]
[]
[1.3,"A.8.3.2.2b","Ablution and latrine facilities","Item",1]
[]
[1.4,"A.8.3.2.2f","Tools and equipment","Item",1]
[]
[1.5,"A.8.3.2.2g","Connection of water, electricity and communication ","Item",1]
[]
[null,null,"This items shall be priced where certain plant will be required to enable the contractor to do the work. Where plant will not be required, the contractor shall not price for the item."]
[]
[1.6,"A.8.3.2.2j","Plant (e.g crane, scaffolding etc where applicable)","Item",1]
[]
[1.7,"8.3.3A","Other fixed charge obligations (Provide breakdown)","Item",1]
[]
[1.8,"8.3.4","Removal of site establishment","Item",1]
[]
[1.9,null,"Health and Safety "]
[]
[null,null,"This section shall be priced in alignment with SHE Specification"]
[]
["1.9.1",null,"a) Preparation of Health and Safety File ","Item",1]
[]
["1.9.2",null,"b) Health and Safety Training (where applicable)","Item",1]
[]
["1.9.3",null,"c) Pre-employment medical assessments and certification (Specify the No.)","Item",1]
[]
["1.9.4",null,"d) SHE Equipment (First aid box/fire equipment)","Item",1]
[]
["1.9.5",null,"e) Personal Protective Clothing ","Item",1]
[]
["1.9.6",null,"f) Fences, signs, barricades and workers eating area","Item",1]
[]
["1.9.7",null,"g) Other safety related items (provide breakdown)","Item",1]
[]
[{"v":1.1,"d":"1.10"},null,"Environmental Management Plan","Item",1]
[]
[1.11,null,"Quality Management plan","Item",1]
[]
[1.12,null,"DESIGN WORK"]
[null,null,"The Contractor constructs and erects the works in accordance with the Contractor’s accepted design and takes cognisance of SANS 2001 and SANS 1200."]
[]
[null,null,"Hours to be used shall be in line with contractors schedule"]
[]
["1.12.1",null,"Detailed designs","Item",1]
[]
[2,"8.4","TIME RELATED ITEMS"]
[]
[2.1,"8.4.2","OPERATE AND MAINTAIN FACILITIES ON THE SITE"]
[]
[null,"8.4.2.1","FACILITIES FOR ENGINEER FOR THE DURATION OF CONSTRUCTION"]
[]
["2.1.1",null,"Telephone services","Months",8]
[]
[null,"8.4.2.2","FACILITIES FOR CONTRACTOR FOR THE DURATION OF CONSTRUCTION"]
[]
[null,null,"This cost shall be for the monthly running costs of the contractors spaces"]
[]
["2.1.2","8.4.2.2a","Offices and Storage sheds","Months",8]
[]
["2.1.3","8.4.2.2e","Ablution and latrine facilities","Months",8]
[]
["2.1.4","8.4.2.2f","Tools and equipment","Months",8]
[]
["2.1.5","8.4.2.2j","Plant (crane, scaffolding etc where applicable)","Months",8]
[]
["2.1.6","8.4.3","Supervision and management cost for duration of construction","Months",8]
[]
["2.1.7",null,"Company and head office overhead costs  for the duration of the contract","Months",8]
[]
["2.1.8","8.4.2.2i","Other time related charge obligations (Provide breakdown)","Months",8]
[]
[3,null,"Health and Safety"]
[]
[null,null,"This section shall be priced in alignment to SHE Specification"]
[]
[3.1,null,"a) Safety Personnel for duration of project as per SHE Specification ","Months",8]
[]
[3.2,null,"b) Maintenance of Personal Protective clothing and equipment","Months",8]
[]
[3.3,null,"c) Covid 19 related supplies","Months",8]
[]
[3.4,null,"d) Other safety related (provide breakdown)","Months",8]
[]
[4,null,"Environmental"]
[]
[4.1,null,"Waste Management for duration of project","Months",8]
[]
[5,null,"Professional Fees for duration of Project"]
[]
[null,null,"Hours shall be in alignment to the schedule duration"]
[{"$nulls":4},"Input hrs","Input rate"]
[5.1,null,"Professional Electrical Engineer","Hrs"]
[]
[]
[]
["TOTAL CARRIED FORWARD TO SECTION SUMMARY"]

{"sheet":"Security Upgrade","index":5,"n_rows":165,"n_cols":6,"rows_kept":165,"merged":[[1,0,1,5],[2,0,2,5],[3,0,3,5],[4,0,4,5],[5,0,5,5]]}
[]
["ESKOM REAL ESTATE PROJECT DELIVERY"]
["ESKOM MEGAWATT PARK"]
["MWP PERIMETER SECURITY UPGRADE"]
["PRICING SCHEDULE"]
[]
["Item no","Description","Unit","Quantity","Rate","Amount"]
[]
[null,"BILL 2: ALTERATIONS"]
[]
[null,"PREAMBLES"]
[]
[null,"The Tenderer is referred to the relevant clauses in the latest edition of the Model Preambles for Trades and to the Supplementary Preambles"]
[]
[null,"The tenderer is advised that any rate must include material, labour, wastage, transport and profit."]
[]
[null,"The Contractor constructs and erects the works in accordance with the Contractor’s accepted design and takes cognisance of SANS 2001 and SANS 1200."]
[]
[null,"The Contractor identifies and includes all items required to form a complete, reliable, fit for purpose operating works, which complies with the requirements as stipulated in this Works Information."]
[]
[null,"EXTERNAL WALL"]
[]
[null,"All demolition work is to be carried out in strict accordance with the instructions and to the satisfaction of the Project Manager"]
[]
["2.1","Break down and removal of existing wall","m²",200]
[]
[2.2,"Removal of existing Palisade Fencing","m",25]
[]
[2.3,"Removal of existing electric fence","m",4200]
[]
["TOTAL CARRIED FORWARD TO SECTION SUMMARY"]
[]
[]
["Item no","Description","Unit","Quantity","Rate","Amount"]
[]
[3,"BILL 3: BRICKWORK"]
[]
[null,"All bricks are to match existing wall and the work is to be left complete and perfect in every aspect. The bricks shall be approved by the project Architect to allow uniformity with the existing."]
[]
[3.1,"Installation of new facebrick wall ","m²",200]
[]
[null,"FENCING"]
[]
[null,"Palisade Fencing to match existing fencing"]
[]
[3.2,"Install new Palisade fencing including fencing posts","m",25]
[]
[]
["TOTAL CARRIED FORWARD TO SECTION SUMMARY"]
[]
[]
["Item no","Description","Unit","Quantity","Rate","Amount"]
[]
[null,"BILL 4: ELECTRICAL WORKS"]
[]
[null,"NOTES:"]
[]
[null,"All electrical works shall be conducted in alignment with works information unde the NEC contract"]
[]
[null,"All Perimeter lights to conform to 240-139282493 Security Lighting for Eskom Applications"]
[]
[null,"Electric fence and boom gates must be as per SANS12222"]
[]
[null,"Certificate of Compliance issued by a Registered Person certifying that the fence meets the requirements of SANS 10222-3:2016. 3. SANS 10142"]
[]
[4.1,"ELECTRIC FENCE"]
[]
["4.1.1","Replacement of Electric Fence incl. brackets, batteries and wiring and related infrastructure","m",4200]
[]
["4.1.2","Replacement of Energisers","No",5]
[]
["4.1.3","Warning signs","No.",20]
[]
[{"v":4.2,"d":"4.20"},"LIGHTINING PROTECTION"]
[]
[null,"The assesment shall be conducted by an Earthing Specialist"]
[]
[null,"Reasonable hours shall be allocated for this activity"]
[]
["4.2.1","Assessment of existing lightning and earthing protection","Item",1]
[]
[null,"All lightning and earthing shall be in accordance to relavant Eskom standard"]
[]
[null,"All earth spikes shall be at approved spacing distances"]
[]
["4.2.2","Installation of Lightning Protection ","Item",1]
[]
["4.2.3","Installation of Earthing ","Item",1]
[]
[4.3,"LIGHTING"]
[]
[null,"Installation of Energy Efficient lighting shall comply with the Eskom Security Lighting requirements"]
[]
["4.3.1","LED Perimeter fence lighting with video motion detection as per works information","No.",162]
[]
["4.3.2","Installation of tampering warning lights with intrusion detection cameras","Item",1]
[]
["4.3.3","Installation of galvanised Light poles including foundation works","No.",60]
[]
["4.3.4","PTZ cameras (perimeter wall and entrance)","No.",220]
[]
["4.3.4","Cabling and other related items (incl. brackets, junction boxes)","Item",1]
[]
[4.4,"ENTRANCES"]
[]
["4.4.1","Camera systems at the two entrances","Item",1]
[]
["4.4.2","LED 'Entrance gate lights as per works information","No.",40]
[]
["4.4.3","Other items not allowed (provide breakdown)","Item",1]
[]
[4.5,"TESTING "]
[]
["4.5.1","Testing, Commissioning incl. COC for entire works","Item",1]
[]
["TOTAL CARRIED FORWARD TO SECTION SUMMARY"]
[]
[]
["Item no","Description","Unit","Quantity","Rate","Amount"]
[]
[null,"BILL 4: EXTERNAL WORKS"]
[]
["4.1","Alterations"]
[]
[4.2,"Replacement of all boom gates with interlocking boom gates with spikes and the replacement of all gate spikes"]
[]
[null,"A breakdown is required "]
[]
["4.1.1","Removal of existing boom gates & related infrastructure","Item",1]
[]
[null,"Replacement of entrance boom gate system including all related infrastructure"]
["4.1.2","Civil works","Item",1]
["4.1.3","Ground Spiking system","Item",1]
["4.1.4","Installation of boom gate and related infrastructure (sally port)","Item",1]
["4.1.5","Card capture unit/stand (gooseneck)","Item",1]
["4.1.6","Electrical infrastructure","Item",1]
["4.1.7","Signage","Item",1]
["4.1.8","Other (list items)"]
[]
["4.1.8","Commisioning of new boom gate system","Item",1]
[]
[4.2,"ROADWORKS"]
[]
["4.2.1","Assessment and report by Roads Engineer","Hrs",80]
[]
["4.2.2","Geotech field tests","Item",1]
[]
["4.2.3","Grading and Rehabilitation of road","m",4200]
[]
[]
[]
["TOTAL CARRIED FORWARD TO SECTION SUMMARY"]
[]
[]
["BILL NO.","DESCRIPTION",{"$nulls":3},"AMOUNT"]
[]
[1,{"$f":"'P&Gs'!C9","v":"BILL 1: PRELIMINARIES AND GENERAL"}]
[]
[2,{"$f":"B9","v":"BILL 2: ALTERATIONS"}]
[]
[3,{"$f":"B54","v":"BILL 4: ELECTRICAL WORKS"}]
[]
[4,{"$f":"B121","v":"BILL 4: EXTERNAL WORKS"}]
[]
[null,"TOTAL COST OF THE PROJECT (excl. VAT)"]