{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["LHWP Security Fence Summary"," Security Fence"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"LHWP Security Fence Summary","index":0,"n_rows":12,"n_cols":4,"rows_kept":12,"flags":["formulas_cached_only"]}
[]
[]
["SECTION","Description","Amount"]
[{"v":1,"d":"001"},"LHWP - Security fence",0]
[]
[]
[]
[null,"SUB-TOTAL",0,"( A )"]
[null,"10% CONTINGENCY  ON SUB-TOTAL ( A )",0,"( B )"]
[null,"SUB-TOTAL ( A + B )",0,"( C )"]
[null,"15% VAT ON SUB-TOTAL ( C )",0,"( D )"]
[null,"TOTAL TENDER SUM",0]

{"sheet":" Security Fence","index":1,"n_rows":30,"n_cols":12,"rows_kept":30,"merged":[[0,0,0,6]],"flags":["formulas_cached_only"]}
["SCHEDULE OF QUANTITIES"]
[null,null,"NB: Supply include transportation."]
[]
["ITEM","REF","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,null,"Preliminary and General"]
[1," OHSACT ","Health and safety file ","Sum",{"v":1,"d":"1.00"}]
[null,null,"Van Zyl house Security"]
[2,null,"Supply- Clear Vu/Clear View/Similar fence mesh opening 76mm x 25 mm ,height 1,8m with poles, green colour.","Length (m)",{"v":76.8,"d":"76.80"}]
[3,null,"Supply- 1,8m x 5,2m sliding gates with wheels and concreted rails with end stops, match fence and green colour","sum",{"v":1,"d":"1.00"}]
[4,null,"Supply- 1,8m x 5,6m sliding gates with wheels and concreted rails with end stops, match fence and green colour","sum",{"v":1,"d":"1.00"}]
[5,null,"Labour-Install new fence, trenching, remove current 1,2m old fence and store at TCTA","Length (m)",{"v":76.8,"d":"76.80"}]
[6,null,"Supply -remote control gate automation - Centurion D5 including gate rack and motor theft bracket","sum",{"v":2,"d":"2.00"},{"$nulls":6},"115m2"]
[7,null,"Supply- standard garage roll up doors, brown colour","sum",{"v":3,"d":"3.00"},{"$nulls":3},120,0.6,72,96]
[8,null,"Labour-Install new standard garage doors, remove current standard garage doors and store at TCTA","sum",{"v":3,"d":"3.00"}]
[9,null,"Supply-remote control garage doors outomation - Centurion SDO4 motor openers","sum",{"v":2,"d":"2.00"}]
[10,"OHSACT","Labour-Install new automation- 2 gate and 2 garage doors, supply electricity from DB boards, cables and isolation switch, trenching, house conduiting , and clean up.                                                                                                                   A single automation for the doubel garage door arrangement. ","sum",{"v":4,"d":"4.00"}]
[11,"OHSACT","Labour-Issue COC certificate for automation isolators installed on DB boards for the Van zyl  house stand.","sum",{"v":1,"d":"1.00"}]
[null,null,"Caledon Adit"]
[12,null,"Supply- Clear View fence mesh opening 76mm x 12,5mm high security fence ,height 2,4 m with poles, green colour.      ","Length (m)",{"v":20,"d":"20.00"}]
[13,null,"Supply- 2,4 m x 4.1m sliding gates with wheels and concreted rails with end stops, match fence and green colour","sum",{"v":1,"d":"1.00"}]
[14,null,"Labour- Install new  fence, trenching, remove current  old fence poles and store at TCTA. ","Length (m)",{"v":20,"d":"20.00"}]
[null,null,"Caledon Dewatering Shaft"]
[13,null,"Supply- Clear View fence mesh opening 76mm x 12,5mm high security fence ,height 2,4 m with poles, green colour.      ","Length (m)",{"v":40.5,"d":"40.50"}]
[14,null,"Supply- 2,4 m x 4,4 m sliding gates with wheels and  concreted rail with end stops, match fence and green colour.       ","sum",{"v":1,"d":"1.00"}]
[15,null,"Labour-Install new fence, trenching, remove current  old palisade fence poles and store at TCTA. ","Length (m)",{"v":40.5,"d":"40.50"}]
[null,null,"Provisional sum"]
[16,null,"provisional sum items to be approved by engineer","sum",null,null,{"v":50000,"d":"R 50,000.00"}]
[17,null,"10% mark up per approved invoice"]
[]
[null,null,"Total Carried Forward to Summary",{"$nulls":3},{"v":50000,"d":"R 50,000.00"}]