{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Bills Of Quantities"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Bills Of Quantities","index":0,"n_rows":1979,"n_cols":34,"rows_kept":1979,"flags":["formulas_cached_only"]}
["Item","Description","Uom","Quantity","Rate","Amount","Total","x","Formatted Qty","x","Abstract RecID","x","Lcode","x","x","x","x","x","x","x","x","x","x","x","x","Package","Section","Bill","Trade","Type","ABUm","PayRef"]
[]
[null,"SECTION NO. 1 : PRELIMINARIES",{"$nulls":23},1,1,1,-2,"H"]
[{"$nulls":33},"NOTE:  the column headings a - z must be present for the importer."]
[{"$nulls":33},"These contain an X which is set forecolor = white"]
[null,"BILL NO.1 : PRELIMINARIES",{"$nulls":23},1,1,1,-2,"H"]
[]
[null,"BUILDING AGREEMENT AND PRELIMINARIES",{"$nulls":8},2170,null,300,{"$nulls":12},1,1,1,-2,"H","0"]
[]
[null,"The JBCC Series 2000 Principal Building Agreement (March 2005 edition) prepared by the Joint Building Contracts Committee shall be the applicable building agreement, amended as hereinafter described",{"$nulls":8},2171,null,400,{"$nulls":12},1,1,1,-2,"c","0"]
[]
[null,"The JBCC Series 2000 Preliminaries (May 2005 edition) prepared by the Joint Building Contracts Committee for use with the said JBCC Principal Building Agreement shall be deemed to be incorporated in these bills of quantities",{"$nulls":8},2172,null,500,{"$nulls":12},1,1,1,-2,"c","0"]
[]
[null,"Contractors are referred to the above mentioned documents for the full intent and meaning of each clause thereof",{"$nulls":8},2173,null,600,{"$nulls":12},1,1,1,-2,"c","0"]
[]
[null,"These clauses are hereinafter referred to by clause number and heading only. Where standard clauses or alternatives are not entirely applicable to this contract such modifications, corrections or supplements as will apply are given under each relevant clause heading and such modifications, corrections or supplements shall take precedence notwithstanding anything contrary contained in the above mentioned documents",{"$nulls":8},2174,null,700,{"$nulls":12},1,1,1,-2,"c","0"]
[]
[null,"Where any item is not relevant to this specific contract such item is marked N/A, signifying \"not applicable\"",{"$nulls":8},2175,null,800,{"$nulls":12},1,1,1,-2,"c","0"]
[]
[null,"PREAMBLES FOR TRADES",{"$nulls":8},2176,null,900,{"$nulls":12},1,1,1,-2,"H","0"]
[]
[null,"The Model Preambles for Trades (1999 edition) as published by the Association of South African Quantity Surveyors shall be deemed to be incorporated in these bills of quantities and no claim arising from brevity of description of items fully described in the said Model Preambles will be entertained",{"$nulls":8},2177,null,1000,{"$nulls":12},1,1,1,-2,"C","0"]
[]
[null,"Supplementary preambles are incorporated in these bills of quantities to satisfy the requirements of this project.  Such supplementary preambles shall take precedence over the provisions of the said Model Preambles",{"$nulls":8},2178,null,1100,{"$nulls":12},1,1,1,-2,"C","0"]
[]
[null,"The contractor's prices for all items throughout these bills of quantities must take account of and include for all of the obligations, requirements and specifications given in the said Model Preambles and in any supplementary preambles",{"$nulls":8},2179,null,1200,{"$nulls":12},1,1,1,-2,"C","0"]
[]
[null,"PRICING OF PRELIMINARIES",{"$nulls":8},2180,null,1300,{"$nulls":12},1,1,1,-2,"H","0"]
[]
[null,"Pricing of Prelims",{"$nulls":8},2181,null,648708,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["1","Should the contractor select Option A in terms of clause 10.3 for the purpose of adjustment of these preliminaries, the amount entered in the amount column in these preliminaries is to be divided into one or more of the three categories provided namely Fixed (F), Value Related (V) and Time Related (T)","Item",1,null,0,null,null,1,null,2182,null,1400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"SECTION A - PRINCIPAL BUILDING AGREEMENT",{"$nulls":8},2183,null,1500,{"$nulls":12},1,1,1,-2,"H","0"]
[]
[null,"Definitions",{"$nulls":8},2184,null,1600,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["2","Clause 1.0 - Definitions and interpretation","Item",1,null,0,null,null,1,null,2185,null,1700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Objective and preparation",{"$nulls":8},2186,null,1800,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["3","Clause 2.0 - Offer, acceptance and performance","Item",1,null,0,null,null,1,null,2187,null,1900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["4","Clause 3.0 - Documents","Item",1,null,0,null,null,1,null,2188,null,2000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["5","Clause 4.0 - Design responsibility","Item",1,null,0,null,null,1,null,2189,null,2100,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["6","Clause 5.0 - Employer's agents","Item",1,null,0,null,null,1,null,2190,null,2200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["7","Clause 6.0 - Site representative","Item",1,null,0,null,null,1,null,2191,null,2300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["8","Clause 7.0 - Compliance with regulations","Item",1,null,0,null,null,1,null,2192,null,2400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["9","Without limiting the generality of the provisions of clause 7.0 the contractor's attention is drawn to the provisions of the Construction Regulations, 2003 issued in terms of the Occupational Health and Safety Act, 1993.  It is specifically stated that the employer shall prepare a documented health and safety specification for the works and that the employer shall ensure that the contractor has made provision for the cost of health and safety measures during the execution of the works.  The contractor shall price opposite this item for compliance with the act and the regulations and the reasonable provisions of the afore mentioned health and safety specification","Item",1,null,0,null,null,1,null,2194,null,2700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["10","Clause 8.0 - Works risk","Item",1,null,0,null,null,1,null,2199,null,3400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["11","Clause 9.0 - Indemnities","Item",1,null,0,null,null,1,null,2200,null,3500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["12","Clause 10.0 - Works insurances","Item",1,null,0,null,null,1,null,2201,null,3600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["13","Clause 11.0 - Liability insurances","Item",1,null,0,null,null,1,null,2202,null,3700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["14","Clause 12.0 - Effecting insurances","Item",1,null,0,null,null,1,null,2203,null,3800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["15","Clause 13.0 - No clause","N/A",0,null,0,null,null,0,null,2204,null,3900,{"$nulls":12},1,1,1,-2,"I","NA"]
[]
["16","Clause 14.0 - Security","Item",1,null,0,null,null,1,null,2205,null,4000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Execution",{"$nulls":8},2206,null,4100,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["17","Clause 15.0 - Preparation for and execution of the works","Item",1,null,0,null,null,1,null,2207,null,4200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["18","Clause 16.0 - Access to the works","Item",1,null,0,null,null,1,null,2208,null,4300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["19","Clause 17.0 - Contract instructions","Item",1,null,0,null,null,1,null,2209,null,4400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["20","Clause 18.0 - Setting out of the works","Item",1,null,0,null,null,1,null,2210,null,4500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["21","The contractor shall notify the principal agent if any encroachments of adjoining foundations, buildings, structures, pavements, boundaries, etc exist in order that the necessary arrangements may be made for the rectification of any such encroachments","Item",1,null,0,null,null,1,null,2211,null,4600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["22","Clause 19.0  - Assignment","Item",1,null,0,null,null,1,null,2212,null,4700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["23","Clause 20.0 - Nominated subcontractors","Item",1,null,0,null,null,1,null,2213,null,4800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["24","Clause 21.0 - Selected subcontractors","Item",1,null,0,null,null,1,null,2214,null,4900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["25","Clause 22.0 - Employer's direct contractors","Item",1,null,0,null,null,1,null,2215,null,5000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["26","Clause 23.0 - Contractor's domestic subcontractors","Item",1,null,0,null,null,1,null,2216,null,5100,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Completion",{"$nulls":8},2217,null,5200,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["27","Clause 24.0 - Practical completion","Item",1,null,0,null,null,1,null,2218,null,5300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["28","Clause 25.0 - Works completion","Item",1,null,0,null,null,1,null,2219,null,5400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["29","Clause 26.0 - Final completion","Item",1,null,0,null,null,1,null,2220,null,5500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["30","Clause 27.0 - Latent defects liability period","Item",1,null,0,null,null,1,null,2221,null,5600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["31","Clause 28.0 - Sectional completion","Item",1,null,0,null,null,1,null,2222,null,5700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["32","Clause 29.0 - Revision of the date for practical completion","Item",1,null,0,null,null,1,null,2223,null,5800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["33","The removal and replacement of materials and/or workmanship which do not conform to specification or drawings shall not constitute grounds for an extension of the construction period nor for an adjustment to the contract value (clause 29.3)","Item",1,null,0,null,null,1,null,2224,null,5900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["34","Clause 30.0 - Penalty for noncompletion","Item",1,null,0,null,null,1,null,2225,null,6000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Payment",{"$nulls":8},2226,null,6100,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["35","Clause 31.0 - Interim payment to the contractor","Item",1,null,0,null,null,1,null,2227,null,6200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["36","The inclusion of materials and goods stored off site in the amount authorised for payment in terms of clause 31.4 shall be at the sole discretion of the principal agent and such inclusion shall only be considered upon the provision, by the contractor, of an approved guarantee issued by a registered commercial bank.  Clause 31.6.5 is therefore not applicable","Item",1,null,0,null,null,1,null,2228,null,6300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["37","Clause 32.0 - Adjustment to the contract value","Item",1,null,0,null,null,1,null,2230,null,6500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["38","All fluctuations in costs, with the exception of fluctuations in the rate of Value Added Tax, shall be for the account of the contractor","Item",1,null,0,null,null,1,null,2231,null,6600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["39","Where prices are submitted by the contractor or nominated/selected subcontractors during the progress of the works in respect of contract instructions or in regard to a claim under the terms of the contract and notwithstanding the fact that such prices may be used in an interim payment certificate, there is to be no presumption of acceptance. Should the principal agent wish to accept any such prices prior to the issue of the final certificate, it will be in writing","Item",1,null,0,null,null,1,null,2232,null,6700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["40","Clause 33.0 - Recovery of expense and loss","Item",1,null,0,null,null,1,null,2233,null,6800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["41","Clause 34.0 - Final account and final payment","Item",1,null,0,null,null,1,null,2234,null,6900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["42","Clause 35.0 - Payment to other parties","Item",1,null,0,null,null,1,null,2235,null,7000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Cancellation",{"$nulls":8},2236,null,7100,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["43","Clause 36.0 - Cancellation by employer - contractor's default","Item",1,null,0,null,null,1,null,2237,null,7200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["44","Clause 37.0 - Cancellation by employer - loss and damage","Item",1,null,0,null,null,1,null,2238,null,7300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["45","Clause 38.0 - Cancellation by contractor - employer's default","Item",1,null,0,null,null,1,null,2239,null,7400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["46","Clause 39.0 - Cancellation - cessation of the works","Item",1,null,0,null,null,1,null,2240,null,7500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Dispute",{"$nulls":8},2241,null,7600,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["47","Clause 40.0 - Dispute settlement","Item",1,null,0,null,null,1,null,2242,null,7700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Substitute provisions",{"$nulls":8},2243,null,7800,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["48","Clause 41.0 - State clauses","Item",1,null,0,null,null,1,null,2244,null,7900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Contract variables",{"$nulls":8},2245,null,8000,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["49","Clause 42.0 - Pre-tender information","Item",1,null,0,null,null,1,null,2246,null,8100,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["50","User Note -All information for this section requires consultation with the contractor.  The principal agent should not pre-select any of the alternatives available to the contractor","Item",1,null,0,null,null,1,null,2247,null,11900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["51","Information necessary for the completion of those clauses contained in the schedule which are necessary for tender purposes is given hereunder","Item",1,null,0,null,null,1,null,2248,null,8200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["52","Clause 42.0 -  Post-tender information","Item",1,null,0,null,null,1,null,2249,null,11600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["53","The required post-tender information shall be inserted in the agreement after consultation with the contractor","Item",1,null,0,null,null,1,null,2250,null,11700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"42.1 CONTRACTING AND OTHER PARTIES",{"$nulls":8},2251,null,8300,{"$nulls":12},1,1,1,-2,"S","I"]
[]
[null,"42.1.1 Employer: ........................................................\r\n",{"$nulls":8},2252,null,8400,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Postal address: ................................................ ..............................................Code: ................\r\n",{"$nulls":8},2252,null,8400,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Tel: ............................Fax: ..............................\r\n",{"$nulls":8},2252,null,8400,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"E-mail: ............................................................. Tax/VAT registration No: ..................................\r\n",{"$nulls":8},2252,null,8400,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Physical address: ............................................. ........................................................................\r\n",{"$nulls":8},2252,null,8400,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"........................................................................",{"$nulls":8},2252,null,8400,{"$nulls":12},1,1,1,-2,"C","I"]
[]
[null,"42.1.2 Principal agent: ..................................................\r\n",{"$nulls":8},2253,null,8500,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Postal address: .................................................. ..............................................Code: ..................\r\n",{"$nulls":8},2253,null,8500,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Tel: ............................Fax: ................................ E-mail: ..............................................................",{"$nulls":8},2253,null,8500,{"$nulls":12},1,1,1,-2,"C","I"]
[]
[null,"42.1.3 Agent (1) .............................................................\r\n",{"$nulls":8},2254,null,8600,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Agent's service: ...................................................\r\n",{"$nulls":8},2254,null,8600,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Postal address: ...................................................\r\n",{"$nulls":8},2254,null,8600,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"..............................................Code: ...................\r\n",{"$nulls":8},2254,null,8600,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Tel: ............................Fax: .................................\r\n",{"$nulls":8},2254,null,8600,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"E-mail: ...............................................................",{"$nulls":8},2254,null,8600,{"$nulls":12},1,1,1,-2,"C","I"]
[]
[null,"42.1.4 Agent (2) .............................................................\r\n",{"$nulls":8},2255,null,8700,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Agent's service: ...................................................\r\n",{"$nulls":8},2255,null,8700,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Postal address: ...................................................\r\n",{"$nulls":8},2255,null,8700,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"..............................................Code: ...................\r\n",{"$nulls":8},2255,null,8700,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Tel: ............................Fax: .................................\r\n",{"$nulls":8},2255,null,8700,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"E-mail: ...............................................................\r\n",{"$nulls":8},2255,null,8700,{"$nulls":12},1,1,1,-2,"C","I"]
[]
[null,"42.1.5 Agent (3) .............................................................\r\n",{"$nulls":8},2256,null,8800,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Agent's service: ...................................................\r\n",{"$nulls":8},2256,null,8800,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Postal address: ...................................................\r\n",{"$nulls":8},2256,null,8800,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"..............................................Code: ...................\r\n",{"$nulls":8},2256,null,8800,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Tel: ............................Fax: .................................\r\n",{"$nulls":8},2256,null,8800,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"E-mail: ...............................................................",{"$nulls":8},2256,null,8800,{"$nulls":12},1,1,1,-2,"C","I"]
[]
[null,"42.1.6 Agent (4) .............................................................\r\n",{"$nulls":8},2257,null,8900,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Agent's service: ...................................................\r\n",{"$nulls":8},2257,null,8900,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Postal address: ...................................................\r\n",{"$nulls":8},2257,null,8900,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"..............................................Code: ...................\r\n",{"$nulls":8},2257,null,8900,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Tel: ............................Fax: .................................\r\n",{"$nulls":8},2257,null,8900,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"E-mail: ...............................................................",{"$nulls":8},2257,null,8900,{"$nulls":12},1,1,1,-2,"C","I"]
[]
[null,"42.1.7 Agent (5) .............................................................\r\n",{"$nulls":8},2258,null,9000,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Agent's service: ...................................................\r\n",{"$nulls":8},2258,null,9000,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Postal address: ...................................................\r\n",{"$nulls":8},2258,null,9000,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"..............................................Code: ...................\r\n",{"$nulls":8},2258,null,9000,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Tel: ............................Fax: .................................\r\n",{"$nulls":8},2258,null,9000,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"E-mail: ...............................................................",{"$nulls":8},2258,null,9000,{"$nulls":12},1,1,1,-2,"C","I"]
[]
[null,"42.1.8 Agent (6) .............................................................\r\n",{"$nulls":8},2259,null,9100,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Agent's service: ...................................................\r\n",{"$nulls":8},2259,null,9100,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Postal address: ...................................................\r\n",{"$nulls":8},2259,null,9100,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"..............................................Code: ...................\r\n",{"$nulls":8},2259,null,9100,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Tel: ............................Fax: .................................\r\n",{"$nulls":8},2259,null,9100,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"E-mail: ...............................................................",{"$nulls":8},2259,null,9100,{"$nulls":12},1,1,1,-2,"C","I"]
[]
[null,"42.1.9 Agent (7) .............................................................\r\n",{"$nulls":8},2260,null,9200,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Agent's service: ...................................................\r\n",{"$nulls":8},2260,null,9200,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Postal address: ...................................................\r\n",{"$nulls":8},2260,null,9200,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"..............................................Code: ...................\r\n",{"$nulls":8},2260,null,9200,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"Tel: ............................Fax: .................................\r\n",{"$nulls":8},2260,null,9200,{"$nulls":12},1,1,1,-2,"C","I"]
[null,"E-mail: ...............................................................",{"$nulls":8},2260,null,9200,{"$nulls":12},1,1,1,-2,"C","I"]
[]
[null,"42.2 CONTRACT DETAILS",{"$nulls":8},2261,null,9300,{"$nulls":12},1,1,1,-2,"S","I"]
[]
["54","42.2.1 Works description: ...............................................  ...........................................................................\r\n",{"$nulls":8},2262,null,9400,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"...........................................................................\r\n",{"$nulls":8},2262,null,9400,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"...........................................................................","Item",1,null,0,null,null,1,null,2262,null,9400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["55","42.2.3 Work or installations by direct contractors .............\r\n",{"$nulls":8},2263,null,9600,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"...........................................................................\r\n",{"$nulls":8},2263,null,9600,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"...........................................................................\r\n",{"$nulls":8},2263,null,9600,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"...........................................................................\r\n",{"$nulls":8},2263,null,9600,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"...........................................................................\r\n",{"$nulls":8},2263,null,9600,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"...........................................................................\r\n",{"$nulls":8},2263,null,9600,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"...........................................................................\r\n",{"$nulls":8},2263,null,9600,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"...........................................................................","Item",1,null,0,null,null,1,null,2263,null,9600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["56","42.2.2 Site description: ..................................................\r\n",{"$nulls":8},2264,null,9500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"..........................................................................\r\n",{"$nulls":8},2264,null,9500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"..........................................................................\r\n",{"$nulls":8},2264,null,9500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"..........................................................................","Item",1,null,0,null,null,1,null,2264,null,9500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["57","42.2.4 Specific options that are applicable to a state  organ only\r\n",{"$nulls":8},2265,null,9700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Where so:\r\n",{"$nulls":8},2265,null,9700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"(1) Interest rate legislation: ............................... \r\n",{"$nulls":8},2265,null,9700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"(2) Lateral support insurance to be effected by the  contractor    ? yes/no ?\r\n",{"$nulls":8},2265,null,9700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"(3) Payment will be made for materials and goods       ? yes/no ?\r\n",{"$nulls":8},2265,null,9700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"(4) Dispute resolution by litigation ? yes/no ?\r\n",{"$nulls":8},2265,null,9700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"(5) Extended defects liability period applicable \r\n",{"$nulls":8},2265,null,9700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"to the following elements: ................................ ......................................................................\r\n",{"$nulls":8},2265,null,9700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2265,null,9700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2265,null,9700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2265,null,9700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................","Item",1,null,0,null,null,1,null,2265,null,9700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["58","42.2.5 Possession of the site is intended to be given on       (date)..............................................................","Item",1,null,0,null,null,1,null,2266,null,9800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["59","42.2.6 Period for the commencement of the works after \r\n",{"$nulls":8},2267,null,9900,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"the contractor takes possession of the site  (No of working days) .......................................","Item",1,null,0,null,null,1,null,2267,null,9900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["60","42.2.7 For the works as a whole: The date for practical  completion and the penalty per calendar day\r\n",{"$nulls":8},2268,null,10000,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Date ............................. Penalty R.......................","Item",1,null,0,null,null,1,null,2268,null,10000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["61","42.2.8 For the works in sections:  The date for practical  completion and the penalty per calendar day  Section 1 Date .................... Penalty R..................\r\n",{"$nulls":8},2269,null,10100,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Section 2 Date .................... Penalty R..................\r\n",{"$nulls":8},2269,null,10100,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Section 3 Date .................... Penalty R..................\r\n",{"$nulls":8},2269,null,10100,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Section 4 Date .................... Penalty R..................\r\n",{"$nulls":8},2269,null,10100,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Section 5 Date .................... Penalty R .................\r\n",{"$nulls":8},2269,null,10100,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Section 6 Date .................... Penalty R .................","Item",1,null,0,null,null,1,null,2269,null,10100,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["62","42.2.9 The law applicable to this agreement shall be that \r\n",{"$nulls":8},2270,null,10200,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"of (country) .........................................................","Item",1,null,0,null,null,1,null,2270,null,10200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"42.3 INSURANCES",{"$nulls":8},2271,null,10300,{"$nulls":12},1,1,1,-2,"S","I"]
[]
["63","42.3.1 Contract works insurance to be effected by \r\n",{"$nulls":8},2272,null,10400,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"? employer ? contractor ?\r\n",{"$nulls":8},2272,null,10400,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"For the sum of:          R ...................................\r\n",{"$nulls":8},2272,null,10400,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"With a deductible of:  R ...................................","Item",1,null,0,null,null,1,null,2272,null,10400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["64","42.3.2 Supplementary insurance is required - ? yes/no ?\r\n",{"$nulls":8},2273,null,10500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"If \"yes\" state requirement ..................................","Item",1,null,0,null,null,1,null,2273,null,10500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["65","42.3.3 Public liability insurance to be effected by \r\n",{"$nulls":8},2274,null,10600,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"? employer ? contractor ?\r\n",{"$nulls":8},2274,null,10600,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"For the sum of:     R.....................................\r\n",{"$nulls":8},2274,null,10600,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"With a deductible of:  R.....................................","Item",1,null,0,null,null,1,null,2274,null,10600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["66","42.3.4 Support insurance to be effected by employer\r\n",{"$nulls":8},2275,null,10700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"For the sum of:  R.....................................\r\n",{"$nulls":8},2275,null,10700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"With a deductible of: R.....................................","Item",1,null,0,null,null,1,null,2275,null,10700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"42.4 DOCUMENTS",{"$nulls":8},2276,null,10800,{"$nulls":12},1,1,1,-2,"S","I"]
[]
["67","42.4.1 Waiver of the contractor's lien or right of continuing  posession is required - ? yes/no ?","Item",1,null,0,null,null,1,null,2277,null,10900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["68","42.4.2 Construction document copies to be supplied to the  contractor free of charge  (No of .......)","Item",1,null,0,null,null,1,null,2278,null,11000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["69","42.4.3 State measuring system used for drawing up bills \r\n",{"$nulls":8},2279,null,11100,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"of quantities (lump sum document?) ..................... ..........................................................................","Item",1,null,0,null,null,1,null,2279,null,11100,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["70","42.4.4 Number of working days for submission of priced \r\n",{"$nulls":8},2280,null,11200,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"documents     (No of .......)","Item",1,null,0,null,null,1,null,2280,null,11200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["71","42.4.5 JBCC Engineering General Conditions are to \r\n",{"$nulls":8},2281,null,11300,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"be included in the contract documents - ? yes/no ?","Item",1,null,0,null,null,1,null,2281,null,11300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["72","42.4.6 The contract value is to be adjusted using CPAP  indices ? yes/no ?\r\n",{"$nulls":8},2282,null,11400,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"\r\n",{"$nulls":8},2282,null,11400,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Where CPAP is to be used (base month) ............\r\n",{"$nulls":8},2282,null,11400,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"\r\n",{"$nulls":8},2282,null,11400,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Alternative indices (if applicable) .........................","Item",1,null,0,null,null,1,null,2282,null,11400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["73","42.4.7 Details of changes made to the provisions of\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"JBCC standard documentation - .................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................\r\n",{"$nulls":8},2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"......................................................................","Item",1,null,0,null,null,1,null,2283,null,11500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"SECTION B - PRELIMINARIES",{"$nulls":8},2284,null,12000,{"$nulls":12},1,1,1,-2,"H","0"]
[]
[null,"Definitions and interpretation",{"$nulls":8},2285,null,12100,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["74","Clause 1.0 - Definitions and interpretation","Item",1,null,0,null,null,1,null,2286,null,12200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Documents",{"$nulls":8},2287,null,12300,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["75","Clause 2.1 - Checking of documents","Item",1,null,0,null,null,1,null,2288,null,12400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["76","Clause 2.2 - Provisional bills of quantities","Item",1,null,0,null,null,1,null,2289,null,12500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["77","Clause 2.3 - Availability of construction documentation","Item",1,null,0,null,null,1,null,2292,null,12900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["78","?The budgetary allowances and ?selected? (nominated?) subcontract amounts allocated for subsequent trades included in this document will be separately procured, based on multiple procurement of ?selected? (nominated?) subcontractors during the construction period?","Item",1,null,0,null,null,1,null,2293,null,13000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["79","Clause 2.4 - Interests of agents","Item",1,null,0,null,null,1,null,2294,null,13100,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["80","Clause 2.5 - Priced documents","Item",1,null,0,null,null,1,null,2295,null,13200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["81","Clause 2.6 - Tender submission","Item",1,null,0,null,null,1,null,2296,null,13300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["82","Tenders shall be valid for a period of ? days from the closing date of tenders?","Item",1,null,0,null,null,1,null,2297,null,13400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"The site",{"$nulls":8},2298,null,13500,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["83","Clause 3.1 - Defined works area","Item",1,null,0,null,null,1,null,2299,null,13600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["84","The area of the works to be occupied by the contractor is indicated on architect's drawing","Item",1,null,0,null,null,1,null,2300,null,13700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["85","Clause 3.2 - Geotechnical investigation","Item",1,null,0,null,null,1,null,2301,null,13800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["86","?No geotechnical investigation report is available?","Item",1,null,0,null,null,1,null,2302,null,13900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["87","?A copy of the geotechnical investigation report is annexed to these bills of quantities?","Item",1,null,0,null,null,1,null,2303,null,14000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["88","Clause 3.3 -  Inspection of the site","Item",1,null,0,null,null,1,null,2304,null,14100,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["89","Clause 3.4 - Existing premises occupied","Item",1,null,0,null,null,1,null,2305,null,14200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["90","Clause 3.5 - Previous work - dimensional accuracy","Item",1,null,0,null,null,1,null,2306,null,14300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["91","Clause 3.6 - Previous work - defects","Item",1,null,0,null,null,1,null,2307,null,14400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["92","Clause 3.7 - Services - known","Item",1,null,0,null,null,1,null,2308,null,14500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["93","Clause 3.8 - Services - unknown","Item",1,null,0,null,null,1,null,2309,null,14600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["94","Clause 3.9 - Protection of trees","Item",1,null,0,null,null,1,null,2310,null,14700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["95","Clause 3.10 - Articles of value","Item",1,null,0,null,null,1,null,2311,null,14800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["96","Clause 3.11 - Inspection of adjoining properties","Item",1,null,0,null,null,1,null,2312,null,14900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Management of contract",{"$nulls":8},2313,null,15000,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["97","Clause 4.1 - Management of the works","Item",1,null,0,null,null,1,null,2314,null,15100,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["98","Clause 4.2 - Programme for the works","Item",1,null,0,null,null,1,null,2315,null,15200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["99","Clause 4.3 - Progress meetings","Item",1,null,0,null,null,1,null,2316,null,15300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["100","Clause 4.4 - Technical meetings","Item",1,null,0,null,null,1,null,2317,null,15400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["101","Clause 4.5 - Labour and plant records","Item",1,null,0,null,null,1,null,2318,null,15500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Samples, shop drawings and manufacturer's instructions",{"$nulls":8},2319,null,15600,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["102","Clause 5.1 - Samples of materials","Item",1,null,0,null,null,1,null,2320,null,15700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["103","Clause 5.2 - Workmanship samples","Item",1,null,0,null,null,1,null,2321,null,15800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["104","Clause 5.3 - Shop drawings","Item",1,null,0,null,null,1,null,2322,null,15900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["105","Clause 5.4 - Compliance with manufacturers' instructions","Item",1,null,0,null,null,1,null,2323,null,16000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Temporary works and plant",{"$nulls":8},2324,null,16100,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["106","Clause 6.1 - Deposits and fees","Item",1,null,0,null,null,1,null,2325,null,16200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["107","Clause 6.2 - Enclosure of the works","Item",1,null,0,null,null,1,null,2326,null,16300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["108","Clause 6.3 - Advertising","Item",1,null,0,null,null,1,null,2327,null,16400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["109","Clause 6.4 - Plant, equipment, sheds and offices","Item",1,null,0,null,null,1,null,2328,null,16500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["110","Clause 6.5 - Main noticeboard","Item",1,null,0,null,null,1,null,2329,null,16600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["111","Clause 6.6 - Subcontractors' noticeboard","Item",1,null,0,null,null,1,null,2330,null,16700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Temporary services",{"$nulls":8},2331,null,16800,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["112","Clause 7.1 - Location","Item",1,null,0,null,null,1,null,2332,null,16900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["113","Clause 7.2 - Water","Item",1,null,0,null,null,1,null,2333,null,17000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["114","Clause 7.3 - Electricity","Item",1,null,0,null,null,1,null,2334,null,17100,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["115","Clause 7.4 - Telecommunication facilities","Item",1,null,0,null,null,1,null,2335,null,17200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["116","Clause 7.5 - Ablution facilities","Item",1,null,0,null,null,1,null,2336,null,17300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Prime cost amounts",{"$nulls":8},2337,null,17400,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["117","Clause 8.1 - Responsibility for prime cost amounts","Item",1,null,0,null,null,1,null,2338,null,17500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Attendance on nominated/selected subcontractors",{"$nulls":8},2339,null,17600,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["118","Clause 9.1 - General attendance","Item",1,null,0,null,null,1,null,2340,null,17700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["119","Clause 9.2 - Special attendance","Item",1,null,0,null,null,1,null,2341,null,17800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["120","Clause 9.3 - Commissioning - fuel, water and electricity","Item",1,null,0,null,null,1,null,2342,null,17900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Financial aspects",{"$nulls":8},2343,null,18000,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["121","Clause 10.1 - Statutory taxes, duties and levies","Item",1,null,0,null,null,1,null,2344,null,18100,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["122","Provision is made in the summary of these bills of quantities for the inclusion of Value Added Tax (VAT)","Item",1,null,0,null,null,1,null,2345,null,18200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["123","Clause 10.2 - Payment of preliminaries","Item",1,null,0,null,null,1,null,2346,null,18300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["124","Clause 10.3 - Adjustment of preliminaries","Item",1,null,0,null,null,1,null,2347,null,18400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["125","Should the contractor select Option B but fail to provide the information required prior to the signing of the contract, the principal agent shall have the right to select either Option A or B for the adjustment of preliminaries.  If the principal agent selects Option B he shall be entitled to make assumptions at his discretion regarding the information which the contractor would normally have provided prior to the signing of the contract","Item",1,null,0,null,null,1,null,2348,null,18500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["126","Clause 10.4 - Payment certificate cash flow","Item",1,null,0,null,null,1,null,2349,null,18600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"General",{"$nulls":8},2350,null,18700,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["127","Clause 11.1 - Protection of the works","Item",1,null,0,null,null,1,null,2351,null,18800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["128","Clause 11.2 - Protection/isolation of existing/sectionally occupied works","Item",1,null,0,null,null,1,null,2352,null,18900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["129","Clause 11.3 - Security of the works","Item",1,null,0,null,null,1,null,2353,null,19000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["130","Clause 11.4 - Notice before covering work","Item",1,null,0,null,null,1,null,2354,null,19100,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["131","Clause 11.5 - Disturbance","Item",1,null,0,null,null,1,null,2355,null,19200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["132","Clause 11.6 - Environmental disturbance","Item",1,null,0,null,null,1,null,2356,null,19300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["133","?A copy of the environmental management plan is annexed to these bills of quantities.  The contractor shall comply with all the requirements of such environmental management plan?","Item",1,null,0,null,null,1,null,2357,null,19400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["134","Clause 11.7 - Works cleaning and clearing","Item",1,null,0,null,null,1,null,2358,null,19500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["135","Clause 11.8 - Vermin","Item",1,null,0,null,null,1,null,2359,null,19600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["136","Clause 11.9 - Overhand work","Item",1,null,0,null,null,1,null,2360,null,19700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["137","Clause 11.10 - Instruction manuals and guarantees","Item",1,null,0,null,null,1,null,2361,null,19800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["138","Clause 11.11 - As built information","Item",1,null,0,null,null,1,null,2362,null,19900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["139","Clause 11.12 - Tenant installations","Item",1,null,0,null,null,1,null,2363,null,20000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Schedule of variables",{"$nulls":8},2364,null,20100,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["140","12.1 - Pre-tender information","Item",1,null,0,null,null,1,null,2365,null,20200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["141","Information necessary for elections and completion of those clauses contained in the schedule which are necessary for tender purposes is given hereunder.  Where no information is given it shall mean that either specific requirements are not required or that the clause is not relevant to this specific contract","Item",1,null,0,null,null,1,null,2366,null,20300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["142","12.1.1 - Provisional bills of quantities [clause 2.2]","Item",1,null,0,null,null,1,null,2367,null,20400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["143","The quantities are provisional - ? yes/no ?","Item",1,null,0,null,null,1,null,2368,null,20500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["144","12.1.2 - Availability of construction documentation [clause 2.3]","Item",1,null,0,null,null,1,null,2369,null,20600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["145","Construction documentation is complete - ? yes/no ?","Item",1,null,0,null,null,1,null,2370,null,20700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["146","12.1.3 - Interests of agents [clause 2.4]","Item",1,null,0,null,null,1,null,2371,null,20800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["147","12.1.4 - Defined works area [clause 3.1]","Item",1,null,0,null,null,1,null,2372,null,20900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["148","12.1.5 - Geotechnical investigation [clause 3.2]","Item",1,null,0,null,null,1,null,2373,null,21000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["149","12.1.6 - Existing premises occupied [clause 3.4]","Item",1,null,0,null,null,1,null,2374,null,21100,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["150","12.1.7 - Previous work - dimensional accuracy [clause 3.5]","Item",1,null,0,null,null,1,null,2375,null,21200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["151","12.1.8 - Previous work - defects [clause 3.6]","Item",1,null,0,null,null,1,null,2376,null,21300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["152","12.1.9 - Services - known [clause 3.7]","Item",1,null,0,null,null,1,null,2377,null,21400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["153","12.1.10 - Protection of trees [clause 3.9]","Item",1,null,0,null,null,1,null,2378,null,21500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["154","12.1.11 - Inspection of adjoining properties [clause 3.11]","Item",1,null,0,null,null,1,null,2379,null,21600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["155","12.1.12 - Enclosure of the works [clause 6.2]","Item",1,null,0,null,null,1,null,2380,null,21700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["156","12.1.13 - Offices [clause 6.4.3]","Item",1,null,0,null,null,1,null,2381,null,21800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["157","12.1.14 - Main noticeboard [clause 6.5]","Item",1,null,0,null,null,1,null,2382,null,21900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["158","12.1.15 - Subcontractors' noticeboard [clause 6.6]","Item",1,null,0,null,null,1,null,2383,null,22000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["159","A noticeboard is required - ? yes/no ?","Item",1,null,0,null,null,1,null,2384,null,22100,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["160","12.1.16 - Water [clause 7.2]","Item",1,null,0,null,null,1,null,2385,null,22200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["161","Option A (by contractor)    ? yes/no ?\r\n",{"$nulls":8},2386,null,22300,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Option B (by employer - free of charge)   ? yes/no ?\r\n",{"$nulls":8},2386,null,22300,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Option C (by employer - metered)   ? yes/no ?","Item",1,null,0,null,null,1,null,2386,null,22300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["162","12.1.17 - Electricity [clause 7.3]","Item",1,null,0,null,null,1,null,2387,null,22400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["163","Option A (by contractor)    ? yes/no ?\r\n",{"$nulls":8},2388,null,22500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Option B (by employer - free of charge)   ? yes/no ?\r\n",{"$nulls":8},2388,null,22500,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Option C (by employer - metered)   ? yes/no ?\r\n","Item",1,null,0,null,null,1,null,2388,null,22500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["164","12.1.18 - Telecommunications [clause 7.4]","Item",1,null,0,null,null,1,null,2389,null,22600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["165","Telephone   ? yes/no ?\r\n",{"$nulls":8},2390,null,22700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Facsimile    ? yes/no ?\r\n",{"$nulls":8},2390,null,22700,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"E-mail   ? yes/no ?","Item",1,null,0,null,null,1,null,2390,null,22700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["166","12.1.19 - Ablution facilities [clause 7.5]","Item",1,null,0,null,null,1,null,2391,null,22800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["167","Option A (by contractor)   ? yes/no ?\r\n",{"$nulls":8},2392,null,22900,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Option B (by employer)    ? yes/no ?","Item",1,null,0,null,null,1,null,2392,null,22900,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["168","12.1.20 - Protection/isolation of existing/sectionally occupied works [clause 11.2]","Item",1,null,0,null,null,1,null,2393,null,23000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["169","Protection/isolation is required - ? yes/no ?","Item",1,null,0,null,null,1,null,2394,null,23100,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["170","12.1.21 - Special attendance [clause 9.2]","Item",1,null,0,null,null,1,null,2395,null,23200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["171","12.1.22 - Protection of the works [clause 11.1]","Item",1,null,0,null,null,1,null,2396,null,23300,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["172","12.1.23 - Disturbance [clause 11.5]","Item",1,null,0,null,null,1,null,2397,null,23400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["173","12.1.24 - Environmental disturbance [clause 11.6]","Item",1,null,0,null,null,1,null,2398,null,23500,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["174","12.2 - Post-tender information","Item",1,null,0,null,null,1,null,2399,null,23600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
["175","The required post-tender information shall be inserted in the preliminaries after consultation with the contractor","Item",1,null,0,null,null,1,null,2400,null,23700,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"SECTION C - SPECIFIC PRELIMINARIES",{"$nulls":8},2401,null,24020,{"$nulls":12},1,1,1,-2,"H","0"]
[]
[null,"User Notes-",{"$nulls":8},2402,null,24150,{"$nulls":12},1,1,1,-2,"S","I"]
[]
[null,"User Note - All information for this section requires consultation with the contractor.  The principal agent should not pre-select any of the alternatives available to the contractor",{"$nulls":8},2403,null,24200,{"$nulls":12},1,1,1,-2,"C","I"]
[]
[null,"User Note - Selected examples of typical clauses are provided to show possible ways of describing such clauses.  Users must delete, adapt or add to these examples to suit their particular circumstances",{"$nulls":8},2404,null,-1,{"$nulls":12},1,1,1,-2,"C","I"]
[]
[null,"Site instructions",{"$nulls":8},2405,null,24300,{"$nulls":12},1,1,1,-2,"S","I"]
[]
["176","Site instructions issued on site are to be recorded in triplicate in a site instruction book which is to be provided and maintained on site by the contractor","Item",1,null,0,null,null,1,null,2406,null,24400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Warranties for materials and workmanship",{"$nulls":8},2407,null,24500,{"$nulls":12},1,1,1,-2,"S","I"]
[]
["177","Where warranties for materials are called for, the contractor shall obtain a written warranty, addressed to the employer, from the firm supplying the materials and/or doing the work and shall deliver same to the principal agent on the certified completion of the contract.  The warranty shall state that workmanship, materials and installation are warranteed for a specified period from the date of certified completion of the contract, and that any defects that may arise during the specified period shall be made good at the expense of the firm supplying the materials and/or doing the work, upon written notice to do so.  The warranty will not be enforced if the work is damaged by defects in the construction of the building in which case the responsibility for replacement shall rest entirely with the contractor.","Item",1,null,0,null,null,1,null,2408,null,24600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Co-operation of contractor for cost management",{"$nulls":8},2409,null,24700,{"$nulls":12},1,1,1,-2,"S","I"]
[]
["178","It is specifically agreed that the contractor accepts the obligation of assisting the principal agent in implementing proper cost management.  The contractor will be advised by the principal agent of all cost management procedures which will be implemented to ensure that the final building cost does not exceed the budget.  The principal agent undertakes to make available to the contractor all budgetary allowances and cost assessments/reports to enable the proper procedures to be implemented and the contractor shall attend all cost plan review and cost management meetings.  The contractor undertakes to extend these procedures, as necessary, to all subcontractors","Item",1,null,0,null,null,1,null,2410,null,24800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Confidentiality",{"$nulls":8},2411,null,24900,{"$nulls":12},1,1,1,-2,"S","I"]
[]
["179","The contractor undertakes to maintain in confidence any and all information regarding this project and shall obtain appropriate similar undertakings from all subcontractors and suppliers.  Such information shall not be used in any way except in connection with the execution of the works\r\n",{"$nulls":8},2412,null,25000,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"\r\n",{"$nulls":8},2412,null,25000,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"No information regarding this project shall be published or disclosed without the prior written consent of the employer","Item",1,null,0,null,null,1,null,2412,null,25000,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Propping of floors below",{"$nulls":8},2413,null,25100,{"$nulls":12},1,1,1,-2,"S","I"]
[]
["180","The contractor is advised that propping of floors below may be required if he wishes to use any areas of completed suspended reinforced concrete slabs for vehicle access, storage of materials and goods and location of plant, scaffolding, etc.  The location of these areas and any necessary propping shall be approved by the principal agent and the cost thereof shall be borne by the contractor","Item",1,null,0,null,null,1,null,2414,null,25200,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Testing of windows for watertightness",{"$nulls":8},2415,null,25300,{"$nulls":12},1,1,1,-2,"S","I"]
[]
["181","Each window shall be tested for watertightness with water sprayed on by means of a 20mm hosepipe using adequate pressure.  If in the opinion of the principal agent, the pressure proves to be inadequate, then the pressure in the hosepipe shall be boosted by means of compressed air or other approved means","Item",1,null,0,null,null,1,null,2416,null,25400,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"Testing of flat roof waterproofing for watertightness",{"$nulls":8},2417,null,25500,{"$nulls":12},1,1,1,-2,"S","I"]
[]
["182","Flat roof waterproof areas shall be prepared with small sand dykes around them of a size and enclosing an area approved by the principal agent, flooded with water and kept \"ponded\" for at least 36 hours as a test to ensure the watertightness of the waterproofing and before any further construction work is carried out above the waterproofing","Item",1,null,0,null,null,1,null,2418,null,25600,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[null,"SUMMARY OF CATEGORIES",{"$nulls":8},2419,null,25700,{"$nulls":12},1,1,1,-2,"H","0"]
[]
[null,"Categories",{"$nulls":8},2420,null,648698,{"$nulls":12},1,1,1,-2,"S","0"]
[]
["183","Category: Fixed F:..............................\r\n",{"$nulls":8},2421,null,25800,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"\r\n",{"$nulls":8},2421,null,25800,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Category: Value V:..............................\r\n",{"$nulls":8},2421,null,25800,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"\r\n",{"$nulls":8},2421,null,25800,{"$nulls":12},1,1,1,-2,"I","I"]
[null,"Category: Time T:................................","Item",1,null,0,null,null,1,null,2421,null,25800,{"$nulls":12},1,1,1,-2,"I","I"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[null,"Section Total ",{"$nulls":4},0]
[]
[]
[null,"SECTION NO. 2 : BUILDINGS",{"$nulls":23},1,2,1,3,"H"]
[]
[]
[null,"BILL NO.1 : ALTERATIONS",{"$nulls":23},1,2,1,3,"H"]
[]
[null,"SUPPLEMENTARY PREAMBLES",{"$nulls":8},1922,null,340,{"$nulls":12},1,2,1,3,"H","0"]
[]
[null,"View site",{"$nulls":8},1923,null,370,{"$nulls":12},1,2,1,3,"S","0"]
[]
[null,"Before submitting his tender the tenderer shall visit the site and satisfy himself as to the nature and extent of the work to be done and the value of the materials salvageable from the alterations.  No claim for any variations of the contract sum in respect of the nature and extent of the work or of inferior or damaged materials will be entertained",{"$nulls":8},1924,null,380,{"$nulls":12},1,2,1,3,"C","0"]
[]
[null,"General",{"$nulls":8},1925,null,410,{"$nulls":12},1,2,1,3,"S","0"]
[]
[null,"Note to tenderers: The removal, storage ,disposal, etc  of asbestos sheeting, etc to be executed in strict accordance to the bye laws (OHS) regarding same by a specialist asbestos sub-contractor. Prices to include for this.",{"$nulls":8},2498,null,410,{"$nulls":12},1,2,1,3,"C","0"]
[]
[null,"The contractor shall carry out the whole of the works with as little mess and noise as possible and with a minimum of disturbance to tenants in the building and to adjoining premises and their tenants. He shall provide proper protection and provide , erect and remove when directed , any temporary tarpaulins that may be necessary during the progress of the works, all to the satisfaction of the principal agent",{"$nulls":8},1926,null,420,{"$nulls":12},1,2,1,3,"C","0"]
[]
[null,"Doors, fanlights, windows, fittings, frames, linings, etc which are to remain the property of the employer shall be carefully taken out, temporarily stored",{"$nulls":8},1927,null,430,{"$nulls":12},1,2,1,3,"C","0"]
[]
[null,"Doors, fanlights, windows, fittings, frames, linings, etc which are to be re-used shall be thoroughly overhauled before refixing including taking off, easing and rehanging, cramping up, re-wedging as required and making good cramps, dowels, etc, and oiling, adjusting and repairing ironmongery  as  necessary, replacing any glass damaged in removal or subsequently and stopping up all nail and screw holes with tinted plastic wood to match timber, unless otherwise described . Re-painting or re-varnishing is given separately",{"$nulls":8},1928,null,440,{"$nulls":12},1,2,1,3,"C","0"]
[]
[null,"The contractor will be required to take all dimensions affecting the existing buildings on the site and he will be held solely responsible for the accuracy of all such dimensions where used in the manufacture of new items (doors, windows, fittings, etc.)",{"$nulls":8},1930,null,490,{"$nulls":12},1,2,1,3,"C","0"]
[]
[null,"REMOVAL OF EXISTING WORK",{"$nulls":8},1879,null,570,{"$nulls":12},1,2,1,3,"H","0"]
[]
[null,"Breaking up and removing reinforced concrete, including cutting off and removing reinforcement",{"$nulls":8},2501,null,610,{"$nulls":12},1,2,1,3,"S","0"]
[]
["1","170mm Thick surface beds","m²",15,null,0,null,null,15,null,2502,null,650,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"Breaking down and removing brickwork etc",{"$nulls":8},2126,null,690,{"$nulls":12},1,2,1,3,"S","0"]
[]
[null,"Taking out and removing doors, windows, etc, including thresholds, sills, etc",{"$nulls":8},1887,null,860,{"$nulls":12},1,2,1,3,"S","0"]
[]
["2","Timber single door and frame, size 813 x 2032mm high","No",32,null,0,null,null,32,null,1888,null,870,{"$nulls":12},1,2,1,3,"I","N"]
[]
["3","Timber single door and frame, size 900 x 2032mm high","No",1,null,0,null,null,1,null,2644,null,870,{"$nulls":12},1,2,1,3,"I","N"]
[]
["4","Glazing from steel window","m²",27,null,0,null,null,27,null,2105,null,910,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"Taking down and removing roofs, floors, panelling, ceilings, partitions, etc",{"$nulls":8},1890,null,1080,{"$nulls":12},1,2,1,3,"S","0"]
[]
["5","Corrugated sheet steel roof covering and steel purlins","m²",355,null,0,null,null,355,null,2499,null,1090,{"$nulls":12},1,2,1,3,"I","2"]
[]
["6","Fibre cement fascias and bargeboards","m",152,null,0,null,null,152,null,2073,null,1090,{"$nulls":12},1,2,1,3,"I","1"]
[]
["7","Gutters and rainwater pipes","m",76,null,0,null,null,76,null,2072,null,1100,{"$nulls":12},1,2,1,3,"I","1"]
[]
["8","Gypsum plasterboard ceilings, including timber brandering, cornices, etc","m²",933,null,0,null,null,933,null,1891,null,1140,{"$nulls":12},1,2,1,3,"I","2"]
[]
["9","Trap door","No",6,null,0,null,null,6,null,2097,null,1140,{"$nulls":12},1,2,1,3,"I","N"]
[]
[null,"Taking out and removing sundry joinery work, fittings, etc",{"$nulls":8},1893,null,1180,{"$nulls":12},1,2,1,3,"S","0"]
[]
["10","Timber skirtings","m","  1 473",null,0,null,null,1473,null,2094,null,1200,{"$nulls":12},1,2,1,3,"I","1"]
[]
["11","3000 x 2000mm Pinning boards","m",2,null,0,null,null,2,null,2666,null,1200,{"$nulls":12},1,2,1,3,"I","1"]
[]
[null,"Taking up and removing wood block floor coverings, vinyl floor coverings, carpets, etc and preparing screeds for new floor coverings",{"$nulls":8},1895,null,1340,{"$nulls":12},1,2,1,3,"S","0"]
[]
["12","Vinyl tile floor covering","m²","  3 167",null,0,null,null,3167,null,1896,null,1360,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"Taking out and removing ironmongery",{"$nulls":8},2648,null,1390,{"$nulls":12},1,2,1,3,"S","0"]
[]
["13","Grab rail 600mm long from wall","No",2,null,0,null,null,2,null,2649,null,1420,{"$nulls":12},1,2,1,3,"I","N"]
[]
[null,"Taking out/off and removing sundry metalwork",{"$nulls":8},1900,null,1450,{"$nulls":12},1,2,1,3,"S","0"]
[]
["14","Steel cupboards, 1050 x 500 x 2100mm high","No",2,null,0,null,null,2,null,2556,null,1470,{"$nulls":12},1,2,1,3,"I","N"]
[]
[null,"Hacking up/off and removing granolithic, screeds, plaster, etc from concrete or brickwork and preparing surfaces for new screed, plaster, tile finishes, etc",{"$nulls":8},1903,null,1500,{"$nulls":12},1,2,1,3,"S","0"]
[]
["15","30mm Screed from floor","m²",42,null,0,null,null,42,null,2531,null,1560,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"Hacking up/off and removing ceramic tiles including  removing mortar bed or adhesive from concrete or brickwork and preparing surfaces for new screed, plaster, tile finish, etc",{"$nulls":8},1906,null,1590,{"$nulls":12},1,2,1,3,"S","0"]
[]
["16","Tiles to walls","m²",5,null,0,null,null,5,null,2125,null,1620,{"$nulls":12},1,2,1,3,"I","2"]
[]
["17","Tiles to floors","m²",32,null,0,null,null,32,null,2659,null,1620,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"Taking out and removing sanitary fittings, tanks, geysers, etc, including disconnecting from pipes, traps, etc and making good floor and wall finishes (making good tiling and paintwork elsewhere)",{"$nulls":8},1911,null,1680,{"$nulls":12},1,2,1,3,"S","0"]
[]
["18","Vitreous china wash hand basin","No",1,null,0,null,null,1,null,1912,null,1710,{"$nulls":12},1,2,1,3,"I","N"]
[]
["19","Vitreous china WC pan with cistern and flush pipe","No",1,null,0,null,null,1,null,1913,null,1720,{"$nulls":12},1,2,1,3,"I","N"]
[]
["20","Vitreous china urinal and flush pipe","No",1,null,0,null,null,1,null,2616,null,1720,{"$nulls":12},1,2,1,3,"I","N"]
[]
["21","Stainless steel urinal 2m long","No",2,null,0,null,null,2,null,2660,null,1720,{"$nulls":12},1,2,1,3,"I","N"]
[]
["22","CP star pillar taps","No",1,null,0,null,null,1,null,2137,null,1720,{"$nulls":12},1,2,1,3,"I","N"]
[]
["23","CP shower head","No",1,null,0,null,null,1,null,2672,null,1720,{"$nulls":12},1,2,1,3,"I","N"]
[]
[null,"Servicing of existing work",{"$nulls":8},2527,null,1720,{"$nulls":12},1,2,1,3,"S","0"]
[]
["24","Investigate and isolate tap leap and repair","No",3,null,0,null,null,3,null,2528,null,1720,{"$nulls":12},1,2,1,3,"I","N"]
[]
[null,"BUILDING UP OPENINGS",{"$nulls":8},2128,null,1890,{"$nulls":12},1,2,1,3,"H","0"]
[]
[null,"Brickwork in NFP bricks in class II mortar in building up openings, including bonding new to existing and making good cement plaster on one (both?) side(s) (making good paintwork elsewhere)",{"$nulls":8},2129,null,1940,{"$nulls":12},1,2,1,3,"S","0"]
[]
["25","One brick wall","m²",10,null,0,null,null,10,null,2130,null,1950,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"MAKING GOOD OF FINISHES ETC",{"$nulls":8},1918,null,2080,{"$nulls":12},1,2,1,3,"H","0"]
[]
[null,"Making good facebrick",{"$nulls":8},2674,null,2080,{"$nulls":12},1,2,1,3,"S","0"]
[]
["26","Chipped face brickwork","m²",28,null,0,null,null,28,null,2675,null,2080,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"Making good existing cement screeds",{"$nulls":8},2670,null,2080,{"$nulls":12},1,2,1,3,"S","0"]
[]
["27","30mm Thick screeds in floors in patches","m²",42,null,0,null,null,42,null,2671,null,2080,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"Pavelite steel trowelled on existing screed",{"$nulls":8},1920,null,2230,{"$nulls":12},1,2,1,3,"S"]
[]
["28","Average 4mm thick on floors and landings","m²","  3 167",null,0,null,null,3167,null,2074,null,2230,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"Wire brush along length of crack and ream open cracks 20mm width x 20mm deep and scratch out any debris that may block the crack in the sides of the hole. Epoxy R8 bars in grooves at 250mm centres over the crack length. Fill the \"V\" grooves and plaster with structural mortar and mesh ref 100.",{"$nulls":8},1934,null,2230,{"$nulls":12},1,2,1,3,"S","0"]
[]
["29","On cracks on plastered walls","m",292,null,0,null,null,292,null,1935,null,2230,{"$nulls":12},1,2,1,3,"I","1"]
[]
[null,"Chip open the crack to form a \"V\" shape 20mm wide x 10mm deep and scratch out the debris that may block the crack in the sides of the hole. Grinding in the floor approximately 200mm to 300mm apart from the rebar to be placed into an epoxy repair mortar 'SIKA TOP-ARMATEC 100'. Fill the crack with structural epoxy repair mortar 'SIKA MONO TOP 615HB'",{"$nulls":8},1936,null,2230,{"$nulls":12},1,2,1,3,"S"]
[]
["30","On cracks on concrete floors, walkways, etc","m",628,null,0,null,null,628,null,1937,null,2230,{"$nulls":12},1,2,1,3,"I","1"]
[]
[null,"Resealing of joints",{"$nulls":8},2530,null,2230,{"$nulls":12},1,2,1,3,"S","0"]
[]
["31","Ream out joint and install UV resistant polysulphide sealant","m",144,null,0,null,null,144,null,2529,null,2230,{"$nulls":12},1,2,1,3,"I","1"]
[]
[null,"Pressure cleaning existing buildings",{"$nulls":8},1932,null,2230,{"$nulls":12},1,2,1,3,"S","0"]
[]
["32","External facebrick","m²","  2 841",null,0,null,null,2841,null,1933,null,2230,{"$nulls":12},1,2,1,3,"I","2"]
[]
[null,"Take out and remove hives, nests, etc.",{"$nulls":8},2650,null,2230,{"$nulls":12},1,2,1,3,"S","0"]
[]
["33","Carefully take out wasp hive","No",1,null,0,null,null,1,null,2651,null,2230,{"$nulls":12},1,2,1,3,"I","N"]
[]
["34","Carefully take out bird's nest","No",1,null,0,null,null,1,null,2667,null,2230,{"$nulls":12},1,2,1,3,"I","N"]
[]
[null,"BUDGETARY ALLOWANCE",{"$nulls":8},1921,null,2470,{"$nulls":12},1,2,1,3,"H","0"]
[]
["35","Allow a budgetary amount of R100 000.00 for Remedial Works","Item",null,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"},null,null,1,null,1931,null,2470,{"$nulls":12},1,2,1,3,"I","I"]
[]
[]
[null,"Bill Total",{"$nulls":4},{"v":100000,"d":"100,000.00"}]
[]
[]
[]
[null,"BILL NO.2 : EARTHWORKS",{"$nulls":23},1,2,2,6,"H"]
[]
[null,"EARTHWORKS (PROVISIONAL)",{"$nulls":8},2443,null,2500,{"$nulls":12},1,2,2,6,"H","0"]
[]
[null,"EXCAVATION, FILLING, ETC OTHER THAN BULK",{"$nulls":8},2444,null,6450,{"$nulls":12},1,2,2,6,"H","0"]
[]
[null,"Excavation in earth not exceeding 2m deep",{"$nulls":8},2445,null,8560,{"$nulls":12},1,2,2,6,"S","0"]
[]
["1","Reduced levels under floors","m³",101,null,0,null,null,101,null,2505,null,8900,{"$nulls":12},1,2,2,6,"I","3"]
[]
["2","Trenches","m³",226,null,0,null,null,226,null,2564,null,8910,{"$nulls":12},1,2,2,6,"I","3"]
[]
["3","Narrow pit","m³",526,null,0,null,null,526,null,2559,null,8950,{"$nulls":12},1,2,2,6,"I","3"]
[]
["4","Underpinning in 1m alternating sections under existing foundations","m³",209,null,0,null,null,209,null,2446,null,8960,{"$nulls":12},1,2,2,6,"I","3"]
[]
[null,"Extra over bulk excavations in earth for excavation in",{"$nulls":8},2447,null,9360,{"$nulls":12},1,2,2,6,"S","0"]
[]
["5","Soft rock","m³",100,null,0,null,null,100,null,2448,null,9370,{"$nulls":12},1,2,2,6,"I","3"]
[]
["6","Hard rock","m³",51,null,0,null,null,51,null,2449,null,9380,{"$nulls":12},1,2,2,6,"I","3"]
[]
[null,"Back excavation of vertical sides of excavations in earth for working space including backfilling compacted to ?% Mod AASHTO density",{"$nulls":8},2450,null,9430,{"$nulls":12},1,2,2,6,"S","0"]
[]
["7","Not exceeding 500mm deep for placing and removing formwork to walls","m²","  1 022",null,0,null,null,1022,null,2451,null,9440,{"$nulls":12},1,2,2,6,"I","2"]
[]
[null,"Extra over all excavations for carting away",{"$nulls":8},2452,null,9620,{"$nulls":12},1,2,2,6,"S","0"]
[]
["8","Surplus material from excavations and/or stock piles on site, to a dumping site to be located by the contractor","m³",581,null,0,null,null,581,null,2453,null,9630,{"$nulls":12},1,2,2,6,"I","3"]
[]
[null,"Risk of collapse of excavations",{"$nulls":8},2455,null,7380,{"$nulls":12},1,2,2,6,"S","0"]
[]
["9","Sides of excavations not exceeding 1,5m deep","m²",781,null,0,null,null,781,null,2456,null,7390,{"$nulls":12},1,2,2,6,"I","2"]
[]
["10","Sides of excavations exceeding 1,5m deep","m²","  2 656",null,0,null,null,2656,null,2638,null,7390,{"$nulls":12},1,2,2,6,"I","2"]
[]
[null,"Keeping excavations free of water",{"$nulls":8},2462,null,9700,{"$nulls":12},1,2,2,6,"S","0"]
[]
["11","Keeping excavations free of all water other than subterranean water","Item",1,null,0,null,null,1,null,2463,null,9710,{"$nulls":12},1,2,2,6,"I","I"]
[]
[null,"FILLING, ETC",{"$nulls":8},2507,null,7480,{"$nulls":12},1,2,2,6,"H","0"]
[]
[null,"Earth filling obtained from the excavations and/or prescribed stock piles on site, compacted to 95% Mod AASHTO density",{"$nulls":8},2508,null,7570,{"$nulls":12},1,2,2,6,"S","0"]
[]
["12","Under floors, steps, pavings, etc","m³",73,null,0,null,null,73,null,2509,null,9770,{"$nulls":12},1,2,2,6,"I","3"]
[]
["13","Backfilling to trenches, holes, etc.","m³",698,null,0,null,null,698,null,2560,null,9770,{"$nulls":12},1,2,2,6,"I","3"]
[]
[null,"Filling of G7 supplied by the contractor, compacted to 95% Mod AASHTO density",{"$nulls":8},2567,null,7610,{"$nulls":12},1,2,2,6,"S","0"]
[]
["14","Backfilling to trenches, holes, etc","m³",92,null,0,null,null,92,null,2568,null,7610,{"$nulls":12},1,2,2,6,"I","3"]
[]
["15","Under floors, steps, paving, etc.","m³",80,null,0,null,null,80,null,2583,null,7610,{"$nulls":12},1,2,2,6,"I","3"]
[]
[null,"Filling of coarse river sand supplied by the contractor, consolidated",{"$nulls":8},2580,null,7830,{"$nulls":12},1,2,2,6,"S","0"]
[]
["16","Under floors etc","m³",17,null,0,null,null,17,null,2581,null,7840,{"$nulls":12},1,2,2,6,"I","3"]
[]
[null,"Compaction of ground surfaces",{"$nulls":8},2514,null,7940,{"$nulls":12},1,2,2,6,"S","0"]
[]
["17","Compaction of natural or excavated ground surface under floors etc, including scarifying for a depth of 150mm, breaking down oversize material, adding suitable material where necessary and compacting to 93% Mod AASHTO density","m²",679,null,0,null,null,679,null,2515,null,7960,{"$nulls":12},1,2,2,6,"I","2"]
[]
["18","Bottoms of trenches, holes, etc","m²",878,null,0,null,null,878,null,2570,null,7960,{"$nulls":12},1,2,2,6,"I","2"]
[]
[null,"WEED KILLERS, INSECTICIDES, ETC",{"$nulls":8},2516,null,8390,{"$nulls":12},1,2,2,6,"H","0"]
[]
[null,"Soil insecticide in accordance with SANS 5859",{"$nulls":8},2517,null,8440,{"$nulls":12},1,2,2,6,"S","0"]
[]
["19","Under floors etc, including forming and poisoning shallow furrows against foundation walls etc, filling in furrows and ramming","m²",679,null,0,null,null,679,null,2518,null,8450,{"$nulls":12},1,2,2,6,"I","2"]
[]
["20","To bottoms and sides of trenches etc","m²","  1 750",null,0,null,null,1750,null,2569,null,8460,{"$nulls":12},1,2,2,6,"I","2"]
[]
[null,"TESTS",{"$nulls":8},2698,null,8470,{"$nulls":12},1,2,2,6,"H","0"]
[]
[null,"Prescribed tests to determine degree of compaction or other properties of ground or filling",{"$nulls":8},2699,null,8480,{"$nulls":12},1,2,2,6,"S","0"]
[]
["21","Modified AASHTO Density test","No",28,null,0,null,null,28,null,2700,null,8490,{"$nulls":12},1,2,2,6,"I","N"]
[]
["22","Field Density test, including Optimum Moisture Content test (four readings per test)","No",34,null,0,null,null,34,null,2701,null,8520,{"$nulls":12},1,2,2,6,"I","N"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.3 : CONCRETE, FORMWORK AND REINFORCEMENT",{"$nulls":23},1,2,3,15,"H"]
[]
[null,"UNREINFORCED CONCRETE CAST AGAINST EXCAVATED SURFACES",{"$nulls":8},2474,null,16890,{"$nulls":12},1,2,3,15,"H","0"]
[]
[null,"15Mpa/19mm concrete",{"$nulls":8},2475,null,81590,{"$nulls":12},1,2,3,15,"S","0"]
[]
["1","Surface blinding under footings","m³",31,null,0,null,null,31,null,2476,null,81630,{"$nulls":12},1,2,3,15,"I","3"]
[]
[null,"REINFORCED CONCRETE",{"$nulls":8},1685,null,2660,{"$nulls":12},1,2,3,15,"H","0"]
[]
[null,"25 Mpa/19mm Concrete:",{"$nulls":8},1811,null,2660,{"$nulls":12},1,2,3,15,"S","0"]
[]
["2","Strip footings","m³",68,null,0,null,null,68,null,2565,null,2671,{"$nulls":12},1,2,3,15,"I","3"]
[]
["3","Surface beds and thickenings cast in panels on waterproofing","m³",95,null,0,null,null,95,null,1710,null,2671,{"$nulls":12},1,2,3,15,"I","3"]
[]
["4","Underpinning strip footings in 1m alternating sections under existing footings","m³",209,null,0,null,null,209,null,2473,null,2671,{"$nulls":12},1,2,3,15,"I","3"]
[]
[null,"TEST BLOCKS",{"$nulls":8},2606,null,2671,{"$nulls":12},1,2,3,15,"H","0"]
[]
["5","Making and testing set of three 150 x 150 x 150mm concrete strength test cubes.","Sets",60,null,0,null,null,60,null,90,null,2926,{"$nulls":12},1,2,3,15,"I","S"]
[]
[null,"CONCRETE SUNDRIES",{"$nulls":8},2519,null,17960,{"$nulls":12},1,2,3,15,"H","0"]
[]
[null,"Finishing top surfaces of concrete smooth with a wood float",{"$nulls":8},2520,null,18110,{"$nulls":12},1,2,3,15,"S","0"]
[]
["6","Surface beds, slabs, etc","m²",463,null,0,null,null,463,null,2521,null,18120,{"$nulls":12},1,2,3,15,"I","2"]
[]
[null,"ROUGH FORMWORK (DEGREE OF ACCURACY II)",{"$nulls":8},91,null,3857,{"$nulls":12},1,2,3,15,"H","0"]
[]
[null,"Rough Formwork to Sides:",{"$nulls":8},92,null,3861,{"$nulls":12},1,2,3,15,"S","0"]
[]
["7","Footings","m","  1 478",null,0,null,null,1478,null,93,null,3928,{"$nulls":12},1,2,3,15,"I","1"]
[]
[null,"Boxing in rough formwork to form",{"$nulls":8},2553,null,3425,{"$nulls":12},1,2,3,15,"S"]
[]
["8","25 x 25mm Chamfers along top or bottom edges","m",12,null,0,null,null,12,null,2526,null,151973,{"$nulls":12},1,2,3,15,"I","1"]
[]
[null,"MOVEMENT JOINTS ETC",{"$nulls":8},105,null,9632,{"$nulls":12},1,2,3,15,"H","0"]
[]
[null,"Slip joints with three layers of damp proof sheeting between horizontal concrete and brick surfaces including cement mortar bed:",{"$nulls":8},106,null,9634,{"$nulls":12},1,2,3,15,"S","0"]
[]
["9","Not exceeding 300mm wide.","m",649,null,0,null,null,649,null,107,null,9636,{"$nulls":12},1,2,3,15,"I","1"]
[]
[null,"Expansion joints with bitumen emulsion paint between horizontal concrete and brick surfaces:",{"$nulls":8},110,null,9641,{"$nulls":12},1,2,3,15,"S","0"]
[]
["10","Joints not exceeding 300mm high.","m",67,null,0,null,null,67,null,111,null,9643,{"$nulls":12},1,2,3,15,"I","1"]
[]
[null,"Saw cut joints:",{"$nulls":8},112,null,9645,{"$nulls":12},1,2,3,15,"S","0"]
[]
["11","3 x 25mm Saw cut joints in two operations in top of concrete.","m",169,null,0,null,null,169,null,113,null,9646,{"$nulls":12},1,2,3,15,"I","1"]
[]
[null,"REINFORCEMENT",{"$nulls":8},116,null,9660,{"$nulls":12},1,2,3,15,"H","0"]
[]
[null,"Mild steel reinforcement to structural concrete work:",{"$nulls":8},117,null,9662,{"$nulls":12},1,2,3,15,"S","0"]
[]
["12","Bars of varying diameters.","Tonnes",16,null,0,null,null,16,null,118,null,9663,{"$nulls":12},1,2,3,15,"I","T"]
[]
["13","Bars of varying diameters.","Tonnes",11,null,0,null,null,11,null,120,null,9663,{"$nulls":12},1,2,3,15,"I","T"]
[]
[null,"Fabric reinforcement:",{"$nulls":8},121,null,9703,{"$nulls":12},1,2,3,15,"S","0"]
[]
["14","Type 193 fabric reinforcement in concrete surface beds, slabs, etc.","m²",679,null,0,null,null,679,null,123,null,9704,{"$nulls":12},1,2,3,15,"I","2"]
[]
[null,"Test blocks:",{"$nulls":8},89,null,2925,{"$nulls":12},1,2,3,15,"S","0"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.4 : MASONRY",{"$nulls":23},1,2,4,21,"H"]
[]
[null,"BRICKWORK IN FOUNDATIONS (PROVISIONAL)",{"$nulls":8},2571,null,28790,{"$nulls":12},1,2,4,21,"H","0"]
[]
[null,"Brickwork of NFX bricks (14 MPa nominal compressive strength) in class II mortar",{"$nulls":8},2572,null,94630,{"$nulls":12},1,2,4,21,"S","0"]
[]
["1","Half brick walls","m²",57,null,0,null,null,57,null,2678,null,94880,{"$nulls":12},1,2,4,21,"I","2"]
[]
["2","One brick walls","m²",568,null,0,null,null,568,null,2573,null,94880,{"$nulls":12},1,2,4,21,"I","2"]
[]
[null,"Fair face to brickwork of selected building bricks in horizontal stretcher bond pointed with flush horizontal and vertical joints",{"$nulls":8},2574,null,29690,{"$nulls":12},1,2,4,21,"S","0"]
[]
["3","Extra over for fair face","m²",42,null,0,null,null,42,null,2575,null,84870,{"$nulls":12},1,2,4,21,"I","2"]
[]
[null,"2,5mm Brickwork reinforcement",{"$nulls":8},2576,null,29890,{"$nulls":12},1,2,4,21,"S","0"]
[]
["4","75mm Wide reinforcement built in horizontally","m",190,null,0,null,null,190,null,2679,null,84900,{"$nulls":12},1,2,4,21,"I","1"]
[]
["5","150mm Wide reinforcement built in horizontally","m","  1 719",null,0,null,null,1719,null,2577,null,84900,{"$nulls":12},1,2,4,21,"I","1"]
[]
[null,"BRICKWORK IN SUPERSTRUCTURE",{"$nulls":8},124,null,10216,{"$nulls":12},1,2,4,21,"H","0"]
[]
[null,"Brickwork in NFP bricks in  Class II mortar:",{"$nulls":8},125,null,46684,{"$nulls":12},1,2,4,21,"S","0"]
[]
["6","Half brick walls.","m²",167,null,0,null,null,167,null,127,null,46691,{"$nulls":12},1,2,4,21,"I","2"]
[]
["7","Half brick walls in beamfilling.","m²",74,null,0,null,null,74,null,130,null,46691,{"$nulls":12},1,2,4,21,"I","2"]
[]
["8","One brick walls","m²",279,null,0,null,null,279,null,2592,null,46691,{"$nulls":12},1,2,4,21,"I","2"]
[]
["9","One brick walls of two half brick skins bagged and sealed.","m²",580,null,0,null,null,580,null,133,null,51287,{"$nulls":12},1,2,4,21,"I","2"]
[]
["10","One brick walls of two half brick skins bagged and sealed (gable walls).","m²",70,null,0,null,null,70,null,134,null,51287,{"$nulls":12},1,2,4,21,"I","2"]
[]
[null,"BRICKWORK SUNDRIES",{"$nulls":8},144,null,10546,{"$nulls":12},1,2,4,21,"H","0"]
[]
[null,"Brickwork reinforcement:",{"$nulls":8},148,null,10596,{"$nulls":12},1,2,4,21,"S","0"]
[]
["11","75mm Wide reinforcement built in horizontally.","m",713,null,0,null,null,713,null,149,null,10597,{"$nulls":12},1,2,4,21,"I","1"]
[]
["12","150mm Wide reinforcement built in horizontally.","m","  3 464",null,0,null,null,3464,null,150,null,10598,{"$nulls":12},1,2,4,21,"I","1"]
[]
[null,"Prestressed concrete fabricated lintels:",{"$nulls":8},151,null,10602,{"$nulls":12},1,2,4,21,"S","0"]
[]
["13","90 x 114mm Lintels laid side by side in lengths not exceeding 3m.","m",146,null,0,null,null,146,null,152,null,10603,{"$nulls":12},1,2,4,21,"I","1"]
[]
[null,"Turning pieces:",{"$nulls":8},154,null,10609,{"$nulls":12},1,2,4,21,"S","0"]
[]
["14","110mm Wide turning piece to lintels etc.","m",0,null,0,null,null,0,null,155,null,10610,{"$nulls":12},1,2,4,21,"I","1"]
[]
[null,"Galvanised hoop iron cramps, ties, etc:",{"$nulls":8},156,null,10614,{"$nulls":12},1,2,4,21,"S","0"]
[]
["15","30 x 1,6mm Roof tie 1,5m long with one end fixed to timber and other end built into brickwork.","No",456,null,0,null,null,456,null,157,null,10619,{"$nulls":12},1,2,4,21,"I","N"]
[]
[null,"Air bricks etc:",{"$nulls":8},158,null,10622,{"$nulls":12},1,2,4,21,"S","0"]
[]
["16","Set of two Terra-cotta 229 x 152mm clay vermin proof air bricks.","No",14,null,0,null,null,14,null,159,null,10625,{"$nulls":12},1,2,4,21,"I","N"]
[]
[null,"FACE BRICKWORK",{"$nulls":8},160,null,10629,{"$nulls":12},1,2,4,21,"H","0"]
[]
[null,"Corobrik Ruby Light Satin FBS or Equivalent/similar approved face bricks pointed with recessed horizontal and vertical joints:",{"$nulls":8},161,null,51530,{"$nulls":12},1,2,4,21,"S","0"]
[]
["17","Extra over brickwork for face brickwork externally.","m²",526,null,0,null,null,526,null,162,null,51531,{"$nulls":12},1,2,4,21,"I","2"]
[]
["18","Extra over brickwork for face brickwork in beamfilling.","m²",65,null,0,null,null,65,null,166,null,51531,{"$nulls":12},1,2,4,21,"I","2"]
[]
["19","Fair raking cutting.","m",46,null,0,null,null,46,null,171,null,51546,{"$nulls":12},1,2,4,21,"I","1"]
[]
["20","Fair splay cutting.","m",3,null,0,null,null,3,null,172,null,51546,{"$nulls":12},1,2,4,21,"I","1"]
[]
[null,"Brick-on-edge header course copings, sills, etc of Corobrik Ruby Light Satin SBS face bricks, pointed with flush joints on all exposed faces",{"$nulls":8},2598,null,30580,{"$nulls":12},1,2,4,21,"S","0"]
[]
["21","170 mm Wide sills set sloping and slightly projecting","m",24,null,0,null,null,24,null,2599,null,30660,{"$nulls":12},1,2,4,21,"I","1"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.5 : WATERPROOFING",{"$nulls":23},1,2,5,24,"H"]
[]
[null,"DAMPPROOFING OF WALLS AND FLOORS",{"$nulls":8},178,null,11302,{"$nulls":12},1,2,5,24,"H","0"]
[]
[null,"Brikgrip SABS approved DPC embossed damp proof course:",{"$nulls":8},179,null,11306,{"$nulls":12},1,2,5,24,"S","0"]
[]
["1","In walls","m²",136,null,0,null,null,136,null,2578,null,11307,{"$nulls":12},1,2,5,24,"I","2"]
[]
["2","In walls under cills.","m²",22,null,0,null,null,22,null,181,null,11307,{"$nulls":12},1,2,5,24,"I","2"]
[]
[null,"One layer of 250 micron Consol Plastics Gunplas USB Green waterproof sheeting sealed at laps with Gunplas Pressure Sensitive Tape:",{"$nulls":8},2478,null,11307,{"$nulls":12},1,2,5,24,"S","0"]
[]
["3","Under surface beds.","m²",679,null,0,null,null,679,null,2479,null,11307,{"$nulls":12},1,2,5,24,"I","2"]
[]
[null,"FLASHINGS ETC.",{"$nulls":8},1391,null,40213,{"$nulls":12},1,2,5,24,"H","0"]
[]
[null,"One coat primer and three coats SABS approved acrylic emulsion.",{"$nulls":8},1392,null,85961,{"$nulls":12},1,2,5,24,"S","0"]
[]
["4","Bandage flashing 300mm wide.","m",58,null,0,null,null,58,null,1393,null,85967,{"$nulls":12},1,2,5,24,"I","1"]
[]
[null,"JOINT SEALANTS ETC",{"$nulls":8},188,null,11582,{"$nulls":12},1,2,5,24,"H","0"]
[]
[null,"Approved clear silicone sealant:",{"$nulls":8},189,null,37239,{"$nulls":12},1,2,5,24,"S","0"]
[]
["5","In joints between steel frames and walls","m",112,null,0,null,null,112,null,190,null,37240,{"$nulls":12},1,2,5,24,"I","1"]
[]
[null,"Two - part polysulphide sealing compound including backing cord, bond breaker, primer, etc",{"$nulls":8},191,null,37254,{"$nulls":12},1,2,5,24,"S","0"]
[]
["6","3 x 25 mm In saw cut joints in floors.","m",169,null,0,null,null,169,null,192,null,37255,{"$nulls":12},1,2,5,24,"I","1"]
[]
["7","10 x 10mm In expansion / seperation joints in floors including raking out expansion joint filler as necessary.","m",716,null,0,null,null,716,null,2477,null,37255,{"$nulls":12},1,2,5,24,"I","1"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.6 : ROOF COVERINGS",{"$nulls":23},1,2,6,27,"H"]
[]
[null,"RIBBED METAL SHEETING AND ACCESSORIES",{"$nulls":8},195,null,12196,{"$nulls":12},1,2,6,27,"H","0"]
[]
[null,"Safintra Saflok 700 AZ 200 0.55mm thick concealed",{"$nulls":8},196,null,41888,{"$nulls":12},1,2,6,27,"S","0"]
[null,"fixing roof sheeting with Colorplus pre-painted white",{"$nulls":8},196,null,41888,{"$nulls":12},1,2,6,27,"S","0"]
[null,"finish fixed to steel purlins at about 1600mm centres",{"$nulls":8},196,null,41888,{"$nulls":12},1,2,6,27,"S","0"]
[null,"in accordance with manufacturers instruction",{"$nulls":8},196,null,41888,{"$nulls":12},1,2,6,27,"S","0"]
[]
["1","Roof covering with pitch not exceeding 25 degrees, in transportable lengths not exceeding 20m.","m²","  1 061",null,0,null,null,1061,null,197,null,41889,{"$nulls":12},1,2,6,27,"I","2"]
[]
[null,"Flashings:",{"$nulls":8},198,null,41725,{"$nulls":12},1,2,6,27,"S","0"]
[]
["2","Ridge capping 462mm girth, three times bent along girth and notched on site to suit roof profile.","m",75,null,0,null,null,75,null,199,null,41728,{"$nulls":12},1,2,6,27,"I","1"]
[]
["3","Polyclosers to suite profile of sheeting.","m",297,null,0,null,null,297,null,202,null,41739,{"$nulls":12},1,2,6,27,"I","1"]
[]
["4","Ridge end cap","No",8,null,0,null,null,8,null,203,null,41739,{"$nulls":12},1,2,6,27,"I","N"]
[]
[null,"ROOF AND WALL LINING AND INSULATION",{"$nulls":8},204,null,12278,{"$nulls":12},1,2,6,27,"H","0"]
[]
[null,"Super Sisalation® Heavy Industrial Grade 430 - Double sided reflective foil laminate incorporating layers of kraft paper and reinforcing scrim, laminated together with low density polyethylene (293gsm).",{"$nulls":8},205,null,59216,{"$nulls":12},1,2,6,27,"S","0"]
[]
["5","Insulation laid taut over timber rafters (at approximately 1200mm centres) and fixed concurrent with tiling battens, purlins, etc.","m²",897,null,0,null,null,897,null,206,null,59217,{"$nulls":12},1,2,6,27,"I","2"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.7 : CARPENTRY AND JOINERY",{"$nulls":23},1,2,7,30,"H"]
[]
[null,"PREFABRICATED ROOF TRUSSES, ETC.",{"$nulls":8},2544,null,12364,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Prefabricated plate nailed timber roof truss construction:",{"$nulls":8},2543,null,12364,{"$nulls":12},1,2,7,30,"S","0"]
[]
["1","Double pitch roof truss with a clear span of 7920mm rising 1400mm to apex with a 750mm eaves overhang on both sides.","No",80,null,0,null,null,80,null,2607,null,12364,{"$nulls":12},1,2,7,30,"I","N"]
[]
[null,"ROOF CONSTRUCTION",{"$nulls":8},215,null,12364,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Sawn softwood :",{"$nulls":8},216,null,12366,{"$nulls":12},1,2,7,30,"S","0"]
[]
["2","38 x 114mm Wall plates","m",149,null,0,null,null,149,null,2493,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
["3","38 x 114mm Bracings.","m",149,null,0,null,null,149,null,2546,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
["4","38 x 114mm Sprockets.","m",8,null,0,null,null,8,null,2547,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
["5","38 x 114mm  Rafters.","m",25,null,0,null,null,25,null,2548,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
["6","38 x 152mm  Rafters bolted.","m",27,null,0,null,null,27,null,2549,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
["7","50 x 76mm Purlins.","m","  1 387",null,0,null,null,1387,null,223,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
["8","50 x 76mm Trimmer batten.","m",12,null,0,null,null,12,null,2551,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
["9","50 x 76mm Gable trim.","m",43,null,0,null,null,43,null,2552,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
[null,"Wrought softwood:",{"$nulls":8},226,null,12402,{"$nulls":12},1,2,7,30,"S","0"]
[]
["10","70 x 70mm Splayed purlins.","m",149,null,0,null,null,149,null,229,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
[null,"LAMINATED TIMBER",{"$nulls":8},2608,null,12372,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Wrought softwood Grade 5:",{"$nulls":8},2609,null,12372,{"$nulls":12},1,2,7,30,"S","0"]
[]
["11","50 x 220mm Beams bolted.","m",58,null,0,null,null,58,null,2610,null,12372,{"$nulls":12},1,2,7,30,"I","1"]
[]
[null,"ROOF SUNDRIES",{"$nulls":8},233,null,12452,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Sundries:",{"$nulls":8},234,null,12454,{"$nulls":12},1,2,7,30,"S","0"]
[]
["12","Two coats creosote on sawn timbers.","m²",121,null,0,null,null,121,null,236,null,12456,{"$nulls":12},1,2,7,30,"I","2"]
[]
["13","300mm Long wrought end to 50 x 75mm sawn timber.","No",48,null,0,null,null,48,null,2611,null,12457,{"$nulls":12},1,2,7,30,"I","N"]
[]
["14","600mm Long wrought end to 50 X 75mm sawn timber.","No",88,null,0,null,null,88,null,237,null,12457,{"$nulls":12},1,2,7,30,"I","N"]
[]
["15","2500mm Long wrought and splay cut end to 38 x 114mm sawn timber.","No",16,null,0,null,null,16,null,2612,null,12457,{"$nulls":12},1,2,7,30,"I","N"]
[]
["16","Teco rafter / beam connector.","No",228,null,0,null,null,228,null,2613,null,12459,{"$nulls":12},1,2,7,30,"I","N"]
[]
["17","2,5mm Diameter galvanised wire tie 400mm girth wrapped around rafter and purlin with ends tied together.","No",16,null,0,null,null,16,null,242,null,12461,{"$nulls":12},1,2,7,30,"I","N"]
[]
[null,"EAVES, VERGES, ETC",{"$nulls":8},243,null,12463,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Pressed fibre-cement:",{"$nulls":8},244,null,12507,{"$nulls":12},1,2,7,30,"S","0"]
[]
["18","12 x 225mm  Medium density fascia boards including galvanised steel H-profile jointing strips.","m",333,null,0,null,null,333,null,245,null,12513,{"$nulls":12},1,2,7,30,"I","1"]
[]
["19","12 x 80 x 200mm Medium density angle section bargeboards including galvanised steel H-profile jointing strips.","m",115,null,0,null,null,115,null,246,null,12513,{"$nulls":12},1,2,7,30,"I","1"]
[]
[null,"SKIRTINGS",{"$nulls":8},250,null,12538,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Wrought meranti:",{"$nulls":8},251,null,12550,{"$nulls":12},1,2,7,30,"S","0"]
[]
["20","19 x 70mm Skirting including 19mm quadrant bead.","m","  1 665",null,0,null,null,1665,null,252,null,12558,{"$nulls":12},1,2,7,30,"I","1"]
[]
[null,"FRAMED DOORS, ETC",{"$nulls":8},2600,null,12558,{"$nulls":12},1,2,7,30,"H"]
[]
[null,"Blaco wrought saligna doors hung to steel frames:",{"$nulls":8},2601,null,12558,{"$nulls":12},1,2,7,30,"S","0"]
[]
["21","40mm Framed ledged and braced batten door 900 x 2032mm (Paraplegic).","No",3,null,0,null,null,3,null,2603,null,12558,{"$nulls":12},1,2,7,30,"I","N"]
[]
[null,"SEMI SOLID CORE FLUSH DOORS",{"$nulls":8},257,null,45924,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Flush doors with hardboard covering on both sides with hardwood finger-jointed stiles hung to steel frames:",{"$nulls":8},258,null,46432,{"$nulls":12},1,2,7,30,"S","0"]
[]
["22","40mm Door 1500 x 2032mm high (BIC).","No",1,null,0,null,null,1,null,260,null,46434,{"$nulls":12},1,2,7,30,"I","N"]
[]
["23","40mm Door 813 x 1932mm high hung 100mm off floor","No",18,null,0,null,null,18,null,2709,null,46434,{"$nulls":12},1,2,7,30,"I","N"]
[]
[null,"SOLID CORE FLUSH DOORS",{"$nulls":8},1364,null,45945,{"$nulls":12},1,2,7,30,"H","0"]
[]
[null,"Flush doors with 3mm thick commercial ply on both sides:",{"$nulls":8},1365,null,46452,{"$nulls":12},1,2,7,30,"S","0"]
[]
["24","44mm Door 813 x 2032mm high","No",54,null,0,null,null,54,null,1366,null,46454,{"$nulls":12},1,2,7,30,"I","N"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.8 : CEILINGS PARTITIONS AND ACCESS FLOORING",{"$nulls":23},1,2,8,33,"H"]
[]
[null,"NAILED UP AND SCREW UP CEILINGS",{"$nulls":8},263,null,13420,{"$nulls":12},1,2,8,33,"H","0"]
[]
[null,"6,4mm 'Rhinoboard' M-Strip ceiling fixed print side up to brandering with 32mm galvanized clout nails or 32mm grabber screws at 150mm centers with 'M-Strip' cover strips over joints with all nail or screw heads stopped and sanded level, all in strict accordance with the manufacturer's instructions:",{"$nulls":8},264,null,49613,{"$nulls":12},1,2,8,33,"S","0"]
[]
["1","Ceilings including 50 x 50 mm sawn softwood brandering at 400mm centres in one direction only to trusses (elsewhere) at 1,5mm centres.","m²","  1 416",null,0,null,null,1416,null,265,null,49615,{"$nulls":12},1,2,8,33,"I","2"]
[]
["2","Extra over ceiling for 600 x 600mm trap door.","No",18,null,0,null,null,18,null,266,null,49629,{"$nulls":12},1,2,8,33,"I","N"]
[]
[null,"Wrot softwood cornices",{"$nulls":8},267,null,49319,{"$nulls":12},1,2,8,33,"S","0"]
[]
["3","19 x 44mm Cornice nailed","m","  1 069",null,0,null,null,1069,null,268,null,49320,{"$nulls":12},1,2,8,33,"I","1"]
[]
[null,"SUSPENDED CEILINGS",{"$nulls":8},2645,null,44380,{"$nulls":12},1,2,8,33,"H","0"]
[]
[null,"Pelican AMF Thermofon ceiling size 1200 x 600 x 12mm with square edge laid on Pelican Econogrid pre-painted white exposed tee grid system including fire safety punch outs. Main tees suspended by means of a 19 x 0,5mm GMS (or 2,5mm wire) hangers at 1200mm centres",{"$nulls":8},2646,null,44530,{"$nulls":12},1,2,8,33,"S","0"]
[]
["4","Ceilings suspended not exceeding 1m below steel purlins","m²",80,null,0,null,null,80,null,2647,null,44550,{"$nulls":12},1,2,8,33,"I","2"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.9 : FLOOR COVERINGS",{"$nulls":23},1,2,9,36,"H"]
[]
[null,"VINYL FLOOR COVERINGS, WALL LININGS, ETC.",{"$nulls":8},270,null,41329,{"$nulls":12},1,2,9,36,"H","0"]
[]
[null,"All vinyl flooring materials require a smooth, hard, clean, true and level surface, not only for appearance but also for achieving a satisfactory adhesive bond and long term durability",{"$nulls":8},1702,null,41329,{"$nulls":12},1,2,9,36,"C","0"]
[]
[null,"The main contractor shall ensure that the sub-floor is acceptable to receive the vinyl flooring specified in respect of levelness, smoothness, soundness and cleanness",{"$nulls":8},1703,null,41329,{"$nulls":12},1,2,9,36,"C","0"]
[]
[null,"300 x 300 x  2,5mm Thick hard wearing  semi-flexible vinyl floor tiles fixed with 'Marley No.60 Acrylic Adhesive':",{"$nulls":8},271,null,41336,{"$nulls":12},1,2,9,36,"S","0"]
[]
["1","On floors.","m²","  3 426",null,0,null,null,3426,null,272,null,41337,{"$nulls":12},1,2,9,36,"I","2"]
[]
[null,"POLISH, SEALERS, ETC",{"$nulls":8},273,null,14681,{"$nulls":12},1,2,9,36,"H","0"]
[]
[null,"Polish, sealers, etc:",{"$nulls":8},274,null,14683,{"$nulls":12},1,2,9,36,"S","0"]
[]
["2","Two coats wax polish on vinyl flooring.","m²","  3 426",null,0,null,null,3426,null,275,null,14684,{"$nulls":12},1,2,9,36,"I","2"]
[]
[null,"EPOXY RESIN SCREED",{"$nulls":8},2687,null,14684,{"$nulls":12},1,2,9,36,"H","0"]
[]
[null,"Prepare, prime with Flowprime and apply 'Peran STB' 4mm thick or equal approved as per manufacturer's instructions",{"$nulls":8},2688,null,14684,{"$nulls":12},1,2,9,36,"S","0"]
[]
["3","On floors","m²",56,null,0,null,null,56,null,2689,null,14684,{"$nulls":12},1,2,9,36,"I","2"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.10 : IRONMONGERY",{"$nulls":23},1,2,10,39,"H"]
[]
[null,"IRONMONGERY",{"$nulls":8},2138,null,46520,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"LOCKS",{"$nulls":8},2480,null,46950,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Manufactured by Union",{"$nulls":8},2605,null,46950,{"$nulls":12},1,2,10,39,"S","0"]
[]
["1","40mm Padlock (gate)","No",10,null,0,null,null,10,null,2604,null,47011,{"$nulls":12},1,2,10,39,"I","N"]
[]
["2","65mm Padlock (trap door)","No",18,null,0,null,null,18,null,2482,null,47011,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"Manufactured by Geze",{"$nulls":8},2481,null,47010,{"$nulls":12},1,2,10,39,"S","0"]
[]
["3","Ref 730/68 - 76 mm Profile arch sashlock S/S","No",74,null,0,null,null,74,null,2483,null,47169,{"$nulls":12},1,2,10,39,"I","N"]
[]
["4","Ref  880-66/78 - 5 Pin NP Double cylinder 66mm 3K N.PL","No",74,null,0,null,null,74,null,2484,null,47173,{"$nulls":12},1,2,10,39,"I","N"]
[]
["5","Master key","No",5,null,0,null,null,5,null,2486,null,47183,{"$nulls":12},1,2,10,39,"I","N"]
[]
["6","Grand master key","No",1,null,0,null,null,1,null,2487,null,47184,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"HANDLES",{"$nulls":8},2111,null,47490,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Manufactured by Geze",{"$nulls":8},2112,null,47500,{"$nulls":12},1,2,10,39,"S","0"]
[]
["7","Ref EDE/101C-Daytona19mm/165X165X1.5/PL.CYL","No",74,null,0,null,null,74,null,2485,null,47501,{"$nulls":12},1,2,10,39,"I","N"]
[]
["8","Ref 295/01 - Helping hand L/H OR R/H","No",22,null,0,null,null,22,null,2488,null,47501,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"PUSH PLATES AND KICK PLATES",{"$nulls":8},2114,null,47590,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Manufactured by 'Geze'",{"$nulls":8},2115,null,47650,{"$nulls":12},1,2,10,39,"S","0"]
[]
["9","160 x 160mm stainless steel push plate","No",27,null,0,null,null,27,null,2116,null,47651,{"$nulls":12},1,2,10,39,"I","N"]
[]
["10","813 x 20mm stainless steel kick plate","No",4,null,0,null,null,4,null,2117,null,47652,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"DOOR CLOSERS",{"$nulls":8},290,null,14985,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Dorma:",{"$nulls":8},291,null,15002,{"$nulls":12},1,2,10,39,"S","0"]
[]
["11","TS91' Overhead door closer with bracket fixed to metal","No",5,null,0,null,null,5,null,292,null,15003,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"LETTERS, NAMEPLATES, ETC.",{"$nulls":8},293,null,15017,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Manufactured by 'Geze'",{"$nulls":8},294,null,15019,{"$nulls":12},1,2,10,39,"S","0"]
[]
["12","90 x 32 x 3mm Thick perspex plate with 25mm high engraved and painted letters or numerals.","No",15,null,0,null,null,15,null,295,null,15022,{"$nulls":12},1,2,10,39,"I","N"]
[]
["13","Ref 079/160E-S/ST P/PL 160 x 160 x 1.2mm annodised aluminium plate with male or female symbol.","No",8,null,0,null,null,8,null,296,null,15024,{"$nulls":12},1,2,10,39,"I","N"]
[]
["14","Ref 079/160E-S/ST P/PL 160 x 160 x 1.2mm anodised aluminium plate with paraplegic symbol.","No",4,null,0,null,null,4,null,297,null,15024,{"$nulls":12},1,2,10,39,"I","N"]
[]
["15","200 x 200 x 3mm Thick perspex plate  with fire exit, fire extinguisher, fire hose reel or fire hydrant symbol.","No",6,null,0,null,null,6,null,298,null,15026,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"BATHROOM FITTINGS",{"$nulls":8},299,null,15061,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Kimberley-Clark:",{"$nulls":8},300,null,15085,{"$nulls":12},1,2,10,39,"S","0"]
[]
["16","Approved lockable two roll toilet roll holder, size 144 x 138 x 301mm, plugged.","No",36,null,0,null,null,36,null,301,null,15093,{"$nulls":12},1,2,10,39,"I","N"]
[]
["17","Approved liquid soap dispenser, size 200 x 85 x 140mm, grade 304 stainless steel unit, plugged.","No",11,null,0,null,null,11,null,302,null,15094,{"$nulls":12},1,2,10,39,"I","N"]
[]
["18","19mm Diameter chromium plated towel rail 600mm long including end brackets.","No",11,null,0,null,null,11,null,303,null,15094,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"SUNDRIES",{"$nulls":8},304,null,15114,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Geze:",{"$nulls":8},305,null,15116,{"$nulls":12},1,2,10,39,"S","0"]
[]
["19","Ref 140/83 - Door stop floor mounted","No",74,null,0,null,null,74,null,308,null,15125,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"Chairman Industries:",{"$nulls":8},309,null,15116,{"$nulls":12},1,2,10,39,"S","0"]
[]
["20","32mm Stainless steel side grab rail plugged.","No",3,null,0,null,null,3,null,310,null,15120,{"$nulls":12},1,2,10,39,"I","N"]
[]
["21","32mm Stainless steel rear grab rail plugged.","No",3,null,0,null,null,3,null,311,null,15120,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"Lecico:",{"$nulls":8},2168,null,15120,{"$nulls":12},1,2,10,39,"S","0"]
[]
["22","Toilet seat cover to match existing toilet","No",6,null,0,null,null,6,null,2169,null,15120,{"$nulls":12},1,2,10,39,"I","N"]
[]
["23","Cistern lid to match existing toilet","No",5,null,0,null,null,5,null,2664,null,15120,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"PINNING BOARDS, WRITING BOARDS, PROJECTION SCREENS, ETC",{"$nulls":8},312,null,15209,{"$nulls":12},1,2,10,39,"H","0"]
[]
[null,"Parrot:",{"$nulls":8},313,null,15211,{"$nulls":12},1,2,10,39,"S","0"]
[]
["24","Educational board side panel green writing board 1220 x 920mm high (ED2068) with aluminium chalk rail plugged (AL0120A).","No",10,null,0,null,null,10,null,315,null,15213,{"$nulls":12},1,2,10,39,"I","N"]
[]
["25","Edu BD Centre Panel magnetic white board 1820 x 1220mm high (ED7068) with aluminium chalk rail plugged (AL0120B).","No",6,null,0,null,null,6,null,2422,null,15213,{"$nulls":12},1,2,10,39,"I","N"]
[]
["26","Pinning board 3000 x 1200mm high plugged","No",5,null,0,null,null,5,null,317,null,15213,{"$nulls":12},1,2,10,39,"I","N"]
[]
[null,"Monetary Allowance",{"$nulls":8},2682,null,15213,{"$nulls":12},1,2,10,39,"S","0"]
[]
["27","Allow a monetary allowance of R25 000.00 for Ironmongery","Item",null,null,0,null,null,1,null,2683,null,15213,{"$nulls":12},1,2,10,39,"I","I"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.11 : METALWORK",{"$nulls":23},1,2,11,45,"H"]
[]
[null,"SUNDRY GALVANISED STEELWORK",{"$nulls":8},2585,null,15717,{"$nulls":12},1,2,11,45,"H","0"]
[]
[null,"Welded columns to walkways (unpainted):",{"$nulls":8},2586,null,15717,{"$nulls":12},1,2,11,45,"S","0"]
[]
["1","76 x 76 x 4mm Hollow section column 3000mm high.","No",10,null,0,null,null,10,null,2587,null,15717,{"$nulls":12},1,2,11,45,"I","N"]
[]
["2","150 x 150 x 8mm Base or cap plate welded on and four times drilled for bolts.","No",10,null,0,null,null,10,null,2588,null,15717,{"$nulls":12},1,2,11,45,"I","N"]
[]
["3","U-shaped bracket formed of 125 x 3mm flat section 380mm girth welded on and twice drilled for bolts.","No",10,null,0,null,null,10,null,2589,null,15717,{"$nulls":12},1,2,11,45,"I","N"]
[]
["4","12mm Diameter x 90mm long fixing bolt.","No",20,null,0,null,null,20,null,2590,null,15717,{"$nulls":12},1,2,11,45,"I","N"]
[]
["5","10mm Expansion bolt.","No",40,null,0,null,null,40,null,2591,null,15717,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"GALVANISED STEEL BALUSTRADING",{"$nulls":8},1411,null,15717,{"$nulls":12},1,2,11,45,"H","0"]
[]
[null,"Framed and welded balustrading to access balconies (unpainted):",{"$nulls":8},1412,null,15719,{"$nulls":12},1,2,11,45,"S","0"]
[]
["6","1100mm High balustrading comprising 25 x 50 x 2,5mm hollow section top and bottom rails, filled with 12 x 12mm solid section balusters at 100mm cenres, 40 x 40 x 3mm hollow section baluster with 100 x 150 x 8mm base plate welded on and twice bolted at 1500mm centres (As per drawing).","m",3,null,0,null,null,3,null,1415,null,15732,{"$nulls":12},1,2,11,45,"I","1"]
[]
[null,"WELDED GALVANISED SCREENS, GATES, ETC.",{"$nulls":8},321,null,15717,{"$nulls":12},1,2,11,45,"H","0"]
[]
[null,"Screens and gates",{"$nulls":8},322,null,15719,{"$nulls":12},1,2,11,45,"S","0"]
[]
["7","Gate 925 x 2032mm high, 10 x 10mm mild steel bars placed at 100mm centres at a 45egress angle with outer frame and inner frame including a pair of suitable hinges welded to frame and lockable sliding bolt with keep in frame","No",5,null,0,null,null,5,null,2151,null,15732,{"$nulls":12},1,2,11,45,"I","N"]
[]
["8","Gate 1600 x 2100mm high of outer frame and inner frame with a pair of suitable hinges welded to frame and lockable sliding bolt with keep in frame","No",2,null,0,null,null,2,null,323,null,15732,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"GALVANISED STEEL CUPBOARDS",{"$nulls":8},2557,null,15732,{"$nulls":12},1,2,11,45,"H","0"]
[]
["9","Lockable steel cupboard, size 1050 x 500 x 2100mm high","No",1,null,0,null,null,1,null,2558,null,15732,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"GALVANISED PRESSED STEEL DOOR FRAMES",{"$nulls":8},1725,null,15732,{"$nulls":12},1,2,11,45,"H"]
[]
[null,"1,2mm Double rebated frames suitable for half brick walls",{"$nulls":8},2710,null,15732,{"$nulls":12},1,2,11,45,"S","0"]
[]
["10","Frame for door 813 x 2032mm high","No",18,null,0,null,null,18,null,2711,null,15732,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"1,2mm Double rebated frames suitable for one brick walls",{"$nulls":8},1726,null,15732,{"$nulls":12},1,2,11,45,"S"]
[]
["11","Frame for door 813 x 2032mm high","No",22,null,0,null,null,22,null,1783,null,15732,{"$nulls":12},1,2,11,45,"I","N"]
[]
["12","Frame for door 900 x 2032mm high","No",2,null,0,null,null,2,null,2712,null,15732,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"GALVANISED STEEL WINDOWS, DOORS, ETC.",{"$nulls":8},336,null,15911,{"$nulls":12},1,2,11,45,"H","0"]
[]
[null,"All windows shall be fitted with standard brass fittings recommended by the manufacturer.",{"$nulls":8},337,null,15923,{"$nulls":12},1,2,11,45,"C","0"]
[]
[null,"Burglar bars shall be standard pattern 5 x 20mm flat section bars corresponding horizontally and vertically with glazing bars.",{"$nulls":8},338,null,15923,{"$nulls":12},1,2,11,45,"C","0"]
[]
[null,"Burglar bars to be fitted to all opening sections only unless otherwise described.",{"$nulls":8},339,null,15923,{"$nulls":12},1,2,11,45,"C","0"]
[]
[null,"Standard school windows:",{"$nulls":8},348,null,15923,{"$nulls":12},1,2,11,45,"S","0"]
[]
["13","Composite window, 1248 x 889mm high","No",2,null,0,null,null,2,null,353,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
["14","Composite window, 1300 x 520mm high","No",15,null,0,null,null,15,null,2696,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"Standard residential windows",{"$nulls":8},2692,null,15924,{"$nulls":12},1,2,11,45,"S","0"]
[]
["15","Window size 530 x 650mm high","No",24,null,0,null,null,24,null,2707,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
["16","Window size 1022 x 650mm high","No",8,null,0,null,null,8,null,2708,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
["17","Window size 1022 x 949mm high","No",4,null,0,null,null,4,null,2694,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
["18","Window size 1022 x 1245mm high","No",10,null,0,null,null,10,null,2693,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
["19","Window size 1511 x 949mm high","No",12,null,0,null,null,12,null,2695,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"Burglar bars",{"$nulls":8},2639,null,15924,{"$nulls":12},1,2,11,45,"S","0"]
[]
["20","Burglar bars for window size 400 x 600mm high","No",11,null,0,null,null,11,null,2640,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
["21","Ditto, but for size 1100 x 800mm high","No",9,null,0,null,null,9,null,2641,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
["22","Ditto, but for size 1300 x 520mm high","No",30,null,0,null,null,30,null,2652,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
["23","Ditto, but for size 1380 x 1500mm high","No",35,null,0,null,null,35,null,2653,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
["24","Ditto, but for size 2500 x 1500mm high","No",11,null,0,null,null,11,null,2642,null,15924,{"$nulls":12},1,2,11,45,"I","N"]
[]
[null,"ALUMINIUM WINDOWS, DOORS, ETC",{"$nulls":8},2684,null,53730,{"$nulls":12},1,2,11,45,"H","0"]
[]
[null,"Epoxy powder coated with 6,38mm thick clear laminated safety glass HBS \"Nuklip\" or equal approved shopfront system with outer frame to consist of NK260 rebated all round with bulb gasket seal complete with hinges and ironmongery",{"$nulls":8},2685,null,108564,{"$nulls":12},1,2,11,45,"S","0"]
[]
["25","Double door size 1600 x 2100mm high","No",2,null,0,null,null,2,null,2686,null,146413,{"$nulls":12},1,2,11,45,"I","N"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.12 : PLASTERING",{"$nulls":23},1,2,12,48,"H"]
[]
[null,"SCREEDS",{"$nulls":8},373,null,16166,{"$nulls":12},1,2,12,48,"H","0"]
[]
[null,"All vinyl flooring materials require a smooth, hard, clean, true and level surface, not only for appearance but also for achieving satisfactory adhesive bond and long term durability",{"$nulls":8},1686,null,16168,{"$nulls":12},1,2,12,48,"C","0"]
[]
[null,"The main contractor should ensure the sub-floor is acceptable to receive vinyl flooring specified in respect of levelness. Smoothness, soundness and cleanness",{"$nulls":8},1687,null,16168,{"$nulls":12},1,2,12,48,"C","0"]
[]
[null,"Screeds on concrete:",{"$nulls":8},374,null,16168,{"$nulls":12},1,2,12,48,"S","0"]
[]
["1","20mm Thick on floors and landings to falls to receive clay tiles.","m²",188,null,0,null,null,188,null,375,null,16173,{"$nulls":12},1,2,12,48,"I","2"]
[]
["2","23mm Thick on floors and landings to receive vinyl tiles.","m²",260,null,0,null,null,260,null,376,null,16173,{"$nulls":12},1,2,12,48,"I","2"]
[]
[null,"INTERNAL PLASTER",{"$nulls":8},385,null,16378,{"$nulls":12},1,2,12,48,"H","0"]
[]
[null,"Cement plaster on brickwork:",{"$nulls":8},386,null,16414,{"$nulls":12},1,2,12,48,"S","0"]
[]
["3","On walls.","m²","  1 709",null,0,null,null,1709,null,387,null,16623,{"$nulls":12},1,2,12,48,"I","2"]
[]
["4","On walls to receive tiles.","m²",89,null,0,null,null,89,null,388,null,16623,{"$nulls":12},1,2,12,48,"I","2"]
[]
["5","On narrow widths.","m²",7,null,0,null,null,7,null,389,null,16423,{"$nulls":12},1,2,12,48,"I","2"]
[]
[null,"CORNER PROTECTORS, DIVIDING STRIPS, ETC",{"$nulls":8},396,null,16839,{"$nulls":12},1,2,12,48,"H","0"]
[]
[null,"Corner protectors, dividing strips, etc",{"$nulls":8},397,null,16841,{"$nulls":12},1,2,12,48,"S","0"]
[]
["6","25 x 3mm Flat section brass dividing strips between different floor finishes.","m",12,null,0,null,null,12,null,398,null,16843,{"$nulls":12},1,2,12,48,"I","1"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.13 : TILING",{"$nulls":23},1,2,13,51,"H"]
[]
[null,"WALL TILING",{"$nulls":8},399,null,16855,{"$nulls":12},1,2,13,51,"H","0"]
[]
[null,"200 x 200 x 4mm White glazed wall tiles  fixed with adhesive to plaster (elsewhere) and flush pointed with tinted jointing compound:",{"$nulls":8},400,null,16987,{"$nulls":12},1,2,13,51,"S","0"]
[]
["1","On walls","m²",86,null,0,null,null,86,null,401,null,16988,{"$nulls":12},1,2,13,51,"I","2"]
[]
["2","On splashbacks.","m²",3,null,0,null,null,3,null,403,null,16988,{"$nulls":12},1,2,13,51,"I","2"]
[]
["3","Fair exposed cutting and fitting around pipe not exceeding 50mm diameter.","No",2,null,0,null,null,2,null,405,null,17043,{"$nulls":12},1,2,13,51,"I","N"]
[]
["4","Ditto but exceeding 50mm and not exceeding 100mm diameter.","No",2,null,0,null,null,2,null,406,null,17043,{"$nulls":12},1,2,13,51,"I","N"]
[]
[null,"FLOOR TILING",{"$nulls":8},407,null,17000,{"$nulls":12},1,2,13,51,"H","0"]
[]
[null,"500 x 500 x 13mm Thick clay tiles, Type B1 laid on",{"$nulls":8},408,null,17042,{"$nulls":12},1,2,13,51,"S","0"]
[null,"polymer cement adhesives",{"$nulls":8},408,null,17042,{"$nulls":12},1,2,13,51,"S","0"]
[]
["5","On floors and landings.","m²",220,null,0,null,null,220,null,409,null,17043,{"$nulls":12},1,2,13,51,"I","2"]
[]
["6","Skirting 100mm high of cut tiles.","m",117,null,0,null,null,117,null,410,null,17043,{"$nulls":12},1,2,13,51,"I","1"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.14 : PLUMBING AND DRAINAGE",{"$nulls":23},1,2,14,54,"H"]
[]
[null,"RAINWATER DISPOSAL",{"$nulls":8},411,null,17852,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Ogee  aluminium:",{"$nulls":8},412,null,17896,{"$nulls":12},1,2,14,54,"S","0"]
[]
["1","125mm Ogee eaves gutters.","m",942,null,0,null,null,942,null,413,null,17899,{"$nulls":12},1,2,14,54,"I","1"]
[]
["2","Extra over Ogee  eaves gutter for stopped end.","No",50,null,0,null,null,50,null,414,null,17903,{"$nulls":12},1,2,14,54,"I","N"]
[]
["3","Extra over Ogee eaves gutter for outlet for 100 x 75mm pipe.","No",50,null,0,null,null,50,null,415,null,17906,{"$nulls":12},1,2,14,54,"I","N"]
[]
["4","100 x 75mm Rainwater pipes.","m",162,null,0,null,null,162,null,416,null,17908,{"$nulls":12},1,2,14,54,"I","1"]
[]
["5","Extra over 100 x 75mm  rainwater pipe for bend.","No",142,null,0,null,null,142,null,417,null,17909,{"$nulls":12},1,2,14,54,"I","N"]
[]
["6","Extra over 100 x 75mm  rainwater pipe for shoe.","No",50,null,0,null,null,50,null,418,null,17910,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"SANITARY FITTINGS",{"$nulls":8},419,null,18028,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Prices are to include for sealing all round with approved silicone waterproofing sealant at junction/gaps with tiled walls, timber fittings, vanity tops, etc.",{"$nulls":8},420,null,75842,{"$nulls":12},1,2,14,54,"C","0"]
[]
[null,"Plumline Sanitaryware' vitreous china wash hand basins and pedestals:",{"$nulls":8},2615,null,75802,{"$nulls":12},1,2,14,54,"S"]
[]
["7","410 x 500mm 'Amaro' white vitreous china lavatory basin (product code 037119) with one taphole including integrated overflow and chainstay hole, fixed with stainless steel screws and washers to plugs in wall  (tap and waste fitting elsewhere).","No",19,null,0,null,null,19,null,2614,null,75802,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"Lecico Sanitaryware' vitreous china WC suites:",{"$nulls":8},425,null,75856,{"$nulls":12},1,2,14,54,"S","0"]
[]
["8","Madison' white vitreous china close couple suite  (product code MADBOXDFL0SCSBE) with 100mm outlet  and matching 6 litre cistern including lid, fitments, flushpipe, etc., bedded in 4:1 cement mortar on concrete floors.","No",29,null,0,null,null,29,null,426,null,75858,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"Plumline' vitreous china urinals:",{"$nulls":8},2540,null,75858,{"$nulls":12},1,2,14,54,"S"]
[]
["9","Amaro' urinal  (code 031129) size 300 x 245 x 400mm high or equal approved with top inlet spreader and waste outlet including wall mounting brackets and connected to water supply, sealed with silicone sealant where urinal meets wall","No",8,null,0,null,null,8,null,2541,null,75858,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"Franke' grade 304 (18/10) 1,2mm thick stainless steel domestic drop on sinks",{"$nulls":8},2690,null,75858,{"$nulls":12},1,2,14,54,"S","0"]
[]
["10","Standard drop on sink and drainer size 1000 x 500mm with single end bowl, set on cupboard fitting (elsewhere) including cutting one tapbole (tap and waste fitting elsewhere)","No",2,null,0,null,null,2,null,2691,null,75858,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"Kwikot stainless steel",{"$nulls":8},2662,null,60390,{"$nulls":12},1,2,14,54,"S","0"]
[]
["11","Grade 304 (18/10) curved back urinal (Code: KCB102) 1 830mm with automatic flushing tank  flush and sparge pipes and hinged domical grating","No",2,null,0,null,null,2,null,2663,null,60480,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"WASTE UNIONS ETC",{"$nulls":8},437,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Cobra Watertech':",{"$nulls":8},438,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
["12","32 mm CP basin waste union.","No",9,null,0,null,null,9,null,439,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
["13","40 mm CP sink waste union.","No",2,null,0,null,null,2,null,2702,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"TRAPS ETC",{"$nulls":8},441,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Priced are to include for jointing to uPVC pipe with and including the necessary adaptors unless otherwise described.",{"$nulls":8},442,null,18034,{"$nulls":12},1,2,14,54,"C","0"]
[]
[null,"Butyl rubber:",{"$nulls":8},443,null,18034,{"$nulls":12},1,2,14,54,"S","0"]
[]
["14","32 mm deep seal \"P\" or \"S\" trap.","No",2,null,0,null,null,2,null,444,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"TAPS,VALVES, ETC",{"$nulls":8},449,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Priced are to include  for jointing to copper pipe with and including the necessary fittings unless otherwise described.",{"$nulls":8},450,null,18034,{"$nulls":12},1,2,14,54,"C","0"]
[]
[null,"Brass.",{"$nulls":8},451,null,18034,{"$nulls":12},1,2,14,54,"S","0"]
[]
["15","15 mm Fulway gate valve.","No",12,null,0,null,null,12,null,452,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
["16","22 mm Fulway gate valve.","No",10,null,0,null,null,10,null,453,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
["17","28 mm Fulway gate valve.","No",4,null,0,null,null,4,null,1206,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"Plumline",{"$nulls":8},455,null,18034,{"$nulls":12},1,2,14,54,"S","0"]
[]
["18","15 mm CP Ballostop.","No",6,null,0,null,null,6,null,456,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
["19","22 mm CP Ballostop.","No",4,null,0,null,null,4,null,457,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
["20","15 mm CP 'Moderna' pillartap (Code: 038735).","No",17,null,0,null,null,17,null,460,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
["21","15 mm CP Shower head","No",1,null,0,null,null,1,null,2673,null,18034,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"SANITARY PLUMBING",{"$nulls":8},467,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"uPVC pipes:",{"$nulls":8},468,null,18200,{"$nulls":12},1,2,14,54,"S","0"]
[]
["22","50mm Pipes.","m",22,null,0,null,null,22,null,469,null,18202,{"$nulls":12},1,2,14,54,"I","1"]
[]
["23","110mm Pipes.","m",15,null,0,null,null,15,null,470,null,18202,{"$nulls":12},1,2,14,54,"I","1"]
[]
["24","50mm Pipes under surface beds.","m",9,null,0,null,null,9,null,471,null,18202,{"$nulls":12},1,2,14,54,"I","1"]
[]
["25","110mm Pipes under surface beds.","m",7,null,0,null,null,7,null,472,null,18202,{"$nulls":12},1,2,14,54,"I","1"]
[]
["26","110mm Pipes laid in and including trenches not exceeding 1m deep.","m",12,null,0,null,null,12,null,473,null,18202,{"$nulls":12},1,2,14,54,"I","1"]
[]
[null,"Extra over uPVC pipes for fittings:",{"$nulls":8},475,null,18321,{"$nulls":12},1,2,14,54,"S","0"]
[]
["27","110mm Reducer.","No",3,null,0,null,null,3,null,477,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["28","50mm Bend.","No",16,null,0,null,null,16,null,478,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["29","110mm Bend.","No",4,null,0,null,null,4,null,479,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["30","50mm Junction.","No",12,null,0,null,null,12,null,480,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["31","110mm Junction.","No",2,null,0,null,null,2,null,481,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["32","110mm Pan connector.","No",1,null,0,null,null,1,null,482,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["33","110mm Acess bent pan connector.","No",2,null,0,null,null,2,null,483,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["34","50mm Acess bend.","No",5,null,0,null,null,5,null,485,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["35","110mm Acess bend.","No",1,null,0,null,null,1,null,486,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["36","50mm Acess junction.","No",1,null,0,null,null,1,null,487,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["37","110mm Acess junction.","No",1,null,0,null,null,1,null,488,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["38","110mm Acess reducing junction.","No",2,null,0,null,null,2,null,489,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["39","110mm Acess double junction.","No",2,null,0,null,null,2,null,490,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"WATER SUPPLIES",{"$nulls":8},493,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Class 1 copper pipes:",{"$nulls":8},494,null,18170,{"$nulls":12},1,2,14,54,"S","0"]
[]
["40","15mm Pipes.","m",24,null,0,null,null,24,null,495,null,18170,{"$nulls":12},1,2,14,54,"I","1"]
[]
["41","22mm Pipes.","m",16,null,0,null,null,16,null,496,null,18170,{"$nulls":12},1,2,14,54,"I","1"]
[]
["42","28mm Pipes.","m",10,null,0,null,null,10,null,497,null,18170,{"$nulls":12},1,2,14,54,"I","1"]
[]
["43","15mm Pipes chased into brick walls.","m",8,null,0,null,null,8,null,500,null,18170,{"$nulls":12},1,2,14,54,"I","1"]
[]
["44","22mm Pipes chased into brick walls.","m",10,null,0,null,null,10,null,501,null,18170,{"$nulls":12},1,2,14,54,"I","1"]
[]
[null,"Extra over copper pipe for capillary fitting:",{"$nulls":8},502,null,18170,{"$nulls":12},1,2,14,54,"S","0"]
[]
["45","15mm Fittings.","No",25,null,0,null,null,25,null,503,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
["46","22mm Fittings.","No",12,null,0,null,null,12,null,504,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
["47","28mm Fittings.","No",10,null,0,null,null,10,null,505,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"Extra over copper pipe for brass compression fitting:",{"$nulls":8},506,null,18170,{"$nulls":12},1,2,14,54,"S","0"]
[]
["48","15mm Fittings.","No",5,null,0,null,null,5,null,507,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
["49","22mm Fittings.","No",8,null,0,null,null,8,null,508,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
["50","28mm Fittings.","No",4,null,0,null,null,4,null,509,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"Copper overflow and service pipes:",{"$nulls":8},510,null,18170,{"$nulls":12},1,2,14,54,"S","0"]
[]
["51","15mm Bent service pipe average 450mm girth and joint to copper pipe and fittings.","No",5,null,0,null,null,5,null,511,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
["52","22mm Bent overflow pipe average 450mm girth and joint to fittings.","No",4,null,0,null,null,4,null,512,null,18170,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"FIRE APPLIANCES ETC.",{"$nulls":8},528,null,18635,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Chubb':",{"$nulls":8},529,null,18637,{"$nulls":12},1,2,14,54,"S","0"]
[]
["53","Everyway' hose reel complete with 30m rubber hose, chromium plated stopcock, shut-off nozzle and wall bracket.","No",2,null,0,null,null,2,null,530,null,18639,{"$nulls":12},1,2,14,54,"I","N"]
[]
["54","4,5kg DPC fire extinguisher complete with backboard and wall bracket plugged to wall.","No",5,null,0,null,null,5,null,531,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["55","Ditto but 9kg.","No",10,null,0,null,null,10,null,532,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
["56","Watertight high impact, UV- stablised clear acrylic fire hose reel cupboard with numbered twist-action closer seal fixed to brick wall.","No",2,null,0,null,null,2,null,533,null,18351,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"WATER SUPPLIES TO FIRE APPLIANCES",{"$nulls":8},534,null,18656,{"$nulls":12},1,2,14,54,"H","0"]
[]
[null,"Class 1 copper pipes:",{"$nulls":8},535,null,18710,{"$nulls":12},1,2,14,54,"S","0"]
[]
["57","28mm Pipes.","m",17,null,0,null,null,17,null,536,null,18715,{"$nulls":12},1,2,14,54,"I","1"]
[]
["58","28mm Pipes under surface bed.","m",9,null,0,null,null,9,null,537,null,18170,{"$nulls":12},1,2,14,54,"I","1"]
[]
[null,"Extra over class 1 copper pipes for capillary fittings:",{"$nulls":8},538,null,18732,{"$nulls":12},1,2,14,54,"S","0"]
[]
["59","28mm Fittings.","No",10,null,0,null,null,10,null,539,null,18733,{"$nulls":12},1,2,14,54,"I","N"]
[]
[null,"TESTING",{"$nulls":8},540,null,18170,{"$nulls":12},1,2,14,54,"H","0"]
[]
["60","Testing all pipe systems.","Item",0,null,0,null,null,1,null,541,null,18351,{"$nulls":12},1,2,14,54,"I","I"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.15 : GLAZING",{"$nulls":23},1,2,15,63,"H"]
[]
[null,"GLAZING TO STEEL WITH PUTTY",{"$nulls":8},545,null,20715,{"$nulls":12},1,2,15,63,"H","0"]
[]
[null,"4 mm Patterned toughened glass:",{"$nulls":8},551,null,20728,{"$nulls":12},1,2,15,63,"S","0"]
[]
["1","Panes exceeding 0,1m2 and not exceeding 0.5m2.","m²",15,null,0,null,null,15,null,552,null,20729,{"$nulls":12},1,2,15,63,"I","2"]
[]
[null,"6.38 mm Clear laminated safety glass",{"$nulls":8},2594,null,20729,{"$nulls":12},1,2,15,63,"S"]
[]
["2","Panes exceeding 0,1m2 and not exceeding 0.5m2.","m²",6,null,0,null,null,6,null,2595,null,20729,{"$nulls":12},1,2,15,63,"I","2"]
[]
["3","Panes exceeding 0,5m2 and not exceeding 2.5m2.","m²",100,null,0,null,null,100,null,2596,null,20729,{"$nulls":12},1,2,15,63,"I","2"]
[]
[null,"TOPS, SHELVES, DOORS, MIRRORS, ETC.",{"$nulls":8},553,null,21649,{"$nulls":12},1,2,15,63,"H","0"]
[]
[null,"3mm Silvered float glass copper backed mirrors with polished edges fixed with double sided adhesive tape:",{"$nulls":8},554,null,21663,{"$nulls":12},1,2,15,63,"S","0"]
[]
["4","Frameless mirror 700 x 450 mm high.","No",6,null,0,null,null,6,null,555,null,21664,{"$nulls":12},1,2,15,63,"I","N"]
[]
[null,"PREPARATORY WORK TO EXISTING WORK",{"$nulls":8},2657,null,21664,{"$nulls":12},1,2,15,63,"C","0"]
[]
[null,"Previously painted glazed surfaces   Windows  shall be thoroughly washed down and allowed to dry completely before installation of vinyl film",{"$nulls":8},2658,null,21664,{"$nulls":12},1,2,15,63,"C","0"]
[]
[null,"SUNSCREEN, ETC",{"$nulls":8},2654,null,21664,{"$nulls":12},1,2,15,63,"H","0"]
[]
[null,"Vinyl frosting film, etc",{"$nulls":8},2655,null,21664,{"$nulls":12},1,2,15,63,"S","0"]
[]
["5","600mm Obscure vinyl frosting film or similar approved to windows","m",125,null,0,null,null,125,null,2656,null,21664,{"$nulls":12},1,2,15,63,"I","1"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.16 : PAINTWORK",{"$nulls":23},1,2,16,66,"H"]
[]
[null,"PAINTWORK ETC. TO NEW SURFACES",{"$nulls":8},557,null,21780,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"ON FLOATED PLASTER",{"$nulls":8},1709,null,21780,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"Prepare surfaces and remove all loose material, apply one coat Alkali Resistant Plaster Primer  and two coats superior quality acrylic emulsion paint:",{"$nulls":8},558,null,43774,{"$nulls":12},1,2,16,66,"S","0"]
[]
["1","On interior walls.","m²","  1 709",null,0,null,null,1709,null,559,null,43775,{"$nulls":12},1,2,16,66,"I","2"]
[]
[null,"ON PLASTER BOARD",{"$nulls":8},568,null,25056,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"Prepare surfaces and remove all loose material, apply one coatAlkali Resistant Plaster Primer and two coats superior quality acrylic emulsion paint:",{"$nulls":8},569,null,44054,{"$nulls":12},1,2,16,66,"S","0"]
[]
["2","On internal ceilings and cornices.","m²","  1 416",null,0,null,null,1416,null,570,null,44055,{"$nulls":12},1,2,16,66,"I","2"]
[]
[null,"ON FIBRE-CEMENT, ETC.",{"$nulls":8},571,null,25602,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"Prepare surfaces and remove all loose material, apply one coat Alkali Resistant Plaster Primer and two coats superior quality acrylic emulsion paint:",{"$nulls":8},572,null,44071,{"$nulls":12},1,2,16,66,"S","0"]
[]
["3","On exterior fascias and barge boards.","m²",183,null,0,null,null,183,null,574,null,44073,{"$nulls":12},1,2,16,66,"I","2"]
[]
[null,"ON METAL",{"$nulls":8},575,null,26148,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"Prepare surfaces and remove all loose material, dust, grease, salts and contamination with one coat ater based primer, one coat alkyd based universal  undercoat  and two coats superior quality universal enamel paint on: galvanised steel or aluminium:",{"$nulls":8},581,null,44120,{"$nulls":12},1,2,16,66,"S","0"]
[]
["4","On door frames.","m²",67,null,0,null,null,67,null,582,null,44123,{"$nulls":12},1,2,16,66,"I","2"]
[]
["5","On window frames with burglar bars (bsm).","m²",89,null,0,null,null,89,null,584,null,44123,{"$nulls":12},1,2,16,66,"I","2"]
[]
["6","On security gates","m²",10,null,0,null,null,10,null,2150,null,44123,{"$nulls":12},1,2,16,66,"I","2"]
[]
[null,"ON WOOD, WOOD BOARD",{"$nulls":8},585,null,26286,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"Stop, fill, sand down and prepare wood surfaces and apply three coats superior quality clear gloss varnish",{"$nulls":8},588,null,44266,{"$nulls":12},1,2,16,66,"S","0"]
[]
["7","On interior / exterior doors.","m²",201,null,0,null,null,201,null,589,null,44270,{"$nulls":12},1,2,16,66,"I","2"]
[]
["8","On interior / exterior skirtings, rails, etc not exceeding 300mm girth.","m","  1 473",null,0,null,null,1473,null,590,null,44277,{"$nulls":12},1,2,16,66,"I","1"]
[]
[null,"SUPPLEMENTARY PREAMBLES",{"$nulls":8},2076,null,70730,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"PREPARATORY WORK TO EXISTING WORK",{"$nulls":8},2077,null,70740,{"$nulls":12},1,2,16,66,"S","0"]
[]
[null,"Previously painted plastered surfaces",{"$nulls":8},2078,null,70760,{"$nulls":12},1,2,16,66,"C","0"]
[null,"Surfaces shall be thoroughly washed down and allowed to dry completely before any paint is applied. Blistered or peeling paint shall be completely removed and cracks shall be opened, filled with a suitable filler and finished smooth",{"$nulls":8},2078,null,70760,{"$nulls":12},1,2,16,66,"C","0"]
[]
[null,"Previously painted metal surfaces",{"$nulls":8},2079,null,70780,{"$nulls":12},1,2,16,66,"C","0"]
[null,"Surfaces shall be thoroughly rubbed and cleaned down.  Blistered or peeling paint shall be completely removed down to bare metal",{"$nulls":8},2079,null,70780,{"$nulls":12},1,2,16,66,"C","0"]
[]
[null,"Previously painted wood surfaces",{"$nulls":8},2080,null,70800,{"$nulls":12},1,2,16,66,"C","0"]
[null,"Surfaces shall be thoroughly cleaned down.  Blistered or peeling paint shall be completely removed and cracks and crevices shall be primed, filled with suitable filler and finished smooth",{"$nulls":8},2080,null,70800,{"$nulls":12},1,2,16,66,"C","0"]
[]
[null,"ON PREVIOUSLY PAINTED SURFACES",{"$nulls":8},1704,null,586000,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"ON EXISTING INTERNAL FLOATED PLASTER SURFACES",{"$nulls":8},2085,null,72190,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"Two coats superior quality acrylic emulsion paint for interior and exterior use",{"$nulls":8},2086,null,72200,{"$nulls":12},1,2,16,66,"S","0"]
[]
["9","Walls","m²","  4 198",null,0,null,null,4198,null,2087,null,72201,{"$nulls":12},1,2,16,66,"I","2"]
[]
[null,"ON EXISTING FIBRE CEMENT",{"$nulls":8},2676,null,72201,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"One coat Alkali Resistant Plaster Primer and two coats superior quality acrylic emulsion paint:",{"$nulls":8},2677,null,72201,{"$nulls":12},1,2,16,66,"S","0"]
[]
["10","Nutec cills","m²",30,null,0,null,null,30,null,1711,null,44073,{"$nulls":12},1,2,16,66,"I","2"]
[]
[null,"ON EXISTING METAL SURFACES",{"$nulls":8},2082,null,72410,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"One coat alkyd based universal undercoat and one coat superior quality universal enamel paint",{"$nulls":8},2083,null,72420,{"$nulls":12},1,2,16,66,"S","0"]
[]
["11","Door frames","m²",100,null,0,null,null,100,null,2084,null,72421,{"$nulls":12},1,2,16,66,"I","2"]
[]
["12","Security gates","m²",34,null,0,null,null,34,null,2147,null,72421,{"$nulls":12},1,2,16,66,"I","2"]
[]
["13","On window frames with burglar bars (bsm).","m²",106,null,0,null,null,106,null,2109,null,72421,{"$nulls":12},1,2,16,66,"I","2"]
[]
["14","Awning, Fire hosereel case, etc","m²",4,null,0,null,null,4,null,2643,null,72421,{"$nulls":12},1,2,16,66,"I","2"]
[]
[null,"ON EXISTING WOOD SURFACES",{"$nulls":8},2091,null,72510,{"$nulls":12},1,2,16,66,"H","0"]
[]
[null,"One coat alkyd based universal undercoat and one coat superior quality universal enamel paint",{"$nulls":8},2092,null,72520,{"$nulls":12},1,2,16,66,"S","0"]
[]
["15","Doors","m²",208,null,0,null,null,208,null,2093,null,72521,{"$nulls":12},1,2,16,66,"I","2"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[null,"Section Total ",{"$nulls":4},{"v":100000,"d":"100,000.00"}]
[]
[]
[null,"SECTION NO. 3 : EXTERNAL WORKS",{"$nulls":23},1,3,1,6,"H"]
[]
[]
[null,"BILL NO.1 : EXTERNAL WORKS (PROVISIONAL)",{"$nulls":23},1,3,1,6,"H"]
[]
[null,"REMOVAL OF EXISTING WORK",{"$nulls":8},1739,null,1650,{"$nulls":12},1,3,1,6,"H","0"]
[]
[null,"All work to be demolished, etc is to be removed off site, unless otherwise stated, prices to include for this.",{"$nulls":8},2495,null,1650,{"$nulls":12},1,3,1,6,"C","0"]
[]
[null,"Demolition of existing work",{"$nulls":8},1740,null,1650,{"$nulls":12},1,3,1,6,"S"]
[]
["1","Blocks E - Single storey building with pitched roof, approximately 6 000mm x 6 000mm on plan, comprising reinforced concrete surface bed, brick walls, and roof sheeting on timber trusses, including grubbing up all foundations, removal and disposal thereof complete","No",1,null,0,null,null,1,null,2490,null,1650,{"$nulls":12},1,3,1,6,"I","N"]
[]
["2","Single storey building with pitched roof, approximately 16 000mm x 8 300mm on plan, comprising reinforced concrete surface bed, brick walls, and roof sheeting on timber trusses, including grubbing up all foundations, removal and disposal thereof complete","No",1,null,0,null,null,1,null,2706,null,1650,{"$nulls":12},1,3,1,6,"I","N"]
[]
["3","Block L - Single storey building with pitched roof, approximately 36 000mm x 7 500mm on plan, comprising reinforced concrete surface bed, brick walls, and roof sheeting on timber trusses, including grubbing up all foundations, removal and disposal thereof complete","No",1,null,0,null,null,1,null,2491,null,1650,{"$nulls":12},1,3,1,6,"I","N"]
[]
[null,"Breaking up and removing reinforced concrete, including cutting off and removing reinforcement",{"$nulls":8},2160,null,1650,{"$nulls":12},1,3,1,6,"S"]
[]
["4","Concrete V-drains 1200mm wide","m",138,null,0,null,null,138,null,2665,null,1650,{"$nulls":12},1,3,1,6,"I","1"]
[]
[null,"Taking out and removing and set aside including later refixing in new position",{"$nulls":8},2153,null,1650,{"$nulls":12},1,3,1,6,"S","0"]
[]
[null,"JOINT SEALANTS",{"$nulls":8},2427,null,1650,{"$nulls":12},1,3,1,6,"H","0"]
[]
[null,"Chip open the crack to form a \"V\" shape 20mm wide x 10mm deep and scratch out the debris that may block the crack in the sides of the hole. Grinding in the floor approximately 200mm to 300mm apart from the rebar to be placed into an",{"$nulls":8},2431,null,1650,{"$nulls":12},1,3,1,6,"S","0"]
[null,"epoxy repair mortar 'SIKA TOP-ARMATEC 100'. Fill the crack with structural epoxy repair mortar SIKA MONO TOP 615HB'",{"$nulls":8},2431,null,1650,{"$nulls":12},1,3,1,6,"S","0"]
[]
["5","Concrete V-drains, walkways, etc.","m",32,null,0,null,null,32,null,2430,null,1650,{"$nulls":12},1,3,1,6,"I","1"]
[]
[null,"TEMPORARY WORKS",{"$nulls":8},596,null,1650,{"$nulls":12},1,3,1,6,"H","0"]
[]
["6","1,5m High 'Bonnox' wire mesh temporary fencing with shade cloth.","m",320,null,0,null,null,320,null,597,null,1650,{"$nulls":12},1,3,1,6,"I","1"]
[]
["7","Single gate 900 x 1,5m high.","No",2,null,0,null,null,2,null,598,null,1650,{"$nulls":12},1,3,1,6,"I","N"]
[]
[null,"GENERAL SITE CLEARANCE, ETC.",{"$nulls":8},599,null,1650,{"$nulls":12},1,3,1,6,"H","0"]
[]
[null,"Site clearance, etc.:",{"$nulls":8},600,null,1652,{"$nulls":12},1,3,1,6,"S","0"]
[]
["8","Allow for clearing of the site all grass, weeds, shrubs, debris, etc and cartwaway all vegetation and stockpile","m²","  1 200",null,0,null,null,1200,null,602,null,1654,{"$nulls":12},1,3,1,6,"I","2"]
[]
["9","Strip average 100mm thick layer of topsoil and stockpile on site","m²",450,null,0,null,null,450,null,1731,null,1654,{"$nulls":12},1,3,1,6,"I","2"]
[]
["10","Spread and level imported topsoil oversite as directed","m²",300,null,0,null,null,300,null,1732,null,1654,{"$nulls":12},1,3,1,6,"I","2"]
[]
[null,"Trimming of trees, etc",{"$nulls":8},1804,null,1654,{"$nulls":12},1,3,1,6,"S"]
[]
["11","Allow a monetary allowance for trimming of trees","Item",null,null,0,null,null,1,null,1805,null,1654,{"$nulls":12},1,3,1,6,"I","I"]
[]
[null,"KEEPING EXCAVATIONS FREE OF WATER",{"$nulls":8},607,null,1812,{"$nulls":12},1,3,1,6,"H","0"]
[]
[null,"Keeping excavations free of water:",{"$nulls":8},608,null,1814,{"$nulls":12},1,3,1,6,"S","0"]
[]
["12","Keeping excavations free of all water other than subterranean water through out this bill .","Item",1,null,0,null,null,1,null,609,null,1815,{"$nulls":12},1,3,1,6,"I","I"]
[]
[null,"Monetary Allowance",{"$nulls":8},1765,null,1668,{"$nulls":12},1,3,1,6,"S"]
[]
["13","Allow a provisional allowance of R 100 000.00 (One Hundred Thousand Rands) for external works to be ascertained on site","Item",null,null,0,null,null,1,null,1806,null,1668,{"$nulls":12},1,3,1,6,"I","I"]
[]
["14","Allow a provisional allowance of R 65 000.00 (Sixty Five Thousand Rands) for refurbishment of carport","Item",null,null,0,null,null,1,null,2703,null,1668,{"$nulls":12},1,3,1,6,"I","I"]
[]
["15","Allow a provisional allowance of R 30 000.00 (Thirty Thousand Rands) for refurbishment of prefab classroom","Item",null,null,0,null,null,1,null,2705,null,1668,{"$nulls":12},1,3,1,6,"I","I"]
[]
[]
[null,"Bill Total",{"$nulls":4},0]
[]
[]
[]
[null,"BILL NO.2 : PLUMBING AND DRAINAGE (PROVISIONAL)",{"$nulls":23},1,3,2,54,"H"]
[]
[null,"STORM WATER CHANNELS.",{"$nulls":8},992,null,1761,{"$nulls":12},1,3,2,54,"H","0"]
[]
[null,"Smooth finished in-situ reinforced concrete 25Mpa/13mm channels:",{"$nulls":8},993,null,1763,{"$nulls":12},1,3,2,54,"S","0"]
[]
["1","900 x 130mm Smooth  finished open V shaped  channel to detail, cast in alternative panels and to falls, including excavations, shaping and grading ground as required, formwork, mesh Ref 193.","m",550,null,0,null,null,550,null,999,null,17287,{"$nulls":12},1,3,2,54,"I","1"]
[]
["2","Extra for angles, intersections, ends, dressing into sides of catchpits, etc.","No",36,null,0,null,null,36,null,995,null,17289,{"$nulls":12},1,3,2,54,"I","N"]
[]
["3","12mm Thick bitumen impregnated softboard between vertical concrete surfaces of channels.","m",550,null,0,null,null,550,null,1000,null,17287,{"$nulls":12},1,3,2,54,"I","1"]
[]
["4","Approved polysulphide sealing compound to joints of channels.","m",550,null,0,null,null,550,null,1001,null,17287,{"$nulls":12},1,3,2,54,"I","1"]
[]
[null,"Monetary Allowance",{"$nulls":8},1808,null,1816,{"$nulls":12},1,3,2,54,"S"]
[]
["5","Allow a monetary allowance fo R50 000.00 for proving and cleaning pipework","Item",null,{"v":50000,"d":"50,000.00"},{"v":50000,"d":"50,000.00"},null,null,1,null,1809,null,1816,{"$nulls":12},1,3,2,54,"I","I"]
[]
["6","Allow a monetary allowance of R45 000.00 for cleaning of all sewer and stormwater manholes","Item",null,{"v":45000,"d":"45,000.00"},{"v":45000,"d":"45,000.00"},null,null,1,null,1810,null,1816,{"$nulls":12},1,3,2,54,"I","I"]
[]
["7","Allow a monetary allowance of R30 000.00 for the construction of stormwater berms","Item",null,{"v":30000,"d":"30,000.00"},{"v":30000,"d":"30,000.00"},null,null,1,null,2704,null,1816,{"$nulls":12},1,3,2,54,"I","I"]
[]
[null,"TESTING",{"$nulls":8},1187,null,1816,{"$nulls":12},1,3,2,54,"H","0"]
[]
["8","Testing all plumbing systems.","Item",1,null,0,null,null,1,null,1188,null,1816,{"$nulls":12},1,3,2,54,"I","I"]
[]
[]
[null,"Bill Total",{"$nulls":4},{"v":125000,"d":"125,000.00"}]
[]
[]
[null,"Section Total ",{"$nulls":4},{"v":125000,"d":"125,000.00"}]
[]
[]
[null,"SECTION NO. 4 : PROVISIONAL SUMS",{"$nulls":23},1,4,1,99,"H"]
[]
[]
[null,"BILL NO.1 : PROVISIONAL SUMS",{"$nulls":23},1,4,1,99,"H"]
[]
[null,"The following Provisional Amounts are all Net amounts Exclusive of commision for the Contractor. These amounts are for the work to be executed complete by the Nominated/Selected Sub-Contractors:",{"$nulls":8},1272,null,27973,{"$nulls":12},1,4,1,99,"S","0"]
[]
[null,"LANDSCAPING",{"$nulls":8},1317,null,28007,{"$nulls":12},1,4,1,99,"H","0"]
[]
["1","Provide the amount of R 30,000.00 (Thirty Thousand Rands) for Landscaping, etc.","Item",1,{"v":30000,"d":"30,000.00"},{"v":30000,"d":"30,000.00"},null,null,1,null,1349,null,28010,{"$nulls":12},1,4,1,99,"I","I"]
[]
["2","Profit on above item.","Item",null,null,0,null,null,1,null,1319,null,28011,{"$nulls":12},1,4,1,99,"I","I"]
[]
["3","Attendance on ditto.","Item",null,null,0,null,null,1,null,1320,null,28012,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"SIGNAGE",{"$nulls":8},1321,null,28007,{"$nulls":12},1,4,1,99,"H","0"]
[]
["4","Provide the amount of R 15,000.00 (Fifteen Thousand Rands) for Signage.","Item",1,{"v":15000,"d":"15,000.00"},{"v":15000,"d":"15,000.00"},null,null,1,null,1350,null,28010,{"$nulls":12},1,4,1,99,"I","I"]
[]
["5","Profit on above item.","Item",null,null,0,null,null,1,null,1323,null,28011,{"$nulls":12},1,4,1,99,"I","I"]
[]
["6","Attendance on ditto.","Item",null,null,0,null,null,1,null,1324,null,28012,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"CARPENTRY & JOINERY",{"$nulls":8},2439,null,36195,{"$nulls":12},1,4,1,99,"H","I"]
[]
["7","Provide the amount of R 450,000.00 (Four Hundred and Fifty Thousand  Rands) for Carpentry & Joinery to Classrooms.","Item",1,{"v":450000,"d":"450,000.00"},{"v":450000,"d":"450,000.00"},null,null,1,null,2440,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["8","Profit on above item.","Item",null,null,0,null,null,1,null,2441,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["9","Attendance on ditto.","Item",null,null,0,null,null,1,null,2442,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"PLUMBING AND DRAINAGE",{"$nulls":8},2626,null,36195,{"$nulls":12},1,4,1,99,"H","I"]
[]
["10","Provide the amount of R 300,000.00 (Three  Hundred Thousand Rands) for Plumbing and Drainage","Item",1,{"v":300000,"d":"300,000.00"},{"v":300000,"d":"300,000.00"},null,null,1,null,2627,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["11","Profit on above item.","Item",null,null,0,null,null,1,null,2628,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["12","Attendance on ditto.","Item",null,null,0,null,null,1,null,2629,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"GEOTECH & SURVEY",{"$nulls":8},2630,null,36195,{"$nulls":12},1,4,1,99,"H","0"]
[]
["13","Provide the amount of R 100,000.00 (One Hundred Thousand  Rands) for Geotech & Survey","Item",1,{"v":100000,"d":"100,000.00"},{"v":100000,"d":"100,000.00"},null,null,1,null,2631,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["14","Profit on above item.","Item",null,null,0,null,null,1,null,2632,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["15","Attendance on ditto.","Item",null,null,0,null,null,1,null,2633,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"TEMPORARY ACCOMODATION & ABLUTIONS",{"$nulls":8},2634,null,36195,{"$nulls":12},1,4,1,99,"H"]
[]
["16","Provide the amount of R 3 305 000.00 (Three Million Three Hundred and Five Thousand Rands) for the Purchase, transportation, ground preparation works and erection of mobile classrooms and ablution facilities, including the regular maintenance of ablution facilities for the duration of construction. The units are made good upon project completion and relocated to another site determined by the Principal Agent and/or client, less than or equal to 200km from the site as per Architectural/Engineering specifications, to be performed by specialist where required","Item",1,{"v":3305000,"d":"3,305,000.00"},{"v":3305000,"d":"3,305,000.00"},null,null,1,null,2635,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["17","Profit on above item.","Item",null,null,0,null,null,1,null,2636,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["18","Attendance on ditto.","Item",null,null,0,null,null,1,null,2637,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"The following Electrical Works are to be undertaken by direct contractors, selected at the client's discretion",{"$nulls":8},2436,null,36195,{"$nulls":12},1,4,1,99,"S","I"]
[]
[null,"ELECTRICAL INSTALLATION",{"$nulls":8},1754,null,36195,{"$nulls":12},1,4,1,99,"H"]
[]
["19","Provide the amount of R 300 000.00 (Three Hundred Thousand Rands) for Electrical Installation","Item",1,{"v":300000,"d":"300,000.00"},{"v":300000,"d":"300,000.00"},null,null,1,null,1755,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["20","Profit on above item.","Item",null,null,0,null,null,1,null,1756,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["21","Attendance on ditto.","Item",null,null,0,null,null,1,null,1757,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"BUDGETARY ALLOWANCES",{"$nulls":8},1677,null,36195,{"$nulls":12},1,4,1,99,"H","0"]
[]
["22","Allow a budgetary amount of R 150 000.00 (One Hundred and Fifty Thousand Rands) for Community Liaison Officer (CLO)","Item",1,{"v":150000,"d":"150,000.00"},{"v":150000,"d":"150,000.00"},null,null,1,null,1683,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
["23","Allow a budgetary amount of R 6 500.00 / month for Project Steering Committee","Item",1,{"v":65000,"d":"65,000.00"},{"v":65000,"d":"65,000.00"},null,null,1,null,2435,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
["24","Allow a budgetary amount of R 5 263.00 / month for CIDB Build / Skill Development","Item",1,{"v":52630,"d":"52,630.00"},{"v":52630,"d":"52,630.00"},null,null,1,null,2435,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
[null,"BUILDER'S WORK IN CONNECTION WITH PROVISIONAL SUMS",{"$nulls":8},2437,null,36195,{"$nulls":12},1,4,1,99,"H","0"]
[]
["25","Provide the amount of R 25.000.00 (Twenty Five Thousand Rands) for Builder's Work in connection with Provisional Sums.","Item",1,{"v":25000,"d":"25,000.00"},{"v":25000,"d":"25,000.00"},null,null,1,null,2438,null,36195,{"$nulls":12},1,4,1,99,"I","I"]
[]
[]
[null,"Bill Total",{"$nulls":4},{"v":4792630,"d":"4,792,630.00"}]
[]
[]
[null,"Section Total ",{"$nulls":4},{"v":4792630,"d":"4,792,630.00"}]