{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["ENVIRONMENTAL COSTING","OHS COSTING"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"ENVIRONMENTAL COSTING","index":0,"n_rows":44,"n_cols":6,"rows_kept":44,"hidden":true,"merged":[[2,0,2,4],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,7,3],[5,4,6,4],[30,0,30,4],[35,0,35,4],[37,0,37,4],[40,0,40,4],[42,0,42,4]],"flags":["formulas_cached_only"]}
[]
[null,"ANNEXURE C: BOQ ENVIRONMENTAL WORKS "]
["          NAME OF PROJECT :                                                                                   "]
[]
[]
["ITEM","DESCRIPTION","UNIT","PRICE PER UNIT","TOTAL"]
[]
[]
["1. Waste Management  ( Costs associated with the management of general, hazardous waste, etc.)"]
["1.1","Waste Bins, skips & lids and covers"]
["1.2","General waste collection and disposal at a registered landfill site as per EMP requirements"]
[1.3,"Hazardous waste transportation and disposal at a registered facility"]
[1.4,"Costs associated with the supply & installation of sceptic tanks"]
[1.5,"Costs associated with sewerage removal contracts."]
[1.6,"Costs associated with the   repair and maintenance of all sewerage pipes.  "]
[1.7,"Oil spill kits"]
[1.8,"Oil separator"]
[1.9,"Drip trays"]
[{"v":1.1,"d":"1.10"},"Container for soaking empty cement bags prior to disposal."]
[1.11,"Any other:  Contractor to specify :  ………………………………………                                                                                              "]
["2. Land Management"]
[2.1,"Rehabilitation: Costs associated with the rehabilitation of disturbed land during construction."]
[2.2,"Costs associated with vegetation clearing and the eradication of Alien / invasive vegetation."]
["2.3.","Costs associated with the supply & installation of gates"]
[2.4,"Erection of fences"]
[2.5,"No Go fencing"]
[2.6,"Signage:  No-go areas / acces route markers"]
[2.7,"Erosion control and berms",{"$nulls":3}," "]
[2.8,"Supply and installation of drainage pipes"]
[2.9,"Maintenance of access road"]
["3. Pollution"]
[3.1,"Costs associated with dust supression and remediation"]
[3.2,"Creation of  bundwalls"]
[3.3,"Building of  Washbays & Workshops"]
[3.4,"Costs associated with water  pollution monitoring (where necessary)"]
["4. Water "]
[4.1,"Costs associated with water use"]
["5. Human Resources"]
[5.1,"Appointment of Environmental Officer (EO) where applicable"]
[5.2,"Costs associated with the appointment of environmental personnel and actual time spent on implementation, managing, documenting, monitoring, reviewing, internal audits, incident investigations and mitigating environmentally related impacts and rehabilitation (air, water, waste, land)"]
["6. Environmental Management Systems"]
[6.1,"Implementation of an Environmental management System e.g ISO 14001( Specify)"]
["7. Other"]
[7.1,"Any other environmental costs for the sole purpose of sustaining, improving, rectifying damage to or protecting the environment from real or perceived impact: (the contractor to specify)"]

{"sheet":"OHS COSTING","index":1,"n_rows":80,"n_cols":7,"rows_kept":80,"merged":[[2,0,3,0],[2,1,3,1],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[5,1,5,6],[6,2,17,2],[18,1,18,6],[19,2,24,2],[25,1,25,6],[26,2,29,2],[32,1,32,6],[33,2,45,2],[46,1,46,6],[47,2,49,2],[51,0,52,6],[58,0,59,0],[58,1,59,1],[58,3,59,3],[58,4,59,4],[58,5,59,5],[58,6,59,6],[61,1,61,6],[62,2,68,2],[69,1,69,6],[71,1,71,6],[73,1,73,6],[74,2,78,2],[81,0,82,6]],"flags":["formulas_cached_only"]}
[]
[null,"Health and Safety Costing"]
["ITEM","DESCRIPTION",null,"UNIT","QUANTITY","PRICE PER UNIT","TOTAL"]
[null,null,"Reference"]
[{"$nulls":4},"(1)","(2)","(1)*(2)"]
["1.","Supply of all items of Personal Protective Clothing/Equipment & ensure use thereof for full compliance"]
["1.1","Steel toe capped safety boots ","General Safety Regulation 2: Personal Safety Equipment and Facilities and Asbestos Abatement Regulation 19: Personal protective equipment and facilities"]
["1.2","Appropriate protective clothing"]
["1.3","Gloves"]
["1.4","Colour coded hardhats [Blue for labourer, Red for First Aider,  Green for SHE Reps and White for Supervisors and Managers]"]
["1.5","Ear protection (earplugs etc)"]
["1.6","Eye protection appropriate to task performed"]
["1.7","Induction tags/cards"]
[1.8,"Dust masks"]
[1.9,"Asbestos PPE"]
["1,10","Covid 19 PPE"]
[1.11,"Luminous high visibility safety vests"]
[1.12,"Any other:  Contractor to specify :  …Rain coats PPE…………………………………………                                                                                                 "]
["2.","Performing work in a Fall Risk Position"]
[2.1,"Fall Protection Plan developer","Construction Regulation 10: Fall Protection"]
[2.2,"Fall Protection Plan  "]
[2.3,"Fall protection equipment (Safety Harness)"]
[2.4,"Fall Prevention equipment (Gaurdrails, barricading, achors)"]
[2.5,"Evaluation of physical  fitness of personnel working at heights"]
[2.6,"Any other:  Contractor to specify :  …………………………………………………………………………………………………………………………………………………………………………                                                                                 "]
[3,"Barricading and Signage"]
[3.1,"Supply & install, including removal upon completion to ensure full compliance to legislation","Construction Regulation 13: Excavataion"]
[3.2,"Rigid type barricading"]
[3.3,"Temporary fence barricading along perimeter of excavated area"]
[3.4,"Appropriate equipment/tools for excavation."]
[3.5,"Provision of all signage for all relevant activities  in terms of latest revision  of legislation","General Safety Regulation 2B: Display of substituted notices and signs"]
[3.5,"Any other:  Contractor to specify : …………………………………………………………………………………………………………………………………………………………………………"]
[4,"Related Training"]
[4.1,"Induction Training","Construction Regulations, General Safety Regulations, ORHVS, Driven Machinery Regulations, Asbestos Abatement Regulations"]
[4.2,"First Aid Training"]
[4.3,"Health and Safety Representative training"]
[4.4,"Incident Investigator Training"]
[4.5,"Hazard Identification & Risk Assessment Training"]
[4.6,"Training of Personnel working at heights"]
[4.7,"Operating for High Voltage systems"]
[4.8,"Ladder Inspector Training"]
[4.9,"Crane Operator Training"]
[4.1,"Construction vehicle & Mobile plant Operator e.g. trucks, drills bakkies etc"]
[4.11,"Training to operate Jackhammer,  etc"]
[4.12,"Fire Fighting Training"]
[4.13,"Any other:  Contractor to specify : Asbestos Awareness ………………………………………………………………………………………                                                                                                "]
[5,"Safety Management System"]
[5.1,"Implementation of Health and Safety Management System  on site as detailed in OHS Plan and associated documentation","Construction Regulation 7: Duties of Principal Contractor and contractor, 32-726: SHE Commercial Process, PLCM"]
[5.2,"Availability of Principal Contractor resources & systems.  Provision of monthly audits to ensure compliance to Client and Legaslative requirements. Submission of monthly statistical data and audit reports to Client"]
[5.3,"Site close out and OHS file submission"]
[]
[]
[]
[]
[]
[]
["HEALTH AND SAFETY WORKS Cont."]
[]
["ITEM","DESCRIPTION",null,"UNIT","QUANTITY","PRICE PER UNIT","TOTAL"]
[]
[{"$nulls":4},"(1)","(2)","(1)*(2)"]
[6,"Occupational Hygiene"]
[6.1,"Health Risk Assessment","Noise Induced Hearing Loss Regulations, Asbestos Abatement Regulations, Hazardous Chemical Substances Regulations, Constructio Regulation 14: Demolition Work"]
[6.2,"Occupational Hygiene Surveys"]
["6.2.1","Ergonomics"]
["6.2.2","Dust survey (asbestos analysis and reporting to DEL)"]
["6.2.3","Noise survey for all noise generating equpment"]
["6.2.4","Structural Engineer Survey"]
["6.2.5","Any other: Contractor to specify: ………………………………………………………………………………"]
[7,"Medical Screeining "]
[7.1,"Medical Screeining (pre, post and during) done by Occupational Health Practitioner","Construction Regulation 7(8), Noise Induced Hearing Loss Regulations, Asbetsos Regulations, Hazardous Chemical Substances Regulations"]
[8,"Transport"]
[8.1,"Transportation of employees in compliance with the Transportation of employees procedure","Construction Regulation 23(2) (i) & (j): Construction Vehicles and Mobile Plant"]
[9,"Human Resources"]
[9.1,"Appointment of a Full-Time Construction Safety Officer","Construction Regulation8(5): Management and Supervision of Construction work, Asbestos Abatement Regulations, Construction Regulation 14: Demolition Work"]
["9.2","Structural Engineer (For any dismantling/ demolition activities)"]
["9.3","Approved Asbestos Inspection Authority (AIA - Asbestos Work)"]
["9.4","Registered Asbestos Contractor (RAC - Asbestos Work)"]
["9.5","Any other: Contractor to specify: ………………………………………………………………………………"]
[{"$nulls":5},"TOTAL"]