Specifications for the potato harvester

Supply and delivery of Small Potato harvester
Small Potato harvester for to be used for sweet potatoes
Must be operated by a normal size tractor for example a Landini 8865
Working width 900-1000 mm
Working depth minimum 30 cm
To connect to the 3-point system of a standard tractor
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