{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":4126,"n_cols":15,"rows_kept":4126,"merged":[[1,1,1,2],[2,1,2,7],[5,5,5,7],[70,1,70,2],[71,1,71,7],[72,1,72,7],[75,5,75,7],[138,1,138,2],[139,1,140,7],[143,5,143,7],[211,1,211,2],[212,1,213,7],[216,5,216,7],[281,1,281,2],[282,1,282,7],[286,5,286,7],[352,1,352,2],[353,1,354,7],[357,5,357,7],[420,1,420,2],[421,1,422,7],[425,5,425,7],[484,1,484,2],[485,1,486,7],[488,5,488,7],[549,1,549,2],[551,1,552,7],[554,5,554,7],[611,1,611,2],[612,1,613,7],[616,5,616,7],[680,1,680,2],[681,1,682,7],[686,5,686,7],[767,1,767,2],[768,1,769,7],[773,5,773,7],[848,1,848,2],[849,1,850,7],[854,5,854,7],[923,1,923,2],[924,1,926,7],[929,5,929,7],[992,1,992,2],[993,1,995,7],[998,5,998,7],[999,3,1000,3],[999,4,1000,4],[999,5,1000,5],[1084,1,1084,2],[1085,1,1086,7],[1090,5,1090,7],[1091,3,1092,3],[1091,4,1092,4],[1091,5,1092,5],[1150,1,1150,2],[1151,1,1152,7],[1156,5,1156,7],[1225,1,1225,2],[1226,1,1227,7],[1231,5,1231,7],[1293,1,1293,2],[1294,1,1295,7],[1299,5,1299,7],[1362,1,1362,2],[1363,1,1364,7],[1367,5,1367,7],[1443,1,1443,2],[1444,1,1445,7],[1449,5,1449,7],[1507,1,1507,2],[1508,1,1509,7],[1513,5,1513,7],[1571,1,1571,2],[1572,1,1573,7],[1577,5,1577,7],[1635,1,1635,2],[1636,1,1637,7],[1641,5,1641,7],[1699,1,1699,2],[1700,1,1701,7],[1705,5,1705,7],[1763,1,1763,2],[1764,1,1765,7],[1769,5,1769,7],[1843,1,1843,2],[1844,1,1845,7],[1849,5,1849,7],[1907,1,1907,2],[1908,1,1909,7],[1913,5,1913,7],[1970,1,1970,2],[1971,1,1972,7],[1976,5,1976,7],[2034,1,2034,2],[2035,1,2036,7],[2040,5,2040,7],[2098,1,2098,2],[2099,1,2100,7],[2104,5,2104,7],[2163,1,2163,2],[2164,1,2165,7],[2169,5,2169,7],[2227,1,2227,2],[2228,1,2229,7],[2233,5,2233,7],[2291,1,2291,2],[2292,1,2293,7],[2297,5,2297,7],[2355,1,2355,2],[2356,1,2357,7],[2361,5,2361,7],[2419,1,2419,2],[2420,1,2421,7],[2425,5,2425,7],[2483,1,2483,2],[2484,1,2485,7],[2489,5,2489,7],[2547,1,2547,2],[2548,1,2549,7],[2553,5,2553,7],[2612,1,2612,2],[2613,1,2614,7],[2618,5,2618,7],[2674,1,2674,2],[2675,1,2676,7],[2680,5,2680,7],[2738,1,2738,2],[2739,1,2740,7],[2744,5,2744,7],[2802,1,2802,2],[2803,1,2804,7],[2808,5,2808,7],[2865,1,2865,2],[2866,1,2867,7],[2871,5,2871,7],[2929,1,2929,2],[2930,1,2931,7],[2935,5,2935,7],[2994,1,2994,2],[2995,1,2996,7],[3000,5,3000,7],[3056,1,3056,2],[3057,1,3058,7],[3062,5,3062,7],[3120,1,3120,2],[3121,1,3122,7],[3126,5,3126,7],[3184,1,3184,2],[3185,1,3186,7],[3190,5,3190,7],[3248,1,3248,2],[3249,1,3250,7],[3254,5,3254,7],[3310,1,3310,2],[3311,1,3312,7],[3316,5,3316,7],[3375,1,3375,2],[3376,1,3377,7],[3380,5,3380,7],[3438,1,3438,2],[3439,1,3440,7],[3444,5,3444,7],[3513,1,3513,2],[3514,1,3515,7],[3519,5,3519,7],[3520,3,3521,3],[3520,4,3521,4],[3520,5,3521,5],[3582,1,3582,2],[3583,1,3584,7],[3588,5,3588,7],[3589,3,3590,3],[3589,4,3590,4],[3589,5,3590,5],[3664,1,3664,2],[3665,1,3666,7],[3670,5,3670,7],[3731,1,3731,2],[3732,1,3733,7],[3737,5,3737,7],[3802,1,3802,2],[3803,1,3804,7],[3808,5,3808,7],[3890,1,3890,2],[3891,1,3892,7],[3896,5,3896,7],[3976,1,3976,2],[3977,1,3978,7],[3982,5,3982,7],[4062,1,4062,2],[4063,1,4064,7],[4067,5,4067,7],[4068,5,4068,7],[4069,1,4069,2],[4069,6,4069,7],[4070,6,4071,7],[4071,1,4071,2],[4072,6,4073,7],[4073,1,4073,2],[4074,6,4076,7],[4075,1,4075,2],[4077,6,4079,7],[4078,1,4078,2],[4080,6,4082,7],[4081,1,4081,2],[4083,6,4085,7],[4084,1,4084,2],[4086,6,4088,7],[4087,1,4087,2],[4089,6,4091,7],[4090,1,4090,2],[4092,6,4094,7],[4093,1,4093,2],[4095,1,4095,2],[4096,1,4096,2],[4096,6,4097,7],[4098,6,4100,7],[4099,1,4099,2],[4101,6,4103,7],[4102,1,4102,2],[4104,6,4106,7],[4105,1,4105,2]],"flags":["formulas_cached_only"]}
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[null,"SCHEDULE 1"]
[]
[null,"SANS 1200 A - PRELIMINARY AND GENERAL"]
[null,"ITEM","PAYMENT","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[null,"No.","REFERS",{"$nulls":4}," R        C"]
[]
[null,null,"SANS ","CONTRACTORS ESTABLISHMENT AND PRELIMINARY AND "]
[null,null,"1200 A","GENERAL"]
[]
[]
[]
[null,null,8.3,"Fixed-charge and value related item"]
[]
[]
[null,"A1","PSA 8.3.1","Contractual requirements for the provision of all sureties, Insurance of ","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"the works and Plant, Third Party Liability Insurance, Unemployment "]
[{"$nulls":3},"Insurance and any other statutory requirements"]
[]
[null,"A2","8.3.1.1","Political riot insurance ","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.3.2","Establishment of Facilities on Site (Only on the written instruction of the "]
[{"$nulls":3},"Engineer)"]
[]
[null,null,"PSA ","Facilities for the Engineer"]
[null,null,"8.3.2.1"]
[null,"A3",null,"(a) Furnished offices (1 No.)","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A4",null,"(b) Telephone (1 Cellphone with Simcard)","Prov. Sum",{"v":1,"d":"1.00"},{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[]
[null,"A5",null,"(c) Percentage mark-up on (c) above","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A6",null,"(d) Nameboards (2 No.)","Sum",{"v":2,"d":"2.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A7","PSA ","(e) PPE for Engineer and assistants","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,null," 8.3.2.1(a)"]
[null,null,"PSA","(f) Survey instruments, etc.","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,null," 8.3.2.1(b)"]
[]
[null,null,"8.3.2.2","Facilities for the Contractor"]
[]
[{"$nulls":3},"All facilities as scheduled in Clause 8.3.2.2 of SANS 1200A"]
[]
[null,"A8",null,"(a) Offices and storage sheds","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A9",null,"(b) Workshops","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A10",null,"(c) Laboratories","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A11",null,"(d) Living accommodation","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A12",null,"(e) Ablution and toilet facilities","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A13",null,"(f) Tools and equipment","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A14",null,"(g) Water supplies, electric power and  communications","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A15",null,"(h) Dealing with water (see 5.8)","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A16",null,"(i) Access (see 5.8)","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A17",null,"(j) Plant","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A18","PSA ","(k) PPE for Contractors staff, suppliers, subcontractors and visitors","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,null,"8.3.2.2(c)","      "]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":10000,"d":"10,000.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[null,"SCHEDULE 1"]
[]
[null,"SABS 1200A - PRELIMINARY AND GENERAL"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":10000,"d":"10,000.00"}]
[]
[null,"A19","PSA 8.3.3","Other fixed-charge obligations","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A20","8.3.4","Removal of Site Establishment (On Instruction by Engineer)","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A21","PSA 8.3.5","Provision of a Safety Plan in terms of OHS Act and Safety Regulations","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,8.4,"Scheduled Time-related items"]
[]
[null,"A22","PSA 8.4.1","Contractual requirements","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.4.2","Operation and maintenance of facilities for the duration of construction"]
[]
[null,null,"PSA ","Facilities for the Engineer"]
[null,null,"8.4.2.1"]
[null,"A23",null,"(a) Furnished offices (1 No.)","Month",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A24",null,"(b) Telephone (R900 per month airtime for cellphone)","Month",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A25",null,"(c) Nameboards (2 No.)","Month",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A26",null,"(d) Survey instruments, etc.","Month",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A27","PSA","(e) PPE for Engineer and assistants","Month",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A28",null,"(a) Offices and storage","Month",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A29",null,"(b) Workshops","Month",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A30",null,"(c) Laboratories","Month",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A31",null,"(d) Living accommodation","Month",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A32",null,"(e) Ablution and toilet","Month",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A33",null,"(f) Tools and equipment","Month",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A34",null,"(g) Water supplies, electric power and  communications","Month",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A35",null,"(h) Dealing with water (Sub-clause5.8)","Month",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A36",null,"(i) Access (Sub-clause 5.8)","Month",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A37",null,"(j) Plant","Month",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A38","PSA 8.4.3","Supervision for duration of construction","Month",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A39","PSA 8.4.4","Company and head office overhead costs for the duration of the contract","Month",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A40","PSA 8.4.5","Other time-related obligations","Month",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A41","PSA 8.4.6","Compliance with approved Safety Plan and Occupational Health and ","Month",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3}," Safety Act Construction Regulations"]
[]
[null,"A42","PSA 8.4.7","Compliance with Record of Decision issued by GDARD","Month",{"v":12,"d":"12.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":10000,"d":"10,000.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 1"]
[null,"SABS 1200A - PRELIMINARY AND GENERAL"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":10000,"d":"10,000.00"}]
[]
[null,null,"PSA 8.5","SUMS STATED PROVISIONALLY BY ENGINEER"]
[]
[null,null,"PSA 8.5.1","Control Testing requested by the Engineer"]
[]
[null,"A43",null,"(i) Provisional Sum",null,{"v":1,"d":"1.00"},"Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"A44",null,"(ii) Contractors mark-up on (A) 43 above","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A45",null,"Pipe and Manufacturing Inspection",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"A46",null,"Contractors Mark-up on A45 above","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A47",null,"Pipe Site Inspection",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"A48",null,"Contractors Mark-up on A47 above","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[null,"A51","PSA 8.5.2","Hire of land for Contractors Camp Site"]
[]
[null,"A52",null,"(i) Leasing land for campsite, plant etc.","Month",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"PSA 8.5.2 (a)","Works executed by Nominated Subcontractors"]
[]
[{"$nulls":3},"(a) Work to be executed by a Nominated Subcontractor.",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[{"$nulls":3},"(b) Overheads, charges and profit on item (a) above.","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
[]
[]
[null,"A53","8.5.3","CLO's"]
[]
[{"$nulls":3},"Payment for CLO"]
[]
[null,"A54",null,"(i) Remuneration of CLO (based on R3650/month incl. traveling ","Month",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"    allowance)"]
[{"$nulls":13},55,100]
[null,"A55",null,"(ii) Cell phone allowance (R150 airtime ","Month",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"},{"$nulls":5},45.5,"x"]
[{"$nulls":3},"      per month)"]
[]
[null,"A56",null,"(iii) Contractors mark-up on items (i) and ","%",{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"      (ii) above for Contractor's overheads,",{"$nulls":9},"55x",4150]
[{"$nulls":3},"     liaison,making payments and supplying office"]
[{"$nulls":3},"     space and associated facilities within his",{"$nulls":9},"x",75.45454545454545]
[{"$nulls":3},"     establishment"]
[]
[null,null,"PSA 8.5.4","Training"]
[]
[null,"A57",null,"(a) Safety rep training","hr",{"v":1,"d":"1.0"},null,{"v":0,"d":"0.00"},{"$nulls":5},50]
[{"$nulls":3},"(b) Project specific technical skills training","hr",{"v":1,"d":"1.0"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"(c) Generic and management skills training","hr",{"v":1,"d":"1.0"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"(d) Training venue ","hr",{"v":1,"d":"1.0"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"(e) Remuneration of workers undergoing skills training","hr",{"v":1,"d":"1.0"},null,{"v":0,"d":"0.00"}]
[]
[null,"A58",null,"(ii) Contractors marp-up on A57 above","%",{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.5.5","Security Guards"]
[]
[null,"A59",null,"Provide Security guard (armed response) for duration of the  ","Month",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"construction works after hours, and on instruction by the Engineer"]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 1"]
[null,"SABS 1200A - PRELIMINARY AND GENERAL"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"TEMPORARY WORKS"]
[null,"A60",null,"Provide and maintain access roads and adjacent streets including"]
[{"$nulls":3},"reinstatement of roads on completion of Works (or accommodation"]
[{"$nulls":3},"of traffic)"]
[]
[{"$nulls":3},"Existing services"]
[]
[null,"A61",null,"Excavate by hand in soft material to expose existing services","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A62",null,"Temporarily protection of existing services",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"A63",null,"Contractor's mark-up on A62 above","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A64",null,"Cast insitu class 20/19 concrete for encasing of existing services","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A65",null,"Welded steel reinforcing mesh (Ref 395)","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A66",null,"Relocation of existing services",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"A67",null,"Contractor's mark-up on A67 above","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A68",null,"POLITICAL UNREST SITUATIONS"]
[{"$nulls":3},"Allow for all costs which might arise due to the interruption of works "]
[{"$nulls":3},"and/or standing time in times of political unrest on site (rate"]
[{"$nulls":3}," to allow for transport of equipment and material)"]
[]
[null,"A69","PSA 8.6","Dayworks","Days",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Note: Executed on Instruction of the Engineer Only"]
[]
[null,"A70","8.6.1","Labour"]
[]
[null,"A71",null,"(i) Un-skilled","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A72",null,"(ii) Semi-skilled","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A73",null,"(iii) Skilled (artisan - welder plumber etc.)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A74",null,"(iv) Engineer","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A75",null,"(v) Technician","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A76",null,"(vi) Foreman","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A77",null,"(vii) Driver (LDV,machine, trucks, etc.)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A78",null,"(viii) Certified Blaster","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A79",null,"(ix) Steelfixer","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A80",null,"(x) Concretor","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A81",null,"(xi) Chargehand","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A82",null,"(xii) Security guard","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 1"]
[null,"SABS 1200A - PRELIMINARY AND GENERAL"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,null,"8.6.2","Plant and equipment"]
[]
[{"$nulls":3},"(a) Tractor loader backhoe (TLB)"]
[]
[null,"A83",null,"(i) Tractor Loader Backhoe (Bigger than ","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"      45kW but smaller than 70kW)"]
[]
[{"$nulls":3},"(b) Crawler Excavators"]
[]
[null,"A84",null,"(i) Smaller than 93kW (small)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A85",null,"(ii) Bigger than 93kW but smaller than 200kW ( Meduim)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"      "]
[null,"A86",null,"(iii) Bigger than 200kW but smaller than 400kW (Large)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"      "]
[{"$nulls":3},"(c) Tipper Trucks"]
[]
[null,"A87",null,"(i) Tipper trucks (3m³) Small","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A88",null,"(ii) Tipper trucks (5m³) Meduim","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A89",null,"(iii) Tipper trucks (10m³) Large","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(d) Flat Bed Trucks"]
[]
[null,"A90",null,"(i) Flat bed 5t capacity","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A91",null,"(ii) Flat bed 7t capacity","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(e) LDV"]
[]
[null,"A92",null," (i) 1t Pick-up","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A93",null,"(f) Mobile Crane 5t at 3m radius","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(g) Walk behind vibrating rollers"]
[]
[null,"A94",null,"(i) Model - Bomag 60 or similar  (small)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"           "]
[null,"A95",null,"(ii) Model - Bomag 76 or similar  (medium)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"           "]
[null,"A96",null,"(iii) Model - Bomag 90 or similar","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(h) Plate compactors"]
[]
[null,"A97",null,"(i) Vipac or similar","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(i) Rammers"]
[]
[null,"A98",null,"(i) Model - Wacker or similar","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(j) Concrete mixers"]
[]
[null,"A99",null,"(i) Volume 100 litre wet (small, towable)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A100",null,"(ii) Volume 175 litre wet (medium)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A101",null,"(iii) Volume 250 litre wet (large)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 1"]
[null,"SABS 1200A - PRELIMINARY AND GENERAL"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[{"$nulls":3},"(k) Diesel compressors including hoses and tools"]
[]
[null,"A102",null,"(i) Capacity smaller than 200 cfm (small)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"            "]
[null,"A103",null,"(ii) Capacity bigger than 200 cfm smaller than 400 cfm (medium)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"    "]
[null,"A104",null,"(iii) Capacity bigger than 400 cfm (large)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"            "]
[{"$nulls":3},"(l) Waterpump"]
[]
[null,"A105",null,"(i) Capacity smaller than 400 litre/min (medium)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":5},{"v":1,"d":"1.00"}]
[null,"A106",null,"(ii) Capacity bigger than 400 but smaller than 600 litre/min (medium) ","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"           "]
[null,"A107",null,"(iii) Capacity bigger than 600 but smaller then 1 100 litre/sec (large)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(m) Low-bed"]
[]
[null,"A108",null,"(i) Low-bed (suitable for the largest piece of equipment above)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A109",null,"(n) Grader (Cat 140 G or similar)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A110",null,"(o) Poker vibrator","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(p) Water tankers"]
[]
[null,"A111",null,"(i) Capacity 500 litre (small, towable)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A112",null,"(ii) Capacity 8 000 litre (medium)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A113",null,"(iii) Capacity 15 000 litre (large)","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A114",null,"Material to be used during execution of day works",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"A115",null,"Percentage adjustment to materials and plant not included in Daywork Schedule to cover contractor's expenses with regard to these items","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A116","PSA 8.9","Compliance with OHS Act and Regulations","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A116 (a)",null,"OHS Safety Officer (Full Time)","Month",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A117","PSA 8.10","Quality Assurance Management Plan ","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A118","PSA 8.11","Compliance with the environmental Management Plan","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"A116 (a)",null,"Environmental Control Officer (Full Time)","Month",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
{"$rows_empty":12}
[null,"CARRIED FORWARD TO SUMMARY"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 2"]
[null,"SABS 1200C - SITE CLEARANCE"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"C","SABS ","SECTION C:  SITE CLEARANCE"]
[null,null,"1200C"]
[null,null,"PSC 8.2.1","Clear and Grub"]
[null,"C1",null,"Areas for chambers, structures, etc","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C2",null,"Pipeline route 3m wide","m",{"v":4500,"d":"4,500.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.2","Remove and grub large trees and tree stumps with girth between:"]
[]
[null,"C3","8.2.2","(a) Over 0.1m and up to and indicating 1.0m (stumps)","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C4","8.2.2","(b) Over 0.1m and up to and indicating 2.0m (stumps)","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C5","8.2.2","(c) Over 0.1m and up to and indicating 3.0m (stumps)","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.7","Dismantle and remove pipelines, electricity transmission cables,"]
[{"$nulls":3}," cables etc. return salvaged material to Municipal stores"]
[]
[null,null,"8.2.7.1","Pipelines regardless of type:"]
[]
[null,"C6",null,"(a) 50mm Ø up to and including 300mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C7",null,"(b) 300mm Ø up to and including 500mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3}," "]
[null,"C8",null,"(c) 500mm Ø up to and including 750mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C9",null,"(d) 750mm Ø up to and including  1 000mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"    "]
[]
[null,"C10",null,"(e) 1 000mm Ø up to and including 1500mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.7.2","Cables (incl sleeves) :"]
[]
[null,"C11",null,"(a) 16mm Ø up to and including 30mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C12",null,"(b) 30mm Ø and larger","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.7.3","Valves complete with all fittings, specials, couplings and fasteners"]
[]
[null,"C13",null,"(i) Isolation valves","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C14",null,"(ii) Control Valves","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C15",null,"(iii) Scour Valves","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C16",null,"(iv) Air Valves","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C17",null,"(v) Fire hydrant valves","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"PSC8.2.8","Demolish and remove structures/buildings and dismantle steelwork, "]
[{"$nulls":3},"including all necessary appurtenances:"]
[]
[]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[null,"SCHEDULE 1"]
[null,"SABS 1200C - SITE CLEARANCE"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,"C18",null,"(a) Hawker shed regardless of type and size","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C19",null,"(b) Brick structures regardless of type and size including","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"      floors & foundations"]
[]
[{"$nulls":3},"(c) Brickwork Manholes Complete (depth 0-2m) with Longest"]
[{"$nulls":3},"      inside dimension:"]
[]
[null,"C20",null,"(i) 0m < Ø < 1.5m","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C21",null,"(ii) 1.5m < Ø < 2.5m","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C22",null,"(iii) > 2.5m","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(d) Circular Precast Concrete Manholes  (depth 0-2m)"]
[{"$nulls":3},"     "]
[{"$nulls":3},"Chamber Sections complete with step irons in sections 250 or "]
[{"$nulls":3},"500 or 1000 lengths"]
[]
[null,"C23",null,"(i) ND 750mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C24",null,"(ii) ND 1 000mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C25",null,"(iii) ND 1 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C26",null,"(iv) ND 1 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Reducer Slabs (Reduce to 750 Ø)  (0 - 2m depth)"]
[]
[null,"C27",null,"(i) ND 1 000mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C28",null,"(ii) ND 1 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C29",null,"(iii) ND 1 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Concrete Lid - remove:"]
[]
[null,"C30",null,"(i) ND 560mm heavy duty","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C31",null,"Base regardless of type, size and thickness.(0 - 2m depth)","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(e) Concrete slab:  0mm up to 350mm thick regardless "]
[{"$nulls":3},"     of type, reinforcement or position"]
[{"$nulls":3},"     "]
[]
[null,"C32",null,"(i) 0m < Ø < 1.5m","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C33",null,"(ii) 1.5m < Ø < 2.5m","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[null,"SCHEDULE 2"]
[null,"SABS 1200C - SITE CLEARANCE"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,"C34",null,"(iii) 2.5m < Ø < 3.5m","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C35",null,"(f) Break out manhole frame & lid regardless of type,","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     size or arrangement"]
[{"$nulls":3},"      "]
[null,"C36",null,"(g) Manhole step irons (0 - 2m depth)","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(h) Cast Iron (C.I.) Lid - remove:"]
[]
[null,"C37",null,"(i) Circular Road manholes (550mm Ø)  with C.I. Lid","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C38",null,"(ii) Circular Road manholes (650mm Ø) with C.I. Lid","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"      "]
[null,"C39",null,"(iii) Circular Road manholes > 650mm Ø, max. 1m","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"      "]
[null,"C40",null,"(i) Concrete benching regardless of  thickness (0 - 2m depth)","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     "]
[{"$nulls":3},"Extra-over item PSC8.2.8(c,d,e,g,i) Manholes  for deep excavations"]
[]
[null,"C41",null,"(i) Depth 2m up to and including 3m","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C42",null,"(ii) Depth 3m up to and including 4m","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C43",null,"(iii) Depth 4m and deeper","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C44",null,"(j) Segmented paving (Stack neatly for reinstatement measured ","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"    separately)"]
[]
[null,"C45","8.2.9","Transport materials and debris to an unspecified site and dump ","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"(All haulage = freehaul)"]
[]
[null,"C46","PSC8.2.10","Remove topsoil to a nominal depth of 150mm and stockpile","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"C44","PSC8.2.11","(j) Take down and re-erect existing fences","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
{"$rows_empty":16}
[null,"CARRIED FORWARD TO SUMMARY",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 3"]
[null,"SABS 1200D - EARTHWORKS"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"DA","SABS ","SECTION D:  EARTHWORKS "]
[null,null,"1200D"]
[null,null,"PSD 8.3.2","Bulk excavation"]
[]
[{"$nulls":3},"(a) Excavate in all materials and use for embankment or backfill as ordered"]
[null,"D1",null,"(i)  Necessary excavations   ","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"(ii)  Designated borrow pits      ","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"(iii)  c) Commercial sources  ","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"PSD","Restricted excavation:"]
[{"$nulls":3},"Excavate for chambers, restricted foundations,etc in"]
[{"$nulls":3},"in all materials, and use for backfill or embankment,"]
[{"$nulls":3},"or dispose:"]
[]
[null,"D1.1",null,"(i)  Depth up to 2,0 m        ","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"D1.2",null,"(ii)  Depth over 2,0 m and up to 4,0 m ","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"D3",null," Excavate for gabion boxes or  mattresses in all "]
[{"$nulls":3},"materials, and use for backfill or embankment,"]
[{"$nulls":3},"or dispose ","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra over items D1 and D3 above for:"]
[null,"D4",null,"(i)  Intermediate excavation  ","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"D5",null,"(ii)  Hard rock excavation     ","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"D6",null,"(iii)  Boulder excavation, class A ","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"D7",null,"(iv)  Boulder excavation, class B ","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"D8",null,"Extra over item D1 and D2 for hand  excavation","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"D9","8.3.5","Extra excavation in all materials to provide working ","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"space around structure"]
[]
[null,null,"PSD","Existing services:"]
[null,null,"8.3.8"]
[{"$nulls":3},"Hand excavation for locating and exposing existing"]
[{"$nulls":3},"services:"]
[]
[null,"D10",null,"(i)  In roadways","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"D11",null,"(ii)  In all other areas","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"D12","PSD","Topsoiling               ","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"D13","8.3.11","Grassing or other vegetation cover:"]
[]
[null,"D13",null,"Planting of grass cuttings       ","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"D14",null,"Hydroseeding             ","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"D15","PSD","Extra over item D1 and D2 for temporary stockpiling"]
[null,null,"8.3.14",null,"m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"D16","PSD","Extra over item D1 and D2 for disposing of spoil material on a "]
[null,null,"8.3.15","site provided by the Contractor","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[]
[]
[null,"CARRIED FORWARD TO SUMMARY",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 4"]
[]
[null,"SABS 1200 DA, DB, PSDA & PSDB - EARTHWORKS (PIPE TRENCH)"]
[null,"ITEM NO","PAYMENT REFERS"," DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,null,"SANS 1200","SECTION 4 : EARTHWORKS (PIPE TRENCH)"]
[null,null,"DA, DB, "]
[null,null,"PSDA, PSDB"]
[null,"DB1",null,"Excavation"]
[]
[null,null,"8.3.2(a)","Excavation in all materials for trenches 1,2m deep, "]
[{"$nulls":3},"backfill and compact, and dispose of surplus material"]
[{"$nulls":3},"for water mains"]
[]
[null,"DB2",null,"800 mm wide","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB3","8.3.2(a)","Excavate in all materials for trenches 1,1m deep, backfill,"]
[null,null,"PSLF 4","compact and dispose of surplus material for erf"]
[{"$nulls":3},"connections (gravel road crossings)","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB4","8.3.2(b)","Excavate in all materials for trenches 0.5m deep, backfill, "]
[{"$nulls":3},"compact and dispose of surplus material for erf "]
[{"$nulls":3},"connections inside stands for communication pipes","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"PSDB","Excavate in all materials, backfill and compact to"]
[null,null,"8.3.2(c)","90% mod AASHTO density, and dispose of "]
[{"$nulls":3},"surplus and unsuitable materials at spoil site"]
[{"$nulls":3},"arranged by the contractor, Over 1m and "]
[{"$nulls":3},"up to 2m wide"]
[]
[null,"DB6",null,"Pipes over and up to:"]
[null,"DB7",null,"(i)   Over 0 m up to 2,0 m    ","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"DB8",null,"(ii)  Over 2.0 m up to 3.0 m    ","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"DB9",null,"(iii) Over 3.0 m up to 4.0 m    ","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"(iii) Over 4.0 m up to5.0 m    ","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.3.2(b)","Extra over item D01 for:"]
[]
[null,"DB10",null,"Intermediate excavation (Provisional)","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"DB11",null,"Hard rock excavation (Provisional)","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"DB12",null,"Boulder excavation, Class A)","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"DB13",null,"Boulder excavation, Class B","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.3.3","Excavation Ancillaries"]
[]
[null,null,"8.3.3.1","Make up deficiency in backfill material"]
[]
[null,"DB14","8.3.3.1(a)","From other necessary excavations","m3",{"v":1,"d":"1.00"}]
[]
[null,"DB15","8.3.3.1(b)","By importation from designated borrow pit","m3",{"v":1,"d":"1.00"}]
[]
[null,"DB16","8.3.3.1(c) .","By importation from commercial or off-site sourcs selected by the Contractor","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB17","8.3.3.2","Opening up and closing down of designated borrow pit","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB18","PSDB 8","Extra over item DB4 for cement  stabilization of backfill"]
[{"$nulls":3},"under roads","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB19","PSDB 11","Remove and store block or brick paving","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB20","PSDB 12","Cutting of existing concrete paving","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB21","PSDB 13","Breaking out of existing concrete paving and dispose","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB22","8.3.3.3","Compaction in road reserves","m3",{"v":1,"d":"1.00"}]
[]
[null,null,"8.3.4","Overhaul "]
[]
[null,"DB23","8.3.3 (a)","Loimited overhaul (provisional)","m3",{"v":1,"d":"1.00"}]
[null,"DB24","8.3.3 (b)","Long overhaul (provisional)","m³.km",{"v":1,"d":"1.00"}]
[]
[null,"DB25","PSDA 3","Excavate by hand","m3",{"v":1,"d":"1.00"}]
[]
[null,null,"8.3.4","Particular items"]
[]
[null,"DB26",null,"a) Shore trench opposite structure","m",{"v":1,"d":"1.00"}]
[]
[null,null,"8.3.5","EXISTING SERVICES"]
[]
[null,"DB27","8.3.5.1","Services that intersect a trench including exposing by"]
[{"$nulls":3},"hand excavation","No",{"v":1,"d":"1.00"}]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 4"]
[]
[null,"SABS 1200 DA, DB, PSDA & PSDB - EARTHWORKS (PIPE TRENCH)"]
[null,"ITEM NO","PAYMENT REFERS"," DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"DB28","8.3.5.2","Services that adjoin a trench","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.3.6","FINISHING"]
[]
[null,null,"8.3.6.1","Reinstate road surfaces complete with all courses"]
[]
[null,"DB29",null,"a) Gravel roads","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB30",null,"b) 25mm Asphalt","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB31",null,"c) Double seal","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[null,"DB32",null,"d) Cement  stabilization (2%)  of backfill under roads","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"PSDA 3"," ",{"$nulls":3},{"v":0,"d":"0.00"}]
[]
[null,null,"8.3.4","Particular items"]
[]
[null,"DB33",null,"a) Shore trench opposite structure","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Temporary Works: Control water inflow in various pipelines:"]
[]
[{"$nulls":3},"(a)  For new tie-in connections to  existing pipelines and"]
[{"$nulls":3},"relocation of pipes (liase with authority and   close valves):"]
[]
[null,"DB34",null,"(i)   100 mm dia to 500mm dia uPVC pipe","Prov. Sum",{"v":1,"d":"1.00"},{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[null,"DB35",null,"(ii)   500 mm dia to 1000mm dia uPVC pipe","Prov. Sum",{"v":1,"d":"1.00"},{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[null,"DB36",null,"(iii)   1000 mm dia to 1500mm dia uPVC pipe","Prov. Sum",{"v":1,"d":"1.00"},{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[null,"DB37",null,"(iv)   1500 mm dia to 2000mm dia uPVC pipe","Prov. Sum",{"v":1,"d":"1.00"},{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[null,"DB38",null,"(v)   2000 mm dia to 3000mm dia uPVC pipe","Prov. Sum",{"v":1,"d":"1.00"},{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[]
[null,"DB39",null,"(vi) Percentage markup on item (i) to (v) above  for handling,","%",{"v":50000,"d":"50,000"}]
[{"$nulls":3},"     transportation and installation"]
[]
[null,null,"PSDB 14","Reinstate paving with stored paving"]
[]
[null,"DB40",null,"a) Half clay brick","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB41",null,"b) Full clay brick","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB42",null,"c) Interlocking concrete block paving","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"PSDB 16","Reinstate concrete (Class 20 Mpa) paving up to"]
[{"$nulls":3},"100mm thick"]
[]
[null,"DB43",null,"a) Wood float finish","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB44",null,"b) Steel float finish","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB45",null,"c) Imprint finish (any pattern)","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB46","PSDB 16","Extra over 3.13 for colouring concrete paving to"]
[{"$nulls":3},"original colour","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"PSDB 15","Extra over item 3.12 for supplying paving only where "]
[{"$nulls":3},"original paving blocks has broken"]
[]
[null,"DB47",null,"a) Clay bricks","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"b) Interlocking concrete bricks"]
[]
[null,"DB48",null,"(i) 60mm thick","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB49",null,"(ii) 80mm thick","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB50","PSDB 17","Reinstate green grass to the required standard ","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 4"]
[]
[null,"SANS 1200 DA, DB, PSDA & PSDB - EARTHWORKS (PIPE TRENCH)"]
[null,"ITEM NO","PAYMENT REFERS"," DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,null,"SANS 1200","Provision of bedding material from trench excavation"]
[null,null,"LB"]
[null,"DB50","8.2.1","a) Selected granular material","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB51",null,"b) Selected fill material","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Provision of bedding material from commercial sources"]
[]
[null,"DB52",null,"a) Selected granular material","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB53",null,"b) Selected fill material","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DB54",null,"c) Crushed stone","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
{"$rows_empty":49}
[null,"CARRIED FORWARD TO SUMMARY",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[]
[null,"SCHEDULE 5"]
[null,"SANS 1200 DK - GABIONS AND PITCHING"]
[null,"ITEM","REFE-","DESCRIPTION","UNIT","QUANT","RATE","AMOUNT"]
[null,"NO.","RENCE",{"$nulls":3},"R      C","R      C"]
[]
[null,"DK","SABS","  GABIONS"]
[null,null,"1200DK"]
[]
[null,"DK 1","8.2.1(a)","  Surface preparation for bedding of gabions"]
[{"$nulls":3},"  and mattresses","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DK 2","8.2.2","  Supply and install 2m long x 1m wide"]
[{"$nulls":3},"  x 1m height, with 80 x 100 Mesh type"]
[{"$nulls":3},"  and 3,0mm ø wire, galvanised to SANS 675"]
[{"$nulls":3},"  Class A, Gabions, filled with stone as per"]
[{"$nulls":3},"  SABS 1200DK","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DK 3","8.2.2","  Supply and install 2m long x 1m wide x 0,3m "]
[{"$nulls":3},"  height, with 80 x 100 mesh type and 2,5mm "]
[{"$nulls":3},"  dia.  Wire, galvanised to SANS 675 Class A, "]
[{"$nulls":3},"  Reno Mattresses filled with stone as per "]
[{"$nulls":3},"  SABS 1200DK","m³",{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"DK 4","8.2.4","  Geotextile"]
[{"$nulls":3},"  Supply and installation of U24 "]
[{"$nulls":3},"  geotextile between the face contact of gabions"]
[{"$nulls":3},"  or mattresses and fill material","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Pitching",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[{"$nulls":7},{"v":0,"d":"R 0.00"}]
[{"$nulls":3},"Grouted Pitching for:","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"R 0.00"}]
[{"$nulls":7},{"v":0,"d":"R 0.00"}]
[{"$nulls":3},"Stormwater V-Drain","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"DK 5","8.2.5","Pitsching","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"R 0.00"}]
[{"$nulls":7},{"v":0,"d":"R 0.00"}]
[null,"DK 6","8.2.6","Backing for Pitching","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"R 0.00"}]
[]
[null,"DK 7","8.2.7","Weepholes","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"R 0.00"}]
{"$rows_empty":22}
[null,"CARRIED FORWARD TO SUMMARY",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 6 "]
[null," "]
[null,"SANS 1200 GA - CONCRETE  (Small Works)"]
[null,"ITEM","REFE-","DESCRIPTION","UNIT","QUANT","RATE","AMOUNT"]
[null,"NO.","RENCE",{"$nulls":3},"R      C","R      C"]
[]
[null,"GA","SABS","CONCRETE  :  SMALL WORKS"]
[null,null,"1200GA"]
[null,null,"8.2.2","Formwork "]
[null,"GA1",null,"Rough","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"GA2",null,"Normal","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"GA3",null,"Special","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.4","REINFORCEMENT"]
[null,null,"(a)","Mild Steel Bars"]
[]
[null,"GA4",null,"i) 10mm","t",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"High - tensile steel bars"]
[]
[null,"GA5",null,"(i) 10mm","t",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"GA6",null,"(ii) 12mm","t",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.5","CONCRETE"]
[null,"GA7","(a)","Blinding layer in 15Mpa concrete up to a thickness of 75mm","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"GA8","(b)","Strength concrete : 25 Mpa/19mm to:"]
[]
[null,"GA9",null,"Floor slabs","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"GA10",null,"Walls","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"GA11",null,"Roof Slabs","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Pipeline"]
[null,null,"8.1.4.1","Pipe Encasement"]
[]
[null,"GS12",null,"25MPa concrete bedding and encasing to all diameter of","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3}," pipes,  including shuttering and blinding.  Excavation, "]
[{"$nulls":3},"stramps and reinforcing elsewhere"]
[]
[null,"GA13",null,"20MPa concrete bedding and encasing to all diameter of","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3}," pipes,  including shuttering and blinding.  Excavation, "]
[{"$nulls":3},"stramps and reinforcing elsewhere"]
[]
[null,"GA14","8.4.3","Mass Concrete"]
[{"$nulls":3},"15MPa concrete to thrust blocks and the like, including ","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"shuttering.  Excavation measured elsewhere."]
{"$rows_empty":39}
[null,"CARRIED FORWARD TO SUMMARY",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 7"]
[]
[null,"SANS 1200G - REINFORCED CONCRETE"]
[null,"ITEM","REFE-","DESCRIPTION","UNIT","QUANT","RATE","AMOUNT"]
[null,"NO.","RENCE",{"$nulls":3},"R      C","R      C"]
[null,"G","SABS","REINFORCED CONCRETE"]
[null,null,"1200G"]
[null,null,8.2,"FORM WORK"]
[]
[null,"G1",8.1,"Rough Formwork"]
[{"$nulls":3},"To sides of wall foundations not exceeding 400mm high","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.2","Smooth Formwork"]
[null,"G2",null,"To soffit of roof slab","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G3",null,"External faces of walls","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G4",null,"Internal faces of walls","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G5",null,"External faces of roof slab","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"G6","8.2.5","Narrow widths up to 300mm wide in:"]
[{"$nulls":3},"Sides of access manholes","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.4","Box out openings in walls and allow for casting in once "]
[{"$nulls":3},"positioning is complete."]
[]
[{"$nulls":3},"For pipes:"]
[null,"G7",null,"700mm dia steel pipe","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G8",null,"600mm dia steel pipe","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G9",null,"500mm dia steel pipe","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G10",null,"450mm dia steel pipe","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G11",null,"400mm dia steel pipe","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G12",null,"350mm dia steel pipe","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G13",null,"300mm dia steel pipe","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G14",null,"250mm dia steel pipe","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G15",null,"200mm dia steel pipe","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G16",null,"150mm dia steel pipe","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G17",null,"100mm dia steel pipe","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,8.3,"REINFORCEMENT"]
[null,null,"8.3.1","Mild Steel Bars"]
[]
[null,"G18",null,"a) 10mm","t",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"High - tensile steel bars"]
[]
[null,"G19",null,"10mm","t",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G20",null,"12mm","t",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G21",null,"16mm","t",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G22",null,"20mm","t",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,8.4,"CONCRETE"]
[null,"G22","8.4.2","Blinding layer in 15Mpa concrete up to a thickness of 75mm","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"G23","8.4.3","Strength concrete : 25 Mpa/19mm to:"]
[]
[null,"G24",null,"Floor slabs","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G25",null,"Walls","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"G26",null,"Roof Slabs","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 7"]
[]
[null,"SANS 1200G - REINFORCED CONCRETE"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Strength Concrete : 30MPa/19mm to:"]
[{"$nulls":3},"Floors slabs","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"Walls","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"Roof slabs","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Manhole Cover and Frame "]
[null,"G27",null,"Supply and cast in concrete roof slab, manhole cover and ","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"frame complete with locking device as per attached drawings"]
[{"$nulls":3},"AC 345/19/SD12"]
[]
[null,"G28",null,"Ventilators on roof slabs",{"$nulls":3},{"v":0,"d":"0.00"}]
[{"$nulls":3},"Supply and cast in concrete roof slab inlet and outlet ","No",{"v":1,"d":"1.00"}]
[{"$nulls":3},"vendilator as indicated as per attached drawings AC345/19/SD01"]
[]
[null,"G29",null,"Access Ladders",{"$nulls":3},{"v":0,"d":"0.00"}]
[{"$nulls":3},"Supply and install submerged GMS to Class A ladder or similar "]
[{"$nulls":3},"fixed to chamber walls as per attached drawings AC345/19/SD16","No",{"v":1,"d":"1.00"}]
{"$rows_empty":46}
[null,"CARRIED FORWARD TO SUMMARY",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"L","SABS ","SECTION L:  MEDIUM - PRESSURE PIPELINES"]
[null,null,"1200L"]
[]
[null,null,"8.2.1","Supply, lay and bed pipes complete with couplings and fittings"]
[]
[null,null,"8.2.1.a","PVC-U spigot and socket pipe with integral socket and locked-in "]
[{"$nulls":3},"rubber ring seal"]
[]
[{"$nulls":3},"Class 12 with nominal size of:"]
[]
[null,"L1",null,"(i) 110mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L2",null,"(ii) 125mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L3",null,"(iii) 140mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L4",null,"(iv) 160mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L5",null,"(v) 200mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L6",null,"(vi) 250mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L7",null,"(vii) 315mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L8",null,"(viii) 355mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L9",null,"(ix) 400mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L10",null,"(x) 450mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L11",null,"(xi) 500mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L12",null,"Class 16 with nominal size of:"]
[]
[null,"L13",null,"(i) 110mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L14",null,"(ii) 125mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":5},{"v":1,"d":"1.00"}]
[null,"L15",null,"(iii) 140mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L16",null,"(iv) 160mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L17",null,"(v) 200mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L18",null,"(vi) 250mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L19",null,"(vii) 315mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L20",null,"(viii) 355mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L21",null,"(ix) 400mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L22",null,"(x) 450mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L23",null,"(xi) 500mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.1.b","Class 12.50 HDPE Pipe  PE 100 to be Butt-Welded with "]
[{"$nulls":3},"Nominal Size:"]
[]
[null,"L24",null,"(i) 160mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L25",null,"(ii) 180mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L26",null,"(iii) 200mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L26",null,"(iv) 225mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L27",null,"(v) 250mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L28",null,"(vi) 280mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L29",null,"(vii) 315mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L30",null,"(viii) 355mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L31",null,"(ix) 400mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L32",null,"(x) 450mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L33",null,"(xi) 500mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L34",null,"(xii) 560mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L35",null,"(xiii) 630mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L36",null,"(xiii) 710mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L34",null,"(xii) 800mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L35",null,"(xiii) 900mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L36",null,"(xiii) 1000mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[null,null,"8.2.1.b","Class 16 HDPE Pipe  PE 100 to be Butt-Welded with "]
[{"$nulls":3},"Nominal Size:"]
[]
[null,"L37",null,"(i) 160mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L38",null,"(ii) 180mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L39",null,"(iii) 200mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L40",null,"(iv) 225mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L41",null,"(v) 250mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L42",null,"(vi) 280mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L43",null,"(vii) 315mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"L44",null,"(viii) 355mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L45",null,"(ix) 400mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L46",null,"(x) 450mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L47",null,"(xi) 500mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L48",null,"(xii) 560mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L49",null,"(xiii) 630mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L50",null,"(xiii) 710mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L51",null,"(xii) 800mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L52",null,"(xiii) 900mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L53",null,"(xiii) 1000mm","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[null,null,"8.2.4.a","Steel Flanges complete to SABS 1123:1977 with all fasteners, "]
[{"$nulls":3},"gaskets and appurtenances.  (Painted as above for corrosion "]
[{"$nulls":3},"protection). (1600/3)"]
[]
[null,"L54",null,"DN100","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L55",null,"DN 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L56",null,"DN 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L57",null,"DN 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L58",null,"DN 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L59",null,"DN 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L60",null,"DN 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L61",null,"DN 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L62",null,"DN 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L63",null,"DN 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L64",null,"DN 600mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L65",null,"DN 700mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L66",null,"DN 100mm Blank flange","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L67",null,"DN 125mm Blank flange","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L68",null,"DN 150mm Blank flange","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L69",null,"DN 200mm Blank flange","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L70",null,"DN 250mm Blank flange","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L71",null,"DN 300mm Blank flange","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L72",null,"DN 350mm Blank flange","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L73",null,"DN 400mm Blank flange","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L74",null,"DN 450mm Blank flange","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,"L75",null,"DN 500mm Blank flange","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L76",null,"DN 600mm Blank flange","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L77",null,"DN 700mm Blank flange","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4a for other types and sizes of flanges"]
[]
[null,"L78",null,"(i) Provisional sum",null,"Provisional",{"v":10000,"d":"10,000.00"},{"v":10000,"d":"10,000.00"}]
[]
[null,"L79",null,"(ii) Percentage markup on item (i) above  for handling,","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     transportation and installation"]
[]
[null,null,"8.2.4b","Viking Johnson Type ('MaxiFit') Flange Adaptors: PN16 to SANS "]
[{"$nulls":3},"1123  (1600/3) to fit pipe, step pipe and adapt to different "]
[{"$nulls":3},"types of material (VJ 'MaxiFit') or similar approved"]
[]
[null,"L80",null,"DN100","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L81",null,"DN 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L82",null,"DN 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L83",null,"DN 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L84",null,"DN 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L85",null,"DN 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L86",null,"DN 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L87",null,"DN 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L88",null,"DN 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L89",null,"DN 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L90",null,"DN 600mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L91",null,"DN 700mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L92",null,"DN 100mm Restrained","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L93",null,"DN 125mm Restrained","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L94",null,"DN 150mm Restrained","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L95",null,"DN 200mm Restrained","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L96",null,"DN 250mm Restrained","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"L97",null,"DN 300mm Restrained","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L98",null,"DN 350mm Restrained","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L99",null,"DN 400mm Restrained","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L100",null,"DN 450mm Restrained","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L101",null,"DN 500mm Restrained","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L102",null,"DN 600mm Restrained","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L103",null,"DN 700mm Restrained","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4b for other types and sizes of flange adaptors"]
[]
[null,"L104",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L105",null,"(ii) Contractors markup on item (i) above for handling,","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     transportation and installation"]
[{"$nulls":3},"      "]
[null,null,"8.2.4c","Hydrant Tee:  C.I. Flanged to SANS 1123 (1600/3), complete with"]
[{"$nulls":3},"all fasteners, gaskets & appurtenances"]
[]
[null,"L106",null,"ND 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L107",null,"ND 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L108",null,"ND 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L109",null,"ND 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L110",null,"ND 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L111",null,"ND 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L112",null,"ND 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L113",null,"ND 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L114",null,"ND 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4c for other types and sizes of hydrant tees"]
[]
[null,"L115",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L116",null,"(ii) Contractors markup on item (i) above ","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     for handling,transportation and  installation"]
[{"$nulls":3},"     "]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,null,"8.2.4d","Scour Tee:  C.I. Flanged to SABS 1123 (1600/3), complete with "]
[{"$nulls":3},"all fasteners, gaskets & appurtenances"]
[]
[null,"L117",null,"ND 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L118",null,"ND 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L119",null,"ND 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L120",null,"ND 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L121",null,"ND 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L122",null,"ND 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L123",null,"ND 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L124",null,"ND 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L125",null,"ND 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L126",null,"ND 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L127",null,"ND 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L128",null,"ND 600mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L129",null,"ND 700mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4d for other types and sizes of scour tees"]
[]
[null,"L130",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L131",null,"(ii) Contractors markup on item (i) above for handling,transportation","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"    and  installation"]
[{"$nulls":3},"     "]
[null,null,"8.2.4e","Equal Tee:  C.I. Flanged to SABS 1123 (1600/3) complete with all "]
[{"$nulls":3},"fasteners, gaskets & appurtenances"]
[]
[null,"L132",null,"ND 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L133",null,"ND 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L134",null,"ND 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L135",null,"ND 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L136",null,"ND 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L137",null,"ND 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,"L138",null,"ND 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L139",null,"ND 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L140",null,"ND 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Equal Tee:  Spigot and socket complete with all appurtenances"]
[]
[null,"L141",null,"ND 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L142",null,"ND 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L143",null,"ND 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L144",null,"ND 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L145",null,"ND 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L146",null,"ND 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L147",null,"ND 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L148",null,"ND 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L149",null,"ND 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L150",null,"ND 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4e for other types and sizes of equal tees"]
[]
[null,"L151",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L152",null,"(ii) Contractors markup on item (i) above for handling,transportation","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     and installation"]
[]
[null,null,"8.2.4f","Reducing Tee:  C.I Spigot and socket (PN16) complete with all "]
[{"$nulls":3},"appurtenances with ND:"]
[]
[null,"L153",null,"125mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L154",null,"140mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L155",null,"140mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L156",null,"160mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L157",null,"160mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L158",null,"160mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"L160",null,"200mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L161",null,"200mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L162",null,"200mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L163",null,"200mm x 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L164",null,"250mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L165",null,"250mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L166",null,"250mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L167",null,"250mm x 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L168",null,"250mm x 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Reducing Tee:  C.I. Flanged to SANS 1123 (1600/3) complete"]
[{"$nulls":3}," with all fasteners, gaskets & appurtenances with ND:"]
[]
[null,"L169",null,"125mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L170",null,"140mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L171",null,"140mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L172",null,"160mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L173",null,"160mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L174",null,"160mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L175",null,"200mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L176",null,"200mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L177",null,"200mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L178",null,"200mm x 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L179",null,"250mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L180",null,"250mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L181",null,"250mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L182",null,"250mm x 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L183",null,"250mm x 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[{"$nulls":3},"Extra-over item 8.2.4f for other types and sizes of reducing tees"]
[]
[null,"L184",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L185",null,"(ii) Percentage markup on item (i) above  for handling, ","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     transportation and  installation"]
[{"$nulls":3},"     "]
[null,null,"8.2.4g","Reducers:  C.I.Spigot and socket (PN16) complete with all "]
[{"$nulls":3},"appurtenances with ND:"]
[]
[null,"L186",null,"125mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L187",null,"140mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L188",null,"140mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L189",null,"160mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L190",null,"160mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L191",null,"160mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L192",null,"200mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L193",null,"200mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L194",null,"200mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L195",null,"200mm x 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L196",null,"250mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L197",null,"250mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L198",null,"250mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L199",null,"250mm x 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L200",null,"250mm x 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L201",null,"315mm x 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L203",null,"Reducers:  C.I. Flanged to SANS 1123 (1600/3) complete with all "]
[{"$nulls":3},"fasteners, gaskets & appurtenances with ND:"]
[]
[null,"L204",null,"125mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L205",null,"140mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L206",null,"140mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
{"$rows_empty":18}
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"L207",null,"160mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L208",null,"160mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L209",null,"160mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L210",null,"200mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L211",null,"200mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L212",null,"200mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L213",null,"200mm x 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L214",null,"250mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L215",null,"250mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L216",null,"250mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L217",null,"250mm x 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L218",null,"250mm x 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L219",null,"700mm x 600mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L220",null,"250mm x 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4g for other types and sizes of reducers"]
[]
[null,"L221",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L222",null,"(ii) Contractors markup on item (i) above  for handling,transportation","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     and  installation"]
[{"$nulls":3},"     "]
[null,null,"8.2.4h","Flange adaptors:  C.I flange drilled to SANS 1123 (1600/3) with nominal "]
[{"$nulls":3},"size:"]
[]
[null,"L223",null,"(i) 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L224",null,"(ii) 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L225",null,"(iii) 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L226",null,"(iv) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L227",null,"(v) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L228",null,"(vi) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,null,"8.2.4h","Flange adaptors:  C.I flange drilled to SANS 1123 (1600/3) with nominal "]
[{"$nulls":3},"size:"]
[]
[null,"L229",null,"(i) 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L230",null,"(ii) 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L231",null,"(iii) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L232",null,"(iv) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4h for other types and sizes of flange adaptors"]
[]
[null,"L233",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L234",null,"(ii) Contractors markup on item (i) above for handling,","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     transportation and installation"]
[]
[null,null,"8.2.4i","Bends - uPVC class 16"]
[]
[{"$nulls":3},"(a) 90° Bend with OD:"]
[]
[null,"L235",null,"      (i) 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.4i","Bends - uPVC class 16"]
[]
[{"$nulls":3},"(a) 90° Bend with OD:"]
[]
[null,"L236",null,"      (i) 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L237",null,"      (ii) 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L238",null,"      (iii) 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L239",null,"      (iv) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L240",null,"      (v) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L241",null,"      (vi) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L242",null,"      (vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(b) 45° Bend with OD:"]
[]
[null,"L243",null,"      (i) 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L244",null,"      (ii) 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L245",null,"      (iii) 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,"L246",null,"      (iv) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L247",null,"      (v) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L248",null,"      (vi) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L249",null,"      (vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(c) 22.5° Bend with OD:"]
[]
[null,"L250",null,"      (i) 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L251",null,"      (ii) 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L252",null,"      (iii) 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L253",null,"      (iv) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L254",null,"      (v) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L255",null,"      (vi) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L256",null,"      (vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(d) 11.25° Bend with OD:"]
[]
[null,"L257",null,"      (i) 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L258",null,"      (ii) 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L259",null,"      (iii) 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L260",null,"      (iv) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L261",null,"      (v) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L262",null,"      (vi) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L263",null,"      (vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4i for other types and sizes of bends"]
[]
[null,"L264",null,"(i) Provisional Sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L265",null,"(ii) Copntractors markup on item (i) above ","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"      for handling, transportation and "]
[{"$nulls":3},"      installation"]
[]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,null,"8.2.4j","Bends - Steel (drilled to SANS 1123 Table 1600/3, both ends flanged)"]
[]
[{"$nulls":3},"(a) 90° Bend with ND:"]
[]
[null,"L266",null,"      (i) 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L267",null,"      (ii) 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L268",null,"      (iii) 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L269",null,"      (iv) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L270",null,"      (v) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L271",null,"      (vi) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L272",null,"      (vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L273",null,"      (viii) 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L274",null,"      (ix) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L275",null,"      (x) 450mm","No.",{"v":4,"d":"4.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L276",null,"      (xi) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(b) 45° Bend with ND:"]
[]
[null,"L267",null,"      (i) 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L268",null,"      (ii) 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L269",null,"      (iii) 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L270",null,"      (iv) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L271",null,"      (v) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L272",null,"      (vi) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L273",null,"      (vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L274",null,"      (viii) 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L275",null,"      (ix) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L276",null,"      (x) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L277",null,"      (xi) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[{"$nulls":3},"(c) 22.5° Bend with ND:"]
[]
[null,"L278",null,"      (i) 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L279",null,"      (ii) 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L280",null,"      (iii) 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L281",null,"      (v) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L282",null,"      (vi) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L283",null,"      (vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L284",null,"      (viii) 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L285",null,"      (ix) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L286",null,"      (x) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L287",null,"      (xi) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(d) 11.25° Bend with ND:"]
[]
[null,"L288",null,"      (i) 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L289",null,"      (ii) 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L290",null,"      (iii) 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L291",null,"      (iv) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L292",null,"      (v) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L293",null,"      (vi) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L294",null,"      (vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L295",null,"      (viii) 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L296",null,"      (ix) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L297",null,"      (x) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L298",null,"      (xi) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
{"$rows_empty":8}
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,null,"8.2.4K","Bends - Steel (drilled to SANS 1123 Table 2500/3, both ends "]
[{"$nulls":3},"flanged)"]
[]
[{"$nulls":3},"(a) 90 Bend with ND:"]
[null,"L299",null,"      (ii) 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L300",null,"      (iii) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L301",null,"      (iv) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L302",null,"      (v) 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L303",null,"      (vi) 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L304",null,"      (vii) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L305",null,"      (viii) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L306",null,"      (ix) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L307",null,"      (x) 600mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L308",null,"      (xi) 700mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(b) 45 Bend with ND:"]
[]
[null,"L309",null,"      (ii) 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L310",null,"      (iii) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L311",null,"      (iv) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L312",null,"      (v) 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L313",null,"      (vi) 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L314",null,"      (vii) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L315",null,"      (viii) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L316",null,"      (ix) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L317",null,"      (x) 600mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L318",null,"      (xi) 700mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
{"$rows_empty":7}
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[{"$nulls":3},"(c) 22.5 Bend with ND:"]
[]
[null,"L319",null,"      (ii) 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L320",null,"      (iii) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L321",null,"      (iv) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L322",null,"      (v) 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L323",null,"      (vi) 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L324",null,"      (vii) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L325",null,"      (viii) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L326",null,"      (ix) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L327",null,"      (x) 600mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L328",null,"      (xi) 700mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(d) 11.25 Bend with ND:"]
[]
[null,"L329",null,"      (ii) 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L330",null,"      (iii) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L331",null,"      (iv) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L332",null,"      (v) 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L333",null,"      (vi) 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L334",null,"      (vii) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L335",null,"      (viii) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L337",null,"      (ix) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L338",null,"      (x) 600mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L339",null,"      (xi) 700mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4k for other types and sizes of bends"]
[]
[null,"L340",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L341",null,"(ii) Contractors markup on item (i) above  for handling,","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     transportation and  installation"]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,null,"8.2.4k","Steel End Caps with ND:"]
[]
[null,"L342",null,"110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L343",null,"160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L344",null,"200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L345",null,"250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L346",null,"315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L347",null,"355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L348",null,"400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4ℓ for other types and sizes of end caps"]
[]
[null,"L349",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L350",null,"(ii) Contractors markup on item (i) above  for handling, ","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     transportation and installation"]
[]
[null,null,"8.2.4m","Saddle Clamp Complete with bolts, nuts, flat gaskets, stiffened ring.  "]
[{"$nulls":3},"Include drilling hole to DN of fitting Ø. Suitable Polypropylene "]
[{"$nulls":3},"Copolymer Compression fittings and specials for coupling of "]
[{"$nulls":3},"HDPE pipes: BSP Include for painting bolts with bituminous "]
[{"$nulls":3},"corrosion resisting paint :"]
[]
[null,"L351",null,"110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L352",null,"125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L353",null,"160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L354",null,"200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4m for other types and sizes of saddles"]
[]
[null,"L355",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L356",null,"(ii) Contractors markup on item (i) above   for handling, ","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"    transportation and  installation"]
[]
[null,null,"8.2.4n","Steel Repair couplings with ND:"]
[]
[null,"L358",null,"110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L359",null,"160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"L360",null,"200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L361",null,"250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L362",null,"315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L363",null,"355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L364",null,"450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L365",null,"500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4n for other types and sizes of repair couplings"]
[]
[null,"L366",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[null,"L367",null,"(ii) Contractors markup on item (i) above  for handling,","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     transportation and installation"]
[]
[null,null,"8.2.4O","HDPE specials, fittings and couplings"]
[]
[{"$nulls":3},"(a) HDPE Segmented bends 90°with  nominal Size:"]
[{"$nulls":3},"     "]
[null,"L368",null,"(i) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L369",null,"(ii) 180mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L370",null,"(iii) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L371",null,"(iv) 225mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L372",null,"(v) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L373",null,"(vi) 280mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L374",null,"(vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L375",null,"(viii) 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(ix) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L376",null,"(x) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L377",null,"(xi) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(b) HDPE Segmented bends 45° with nominal size:"]
[]
[null,"L378",null,"(i) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"L379",null,"(ii) 180mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L380",null,"(iii) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L3381",null,"(iv) 225mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L382",null,"(v) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L383",null,"(vi) 280mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L384",null,"(vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L385",null,"(viii) 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L386",null,"(ix) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L387",null,"(x) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L388",null,"(xi) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(c) HDPE Seamless bends 90° with  nominal size"]
[{"$nulls":3},"     "]
[null,"L389",null,"(i) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L390",null,"(ii) 180mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L391",null,"(iii) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L392",null,"(iv) 225mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L393",null,"(v) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[null,"L394",null,"(iv) 225mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L395",null,"(v) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L396",null,"(vi) 280mm","No.",{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L397",null,"(vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L398",null,"(viii) 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L400",null,"(ix) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L401",null,"(x) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L402",null,"(xi) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[{"$nulls":3},"(c) HDPE Seamless bends 90° with  nominal size"]
[{"$nulls":3},"     "]
[null,"L403",null,"(i) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L404",null,"(ii) 180mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L405",null,"(iii) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L406",null,"(iv) 225mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L407",null,"(v) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L408",null,"(vi) 280mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L409",null,"(vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L410",null,"(viii) 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L411",null,"(ix) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L412",null,"(x) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L413",null,"(xi) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(d) HDPE Seamless bends 45° with nominal size"]
[]
[null,"L414",null,"(i) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L415",null,"(ii) 180mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L416",null,"(iii) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L417",null,"(iv) 225mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L418",null,"(v) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L419",null,"(vi) 280mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L420",null,"(vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L421",null,"(viii) 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L422",null,"(ix) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L423",null,"(x) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L424",null,"(xi) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L425",null,"Extra-over item 8.2.4o (a,b,c,d) for other types and sizes of bends"]
[]
[null,"L426",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,"L427",null,"(ii) Contractors markup on item (i) above for handling,","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     transportation and installation"]
[]
[{"$nulls":3},"(e) HDPE Tees with nominal size:"]
[]
[null,"L428",null,"(i) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L429",null,"(ii) 180mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L430",null,"(iii) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L431",null,"(iv) 225mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L432",null,"(v) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L434",null,"(vi) 280mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L435",null,"(vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L436",null,"(viii) 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L437",null,"(ix) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L438",null,"(x) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L439",null,"(xi) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4n (e) for other types and sizes of tees"]
[]
[null,"L440",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L441",null,"(ii) Contractors markup on item (i) above  for handling,","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"    transportation and installation"]
[{"$nulls":3},"      "]
[{"$nulls":3},"(f) HDPE reducing tees with nominal size:"]
[{"$nulls":3},"      "]
[null,"L442",null,"125mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L443",null,"140mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L444",null,"140mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L445",null,"160mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L446",null,"160mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L447",null,"160mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L448",null,"200mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L449",null,"200mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"L450",null,"200mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L451",null,"200mm x 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L452",null,"250mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L453",null,"250mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L454",null,"250mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L455",null,"250mm x 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L456",null,"250mm x 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4n (f) for other types and sizes of reducing tees"]
[]
[null,"L457",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L458",null,"(ii) Contractors markup on item (i) above   for handling, ","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"    transportation and  installation"]
[]
[{"$nulls":3},"(g) HDPE stub flange  with nominal size:"]
[]
[null,"L459",null,"(i) 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L460",null,"(ii) 180mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L461",null,"(iii) 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L462",null,"(iv) 225mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L463",null,"(v) 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L464",null,"(vi) 280mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L465",null,"(vii) 315mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[null,"L466",null,"(viii) 355mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L467",null,"(ix) 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L468",null,"(x) 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L469",null,"(xi) 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"Extra-over item 8.2.4n (g) for other types and sizes of tees"]
[]
[null,"L470",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"L471",null,"(ii) Contractors markup on item (i) above for handling, ","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     transportation and  installation"]
[{"$nulls":3},"     "]
[{"$nulls":3},"(h) HDPE Reducers with nominal size:"]
[]
[null,"L472",null,"125mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L473",null,"140mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L474",null,"140mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L475",null,"160mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L476",null,"160mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L477",null,"160mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L478",null,"200mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L479",null,"200mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L480",null,"200mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L481",null,"200mm x 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L482",null,"250mm x 110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L483",null,"250mm x 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L484",null,"250mm x 140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L485",null,"250mm x 160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L486",null,"250mm x 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L487",null,"Extra-over item 8.2.4n (h) for other types and sizes of reducers"]
[]
[null,"L488",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L489",null,"(ii) Contractors markup on item (i) above for handling, ","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     transportation and installation"]
[]
[{"$nulls":3},"(i) HDPE end caps with nominal size:"]
[]
[null,"L490",null,"110mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L491",null,"125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L492",null,"140mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L493",null,"160mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"L494",null,"180mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L495",null,"200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L496",null,"225mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4n (i) for other types and sizes of end caps"]
[]
[null,"L497",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L498",null,"(ii) Contractors markup on item (i) above for handling, ","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     transportation and  installation"]
[{"$nulls":3},"   "]
[{"$nulls":3},"(j) Puddle flanges"]
[]
[null,"L499",null,"DN 100mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L500",null,"DN 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L501",null,"DN 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L502",null,"DN 225mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L503",null,"DN 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L504",null,"DN 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L505",null,"DN 375mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L506",null,"DN 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L507",null,"DN 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L508",null,"DN 600mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L509",null,"DN 750mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.4n (j) for other types and sizes of puddle flanges"]
[]
[null,"L510",null,"(i) Provisional Sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L511",null,"(ii) Contractors markup on item (i) above  for handling,","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"    transportation and installation"]
[{"$nulls":3},"    "]
[{"$nulls":3},"Extra-over item 8.2.4 for Ductile Iron fittings and specials"]
[]
[null,"L512",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L513",null,"(ii) Contractors markup on item (i) above for handling, ","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     transportation and installation"]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,null,"8.2.5","Supply and Place Pipes, Valves & Specials"]
[]
[{"$nulls":3},"Supply, Install & Finish installation -Suitable Cast Iron, Mild steel    "]
[{"$nulls":3},"(minimum wall thickness of 4,5mm) & uPVC fittings for coupling onto "]
[{"$nulls":3},"pipes.  Complete with bolts, nuts, gaskets, seals & corrosion protection."]
[{"$nulls":3},"If flanged : drilled to SANS 1123(1600/3) Boss flanges:  Drilled to SANS"]
[{"$nulls":3},"1123(1600/4) If screwed:  BSP thread Bolts:  Stainless steel grade 304"]
[{"$nulls":3},"Pipes to SANS 62"]
[]
[{"$nulls":3},"Corrosion protection:  Powder coated Final surface shall be smooth,  "]
[{"$nulls":3},"glossy and uniform before powder coating, clean the surface - sand blast"]
[{"$nulls":3},"to Sa 3 Cl. 10.2 Primer:  to manufacturer's specification Materials:  "]
[{"$nulls":3},"Powder coating - High build Epoxy (SABS 1217 Type 2): DFT:  300 to "]
[{"$nulls":3},"500 micron - Polyurethane (SABS 1578) on G.I DFT:  50 to 100 micron"]
[]
[{"$nulls":3},"Alternative corrosion protection:  Hot-dipped galvanized to SANS ISO "]
[{"$nulls":3},"1461 and SANS EN 10240."]
[]
[null,null,"8.2.5a","Isolating Valves"]
[]
[{"$nulls":3},"(a) Resilient seal gate valve non-rising spindle with stem cap, flanges"]
[{"$nulls":3},"    drilled to SANS1123 (1600/3) Anti-clockwise closing. "]
[{"$nulls":3},"    Complete with all components and gaskets and "]
[{"$nulls":3},"    appurtenances"]
[{"$nulls":3},"      "]
[null,"L514",null,"(i) DN 80mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L515",null,"(ii) DN 100mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L516",null,"(iii) DN 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L517",null,"(iv) DN 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L518",null,"(v) DN 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L519",null,"(vi) DN 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L520",null,"(vii) DN 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L521",null,"(viii) DN 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(b) Resilient seal gate valve non-rising spindle with stem cap, flanges"]
[{"$nulls":3},"    drilled to SANS1123 (2500/3) Anti-clockwise closing. "]
[{"$nulls":3},"    Complete with all components and gaskets and "]
[{"$nulls":3},"    appurtenances"]
[]
[null,"L522",null,"(i) DN 80mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"L523",null,"(ii) DN 100mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L524",null,"(iii) DN 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L525",null,"(iv) DN 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L526",null,"(v) DN 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L527",null,"(vi) DN 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L528",null,"(vii) DN 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L529",null,"(viii) DN 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L530",null,"(viii) DN 500mm","No.",{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L531",null,"(ix) DN 700mm","No.",{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[{"$nulls":3},"(c) Resilient seal gate valve non-rising spindle with stem  cap, spigot "]
[{"$nulls":3},"    and socket Anti-clockwise closing.  Complete with all appurtenances"]
[{"$nulls":3},"    "]
[]
[null,"L532",null,"(i) DN 80mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L533",null,"(ii) DN 100mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L534",null,"(iii) DN 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L535",null,"(iv) DN 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L536",null,"(v) DN 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L537",null,"(vi) DN 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L538",null,"(c) Wedge gate valve non rising spindle PN 16 rated-hand"]
[{"$nulls":3},"     wheel operated,  anitclockwise closing, epoxy coated "]
[{"$nulls":3},"     Flanges drilled to SANS 1123 (1600/3) complete with "]
[{"$nulls":3},"     all gaskets and appurtenances"]
[{"$nulls":3},"      "]
[null,"L538",null,"(i) DN 80mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L539",null,"(ii) DN 100mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L540",null,"(iii) DN 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L541",null,"(iv) DN 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L542",null,"(v) DN 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"L543",null,"(vi) DN 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L544",null,"(vii) DN 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L545",null,"(viii) DN 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(d) Wedge gate valve non rising spindle PN 16 rated-hand wheel "]
[{"$nulls":3},"    operated, anti-clockwise closing, epoxy coated  "]
[{"$nulls":3},"    Flanges drilled to SANS 1123 (1600/3) complete with all gaskets"]
[{"$nulls":3},"and appurtenances"]
[]
[null,"L546",null,"(i) DN 80mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L547",null,"(ii) DN 100mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L548",null,"(iii) DN 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L549",null,"(iv) DN 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L550",null,"(v) DN 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L551",null,"(vi) DN 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L552",null,"(vii) DN 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L553",null,"(viii) DN 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.5a for other types and sizes of isolating valves"]
[]
[null,"L554",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L555",null,"(ii) Contractors mark-up on item (i) above for handling, transportation ","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"    and installation"]
[]
[null,null,"8.2.5b","Scour valves"]
[]
[{"$nulls":3},"Supply and install complete with all components scour valves, epoxy "]
[{"$nulls":3},"coated, anticlockwise closing PN16 flanged with all components and "]
[{"$nulls":3},"gaskets and appurtenances"]
[]
[null,"L556",null,"(i) DN 80mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L557",null,"(ii) DN 100mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L558",null,"(iii) DN 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L559",null,"(iv) DN 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L560",null,"(v) DN 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L561",null,"(vi) DN 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L562",null,"(iii) DN 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[{"$nulls":3},"Supply and install complete with all components scour valves, epoxy "]
[{"$nulls":3},"coated, anticlockwise closing PN 25 flanged with all components and "]
[{"$nulls":3},"gaskets and appurtenances"]
[]
[null,"L563",null,"(i) DN 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L564",null,"(ii) DN 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L565",null,"(iii) DN 450mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L566",null,"(iv) DN 500mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L567",null,"(v) DN 650mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L568",null,"(vi) DN 700mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.5b for other types and sizes of scour valves"]
[]
[null,"L569",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L570",null,"(ii) Contractors mark-up on item (i) above for handling, transportation "]
[{"$nulls":3},"    and installation","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.5c","Control valves"]
[]
[{"$nulls":3},"(a) Rate of flow control valve CLA-VAL SERIES 40/640 (or similar  "]
[{"$nulls":3},"approved) flanged complete with all components and gaskets and"]
[{"$nulls":3},"     appurtenances"]
[]
[null,"L571",null,"(i) DN 80mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L572",null,"(ii) DN 100mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L573",null,"(iii) DN 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L574",null,"(iv) DN 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L575",null,"(v) DN 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L576",null,"(vi) DN 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L577",null,"(vii) DN 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L578",null,"(viii) DN 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L579",null,"(xv) DN 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[{"$nulls":3},"(b) Pressure sustaining valve CLA-VAL SERIES 50/650"]
[{"$nulls":3},"     (or similar  approved) flanged complete with all "]
[{"$nulls":3},"     components and gaskets and appurtenances"]
[{"$nulls":3},"      "]
[null,"L580",null,"(i) DN 80mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L581",null,"(ii) DN 100mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L582",null,"(iii) DN 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L583",null,"(iv) DN 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L584",null,"(v) DN 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L585",null,"(vi) DN 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L586",null,"(vii) DN 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L587",null,"(viii) DN 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L588",null,"(xv) DN 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(c) Pump control valve CLA-VAL SERIES 60/660 flanged complete"]
[{"$nulls":3},"      with all components and gaskets and appurtenances"]
[{"$nulls":3},"      "]
[null,"L589",null,"(i) DN 80mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L590",null,"(ii) DN 100mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L591",null,"(iii) DN 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L592",null,"(iv) DN 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L593",null,"(v) DN 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L594",null,"(vi) DN 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L595",null,"(vii) DN 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L596",null,"(viii) DN 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L597",null,"(xv) DN 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(d) Pressure Reducing valve CLA-VAL SERIES 90/690"]
[{"$nulls":3},"    (or similar approved) flanged complete with all "]
[{"$nulls":3},"    components and gaskets and appurtenances"]
[]
[null,"L598",null,"(i) DN 80mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L599",null,"(ii) DN 100mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"L600",null,"(iii) DN 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L601",null,"(iv) DN 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L602",null,"(v) DN 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L603",null,"(vi) DN 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L604",null,"(vii) DN 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L605",null,"(viii) DN 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L606",null,"(xv) DN 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"(e) Non Return/Check valve CLA-VAL SERIES 81"]
[{"$nulls":3},"    (or similar approved)  flanged complete with all"]
[{"$nulls":3},"    components and gaskets and  appurtenances"]
[{"$nulls":3},"     "]
[null,"L607",null,"(i) DN 80mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L608",null,"(ii) DN 100mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L609",null,"(iii) DN 125mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L610",null,"(iv) DN 150mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L611",null,"(v) DN 200mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L612",null,"(vi) DN 250mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L613",null,"(vii) DN 300mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L614",null,"(viii) DN 350mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L615",null,"(xv) DN 400mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.5c for other types and sizes of Control Valves"]
[]
[null,"L616",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L617",null,"(ii) Contractors markup on item (i) above  for handling, ","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     transportation and  installation"]
[]
[null,null,"8.2.5d","Air Valves"]
{"$rows_empty":8}
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[{"$nulls":3},"Air and vacuum break valve, Vent-o-Mat Series RBX or similar approved "]
[{"$nulls":3},"complete with mounting flange gaskets and bolts and nuts and "]
[{"$nulls":3},"appurtenances"]
[]
[null,"L618",null,"ND 25 (2511) - Screwed","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L619",null,"ND 50 (2511) - Screwed","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L620",null,"ND 80 (1601) - Flanged","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L621",null,"ND 80 (2501) - Flanged","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L622",null,"ND 100 (1601) - Flanged","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L623",null,"ND 100 (2501) - Flanged","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L624",null,"ND 150 (1601) - Flanged","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L625",null,"ND 150 (2501) - Flanged","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L626",null,"ND 200 (1601) - Flanged","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L627",null,"ND 200 (2501) - Flanged","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.5d for other types and sizes of Air Valves"]
[]
[null,"L628",null,"(i) Provisional Sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L629",null,"(ii) Contractors markup on item (i) above ","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"      for handling, transportation and "]
[{"$nulls":3},"      installation"]
[]
[null,null,"8.2.5e","Fire Hydrant Valves"]
[]
[{"$nulls":3},"Supply and install complete with all components and gaskets and "]
[{"$nulls":3},"appurtenances"]
[]
[null,"L630",null,"(i) Below ground level type","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L631",null,"(ii) Above ground level type","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.5e for other types and sizes of fire hydrant valves"]
[]
[null,"L632",null,"(i) Provisional sum",null,"Provisional","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L633",null,"(ii) Contractors markup on item (i) above for handling, transportation","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     and installation"]
[{"$nulls":3},"      "]
[]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,null,"8.2.5f","Manzi Lock"]
[]
[null,"L634",null,"Supply and install complete to fit onto Resilient Seal Gate Valve stem ","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"cap"]
[]
[null,null,"8.2.5g","Pressure Gauge"]
[]
[{"$nulls":3},"Supply and install complete to it onto G.I pipe complete with couplers "]
[{"$nulls":3},"and fasteners and appurtenances"]
[]
[null,"L635",null,"Pressure Gauge: DN15mm","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Extra-over item 8.2.5g for other types and sizes of pressure gauges"]
[]
[null,"L636",null,"(i) Provisional sum","_","Provisional ","Sum",{"v":10000,"d":"10,000.00"}]
[]
[null,"L637",null,"(ii) Contractors markup on item (i) above for handling, ","%",{"v":10000,"d":"10,000.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"     transportation and  installation "]
[{"$nulls":3},"     "]
[null,null,"8.2.5h","Fire Hydrant Fittings: above ground level"]
[]
[null,"L638",null,"Complete as per Drawing No. AC345/19/FD01","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.5i","Fire Hydrant Fittings: Below ground level"]
[]
[null,"L639",null,"Complete as per Drawing No. AC345/19/FD01","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.5j","Fire Hydrant Fittings: Woodland type or similar"]
[]
[null,"L640",null,"Complete as per Drawing No. AC345/19/FD01","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.11","Anchor/Thrust blocks and pedestals"]
[]
[{"$nulls":3},"Complete as per Drawing No. AC345/19/SD/10"]
[]
[null,"L641",null,"Concrete (20MPa/19mm)","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L642",null,"Formwork","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.13","Valve and hydrant chambers"]
[]
[null,"L643",null,"Valve chamber as per  Drawing No. AC345/19/CD01","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L644",null,"Air Valve chamber as per  Drawing No. AC345/19/SD01","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L645",null,"Scour Valve chamber as per  Drawing No. AC345/19/SD03","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,"L646",null,"Formwork","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L647","8.2.13","Valve and hydrant chambers"]
[]
[null,"L648",null,"Valve chamber as per  Drawing No. AC345/19/CD02","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L649",null,"Air Valve chamber as per  Drawing No. AC345/19/SD02","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L650",null,"Scour Valve chamber as per  Drawing No. AC345/19/SD03a","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L651",null,"Formwork","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L652","8.2.13","Valve and hydrant chambers"]
[]
[null,"L653",null,"Air Valve chamber 1500mm dia. Rings with 650mm dia Composite Fiber lid, painted yellow with 75mm blackstenciled letters, stating chainage and marked AV No.","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L654",null,"Valve chamber minimum scour pipe of 160mm dia. With 650mm dia. Composite Fiber lid, painted yellow with 75mm black tenciled letters, stating chainage and marked SV No.","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":3},"Scour Valve chamber as per  Drawing No. AC","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"PSL8.2.15","Special Wrapping (Denso lay flat or similar approved in writing)"]
[]
[null,"L655",null,"(a) Buried Flanges"]
[]
[null,"L656",null,"DN50 to DN150","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L657",null,"DN150  to DN200","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L658",null,"DN200 to DN250","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L659",null,"DN250 to DN300","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L660",null,"DN300 to DN350","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L661",null,"DN350 to DN400","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L662",null,"DN400 to DN450","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L663",null,"DN450 to DN500","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L664",null,"(b) Viking Johnson Type coupling: Buried"]
{"$rows_empty":9}
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[null,"SCHEDULE 8"]
[]
[null,"SANS 1200L  -  MEDIUM PRESSURE PIPELINES"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,"L665",null,"DN50 to DN150","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L666",null,"DN150 to DN200","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L667",null,"DN200 to DN250","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L668",null,"DN250 to DN300","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L669",null,"DN300 to DN350","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L670",null,"DN350 to DN400","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L671",null,"DN400 to DN450","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L672",null,"DN450 to DN500","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L673",null,"(c) Buried steel pipes: only where directed by Engineer in writing"]
[]
[null,"L674",null,"DN50 to DN150","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L675",null,"DN150  to DN200","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L676",null,"DN200 to DN250","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L677",null,"DN250 to DN300","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L678",null,"DN300 to DN350","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L679",null,"DN350 to DN400","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L680",null,"DN400 to DN450","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L681",null,"DN450 to DN500","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"L682","PSL8.2.16","Marker Posts","No.",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
{"$rows_empty":16}
[null,"CARRIED FORWARD TO SUMMARY",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 9"]
[]
[null,"SANS 1200LB  - BEDDING"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"LB","SABS","SECTION LB:  BEDDING"]
[null,null,"1200 LB"]
[{"$nulls":3},"PROVISION OF BEDDING"]
[]
[{"$nulls":3},"Available from trench within 0,5 km (Subclause 3.4.1)"]
[]
[null,"LB1","8.2.1","(a) Selected granular material ","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LB2",null,"(b) Selected fill material","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[null,null,"8.2.2","Supply only of bedding by Importtation"]
[]
[null,null,"8.2.2.2","From Commercial sources (Provisional)"]
[]
[null,"LB3",null,"(1) Selected granular material","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LB4",null,"(2) Selected fill material","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LB5",null,"(3) 19mm stone","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.2.3","From Commercial sources (Provisional)"]
[]
[null,"LB3",null,"(1) Selected granular material","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LB4",null,"(2) Selected fill material","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LB5",null,"(3) 19mm stone","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LB6","PSA","Extra-over items LB3 to LB9 for screening of bedding materials","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LB7",null,"Extra-over items LB3 to LB 9 for bedding stabilized with 5% cement","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LB8",null,"Extra-over items LB9 for geotextile (Bidem U19 or similar)","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LB9","8.2.3","Concrete Bedding Cradle","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LB10","8.2.4","Encasing of pipes in concrete","m³",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"8.2.5","Overhaul of material for bedding (Provisional) where ordered Extra-over "]
[{"$nulls":3},"items LB3 TO LB4"]
[]
[null,"LB11",null,"a) Selected granular material","m³.km",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LB12",null,"b) Selected fill material","m³.km",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"SABS","High-tensile welded mesh in the following:",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null,null,"1200 G",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[null,null,"8.3.2","Ref 395 in concrete encasing around pipes","m²",{"v":1,"d":"1.00"},0,{"v":0,"d":"R 0.00"}]
{"$rows_empty":13}
[null,"CARRIED FORWARD TO SUMMARY",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 10"]
[null," "]
[null,"SANS 1200 LC : CABLE DUCTS"]
[null,"ITEM","REFE-","DESCRIPTION","UNIT","QUANT","RATE","AMOUNT"]
[null,"NO.","RENCE",{"$nulls":3},"R      C","R      C"]
[null,null,"SANS 1200 LF","SECTION 5 : CABLE DUCTS"]
[]
[{"$nulls":3},"Supply, Lay, Bed and Prove Duct:"]
[]
[null,null,"8.2.2","Excavation"]
[]
[null,"LC01",null,"(a) Excavate in all material for trenches, backfill, compact and dispose of surplus","m³",{"v":1,"d":"1.00"}]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[null,"LC02",null,"(b) Extra over items (a) above for:"]
[null,"LC03",null,"(i)  Intermediate excavation  ","m³",{"v":1,"d":"1.00"}]
[null,"LC04",null,"(ii)  Hard rock excavation     ","m³",{"v":1,"d":"1.00"}]
[null,"LC05",null,"(iii)  Boulder excavation, class A ","m³",{"v":1,"d":"1.00"}]
[null,"LC06",null,"(iv)  Boulder excavation, class B ","m³",{"v":1,"d":"1.00"}]
[]
[null,"LC07","8.2.3","Shore trench at structures","m",{"v":1,"d":"1.00"}]
[]
[null,"LC08","8.2.5","Supply, Lay, Bed and Prove Duct:","m",{"v":1,"d":"1.00"}]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[]
[]
[]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[{"$nulls":7},{"v":0,"d":"0.00"}]
{"$rows_empty":7}
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 10"]
[null," "]
[null,"SANS 1200 LF : WATER -ERF CONNECTION"]
[null,"ITEM","REFE-","DESCRIPTION","UNIT","QUANT","RATE","AMOUNT"]
[null,"NO.","RENCE",{"$nulls":3},"R      C","R      C"]
[null,null,"SANS 1200 LF","SECTION 5 : WATER - ERF CONNECTIONS"]
[]
[null,"LF1","8.2.1","Provide erf connection complete as per drawing "]
[{"$nulls":3},"AC265/11/10"]
[]
[null,"LF1.1",null,"a) Double","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF1.2",null,"b) Single","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF2","8.2.2","Supply, lay and test erf connection"]
[]
[null,"LF2.1",null,"a) Type V, Class 12 PN 12.5 PE 80 HDPE pipes"]
[{"$nulls":3},"    including all fittings, couplings and saddles:"]
[]
[null,"LF2.1"," ","    20 mm dia","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF2.1.1",null,"    25 mm dia","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF2.1.3",null,"    32 mm dia","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF2.2",null,"b) Galvanized mild steel, medium class pipes, including"]
[{"$nulls":3},"    all fittings and couplings:"]
[]
[null,"LF2.2.1",null,"    20 mm dia","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF2.2.2",null,"    25 mm dia","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF2.2.3",null,"    40 mm dia","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF3","8.2.3","Extra over item 8.2.2 for specials"]
[]
[null,"LF3.1",null,"a) GMS - 90° Bends"]
[]
[null,"LF3.1.1",null,"        ½ \" ","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.1.2",null,"        ¾ \"","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF3.2",null,"b) Plasson 90° elbow with male offtake"]
[]
[null,"LF3.2.1",null,"      25 x ¾ \"","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF3.3",null,"c) Plasson 90° elbow with female offtake"]
[]
[null,"LF3.3.1",null,"      32 x 1\"","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF3.4",null,"d) GMS Nipples"]
[]
[null,"LF3.4.1",null,"        ½ \"","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.4.2",null,"        ¾ \"","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF3.5",null,"e) Plasson female adapter"]
[]
[null,"LF3.5.1",null,"      25 x ½ \"","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.5.2",null,"      25 x ¾ \"","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
{"$rows_empty":21}
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 10"]
[null," "]
[null,"SANS 1200 LF : WATER -ERF CONNECTION"]
[null,"ITEM NO","PAYMENT REFERS"," DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[null,"LF3.6",null,"f) Plasson male adapter"]
[]
[null,"LF3.6.1",null,"      25 x ½ \"","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.6.2",null,"      25 x ¾ \"","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.6.3",null,"      32 x 1¼\"","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF3.7",null,"g) Plasson 90° Tee with female offtake"]
[]
[null,"LF3.7.1",null,"      25 x 1¼\" x 25","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF3.8",null,"h) Cobra brass ball valve (Ball-o-stop)"]
[]
[null,"LF3.8.1",null,"        ¾ \"","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF3.9",null,"i) Plasson saddles"]
[]
[null,"LF3.9.1",null,"       75 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.9.2",null,"       90 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.9.3",null,"       110 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.9.4",null,"       160 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.9.5",null,"       200 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.9.6",null,"       250 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF3.10",null,"j) Mild steel saddles"]
[]
[null,"LF3.10.1",null,"       315 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.10.2",null,"       355 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.10.3",null,"       400 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF3.11",null,"k) Cast iron saddles"]
[]
[null,"LF3.11.1",null,"       50 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.11.2",null,"       75 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.11.3",null,"       90 x 30 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.11.4",null,"       100 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.11.5",null,"       150 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.11.6",null,"       200 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.11.7",null,"       250 x 32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF3.12","PSLF 7","l) Collect, store and installation of water meters","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF3.13","PSLF 8","m) Secure and deliver old of water meters to MLM depot","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF3.14","PSLF 9","n) Provision of Pillar type meter box complete with Class C 15mm "]
[{"$nulls":3},"    water meter","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
{"$rows_empty":10}
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 10"]
[null," "]
[null,"SANS 1200 LF : WATER -ERF CONNECTION"]
[null,"ITEM NO","PAYMENT REFERS"," DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,"LF3.15",null,"p) 110 mm dia Polyethylene round valve box","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF.3.16",null,"q) GMS End Caps"]
[]
[null,"LF3.16.1",null,"        ½ \"","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.16.2",null,"        ¾ \"","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.16.3",null,"        1 \"","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF.3.17",null,"r) Plasson End Caps"]
[]
[null,"LF3.17.1",null,"        20 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.17.2",null,"        25 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,"LF3.17.3",null,"        32 mm","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF.4",null,"Ancilliaries"]
[]
[null,"LF4.1",null,"Remove existing water meter ","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LF4.2",null,"Connect, new communication pipe at old water"]
[{"$nulls":3},"meter connection","No",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
{"$rows_empty":39}
[null,"CARRIED FORWARD TO SUMMARY",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 11"]
[]
[null,"PSLV  -  PIPE JACKING AND BORING"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,null,"LG"," PIPE JACKING "]
[]
[null," ","8.2.1","Jacking Establishment"]
[]
[null,"LG1"," ","(a) Fixed charges","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG2"," ","(b) Time related charges","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3}," "," "," "]
[null,null,"8.2.2","Supply of concrete pipes to be jacked - D-Load designation 100D",null,{"v":1,"d":"1.00"}]
[null," "," "," "]
[null,"LG3",null,"(a)  300mm Diameter","m ",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,null," "," "," "," "]
[null,"LG4",null,"(b)  400mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,null," "," "," "," "]
[null,"LG5",null,"( c ) 500 mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,null," "," "]
[null,"LG6",null,"(d)   600 mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null,null," "," "]
[null,"LG7.12",null,"( e ) 700mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3}," "," "," "]
[null,"LG8",null,"(f )   800mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG9",null,"(g)  900mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG10",null,"(h)   1000mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null," ",null," "," "," "]
[null,null,"8.2.3","Jacking  of concrete pipes - D-Load designation 100D"]
[null," "," "," "]
[null,"LG11",null,"(a)  300mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null," "," "," ",null," "]
[null,"LG12",null,"(b)  400mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null," ",null," ","  "," "]
[null,"LG13",null,"( c ) 500 mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null," ",null," "," "]
[null,"LG14",null,"(d)   600 mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null," ",null," "," "]
[null,"LG15",null,"( e ) 700mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null," ",null," "," "," "]
[null,"LG16",null,"(f )   800mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null," ",null,null," "]
[null,"LG17",null,"(g)  900mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null," "," ",null," "]
[null,"LG18",null,"(h)   1000mm Diameter","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[null," ",null," "," "," "]
[null,null,"8.2.4","Excavation for Jacking"]
[null," ",null," "," "," "]
[null,"LG19",null,"(i)  soft excavation  ","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG20",null,"(ii)  intermediate excavation     ","m3",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3}," "]
[null,"LG21","8.2.5","Extra-Over 8.2.1 and 8.2.4 for unseen rock and boulders","Pov Sum ",{"v":1,"d":"1.00"},null,{"v":10000,"d":"10,000.00"}]
[{"$nulls":3}," "," "," "]
[null," ","8,2,6","Supply and install Pipeline by Pipe Jacking Method, Complete"," "," "]
[{"$nulls":3},"with Excavation"," "," "]
[]
[null,"LG22",null,"50 mm dia. HDPE PE63 (TYPE IV) Class 12","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG23",null,"75 mm dia. HDPE PE63 (TYPE IV) Class 12","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG24",null,"110 mm dia. HDPE PE63 (TYPE IV) Class 12","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG25",null,"160 mm dia. HDPE PE63 (TYPE IV) Class 12","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG26",null,"250 mm dia. HDPE PE63 (TYPE IV) Class 12","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG27",null,"315 mm dia. HDPE PE63 (TYPE IV) Class 12","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG28",null,"400 mm dia. HDPE PE63 (TYPE IV) Class 12","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG29",null,"500 mm dia. HDPE PE63 (TYPE IV) Class 12","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG30",null,"600 mm dia. HDPE PE63 (TYPE IV) Class 12","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG31",null,"800 mm dia. HDPE PE63 (TYPE IV) Class 12","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG32",null,"900 mm dia. HDPE PE63 (TYPE IV) Class 12","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[null,"TOTAL CARRIED FORWARD TO SUMMARY",{"$nulls":5},{"v":10000,"d":"10,000.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 11"]
[]
[null,"PSLV  -  PIPE JACKING AND BORING"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[null,"BROUGHT FORWARD",{"$nulls":5},{"v":10000,"d":"10,000.00"}]
[]
[null,"LG33","8.2.7","Extra-Over 8.2.6 for length of pipeline greater than 85m","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null," ","8.2.8","Extra-Over 8.2.6 for length of pipeline greater than 85m",{"$nulls":3},{"v":0,"d":"0.00"}]
[]
[null,"LG33",null,"(a) Using pneumatic tools or other techniques where blasting is not permitted","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG34",null,"(b) Using explosives, where permited","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null," ","8,2,9","Stabilazation of Unstable Areas or Grouting of Voids where ordered",{"$nulls":3},{"v":0,"d":"0.00"}]
[]
[null,"LG35",null,"(a) Provision and establishment of equipment on Site, and removal of on completion","Sum",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG36",null,"(b) Operation of equipment","Day",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG37",null,"(c) Materials used ","kg",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"LG38","8.2.10","Standing time for pipe Jacking Gang and the Jacking ","hr",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"Equipment covered by 8.2.1"]
{"$rows_empty":27}
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[{"$nulls":7},{"v":0,"d":"0.00"}]
[]
[]
[null,"TOTAL CARRIED FORWARD"]
[]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[null,"SCHEDULE 12"]
[]
[null,"SANS 0400 - PUMP STATION BUILDING"]
[null,"ITEM NO","PAYMENT REFERS","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"PSB 1","SANS 0400","BRICKWORK"]
[]
[]
[{"$nulls":3},"BRICKWORK"]
[]
[null,"PSB 2",null,"One brick wall in clay bricks , minimum 7MPA compressive ","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"strength  complying to SANS 227 in cement  sand mortar 1:6 "]
[]
[null,"PSB 3",null,"Brick on edge window cill","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":5}," "]
[{"$nulls":3},"FACINGS"]
[]
[null,"PSB 4",null,"Extra over common brick as described above for  ","m²",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"facebrickwork in dark facebrick 'corobrick country classic "]
[{"$nulls":3},"traventine."]
[]
[{"$nulls":3},"Builders Work In Connection with "]
[]
[null,"PSB 5",null,"Form hole in facebrick  size 860x860mm for 500mm diameter steel ","no",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"pipe, enclose pipe in  concrete (10Mpa) , including all formwork "]
[{"$nulls":3},"as necessary making good around brickwork and finishing as "]
[{"$nulls":3},"specified."]
[]
[null,"PSB 6",null,"Form hole in common brick  size 860x860mm for 500mm diameter ","no",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"steel pipe, enclose pipe in  concrete (10Mpa) , including all "]
[{"$nulls":3},"formwork as necessary making good around brickwork and "]
[{"$nulls":3},"finishing as specified."]
[]
[null,"PSB 7",null,"Pin or build in end of steel joists to brickwork in cement mortar.","no",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"Cotts' or other equal and approved mesh brick reinforcement "]
[{"$nulls":3},"lapped at all angles and junctions (measured nett)"]
[]
[null,"PSB 8",null,"Ref. C2  in one brick walls","m",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,null,"SANS 0400","Building In"]
[]
[null,"PSB 9",null,"Set up in position, cross brace and build in pressed steel door ","no",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"frame not exceeding 5 square metres."]
[]
[null,"PSB 10",null,"Set up in position, cross brace and build in roller shutter doors.","no",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"PSB 11",null,"Ditto steel louvres","no",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[]
[null,"PSB 12",null,"Set up in position and build in steel window and frame not ","no",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"exceeding 5 square metres."]
[]
[{"$nulls":3},"Damp Proofing"]
[]
[null,"PSB 13",null,"One layer of three ply bituminous felt sheeting laid on walls, ","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
[{"$nulls":3},"lapped and sealed at all angles and junctions on and including "]
[{"$nulls":3},"a bed of mortar trowelled smooth (measured nett)."]
[]
[null,"PSB 14",null,"Ditto laid under cills including dressing as required (ditto)","m2",{"v":1,"d":"1.00"},null,{"v":0,"d":"0.00"}]
{"$rows_empty":21}
[null,"TOTAL CARRIED FORWARD",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[]
[null,"CONTRACT NO.: ",null,"BID 8/2/2/434 (2025-2028)"]
[null,"BID TO APPOINT A SERVICE PROVIDER FOR THE CONSTRUCTION OF BULK WATER SUPPLY LINE FOR MIDVAAL LOCAL MUNICIPALITY ON AN AS AND WHEN REQUIRED BASIS FROM 1 JULY 2025 TO 30 JUNE 2028"]
[]
[]
[]
[{"$nulls":3},"SUMMARY TO SCHEDULE OF QUANTITIES "]
[]
[null,"SECTION",null,"DESCRIPTION",null,null,"AMOUNT (RAND)"]
[{"$nulls":6},{"v":0,"d":"0.00"}]
[null,"A",null,"Preliminary and General"]
[{"$nulls":6},{"v":0,"d":"0.00"}]
[null,"C",null,"Site Clearance"]
[{"$nulls":6},{"v":0,"d":"0.00"}]
[null,"D",null,"Earthworks"]
[]
[]
[null,"DB",null,"Earthworks (Pipe Trenches)"]
[]
[{"$nulls":6},{"v":0,"d":"0.00"}]
[null,"DK",null,"Gabions"]
[]
[{"$nulls":6},{"v":0,"d":"0.00"}]
[null,"GA",null,"Concrete : Small Works"]
[]
[{"$nulls":6},{"v":0,"d":"0.00"}]
[null,"G",null,"Reinforced Concrete"]
[]
[{"$nulls":6},{"v":0,"d":"0.00"}]
[null,"L",null,"Medium Pressure Pipelines"]
[]
[{"$nulls":6},{"v":0,"d":"0.00"}]
[null,"LB",null,"Bedding"]
[]
[]
[null,"LC",null,"CABLE DUCTS",null,null,{"v":0,"d":"0.00"}]
[]
[{"$nulls":6},{"v":0,"d":"0.00"}]
[null,"LF",null,"Water Erf Connection"]
[]
[]
[null,"LG",null,"Pipe Jacking and Boring"]
[]
[{"$nulls":6},{"v":0,"d":"0.00"}]
[null,"PSB",null,"PUMP STATION BUILDING"]
[]
[null,"Total Carried Forward to Summary of Schedules",{"$nulls":5},{"v":0,"d":"0.00"}]
[]
[null,null,"N.B."]
[null,null,"1. THREE YEARS FINANCIAL STATEMENTS MUST SUBMITTED WITH THIS BID"]
[null,null,"2. THE ESTIMATED QUANTITIES IN THIS BILL OF QUATINTIES ARE FOR EVALUATION PURPOSE ONLY"]
[null,null,"3. IT IS THE INTENTION OF THE EMM TO APPOINT A MINIMUM OF FOUR CONTRACTORS. EMM RESERVES THE "]
[null,null,"RIGHT TO OFFER RATES TO BIDDERS WHOSE RATES EXCEED THAT OF THE HIGHEST SCORING BIDDER"]
[null,null,"4.ALL ITEMS IN THE BILL OF QUANTITIES MUST BE PRICED AS PER THE PRICING INSTRUCTIONS"]
[]
[]
[null,null,"BIDDING ENTITY:"]
[]
[null,null,"ADDRESS:"]
[]
[null,null,"AUTHORISED SIGNATORY:"]
[]
[null,null,"CAPACITY OF SIGNATORY:"]
[]
[null,null,"SIGNATURE:                                                                                        DATE:"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}