{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["List of Switchboards"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"List of Switchboards","index":0,"n_rows":22,"n_cols":16,"rows_kept":22}
[]
[{"$nulls":3},"LIST OF SWITCHBOARDS INCLUDING THEIR BASIC TECHNICAL REQUIREMENTS "]
[]
["Board Identification","Nominal current rating","Voltage Nominal kV","Voltage Maximum kV","Impulse level kV","Power Frequency 60 sec kV","Short Circuit Fault Current r.m.s. 3 sec kA","Short Circuit Fault Current Peak kA","Type AIS/GIS","MODEL","Heat Loading Based on full Load Current (Watts)","Width of Switchboard (m)","Length of Switchboard (m)","Length of Switchboard (m)","Estimated Weight of each Switchboard (kg)","DC Loading of the Switchboard (Watts) Worse Case"]
["11kV Station board 1",2000,11,12,95,38,25,63,"AIS"]
["11kV Station board 2 ",2000,11,12,95,38,25,63,"AIS"]
["11kV Coal conveyor board 1",1250,11,12,95,38,25,63,"AIS"]
["11kV Coal conveyor board 2",1250,11,12,95,38,25,63,"AIS"]
["11kV Coal conveyor board 3",630,11,12,95,38,20,50,"RMU AIS"]
["11kV Coal conveyor board 4",630,11,12,95,38,20,50,"RMU AIS"]
["11kV Coal conveyor board 5",630,11,12,95,38,20,50,"RMU AIS"]
["11kV Coal conveyor board 6",630,11,12,95,38,20,50,"RMU AIS"]
["11kV Coal conveyor board 7",630,11,12,95,38,20,50,"RMU AIS"]
["11kV Coal conveyor board 8",630,11,12,95,38,20,50,"RMU AIS"]
["11kV Coal conveyor board 9",630,11,12,95,38,20,50,"RMU AIS"]
["11kV Coal conveyor board 10",630,11,12,95,38,20,50,"RMU AIS"]
["11kV Coal conveyor board 11",630,11,12,95,38,20,50,"RMU AIS"]
["11kV Coal conveyor board 12",630,11,12,95,38,20,50,"RMU AIS"]
["11kV Coal conveyor board 13",630,11,12,95,38,20,50,"RMU AIS"]
["11kV ASQ board 1",630,11,12,95,38,20,50,"RMU GIS "]
["11kV ASQ board 2",630,11,12,95,38,20,50,"RMU GIS "]
["11kV Sewage plant board",630,11,12,95,38,20,50,"RMU GIS "]