{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["TRADE SECTIONS","P&G's","BOQ","TRANSPORT","LABOUR ONLY","ADHOC MATERIAL","BOM","DRAWING NUMBERS","Proposed by FS"],"not_rendered":{"images":6,"macros":1,"external_links":1,"defined_names":15},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"TRADE SECTIONS","index":0,"n_rows":12,"n_cols":2,"rows_kept":12,"merged":[[0,0,0,1],[4,0,4,1]],"flags":["formulas_cached_only"]}
[]
["2025-2028 SMART TECHNOLOGY BoQ Rev0"]
[]
["TRADE SECTIONS"]
["2026-03-10"]
[]
["SECTION","DESCRIPTION"]
["A&B","PRELIMINARY AND GENERAL ITEMS"]
["C","SERVICE CONDUCTOR INSTALLATION"]
["D","TRANSPORT"]
["E","ADHOC MATERIAL"]
[null,"AVERAGE SAVINGS ACHIEVED "]

{"sheet":"P&G's","index":1,"n_rows":39,"n_cols":9,"rows_kept":39,"merged":[[0,0,0,2],[4,0,4,2],[11,1,11,2],[22,1,22,3],[23,1,23,3],[36,2,36,3],[37,2,37,3],[38,0,38,2]],"flags":["formulas_cached_only"]}
[]
["2025-2028 SMART TECHNOLOGY BoQ Rev0"]
[]
["PRELIMINARY AND GENERAL ITEMS"]
["2026-03-10"]
[]
[]
[]
["PO NUMBER:"]
["Bill No:1",null,"PRELIMINARY AND GENERAL ITEMS"]
["No",null,"DESCRIPTION","UNIT"," RATE "]
["A","FIXED CHARGE ITEMS"]
["A.3.","Sample Board and Stubby Line"]
["A.3.1",null,"Construct a sample board and stubby line as per the drawings and specification stated in the latest revision of MVL-EI-048 published by Eskom Standards Implementation Department. ","Sum"]
[]
["A.1.","Health and Safety measures                               (In terms of 34-333)","Safety & Health, Environmental"]
["A.1.1","3.1.1","Compliance with OH&S Act & Construction Regulations. (for projects where task order value exceed R100,000-00) ","Sum",{"$nulls":3},32497.248767999998,{"v":33770.65346097408,"d":"R 33,770.65"}]
[]
["A.2.","Materials Management"]
["A2.1",null,"The Contractor shall make allowance to receive at Eskom stores, offload and stack the free-issue materials supplied to the contractor. ","Sum"]
["A.3.","Contractual requirements  "," Comply ,maintain all insurance  and statutory contributions, etc."]
["A.3.1",null," Allowance to Comply ,maintain all insurance  and statutory contributions, etc. (Actual cost will be paid at the end of the project and proof of policy must be provided and must be compliant to contractual requirements)","Sum"]
[null,"Sub-Total A"]
["B.","TIME RELATED ITEMS"]
["B.1","Site Establishment"]
["B.2","Accommodation","Accommodation Allowance is for the Contractors Staff excluding the casual labourers which are assumed to be residing in the area where the works are executed."]
["B.2.1.",null,"Staff Accommodation Allowance","Weeks"]
["B.3","Security"]
["B.3.1.",null,"Security on site - 24 Hour Unarmed Security (Must be registered with the appropriate body)","Weeks"]
["B.4.","Labour","The Contractor need to submit Weekly Time Sheets for all hourly compensation claims and a Daily attendance register "]
["B.4.1.",null,"Supervisor per team","hourly"]
["B.4.2.",null,"Community Liaison Officer","Daily (Max)"]
["B.4.3.",null,"Safety Officer (SACPMP Registered)","hourly"]
["B.4.4.",null,"Maintenance of H&S file (only applicable for projects exceeding 1 month in duration) ","Monthly "]
["B.4.5.",null,"Tools and equipment (Provision made for only rental of Specialized Tools) - minimum of 3 supplier quotes required at task order approval stage.  ","Sum"]
["B.5",null,"Android device for use as EDA tool to capture MMF (Meter movement Form). Note: EDA guideline to be applied:\n•\tAndroid 10 or earlier\n•\tCamera 13MP or higher\n•\tBarcode scanning keyboard installedl (one per team)","each"]
[null,null,"Sub-Total B"]
[null,null,"Total P & G's Carried To Summary"]
["Contractor's Signature:"]

{"sheet":"BOQ","index":2,"n_rows":169,"n_cols":5,"rows_kept":169,"merged":[[0,0,0,2],[4,0,4,2],[7,0,7,3],[167,0,167,3],[168,0,168,4]],"flags":["formulas_cached_only"]}
[]
["2025-2028 SMART TECHNOLOGY BoQ Rev0"]
[]
["BOQ ITEMS"]
["2026-03-10"]
[]
[]
["BILL OF ACTIVITIES",{"$nulls":3},"RATE "]
["ITEM","REFERENCE DRAWING","DESCRIPTION","UNIT"]
["C",null,"SERVICE CONNECTION"]
[1.1,null,"Survey area to determine the installed base of meters and classify installations into predefined categories provided\n"]
["1.1.1",null,"Perform a survey in the allocated area to identify each type of installation.","each"]
["1.1.2",null,"Compile and issue report with detailed information","each"]
[]
[1.2,null,"Replace existing basic split meter with smart meter (Basic split meter installed inside existing pole mounted split meter kiosk to be replaced with smart meter)\n"]
["1.2.1","DDT 9421","Replace split meter in pole top box with smart meter","each"]
["1.2.2","DDT 9422","Replace and Pair CIU and explain basic operation to customer","each"]
["1.2.3",null,"Complete meter movement form","each"]
["1.2.4",null,"Return replaced material to Eskom stores.","sum"]
[]
[1.3,null,"Replace existing basic split meter with smart meter (Basic split meter installed inside existing ground mounted split meter kiosk to be replaced with smart meter)\n"]
["1.3.1","\nDDT 9421","Replace split meter in ground mounted kiosk with smart meter","each"]
["1.3.2",null,"Replace and pair CIU and explain basic operation to customer","each"]
["1.3.3",null,"Complete meter movement form","each"]
["1.3.4",null,"Return replaced material to stores.","sum"]
["1.3.5",null,"Install meter blank-off plate"]
[]
[1.4,null,"Replace existing pole mounted distribution kiosk with Split meter kiosk\n"]
["1.4.1",null,"Remove existing pole top distribution kiosk with meters","each"]
["1.4.2","D-DT 3063","Install split meter pole top box with new smart meters","each"]
["1.4.3","\nDDT 9421","Reconnect service cables to meters","each"]
["1.4.4",null,"Pair CIU with meter","each"]
["1.4.5",null,"Return replaced material to stores.","sum"]
[]
[1.5,null,"Replace existing ground mounted kiosk with Split meter kiosk\n"]
["1.5.1",null,"Remove shell of existing ground mounted distribution kiosk","each"]
["1.5.2",null,"Install retrofit ground mounted split meter pole top kiosk over existing kiosk core.","each"]
["1.5.3",null,"Complete wiring ","each"]
["1.5.4",null,"Pair CIU with meter","each"]
[null,null,"Return the removed kiosk shell to Eskom"]
[]
[1.6,null,"Replace existing common base meter (ECU) with smart meter\n"]
["1.6.1",null,"Remove ECU","each"]
["1.6.2",null,"Replace existing Readyboard with split meter Readyboard","each"]
["1.6.3",null,"Complete meter movement form","each"]
["1.6.4",null,"Pair CIU with new meter","each"]
["1.6.5",null,"Perform commissioning test","each"]
["1.6.6",null,"Issue COC","each"]
[]
[1.7,null,"Replace existing common base meter (ED) with smart meter\n"]
["1.7.1",null,"Remove ED","each"]
["1.7.2",null,"Installation of meter blank-off cover (To by-pass common base)","each"]
["1.7.3",null,"Completion of meter movement form","each"]
["1.7.4",null,"Complete meter movement form","each"]
["1.7.5",null,"Return all removed material to Eskom stores","sum"]
[]
[1.8,null,"Replace 1Ph conventional meter up to 16kVA with smart meter (Din rail)\n"]
["1.8.1","DDT 9421","Remove conventional meter","each"]
["1.8.2",null,"Supply and install Din-rail (60mm)","each"]
["1.8.3",null,"Install preconfigured 1ph smart meter","each"]
["1.8.4",null,"Pair CIU with new meter","each"]
["1.8.5",null,"Complete meter movement form","each"]
[]
[1.9,null,"Replace 3Ph meter up to 50kVA with smart meter \n"]
["1.9.1",null,"Remove 3ph meter","each"]
["1.9.2","DDT 9421"," Install preconfigured 3ph Smart meter","each"]
["1.9.3","D-DT 9503","Mount external antenna","each"]
[]
[{"v":1.1,"d":"1.10"},null,"Install new 4Way pole mounted split meter kiosk\n\n"]
["1.10.1","D-WC-6461-02-02"," Install pole top box (4 way)  ","each"]
["1.10.2","DDT 9421"," Install Smart meters","each"]
["1.10.3",null,"Install service pole","each"]
["1.10.4","D-DT-3140"," Replace concentric service cable","each"]
["1.10.5","D-DT-3140"," Adjust tensioning on concentric service cable","each"]
["1.10.6",null," Pair CIU and educate customer","each"]
["1.10.7",null,"Return all removed material to Eskom Brackenfell","sum"]
[]
[1.11,null,"Install new 6Way Or 9Way pole mounted split meter kiosk"]
["1.11.1","D-WC-6461-10-03","Install pole top box (6 way Or 9way)  ","each"]
["1.11.2","DDT 9421","Install Smart meters","each"]
["1.11.3","D-DT-3140","Install service pole","m"]
["1.11.4","D-DT-3140","Replace concentric service cable","m"]
["1.11.5","D-DT-3141","Adjust tensioning on concentric service cable","each"]
["1.11.6",null,"Pair CIU and educate customer","each"]
["1.11.7",null,"Return all removed material to Eskom Brackenfell","sum"]
[]
[1.12,null,"Install 12 way Ground Mounted Split meter kiosk + smart meters"]
["1.12.1","D-DT 3236"," Install 12way Ground Mounted Split meter kiosk + base","each"]
["1.12.2",null,"  Install meter","each"]
["1.12.3",null,"Terminate LV service cable","m"]
[]
[1.13,null,"Install DC pole mounted\n"]
["1.13.1",null,"Mount DC kiosk","each"]
["1.13.2",null,"Install LV cable between DC kiosk and Transformer bushing","each"]
["1.13.3",null,"Terminate LV cable at DC kiosk using compression gland(Indoor termination)","each"]
["1.13.4",null,"Terminate LV cable at Transformer bushing (Outdoor termination)","each"]
[]
[1.14,null,"Install DC and summation meter inside new type minisub with meter panel\n"]
["1.14.1",null,"Mount DC kiosk","each"]
["1.14.2",null,"Connect DC wiring","each"]
["1.14.3",null,"Mount meter","each"]
["1.14.4",null,"Connect meter wiring","each"]
[]
[1.15,null,"Install DC in older minisub\n"]
["1.15.1",null,"Install CT/VT kiosks","each"]
["1.15.2",null,"Install CTs on minisub LV busbar","ea"]
["1.15.3",null,"Trenching for multicore LV cable","m3"]
["1.15.4",null,"Laying of LV multicore cable between minisub and CT/VT kiosk","m"]
["1.15.5",null,"Backfilling and compaction for LV multicore cable","m3"]
["1.15.6",null,"Terminating of LV multicore cable on CTs and LV busbar","each"]
["1.15.7",null,"Terminating of LV multicore cable on 3ph meter","each"]
["1.15.8",null,"Terminating of LV multicore cable on DC","each"]
[]
["1.16",null,"Install bulk load limiting solution kiosk 100-200kVA (LPU – Ground mounted)\n"]
["1.16.1",null,"Install bulk load limiting kiosks","each"]
["1.16.2",null,"Trenching for LV cable and reroute and terminate existing LV from transformer to Bulk load limiting kiosk.","m3"]
["1.16.3",null,"Laying of LV cable between existing LPU kiosk and Bulk load limiting kiosk","m"]
["1.16.4",null,"Backfilling and compaction for LV cable","m3"]
["1.16.5",null,"Terminate of LV cable","per cable"]
[]
["1.17",null,"Install bulk load limiting solution kiosk 100-200kVA (LPU – Pole mounted)\n"]
["1.17.1",null,"Install bulk load limiting kiosks","each"]
["1.17.2",null,"Reroute and terminate existing LV from transformer to Bulk load limiting kiosk.","each"]
["1.17.3",null,"Installation of LV cable between existing LPU kiosk and Bulk load limiting kiosk","m"]
["1.17.4",null,"Terminate LV cable","per cable"]
[]
[1.18,null,"Install bulk load limiting solution kiosk 315-500kVA (LPU -Ground mounted)\n"]
["1.18.1",null,"Install bulk load limiting kiosks","each"]
["1.18.2",null,"Trenching for LV cables","m3"]
["1.18.3",null,"Reroute and terminate existing LV from transformer to Bulk load limiting kiosk.","each"]
["1.18.4",null,"Laying of LV cable between existing LPU kiosk and Bulk load limiting kiosk","m"]
["1.18.5",null,"Backfilling and compaction for LV cables","m3"]
["1.18.6",null,"Terminate of LV cable","per cable"]
[]
["1.19",null,"Install bulk load limiting solution kiosk 315-500kVA (LPU – Pole mounted)\n"]
["1.19.1",null,"Install bulk load limiting kiosks","each"]
["1.19.2",null," Reroute and terminate existing LV from transformer to Bulk load limiting kiosk.","each"]
["1.19.3",null,"Installation of LV cable between existing LPU kiosk and Bulk load limiting kiosk","m"]
["1.19.4",null,"Terminating of LV cable","per cable"]
[]
["1.20",null,"Reporting on installations completed"]
["1.20.1",null,"Submit detailed reports on all installations completed using the template provided"]
[]
[1.21,null,"Replace 1Ph conventional meter up to 16kVA with smart meter (BS footprint)"]
["1.21.1",null,"Remove conventional meter","each"]
["1.21.2",null,"Install preconfigured 1ph smart meter (BS footprint)","each"]
["1.21.3",null,"Mount external antenna","each"]
["1.21.4",null,"Pair CIU with new meter ","each"]
["1.21.5",null,"Complete meter movement form","each"]
["1.21.6",null,"Return all removed material to Eskom Brackenfell"]
[]
[1.22,null,"Replace 1Ph 16kVA metering kiosk"]
["1.22.1",null,"Disconnect supply and service cables","each"]
["1.22.2",null,"Remove existing meter kiosk","each"]
["1.22.3",null,"Install new kiosk","each"]
["1.22.4",null,"Reconnect supply and service cables","each"]
["1.22.5",null,"Mount external antenna","each"]
["1.22.6",null,"Return all removed material to Eskom Brackenfell"]
[]
[1.23,null,"Replace 3Ph 25-50 kVA metering kiosk"]
["1.23.1",null,"Disconnect supply and service cables","each"]
["1.23.2",null,"Remove existing meter kiosk","each"]
["1.23.3",null,"Install new kiosk","each"]
["1.23.4",null,"Reconnect supply and service cables","each"]
["1.23.5",null,"Mount external antenna","each"]
["1.23.6",null,"Return all removed material to Eskom Brackenfell","each"]
[]
["TOTAL SUMMARY C"]
["Contractor's Signature:"]

{"sheet":"TRANSPORT","index":3,"n_rows":29,"n_cols":4,"rows_kept":29,"merged":[[0,0,0,2],[4,0,4,2],[8,0,8,3],[11,0,11,3],[22,0,22,3],[23,0,23,3],[27,0,27,3],[28,0,28,3]],"flags":["formulas_cached_only"]}
[]
["2025-2028 SMART TECHNOLOGY BoQ Rev0"]
[]
["TRANSPORT ITEMS"]
["2026-03-10"]
[]
[]
[]
["BILL OF ACTIVITIES"]
["ITEM","DESCRIPTION","UNIT","RATE "]
["D","TRANSPORT"]
["Unless otherwise specified, transport is to be used under specific instruction from the Project Manager only.  This excludes staff transport.  Staff transport is to be paid to transport workers from base location to site only.  LDV/4x4 will only be paid for justifiable use and will be to the sole discretion of the Project Manager"]
[1.1,"LDV 4x2","km"]
[1.2000000000000002,"LDV/4x4","km"]
[1.3,"Personnel Transport for Staff","km"]
[1.4000000000000001,"10 m³ Tipper Truck","km"]
[1.5,"6 m³ Tipper Truck","km"]
[1.6,"Transport Truck 2-4 ton","km"]
[1.7000000000000002,"Transport Truck 5-8 ton","km"]
[1.8000000000000003,"Transport Truck 5-8 ton with crane","km"]
[1.9000000000000001,"Transport Truck 9-14 ton","km"]
[{"v":1.1,"d":"1.10"},"Transport Truck 9-14 ton with crane","km"]
["SUB-TOTAL D"]
["WORKER RATES (These rates are only to be used if no other item in the BOQ caters for the activity)"]
[1.1,"Linesman per hour (normal)","hr"]
[1.2,"Labourer per hour (normal)","hr"]
[1.3,"Supervisor per hour (normal)","hr"]
["SUB-TOTAL D"]
["Contractor's Signature:"]

{"sheet":"LABOUR ONLY","index":4,"n_rows":18,"n_cols":4,"rows_kept":18,"hidden":true,"merged":[[0,0,0,2],[4,0,4,2],[9,0,9,1],[16,1,16,2]],"flags":["formulas_cached_only"]}
[]
["2024-2027 National Electrfication BoQ Rev0"]
[]
["LABOUR ITEMS"]
["2026-03-10"]
[]
[]
["ITEM: X","LABOUR"]
[null,"DESCRIPTION","UNIT","RATE "]
["This schedule is used to assist with the valuation of Compensation Events/overtime work - these rates are flat hourly rates as labour is already catered for in the activity rate hence no additional time i.e. half or double time rates will be applied.  "]
[1.1,"Electrician (qualified trade test)-skilled","hour",{"v":125.15,"d":"R 125.15"}]
[1.2000000000000002,"Linesman (Proof of qualification required)-semi skilled","hour",{"v":72.92,"d":"R 72.92"}]
[1.3,"Cable Jointer-skilled","hour",{"v":125.15,"d":"R 125.15"}]
[1.4000000000000001,"Storeman","hour",{"v":41.97,"d":"R 41.97"}]
[1.5,"Semi-skilled Labour (Proof of qualification required)","hour",{"v":72.92,"d":"R 72.92"}]
[1.6,"Unskilled Labour-no formal NQFqualification","hour",{"v":25.62,"d":"R 25.62"}]
[null,"TOTAL - X"]
[null,"Contractor's Signature:"]

{"sheet":"ADHOC MATERIAL","index":5,"n_rows":14,"n_cols":4,"rows_kept":14,"merged":[[0,0,0,2],[4,0,4,2],[7,2,7,3],[10,0,10,1],[12,1,12,2],[13,0,13,3]],"flags":["formulas_cached_only"]}
[]
["2025-2028 SMART TECHNOLOGY BoQ Rev0"]
[]
["AD HOC MATERIAL  ITEMS"]
["2026-03-10"]
[]
[]
["E","Adhoc material"]
[]
[null,"DESCRIPTION","UNIT","RATE"]
["This schedule is used to assist with all the adhoc material that is purchased on the request of the PM/PC. A % handling fee will be compensated to the contractor for the amount before VAT"]
[1.1,"Material bought","%"]
[null,"TOTAL - E"]
["Contractor's Signature:"]

{"sheet":"BOM","index":6,"n_rows":96,"n_cols":5,"rows_kept":96,"merged":[[8,0,8,2],[12,0,12,2],[16,0,16,2],[35,0,35,4]],"flags":["formulas_cached_only"]}
["BILL OF MATERIAL"]
["DWG NO.","SAP NO.","DESCRIPTION","UNIT","QUANTITY"]
["DDT 9421",750638,"METER, ELECTRICAL SERVICE: TYPE: SMART(DIN) G3-PLC) 80A; ","EA",1]
["D-DT 3063",662703,"KIT: SPLITMETER WITH BULK HEAD;READYBOARD","EA",1]
["D-DT 3171",575056,"COVER,ACCESS:PROTECTIVE ;IVORY B77","EA",1]
["DDT 9421",750638,"METER, ELECTRICAL SERVICE: TYPE: SMART(DIN) G3-PLC) 80A; ","EA",9]
["D-DT 9503",246197,"ANTENNA, WEBB ESKANT GSM D9503","EA",1]
["B/Out",null,"Pop rivets","EA",4]
["1. Overhead 4 Way"]
["D-WC-6461-02-02",567826,"BOX, POLE TOP, SPLIT METER, 4 WAY","EA",1]
["DDT 9421",750638,"METER, ELECTRICAL SERVICE: TYPE: SMART(DIN) G3-PLC) 80A; ","EA",4]
["D-DT-3140",632881,"CABLE,ELECT:1000 V ;TCU GSW;6 MM2","M",40]
["2. Overhead 6 Way"]
["D-WC-6461-10-03",669215,"BOX, POLE TOP, SPLIT METER, 6 WAY","EA",1]
["DDT 9421",750638,"METER, ELECTRICAL SERVICE: TYPE: SMART(DIN) G3-PLC) 80A; ","EA",6]
["D-DT-3140",632881,"CABLE,ELECT:1000 V ;TCU GSW;6 MM2","M",40]
["3. Overhead 9 Way"]
["D-WC-6461-10-02",669215,"BOX, POLE TOP, SPLIT METER, 9 WAY","EA",1]
["DDT 9421",750638,"METER, ELECTRICAL SERVICE: TYPE: SMART(DIN) G3-PLC) 80A; ","EA",6]
["D-DT-3140",632881,"CABLE,ELECT:1000 V ;TCU GSW;6 MM2","M",40]
["D-DT 3236",615216,"KSK MTR:1PH;16 KVA;12 WAY PREPAY ","EA",1]
["DDT 9421",750638,"METER, ELECTRICAL SERVICE: TYPE: SMART(DIN) G3-PLC) 80A; ","EA",9]
["D-DT 9503",246197,"ANTENNA, WEBB ESKANT GSM D9503","EA",1]
["B/Out",null,"Pop rivets","EA",4]
["Overhead line applications Option 1 -Armoured cable"]
["DDT","SAP nr","Description","UOM","Quantity"]
["D-DT 1034",571155,"KSK MTR:3PH;0 KVA;DC SECURE POLE MOUNT","EA",1]
["D-DT 9421",621052,"INTERFACE:DC450 G3;PLC DC;230 V (INTERNAL MODEM)","EA",1]
["D-DT 3110",400900,"BUCKLE,STRAP 12 C254 D3110","EA",10]
["D-DT 3111",400902,"STRAP,TIE DOWN:WD 12MM X THK 0.75MM ","M",0.35]
["D-DT 3148",168958,"CABLE END 4-25mm SQ D3148","EA",1]
["D-DT 3102",707881,"LUG, CRIMP CU 4.0SQxM12 F/H D3102","EA",4]
["D-DT 3138",707885,"TUBING SET 2.5-4 SQ 4C LV CABLE D3138","EA",1]
["D-DT 3128",404764,"CABLE ELECT:1 KV;4C;CU;4 MM2;STL WIRE","M",3]
["D-DT 3070",168367,"GLAND,CABLE:ADJUSTABLE;NO 1;BRS CD PLTD","EA",1]
["Overhead line applications Option 2 -Insulated copper conductors"]
["DDT","SAP nr","Description","UOM","Quantity"]
["D-DT 1034",571155,"KSK MTR:3PH;0 KVA;DC SECURE POLE MOUNT","EA",1]
["D-DT 9421",621052,"INTERFACE:DC450 G3;PLC DC;230 V (INTERNAL MODEM)","EA",1]
["D-DT 3110",400900,"BUCKLE,STRAP 12 C254 D3110","EA",10]
["D-DT 3111",400902,"STRAP,TIE DOWN:WD 12MM X THK 0.75MM ","M",0.35]
["D-DT 3039   ",165494,"CLAMP,IPC BIMET 35-95I/6-25I D3039","EA",4]
["D-DT 3137",400660,"WIRE,CU 16SQ 7/1.79 STR PVC BLACK D3137 (4 x 3m)  ","m",12]
["D-DT 3070",404471,"GLAND,CABLE:COMPRESSION A2;NO 1","EA",4]
["D-DT 9503",246197,"ANTENNA, WEBB ESKANT GSM D9503","EA",1]
["DDT","SAP nr","Description","UOM","Quantity"]
["D-DT 9421",621052,"INTERFACE:DC450 G3;PLC DC;230 V (INTERNAL MODEM)","EA",1]
["D-DT 9421",686390,"Landis+Gyr description: E650 - ZMD405CT44.2407.00 B2 1//5A","EA",1]
["D-DT 9503",246197,"ANTENNA, WEBB ESKANT GSM D9503","EA",1]
["B/Out",null,"Pop rivets","EA",4]
["DDT","SAP nr","Description","UOM","Quantity"]
["D-DT 9421",621052,"INTERFACE:DC450 G3;PLC DC;230 V (INTERNAL MODEM)","EA",1]
["D-DT 9421",686390,"Landis+Gyr description: E650 - ZMD405CT44.2407.00 B2 1//5A","EA",1]
["D-DT 3236",730492,"KSK MTR:3PH;230 V;CTVT","EA",1]
["D-DT-3128",404761,"CABLE ELECT:1 KV;12C;CU;2.5 MM2;STL WIRE","M",15]
["D-DT-3102",404438,"LUG, CRIMP CU 2.5SQxM6 F/H D3102","EA",16]
["D-DT 3070",168279,"GLAND,CABLE:ADJUSTABLE;NO 2;BRS NI PLTD","EA",2]
["D-DT 9503",246197,"ANTENNA, WEBB ESKANT GSM D9503","EA",1]
[]
["Supply of material"]
["BILL OF MATERIAL"]
["DWG NO.","SAP NO.","DESCRIPTION","UNIT","QUANTITY"]
["DDT","SAP nr","Description"]
["DDT","SAP nr","Description"]
["D-DT 1034",571155,"KSK MTR:3PH;0 KVA;DC SECURE POLE MOUNT"]
["D-DT 9421",621052,"INTERFACE:DC450 G3;PLC DC;230 V (INTERNAL MODEM)"]
["D-DT 3110",400900,"BUCKLE,STRAP 12 C254 D3110"]
["D-DT 3111",400902,"STRAP,TIE DOWN:WD 12MM X THK 0.75MM "]
["D-DT 3148",168958,"CABLE END 4-25mm SQ D3148"]
["D-DT 3102",707881,"LUG, CRIMP CU 4.0SQxM12 F/H D3102"]
["D-DT 3138",707885,"TUBING SET 2.5-4 SQ 4C LV CABLE D3138"]
["D-DT 3128",404764,"CABLE ELECT:1 KV;4C;CU;4 MM2;STL WIRE"]
["D-DT 3070",168367,"GLAND,CABLE:ADJUSTABLE;NO 1;BRS CD PLTD"]
["D-DT 3039   ",165494,"CLAMP,IPC BIMET 35-95I/6-25I D3039"]
["D-DT 3137",400660,"WIRE,CU 16SQ 7/1.79 STR PVC BLACK D3137 (4 x 3m)  "]
["D-DT 3070",404471,"GLAND,CABLE:COMPRESSION A2;NO 1"]
["D-DT 3236",730492,"KSK MTR:3PH;230 V;CTVT"]
["D-DT-3128",404761,"CABLE ELECT:1 KV;12C;CU;2.5 MM2;STL WIRE"]
["D-DT-3102",404438,"LUG, CRIMP CU 2.5SQxM6 F/H D3102"]
["D-DT 3070",168279,"GLAND,CABLE:ADJUSTABLE;NO 2;BRS NI PLTD"]
["D-DT 9421",686390,"Landis+ E650 - ZMD405CT44.2407.00 B2 1//5A"]
["D-DT 3063",662703,"KIT:SPLITMETER WITH BULK HEAD;READYBOARD"]
["D-DT 3171",575056,"COVER,ACCESS:PROTECTIVE ;IVORY B77"]
["D-WC-6461-02-02",567826,"BOX, POLE TOP, SPLIT METER, 4 WAY"]
["D-WC-6461-10-03",669215,"BOX, POLE TOP, SPLIT METER, 6 WAY"]
["D-WC-6461-10-02",567825,"BOX, POLE TOP, SPLIT METER, 9 WAY"]
["D-DT 3236",615216,"KSK MTR:1PH;16 KVA;12 WAY PREPAY "]
[" D-DT1048",736858,"IED:LOAD LIMITER 100 KVA;400 V"]
[" D-DT1048",736860,"IED:LOAD LIMITER 200 KVA;400 V"]
[" D-DT1048",736859,"IED:LOAD LIMITER 315 KVA;400 V"]
[" D-DT1048",736861,"IED:LOAD LIMITER 500 KVA;400 V"]
["D-DT9421",750638,"SMART(DIN) G3-PLC) 80A"]
["D-DT9421",750641,"SMART(3PH BS PLC)100A"]
["D-DT9421",750644,"SMART(1PH BS GSM) 80A;"]
["D-DT3236",168611,"KIOSK METER:1PH ;16 KVA ;EMPTY"]
["D-DT3236",168612,"KIOSK METER:3PH;25-50 KVA;EMPTY"]

{"sheet":"DRAWING NUMBERS","index":7,"n_rows":62,"n_cols":5,"rows_kept":62,"merged":[[8,0,8,2],[12,0,12,2],[16,0,16,2],[25,0,25,4],[37,0,37,4]],"flags":["formulas_cached_only"]}
[]
["DDT 9421",750638,"METER, ELECTRICAL SERVICE: TYPE: SMART(DIN) G3-PLC) 80A; ","EA",1]
["D-DT 3063",662703,"KIT: SPLITMETER WITH BULK HEAD;READYBOARD","EA",1]
["D-DT 3171",575056,"COVER,ACCESS:PROTECTIVE ;IVORY B77","EA",1]
["DDT 9421",750638,"METER, ELECTRICAL SERVICE: TYPE: SMART(DIN) G3-PLC) 80A; ","EA",1]
["DDT 9421",750641,"METER, SMART(3PH BS PLC)100A,","EA",9]
["D-DT 9503",246197,"ANTENNA, WEBB ESKANT GSM D9503","EA",1]
["B/Out",null,"Pop rivets","EA",4]
["1. Overhead 4 Way"]
["D-WC-6461-02-02",567826,"BOX, POLE TOP, SPLIT METER, 4 WAY","EA",1]
["DDT 9421",750638,"METER, ELECTRICAL SERVICE: TYPE: SMART(DIN) G3-PLC) 80A; ","EA",4]
["D-DT-3140",632881,"CABLE,ELECT:1000 V ;TCU GSW;6 MM2","M",40]
["2. Overhead 6 Way"]
["D-WC-6461-10-03",669215,"BOX, POLE TOP, SPLIT METER, 6 WAY","EA",1]
["DDT 9421",750638,"METER, ELECTRICAL SERVICE: TYPE: SMART(DIN) G3-PLC) 80A; ","EA",6]
["D-DT-3140",632881,"CABLE,ELECT:1000 V ;TCU GSW;6 MM2","M",40]
["3. Overhead 9 Way"]
["D-WC-6461-10-02",669215,"BOX, POLE TOP, SPLIT METER, 9 WAY","EA",1]
["DDT 9421",750638,"METER, ELECTRICAL SERVICE: TYPE: SMART(DIN) G3-PLC) 80A; ","EA",6]
["D-DT-3140",632881,"CABLE,ELECT:1000 V ;TCU GSW;6 MM2","M",40]
[]
["D-DT 3236",615216,"KSK MTR:1PH;16 KVA;12 WAY PREPAY ","EA",1]
["DDT 9421",750638,"METER, ELECTRICAL SERVICE: TYPE: SMART(DIN) G3-PLC) 80A; ","EA",9]
["D-DT 9503",246197,"ANTENNA, WEBB ESKANT GSM D9503","EA",1]
["B/Out",null,"Pop rivets","EA",4]
["Overhead line applications Option 1 -Armoured cable"]
["DDT","SAP nr","Description","UOM","Quantity"]
["D-DT 1034",571155,"KSK MTR:3PH;0 KVA;DC SECURE POLE MOUNT","EA",1]
["D-DT 9421",621052,"INTERFACE:DC450 G3;PLC DC;230 V (INTERNAL MODEM)","EA",1]
["D-DT 3110",400900,"BUCKLE,STRAP 12 C254 D3110","EA",10]
["D-DT 3111",400902,"STRAP,TIE DOWN:WD 12MM X THK 0.75MM ","M",0.35]
["D-DT 3148",168958,"CABLE END 4-25mm SQ D3148","EA",1]
["D-DT 3102",707881,"LUG, CRIMP CU 4.0SQxM12 F/H D3102","EA",4]
["D-DT 3138",707885,"TUBING SET 2.5-4 SQ 4C LV CABLE D3138","EA",1]
["D-DT 3128",404764,"CABLE ELECT:1 KV;4C;CU;4 MM2;STL WIRE","M",3]
["D-DT 3070",168367,"GLAND,CABLE:ADJUSTABLE;NO 1;BRS CD PLTD","EA",1]
[]
["Overhead line applications Option 2 -Insulated copper conductors"]
["DDT","SAP nr","Description","UOM","Quantity"]
["D-DT 1034",571155,"KSK MTR:3PH;0 KVA;DC SECURE POLE MOUNT","EA",1]
["D-DT 9421",621052,"INTERFACE:DC450 G3;PLC DC;230 V (INTERNAL MODEM)","EA",1]
["D-DT 3110",400900,"BUCKLE,STRAP 12 C254 D3110","EA",10]
["D-DT 3111",400902,"STRAP,TIE DOWN:WD 12MM X THK 0.75MM ","M",0.35]
["D-DT 3039   ",165494,"CLAMP,IPC BIMET 35-95I/6-25I D3039","EA",4]
["D-DT 3137",400660,"WIRE,CU 16SQ 7/1.79 STR PVC BLACK D3137 (4 x 3m)  ","m",12]
["D-DT 3070",404471,"GLAND,CABLE:COMPRESSION A2;NO 1","EA",4]
["D-DT 9503",246197,"ANTENNA, WEBB ESKANT GSM D9503","EA",1]
[]
["DDT","SAP nr","Description","UOM","Quantity"]
["D-DT 9421",621052,"INTERFACE:DC450 G3;PLC DC;230 V (INTERNAL MODEM)","EA",1]
["D-DT 9421",686390,"Landis+Gyr description: E650 - ZMD405CT44.2407.00 B2 1//5A","EA",1]
["D-DT 9503",246197,"ANTENNA, WEBB ESKANT GSM D9503","EA",1]
["B/Out",null,"Pop rivets","EA",4]
[]
["DDT","SAP nr","Description","UOM","Quantity"]
["D-DT 9421",621052,"INTERFACE:DC450 G3;PLC DC;230 V (INTERNAL MODEM)","EA",1]
["D-DT 9421",686390,"E650 - ZMD405CT44.2407.00 B2 1//5A","EA",1]
["D-DT 3236",730492,"KSK MTR:3PH;230 V;CTVT","EA",1]
["D-DT-3128",404761,"CABLE ELECT:1 KV;12C;CU;2.5 MM2;STL WIRE","M",15]
["D-DT-3102",404438,"LUG, CRIMP CU 2.5SQxM6 F/H D3102","EA",16]
["D-DT 3070",168279,"GLAND,CABLE:ADJUSTABLE;NO 2;BRS NI PLTD","EA",2]
["D-DT 9503",246197,"ANTENNA, WEBB ESKANT GSM D9503","EA",1]

{"sheet":"Proposed by FS","index":8,"n_rows":1195,"n_cols":7,"rows_kept":1195,"hidden":true,"merged":[[4,4,4,6],[6,1,6,2],[19,1,19,3],[20,1,20,3],[24,4,24,5],[31,2,31,5],[32,2,32,5],[42,0,42,3],[45,0,45,3],[47,0,47,3],[50,0,50,3],[52,0,52,3],[259,0,259,3],[261,0,261,3],[458,0,458,3],[459,0,460,0],[459,1,459,3],[460,1,460,3],[662,0,662,3],[664,0,664,3],[672,0,672,3],[674,0,674,3],[685,0,685,3],[696,0,696,3],[706,0,706,3],[708,0,708,3],[713,0,713,3],[715,0,715,3],[735,0,735,3],[737,0,737,3],[765,0,765,3],[767,0,767,3],[946,0,946,3],[948,0,948,3],[977,0,977,3],[979,0,979,3],[996,0,996,3],[1004,0,1004,3],[1005,1,1005,2],[1055,0,1055,3],[1057,0,1057,3],[1098,0,1098,3],[1100,0,1100,3],[1121,0,1121,3],[1123,0,1123,3],[1156,0,1156,3],[1158,0,1158,3],[1163,0,1163,3],[1165,0,1165,3],[1176,0,1176,3],[1178,0,1178,3],[1180,0,1180,3],[1182,0,1182,3],[1190,0,1190,2]],"flags":["formulas_cached_only"]}
["PROJECT NAME:",null,"START DATE:"]
["CONTRACTOR:",null,"END DATE:"]
["CONTRACT #:"]
["PO NUMBER:"]
["Bill No:1",null,"PRELIMINARY AND GENERAL ITEMS",null,"SCOPE"]
["No",null,"DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
["A","FIXED CHARGE ITEMS"]
["A.1","Site Establishment:","The Contractor shall establish the site camp and maintain throughout the construction period and allow for removal of such upon completion of Works. Establishment include office,store etc.","%",null,{"v":0.1,"d":"10.00%"}]
["A.2.","Sign Board Labour"]
["A.2.1",null,"Contractor shall erect on site, maintain throughout the construction duration(Safety)","each",null,{"v":412.68322567999996,"d":"R 412.68"},{"v":0,"d":"R 0.00"}]
[null,null,"Project sign baord","each",null,{"v":3500,"d":"R 3,500.00"},{"v":0,"d":"R 0.00"}]
["A.3.","Sample Board and Stubby Line"]
["A.3.1",null,"Construct a sample board and stubby line as per the drawings and specification stated in the latest revision of MVL-EI-048 published by Eskom Standards Implementation Department. ","Sum",null,{"v":2310.7323869599995,"d":"R 2,310.73"},{"v":0,"d":"R 0.00"}]
["A.4.","Health and Safety measures                               (In terms of 34-333)","Safety & Health, Environmental"]
["A.4.1",null,"Compliance with OH&S Act & Construction Regulations. ","%",null,{"v":0.05,"d":"5%"},{"v":0,"d":"R 0.00"}]
["A.7.","Materials Management"]
["A.7.1",null,"The Contractor shall make allowance to receive at Eskom stores, offload and stack the free-issue materials supplied to the contractor. ","Sum",null,{"v":11209.039999999999,"d":"R 11,209.04"},{"v":0,"d":"R 0.00"}]
["A.8.","Contractual requirements  "," Comply ,maintain all insurance  and statutory contributions, etc."]
["A.8.1",null," Allowance to Comply ,maintain all insurance  and statutory contributions, etc. (Actual cost will be paid at the end of the project and proof of policy must be provided and must be compliant to contractual requirements)","Sum",null,"cost + 5% fee",{"v":0,"d":"R 0.00"}]
[null,"Sub-Total A",{"$nulls":4},{"v":0,"d":"R 0.00"}]
["B.","TIME RELATED ITEMS"]
["B.2","Accommodation","Accommodation Allowance is for the Contractors Staff excluding the casual labourers which are assumed to be residing in the area where the works are executed."]
["B.2.1.",null,"Staff Accommodation Allowance","Weeks",null,{"v":1232.9943999999998,"d":"R 1,232.99"},{"v":0,"d":"R 0.00"}]
["B.3","Security"]
["B.3.1.",null,"Security on site - 24 Hour Unarmed Security (Must be registered with the appropriate body)","Weeks","cost +  5% fee inline with PSIRA ",null,{"v":0,"d":"R 0.00"}]
["B.5.","Labour","The Contractor need to submit Weekly Time Sheets for all hourly compensation claims and a Daily attendance register "]
["B.5.1.",null,"Supervisor per team","hourly",null,{"v":99.57,"d":"R 99.57"},{"v":0,"d":"R 0.00"}]
["B.5.2.",null,"Construction Manager (SACPMP Registered)","hourly",null,{"v":202.96,"d":"R 202.96"},{"v":0,"d":"R 0.00"}]
["B.5.5.",null,"Storeman \n(Storeman is required to reconcile and quantify All material on site including Eskom supplied material using the correct material return to stores forms. The Storeman shall adhere to the implementation and maintenance plan for Materials Management System for the duration of the contract).","hourly",null,{"v":57.05,"d":"R 57.05"},{"v":0,"d":"R 0.00"}]
["B.5.6.",null,"Community Liaison Officer","Daily (Max)",null,{"v":350,"d":"R 350.00"},{"v":0,"d":"R 0.00"}]
["B.5.7.",null,"Safety Officer (SACPMP Registered)","hourly",null,{"v":139.03,"d":"R 139.03"},{"v":0,"d":"R 0.00"}]
[null,null,"Sub-Total B",{"$nulls":3},{"v":0,"d":"R 0.00"}]
[null,null,"Total P & G's Carried To Summary",{"$nulls":3},{"v":0,"d":"R 0.00"}]
["Verified By:","Clerk of Works",null,"DATE"]
[null,"………………………………………………………………………………………………………………………………………………..",null,"………………………………."]
["Cost Checked By:","Quantity Surveyor",null,"DATE"]
[null,"………………………………………………………………………………………………………………………………………………..",null,"………………………………."]
["Accepted By:","Contractor",null,"DATE"]
[null,"………………………………………………………………………………………………………………………………………………..",null,"………………………………."]
["Approved By:","Program Manager",null,"DATE"]
[]
[]
["BILL OF ACTIVITIES"]
["ITEM","REFERENCE DRAWING","DESCRIPTION","UNIT","LABOUR RATE","LABOUR RATE"]
["A",null,"PRELIMINARY AND GENERAL ITEMS"]
["SUB-TOTAL A"]
["B",null,"BUSH CLEARING & TREE FELLING"]
["In the event where the contractor is required to cut, remove and clear trees on site. This activity shall be used to execute such work provided that the quotation submitted is from a contractor who meets all the necessary requirements for Bush Clearing plus fee. ",{"$nulls":3},"ACCEPTED QUOTE  ",{"v":0.05,"d":"5%"}]
[1,null,"Bush Clearing and Tree Felling (Scattered Formation)","m",{"v":0,"d":"R 0.00"}]
[2,null,"Bush Clearing and Tree Felling (Dense Formation)","m2",{"v":0,"d":"R 0.00"}]
["SUB-TOTAL B"]
["C",null,"EXCAVATIONS"]
["Excavate only as per Eskom Standard for Holes and Trenches for Poles, Stays and Struts.  All  material will be elsewhere measured.  Cement to be priced elsewhere"]
[1,null,"STAYS & STRUTS",null,"Proposed rate","Current Rate","Changes, Proposals and Comments"]
[1.1,"D-DT-0350","LV Stay Back-Actor or Hand excavations","Each",{"v":80,"d":"R 80.00"},{"v":177,"d":"R 177.00"},"Proposed Rate "]
[1.2,"D-DT-0350","LV Stay Bobcat or similar Auger","Each",{"v":495,"d":"R 495.00"},{"v":1306.34,"d":"R 1,306.34"},"Change in Description"]
[1.3,"D-DT-0351","LV/MV Strut Back-Actor or Hand Excavations 9m strut","Each",{"v":150,"d":"R 150.00"},null,"New activity"]
[1.4,"D-DT-0351","LV/MV Strut Back-Actor or Hand Excavations 11m strut","Each",{"v":125,"d":"R 125.00"},{"v":177,"d":"R 177.00"},"See proposed rate and change in Description"]
[1.5,"D-DT-0351","LV/MV Strut Back-Actor or Hand Excavations 12m strut","Each",{"v":55,"d":"R 55.00"},{"v":177,"d":"R 177.00"},"See proposed rate and change in Description"]
[1.5999999999999999,"D-DT-0351","LV/MV Strut Back-Actor or Hand Excavations 15 & 15m strut","Each",{"v":115,"d":"R 115.00"},{"v":177,"d":"R 177.00"},"See proposed rate and change in Description"]
[1.7,"D-DT-0337","LV Short Strut Back-Actor or Hand Excavations","Each",{"v":177,"d":"R 177.00"},{"v":177,"d":"R 177.00"},"See proposed rate and change in Description"]
[1.7999999999999998,"D-DT-0337","LV Short Strut Bobcat or similar Auger (Two Auger Holes)","Each",{"v":945,"d":"R 945.00"},{"v":1306.34,"d":"R 1,306.34"},"Rates correct two auger holes"]
[1.9,"D-DT-0350","MV Stay Back-Actor or Hand Excavations","Each",{"v":105,"d":"R 105.00"},{"v":193.9,"d":"R 193.90"},"See proposed rate and change in Description"]
[{"v":1.1,"d":"1.10"},"D-DT-0350","MV Stay Bobcat or similarly Auger","Each",{"v":685,"d":"R 685.00"},{"v":1317.93,"d":"R 1,317.93"},"See proposed rate and change in Description"]
[1.11,"D-DT-0350","MV/LV Strut Bobcat or similar Auger 9m strut (Two Auger Holes)","Each",{"v":895,"d":"R 895.00"},{"v":1317.93,"d":"R 1,317.93"},"New activity, Rates correct 1.9m deep 1st hole"]
[1.12,"D-DT-0350","MV/LV Strut Bobcat or similar Auger 11m strut (Two Auger Holes)","Each",{"v":790,"d":"R 790.00"},{"v":1317.93,"d":"R 1,317.93"},"New activity, Rates correct 1.6m deep 1st hole"]
[1.13,"D-DT-0350","MV/LV Strut Bobcat or similar Auger 12m strut (Two Auger Holes)","Each",{"v":360,"d":"R 360.00"},{"v":1317.93,"d":"R 1,317.93"},"New activity, Rates are correct 0.76m deep 1st hole"]
[1.14,"D-DT-0350","MV/LV Strut Bobcat or similar Auger 14m strut (Two Auger Holes)","Each",{"v":725,"d":"R 725.00"},{"v":1317.93,"d":"R 1,317.93"},"New activity, Rates are correct 1.53m deep 1st hole"]
[1.15,"D-DT-0350","MV/LV Strut Bobcat or similar Auger 15m strut (Two Auger Holes)","Each",{"v":720,"d":"R 720.00"},{"v":1317.93,"d":"R 1,317.93"},"New activity, Rates are correct 1.52m deep 1st hole"]
[2,null,"WOOD POLES"]
[2.1,"D-DT-0338","2.5m Pole Wood Back-Actor or Hand (0.5m Deep)","Each",{"v":40,"d":"R 40.00"},null,"New activity"]
[2.2,"D-DT-0338","2.5m Pole Wood Bobcat or similar Auger (0.5m Deep)","Each",{"v":160,"d":"R 160.00"},null,"New activity"]
[2.3,"D-DT-0330","5m Pole Wood Back-Actor or Hand (1.0m Deep)","Each",{"v":75,"d":"R 75.00"},{"v":138.67374751,"d":"R 138.67"},"Rate only"]
[2.4,"D-DT-0330","5m Pole Wood Bobcat or similar Auger (1.0m Deep)","Each",{"v":315,"d":"R 315.00"},{"v":1004.8747570899999,"d":"R 1,004.87"},"See proposed rate and change in Description"]
[2.5,"D-DT-0330","5m Pole Wood Hard Rock Drilling (1.0m Deep)","Each",{"v":905,"d":"R 905.00"},{"v":1884.8940604,"d":"R 1,884.89"},"Rate only"]
[2.6,"D-DT-0330","5m Pole Wood Back-Actor or Hand (1.5m Deep)","Each",{"v":110,"d":"R 110.00"},{"v":180.26242352499997,"d":"R 180.26"},"Remove item no longer needed"]
[2.7,"D-DT-0330","5m Pole Wood Bobcat or similar Auger (1.5m Deep)","Each",{"v":475,"d":"R 475.00"},{"v":1306.33942559,"d":"R 1,306.34"},"Remove item no longer needed"]
[2.8,"D-DT-0330","5m Pole Wood Hard Rock Drilling (1.5m Deep)","Each",{"v":1238.8516845600002,"d":"R 1,238.85"},{"v":1238.8516845600002,"d":"R 1,238.85"},"Remove item no longer needed"]
[2.9,"D-DT-0330","7m Pole Wood Back-Actor or Hand (1.3m Deep)","Each",{"v":95,"d":"R 95.00"},{"v":221.872,"d":"R 221.87"},"Proposed Rate "]
["2.10","D-DT-0330","7m Pole Wood Bobcat or similar Auger (1.3m Deep)","Each",{"v":410,"d":"R 410.00"},{"v":1492.96,"d":"R 1,492.96"},"See proposed rate and change in Description"]
[2.11,"D-DT-0330","7m Pole Wood Hard Rock Drilling (1.3m Deep)","Each",{"v":1175,"d":"R 1,175.00"},{"v":1415.83,"d":"R 1,415.83"},"Proposed Rate "]
[2.12,"D-DT-1866","8m  Wooden Pole/X-Arm 160-179 Top Diameter Back-Actor or Hand (1.3m Deep)","Each",{"v":95,"d":"R 95.00"},{"v":208.010621265,"d":"R 208.01"},"Proposed Rate "]
[2.13,"D-DT-1866","8m  Wooden Pole/X-Arm 160-179 Top Diameter auger (1.3m Deep)","Each",{"v":410,"d":"R 410.00"},{"v":1507.3233425,"d":"R 1,507.32"},"Proposed Rate "]
[2.14,"D-DT-1866","8m  Wooden Pole/X-Arm 160-179 Top Diameter Hard Rock Drilling (1.3m Deep)","Each",{"v":1175,"d":"R 1,175.00"},{"v":1592.80930872,"d":"R 1,592.81"},"Proposed Rate "]
[2.15,"D-DT-0330","9m Pole Wood Back-Actor or Hand (1.5m Deep)","Each",{"v":110,"d":"R 110.00"},{"v":277.34749502,"d":"R 277.35"},"See proposed rate and change in Description"]
[2.16,"D-DT-0330","9m Pole Wood Bobcat or similar Auger (1.5m Deep)","Each",{"v":475,"d":"R 475.00"},{"v":2123.74574496,"d":"R 2,123.75"},"See proposed rate and change in Description"]
[2.17,"D-DT-0330","9m Pole Wood Hard Rock Drilling (1.5m Deep)","Each",{"v":1355,"d":"R 1,355.00"},{"v":2279,"d":"R 2,279.00"},"Proposed Rate "]
[2.18,"D-DT-0330","10m Pole Wood Back-Actor or Hand (1.7m Deep)","Each",{"v":125,"d":"R 125.00"},{"v":305.084485895,"d":"R 305.08"},"Proposed Rate "]
[2.19,"D-DT-0330","10m Pole Wood Bobcat or similar auger (1.7m Deep)","Each",{"v":535,"d":"R 535.00"},{"v":2210.73343109,"d":"R 2,210.73"},"See proposed rate and change in Description"]
[{"v":2.2,"d":"2.20"},"D-DT-0330","10m Pole Wood Hard Rock Drilling (1.7m Deep)","Each",{"v":1540,"d":"R 1,540.00"},{"v":2381,"d":"R 2,381.00"},"Proposed Rate "]
[2.21,"D-DT-0330","11m Pole Wood Back-Actor or Hand (1.8m Deep) ","Each",{"v":130,"d":"R 130.00"},{"v":333.146475855,"d":"R 333.15"},"Proposed Rate "]
[2.22,"D-DT-0330","11m Pole Wood Bobcat or similar auger (1.8m Deep)","Each",{"v":570,"d":"R 570.00"},{"v":2411.7061411349996,"d":"R 2,411.71"},"See proposed rate and change in Description"]
[2.23,"D-DT-0330","11m Pole Wood Hard Rock Drilling (1.8m Deep)","Each",{"v":1630,"d":"R 1,630.00"},{"v":2519,"d":"R 2,519.00"},"Proposed Rate "]
[2.24,"D-DT-0330","12m Pole Wood Back-Actor or Hand (2.0m Deep)","Each",{"v":145,"d":"R 145.00"},{"v":277.34749502,"d":"R 277.35"},"Proposed Rate "]
[2.25,"D-DT-0330","12m Pole Wood Bobcat or similar auger (2.0m Deep)","Each",{"v":630,"d":"R 630.00"},{"v":3130.4360141800003,"d":"R 3,130.44"},"See proposed rate and change in Description"]
[2.26,"D-DT-0330","12m Pole Wood Hard Rock Drilling (2.0m Deep)","Each",{"v":1810,"d":"R 1,810.00"},{"v":2123.74574496,"d":"R 2,123.75"},"Proposed Rate "]
[2.27,"D-DT-0330","13m - 16m Pole Wood Back-Actor or Hand (2.2m Deep)","Each",{"v":160,"d":"R 160.00"},{"v":305.084485895,"d":"R 305.08"},"Proposed Rate "]
[2.28,"D-DT-0330","13m - 16m Pole Wood Bobcat or similar auger (2.2m Deep)","Each",{"v":695,"d":"R 695.00"},{"v":2210.73343109,"d":"R 2,210.73"},"See proposed rate and change in Description"]
[2.29,"D-DT-0330","13m - 16m Pole Wood Hard Rock Drilling (2.2m Deep)","Each",{"v":1990,"d":"R 1,990.00"},{"v":2300.7245570400005,"d":"R 2,300.72"},"Proposed Rate "]
[{"v":2.3,"d":"2.30"},"D-DT-0330","18m Pole Wood Back-Actor or Hand (2.4m Deep)","Each",{"v":175,"d":"R 175.00"},{"v":333.146475855,"d":"R 333.15"},"Proposed Rate "]
[2.31,"D-DT-0330","18m Pole Wood Bobcat or similar auger (2.4m Deep)","Each",{"v":755,"d":"R 755.00"},{"v":2411.7061411349996,"d":"R 2,411.71"},"See proposed rate and change in Description"]
[2.32,"D-DT-0330","18m Pole Wood Hard Rock Drilling (2.4m Deep)","Each",{"v":2170,"d":"R 2,170.00"},{"v":2688,"d":"R 2,688.00"},"Proposed Rate "]
[3,null,"CONCRETE POLES"]
[3.1,"D-DT-0330","11m Pole Concrete Back-Actor or Hand (1.8m Deep)","Each",{"v":249.6,"d":"R 249.60"},{"v":249.59929728,"d":"R 249.60"}]
[3.2,"D-DT-0330","11m Pole Concrete Bobcat or similar auger (1.8m Deep)","Each",{"v":570,"d":"R 570.00"},{"v":1808.776804135,"d":"R 1,808.78"},"See proposed rate and change in Description"]
[3.3,"D-DT-0330","11m Pole Concrete Hard Rock Drilling (1.8m Deep)","Each",{"v":1946.77,"d":"R 1,946.77"},{"v":1946.7669328799998,"d":"R 1,946.77"}]
[3.4,"D-DT-0330","12m Pole Concrete Pole Back-Actor or Hand (2m Deep)","Each",{"v":277.35,"d":"R 277.35"},{"v":277.34749502,"d":"R 277.35"}]
[3.5,"D-DT-0330","12m Pole Concrete Pole Bobcat or similar auger (2m Deep)","Each",{"v":630,"d":"R 630.00"},{"v":3130.4360141800003,"d":"R 3,130.44"},"See proposed rate and change in Description"]
[3.6,"D-DT-0330","12m Pole Concrete Hard Rock Drilling (1.0m Deep)","Each",{"v":2123.75,"d":"R 2,123.75"},{"v":2123.74574496,"d":"R 2,123.75"}]
[3.7,"D-DT-0330","13m Pole Concrete Back-Actor or Hand (2.2m Deep)","Each",{"v":305.08,"d":"R 305.08"},{"v":305.084485895,"d":"R 305.08"}]
[3.8,"D-DT-0330","13m Pole Concrete Bobcat or similar auger (2.2m Deep)","Each",{"v":695,"d":"R 695.00"},{"v":2210.73343109,"d":"R 2,210.73"},"See proposed rate and change in Description"]
[3.9,"D-DT-0330","13m Pole Concrete Hard Rock Drilling (1.0m Deep)","Each",{"v":2300.72,"d":"R 2,300.72"},{"v":2300.7245570400005,"d":"R 2,300.72"}]
[{"v":3.1,"d":"3.10"},"D-DT-0330","14m Pole Concrete Back-Actor or Hand (2.3m Deep)","Each",{"v":318.94,"d":"R 318.94"},{"v":318.936171035,"d":"R 318.94"}]
[3.11,"D-DT-0330","14m Pole Concrete Bobcat or similar auger (2.3m Deep)","Each",{"v":725,"d":"R 725.00"},{"v":2311.21418268,"d":"R 2,311.21"},"See proposed rate and change in Description"]
[3.12,"D-DT-0330","14m Pole Concrete Hard Rock Drilling (2.3m Deep)","Each",{"v":2477.7,"d":"R 2,477.70"},{"v":2477.7033691200004,"d":"R 2,477.70"}]
[4,null,"Heavy Conductor Wood Poles "]
[4.1,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 700mm Diameter ","Each",{"v":249.59929728,"d":"R 249.60"},{"v":249.59929728,"d":"R 249.60"}]
[4.2,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 800mm Diameter ","Each",{"v":249.59929728,"d":"R 249.60"},{"v":249.59929728,"d":"R 249.60"}]
[4.3,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 1000mm Diameter ","Each",{"v":249.59929728,"d":"R 249.60"},{"v":249.59929728,"d":"R 249.60"}]
[4.4,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 1000mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil .cement is excluded","Each",{"v":771.59929728,"d":"R 771.60"},{"v":771.59929728,"d":"R 771.60"},"Rate to low if supply of material(cement) is included. Description change in red"]
[4.5,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 1000mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":945.59929728,"d":"R 945.60"},{"v":945.59929728,"d":"R 945.60"},"Rate to low if supply of material(cement) is included. Description change in red"]
[4.6,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 1200mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil. cement is excluded","Each",{"v":771.59929728,"d":"R 771.60"},{"v":771.59929728,"d":"R 771.60"},"Rate to low if supply of material(cement) is included. Description change in red"]
[4.7,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 1200mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":771.59929728,"d":"R 771.60"},{"v":771.59929728,"d":"R 771.60"},"Rate to low if supply of material(cement) is included. Description change in red"]
[4.8,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 1800mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil. cement is excluded","Each",{"v":771.59929728,"d":"R 771.60"},{"v":771.59929728,"d":"R 771.60"},"Rate to low if supply of material(cement) is included. Description change in red"]
[4.9,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 1800mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":945.59929728,"d":"R 945.60"},{"v":945.59929728,"d":"R 945.60"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.1,"d":"4.10"},"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 1800mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1321.34749502,"d":"R 1,321.35"},{"v":1321.34749502,"d":"R 1,321.35"},"Rate to low if supply of material(cement) is included. Description change in red"]
[4.11,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 2000mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1321.34749502,"d":"R 1,321.35"},{"v":1321.34749502,"d":"R 1,321.35"},"Rate to low if supply of material(cement) is included. Description change in red"]
[4.12,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 2200mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1321.34749502,"d":"R 1,321.35"},{"v":1321.34749502,"d":"R 1,321.35"},"Rate to low if supply of material(cement) is included. Description change in red"]
[4.13,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 2500mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1321.34749502,"d":"R 1,321.35"},{"v":1321.34749502,"d":"R 1,321.35"},"Rate to low if supply of material(cement) is included. Description change in red"]
[4.14,"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 700mm Diameter ","Each",{"v":308.1638833555555,"d":"R 308.16"},{"v":308.1638833555555,"d":"R 308.16"}]
[4.15,"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 800mm Diameter ","Each",{"v":308.1638833555555,"d":"R 308.16"},{"v":308.1638833555555,"d":"R 308.16"}]
[4.16,"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 1000mm Diameter","Each",{"v":308.1638833555555,"d":"R 308.16"},{"v":308.1638833555555,"d":"R 308.16"}]
[4.17,"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 1000mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil","Each",{"v":830.163883355556,"d":"R 830.16"},{"v":830.163883355556,"d":"R 830.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.18000000000001,"d":"4.18"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 1000mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":1004.163883355556,"d":"R 1,004.16"},{"v":1004.163883355556,"d":"R 1,004.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.19000000000001,"d":"4.19"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 1200mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil. cement is excluded","Each",{"v":830.163883355556,"d":"R 830.16"},{"v":830.163883355556,"d":"R 830.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.20000000000001,"d":"4.20"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 1200mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":1004.163883355556,"d":"R 1,004.16"},{"v":1004.163883355556,"d":"R 1,004.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.21000000000001,"d":"4.21"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 1800mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil. cement is excluded","Each",{"v":830.163883355556,"d":"R 830.16"},{"v":830.163883355556,"d":"R 830.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.22000000000001,"d":"4.22"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 1800mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":1004.163883355556,"d":"R 1,004.16"},{"v":1004.163883355556,"d":"R 1,004.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.23000000000001,"d":"4.23"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 1800mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1352.163883355556,"d":"R 1,352.16"},{"v":1352.163883355556,"d":"R 1,352.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.24000000000001,"d":"4.24"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 2000mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1352.163883355556,"d":"R 1,352.16"},{"v":1352.163883355556,"d":"R 1,352.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.25000000000001,"d":"4.25"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 2200mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1352.163883355556,"d":"R 1,352.16"},{"v":1352.163883355556,"d":"R 1,352.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.26000000000001,"d":"4.26"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 2500mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1352.163883355556,"d":"R 1,352.16"},{"v":1352.163883355556,"d":"R 1,352.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.27000000000001,"d":"4.27"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 700mm Diameter ","Each",{"v":318.936171035,"d":"R 318.94"},{"v":318.936171035,"d":"R 318.94"}]
[{"v":4.28000000000001,"d":"4.28"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 800mm Diameter ","Each",{"v":318.936171035,"d":"R 318.94"},{"v":318.936171035,"d":"R 318.94"}]
[{"v":4.29000000000001,"d":"4.29"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1000mm Diameter ","Each",{"v":318.936171035,"d":"R 318.94"},{"v":318.936171035,"d":"R 318.94"}]
[{"v":4.30000000000001,"d":"4.30"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1000mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil. cement is excluded","Each",{"v":840.9361710349999,"d":"R 840.94"},{"v":840.9361710349999,"d":"R 840.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.31000000000001,"d":"4.31"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1000mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":1014.9361710349999,"d":"R 1,014.94"},{"v":1014.9361710349999,"d":"R 1,014.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.32000000000001,"d":"4.32"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1200mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil. cement is excluded","Each",{"v":840.9361710349999,"d":"R 840.94"},{"v":840.9361710349999,"d":"R 840.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.33000000000002,"d":"4.33"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1200mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":1014.9361710349999,"d":"R 1,014.94"},{"v":1014.9361710349999,"d":"R 1,014.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.34000000000002,"d":"4.34"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1800mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil. cement is excluded","Each",{"v":840.9361710349999,"d":"R 840.94"},{"v":840.9361710349999,"d":"R 840.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.35000000000002,"d":"4.35"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1800mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":1014.9361710349999,"d":"R 1,014.94"},{"v":1014.9361710349999,"d":"R 1,014.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.36000000000002,"d":"4.36"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1800mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1362.936171035,"d":"R 1,362.94"},{"v":1362.936171035,"d":"R 1,362.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.37000000000002,"d":"4.37"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 2000mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1362.936171035,"d":"R 1,362.94"},{"v":1362.936171035,"d":"R 1,362.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.38000000000002,"d":"4.38"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 2200mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1362.936171035,"d":"R 1,362.94"},{"v":1362.936171035,"d":"R 1,362.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":4.39000000000002,"d":"4.39"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 2500mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1362.936171035,"d":"R 1,362.94"},{"v":1362.936171035,"d":"R 1,362.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[5,null,"Heavy Conductor Concrete Poles "]
[5.1,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 700mm Diameter ","Each",{"v":249.59929728,"d":"R 249.60"},{"v":249.59929728,"d":"R 249.60"}]
[5.2,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 900mm Diameter ","Each",{"v":249.59929728,"d":"R 249.60"},{"v":249.59929728,"d":"R 249.60"}]
[5.3,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 1000mm Diameter ","Each",{"v":249.59929728,"d":"R 249.60"},{"v":249.59929728,"d":"R 249.60"}]
[5.4,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 1200mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil","Each",{"v":771.59929728,"d":"R 771.60"},{"v":771.59929728,"d":"R 771.60"}]
[5.5,"D-DT-0330 & 240-758831148","11m Pole Back-Actor or Hand - 1800mm Deep x 1200mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil","Each",{"v":945.59929728,"d":"R 945.60"},{"v":945.59929728,"d":"R 945.60"}]
[5.6,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 1250mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil. cement is excluded","Each",{"v":771.59929728,"d":"R 771.60"},{"v":771.59929728,"d":"R 771.60"},"Rate to low if supply of material(cement) is included. Description change in red"]
[5.7,"D-DT-0330 & 240-758831148","11m Pole Back-Actor or Hand - 1800mm Deep x 1250mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":771.59929728,"d":"R 771.60"},{"v":771.59929728,"d":"R 771.60"},"Rate to low if supply of material(cement) is included. Description change in red"]
[5.8,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 1500mm Diameter ","Each",{"v":771.59929728,"d":"R 771.60"},{"v":771.59929728,"d":"R 771.60"},"Rate to low if supply of material(cement) is included. Description change in red"]
[5.9,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 1500mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil. cement is excluded","Each",{"v":945.59929728,"d":"R 945.60"},{"v":945.59929728,"d":"R 945.60"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.1,"d":"5.10"},"D-DT-0330 & 240-758831148","11m Pole Back-Actor or Hand - 1800mm Deep x 1500mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":1321.34749502,"d":"R 1,321.35"},{"v":1321.34749502,"d":"R 1,321.35"},"Rate to low if supply of material(cement) is included. Description change in red"]
[5.11,"D-DT-0330","11m Pole Back-Actor or Hand - 1800mm Deep x 2000mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil","Each",{"v":1321.34749502,"d":"R 1,321.35"},{"v":1321.34749502,"d":"R 1,321.35"},"Rate to low if supply of material(cement) is included. Description change in red"]
[5.12,"D-DT-0330 & 240-758831148","11m Pole Back-Actor or Hand - 1800mm Deep x 2000mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":1321.34749502,"d":"R 1,321.35"},{"v":1321.34749502,"d":"R 1,321.35"},"Rate to low if supply of material(cement) is included. Description change in red"]
[5.13,"D-DT-0330 & 240-758831148","11m Pole Back-Actor or Hand - 1800mm Deep x 2000mm Diameter  Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1321.34749502,"d":"R 1,321.35"},{"v":1321.34749502,"d":"R 1,321.35"},"Rate to low if supply of material(cement) is included. Description change in red"]
[5.14,"D-DT-0330 & 240-758831148","11m Pole Back-Actor or Hand - 1800mm Deep x 2500mm Diameter  Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":308.1638833555555,"d":"R 308.16"},{"v":308.1638833555555,"d":"R 308.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[5.15,"D-DT-0330 & 240-758831148","11m Pole Back-Actor or Hand - 1800mm Deep x 3000mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":308.1638833555555,"d":"R 308.16"},{"v":308.1638833555555,"d":"R 308.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[5.16,"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 700mm Diameter ","Each",{"v":308.1638833555555,"d":"R 308.16"},{"v":308.1638833555555,"d":"R 308.16"}]
[5.17,"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 900mm Diameter ","Each",{"v":830.163883355556,"d":"R 830.16"},{"v":830.163883355556,"d":"R 830.16"}]
[{"v":5.18000000000001,"d":"5.18"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 1000mm Diameter ","Each",{"v":1004.163883355556,"d":"R 1,004.16"},{"v":1004.163883355556,"d":"R 1,004.16"}]
[{"v":5.19000000000001,"d":"5.19"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 1200mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil","Each",{"v":830.163883355556,"d":"R 830.16"},{"v":830.163883355556,"d":"R 830.16"}]
[{"v":5.20000000000001,"d":"5.20"},"D-DT-0330 & 240-758831148","12m Pole Back-Actor or Hand - 2000mm Deep x 1200mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":1004.163883355556,"d":"R 1,004.16"},{"v":1004.163883355556,"d":"R 1,004.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.21000000000001,"d":"5.21"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 1250mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil. cement is excluded","Each",{"v":830.163883355556,"d":"R 830.16"},{"v":830.163883355556,"d":"R 830.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.22000000000001,"d":"5.22"},"D-DT-0330 & 240-758831148","12m Pole Back-Actor or Hand - 2000mm Deep x 1250mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":1004.163883355556,"d":"R 1,004.16"},{"v":1004.163883355556,"d":"R 1,004.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.23000000000001,"d":"5.23"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 1500mm Diameter ","Each",{"v":1352.163883355556,"d":"R 1,352.16"},{"v":1352.163883355556,"d":"R 1,352.16"}]
[{"v":5.24000000000001,"d":"5.24"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 1500mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil","Each",{"v":1352.163883355556,"d":"R 1,352.16"},{"v":1352.163883355556,"d":"R 1,352.16"}]
[{"v":5.25000000000001,"d":"5.25"},"D-DT-0330 & 240-758831148","12m Pole Back-Actor or Hand - 2000mm Deep x 1500mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":1352.163883355556,"d":"R 1,352.16"},{"v":1352.163883355556,"d":"R 1,352.16"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.26000000000001,"d":"5.26"},"D-DT-0330","12m Pole Back-Actor or Hand - 2000mm Deep x 2000mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil","Each",{"v":1352.163883355556,"d":"R 1,352.16"},{"v":1352.163883355556,"d":"R 1,352.16"}]
[{"v":5.27000000000001,"d":"5.27"},"D-DT-0330 & 240-758831148","12m Pole Back-Actor or Hand - 2000mm Deep x 2000mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":318.936171035,"d":"R 318.94"},{"v":318.936171035,"d":"R 318.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.28000000000001,"d":"5.28"},"D-DT-0330 & 240-758831148","12m Pole Back-Actor or Hand - 2000mm Deep x 2000mm Diameter  Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":318.936171035,"d":"R 318.94"},{"v":318.936171035,"d":"R 318.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.29000000000001,"d":"5.29"},"D-DT-0330 & 240-758831148","12m Pole Back-Actor or Hand - 2000mm Deep x 2500mm Diameter  Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":318.936171035,"d":"R 318.94"},{"v":318.936171035,"d":"R 318.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.30000000000001,"d":"5.30"},"D-DT-0330 & 240-758831148","12m Pole Back-Actor or Hand - 2000mm Deep x 3000mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":840.9361710349999,"d":"R 840.94"},{"v":840.9361710349999,"d":"R 840.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.31000000000001,"d":"5.31"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 700mm Diameter ","Each",{"v":1014.9361710349999,"d":"R 1,014.94"},{"v":1014.9361710349999,"d":"R 1,014.94"}]
[{"v":5.32000000000001,"d":"5.32"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 900mm Diameter ","Each",{"v":840.9361710349999,"d":"R 840.94"},{"v":840.9361710349999,"d":"R 840.94"}]
[{"v":5.33000000000002,"d":"5.33"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1000mm Diameter ","Each",{"v":1014.9361710349999,"d":"R 1,014.94"},{"v":1014.9361710349999,"d":"R 1,014.94"}]
[{"v":5.34000000000002,"d":"5.34"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1200mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil. cement is excluded","Each",{"v":840.9361710349999,"d":"R 840.94"},{"v":840.9361710349999,"d":"R 840.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.35000000000002,"d":"5.35"},"D-DT-0330 & 240-758831148","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1200mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":1014.9361710349999,"d":"R 1,014.94"},{"v":1014.9361710349999,"d":"R 1,014.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.36000000000002,"d":"5.36"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1250mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil. cement is excluded","Each",{"v":1362.936171035,"d":"R 1,362.94"},{"v":1362.936171035,"d":"R 1,362.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.37000000000002,"d":"5.37"},"D-DT-0330 & 240-758831148","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1250mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":1362.936171035,"d":"R 1,362.94"},{"v":1362.936171035,"d":"R 1,362.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.38000000000002,"d":"5.38"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1500mm Diameter ","Each",{"v":1362.936171035,"d":"R 1,362.94"},{"v":1362.936171035,"d":"R 1,362.94"}]
[{"v":5.39000000000002,"d":"5.39"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1500mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil. cement is excluded","Each",{"v":1362.936171035,"d":"R 1,362.94"},{"v":1362.936171035,"d":"R 1,362.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.40000000000002,"d":"5.40"},"D-DT-0330 & 240-758831148","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 1500mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil. cement is excluded","Each",{"v":1362.936171035,"d":"R 1,362.94"},{"v":1362.936171035,"d":"R 1,362.94"}]
[{"v":5.41000000000002,"d":"5.41"},"D-DT-0330","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 2000mm Diameter - Add 6 Pockets of Cement to Moistened Excavated Soil. cement is excluded","Each",{"v":1362.936171035,"d":"R 1,362.94"},{"v":1362.936171035,"d":"R 1,362.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.42000000000002,"d":"5.42"},"D-DT-0330 & 240-758831148","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 2000mm Diameter - Clay and Turf - Add 8 Pockets of Cement to Moistened Imported Soil","Each",{"v":1362.936171035,"d":"R 1,362.94"},{"v":1362.936171035,"d":"R 1,362.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.43000000000002,"d":"5.43"},"D-DT-0330 & 240-758831148","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 2000mm Diameter  Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1362.936171035,"d":"R 1,362.94"},{"v":1362.936171035,"d":"R 1,362.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.44000000000002,"d":"5.44"},"D-DT-0330 & 240-758831148","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 2500mm Diameter  Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1362.936171035,"d":"R 1,362.94"},{"v":1362.936171035,"d":"R 1,362.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[{"v":5.45000000000002,"d":"5.45"},"D-DT-0330 & 240-758831148","13m - 14m Pole Back-Actor or Hand - 2200mm Deep x 3000mm Diameter - Add 12 Pockets of Cement to Moistened/Imported Excavated Soil. cement is excluded","Each",{"v":1362.936171035,"d":"R 1,362.94"},{"v":1362.936171035,"d":"R 1,362.94"},"Rate to low if supply of material(cement) is included. Description change in red"]
[6,null,"Free Standing Poles "]
[6.1,"2-WT/0000","9m Pole Free Standing 18kN Back-Actor or Hand (1.5m Deep) - Soil Type 1 & 2","Each",{"v":311.7460705883,"d":"R 311.75"},{"v":311.7460705883,"d":"R 311.75"}]
[6.2,"D-DT-1650","12m Pole Free Standing 8kN Back-Actor or Hand (2.5m Deep) - Soil Type 1 & 2","Each",{"v":311.7460705883,"d":"R 311.75"},{"v":311.7460705883,"d":"R 311.75"}]
[6.3,"D-DT-1650","12m Pole Free Standing 8kN Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":467.6191058824501,"d":"R 467.62"},{"v":467.6191058824501,"d":"R 467.62"}]
[6.4,"D-DT-1650","12m Pole Free Standing 8kN Back-Actor or Hand (2.5m Deep) - Soil Type 4","Each",{"v":623.4921411766002,"d":"R 623.49"},{"v":623.4921411766002,"d":"R 623.49"}]
[6.5,"D-DT-1651","12m Pole Free Standing 15kN Back-Actor or Hand (2.5m Deep) - Soil Type 1 & 2","Each",{"v":584.5238823530626,"d":"R 584.52"},{"v":584.5238823530626,"d":"R 584.52"}]
[6.6,"D-DT-1651","12m Pole Free Standing 15kN Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":876.7858235295939,"d":"R 876.79"},{"v":876.7858235295939,"d":"R 876.79"}]
[6.7,"D-DT-1651","12m Pole Free Standing 15kN Back-Actor or Hand (2.5m Deep) - Soil Type 4","Each",{"v":1169.0477647061252,"d":"R 1,169.05"},{"v":1169.0477647061252,"d":"R 1,169.05"}]
[6.8,"D-DT-1652","12m Pole Free Standing 27kN Back-Actor or Hand (2.5m Deep) - Soil Type 1 & 2","Each",{"v":1052.1429882355128,"d":"R 1,052.14"},{"v":1052.1429882355128,"d":"R 1,052.14"}]
[6.9,"D-DT-1652","12m Pole Free Standing 27kN Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":1578.2144823532692,"d":"R 1,578.21"},{"v":1578.2144823532692,"d":"R 1,578.21"}]
[{"v":6.1,"d":"6.10"},"D-DT-1652","12m Pole Free Standing 27kN Back-Actor or Hand (2.5m Deep) - Soil Type 4","Each",{"v":2104.2859764710256,"d":"R 2,104.29"},{"v":2104.2859764710256,"d":"R 2,104.29"}]
[6.11,"D-DT-1653","12m Pole Free Standing 42kN Back-Actor or Hand (2.5m Deep) - Soil Type 1","Each",{"v":1636.6668705885754,"d":"R 1,636.67"},{"v":1636.6668705885754,"d":"R 1,636.67"}]
[6.12,"D-DT-1653","12m Pole Free Standing 42kN Back-Actor or Hand (2.5m Deep) - Soil Type 2","Each",{"v":1636.6668705885754,"d":"R 1,636.67"},{"v":1636.6668705885754,"d":"R 1,636.67"}]
[6.13,"D-DT-1653","12m Pole Free Standing 42kN Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":2455.0003058828634,"d":"R 2,455.00"},{"v":2455.0003058828634,"d":"R 2,455.00"}]
[6.14,"D-DT-1653","12m Pole Free Standing 42kN Back-Actor or Hand (2.5m Deep) - Soil Type 4","Each",{"v":3273.333741177151,"d":"R 3,273.33"},{"v":3273.333741177151,"d":"R 3,273.33"}]
[6.15,"D-DT-1654","12m Pole Free Standing 58kN Back-Actor or Hand (2.5m Deep) - Soil Type 1","Each",{"v":2260.159011765176,"d":"R 2,260.16"},{"v":2260.159011765176,"d":"R 2,260.16"}]
[6.16,"D-DT-1654","12m Pole Free Standing 58kN Back-Actor or Hand (2.5m Deep) - Soil Type 2","Each",{"v":2260.159011765176,"d":"R 2,260.16"},{"v":2260.159011765176,"d":"R 2,260.16"}]
[6.17,"D-DT-1654","12m Pole Free Standing 58kN Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":3390.2385176477637,"d":"R 3,390.24"},{"v":3390.2385176477637,"d":"R 3,390.24"}]
[{"v":6.18000000000001,"d":"6.18"},"D-DT-1654","12m Pole Free Standing 58kN Back-Actor or Hand (2.5m Deep) - Soil Type 4","Each",{"v":3390.2385176477637,"d":"R 3,390.24"},{"v":3390.2385176477637,"d":"R 3,390.24"}]
[6.19000000000001,"D-DT-1655","12m Pole Free Standing Terminal Back-Actor or Hand (2.5m Deep) - Soil Type 1","Each",{"v":311.7460705883,"d":"R 311.75"},{"v":311.7460705883,"d":"R 311.75"}]
[{"v":6.20000000000001,"d":"6.20"},"D-DT-1655","12m Pole Free Standing Terminal Back-Actor or Hand (2.5m Deep) - Soil Type 2","Each",{"v":311.7460705883,"d":"R 311.75"},{"v":311.7460705883,"d":"R 311.75"}]
[6.21000000000001,"D-DT-1655","12m Pole Free Standing Terminal Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":467.6191058824501,"d":"R 467.62"},{"v":467.6191058824501,"d":"R 467.62"}]
[{"v":6.22000000000001,"d":"6.22"},"D-DT-1655","12m Pole Free Standing Terminal Back-Actor or Hand (2.5m Deep) - Soil Type 4","Each",{"v":623.4921411766002,"d":"R 623.49"},{"v":623.4921411766002,"d":"R 623.49"}]
[6.23000000000001,"D-DT-1656","12m Pole Free Standing 73kN Back-Actor or Hand (2.5m Deep) - Soil Type 1","Each",{"v":2844.682894118237,"d":"R 2,844.68"},{"v":2844.682894118237,"d":"R 2,844.68"}]
[{"v":6.24000000000001,"d":"6.24"},"D-DT-1656","12m Pole Free Standing 73kN Back-Actor or Hand (2.5m Deep) - Soil Type 2","Each",{"v":2844.682894118237,"d":"R 2,844.68"},{"v":2844.682894118237,"d":"R 2,844.68"}]
[6.25000000000001,"D-DT-1656","12m Pole Free Standing 73kN Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":4267.024341177355,"d":"R 4,267.02"},{"v":4267.024341177355,"d":"R 4,267.02"}]
[{"v":6.26000000000001,"d":"6.26"},"D-DT-1656","12m Pole Free Standing 73kN Back-Actor or Hand (2.5m Deep) - Soil Type 4","Each",{"v":4267.024341177355,"d":"R 4,267.02"},{"v":4267.024341177355,"d":"R 4,267.02"}]
[6.27000000000001,"D-DT-1657","12m Pole Free Standing 106kN Back-Actor or Hand (2.5m Deep) - Soil Type 1","Each",{"v":4130.635435294975,"d":"R 4,130.64"},{"v":4130.635435294975,"d":"R 4,130.64"}]
[{"v":6.28000000000001,"d":"6.28"},"D-DT-1657","12m Pole Free Standing 106kN Back-Actor or Hand (2.5m Deep) - Soil Type 2","Each",{"v":4130.635435294975,"d":"R 4,130.64"},{"v":4130.635435294975,"d":"R 4,130.64"}]
[6.29000000000001,"D-DT-1657","12m Pole Free Standing 106kN Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":6195.953152942462,"d":"R 6,195.95"},{"v":6195.953152942462,"d":"R 6,195.95"}]
[{"v":6.30000000000001,"d":"6.30"},"D-DT-1650","13m Pole Free Standing 8kN Back-Actor or Hand (2.5m Deep) - Soil Type 1 & 2","Each",{"v":311.7460705883,"d":"R 311.75"},{"v":311.7460705883,"d":"R 311.75"}]
[6.31000000000001,"D-DT-1650","13m Pole Free Standing 8kN Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":467.6191058824501,"d":"R 467.62"},{"v":467.6191058824501,"d":"R 467.62"}]
[{"v":6.32000000000001,"d":"6.32"},"D-DT-1650","13m Pole Free Standing 8kN Back-Actor or Hand (2.5m Deep) - Soil Type 4","Each",{"v":623.4921411766002,"d":"R 623.49"},{"v":623.4921411766002,"d":"R 623.49"}]
[6.33000000000002,"D-DT-1651","13m Pole Free Standing 15kN Back-Actor or Hand (2.5m Deep) - Soil Type 1 & 2","Each",{"v":584.5238823530626,"d":"R 584.52"},{"v":584.5238823530626,"d":"R 584.52"}]
[{"v":6.34000000000002,"d":"6.34"},"D-DT-1651","13m Pole Free Standing 15kN Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":876.7858235295939,"d":"R 876.79"},{"v":876.7858235295939,"d":"R 876.79"}]
[6.35000000000002,"D-DT-1651","13m Pole Free Standing 15kN Back-Actor or Hand (2.5m Deep) - Soil Type 4","Each",{"v":1169.0477647061252,"d":"R 1,169.05"},{"v":1169.0477647061252,"d":"R 1,169.05"}]
[{"v":6.36000000000002,"d":"6.36"},"D-DT-1652","13m Pole Free Standing 27kN Back-Actor or Hand (2.5m Deep) - Soil Type 1 & 2","Each",{"v":1052.1429882355128,"d":"R 1,052.14"},{"v":1052.1429882355128,"d":"R 1,052.14"}]
[6.37000000000002,"D-DT-1652","13m Pole Free Standing 27kN Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":1578.2144823532692,"d":"R 1,578.21"},{"v":1578.2144823532692,"d":"R 1,578.21"}]
[{"v":6.38000000000002,"d":"6.38"},"D-DT-1652","13m Pole Free Standing 27kN Back-Actor or Hand (2.5m Deep) - Soil Type 4","Each",{"v":2104.2859764710256,"d":"R 2,104.29"},{"v":2104.2859764710256,"d":"R 2,104.29"}]
[6.39000000000002,"D-DT-1653","13m Pole Free Standing 42kN Back-Actor or Hand (2.5m Deep) - Soil Type 1","Each",{"v":1636.6668705885754,"d":"R 1,636.67"},{"v":1636.6668705885754,"d":"R 1,636.67"}]
[{"v":6.40000000000002,"d":"6.40"},"D-DT-1653","13m Pole Free Standing 42kN Back-Actor or Hand (2.5m Deep) - Soil Type 2","Each",{"v":1636.6668705885754,"d":"R 1,636.67"},{"v":1636.6668705885754,"d":"R 1,636.67"}]
[6.41000000000002,"D-DT-1653","13m Pole Free Standing 42kN Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":2455.0003058828634,"d":"R 2,455.00"},{"v":2455.0003058828634,"d":"R 2,455.00"}]
[{"v":6.42000000000002,"d":"6.42"},"D-DT-1653","13m Pole Free Standing 42kN Back-Actor or Hand (2.5m Deep) - Soil Type 4","Each",{"v":3273.333741177151,"d":"R 3,273.33"},{"v":3273.333741177151,"d":"R 3,273.33"}]
[6.43000000000002,"D-DT-1654","13m Pole Free Standing 58kN Back-Actor or Hand (2.5m Deep) - Soil Type 1","Each",{"v":2260.159011765176,"d":"R 2,260.16"},{"v":2260.159011765176,"d":"R 2,260.16"}]
[{"v":6.44000000000002,"d":"6.44"},"D-DT-1654","13m Pole Free Standing 58kN Back-Actor or Hand (2.5m Deep) - Soil Type 2","Each",{"v":2260.159011765176,"d":"R 2,260.16"},{"v":2260.159011765176,"d":"R 2,260.16"}]
[6.45000000000002,"D-DT-1654","13m Pole Free Standing 58kN Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":3390.2385176477637,"d":"R 3,390.24"},{"v":3390.2385176477637,"d":"R 3,390.24"}]
[{"v":6.46000000000002,"d":"6.46"},"D-DT-1654","13m Pole Free Standing 58kN Back-Actor or Hand (2.5m Deep) - Soil Type 4","Each",{"v":3390.2385176477637,"d":"R 3,390.24"},{"v":3390.2385176477637,"d":"R 3,390.24"}]
[6.47000000000002,"D-DT-1655","13m Pole Free Standing Terminal Back-Actor or Hand (2.5m Deep) - Soil Type 1","Each",{"v":311.7460705883,"d":"R 311.75"},{"v":311.7460705883,"d":"R 311.75"}]
[{"v":6.48000000000003,"d":"6.48"},"D-DT-1655","13m Pole Free Standing Terminal Back-Actor or Hand (2.5m Deep) - Soil Type 2","Each",{"v":311.7460705883,"d":"R 311.75"},{"v":311.7460705883,"d":"R 311.75"}]
[6.49000000000003,"D-DT-1655","13m Pole Free Standing Terminal Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":467.6191058824501,"d":"R 467.62"},{"v":467.6191058824501,"d":"R 467.62"}]
[{"v":6.50000000000003,"d":"6.50"},"D-DT-1655","13m Pole Free Standing Terminal Back-Actor or Hand (2.5m Deep) - Soil Type 4","Each",{"v":623.4921411766002,"d":"R 623.49"},{"v":623.4921411766002,"d":"R 623.49"}]
[6.51000000000003,"D-DT-1656","13m Pole Free Standing 73kN Back-Actor or Hand (2.5m Deep) - Soil Type 1","Each",{"v":2844.682894118237,"d":"R 2,844.68"},{"v":2844.682894118237,"d":"R 2,844.68"}]
[{"v":6.52000000000003,"d":"6.52"},"D-DT-1656","13m Pole Free Standing 73kN Back-Actor or Hand (2.5m Deep) - Soil Type 2","Each",{"v":2844.682894118237,"d":"R 2,844.68"},{"v":2844.682894118237,"d":"R 2,844.68"}]
[6.53000000000003,"D-DT-1656","13m Pole Free Standing 73kN Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":4267.024341177355,"d":"R 4,267.02"},{"v":4267.024341177355,"d":"R 4,267.02"}]
[{"v":6.54000000000003,"d":"6.54"},"D-DT-1656","13m Pole Free Standing 73kN Back-Actor or Hand (2.5m Deep) - Soil Type 4","Each",{"v":4267.024341177355,"d":"R 4,267.02"},{"v":4267.024341177355,"d":"R 4,267.02"}]
[6.55000000000003,"D-DT-1657","13m Pole Free Standing 106kN Back-Actor or Hand (2.5m Deep) - Soil Type 1","Each",{"v":4130.635435294975,"d":"R 4,130.64"},{"v":4130.635435294975,"d":"R 4,130.64"}]
[{"v":6.56000000000003,"d":"6.56"},"D-DT-1657","13m Pole Free Standing 106kN Back-Actor or Hand (2.5m Deep) - Soil Type 2","Each",{"v":4130.635435294975,"d":"R 4,130.64"},{"v":4130.635435294975,"d":"R 4,130.64"}]
[6.57000000000003,"D-DT-1657","13m Pole Free Standing 106kN Back-Actor or Hand (2.5m Deep) - Soil Type 3","Each",{"v":6195.953152942462,"d":"R 6,195.95"},{"v":6195.953152942462,"d":"R 6,195.95"}]
["SUB-TOTAL C"]
["D",null,"PLANTING OF POLES"]
["Planting including backfilling and compaction are measured here.  The costs are also inclusive of plant and equipment required to plant the Structures. Stay, Struts and Flying Stay are elsewhere measured. All backfill material included in price. Any other soil type claimed than specified by designer to be supported by DCP soil clasification test completed by the contractor and reviewed by the designer according to 240-75883148 annex A. (At least 60% of tested hole must be the soil type claimed to be approved)",{"$nulls":5},"Description changed in red"]
[1,null," Soil Type 1"]
[1.1,"D-DT-0058","5m Wooden Pole 80-100mm Top Diameter Soil Type 1","Each",{"v":126.518781731,"d":"R 126.52"},{"v":126.518781731,"d":"R 126.52"}]
[1.2,"D-DT-0058","5m Wooden Pole 80-100mm Top Diameter Soil Type 2","Each",{"v":358.15,"d":"R 358.15"},{"v":358.15,"d":"R 358.15"},"Why such a big difference between 5m type 1 and 2 and not between 9m type 1 and 2. Re-look at these rates or claritiy needed for this item."]
[1.3,"D-DT-0058","5m Wooden Pole 80-100mm Top Diameter Soil Type 3","Each",{"v":991.61,"d":"R 991.61"},{"v":991.61,"d":"R 991.61"}]
[1.4,"D-DT-0058","5m Wooden Pole 80-100mm Top Diameter Soil Type 4","Each",{"v":879.61,"d":"R 879.61"},{"v":879.61,"d":"R 879.61"}]
[1.5,"D-DT-0066","6m Wooden Pole/X-Arm 160-179 Top Diameter Soil Type 1","Each",{"v":151.8225380772,"d":"R 151.82"},{"v":151.8225380772,"d":"R 151.82"}]
[1.6,"D-DT-0066","6m Wooden Pole/X-Arm 160-179 Top Diameter Soil Type 2","Each",{"v":204.96,"d":"R 204.96"},{"v":204.96,"d":"R 204.96"}]
[1.7,"D-DT-0066","6m Wooden Pole/X-Arm 160-179 Top Diameter Soil Type 3","Each",{"v":1388.24,"d":"R 1,388.24"},{"v":1388.24,"d":"R 1,388.24"}]
[1.8,"D-DT-0066","6m Wooden Pole/X-Arm 160-179 Top Diameter Soil Type 4","Each",{"v":1055.52,"d":"R 1,055.52"},{"v":1055.52,"d":"R 1,055.52"}]
[1.9,"D-DT-0050","7m Wooden Pole 100-120mm Top Diameter Soil Type 1","Each",{"v":151.81200362410002,"d":"R 151.81"},{"v":151.81200362410002,"d":"R 151.81"}]
[{"v":1.1,"d":"1.10"},"D-DT-0050","7m Wooden Pole 100-120mm Top Diameter Soil Type 2","Each",{"v":204.95,"d":"R 204.95"},{"v":204.95,"d":"R 204.95"}]
[1.11,"D-DT-0050","7m Wooden Pole 100-120mm Top Diameter Soil Type 3","Each",{"v":1388.24,"d":"R 1,388.24"},{"v":1388.24,"d":"R 1,388.24"}]
[1.12,"D-DT-0050","7m Wooden Pole 100-120mm Top Diameter Soil Type 4","Each",{"v":1231.44,"d":"R 1,231.44"},{"v":1231.44,"d":"R 1,231.44"}]
[1.13,"D-DT-0050","7m Wooden Pole 120-139mm Top Diameter Soil Type 1","Each",{"v":177.1157599703,"d":"R 177.12"},{"v":177.1157599703,"d":"R 177.12"}]
[1.14,"D-DT-0050","7m Wooden Pole 120-139mm Top Diameter Soil Type 2","Each",{"v":239.11,"d":"R 239.11"},{"v":239.11,"d":"R 239.11"}]
[1.15,"D-DT-0050","7m Wooden Pole 120-139mm Top Diameter Soil Type 3","Each",{"v":1388.24,"d":"R 1,388.24"},{"v":1388.24,"d":"R 1,388.24"}]
[1.16,"D-DT-0050","7m Wooden Pole 120-139mm Top Diameter Soil Type 4","Each",{"v":1231.44,"d":"R 1,231.44"},{"v":1231.44,"d":"R 1,231.44"}]
[1.17,"D-DT-1866","8m Wooden Pole/X-Arm 160-179 Top Diameter Soil Type 1","Each",{"v":202.4300507696,"d":"R 202.43"},{"v":202.4300507696,"d":"R 202.43"}]
[1.18,"D-DT-0050","8m Wooden Pole/X-Arm 160-179 Top Diameter Soil Type 2","Each",{"v":273.28,"d":"R 273.28"},{"v":273.28,"d":"R 273.28"}]
[1.19,"D-DT-0050","8m Wooden Pole/X-Arm 160-179 Top Diameter Soil Type 3","Each",{"v":1586.56,"d":"R 1,586.56"},{"v":1586.56,"d":"R 1,586.56"}]
[{"v":1.2,"d":"1.20"},"D-DT-0050","8m Wooden Pole/X-Arm 160-179 Top Diameter Soil Type 4","Each",{"v":1407.36,"d":"R 1,407.36"},{"v":1407.36,"d":"R 1,407.36"}]
[1.21,"D-DT-0055","9m Wooden Pole 140-159mm Top Diameter Soil Type 1","Each",{"v":217.8208867487,"d":"R 217.82"},{"v":217.8208867487,"d":"R 217.82"}]
[1.22,"D-DT-0055","9m Wooden Pole 140-159mm Top Diameter Soil Type 2","Each",{"v":294.06,"d":"R 294.06"},{"v":294.06,"d":"R 294.06"}]
[1.23,"D-DT-0055","9m Wooden Pole 140-159mm Top Diameter Soil Type 3","Each",{"v":1784.88,"d":"R 1,784.88"},{"v":1784.88,"d":"R 1,784.88"}]
[1.24,"D-DT-0055","9m Wooden Pole 140-159mm Top Diameter Soil Type 4","Each",{"v":1583.28,"d":"R 1,583.28"},{"v":1583.28,"d":"R 1,583.28"}]
[1.25,"D-DT-0055","9m Wooden Pole  160-179 mm Top Diameter Soil Type 1","Each",{"v":245.0524480122,"d":"R 245.05"},{"v":245.0524480122,"d":"R 245.05"}]
[1.26,"D-DT-0055","9m Wooden Pole  160-179 mm Top Diameter Soil Type 2","Each",{"v":330.82,"d":"R 330.82"},{"v":330.82,"d":"R 330.82"}]
[1.27,"D-DT-0055","9m Wooden Pole  160-179 mm Top Diameter Soil Type 3","Each",{"v":1784.88,"d":"R 1,784.88"},{"v":1784.88,"d":"R 1,784.88"}]
[1.28,"D-DT-0055","9m Wooden Pole  160-179 mm Top Diameter Soil Type 4","Each",{"v":1583.28,"d":"R 1,583.28"},{"v":1583.28,"d":"R 1,583.28"}]
[1.29,"D-DT-0055","9m Wooden Pole 180-199mm Top Diameter Soil Type 1","Each",{"v":272.28400927570004,"d":"R 272.28"},{"v":272.28400927570004,"d":"R 272.28"}]
[{"v":1.3,"d":"1.30"},"D-DT-0055","9m Wooden Pole 180-199mm Top Diameter Soil Type 2","Each",{"v":367.58,"d":"R 367.58"},{"v":367.58,"d":"R 367.58"}]
[1.31,"D-DT-0055","9m Wooden Pole 180-199mm Top Diameter Soil Type 3","Each",{"v":1784.88,"d":"R 1,784.88"},{"v":1784.88,"d":"R 1,784.88"}]
[1.32,"D-DT-0055","9m Wooden Pole 180-199mm Top Diameter Soil Type 4","Each",{"v":1583.28,"d":"R 1,583.28"},{"v":1583.28,"d":"R 1,583.28"}]
[1.33,"D-DT-0052","10m Wooden Pole 160-179mm Top Diameter H4 Soil Type 1","Each",{"v":255.04964400410003,"d":"R 255.05"},{"v":255.04964400410003,"d":"R 255.05"}]
[1.34,"D-DT-0052","10m Wooden Pole 160-179mm Top Diameter H4 Soil Type 2","Each",{"v":344.32,"d":"R 344.32"},{"v":344.32,"d":"R 344.32"}]
[1.35,"D-DT-0052","10m Wooden Pole 160-179mm Top Diameter H4 Soil Type 3","Each",{"v":1983.2,"d":"R 1,983.20"},{"v":1983.2,"d":"R 1,983.20"}]
[1.36,"D-DT-0052","10m Wooden Pole 160-179mm Top Diameter H4 Soil Type 4","Each",{"v":1759.2,"d":"R 1,759.20"},{"v":1759.2,"d":"R 1,759.20"}]
[1.37,"D-DT-0052","10m Wooden Pole 160-179mm Top Diameter H5 Soil Type 1","Each",{"v":255.04964400410003,"d":"R 255.05"},{"v":255.04964400410003,"d":"R 255.05"}]
[1.38,"D-DT-0052","10m Wooden Pole 160-179mm Top Diameter H5 Soil Type 2","Each",{"v":344.32,"d":"R 344.32"},{"v":344.32,"d":"R 344.32"}]
[1.39,"D-DT-0052","10m Wooden Pole 160-179mm Top Diameter H5 Soil Type 3","Each",{"v":1983.2,"d":"R 1,983.20"},{"v":1983.2,"d":"R 1,983.20"}]
[{"v":1.4,"d":"1.40"},"D-DT-0052","10m Wooden Pole 160-179mm Top Diameter H5 Soil Type 4","Each",{"v":1759.2,"d":"R 1,759.20"},{"v":1759.2,"d":"R 1,759.20"}]
[1.41,"D-DT-0052","10m Wooden Pole 180-199mm Top Diameter H4 Soil Type 1","Each",{"v":283.3873228431,"d":"R 283.39"},{"v":283.3873228431,"d":"R 283.39"}]
[1.42,"D-DT-0052","10m Wooden Pole 180-199mm Top Diameter H4 Soil Type 2","Each",{"v":382.57,"d":"R 382.57"},{"v":382.57,"d":"R 382.57"}]
[1.43,"D-DT-0052","10m Wooden Pole 180-199mm Top Diameter H4 Soil Type 3","Each",{"v":1983.2,"d":"R 1,983.20"},{"v":1983.2,"d":"R 1,983.20"}]
[1.44,"D-DT-0052","10m Wooden Pole 180-199mm Top Diameter H4 Soil Type 4","Each",{"v":1759.2,"d":"R 1,759.20"},{"v":1759.2,"d":"R 1,759.20"}]
[1.45,"D-DT-0052","10m Wooden Pole 180-199mm Top Diameter H5 Soil Type 1","Each",{"v":283.3873228431,"d":"R 283.39"},{"v":283.3873228431,"d":"R 283.39"}]
[1.46,"D-DT-0052","10m Wooden Pole 180-199mm Top Diameter H5 Soil Type 2","Each",{"v":238.57,"d":"R 238.57"},{"v":238.57,"d":"R 238.57"}]
[1.47,"D-DT-0052","10m Wooden Pole 180-199mm Top Diameter H5 Soil Type 3","Each",{"v":1983.2,"d":"R 1,983.20"},{"v":1983.2,"d":"R 1,983.20"}]
[1.48,"D-DT-0052","10m Wooden Pole 180-199mm Top Diameter H5 Soil Type 4","Each",{"v":1759.2,"d":"R 1,759.20"},{"v":1759.2,"d":"R 1,759.20"}]
[1.49,"D-DT-0052","10m Wooden Pole 200-219mm Top Diameter H4 Soil Type 1","Each",{"v":311.73553613520005,"d":"R 311.74"},{"v":311.73553613520005,"d":"R 311.74"}]
[{"v":1.5,"d":"1.50"},"D-DT-0052","10m Wooden Pole 200-219mm Top Diameter H4 Soil Type 2","Each",{"v":420.84,"d":"R 420.84"},{"v":420.84,"d":"R 420.84"}]
[1.51,"D-DT-0052","10m Wooden Pole 200-219mm Top Diameter H4 Soil Type 3","Each",{"v":1983.2,"d":"R 1,983.20"},{"v":1983.2,"d":"R 1,983.20"}]
[1.52,"D-DT-0052","10m Wooden Pole 200-219mm Top Diameter H4 Soil Type 4","Each",{"v":1759.2,"d":"R 1,759.20"},{"v":1759.2,"d":"R 1,759.20"}]
[1.53,"D-DT-0052","10m Wooden Pole 200-219mm Top Diameter H5 Soil Type 1","Each",{"v":311.73553613520005,"d":"R 311.74"},{"v":311.73553613520005,"d":"R 311.74"}]
[1.54,"D-DT-0052","10m Wooden Pole 200-219mm Top Diameter H5 Soil Type 2","Each",{"v":420.84,"d":"R 420.84"},{"v":420.84,"d":"R 420.84"}]
[1.55,"D-DT-0052","10m Wooden Pole 200-219mm Top Diameter H5 Soil Type 3","Each",{"v":1983.2,"d":"R 1,983.20"},{"v":1983.2,"d":"R 1,983.20"}]
[1.56,"D-DT-0052","10m Wooden Pole 200-219mm Top Diameter H5 Soil Type 4","Each",{"v":1759.2,"d":"R 1,759.20"},{"v":1759.2,"d":"R 1,759.20"}]
[1.57,"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter H4 Soil Type 1","Each",{"v":274.2328830992,"d":"R 274.23"},{"v":274.2328830992,"d":"R 274.23"}]
[1.58,"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter H4 Soil Type 2","Each",{"v":370.21,"d":"R 370.21"},{"v":370.21,"d":"R 370.21"}]
[1.59,"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter H4 Soil Type 3","Each",{"v":2181.52,"d":"R 2,181.52"},{"v":2181.52,"d":"R 2,181.52"}]
[{"v":1.6,"d":"1.60"},"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter H4 Soil Type 4","Each",{"v":1935.12,"d":"R 1,935.12"},{"v":1935.12,"d":"R 1,935.12"}]
[1.61,"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter 75MPA H4 Soil Type 1","Each",{"v":274.2328830992,"d":"R 274.23"},{"v":274.2328830992,"d":"R 274.23"}]
[1.62,"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter 75MPA H4 Soil Type 2","Each",{"v":370.21,"d":"R 370.21"},{"v":370.21,"d":"R 370.21"}]
[1.63,"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter 75MPA H4 Soil Type 3","Each",{"v":2181.52,"d":"R 2,181.52"},{"v":2181.52,"d":"R 2,181.52"}]
[1.64,"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter 75MPA H4 Soil Type 4","Each",{"v":1935.12,"d":"R 1,935.12"},{"v":1935.12,"d":"R 1,935.12"}]
[1.65,"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter H5 Soil Type 1","Each",{"v":274.2328830992,"d":"R 274.23"},{"v":274.2328830992,"d":"R 274.23"}]
[1.66,"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter H5 Soil Type 2","Each",{"v":370.21,"d":"R 370.21"},{"v":370.21,"d":"R 370.21"}]
[1.67,"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter H5 Soil Type 3","Each",{"v":2181.52,"d":"R 2,181.52"},{"v":2181.52,"d":"R 2,181.52"}]
[1.68,"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter H5 Soil Type 4","Each",{"v":1935.12,"d":"R 1,935.12"},{"v":1935.12,"d":"R 1,935.12"}]
[1.69,"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter 75MPA H5 Soil Type 1","Each",{"v":308.5119934866,"d":"R 308.51"},{"v":308.5119934866,"d":"R 308.51"}]
[{"v":1.7,"d":"1.70"},"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter 75MPA H5 Soil Type 2","Each",{"v":416.49,"d":"R 416.49"},{"v":416.49,"d":"R 416.49"}]
[1.71,"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter 75MPA H5 Soil Type 3","Each",{"v":2181.52,"d":"R 2,181.52"},{"v":2181.52,"d":"R 2,181.52"}]
[1.72,"D-DT-0051","11m Wooden Pole 140-159mm Top Diameter 75MPA H5 Soil Type 4","Each",{"v":1935.12,"d":"R 1,935.12"},{"v":1935.12,"d":"R 1,935.12"}]
[1.73,"D-DT-0051","11m Wooden Pole 160-179mm Top Diameter H4 Soil Type 1","Each",{"v":308.5119934866,"d":"R 308.51"},{"v":308.5119934866,"d":"R 308.51"}]
[1.74,"D-DT-0051","11m Wooden Pole 160-179mm Top Diameter H4 Soil Type 2","Each",{"v":416.49,"d":"R 416.49"},{"v":416.49,"d":"R 416.49"}]
[1.75,"D-DT-0051","11m Wooden Pole 160-179mm Top Diameter H4 Soil Type 3","Each",{"v":2181.52,"d":"R 2,181.52"},{"v":2181.52,"d":"R 2,181.52"}]
[1.76,"D-DT-0051","11m Wooden Pole 160-179mm Top Diameter H4 Soil Type 4","Each",{"v":1935.12,"d":"R 1,935.12"},{"v":1935.12,"d":"R 1,935.12"}]
[1.77,"D-DT-0051","11m Wooden Pole 180-199mm Top Diameter H4 Soil Type 1","Each",{"v":342.791103874,"d":"R 342.79"},{"v":342.791103874,"d":"R 342.79"}]
[1.78,"D-DT-0051","11m Wooden Pole 180-199mm Top Diameter H4 Soil Type 2","Each",{"v":462.77,"d":"R 462.77"},{"v":462.77,"d":"R 462.77"}]
[1.79,"D-DT-0051","11m Wooden Pole 180-199mm Top Diameter H4 Soil Type 3","Each",{"v":2181.52,"d":"R 2,181.52"},{"v":2181.52,"d":"R 2,181.52"}]
[{"v":1.8,"d":"1.80"},"D-DT-0051","11m Wooden Pole 180-199mm Top Diameter H4 Soil Type 4","Each",{"v":1935.12,"d":"R 1,935.12"},{"v":1935.12,"d":"R 1,935.12"}]
[1.81,"D-DT-0051","11m Wooden Pole 200-219mm Top Diameter H4 Soil Type 1","Each",{"v":377.0702142614,"d":"R 377.07"},{"v":377.0702142614,"d":"R 377.07"}]
[1.82,"D-DT-0051","11m Wooden Pole 200-219mm Top Diameter H4 Soil Type 2","Each",{"v":509.04,"d":"R 509.04"},{"v":509.04,"d":"R 509.04"}]
[1.83,"D-DT-0051","11m Wooden Pole 200-219mm Top Diameter H4 Soil Type 3","Each",{"v":2181.52,"d":"R 2,181.52"},{"v":2181.52,"d":"R 2,181.52"}]
[1.84,"D-DT-0051","11m Wooden Pole 200-219mm Top Diameter H4 Soil Type 4","Each",{"v":1935.12,"d":"R 1,935.12"},{"v":1935.12,"d":"R 1,935.12"}]
[1.85,"D-DT-0053","12m Wooden Pole 160-179mm Top Diameter Soil Type 1","Each",{"v":307.4901515359,"d":"R 307.49"},{"v":307.4901515359,"d":"R 307.49"}]
[1.86,"D-DT-0053","12m Wooden Pole 160-179mm Top Diameter Soil Type 2","Each",{"v":415.11,"d":"R 415.11"},{"v":415.11,"d":"R 415.11"}]
[1.87,"D-DT-0053","12m Wooden Pole 160-179mm Top Diameter Soil Type 3","Each",{"v":2379.84,"d":"R 2,379.84"},{"v":2379.84,"d":"R 2,379.84"}]
[1.88,"D-DT-0053","12m Wooden Pole 160-179mm Top Diameter Soil Type 4","Each",{"v":2111.04,"d":"R 2,111.04"},{"v":2111.04,"d":"R 2,111.04"}]
[1.89,"D-DT-0053","12m Wooden Pole 180-199mm Top Diameter Soil Type 1","Each",{"v":341.6639173923,"d":"R 341.66"},{"v":341.6639173923,"d":"R 341.66"}]
[{"v":1.9,"d":"1.90"},"D-DT-0053","12m Wooden Pole 180-199mm Top Diameter Soil Type 2","Each",{"v":461.25,"d":"R 461.25"},{"v":461.25,"d":"R 461.25"}]
[1.91,"D-DT-0053","12m Wooden Pole 180-199mm Top Diameter Soil Type 3","Each",{"v":2379.84,"d":"R 2,379.84"},{"v":2379.84,"d":"R 2,379.84"}]
[1.92,"D-DT-0053","12m Wooden Pole 180-199mm Top Diameter Soil Type 4","Each",{"v":2111.04,"d":"R 2,111.04"},{"v":2111.04,"d":"R 2,111.04"}]
[1.93,"D-DT-0053","12m Wooden Pole 200-219mm Top Diameter Soil Type 1","Each",{"v":375.8271487956,"d":"R 375.83"},{"v":375.8271487956,"d":"R 375.83"}]
[1.94,"D-DT-0053","12m Wooden Pole 200-219mm Top Diameter Soil Type 2","Each",{"v":507.37,"d":"R 507.37"},{"v":507.37,"d":"R 507.37"}]
[1.95,"D-DT-0053","12m Wooden Pole 200-219mm Top Diameter Soil Type 3","Each",{"v":2379.84,"d":"R 2,379.84"},{"v":2379.84,"d":"R 2,379.84"}]
[1.96,"D-DT-0053","12m Wooden Pole 200-219mm Top Diameter Soil Type 4","Each",{"v":2111.04,"d":"R 2,111.04"},{"v":2111.04,"d":"R 2,111.04"}]
[1.97,"D-DT-0056","13m Wooden Pole 160-179mm Top Diameter H4 Soil Type 1","Each",{"v":337.32372271509996,"d":"R 337.32"},{"v":337.32372271509996,"d":"R 337.32"}]
[1.98,"D-DT-0056","13m Wooden Pole 160-179mm Top Diameter H4 Soil Type 2","Each",{"v":455.39,"d":"R 455.39"},{"v":455.39,"d":"R 455.39"}]
[1.99,"D-DT-0056","13m Wooden Pole 160-179mm Top Diameter H4 Soil Type 3","Each",{"v":2578.16,"d":"R 2,578.16"},{"v":2578.16,"d":"R 2,578.16"}]
[{"v":1.1,"d":"1.100"},"D-DT-0056","13m Wooden Pole 160-179mm Top Diameter H4 Soil Type 4","Each",{"v":2286.96,"d":"R 2,286.96"},{"v":2286.96,"d":"R 2,286.96"}]
[1.101,"D-DT-0056","13m Wooden Pole 160-179mm Top Diameter H5 Soil Type 1","Each",{"v":337.32372271509996,"d":"R 337.32"},{"v":337.32372271509996,"d":"R 337.32"}]
[1.102,"D-DT-0056","13m Wooden Pole 160-179mm Top Diameter H5 Soil Type 2","Each",{"v":455.39,"d":"R 455.39"},{"v":455.39,"d":"R 455.39"}]
[1.103,"D-DT-0056","13m Wooden Pole 160-179mm Top Diameter H5 Soil Type 3","Each",{"v":2578.16,"d":"R 2,578.16"},{"v":2578.16,"d":"R 2,578.16"}]
[1.104,"D-DT-0056","13m Wooden Pole 160-179mm Top Diameter H5 Soil Type 4","Each",{"v":2286.96,"d":"R 2,286.96"},{"v":2286.96,"d":"R 2,286.96"}]
[1.105,"D-DT-0056","13m Wooden Pole 180-199mm Top Diameter H4 Soil Type 1","Each",{"v":374.79477239179994,"d":"R 374.79"},{"v":374.79477239179994,"d":"R 374.79"}]
[1.106,"D-DT-0056","13m Wooden Pole 180-199mm Top Diameter H4 Soil Type 2","Each",{"v":505.97,"d":"R 505.97"},{"v":505.97,"d":"R 505.97"}]
[1.107,"D-DT-0056","13m Wooden Pole 180-199mm Top Diameter H4 Soil Type 3","Each",{"v":2578.16,"d":"R 2,578.16"},{"v":2578.16,"d":"R 2,578.16"}]
[1.108,"D-DT-0056","13m Wooden Pole 180-199mm Top Diameter H4 Soil Type 4","Each",{"v":2286.96,"d":"R 2,286.96"},{"v":2286.96,"d":"R 2,286.96"}]
[1.109,"D-DT-0056","13m Wooden Pole 180-199mm Top Diameter H5 Soil Type 1","Each",{"v":374.79477239179994,"d":"R 374.79"},{"v":374.79477239179994,"d":"R 374.79"}]
[{"v":1.11,"d":"1.110"},"D-DT-0056","13m Wooden Pole 180-199mm Top Diameter H5 Soil Type 2","Each",{"v":505.97,"d":"R 505.97"},{"v":505.97,"d":"R 505.97"}]
[1.111,"D-DT-0056","13m Wooden Pole 180-199mm Top Diameter H5 Soil Type 3","Each",{"v":2578.16,"d":"R 2,578.16"},{"v":2578.16,"d":"R 2,578.16"}]
[1.112,"D-DT-0056","13m Wooden Pole 180-199mm Top Diameter H5 Soil Type 4","Each",{"v":2286.96,"d":"R 2,286.96"},{"v":2286.96,"d":"R 2,286.96"}]
[1.113,"D-DT-0056","13m Wooden Pole 200-219mm Top Diameter H4 Soil Type 1","Each",{"v":412.27635652160006,"d":"R 412.28"},{"v":412.27635652160006,"d":"R 412.28"}]
[1.114,"D-DT-0056","13m Wooden Pole 200-219mm Top Diameter H4 Soil Type 2","Each",{"v":556.57,"d":"R 556.57"},{"v":556.57,"d":"R 556.57"}]
[1.115,"D-DT-0056","13m Wooden Pole 200-219mm Top Diameter H4 Soil Type 3","Each",{"v":2578.16,"d":"R 2,578.16"},{"v":2578.16,"d":"R 2,578.16"}]
[1.116,"D-DT-0056","13m Wooden Pole 200-219mm Top Diameter H4 Soil Type 4","Each",{"v":2286.96,"d":"R 2,286.96"},{"v":2286.96,"d":"R 2,286.96"}]
[1.117,"D-DT-0056","13m Wooden Pole 200-219mm Top Diameter H5 Soil Type 1","Each",{"v":412.27635652160006,"d":"R 412.28"},{"v":412.27635652160006,"d":"R 412.28"}]
[1.118,"D-DT-0056","13m Wooden Pole 200-219mm Top Diameter H5 Soil Type 2","Each",{"v":556.57,"d":"R 556.57"},{"v":556.57,"d":"R 556.57"}]
[1.119,"D-DT-0056","13m Wooden Pole 200-219mm Top Diameter H5 Soil Type 3","Each",{"v":2578.16,"d":"R 2,578.16"},{"v":2578.16,"d":"R 2,578.16"}]
[{"v":1.12,"d":"1.120"},"D-DT-0056","13m Wooden Pole 200-219mm Top Diameter H5 Soil Type 4","Each",{"v":2286.96,"d":"R 2,286.96"},{"v":2286.96,"d":"R 2,286.96"}]
[1.121,"D-DT-0054","14m Wooden Pole 160-179mm Top Diameter H4 Soil Type 1","Each",{"v":370.92862810409997,"d":"R 370.93"},{"v":370.92862810409997,"d":"R 370.93"}]
[1.122,"D-DT-0054","14m Wooden Pole 160-179mm Top Diameter H4 Soil Type 2","Each",{"v":500.75,"d":"R 500.75"},{"v":500.75,"d":"R 500.75"}]
[1.123,"D-DT-0054","14m Wooden Pole 160-179mm Top Diameter H4 Soil Type 3","Each",{"v":2578.16,"d":"R 2,578.16"},{"v":2578.16,"d":"R 2,578.16"}]
[1.124,"D-DT-0054","14m Wooden Pole 160-179mm Top Diameter H4 Soil Type 4","Each",{"v":2286.96,"d":"R 2,286.96"},{"v":2286.96,"d":"R 2,286.96"}]
[1.125,"D-DT-0054","14m Wooden Pole 160-179mm Top Diameter H5 Soil Type 1","Each",{"v":370.92862810409997,"d":"R 370.93"},{"v":370.92862810409997,"d":"R 370.93"}]
[1.126,"D-DT-0054","14m Wooden Pole 160-179mm Top Diameter H5 Soil Type 2","Each",{"v":500.75,"d":"R 500.75"},{"v":500.75,"d":"R 500.75"}]
[1.127,"D-DT-0054","14m Wooden Pole 160-179mm Top Diameter H5 Soil Type 3","Each",{"v":2578.16,"d":"R 2,578.16"},{"v":2578.16,"d":"R 2,578.16"}]
[1.128,"D-DT-0054","14m Wooden Pole 160-179mm Top Diameter H5 Soil Type 4","Each",{"v":2286.96,"d":"R 2,286.96"},{"v":2286.96,"d":"R 2,286.96"}]
[1.129,"D-DT-0054","14m Wooden Pole 180-199mm Top Diameter H4 Soil Type 1","Each",{"v":412.13940863130006,"d":"R 412.14"},{"v":412.13940863130006,"d":"R 412.14"}]
[{"v":1.13,"d":"1.130"},"D-DT-0054","14m Wooden Pole 180-199mm Top Diameter H4 Soil Type 2","Each",{"v":556.39,"d":"R 556.39"},{"v":556.39,"d":"R 556.39"}]
[1.131,"D-DT-0054","14m Wooden Pole 180-199mm Top Diameter H4 Soil Type 3","Each",{"v":2578.16,"d":"R 2,578.16"},{"v":2578.16,"d":"R 2,578.16"}]
[1.132,"D-DT-0054","14m Wooden Pole 180-199mm Top Diameter H4 Soil Type 4","Each",{"v":2286.96,"d":"R 2,286.96"},{"v":2286.96,"d":"R 2,286.96"}]
[1.133,"D-DT-0054","14m Wooden Pole 180-199mm Top Diameter H5 Soil Type 1","Each",{"v":412.13940863130006,"d":"R 412.14"},{"v":412.13940863130006,"d":"R 412.14"}]
[1.134,"D-DT-0054","14m Wooden Pole 180-199mm Top Diameter H5 Soil Type 2","Each",{"v":556.39,"d":"R 556.39"},{"v":556.39,"d":"R 556.39"}]
[1.135,"D-DT-0054","14m Wooden Pole 180-199mm Top Diameter H5 Soil Type 3","Each",{"v":2578.16,"d":"R 2,578.16"},{"v":2578.16,"d":"R 2,578.16"}]
[1.136,"D-DT-0054","14m Wooden Pole 180-199mm Top Diameter H5 Soil Type 4","Each",{"v":2286.96,"d":"R 2,286.96"},{"v":2286.96,"d":"R 2,286.96"}]
[1.137,"D-DT-0054","14m Wooden Pole 200-219mm Top Diameter H4 Soil Type 1","Each",{"v":453.35018915850003,"d":"R 453.35"},{"v":453.35018915850003,"d":"R 453.35"}]
[1.138,"D-DT-0054","14m Wooden Pole 200-219mm Top Diameter H4 Soil Type 2","Each",{"v":612.02,"d":"R 612.02"},{"v":612.02,"d":"R 612.02"}]
[1.139,"D-DT-0054","14m Wooden Pole 200-219mm Top Diameter H4 Soil Type 3","Each",{"v":2578.16,"d":"R 2,578.16"},{"v":2578.16,"d":"R 2,578.16"}]
[{"v":1.14,"d":"1.140"},"D-DT-0054","14m Wooden Pole 200-219mm Top Diameter H4 Soil Type 4","Each",{"v":2286.96,"d":"R 2,286.96"},{"v":2286.96,"d":"R 2,286.96"}]
[1.141,"D-DT-0054","14m Wooden Pole 200-219mm Top Diameter H5 Soil Type 1","Each",{"v":453.35018915850003,"d":"R 453.35"},{"v":453.35018915850003,"d":"R 453.35"}]
[1.142,"D-DT-0054","14m Wooden Pole 200-219mm Top Diameter H5 Soil Type 2","Each",{"v":612.02,"d":"R 612.02"},{"v":612.02,"d":"R 612.02"}]
[1.143,"D-DT-0054","14m Wooden Pole 200-219mm Top Diameter H5 Soil Type 3","Each",{"v":2578.16,"d":"R 2,578.16"},{"v":2578.16,"d":"R 2,578.16"}]
[1.144,"D-DT-0054","14m Wooden Pole 200-219mm Top Diameter H5 Soil Type 4","Each",{"v":2286.96,"d":"R 2,286.96"},{"v":2286.96,"d":"R 2,286.96"}]
[1.145,"D-DT-0057","15m Wooden Pole 160-179mm Top Diameter Soil Type 1","Each",{"v":453.35018915850003,"d":"R 453.35"},{"v":453.35018915850003,"d":"R 453.35"}]
[1.146,"D-DT-0057","15m Wooden Pole 160-179mm Top Diameter Soil Type 2","Each",{"v":612.02,"d":"R 612.02"},{"v":612.02,"d":"R 612.02"}]
[{"v":1.14699999999999,"d":"1.147"},"D-DT-0057","15m Wooden Pole 160-179mm Top Diameter Soil Type 3","Each",{"v":2974.8,"d":"R 2,974.80"},{"v":2974.8,"d":"R 2,974.80"}]
[{"v":1.14799999999999,"d":"1.148"},"D-DT-0057","15m Wooden Pole 160-179mm Top Diameter Soil Type 4","Each",{"v":2638.8,"d":"R 2,638.80"},{"v":2638.8,"d":"R 2,638.80"}]
[{"v":1.14899999999999,"d":"1.149"},"D-DT-0057","15m Wooden Pole 190-199mm Top Diameter Soil Type 1","Each",{"v":453.35018915850003,"d":"R 453.35"},{"v":453.35018915850003,"d":"R 453.35"}]
[{"v":1.14999999999999,"d":"1.150"},"D-DT-0057","15m Wooden Pole 190-199mm Top Diameter Soil Type 2","Each",{"v":612.02,"d":"R 612.02"},{"v":612.02,"d":"R 612.02"}]
[{"v":1.15099999999999,"d":"1.151"},"D-DT-0057","15m Wooden Pole 190-199mm Top Diameter Soil Type 3","Each",{"v":2974.8,"d":"R 2,974.80"},{"v":2974.8,"d":"R 2,974.80"}]
[{"v":1.15199999999999,"d":"1.152"},"D-DT-0057","15m Wooden Pole 190-199mm Top Diameter Soil Type 4","Each",{"v":2638.8,"d":"R 2,638.80"},{"v":2638.8,"d":"R 2,638.80"}]
[{"v":1.15299999999999,"d":"1.153"},"D-DT-0057","15m Wooden Pole 200-219mm Top Diameter Soil Type 1","Each",{"v":407.8624206727,"d":"R 407.86"},{"v":407.8624206727,"d":"R 407.86"}]
[{"v":1.15399999999999,"d":"1.154"},"D-DT-0057","15m Wooden Pole 200-219mm Top Diameter Soil Type 2","Each",{"v":550.61,"d":"R 550.61"},{"v":550.61,"d":"R 550.61"}]
[{"v":1.15499999999999,"d":"1.155"},"D-DT-0057","15m Wooden Pole 200-219mm Top Diameter Soil Type 3","Each",{"v":2974.8,"d":"R 2,974.80"},{"v":2974.8,"d":"R 2,974.80"}]
[{"v":1.15599999999999,"d":"1.156"},"D-DT-0057","15m Wooden Pole 200-219mm Top Diameter Soil Type 4","Each",{"v":2638.8,"d":"R 2,638.80"},{"v":2638.8,"d":"R 2,638.80"}]
[{"v":1.15699999999999,"d":"1.157"},"D-DT-0049","16m Wooden Pole 180-199mm Top Diameter Soil Type 1","Each",{"v":448.48327182630004,"d":"R 448.48"},{"v":448.48327182630004,"d":"R 448.48"}]
[{"v":1.15799999999999,"d":"1.158"},"D-DT-0049","16m Wooden Pole 180-199mm Top Diameter Soil Type 2","Each",{"v":605.45,"d":"R 605.45"},{"v":605.45,"d":"R 605.45"}]
[{"v":1.15899999999999,"d":"1.159"},"D-DT-0049","16m Wooden Pole 180-199mm Top Diameter Soil Type 3","Each",{"v":3173.12,"d":"R 3,173.12"},{"v":3173.12,"d":"R 3,173.12"}]
[{"v":1.15999999999999,"d":"1.160"},"D-DT-0049","16m Wooden Pole 180-199mm Top Diameter Soil Type 4","Each",{"v":2814.72,"d":"R 2,814.72"},{"v":2814.72,"d":"R 2,814.72"}]
[{"v":1.16099999999999,"d":"1.161"},"D-DT-0049","16m Wooden Pole 200-219mm Top Diameter Soil Type 1","Each",{"v":493.3389731261001,"d":"R 493.34"},{"v":493.3389731261001,"d":"R 493.34"}]
[{"v":1.16199999999999,"d":"1.162"},"D-DT-0049","16m Wooden Pole 200-219mm Top Diameter Soil Type 2","Each",{"v":666.01,"d":"R 666.01"},{"v":666.01,"d":"R 666.01"}]
[{"v":1.16299999999999,"d":"1.163"},"D-DT-0049","16m Wooden Pole 200-219mm Top Diameter Soil Type 3","Each",{"v":3173.12,"d":"R 3,173.12"},{"v":3173.12,"d":"R 3,173.12"}]
[{"v":1.16399999999999,"d":"1.164"},"D-DT-0049","16m Wooden Pole 200-219mm Top Diameter Soil Type 4","Each",{"v":2814.72,"d":"R 2,814.72"},{"v":2814.72,"d":"R 2,814.72"}]
[{"v":1.16499999999999,"d":"1.165"},"D-DT-0048","18m Wooden Pole 180-199mm Top Diameter Soil Type 1","Each",{"v":493.1598874234,"d":"R 493.16"},{"v":493.1598874234,"d":"R 493.16"}]
[{"v":1.16599999999999,"d":"1.166"},"D-DT-0048","18m Wooden Pole 180-199mm Top Diameter Soil Type 2","Each",{"v":665.77,"d":"R 665.77"},{"v":665.77,"d":"R 665.77"}]
[{"v":1.16699999999999,"d":"1.167"},"D-DT-0048","18m Wooden Pole 180-199mm Top Diameter Soil Type 3","Each",{"v":3569.76,"d":"R 3,569.76"},{"v":3569.76,"d":"R 3,569.76"}]
[{"v":1.16799999999999,"d":"1.168"},"D-DT-0048","18m Wooden Pole 180-199mm Top Diameter Soil Type 4","Each",{"v":3166.56,"d":"R 3,166.56"},{"v":3166.56,"d":"R 3,166.56"}]
[{"v":1.16899999999999,"d":"1.169"},"D-DT-0048","18m Wooden Pole 200-219mm Top Diameter Soil Type 1","Each",{"v":542.4716623845002,"d":"R 542.47"},{"v":542.4716623845002,"d":"R 542.47"}]
[{"v":1.16999999999999,"d":"1.170"},"D-DT-0048","18m Wooden Pole 200-219mm Top Diameter Soil Type 2","Each",{"v":732.34,"d":"R 732.34"},{"v":732.34,"d":"R 732.34"}]
[{"v":1.17099999999999,"d":"1.171"},"D-DT-0048","18m Wooden Pole 200-219mm Top Diameter Soil Type 3","Each",{"v":3569.76,"d":"R 3,569.76"},{"v":3569.76,"d":"R 3,569.76"}]
[{"v":1.17199999999999,"d":"1.172"},"D-DT-0048","18m Wooden Pole 200-219mm Top Diameter Soil Type 4","Each",{"v":3166.56,"d":"R 3,166.56"},{"v":3166.56,"d":"R 3,166.56"}]
[2,null,"Concrete Poles"]
[2.1,"D-DT-0017","11m Concrete Pole 10kN Ultimate Load","Each",{"v":311.7460705883001,"d":"R 311.75"},{"v":311.7460705883001,"d":"R 311.75"}]
[2.2,"D-DT-0015","12m Concrete Pole 10kN Ultimate Load","Each",{"v":340.0837494273,"d":"R 340.08"},{"v":340.0837494273,"d":"R 340.08"}]
[2.3,"D-DT-0016","13m Concrete Pole 10kN Ultimate Load","Each",{"v":368.4214282663,"d":"R 368.42"},{"v":368.4214282663,"d":"R 368.42"}]
[2.4,"D-DT-0018","14m Concrete Pole 10kN Ultimate Load","Each",{"v":396.7591071053,"d":"R 396.76"},{"v":396.7591071053,"d":"R 396.76"}]
[3,null,"Free Standing(Unsupported)"]
[3.1,"PA09599B01","9m Concrete Pole 18kN","Each",{"v":311.7460705883001,"d":"R 311.75"},{"v":311.7460705883001,"d":"R 311.75"}]
[3.2,"D-DT-1650","12m Concrete Pole 8kN","Each",{"v":311.7460705883001,"d":"R 311.75"},{"v":311.7460705883001,"d":"R 311.75"}]
[3.3,"D-DT-1651","12m Concrete Pole 15kN","Each",{"v":584.5238823530626,"d":"R 584.52"},{"v":584.5238823530626,"d":"R 584.52"}]
[3.4,"D-DT-1652","12m Concrete Pole 27kN","Each",{"v":1052.1429882355128,"d":"R 1,052.14"},{"v":1052.1429882355128,"d":"R 1,052.14"}]
[3.5,"D-DT-1653","12m Concrete Pole 42kN","Each",{"v":1636.6668705885754,"d":"R 1,636.67"},{"v":1636.6668705885754,"d":"R 1,636.67"}]
[3.6,"D-DT-1654","12m Concrete Pole 58kN","Each",{"v":2260.159011765176,"d":"R 2,260.16"},{"v":2260.159011765176,"d":"R 2,260.16"}]
[3.7,"D-DT-1655","12m Concrete Pole 65kN - Terminal Structure","Each",{"v":2532.936823529938,"d":"R 2,532.94"},{"v":2532.936823529938,"d":"R 2,532.94"}]
[3.8,"D-DT-1656","12m Concrete Pole 73kN","Each",{"v":2844.6828941182384,"d":"R 2,844.68"},{"v":2844.6828941182384,"d":"R 2,844.68"}]
[3.9,"D-DT-1657","12m Concrete Pole 106kN","Each",{"v":4130.635435294977,"d":"R 4,130.64"},{"v":4130.635435294977,"d":"R 4,130.64"}]
[{"v":3.1,"d":"3.10"},"D-DT-1650","13m Concrete Pole 8kN","Each",{"v":337.72490980399175,"d":"R 337.72"},{"v":337.72490980399175,"d":"R 337.72"}]
[3.11,"D-DT-1651","13m Concrete Pole 15kN","Each",{"v":633.2342058824845,"d":"R 633.23"},{"v":633.2342058824845,"d":"R 633.23"}]
[3.12,"D-DT-1652","13m Concrete Pole 27kN","Each",{"v":1139.8215705884722,"d":"R 1,139.82"},{"v":1139.8215705884722,"d":"R 1,139.82"}]
[3.13,"D-DT-1653","13m Concrete Pole 42kN","Each",{"v":1773.0557764709567,"d":"R 1,773.06"},{"v":1773.0557764709567,"d":"R 1,773.06"}]
[3.14,"D-DT-1654","13m Concrete Pole 58kN","Each",{"v":2448.50559607894,"d":"R 2,448.51"},{"v":2448.50559607894,"d":"R 2,448.51"}]
[3.15,"D-DT-1655","13m Concrete Pole 65kN - Terminal Structure","Each",{"v":2744.0148921574328,"d":"R 2,744.01"},{"v":2744.0148921574328,"d":"R 2,744.01"}]
[3.16,"D-DT-1656","13m Concrete Pole 73kN","Each",{"v":3081.7398019614247,"d":"R 3,081.74"},{"v":3081.7398019614247,"d":"R 3,081.74"}]
[3.17,"D-DT-1657","13m Concrete Pole 106kN","Each",{"v":4474.8550549028905,"d":"R 4,474.86"},{"v":4474.8550549028905,"d":"R 4,474.86"}]
["SUB-TOTAL D"]
["E","Single Phase MV Structure, BONDING INCL (BIL DOWNWIRE,SPARK GAP DEVICE INCLUDED OR EXCLUDED AS PER DESIGN)",{"$nulls":4},"Description change in red"]
[null,"Supply and erect MV support structures as per Eskom DDT 0400, 1300, 1700, 1800 drawings and OU specific SI Engineering instructions.  Auxiliary equipment such as bonding, jumpers, jumper terminations, pole and x-arm mounting and mounting hardware, conductor attachment hardware and insulators to be included.  Poles are measured elsewhere, cross arms are included.  Stay, strut material measured elsewhere.  Pole, stay and strut  excavations are measured elsewhere.  Where road crossing structures are to be used the line hardware needs to be changed to include : For intermediate a suitable full wrap road crossing tie and for a strain structure a 3bolt suitable pistol grip.  Other relevant road crossing hardware to be included where required.  Road crossings to be inserted in BOQ where required and marked with \"RX\" as part of the description.  MV intermediate structures that fall within high lightning zones in the OU shall have a spark gap device installed on its BIL down wire.  Refer DDT3134. All other intermediate structures will have a normal BIL.  All line hardware purchased will be paid elsewhere as cost plus fee.",{"$nulls":4},"Propose to remove description in red"]
[null,null,"Intermediate - 0 deg"]
[1.1,1390,"Phase / phase - T-frame / 2m Steel X-arm – Intermediate - 0° Deviation ","Each",{"v":246.58603200000002,"d":"R 246.59"},{"v":246.58603200000002,"d":"R 246.59"}]
[1.2000000000000002,1390,"Phase / phase - T-frame / 2m Steel X-arm – Intermediate - 0° Deviation -RX","Each",{"v":246.58603200000002,"d":"R 246.59"},{"v":246.58603200000002,"d":"R 246.59"}]
[1.3,1390,"Phase / phase - T-frame / 2m Steel X-arm – Intermediate - 0° Deviation -With Spark Gap device","Each",{"v":246.58603200000002,"d":"R 246.59"},{"v":246.58603200000002,"d":"R 246.59"}]
[1.4000000000000001,1390,"Phase / phase - T-frame / 2m Steel X-arm – Intermediate - 0° Deviation -With Spark Gap device - RX","Each",{"v":246.58603200000002,"d":"R 246.59"},{"v":246.58603200000002,"d":"R 246.59"}]
[1.5,1370,"Phase / phase - H-Pole / 4,5m Wood X-arm – Intermediate - 0° Deviation ","Each",{"v":393.19378560000007,"d":"R 393.19"},{"v":393.19378560000007,"d":"R 393.19"}]
[1.6,1370,"Phase / phase - H-Pole / 4,5m Wood X-arm – Intermediate - 0° Deviation -RX","Each",{"v":393.19378560000007,"d":"R 393.19"},{"v":393.19378560000007,"d":"R 393.19"}]
[1.7000000000000002,1370,"Phase / phase - H-Pole / 4,5m Wood X-arm – Intermediate - 0° Deviation -With Spark Gap device","Each",{"v":420.76188,"d":"R 420.76"},{"v":420.76188,"d":"R 420.76"}]
[1.8000000000000003,1370,"Phase / phase - H-Pole / 4,5m Wood X-arm – Intermediate - 0° Deviation -With Spark Gap device-RX","Each",{"v":420.76188,"d":"R 420.76"},{"v":420.76188,"d":"R 420.76"}]
[null,null,"Strainer - Small (1 - 30) deg"]
[2.1,1371,"Phase / phase – H-Pole / 4.5m Wood x-arm – Intermediate – Small (1 –10°) deviation","Each",{"v":391.4064,"d":"R 391.41"},{"v":391.4064,"d":"R 391.41"}]
[2.2,1371,"Phase / phase – H-Pole / 4.5m Wood x-arm – Intermediate – Small (1 –10°) deviation-RX","Each",{"v":391.4064,"d":"R 391.41"},{"v":391.4064,"d":"R 391.41"}]
[2.3000000000000003,1391,"Phase / phase - T-frame/ 2m Steel X-arm – Intermediate -  Small (1- +/-10°) Deviation ","Each",{"v":246.58603200000002,"d":"R 246.59"},{"v":246.58603200000002,"d":"R 246.59"}]
[2.4000000000000004,1391,"Phase / phase - T-frame/ 2m Steel X-arm – Intermediate -  Small (1- +/-10°) Deviation -RX","Each",{"v":215.762778,"d":"R 215.76"},{"v":215.762778,"d":"R 215.76"}]
[null,null,"Strainer - 0 deg"]
[3.1,1340,"Phase / phase – Delta/2.5M Wooden X-arm –Strain - 0° Deviation ","Each",{"v":247.70988000000003,"d":"R 247.71"},{"v":247.70988000000003,"d":"R 247.71"}]
[3.2,1340,"Phase / phase – Delta/2.5M Wooden X-arm –Strain - 0° Deviation Rx ","Each",{"v":247.70988000000003,"d":"R 247.71"},{"v":247.70988000000003,"d":"R 247.71"}]
[3.3,"1340B","Phase / phase – Delta/2.5M Wooden X-arm –Strain - 0° Deviation ","Each",{"v":247.70988000000003,"d":"R 247.71"},{"v":247.70988000000003,"d":"R 247.71"}]
[3.4,"1340B","Phase / phase – Delta/2.5M Wooden X-arm –Strain - 0° Deviation Rx","Each",{"v":247.70988000000003,"d":"R 247.71"},{"v":247.70988000000003,"d":"R 247.71"}]
[3.5,"1340B","Phase / phase – Delta/2.5M Wooden X-arm –Strain - 0° Deviation With Spark Gap Device ","Each",{"v":266.29308,"d":"R 266.29"},{"v":266.29308,"d":"R 266.29"}]
[3.6,"1340B","Phase / phase – Delta/2.5M Wooden X-arm –Strain - 0° Deviation With Spark Gap Device-Rx","Each",{"v":266.29308,"d":"R 266.29"},{"v":266.29308,"d":"R 266.29"}]
[3.7,1343,"Phase / phase – Delta/2.5M Wooden X-arm –Strain - 0° Deviation ","Each",{"v":247.70988000000003,"d":"R 247.71"},{"v":247.70988000000003,"d":"R 247.71"}]
[3.8,1343,"Phase / phase – Delta/2.5M Wooden X-arm –Strain - 0° Deviation - Rx","Each",{"v":247.70988000000003,"d":"R 247.71"},{"v":247.70988000000003,"d":"R 247.71"}]
[3.9,1373,"Phase / phase - H-Pole / 4,5m Wood X-arm – Strain – 0° Deviation ","Each",{"v":391.4064,"d":"R 391.41"},{"v":391.4064,"d":"R 391.41"}]
[{"v":3.1,"d":"3.10"},1373,"Phase / phase - H-Pole / 4,5m Wood X-arm – Strain – 0° Deviation -RX","Each",{"v":391.4064,"d":"R 391.41"},{"v":391.4064,"d":"R 391.41"}]
[null,null,"Strainer - Medium (1 - 60) deg"]
[4.1,1344,"Phase / phase – Delta/2.5M Wooden X-arm –Strain - Medium (1-60°) Deviation ","Each",{"v":247.70988000000003,"d":"R 247.71"},{"v":247.70988000000003,"d":"R 247.71"}]
[4.199999999999999,1344,"Phase / phase – Delta/2.5M Wooden X-arm –Strain - Medium (1-60°) Deviation -Rx","Each",{"v":247.70988000000003,"d":"R 247.71"},{"v":247.70988000000003,"d":"R 247.71"}]
[4.3,1374,"Phase / phase - H-Pole / 4,5m Wood X-arm – Strain - Medium(1°- 60°) Deviation ","Each",{"v":391.4064,"d":"R 391.41"},{"v":391.4064,"d":"R 391.41"}]
[4.3999999999999995,1374,"Phase / phase - H-Pole / 4,5m Wood X-arm – Strain - Medium(1°- 60°) Deviation -RX","Each",{"v":391.4064,"d":"R 391.41"},{"v":391.4064,"d":"R 391.41"}]
[null,null,"Strainer - Terminal"]
[5.1,1346,"Phase / phase – Delta/2.5M Wood X-arm – Strain - Terminal ","Each",{"v":247.70988000000003,"d":"R 247.71"},{"v":247.70988000000003,"d":"R 247.71"}]
[5.199999999999999,1346,"Phase / phase – Delta/2.5M Wood X-arm – Strain - Terminal -Rx","Each",{"v":247.70988000000003,"d":"R 247.71"},{"v":247.70988000000003,"d":"R 247.71"}]
[5.3,1376,"Phase / phase - H-Pole / 4,5m Wood X-arm – Strain – Terminal ","Each",{"v":391.4064,"d":"R 391.41"},{"v":391.4064,"d":"R 391.41"}]
[5.3999999999999995,1376,"Phase / phase - H-Pole / 4,5m Wood X-arm – Strain – Terminal -RX","Each",{"v":391.4064,"d":"R 391.41"},{"v":391.4064,"d":"R 391.41"}]
[null,null,"Take-Off"]
[6.1,1811,"Phase / phase Take-off – Vertical (600mm spacing)","Each",{"v":146.7774,"d":"R 146.78"},{"v":146.7774,"d":"R 146.78"}]
[6.199999999999999,1811,"Phase / phase Take-off – Vertical (600mm spacing)-RX","Each",{"v":146.7774,"d":"R 146.78"},{"v":146.7774,"d":"R 146.78"}]
[6.3,1814,"Phase / phase Take-off - 2,5m Wooden X-arm","Each",{"v":184.939524,"d":"R 184.94"},{"v":184.939524,"d":"R 184.94"}]
[6.3999999999999995,1814,"Phase / phase Take-off - 2,5m Wooden X-arm-RX","Each",{"v":184.939524,"d":"R 184.94"},{"v":184.939524,"d":"R 184.94"}]
[6.5,1815,"Phase / phase Take-off - 2 x 2,5m Wooden X-arm","Each",{"v":293.5548,"d":"R 293.55"},{"v":293.5548,"d":"R 293.55"}]
[6.6,1815,"Phase / phase Take-off - 2 x 2,5m Wooden X-arm-RX","Each",{"v":293.5548,"d":"R 293.55"},{"v":293.5548,"d":"R 293.55"}]
[6.699999999999999,1816,"Phase / phase Take-off - H-Pole (3,5m Wooden X-arm)","Each",{"v":342.48060000000004,"d":"R 342.48"},{"v":342.48060000000004,"d":"R 342.48"}]
[6.8,1816,"Phase / phase Take-off - H-Pole (3,5m Wooden X-arm)-RX","Each",{"v":342.48060000000004,"d":"R 342.48"},{"v":342.48060000000004,"d":"R 342.48"}]
[6.8999999999999995,1817,"Phase / phase Take-off - H-Pole (2 x 3,5m Wooden X-arm) ","Each",{"v":391.4064,"d":"R 391.41"},{"v":391.4064,"d":"R 391.41"}]
[{"v":6.1,"d":"6.10"},1817,"Phase / phase Take-off - H-Pole (2 x 3,5m Wooden X-arm) -RX","Each",{"v":391.4064,"d":"R 391.41"},{"v":391.4064,"d":"R 391.41"}]
[null,null,"Assemble Three Phase MV Structures,BONDING INCL (BIL DOWNWIRE,SPARK GAP DEVICE INCLUDED OR EXCLUDED AS PER DESIGN)",{"$nulls":3},"Description change in red"]
[7,null,"Intermediate - 0 deg"]
[7.1,"D-DT-1700","3 Phase - Staggered Vertical (450mm Spacing) ","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[7.199999999999999,"D-DT-1710","3 Phase - Staggered Vertical (600mm Spacing)","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[7.3,"D-DT-1720","3 Phase - Delta (450mm Stud)","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[7.3999999999999995,"D-DT-1730","3 Phase - Delta (Intermediate 'T' Cross arm)","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[7.5,"D-DT-1740","3 Phase - Delta / 2,5m Wood Cross arm","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[7.6,"D-DT-1750","3 Phase - Delta / 4,5m Wood Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[7.699999999999999,"D-DT-1760","3 Phase - H-Pole / 3,5m Wood Cross arm","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[7.8,"D-DT-1770","3 Phase - H-Pole / 4,5m Wood Cross arm","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[7.8999999999999995,"D-DT-1785","MV Heavy Conductor - 3 Phase Staggered Vertical 800mm Spacing","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[{"v":7.1,"d":"7.10"},"D-DT-1790","MV Heavy Conductor - 3 Phase - Delta - 3500mm Wooden Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[{"v":7.109999999999999,"d":"7.11"},"D-DT-1793","MV Heavy Conductor - 22kV H-Pole Suspension Structure General Arrangement","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[{"v":7.119999999999999,"d":"7.12"},"D-DT-1870","Three Phase T-Frame / 2m Steel Cross arm","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[7.13,"D-DT-1870B","Three Phase T-Frame / 2m Steel Cross arm, Horizontal Configuration","Each",{"v":246.58603200000002,"d":"R 246.59"},{"v":246.58603200000002,"d":"R 246.59"},"Additional item,proposed the same rate"]
[7.14,"1740B","3 Phase - Delta / 2,5m Wood X-arm – Intermediate - 0° Deviation ","Each",{"v":246.58603200000002,"d":"R 246.59"},{"v":246.58603200000002,"d":"R 246.59"}]
[7.15,"1740B","3 Phase - Delta / 2,5m Wood X-arm – Intermediate - 0° Deviation -RX","Each",{"v":246.58603200000002,"d":"R 246.59"},{"v":246.58603200000002,"d":"R 246.59"}]
[7.16,"1740B","3 Phase - Delta / 2,5m Wood X-arm – Intermediate - 0° Deviation -With Spark Gap Device","Each",{"v":265.084644,"d":"R 265.08"},{"v":265.084644,"d":"R 265.08"}]
[7.17,"1740B","3 Phase - Delta / 2,5m Wood X-arm – Intermediate - 0° Deviation -With Spark Gap Device-RX","Each",{"v":265.084644,"d":"R 265.08"},{"v":265.084644,"d":"R 265.08"}]
[7.18,1750,"3 Phase - Delta / 4,5m Wood X-arm – Intermediate - 0° Deviation -RX","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[7.19,1750,"3 Phase - Delta / 4,5m Wood X-arm – Intermediate - 0° Deviation -With Spark Gap Device","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[{"v":7.2,"d":"7.20"},1750,"3 Phase - Delta / 4,5m Wood X-arm – Intermediate - 0° Deviation -With Spark Gap Device-RX","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[7.21,1710,"3 Phase - Staggered Vertical (600mm Spacing) Intermediate 0° Deviation Rx","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[7.22,1770,"3 Phase - H-Pole / 4,5m Wood X-arm – Intermediate - 0° Deviation -RX","Each",{"v":391.4064,"d":"R 391.41"},{"v":391.4064,"d":"R 391.41"}]
[7.23,1770,"3 Phase - H-Pole / 4,5m Wood X-arm – Intermediate - 0° Deviation - With Spark Gap Device","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[7.24,1770,"3 Phase - H-Pole / 4,5m Wood X-arm – Intermediate - 0° Deviation - With Spark Gap Device -RX","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[7.25,1790,"Heavy Conductor - 3 Phase Delta-3500mm Wooden X-arm Intermediate 0° Deviation Rx","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[7.26,1710,"3 Phase - Staggered Vertical (600mm Spacing) Intermediate 0° Deviation Rx","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[8,null,"Intermediate - (0 - 10) deg"]
[8.1,"D-DT-1701","3 Phase - Vertical (450mm Spacing) ","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[8.2,"D-DT-1711","3 Phase - Vertical (600mm Spacing) ","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[8.299999999999999,"D-DT-1771","3 Phase - H-Pole / 4,5m Wood Cross arm","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[8.4,"D-DT-1871","Three Phase T-Frame / 2m Steel Cross arm","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[8.5,1771,"3 Phase - H-Pole / 4,5m Wood X-arm – Intermediate - Small(1°-±10°) Deviation -RX","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[8.6,1711,"3 Phase - Vertical (600mm Spacing) Intermediate-Small (1- ±10°) Deviation Rx","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[9,null,"Intermediate - (15 - 30) deg"]
[9.1,"D-DT-1702","3 Phase - Vertical (450mm Spacing) ","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[9.2,"D-DT-1712","3 Phase - Vertical (600mm Spacing) ","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[9.3,1712,"3 Phase - Vertical (600mm Spacing) Intermediate-Medium (±15-30°) Deviation Rx","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[10,null,"Strainer - 0 deg"]
[10.1,"D-DT-1703","3 Phase - Vertical (450mm Spacing) ","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[10.2,"D-DT-1713","3 Phase - Vertical (600mm Spacing) ","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[10.299999999999999,"D-DT-1733","3 Phase - Delta / 1,3m Steel Cross arm","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[10.4,"D-DT-1743","3 Phase - 600mm Phase Spacing Delta / 2,5m Wood Cross arm","Each",{"v":266.93,"d":"R 266.93"},{"v":266.93,"d":"R 266.93"}]
[10.5,"D-DT-1747","3 Phase - 600mm Phase Spacing Delta / 2 x 2,5m Wood Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[10.6,"D-DT-1747","3 Phase - 800mm Phase Spacing Delta / 2 x 2,5m Wood Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[10.7,"D-DT-1753","3 Phase - Delta / 4,5m Wood Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[10.799999999999999,"D-DT-1763","3 Phase - Delta / 3,5m Wood Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[10.9,"D-DT-1767","3 Phase - H-Pole / 2 x 3,5m Wood Cross arm","Each",{"v":819.16,"d":"R 819.16"},{"v":819.16,"d":"R 819.16"}]
[{"v":10.1,"d":"10.10"},"D-DT-1773","3 Phase - H-Pole / 4,5m Wood Cross arm","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[10.11,"D-DT-1777","3 Phase - H-Pole / 2 x 4,5m Wood Cross arm","Each",{"v":819.16,"d":"R 819.16"},{"v":819.16,"d":"R 819.16"}]
[10.12,"D-DT-1783","3 Phase - Trips","Each",{"v":847.4,"d":"R 847.40"},{"v":847.4,"d":"R 847.40"}]
[{"v":10.129999999999999,"d":"10.13"},"D-DT-1786","MV Heavy Conductor - 22kV 3 Phase - Vertical 800mm Spacing","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[{"v":10.139999999999999,"d":"10.14"},"D-DT-1794","MV Heavy Conductor - 22kV H-Pole Braced ","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[10.15,1767,"3 Phase - H-Pole / 2 x 3,5m Wood X-arm – Strain - 0° Deviation -RX","Each",{"v":819.16,"d":"R 819.16"},{"v":819.16,"d":"R 819.16"}]
[10.16,1773,"3 Phase - H-Pole / 4,5m Wood X-arm - Strain - 0° Deviation-RX ","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[10.17,1777,"3 Phase – H-Pole / 2 x 4,5m Wood X-arm – Strain - 0° Deviation -RX","Each",{"v":819.16,"d":"R 819.16"},{"v":819.16,"d":"R 819.16"}]
[10.18,1713,"3 Phase - Vertical (600mm Spacing) Strain 0° Deviation Rx","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[10.19,1743,"3 Phase - Delta / 2,5m Wood X-arm - Strain – 0° Deviation -RX","Each",{"v":266.93,"d":"R 266.93"},{"v":266.93,"d":"R 266.93"}]
[{"v":10.2,"d":"10.20"},1747,"3 Phase - Delta / 2 x 2,5m Wood X-arm - Strain - 0° Deviation -RX","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[{"v":10.209999999999999,"d":"10.21"},1753,"3 Phase - Delta / 4,5m Wood X-arm - Strain – 0° Deviation -RX","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[{"v":10.219999999999999,"d":"10.22"},1763,"3 Phase - H-Pole / 3,5m Wood X-arm - Strain - 0° Deviation -RX","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[10.23,1785,"3 Phase - Staggered Vertical (800mm spacing) 0° Deviation Rx Wood Poles Rx","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[10.24,1786,"3 Phase - Vertical (800mm spacing) Strain 0° Deviation 10kN Wood Poles Rx","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[10.25,1783,"3 Phase – Trips – Strain - 0° Deviation (Front view) -RX","Each",{"v":847.4,"d":"R 847.40"},{"v":847.4,"d":"R 847.40"}]
[10.26,1794,"Heavy Conductor H-Pole Braced In-Line strain-RX","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[11,null,"Strainer - Small (1 - 30) deg"]
[11.1,"D-DT-1704","3 Phase - Vertical (450mm Spacing) ","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[11.2,"D-DT-1714","3 Phase - Vertical (600mm Spacing) ","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[11.299999999999999,"D-DT-1734","3 Phase - Delta / 1,3m Steel Cross arm","Each",{"v":266.93,"d":"R 266.93"},{"v":266.93,"d":"R 266.93"}]
[11.4,"D-DT-1787","MV Heavy Conductor - 22kV 3 Phase - Vertical 800mm Spacing","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[11.5,1714,"3 Phase - Vertical (600mm Spacing) Strain - Small(1-30°) Deviation Rx","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[11.6,1787,"3 Phase - Vertical (800mm spacing) Strain 0-30° Deviation 10kN Wood Poles Rx","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[12,null,"Strainer - Medium (1 - 60) deg"]
[12.1,"D-DT-1744","3 Phase - Delta / 2,5m Wood Cross arm","Each",{"v":266.93,"d":"R 266.93"},{"v":266.93,"d":"R 266.93"}]
[12.2,"D-DT-1748","3 Phase - Delta / 2 x 2,5m Wood Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[12.299999999999999,"D-DT-1754","3 Phase - Delta / 4,5m Wood Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[12.4,"D-DT-1754","3 Phase - Delta / 2 x 4,5m Wood Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[12.5,"D-DT-1764","3 Phase - H-Pole / 3,5m Wood Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[12.6,"D-DT-1768","3 Phase - Pole / 2 x 3,5m Wood Cross arm","Each",{"v":819.16,"d":"R 819.16"},{"v":819.16,"d":"R 819.16"}]
[12.7,"D-DT-1774","3 Phase - H-Pole / 4,5m Wood Cross arm","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[12.799999999999999,"D-DT-1778","3 Phase - Pole / 2 x 4,5m Wood Cross arm","Each",{"v":819.16,"d":"R 819.16"},{"v":819.16,"d":"R 819.16"}]
[12.9,"D-DT-1795","MV Heavy Conductor - 22kV H-Pole Braced","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[{"v":12.1,"d":"12.10"},1744,"3 Phase - Delta / 2,5m Wood X-arm - Strain – Medium(1°-60°) Deviation -RX","Each",{"v":266.93,"d":"R 266.93"},{"v":266.93,"d":"R 266.93"}]
[12.11,1748,"3 Phase - Delta / 2 x 2,5m Wood X-arm - Strain - Medium(1°-60°) Deviation -RX","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[12.12,1754,"3 Phase - Delta / 4,5m Wood X-arm - Strain – Medium(1°-60°) Deviation -RX","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[{"v":12.129999999999999,"d":"12.13"},1754,"3 Phase - Delta / 2x4,5m Wood X-arm - Strain – Medium(1°-60°) Deviation -RX","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[{"v":12.139999999999999,"d":"12.14"},1764,"3 Phase - H-Pole / 3,5m Wood X-arm - Strain - Medium(1°-60°) Deviation -RX","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[12.15,1768,"3 Phase - H-Pole / 2 x 3,5m Wood X-arm – Strain - Medium(1°-60°) Deviation -RX","Each",{"v":819.16,"d":"R 819.16"},{"v":819.16,"d":"R 819.16"}]
[12.16,1774,"3 Phase – H-Pole / 4,5m Wood X-arm - Strain - Medium(1°-60°) Deviation -RX","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[12.17,1778,"3 Phase – H-Pole / 2 x 4,5m Wood X-arm – Strain – Medium(1°-60°) Deviation -RX","Each",{"v":819.16,"d":"R 819.16"},{"v":819.16,"d":"R 819.16"}]
[12.18,1795,"Heavy Conductor H-Pole Braced Angle strain (1-60˚)-RX","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[13,null,"Strainer - Large (61- 90) deg"]
[13.1,"D-DT-1705","3 Phase - Vertical (450mm Spacing) ","Each",{"v":266.93,"d":"R 266.93"},{"v":266.93,"d":"R 266.93"}]
[13.2,"D-DT-1715","3 Phase - Vertical (600mm Spacing) ","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[13.299999999999999,"D-DT-1735","3 Phase - Delta / 1,3m Steel Cross arm","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[13.4,"D-DT-1742","3 Phase - Delta 2,5m Wood Cross arm / 1700 Steel Cross arm","Each",{"v":431.25,"d":"R 431.25"},{"v":431.25,"d":"R 431.25"}]
[13.5,"D-DT-1742","3 Phase - Delta  2,5m Wood Cross arm / 2,5m Wood Cross arm","Each",{"v":431.25,"d":"R 431.25"},{"v":431.25,"d":"R 431.25"}]
[13.6,"D-DT-1745","3 Phase - Delta 2 x 2,5m Wood Cross arm / 1700 Steel Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[13.7,"D-DT-1745","3 Phase - Delta 2 x 2,5m Wood Cross arm / 2 x 2,5m Wood Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[13.799999999999999,"D-DT-1745","3 Phase - Delta 1 x 2,5m Wood Cross arm / 1700 Steel Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[13.9,"D-DT-1745","3 Phase - Delta 2,5m Wood Cross arm 2,5m Wood Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[{"v":13.1,"d":"13.10"},"D-DT-1784","3 Phase - Trips","Each",{"v":847.4,"d":"R 847.40"},{"v":847.4,"d":"R 847.40"}]
[13.11,"D-DT-1788","MV Heavy Conductor - 22kV 3 Phase - Vertical 800mm Spacing","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[13.12,"D-DT-1791","MV Heavy Conductor - 22kV 3 Phase - Vertical 800mm Spacing (Double Wood Poles)","Each",{"v":862.5,"d":"R 862.50"},{"v":862.5,"d":"R 862.50"}]
[{"v":13.129999999999999,"d":"13.13"},"D-DT-1792","MV Heavy Conductor - 22kV 3 Phase - Vertical 800mm Spacing (Double Wood Poles)","Each",{"v":862.5,"d":"R 862.50"},{"v":862.5,"d":"R 862.50"}]
[{"v":13.139999999999999,"d":"13.14"},"D-DT-1873","3 Phase - H-Pole / 2 x 4.5m Wooden Cross arm ","Each",{"v":819.16,"d":"R 819.16"},{"v":819.16,"d":"R 819.16"}]
[13.15,1715,"3 Phase - Vertical (600mm Spacing) Strain - Large(30-90°) Deviation Rx","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[13.16,1745,"3 Phase - Delta /2 x 2,5m wood x-arms/1700 WOOD x-arm - strain - (60° - 90°) deviation-RX","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[13.17,1745,"3 Phase - Delta /2 x 2,5m wood x-arms/ 3x2.5 wood x-arms - strain - (60° - 90°) deviation","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[13.18,1745,"3 Phase - Delta /2 x 2,5m wood x-arms/ 3x2.5 wood x-arms - strain - (60° - 90°) deviation-RX","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[13.19,1784,"3 Phase – Trips – Strain - Large(1°-90°) Deviation (Front view) -RX","Each",{"v":847.4,"d":"R 847.40"},{"v":847.4,"d":"R 847.40"}]
[{"v":13.2,"d":"13.20"},1873,"3 Phase H-pole /2X4.5m Wooden X-arm Strain Large (60-90˚) Deviation Rx","Each",{"v":819.16,"d":"R 819.16"},{"v":819.16,"d":"R 819.16"}]
[14,null,"Strainer - Terminal"]
[14.1,"D-DT-1706","3 Phase - Vertical (450mm Spacing) ","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[14.2,"D-DT-1716","3 Phase - Vertical (600mm Spacing) ","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[14.299999999999999,"D-DT-1736","3 Phase - Delta / 1,3m Steel Cross arm","Each",{"v":237.27,"d":"R 237.27"},{"v":237.27,"d":"R 237.27"}]
[14.4,"D-DT-1746","3 Phase - Delta / 2,5M Wood Cross arm","Each",{"v":266.93,"d":"R 266.93"},{"v":266.93,"d":"R 266.93"}]
[14.5,"D-DT-1749","3 Phase - Delta / 2 x 2,5m Wood Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[14.6,"D-DT-1756","3 Phase - Delta / 4,5M Wood Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[14.7,"D-DT-1766","3 Phase - H-pole / 3,5m Wood Cross arm","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[14.799999999999999,"D-DT-1769","3 Phase - H-pole / 2 x 3,5m Wood Cross arm","Each",{"v":819.16,"d":"R 819.16"},{"v":819.16,"d":"R 819.16"}]
[14.9,"D-DT-1776","3 Phase - H-pole / 4,5m Wood Cross arm","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[{"v":14.1,"d":"14.10"},"D-DT-1779","3 Phase - H-pole / 2 x 4,5m Wood Cross arm","Each",{"v":819.16,"d":"R 819.16"},{"v":819.16,"d":"R 819.16"}]
[14.11,"D-DT-1789","MV Heavy Conductor - 22kV 3 Phase - Vertical 800mm Spacing","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[14.12,"D-DT-1796","MV Heavy Conductor - 22kV H-Pole Braced ","Each",{"v":470.78,"d":"R 470.78"},{"v":470.78,"d":"R 470.78"}]
[{"v":14.129999999999999,"d":"14.13"},1746,"3 Phase - Delta / 2,5m Wood X-arm - Strain – Terminal -RX","Each",{"v":277.409286,"d":"R 277.41"},{"v":277.409286,"d":"R 277.41"}]
[{"v":14.139999999999999,"d":"14.14"},1749,"3 Phase - Delta / 2 x 2,5m Wood X-arm - Strain - Terminal -RX","Each",{"v":489.25800000000004,"d":"R 489.26"},{"v":489.25800000000004,"d":"R 489.26"}]
[14.15,1756,"3 Phase - Delta / 4,5m Wood X-arm - Strain – Terminal -RX","Each",{"v":489.25800000000004,"d":"R 489.26"},{"v":489.25800000000004,"d":"R 489.26"}]
[14.16,1766,"3 Phase - H-Pole / 3,5m Wood X-arm - Strain - Terminal -RX","Each",{"v":489.25800000000004,"d":"R 489.26"},{"v":489.25800000000004,"d":"R 489.26"}]
[14.17,1769,"3 Phase - H-Pole / 2 x 3,5m Wood X-arm - Strain – Terminal -RX","Each",{"v":851.30892,"d":"R 851.31"},{"v":851.30892,"d":"R 851.31"}]
[14.18,1776,"3 Phase – H-Pole / 4,5m Wood X-arm - Strain - Terminal -RX","Each",{"v":391.4064,"d":"R 391.41"},{"v":391.4064,"d":"R 391.41"}]
[14.19,1779,"3 Phase – H-Pole / 2 x 4,5m Wood X-arm – Strain – Terminal-RX ","Each",{"v":851.30892,"d":"R 851.31"},{"v":851.30892,"d":"R 851.31"}]
[{"v":14.2,"d":"14.20"},1789,"3 Phase - Vertical (800mm spacing) Strain -Terminal (10kN Wood Poles) Rx","Each",{"v":489.25800000000004,"d":"R 489.26"},{"v":489.25800000000004,"d":"R 489.26"}]
[{"v":14.209999999999999,"d":"14.21"},1716,"3 Phase - Vertical (600mm Spacing) Strain - Terminal Rx","Each",{"v":215.762778,"d":"R 215.76"},{"v":215.762778,"d":"R 215.76"}]
[{"v":14.219999999999999,"d":"14.22"},1796,"Heavy Conductor H-Pole Braced Terminal structure-RX","Each",{"v":489.25800000000004,"d":"R 489.26"},{"v":489.25800000000004,"d":"R 489.26"}]
[14.23,1793,"Heavy Conductor H-Pole Suspension Structure-RX","Each",{"v":489.25800000000004,"d":"R 489.26"},{"v":489.25800000000004,"d":"R 489.26"}]
[14.24,1793,"Heavy Conductor H-Pole Suspension Structure- With Spark Gap Device","Each",{"v":518.61348,"d":"R 518.61"},{"v":518.61348,"d":"R 518.61"}]
[14.25,1793,"Heavy Conductor H-Pole Suspension Structure- With Spark Gap Device-RX","Each",{"v":518.61348,"d":"R 518.61"},{"v":518.61348,"d":"R 518.61"}]
[15,null,"Take-Off"]
[15.1,"D-DT-1800","3 Phase Take-Off - Vertical (450mm Spacing)","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[15.2,"D-DT-1801","3 Phase Take-Off - Vertical (600mm Spacing)","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[15.299999999999999,"D-DT-1803","3 Phase Take-Off - Delta / 1.3m Steel Cross arm","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[15.4,"D-DT-1804","3 Phase Take-Of - 2,5M Wooden Cross arm","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[15.5,"D-DT-1805","3 Phase Take-Of - 2 x 2,5M Wooden Cross arm","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[15.6,"D-DT-1806","3 Phase Take-Of - H-Pole 3,5M Wooden Cross arm","Each",{"v":329.55,"d":"R 329.55"},{"v":329.55,"d":"R 329.55"}]
[15.7,"D-DT-1807","3 Phase Take-Of - H-Pole 2 x 3,5M Wooden Cross arm","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[15.799999999999999,"D-DT-1808","3 Phase Take-Off - 1.7m Steel Cross arm (Fox) ","Each",{"v":164.77,"d":"R 164.77"},{"v":164.77,"d":"R 164.77"}]
[15.9,"D-DT-1809","3 Phase Take-Off - 1.7m Steel Cross arm (Hare) ","Each",{"v":164.77,"d":"R 164.77"},{"v":164.77,"d":"R 164.77"}]
[{"v":15.1,"d":"15.10"},1801,"3 Phase Take-off – Vertical 600mm Spacing Rx","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[15.11,1804,"3 Phase Take-off - 2,5m Wooden X-arm-RX","Each",{"v":207.61,"d":"R 207.61"},{"v":207.61,"d":"R 207.61"}]
[15.12,1805,"3 Phase Take-off - 2 x 2,5m Wooden X-arm-RX","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[{"v":15.129999999999999,"d":"15.13"},1806,"3 Phase Take-off - H-Pole (3,5m Wooden X-arm)-RX","Each",{"v":329.55,"d":"R 329.55"},{"v":329.55,"d":"R 329.55"}]
[{"v":15.139999999999999,"d":"15.14"},1807,"3 Phase Take-off - H-Pole (2 x 3,5m Wooden X-arm) -RX","Each",{"v":376.62,"d":"R 376.62"},{"v":376.62,"d":"R 376.62"}]
[15.15,"(OU Specific Drawing No)","Erect goal posts, supply and erect temporary structures and traffic signs and regulate traffic during construction for all road crossings/railways crossings. (This includes any loss of production during road crossings and ensuring that access is maintained to roads and properties as well as any fees by Prov. Traffic Dept.) ","Each",{"v":2965.8354,"d":"R 2,965.84"},{"v":2965.8354,"d":"R 2,965.84"}]
["SUB-TOTAL E"]
["F",null,"ASSEMBLE MV STAYS"]
["Supply and install stays, flying stays, struts Hip Stay including backfilling & compaction (cement measured elsewhere).  Accessories include stay wire, stay rods, stay plates, soil anchors, stay insulators, guy grips stay mounting brackets, mounting hardware, anti climbing devices, stay guards and danger labels. Poles and excavations are measured elsewhere. The installation and erection of strut poles are measured here.  All hardware purchased will be paid elsewhere as cost plus fee.",{"$nulls":5},"Description change in red"]
[1.1,"D-DT-0341","Make-Off Convential Stay","Each",{"v":348.6061219852,"d":"R 348.61"},{"v":348.6061219852,"d":"R 348.61"}]
[1.2000000000000002,"D-DT-0343","Make-Off Flying Stay","Each",{"v":416.1214319031,"d":"R 416.12"},{"v":416.1214319031,"d":"R 416.12"}]
[1.3,"D-DT-0342/0351","Make-Off Strut Pole","Each",{"v":308.9649749699,"d":"R 308.96"},{"v":308.9649749699,"d":"R 308.96"}]
[1.4000000000000001,"D-DT-0344","Hip Stay","Each",{"v":545.473981518,"d":"R 545.47"},{"v":545.473981518,"d":"R 545.47"}]
[1.5000000000000002,"0357\n(Sh 1 of 3)","LV/MV-ROCK ANCHOR INSTALLATION (EXPANDABLE SHELL & RESIN TYPE) ","Each",{"v":245.74716,"d":"R 245.75"},{"v":245.74716,"d":"R 245.75"}]
[1.6,"0357\n(Sh 2 of 3)","LV/MV-ROCK ANCHOR INSTALLATION (2 EYED ROD AND PIN TYPE) ","Each",{"v":196.59564,"d":"R 196.60"},{"v":196.59564,"d":"R 196.60"}]
[1.7000000000000002,"0357\n(Sh 3 of 3)","MV- SOFT ROCK ANCHOR INSTALLATION","Each",{"v":196.59564,"d":"R 196.60"},{"v":196.59564,"d":"R 196.60"}]
["SUB-TOTAL F"]
["G",null,"ASSEMBLE SINGLE PHASE LV STRUCTURES"]
["Supply and erect LV support structures as per Eskom DDT 1100(use insulated/bare neutral ABC). Auxiliary equipment such as strain clamps, suspension clamps, cable ties, IPC's , end caps, LV shackle  insulators, binding wires, D brackets, dead end preforms, threaded rods, pigtail bolts, eyenuts, terminations to be included. Pole, stay and strut material and excavations are measured elsewhere.  All hardware purchased will be paid elsewhere as cost plus fee.A436",{"$nulls":5},"Description changes in red"]
[1,null,"A. List of single-phase ABC wood pole"]
[1.1,1153,"LV 1 phase insulated/bare neutral ABC Suspension Assembly (0°- 30°) ","Each",{"v":73.3887,"d":"R 73.39"},{"v":73.3887,"d":"R 73.39"}]
[1.2000000000000002,1154,"LV 1 phase insulated/bare neutral  ABC Terminal Assembly ","Each",{"v":97.8516,"d":"R 97.85"},{"v":97.8516,"d":"R 97.85"}]
[1.3,1155,"LV 1 phase insulated/bare neutral  ABC Strain Assembly (0°- 60°) ","Each",{"v":97.8516,"d":"R 97.85"},{"v":97.8516,"d":"R 97.85"}]
[1.4000000000000001,1156,"LV 1 phase insulated/bare neutral LV 2 phase bare neutral (60°- 90°)","Each",{"v":97.8516,"d":"R 97.85"},{"v":97.8516,"d":"R 97.85"}]
[1.5,1157,"LV 1 phase insulated/bare neutral ABC T from Intermediate ","Each",{"v":97.8516,"d":"R 97.85"},{"v":97.8516,"d":"R 97.85"}]
[1.6,1158,"LV 1 phase insulated/bare neutral ABC Cross Intermediate Suspension Assembly ","Each",{"v":122.31450000000001,"d":"R 122.31"},{"v":122.31450000000001,"d":"R 122.31"}]
[1.7000000000000002,1159,"LV 1 phase insulated/bare neutral ABC T from Strain ","Each",{"v":146.7774,"d":"R 146.78"},{"v":146.7774,"d":"R 146.78"}]
[1.8000000000000003,1160,"LV 1 phase insulated/bare neutral ABC X Intermediate-Strain Assembly ","Each",{"v":171.24030000000002,"d":"R 171.24"},{"v":171.24030000000002,"d":"R 171.24"}]
[null,null,"ASSEMBLE DUAL PHASE LV STRUCTURES"]
["Supply and erect LV support structures as per Eskom DDT 1100( use insulated/bare  neutral ABC). Auxiliary equipment such as strain clamps, suspension clamps, cable ties, IPC's , end caps, LV shackle  insulators, binding wires, D brackets, dead end preforms, threaded rods, pigtail bolts, eyenuts, terminations to be included. Pole, stay and strut material and excavations are measured elsewhere.  All hardware purchased will be paid elsewhere as cost plus fee.A436",{"$nulls":5},"Description changes in red"]
[2,null,"B. List of Dual - phase ABC wood pole"]
[2.1,1145,"LV 2 phase insulated/bare neutral ABC Suspension Assembly (0°- 30°) ","Each",{"v":73.3887,"d":"R 73.39"},{"v":73.3887,"d":"R 73.39"}]
[2.2,1146,"LV 2 phase insulated/bare neutral LABC Terminal Assembly ","Each",{"v":97.8516,"d":"R 97.85"},{"v":97.8516,"d":"R 97.85"}]
[2.3000000000000003,1147,"LV 2 phase insulated/bare neutral ABC Strain Assembly (0° - 60°) ","Each",{"v":97.8516,"d":"R 97.85"},{"v":97.8516,"d":"R 97.85"}]
[2.4000000000000004,1148,"LV 2 phase insulated/bare neutral ABC Strain Assembly (60° - 90°) ","Each",{"v":97.8516,"d":"R 97.85"},{"v":97.8516,"d":"R 97.85"}]
[2.5,1149,"LV 2 phase insulated/bare neutral ABC T from Intermediate ","Each",{"v":97.8516,"d":"R 97.85"},{"v":97.8516,"d":"R 97.85"}]
[2.6,1150,"LV 2 phase insulated/bare neutral ABC Intermediate Suspension Assembly ","Each",{"v":122.31450000000001,"d":"R 122.31"},{"v":122.31450000000001,"d":"R 122.31"}]
[2.7,1151,"LV 2 phase insulated/bare neutral ABC T from Strain ","Each",{"v":146.7774,"d":"R 146.78"},{"v":146.7774,"d":"R 146.78"}]
[2.8000000000000003,1152,"LV 2 phase insulated/bare neutral ABC X Intermediate-Strain Assembly ","Each",{"v":171.24030000000002,"d":"R 171.24"},{"v":171.24030000000002,"d":"R 171.24"}]
[null,null,"ASSEMBLE 3 PHASE LV STRUCTURES"]
["Supply and erect LV support structures as per Eskom DDT 1100( use insulated/bare neutral ABC). Auxiliary equipment such as strain clamps, suspension clamps, cable ties, IPC's , end caps, LV shackle  insulators, binding wires, D brackets, dead end preforms, threaded rods, pigtail bolts, eyenuts, terminations to be included. Pole, stay and strut material and excavations are measured elsewhere.  All hardware purchased will be paid elsewhere as cost plus fee.A436",{"$nulls":5},"Description changes in red"]
[3,null,"A. List of 3-phase ABC wood pole"]
[3.1,"D-DT-1100","LV - 3 Phase insulated/bare neutral ABC Suspension Assembly 0-30 Deg.","Each",{"v":91.8,"d":"R 91.80"},{"v":91.8,"d":"R 91.80"}]
[3.2,"D-DT-1121","LV - 3 Phase insulated/bare neutral ABC Strain Assembly 0-60 Deg.","Each",{"v":122.4,"d":"R 122.40"},{"v":122.4,"d":"R 122.40"}]
[3.3000000000000003,"D-DT-1122","LV - 3 Phase insulated/bare neutral ABC Strain Assembly 60-90 Deg.","Each",{"v":122.4,"d":"R 122.40"},{"v":122.4,"d":"R 122.40"}]
[3.4000000000000004,"D-DT-1120","LV - 3 Phase insulated/bare neutral ABC Terminal Assembly","Each",{"v":122.4,"d":"R 122.40"},{"v":122.4,"d":"R 122.40"}]
[3.5,"D-DT-1140","LV - 3 Phase insulated/bare neutral ABC T-Off Assembly from Intermediate","Each",{"v":122.4,"d":"R 122.40"},{"v":122.4,"d":"R 122.40"}]
[3.6,"D-DT-1141","LV - 3 Phase insulated/bare neutral ABC Cross Intermediate - Intermediate Assembly","Each",{"v":153,"d":"R 153.00"},{"v":153,"d":"R 153.00"}]
[3.7,"D-DT-1142","LV - 3 Phase insulated/bare neutral ABC T-Off Assembly From Strain","Each",{"v":183.6,"d":"R 183.60"},{"v":183.6,"d":"R 183.60"}]
[3.8000000000000003,"D-DT-1143","LV - 3 Phase insulated/bare neutral ABC Cross Intermediate - Strain Assembly","Each",{"v":214.2,"d":"R 214.20"},{"v":214.2,"d":"R 214.20"}]
["SUB-TOTAL G"]
["H",null,"ASSEMBLE LV STAYS"]
["Supply and install stays, flying stays, struts Short Stay including backfilling & compaction.  Accessories include stay wire, stay rods, stay plates, soil anchors, stay insulators, guy grips stay mounting brackets, mounting hardware, anti climbing devices, stay guards and danger labels.  Poles and excavations are measured elsewhere. The installation and erection of strut poles  are measured here. All hardware purchased will be paid elsewhere as cost plus fee."]
[1.1,"D-DT-0341","Make-Off Convential Stay","Each",{"v":331.17160210469996,"d":"R 331.17"},{"v":331.17160210469996,"d":"R 331.17"}]
[1.2000000000000002,"D-DT-0343","Make-Off Flying Stay","Each",{"v":395.32642148369996,"d":"R 395.33"},{"v":395.32642148369996,"d":"R 395.33"}]
[1.3,"D-DT-0342/0351","Make-Off Strut Pole","Each",{"v":293.52146672530006,"d":"R 293.52"},{"v":293.52146672530006,"d":"R 293.52"}]
[1.4000000000000001,"D-DT-0344","Make-Off Short Strut Pole","Each",{"v":293.52146672530006,"d":"R 293.52"},{"v":293.52146672530006,"d":"R 293.52"}]
["SUB-TOTAL H"]
["I",null,"POLE TOP BOX INSTALLATION"]
["Install on a wooden and/or concrete pole a pole mounted distribution box as specified complete with pole mounting brackets (including sealing), cable ties, PG clamps, miniature circuit breaker(s), neutral, phase and earth bars, insulated copper tails for connecting to LV ABC, insulation piercing connectors and factory installed cable openings. Included shall be the stainless steel strapping, buckles and terminations of the tails onto the LV ABC. Eskom D-DT standards as amended will apply."]
[1.1,"D-DT-3236","2 Way Fibre Glass Box for Split/Smart Metering","Each",{"v":173.34,"d":"R 173.34"},{"v":173.34,"d":"R 173.34"},"Drawing refering to does not specify Fibre glass box?"]
[1.2000000000000002,"D-DT-3236","4 Way Fibre Glass Box for Split/Smart Metering","Each",{"v":173.34,"d":"R 173.34"},{"v":173.34,"d":"R 173.34"},"Drawing refering to does not specify Fibre glass box?"]
[1.3,null,"6 Way Fibre Glass Box for Split/Smart Metering","Each",{"v":173.34,"d":"R 173.34"},{"v":173.34,"d":"R 173.34"},"Drawing refering to does not specify Fibre glass box?"]
[1.4,"D-DT-3055","8 Way Fibre Glass Box for Split/Smart Metering","Each",{"v":173.34,"d":"R 173.34"},{"v":173.34,"d":"R 173.34"},"Drawing refering to does not specify Fibre glass box?"]
[1.5,"D-DT-3236","2 Way Steel Box for Split/Smart Metering","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"Description change in red"]
[1.6,"D-DT-3236","4 Way Steel Box for Split/Smart Metering","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"Description change in red"]
[1.7,"D-DT-3236","6 Way Steel Box for Split/Smart Metering","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"Description change in red"]
[1.8,"D-DT-3236","8 Way Steel Box for Split/Smart Metering","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"Description change in red"]
[1.9,3055,"BOX,POLE TOP Split/Smart METER 2-WAY 50A D3055 ","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"Description change in red"]
["1.10",3055,"BOX,POLE TOP Split/Smart METER 4-WAY 50A D3055 ","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"Description change in red"]
[null,null,"BOX,POLE TOP Split/Smart METER 6-WAY 50A D3055 ","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"New additional activity and change in description"]
[1.11,3055,"BOX,POLE TOP Split/Smart METER 2-WAY 120A D3055 ","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"Description change in red"]
[1.12,3055,"BOX,POLE TOP Split/Smart METER 8-WAY 50A D3055","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"Description change in red"]
[1.13,"D-DT-0338","LV Services Ground (Cross arm) Mounted Small Power User Outdoor Supply","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"New activity"]
[1.14,"D-DT-0338","LV Services Pole (H-Pole F Bracket) mounted Large Power User Outdoor Supply","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"New activity"]
[1.15,"D-DT-0338","LV Services Pole Mounted Small Power User Outdoor Supply","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"New activity"]
[1.16,"D-DT-0338","LV Services Ground Mounted LPU Outdoor Supply","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"New activity"]
[1.17,"D-DT-0338","LV Services Ground (Cross Arm) Mounted SPU outdoor Supply (Away From Transformer)","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"New activity"]
[1.18,"D-DT-0338","LV Services Ground Mounted Large Power User < 200kVA Outdoor Supply (away from Transformer)","Each",{"v":260,"d":"R 260.00"},{"v":260,"d":"R 260.00"},"New activity"]
["SUB-TOTAL I"]
["J",null,"CONDUCTOR STRINGING (TENSION, REGULATE & BIND IN)"]
["Install Eskom issued marked conductor.  Material quantity to allow for 5% sag in addition to actual  conductor length quantity.  Installation includes handling, stringing and final sagging. This will be for greased/ ungreased conductor"]
[1.1,null,"Fox Conductor 1-Phase","m",{"v":3.7607997566999996,"d":"R 3.76"},{"v":3.7607997566999996,"d":"R 3.76"}]
[1.2000000000000002,null,"Fox Full Tension Joint*","Each",{"v":92.1975335312,"d":"R 92.20"},{"v":92.1975335312,"d":"R 92.20"}]
[1.3,null,"Mink Conductor 1-Phase","m",{"v":3.7607997566999996,"d":"R 3.76"},{"v":3.7607997566999996,"d":"R 3.76"}]
[1.4000000000000001,null,"Mink Full Tension Joint*","Each",{"v":92.1975335312,"d":"R 92.20"},{"v":92.1975335312,"d":"R 92.20"}]
[1.5,null,"Hare Conductor 1-Phase","m",{"v":3.7607997566999996,"d":"R 3.76"},{"v":3.7607997566999996,"d":"R 3.76"}]
[1.6,null,"Hare Full Tension Joint*","Each",{"v":92.1975335312,"d":"R 92.20"},{"v":92.1975335312,"d":"R 92.20"}]
[1.7000000000000002,null,"Chickadee Conductor 1-Phase","m",{"v":15.80167965,"d":"R 15.80"},{"v":15.80167965,"d":"R 15.80"}]
[1.8000000000000003,null,"Chickadee Full Tension Joint*","Each",{"v":173.81847614999998,"d":"R 173.82"},{"v":173.81847614999998,"d":"R 173.82"}]
[1.9000000000000001,null,"Kingbird Conductor 1-Phase","m",{"v":15.80167965,"d":"R 15.80"},{"v":15.80167965,"d":"R 15.80"}]
[{"v":1.1,"d":"1.10"},null,"Kingbird Full Tension Joint*","Each",{"v":173.81847614999998,"d":"R 173.82"},{"v":173.81847614999998,"d":"R 173.82"}]
[1.11,3136,"MV Bare AAAC  Pine Greased ","m",{"v":3.7607997566999996,"d":"R 3.76"},{"v":3.7607997566999996,"d":"R 3.76"}]
[1.12,null,"Pine Conductor Full Tension Joint","Each",{"v":92.1975335312,"d":"R 92.20"},{"v":92.1975335312,"d":"R 92.20"}]
[{"v":1.1300000000000001,"d":"1.13"},3136,"MV Bare AAAC  Oak Greased ","m",{"v":3.7607997566999996,"d":"R 3.76"},{"v":3.7607997566999996,"d":"R 3.76"}]
[{"v":1.1400000000000001,"d":"1.14"},null,"Oak Conductor Full Tension Joint","Each",{"v":92.1975335312,"d":"R 92.20"},{"v":92.1975335312,"d":"R 92.20"}]
[{"v":1.1500000000000001,"d":"1.15"},3136,"MV Bare AAAC 35mmsq Greased","m",{"v":3.7607997566999996,"d":"R 3.76"},{"v":3.7607997566999996,"d":"R 3.76"}]
[{"v":1.1600000000000001,"d":"1.16"},"0831","35mm sq. Full Tension Joint* 2 Core","Each",{"v":92.1975335312,"d":"R 92.20"},{"v":92.1975335312,"d":"R 92.20"}]
[{"v":1.1700000000000002,"d":"1.17"},"0831","35mm sq. Full Tension Joint* 3 Core","Each",{"v":138.8,"d":"R 138.80"},{"v":138.8,"d":"R 138.80"}]
[{"v":1.1800000000000002,"d":"1.18"},"0831","35mm sq. Full Tension Joint* 4 Core","Each",{"v":368.79,"d":"R 368.79"},{"v":368.79,"d":"R 368.79"}]
[{"v":1.1900000000000002,"d":"1.19"},null,"35 mm sq. ABC 3-phase","m",{"v":3.7607997566999996,"d":"R 3.76"},{"v":3.7607997566999996,"d":"R 3.76"},"Duplicated in 1.24 can be removed"]
[{"v":1.2000000000000002,"d":"1.20"},"0800 series","70mm sq. Full Tension Joint* 4 Core","Each",{"v":92.1975335312,"d":"R 92.20"},{"v":92.1975335312,"d":"R 92.20"}]
[{"v":1.2100000000000002,"d":"1.21"},null,"70 mm sq. ABC  3-phase","m",{"v":3.7607997566999996,"d":"R 3.76"},{"v":3.7607997566999996,"d":"R 3.76"},"Duplicated in 1.26 can be removed"]
[{"v":1.2200000000000002,"d":"1.22"},3141,"COND,ABC 2C XLPE 35SQ INS/Bare NEUT ","m",{"v":2.3,"d":"R 2.30"},{"v":2.3,"d":"R 2.30"},"Description change in red"]
[1.23,3141,"COND,ABC 3C XLPE 35SQ INS/Bare NEUT ","m",{"v":2.4462900000000003,"d":"R 2.45"},{"v":2.4462900000000003,"d":"R 2.45"},"Description change in red"]
[{"v":1.2400000000000002,"d":"1.24"},3141,"COND,ABC 4C XLPE 35SQ INS/Bare NEUT ","m",{"v":3.26172,"d":"R 3.26"},{"v":3.26172,"d":"R 3.26"},"Description change in red"]
[1.25,3141,"COND,ABC 3C XLPE 70SQ INS/Bare NEUT ","m",{"v":2.4462900000000003,"d":"R 2.45"},{"v":2.4462900000000003,"d":"R 2.45"},"Description change in red"]
[1.26,3141,"COND,ABC 4C XLPE 70SQ INS/Bare NEUT ","m",{"v":3.26172,"d":"R 3.26"},{"v":3.26172,"d":"R 3.26"},"Description change in red"]
[1.27,3141,"COND,ABC 4C XLPE 95SQ INS/Bare NEUT ","m",{"v":3.26,"d":"R 3.26"},null,"New activity"]
["SUB-TOTAL J"]
["K",null,"EQUIPMENT INSTALLATION"]
["Install Transformer/Recloser/Voltage Regulator/MV Metering Units as per relevant Eskom DDT 1800 Series Assembly Drawing and OU Specific SI Engineering Instructions. All Auxiliary Equipment to include  Station and Distribution MV, LV Surge Arrestors, Control Boxes, Metering Kiosks, Jumper Terminations, Anti Climbing Devices , LDPE Pipe Covered Jumpers as per 02TB-023 and Danger Labels, Channel Irons, Cradles, Standoff Insulators, Conductor Busbars and suitable Equipment Labels & X Arms. Pole Planting, Stays, Struts, Isolators Earthing Material and Excavations are elsewhere measured. Transformers/Reclosers/Voltage Regulators and MV Metering Units will be Eskom Free Issue Material.  Main Line Structures and Auxiliary Equipment are elsewhere measured. All material purchased will be paid elsewhere as cost plus fee."]
[1,null,"Transformers"]
[1.1,"D-DT-1862","Install 5-Pole Double Platform Mounted Transformer Structure","Each",{"v":2695.3125,"d":"R 2,695.31"},{"v":2695.3125,"d":"R 2,695.31"}]
[1.2,"D-DT-1863","Install 2-Pole Platform Mounted Transformer Structure","Each",{"v":2432.29,"d":"R 2,432.29"},{"v":2432.29,"d":"R 2,432.29"}]
[1.3,"D-DT-1864","Install 5-Pole Double Platform Mounted Transformer Structure (Out of Line)","Each",{"v":3678.75,"d":"R 3,678.75"},{"v":3678.75,"d":"R 3,678.75"}]
[1.4,"D-DT-1865","Install 2-Pole Platform Mounted Transformer Structure (Out of Line)","Each",{"v":2432.29,"d":"R 2,432.29"},{"v":2432.29,"d":"R 2,432.29"}]
[1.5,"D-DT-1865B","Transformer - Out- of- Line 100kVA to 200KVA","Each",{"v":2432.29,"d":"R 2,432.29"},{"v":2432.29,"d":"R 2,432.29"}]
[1.6,"D-DT-1866","Install Single Pole Mounted Out of Line Transformer Structure (Out of Line)","Each",{"v":2138.86,"d":"R 2,138.86"},{"v":2138.86,"d":"R 2,138.86"}]
[1.7,"D-DT-1866B","Transformer - Out- of- Line 16kVA to 100kVA/64kVA","Each",{"v":2138.86,"d":"R 2,138.86"},{"v":2138.86,"d":"R 2,138.86"}]
[1.8,"D-DT-3021","Relocate - 300-500kVA x 3-Phase ","Each",{"v":8208.9304403626,"d":"R 8,208.93"},{"v":8208.9304403626,"d":"R 8,208.93"}]
[1.9,"D-DT-3021","Install Transformer - 300-500kVA x 3-Phase ","Each",{"v":6616.1211316426,"d":"R 6,616.12"},{"v":6616.1211316426,"d":"R 6,616.12"}]
[{"v":1.1,"d":"1.10"},"D-DT-3021","Relocate - 200kVA x 3-Phase","Each",{"v":3987.8909621766998,"d":"R 3,987.89"},{"v":3987.8909621766998,"d":"R 3,987.89"}]
[1.11,"D-DT-3021","Install Transformer - 200kVA x 3-Phase ","Each",{"v":2432.2893418059,"d":"R 2,432.29"},{"v":2432.2893418059,"d":"R 2,432.29"}]
[1.12,"D-DT-3021","Relocate - 100kVA x 3-Phase ","Each",{"v":3987.8909621766998,"d":"R 3,987.89"},{"v":3987.8909621766998,"d":"R 3,987.89"}]
[1.13,"D-DT-3021","Install Transformer - 100kVA x 3-Phase ","Each",{"v":2432.2893418059,"d":"R 2,432.29"},{"v":2432.2893418059,"d":"R 2,432.29"}]
[1.16,"D-DT-3021","Relocate - 50kVA x 3-Phase","Each",{"v":2463.4081162632997,"d":"R 2,463.41"},{"v":2463.4081162632997,"d":"R 2,463.41"}]
[1.17,"D-DT-3021","Install Transformer - 50kVA x 3-Phase ","Each",{"v":2138.8626851585,"d":"R 2,138.86"},{"v":2138.8626851585,"d":"R 2,138.86"}]
[1.18,"D-DT-3021","Relocate - 25kVA x 3-Phase ","Each",{"v":2463.4081162632997,"d":"R 2,463.41"},{"v":2463.4081162632997,"d":"R 2,463.41"}]
[1.19,"D-DT-3021","Install Transformer - 25kVA x 3-Phase","Each",{"v":2138.8626851585,"d":"R 2,138.86"},{"v":2138.8626851585,"d":"R 2,138.86"}]
[{"v":1.2,"d":"1.20"},"D-DT-3021","Relocate Transformer - 16kVA x 1-Phase","Each",{"v":2463.4081162632997,"d":"R 2,463.41"},{"v":2463.4081162632997,"d":"R 2,463.41"}]
[1.22,"D-DT-3021","Install Transformer - 16kVA x 1-Phase ","Each",{"v":2138.8626851585,"d":"R 2,138.86"},{"v":2138.8626851585,"d":"R 2,138.86"}]
[1.23,null,"Install Labels  (Chromadek)","Each",{"v":462.3255431997,"d":"R 462.33"},{"v":462.3255431997,"d":"R 462.33"}]
[1.24,1860,"Transformer - 5-100kVA Single Pole Mounted ","Each",{"v":1647.21830625,"d":"R 1,647.22"},{"v":1647.21830625,"d":"R 1,647.22"}]
[1.25,1861,"TRANSFORMER - 100-200kVA / 2-POLE PLATFORM MOUNTED (H-POLE) GENERAL ARRANGEMENT","Each",{"v":1709.612142857143,"d":"R 1,709.61"},{"v":1709.612142857143,"d":"R 1,709.61"}]
[1.26,"D-FS 14414","TRANSFORMER - 100-200kVA / 2-POLE PLATFORM MOUNTED (H-POLE) GENERAL ARRANGEMENT","Each",{"v":1709.612142857143,"d":"R 1,709.61"},null,"FS only new activity  "]
[1.27,null,"Install 2.5/3.5cross arm on H-Pole with 3x Post insulators. For very long jumpers.","Each",{"v":425.63,"d":"R 425.63"},null,"New activity  "]
[2,null,"Transformer MV Protection"]
[2.1,"D-DT-1849","Equipment Links Cut-Outs Or Disconnections 2.5m Wood Cross arm / Single Pole","Each",{"v":425.63,"d":"R 425.63"},{"v":425.63,"d":"R 425.63"}]
[2.2,"D-DT-1850","Section / Equipment Links Or Disconnections 1.3m Steel Cross arm / Single Pole","Each",{"v":425.63,"d":"R 425.63"},{"v":425.63,"d":"R 425.63"}]
[2.3,"D-DT-1869","Section / Equipment Links Cut/Out Or Disconnections 1.7m Steel Cross arm/Single Pole","Each",{"v":255.38,"d":"R 255.38"},{"v":255.38,"d":"R 255.38"}]
[2.4,"D-DT-0261","Install Surge Arresters (3-phase)","Each",{"v":344.7083743382001,"d":"R 344.71"},{"v":344.7083743382001,"d":"R 344.71"}]
[2.5,null,"Supply and Install all Labels per structure, excludes pole aluminium label  (Chromadek)","Each",{"v":462.3255431997,"d":"R 462.33"},{"v":462.3255431997,"d":"R 462.33"},"Description change to supply & install"]
[3,null,"Transformer LV Protection"]
[3.1,"D-DT-0309","80A Morsdorf Type Fuses - 3-Phase","Set",{"v":188.5245726776,"d":"R 188.52"},{"v":188.5245726776,"d":"R 188.52"}]
[3.2,"D-DT-0309","125A Morsdorf Type Fuses - 3-Phase","Set",{"v":377.0702142614,"d":"R 377.07"},{"v":377.0702142614,"d":"R 377.07"}]
[3.3,"D-DT-0309","160A Morsdorf Type Fuses - 3-Phase","Set",{"v":377.0702142614,"d":"R 377.07"},{"v":377.0702142614,"d":"R 377.07"}]
[3.4,"D-DT-3034","150A MCCB - 3-Phase(Circuit breaker)","Each",{"v":377.0702142614,"d":"R 377.07"},{"v":377.0702142614,"d":"R 377.07"}]
[3.5,"D-DT-3034","300A MCCB - 3-Phase(Circuit breaker)","Each",{"v":412.95056151999995,"d":"R 412.95"},{"v":412.95056151999995,"d":"R 412.95"}]
[3.6,"0309","Three phase trf and LV fuse holder connection - ABC conductor- 40A NH00 ","Set",{"v":111.06156600000001,"d":"R 111.06"},{"v":111.06156600000001,"d":"R 111.06"}]
[3.7,"0309","Three phase trf and LV fuse holder connection - ABC conductor- 63A NH00","Set",{"v":111.06156600000001,"d":"R 111.06"},{"v":111.06156600000001,"d":"R 111.06"}]
[3.8,"0309","Dual phase trf and LV fuse holder connection - ABC conductor- 40A NH00 ","Set",{"v":111.06156600000001,"d":"R 111.06"},{"v":111.06156600000001,"d":"R 111.06"}]
[3.9,"0309","Dual phase trf and LV fuse holder connection - ABC conductor- 63A NH00","Set",{"v":111.06156600000001,"d":"R 111.06"},{"v":111.06156600000001,"d":"R 111.06"}]
[{"v":3.1,"d":"3.10"},"0309","Dual phase trf and LV fuse holder connection - ABC conductor- 80A NH00","Set",{"v":188.5245726776,"d":"R 188.52"},{"v":188.5245726776,"d":"R 188.52"}]
[3.11,"0309","Dual phase trf and LV fuse holder connection - ABC conductor- 125A NH00","Set",{"v":377.0702142614,"d":"R 377.07"},{"v":377.0702142614,"d":"R 377.07"}]
[3.12,"0309","Dual phase trf and LV fuse holder connection - ABC conductor- 160A NH00","Set",{"v":377.0702142614,"d":"R 377.07"},{"v":377.0702142614,"d":"R 377.07"}]
[3.13,"0309","Single phase trf and LV fuse holder connection - ABC conductor- 40A NH00 ","Set",{"v":111.06156600000001,"d":"R 111.06"},{"v":111.06156600000001,"d":"R 111.06"}]
[3.14,"0309","Single phase trf and LV fuse holder connection - ABC conductor- 63A NH00","Set",{"v":111.06156600000001,"d":"R 111.06"},{"v":111.06156600000001,"d":"R 111.06"}]
[3.15,"0309","Single phase trf and LV fuse holder connection - ABC conductor- 80A NH00","Set",{"v":188.5245726776,"d":"R 188.52"},{"v":188.5245726776,"d":"R 188.52"}]
[3.16,"0309","Single phase trf and LV fuse holder connection - ABC conductor- 125A NH00","Set",{"v":377.0702142614,"d":"R 377.07"},{"v":377.0702142614,"d":"R 377.07"}]
[3.17,"0309","Single phase trf and LV fuse holder connection - ABC conductor- 160A NH00","Set",{"v":377.0702142614,"d":"R 377.07"},{"v":377.0702142614,"d":"R 377.07"}]
[3.18,null,"Install Data Concentrator (Complete)","Each",{"v":120,"d":"R 120.00"},{"v":120,"d":"R 120.00"}]
[3.19,null,"Supply and Install all Labels per structure, excludes pole aluminium label  (Chromadek) To maximum of 3 LV feeders","Each",{"v":462.3255431997,"d":"R 462.33"},{"v":462.3255431997,"d":"R 462.33"},"Description change to supply & install"]
[4,null,"Pole Mounted Sectionaliser"]
[4.1,"D-DT-1821","Install Sectionaliser Structure","Each",{"v":955.69,"d":"R 955.69"},{"v":955.69,"d":"R 955.69"}]
[4.2,"D-DT-1828","Install Sectionaliser - Out-Of-Line Structure","Each",{"v":1433.53,"d":"R 1,433.53"},{"v":1433.53,"d":"R 1,433.53"}]
[4.3,"D-DT-1821","Install Sectionaliser","Each",{"v":1433.53,"d":"R 1,433.53"},{"v":1433.53,"d":"R 1,433.53"}]
[4.4,"D-DT-1848","Section Links Cut/Outs Or Disconnections 2.5m Wood Cross arm / Single Pole","Each",{"v":255.38,"d":"R 255.38"},{"v":255.38,"d":"R 255.38"}]
[4.5,"D-DT-1852","Equipment Links - Cut-Outs Or Disconnections - 3.5/4.5m Wood Cross arm / H-Pole","Each",{"v":425.63,"d":"R 425.63"},{"v":425.63,"d":"R 425.63"}]
[4.6,"D-DT-1853","Equipment Isolating (In-Out) Links - Cut-Outs Or Disconnections - 2 x 2.5m Wood Cross arm / H-Pole","Each",{"v":766.13,"d":"R 766.13"},{"v":766.13,"d":"R 766.13"}]
[4.7,"D-DT-1854","Equipment Isolating (In-Out) Links - Cut-Outs Or Disconnections - 4.5m Wood Cross arm / Out-Of-Line","Each",{"v":766.13,"d":"R 766.13"},{"v":766.13,"d":"R 766.13"}]
[4.8,"D-DT-1857","3 Phase Switch Disconnector Ganged, Link Stick Operated Horizontal Assembly H-Pole 1800 And 2200 Centres","Each",{"v":510.75,"d":"R 510.75"},{"v":510.75,"d":"R 510.75"}]
[4.9,"D-DT-1858","3 Phase Switch Disconnector Ganged, Link Stick Operated Assembly Single Pole Mounted ","Each",{"v":510.75,"d":"R 510.75"},{"v":510.75,"d":"R 510.75"}]
[{"v":4.1,"d":"4.10"},"D-DT-1875","Equipment Isolating (In-Out) Links Cut/Outs Or Disconnections 2x2.4m Steel Cross arm / H-Pole","Each",{"v":766.13,"d":"R 766.13"},{"v":766.13,"d":"R 766.13"}]
[4.11,"D-DT-0261","Install Surge Arresters","Each",{"v":344.7083743382001,"d":"R 344.71"},{"v":344.7083743382001,"d":"R 344.71"}]
[4.12,null,"Supply and Install all Labels per structure, excludes pole aluminium label  (Chromadek)","Each",{"v":462.3255431997,"d":"R 462.33"},{"v":462.3255431997,"d":"R 462.33"},"Description change to supply & install"]
[5,null,"Pole Mounted Recloser"]
[5.1,"D-DT-1825","Install Recloser Structure","Each",{"v":1464.76,"d":"R 1,464.76"},{"v":1464.76,"d":"R 1,464.76"}]
[5.2,"D-DT-1829","Install Recloser - Out-Of-Line Structure","Each",{"v":1674,"d":"R 1,674.00"},{"v":1674,"d":"R 1,674.00"}]
[5.3,"D-FS-15735","Install Recloser Structure","Each",{"v":1464.76,"d":"R 1,464.76"},null,"FS Only"]
[5.4,"D-FS-15688","Install Recloser Structure","Each",{"v":1464.76,"d":"R 1,464.76"},null,"FS Only"]
[5.5,3249,"Install Recloser Aux Supply Box","Each",{"v":260,"d":"R 260.00"},null,"New activity"]
[5.6,"D-DT-0272","Install Recloser On Existing Structure","Each",{"v":1674,"d":"R 1,674.00"},{"v":1674,"d":"R 1,674.00"}]
[5.7,"D-DT-1848","Section Links Cut/Oots Or Disconnections 2.5m Wood Cross arm / Single Pole","Each",{"v":255.38,"d":"R 255.38"},{"v":255.38,"d":"R 255.38"}]
[5.8,"D-DT-1852","Equipment Links - Cut-Outs Or Disconnections - 3.5/4.5m Wood Cross arm / H-Pole","Each",{"v":425.63,"d":"R 425.63"},{"v":425.63,"d":"R 425.63"}]
[5.9,"D-DT-1853","Equipment Isolating (In-Out) Links - Cut-Outs Or Disconnections - 2 x 2.5m Wood Cross arm / H-Pole","Each",{"v":766.13,"d":"R 766.13"},{"v":766.13,"d":"R 766.13"}]
["5.10","D-DT-1854","Equipment Isolating (In-Out) Links - Cut-Outs Or Disconnections - 4.5m Wood Cross arm / Out-Of-Line","Each",{"v":766.13,"d":"R 766.13"},{"v":766.13,"d":"R 766.13"}]
[5.11,"D-DT-1857","3 Phase Switch Disconnector Ganged, Link Stick Operated Horizontal Assembly H-Pole 1800 And 2200 Centres","Each",{"v":510.75,"d":"R 510.75"},{"v":510.75,"d":"R 510.75"}]
[5.12,"D-DT-1858","3 Phase Switch Disconnector Ganged, Link Stick Operated Assembly Single Pole Mounted ","Each",{"v":510.75,"d":"R 510.75"},{"v":510.75,"d":"R 510.75"}]
[5.13,"D-DT-1875","Equipment Isolating (In-Out) Links Cut/Outs Or Disconnections 2x2.4m Steel Cross arm / H-Pole","Each",{"v":766.13,"d":"R 766.13"},{"v":766.13,"d":"R 766.13"}]
[5.14,"D-DT-0270","Install Auxiliary Transformer","Each",{"v":2138.8626851585,"d":"R 2,138.86"},{"v":2138.8626851585,"d":"R 2,138.86"}]
[5.15,"D-DT-0261","Install Surge Arresters","Each",{"v":344.7083743382001,"d":"R 344.71"},{"v":344.7083743382001,"d":"R 344.71"}]
[5.16,null,"Supply and Install all Labels per structure, excludes pole aluminium label  (Chromadek)","Each",{"v":462.3255431997,"d":"R 462.33"},{"v":462.3255431997,"d":"R 462.33"},"Description change to supply & install"]
[5.17,"D-DT-1829B","Recloser structure – General arrangement (INCLUDING PMRTV) (sheet 1 of 2) (Bypass structure not included)","Each",{"v":1950.0426,"d":"R 1,950.04"},{"v":1950.0426,"d":"R 1,950.04"}]
[6,null,"Voltage Regulator"]
[6.1,"D-DT-1830","Install Voltage Regulator - 11/22kV 100/200A Open Delta Structure","Each",{"v":1989.75,"d":"R 1,989.75"},{"v":1989.75,"d":"R 1,989.75"}]
[6.2,"D-DT-1831","Install Voltage Regulator - 11/22kV 100/200A Closed Delta Structure","Each",{"v":1989.75,"d":"R 1,989.75"},{"v":1989.75,"d":"R 1,989.75"}]
[6.3,"D-DT-1833","Install Voltage Regulator - 11/22kV 100/200A Open Delta - Out-Of-Line Structure","Each",{"v":2274,"d":"R 2,274.00"},{"v":2274,"d":"R 2,274.00"}]
[6.4,"1833B","Regulator - 100 / 200A Open Delta – General Arrangement (sheet 1 of 3)","Each",{"v":2648.9826000000003,"d":"R 2,648.98"},{"v":2648.9826000000003,"d":"R 2,648.98"}]
[6.5,"D-DT-1834","Install Voltage Regulator - 11/22kV 100/200A Closed Delta - Out-Of-Line Structure","Each",{"v":2274,"d":"R 2,274.00"},{"v":2274,"d":"R 2,274.00"}]
[6.6,"1834B","Regulator - 100 / 200A Closed Delta - General Arrangement (Sheet 1 of 2)","Each",{"v":2648.9826000000003,"d":"R 2,648.98"},{"v":2648.9826000000003,"d":"R 2,648.98"}]
[6.7,"D-DT-3119","Install Voltage Regulator On Existing Structure","Each",{"v":2648.98,"d":"R 2,648.98"},{"v":2648.98,"d":"R 2,648.98"}]
[6.8,"D-DT-1848","Section Links Cut/Oots Or Disconnections 2.5m Wood Cross arm / Single Pole","Each",{"v":255.38,"d":"R 255.38"},{"v":255.38,"d":"R 255.38"}]
[6.9,"D-DT-1851","Equipment Links - Cut-Outs Or Disconnections - 2.5m Wood Cross arm / H-Pole","Each",{"v":255.38,"d":"R 255.38"},{"v":255.38,"d":"R 255.38"}]
[{"v":6.1,"d":"6.10"},"D-DT-1852","Equipment Links - Cut-Outs Or Disconnections - 3.5/4.5m Wood Cross arm / H-Pole","Each",{"v":425.63,"d":"R 425.63"},{"v":425.63,"d":"R 425.63"}]
[6.11,"D-DT-1854","Equipment Isolating (In-Out) Links - Cut-Outs Or Disconnections - 4.5m Wood Cross arm / Out-Of-Line","Each",{"v":425.63,"d":"R 425.63"},{"v":425.63,"d":"R 425.63"}]
[6.12,"D-DT-1857","3 Phase Switch Disconnector Ganged, Link Stick Operated Horizontal Assembly H-Pole 1800 And 2200 Centres","Each",{"v":510.75,"d":"R 510.75"},{"v":510.75,"d":"R 510.75"}]
[6.13,"D-DT-1858","3 Phase Switch Disconnector Ganged, Link Stick Operated Assembly Single Pole Mounted ","Each",{"v":510.75,"d":"R 510.75"},{"v":510.75,"d":"R 510.75"}]
[6.14,"D-DT-1874","Equipment Links Or Disconnections 2.4m Steel Cross arm / H-Pole","Each",{"v":766.13,"d":"R 766.13"},{"v":766.13,"d":"R 766.13"}]
[6.15,"D-DT-0261","Install Surge Arresters","Each",{"v":344.7083743382001,"d":"R 344.71"},{"v":344.7083743382001,"d":"R 344.71"}]
[6.16,null,"Supply and Install all Labels per structure, excludes pole aluminium label  (Chromadek)","Each",{"v":462.3255431997,"d":"R 462.33"},{"v":462.3255431997,"d":"R 462.33"},"Description change to supply & install"]
[7,null,"Pole Mounted CT-VT Unit"]
[7.1,"D-DT-1839","Install MV CT / VT Metering Bulk Tariff Out-Of-Line Structure","Each",{"v":1674,"d":"R 1,674.00"},{"v":1674,"d":"R 1,674.00"}]
[7.2,"D-DT-1840","Install MV CT / VT Metering Bulk Tariff In Line Structure","Each",{"v":1674,"d":"R 1,674.00"},{"v":1674,"d":"R 1,674.00"}]
[7.3,"D-DT-1841","Install CT/VT Metering Statistical Structure","Each",{"v":1989.75,"d":"R 1,989.75"},{"v":1989.75,"d":"R 1,989.75"}]
[7.4,"D-DT-1846","Install CT/VT Metering Statistical Out-Of-Line Structure","Each",{"v":1989.75,"d":"R 1,989.75"},{"v":1989.75,"d":"R 1,989.75"}]
[7.5,"D-DT-3118","Install CT/VT unit","Each",{"v":2274,"d":"R 2,274.00"},{"v":2274,"d":"R 2,274.00"}]
[7.6,"D-DT-1848","Section Links Cut/Oots Or Disconnections 2.5m Wood Cross arm / Single Pole","Each",{"v":255.38,"d":"R 255.38"},{"v":255.38,"d":"R 255.38"}]
[7.7,"D-DT-1850","Section / Equipment  Links Or Disconnections 1.3m Steel Cross arm / Single Pole","Each",{"v":194.04,"d":"R 194.04"},{"v":194.04,"d":"R 194.04"}]
[7.8,"D-DT-1852","Equipment Links - Cut-Outs Or Disconnections - 3.5/4.5m Wood Cross arm / H-Pole","Each",{"v":425.63,"d":"R 425.63"},{"v":425.63,"d":"R 425.63"}]
[7.9,"D-DT-1853","Equipment Isolating (In-Out) Links - Cut-Outs Or Disconnections - 2 x 2.5m Wood Cross arm / H-Pole","Each",{"v":766.13,"d":"R 766.13"},{"v":766.13,"d":"R 766.13"}]
[{"v":7.1,"d":"7.10"},"D-DT-1854","Equipment Isolating (In-Out) Links - Cut-Outs Or Disconnections - 4.5m Wood Cross arm / Out-Of-Line","Each",{"v":425.63,"d":"R 425.63"},{"v":425.63,"d":"R 425.63"}]
[7.11,"D-DT-1857","3 Phase Switch Disconnector Ganged, Link Stick Operated Horizontal Assembly H-Pole 1800 And 2200 Centres","Each",{"v":510.75,"d":"R 510.75"},{"v":510.75,"d":"R 510.75"}]
[7.12,"D-DT-1858","3 Phase Switch Disconnector Ganged, Link Stick Operated Assembly Single Pole Mounted ","Each",{"v":510.75,"d":"R 510.75"},{"v":510.75,"d":"R 510.75"}]
[7.13,"D-DT-1875","Equipment Isolating (In-Out) Links Cut/Outs Or Disconnections 2x2.4m Steel Cross arm / H-Pole","Each",{"v":766.13,"d":"R 766.13"},{"v":766.13,"d":"R 766.13"}]
[7.14,"D-DT-3236","Install CT/VT Metering Kiosk","Each",{"v":144.8171267657,"d":"R 144.82"},{"v":144.8171267657,"d":"R 144.82"}]
[7.15,"D-DT-0261","Install Surge Arresters","Each",{"v":344.7083743382001,"d":"R 344.71"},{"v":344.7083743382001,"d":"R 344.71"}]
[7.16,null,"Supply and Install all Labels per structure, excludes pole aluminium label  (Chromadek)","Each",{"v":462.3255431997,"d":"R 462.33"},{"v":462.3255431997,"d":"R 462.33"},"Description change to supply & install"]
[8,null,"Pole Mounted Shunt Capacitor Banks"]
[8.1,"D-DT-1832","Install Capacitor Structure","Each",{"v":2274,"d":"R 2,274.00"},{"v":2274,"d":"R 2,274.00"}]
[8.2,"D-DT-3218","Install Capacitor Bank","Each",{"v":2274,"d":"R 2,274.00"},{"v":2274,"d":"R 2,274.00"}]
[8.3,"D-DT-1849","Equipment Links Cut-Outs Or Disconnections 2.5m Wood Cross arm / Single Pole","Each",{"v":425.63,"d":"R 425.63"},{"v":425.63,"d":"R 425.63"}]
[8.4,"D-DT-1850","Section / Equipment Links Or Disconnections 1.3m Steel Cross arm / Single Pole","Each",{"v":425.63,"d":"R 425.63"},{"v":425.63,"d":"R 425.63"}]
[8.5,"D-DT-0261","Install Surge Arresters","Each",{"v":344.7083743382001,"d":"R 344.71"},{"v":344.7083743382001,"d":"R 344.71"}]
[8.6,null,"Supply and Install all Labels per structure, excludes pole aluminium label  (Chromadek)","Each",{"v":462.3255431997,"d":"R 462.33"},{"v":462.3255431997,"d":"R 462.33"},"Description change to supply & install"]
[9,null,"Line Arrester"]
[9.1,null,"Install Equipment Links","Each",{"v":572.5,"d":"R 572.50"},{"v":572.5,"d":"R 572.50"}]
[9.2,"D-DT-1842","Line Arresters 1.3m Long Steel Cross arm Staggered Vertical Configuration","Each",{"v":344.7083743382001,"d":"R 344.71"},{"v":344.7083743382001,"d":"R 344.71"}]
[9.3,"D-DT-1843","Line Arresters 2.5m Long Wooden Cross arm Vertical Configuration","Each",{"v":344.7083743382001,"d":"R 344.71"},{"v":344.7083743382001,"d":"R 344.71"}]
[9.4,"D-DT-1844","Line Arresters H-Pole Configuration","Each",{"v":398.7241765969959,"d":"R 398.72"},{"v":398.7241765969959,"d":"R 398.72"}]
[9.5,"D-DT-1845","Line Arresters Delta Configuration","Each",{"v":344.7083743382001,"d":"R 344.71"},{"v":344.7083743382001,"d":"R 344.71"}]
[9.6,null,"Supply and Install all Labels per structure, excludes pole aluminium label  (Chromadek)","Each",{"v":462.3255431997,"d":"R 462.33"},{"v":462.3255431997,"d":"R 462.33"},"Description change to supply & install"]
[10,null,"3 Phase Sectional Links"]
[10.1,"D-DT-1847","Section Links Cut/Outs Or Disconnections 3.5/4.5m Wood Cross arm / H-Pole","Each",{"v":425.63,"d":"R 425.63"},{"v":425.63,"d":"R 425.63"}]
[10.2,"D-DT-1848","Section Links Cut/Outs Or Disconnections 2.5m Wood Cross arm / Single Pole","Each",{"v":255.38,"d":"R 255.38"},{"v":255.38,"d":"R 255.38"}]
[10.3,"D-DT-1850","Section / Equipment  Links Or Disconnections 1.3m Steel Cross arm / Single Pole","Each",{"v":255.38,"d":"R 255.38"},{"v":255.38,"d":"R 255.38"}]
[10.4,"D-DT-1857","3 Phase Switch Disconnector Ganged, Link Stick Operated Horizontal Assembly H-Pole 1800 And 2200 Centres","Each",{"v":510.75,"d":"R 510.75"},{"v":510.75,"d":"R 510.75"}]
[10.5,"D-DT-1858","3 Phase Switch Disconnector Ganged, Link Stick Operated Assembly Single Pole Mounted ","Each",{"v":510.75,"d":"R 510.75"},{"v":510.75,"d":"R 510.75"}]
[10.6,"D-DT-1869","Section / Equipment Links Cut/Out Or Disconnections 1.7m Steel Cross arm/Single Pole","Each",{"v":255.38,"d":"R 255.38"},{"v":255.38,"d":"R 255.38"}]
[10.7,"D DT 3086","CUT - OUT (Single Phase)","Each",{"v":125,"d":"R 125.00"},null,"New activity"]
[10.8,null,"Supply and Install all Labels per structure, excludes pole aluminium label  (Chromadek)","Each",{"v":462.3255431997,"d":"R 462.33"},{"v":462.3255431997,"d":"R 462.33"},"Description change to supply & install"]
[11,null,"Bird Flight Diverter"]
[11.1,"D-DT-3029","Install Bird Flight Diverter","Each",{"v":7,"d":"R 7.00"},{"v":7,"d":"R 7.00"}]
[12,null,"Miniature Substation"]
[12.1,null,"Prepare Site Including Excavation and Compaction for Pre-Cast Plinth","m2",{"v":347.56,"d":"R 347.56"},{"v":347.56,"d":"R 347.56"}]
[12.2,"D-DT-0859","Install Pre-Cast Plinth","Each",{"v":4672.4723968802,"d":"R 4,672.47"},{"v":4672.4723968802,"d":"R 4,672.47"}]
[12.3,"D-DT-0859","Install Miniature Substation","Each",{"v":2005.7598702400003,"d":"R 2,005.76"},{"v":2005.7598702400003,"d":"R 2,005.76"}]
[12.4,"D-DT-3034","MCCB - 3-Phase","Each",{"v":412.95,"d":"R 412.95"},{"v":412.95,"d":"R 412.95"}]
[12.5,null,"Vermin Proofing","Each",{"v":463.67,"d":"R 463.67"},{"v":463.67,"d":"R 463.67"}]
[12.6,null,"Stencilling (paint)","Each",{"v":17.7,"d":"R 17.70"},{"v":17.7,"d":"R 17.70"},"Description change in red"]
[12.7,null,"Install Labels  (Chromadek and Aluminium)","SET",{"v":462.3255431997,"d":"R 462.33"},{"v":462.3255431997,"d":"R 462.33"}]
[12.8,"D-DT-3409","Install Vertical Fuse Pillar","Each",{"v":225,"d":"R 225.00"},{"v":225,"d":"R 225.00"}]
[12.9,"D-DT-3181","Install NH02 Fuse","Each",{"v":225,"d":"R 225.00"},{"v":225,"d":"R 225.00"}]
[13,null,"Ring Main Unit"]
[13.1,null,"Prepare Site Including Excavation and Compaction for Pre-Cast Plinth","m2",{"v":347.56,"d":"R 347.56"},{"v":347.56,"d":"R 347.56"}]
[13.2,"D-DT-0863","Install Pre-Cast Plinth","Each",{"v":2359.7174944,"d":"R 2,359.72"},{"v":2359.7174944,"d":"R 2,359.72"}]
[13.3,"D-DT-8060","Install Ring Main Unit","Each",{"v":1415.83049664,"d":"R 1,415.83"},{"v":1415.83049664,"d":"R 1,415.83"}]
[13.4,null,"Vermin Proofing","Each",{"v":463.67,"d":"R 463.67"},{"v":463.67,"d":"R 463.67"}]
[13.5,null,"Stencilling (paint)","p/letter",{"v":17.697881208,"d":"R 17.70"},{"v":17.697881208,"d":"R 17.70"},"Description change in red"]
[13.6,null,"Install Labels  (Chromadek)","Each",{"v":462.3255431997,"d":"R 462.33"},{"v":462.3255431997,"d":"R 462.33"}]
[14,null,"Ground Mounted CT-VT Unit"]
[14.1,null,"Prepare Site Including Excavation and Compaction for Pre-Cast Plinth","m2",{"v":347.56,"d":"R 347.56"},{"v":347.56,"d":"R 347.56"}]
[14.2,"D-DT-0865","Install Pre-Cast Plinth","Each",{"v":2359.7174944,"d":"R 2,359.72"},{"v":2359.7174944,"d":"R 2,359.72"}]
[14.3,"D-DT-0865","Install CT-VT Unit","Each",{"v":1002.8799351200001,"d":"R 1,002.88"},{"v":1002.8799351200001,"d":"R 1,002.88"}]
[14.4,null,"Vermin Proofing","Each",{"v":463.67,"d":"R 463.67"},{"v":463.67,"d":"R 463.67"}]
[14.5,null,"Stencilling (paint)","p/letter",{"v":17.697881208,"d":"R 17.70"},{"v":17.697881208,"d":"R 17.70"},"Description change in red"]
[14.6,null,"Install Labels  (Chromadek)","Each",{"v":462.3255431997,"d":"R 462.33"},{"v":462.3255431997,"d":"R 462.33"}]
[15,null,"Meter Kiosk"]
[15.1,null,"Prepare Site Including Excavation and Compaction for Pre-Cast Plinth","m2",{"v":347.56,"d":"R 347.56"},{"v":347.56,"d":"R 347.56"}]
[15.2,"D-DT-0865","Install Pre-Cast Plinth","Each",{"v":2772.6680559199995,"d":"R 2,772.67"},{"v":2772.6680559199995,"d":"R 2,772.67"}]
[15.3,"D-DT-0865","Install LPU Meter Kiosk","Each",{"v":144.8171267657,"d":"R 144.82"},{"v":144.8171267657,"d":"R 144.82"}]
[15.4,"D-DT-3236","4 Way High Risk Steel Kiosk ","Each",{"v":711.33,"d":"R 711.33"},{"v":711.33,"d":"R 711.33"}]
[15.5,"D-DT-3236","6 Way High Risk Steel Kiosk ","Each",{"v":711.33,"d":"R 711.33"},{"v":711.33,"d":"R 711.33"}]
[15.6,"D-DT-3236","8 Way High Risk Steel Kiosk ","Each",{"v":711.33,"d":"R 711.33"},{"v":711.33,"d":"R 711.33"}]
[15.7,"D-DT-3236","12 Way High Risk Steel Kiosk ","Each",{"v":711.33,"d":"R 711.33"},{"v":711.33,"d":"R 711.33"}]
[15.8,"D-DT-3236 / 1034","Data concentrator/RAT kiosk ","Each",{"v":260,"d":"R 260.00"},null,"New activity"]
[15.9,null,"Energy Management Units (Meter)","Each",{"v":405.15506622600003,"d":"R 405.16"},{"v":405.15506622600003,"d":"R 405.16"}]
["15.10",null,"Vermin Proofing","Each",{"v":463.67,"d":"R 463.67"},{"v":463.67,"d":"R 463.67"}]
[15.11,null,"Stencilling (paint)","p/letter",{"v":17.697881208,"d":"R 17.70"},{"v":17.697881208,"d":"R 17.70"},"Description change in red"]
[15.12,null,"Supply and Install all Labels per kiosk, excludes cable aluminium label  (Chromadek)","Each",{"v":462.3255431997,"d":"R 462.33"},{"v":462.3255431997,"d":"R 462.33"},"Description change to supply & install"]
["SUB-TOTAL K"]
["L",null,"EARTHING INSTALLATION"]
["MV & LV Earthing Trenching shall include Excavation, Backfilling, Compaction and Installation of electrode and conductor as per the Eskom Standard for Earthing"]
[1,null,"Transformer - MV Earthing"]
[1.1,null,"Excavation - length long, 0.5m deep and 0.6m wide","m3",{"v":147.4823434,"d":"R 147.48"},{"v":147.4823434,"d":"R 147.48"}]
[1.2000000000000002,"D-DT-3139","16mm sq. Bare Stranded Cu Conductor","m",{"v":11.798587471999998,"d":"R 11.80"},{"v":11.798587471999998,"d":"R 11.80"}]
[1.3,"D-DT-3137","16mm sq. Insulated Stranded Cu Conductor","m",{"v":11.798587471999998,"d":"R 11.80"},{"v":11.798587471999998,"d":"R 11.80"}]
[1.4000000000000001,"D-DT-3091","Earth Electrode (Type as per the design)","Each",{"v":247.770336912,"d":"R 247.77"},{"v":247.770336912,"d":"R 247.77"}]
[1.5,null,"Backfill - length long, 0.5m deep and 0.6m wide","m3",{"v":120.34559221439999,"d":"R 120.35"},{"v":120.34559221439999,"d":"R 120.35"}]
[2,null,"Transformer - LV Earthing"]
[2.1,null,"Excavation - length long, 0.5m deep and 0.6m wide","m3",{"v":147.4823434,"d":"R 147.48"},{"v":147.4823434,"d":"R 147.48"}]
[2.2,"D-DT-3139","16mm sq. Bare Stranded Cu Conductor","m",{"v":11.798587471999998,"d":"R 11.80"},{"v":11.798587471999998,"d":"R 11.80"}]
[2.3000000000000003,"D-DT-3137","16mm sq. Insulated Stranded Cu Conductor","m",{"v":11.798587471999998,"d":"R 11.80"},{"v":11.798587471999998,"d":"R 11.80"}]
[2.4000000000000004,"D-DT-3091","Earth Electrode (Type as per the design)","Each",{"v":247.770336912,"d":"R 247.77"},{"v":247.770336912,"d":"R 247.77"}]
[2.5,null,"Backfill - length long, 0.5m deep and 0.6m wide","m3",{"v":120.34559221439999,"d":"R 120.35"},{"v":120.34559221439999,"d":"R 120.35"}]
[3,null,"Other Overhead System Equipment Earthing - Capacitor Bank / CT-VT Unit / Line Arrester / Recloser / Sectionaliser / Voltage Regulator"]
[3.1,null,"Excavation - length long, 0.5m deep and 0.6m wide","m3",{"v":147.4823434,"d":"R 147.48"},{"v":147.4823434,"d":"R 147.48"}]
[3.2,"D-DT-3139","16mm sq. Bare Stranded Cu Conductor","m",{"v":11.798587471999998,"d":"R 11.80"},{"v":11.798587471999998,"d":"R 11.80"}]
[3.3,"D-DT-3137","16mm sq. Insulated Stranded Cu Conductor","m",{"v":11.798587471999998,"d":"R 11.80"},{"v":11.798587471999998,"d":"R 11.80"}]
[3.4,"D-DT-3091","Earth Electrode (Type as per the design)","Each",{"v":247.770336912,"d":"R 247.77"},{"v":247.770336912,"d":"R 247.77"}]
[3.5,null,"Backfill - length long, 0.5m deep and 0.6m wide","m3",{"v":120.34559221439999,"d":"R 120.35"},{"v":120.34559221439999,"d":"R 120.35"}]
[4,null,"Other Underground System Equipment Earthing - Miniature Substation / Ring Main Unit / CT-VT Unit"]
[4.1,null,"Excavation - length long, 0.5m deep and 0.6m wide","m3",{"v":147.4823434,"d":"R 147.48"},{"v":147.4823434,"d":"R 147.48"}]
[4.2,"D-DT-3139","16mm sq. Bare Stranded Cu Conductor","m",{"v":11.798587471999998,"d":"R 11.80"},{"v":11.798587471999998,"d":"R 11.80"}]
[4.3,"D-DT-3091","Earth Electrode (Type as per the design)","Each",{"v":247.770336912,"d":"R 247.77"},{"v":247.770336912,"d":"R 247.77"}]
[4.4,null,"Backfill - length long, 0.5m deep and 0.6m wide","m3",{"v":120.34559221439999,"d":"R 120.35"},{"v":120.34559221439999,"d":"R 120.35"}]
[5,null,"Earthing Installation excluding trenching",{"$nulls":3},"Remove duplicate of above activity"]
[5.1,"D-DT-3066","MV Earthing (Type 1 Crowfoot)","Each",{"v":2800,"d":"R 2,800.00"},{"v":2800,"d":"R 2,800.00"},"Remove duplicate of above activity"]
[5.199999999999999,"D-DT-3066","MV Earthing (Type 2 Crowfoot)","Each",{"v":3100,"d":"R 3,100.00"},{"v":3100,"d":"R 3,100.00"},"Remove duplicate of above activity"]
[5.3,"D-DT-3066","MV Earthing (Type 3 Crowfoot)","Each",{"v":3400,"d":"R 3,400.00"},{"v":3400,"d":"R 3,400.00"},"Remove duplicate of above activity"]
[5.3999999999999995,"D-DT-3066","MV Earthing (Type 4 Crowfoot)","Each",{"v":3600,"d":"R 3,600.00"},{"v":3600,"d":"R 3,600.00"},"Remove duplicate of above activity"]
["SUB-TOTAL - L"]
["M",null,"SERVICE CONNECTION INSTALLATION"]
["House Connections include installation of ready board, mounting hardware, wooden backboards, customer interface units, conduit pipe, excavations and backfilling of underground connection, capturing of customer data including GPS coordinates. Digging and bulleting for road crossing including installation of sleeves and warning tape are measured here"]
[1.1,"D-DT-0360/361","Overhead service connection direct to dwelling or kicker pole(from the pole top box to the pre-paid meter)  (Type A) to brick dwelling","Each",{"v":72.03,"d":"R 72.03"},{"v":72.03,"d":"R 72.03"},"Description change in red"]
[1.2000000000000002,"D-DT-0360","Overhead service connection with service pole (from the pole top box to the pre-paid meter) (Type B) to mud dwelling","Each",{"v":72.03,"d":"R 72.03"},{"v":72.03,"d":"R 72.03"},"Remove item activity in above item"]
[1.3,"D-DT-0367","Underground Service Connection","Each",{"v":490.800169929,"d":"R 490.80"},{"v":490.800169929,"d":"R 490.80"}]
[1.4000000000000001,null,"25mm Conduit LDPE Pipe","m",{"v":147.4823434,"d":"R 147.48"},{"v":147.4823434,"d":"R 147.48"}]
[1.5,"D-DT-0854","Excavation - 0.75m Deep and 0.45 Wide","m3",{"v":147.48,"d":"R 147.48"},{"v":147.48,"d":"R 147.48"}]
[1.6,null,"Road Crossing - Digging","m",{"v":926.1891165520001,"d":"R 926.19"},{"v":926.1891165520001,"d":"R 926.19"}]
[1.7000000000000002,null,"Road Crossing - Bulleting","Each",{"v":421.59,"d":"R 421.59"},{"v":421.59,"d":"R 421.59"}]
[1.8000000000000003,"D-DT-8018","Install Sleeves","m",{"v":4.7194349888,"d":"R 4.72"},{"v":4.7194349888,"d":"R 4.72"}]
[1.9000000000000001,"D-DT-0854","Laying of Warning Tape","m",{"v":2.75,"d":"R 2.75"},{"v":2.75,"d":"R 2.75"},"Price too high same as stringing conductor and dynamometer not needed for activity. Remove activity is included in backfill"]
[{"v":1.1,"d":"1.10"},"D-DT-0854","Backfill - 0.75m Deep and 0.45 Wide (includes laying of warning tape)","m3",{"v":120.35,"d":"R 120.35"},{"v":120.35,"d":"R 120.35"},"Description change in red"]
[2,null,"Split / Smart Metering"]
[2.1,"D-DT-3145","Customer Interface Unit","Each",{"v":35,"d":"R 35.00"},{"v":35,"d":"R 35.00"},"Need clarity, if this item is not included in activity below 2.2"]
[2.2,"D-DT-3176","Split/Smart  Meter Ready-Board ","Each",{"v":176.97881208,"d":"R 176.98"},{"v":176.97881208,"d":"R 176.98"},"Name changes to Split/Smart metering"]
[2.3000000000000003,"D-ST-2351","Wooden Backboard for Ready board mounting (for Tin and Mud houses) as specified in design","Each",{"v":147.4823434,"d":"R 147.48"},{"v":147.4823434,"d":"R 147.48"},"Description change in red"]
[2.4,null,"Split/Smart Meter Installation","Each",{"v":325,"d":"R 325.00"},{"v":325,"d":"R 325.00"},"Name changes to Split/Smart metering"]
[2.5,null,"Capture and Upload of Customer Data New & Existing Including GPS Coordinates","Each",{"v":9.72,"d":"R9.72"},{"v":9.72,"d":"R9.72"}]
["SUB-TOTAL M"]
["N",null,"Service Conductor Installation:\nAccessories for Service Conductor installation shall include installation of pigtails, bolts, strain clamps,  threaded rod, cable saddles, stringing of all types of service cable.  Installation of poles and its accessories are measured elsewhere"]
[1,"D-DT-3140","6mm sq. Tinned Copper Airdac with Communication Core","m",{"v":2.14,"d":"R2.14"},{"v":2.14,"d":"R2.14"}]
[3,"D-DT-0360","Connection to house","Each",{"v":27.38957806,"d":"R27.39"},{"v":27.38957806,"d":"R27.39"},"Remove if the activity is included under 360/361"]
[4,"D-DT-0361","Service Pole Dressing","Each",{"v":27.38957806,"d":"R27.39"},{"v":27.38957806,"d":"R27.39"},"Remove if the activity is included under 360/362"]
[5,"D-DT-3128","16mm sq. Underground","m",{"v":6.44,"d":"R6.44"},{"v":6.44,"d":"R6.44"}]
[6,"0366","Service suspension assembly","Each",{"v":24.4629,"d":"R 24.46"},{"v":24.4629,"d":"R 24.46"}]
[7,"0384","Service strain assembly/arrangement","Each",{"v":48.9258,"d":"R 48.93"},{"v":48.9258,"d":"R 48.93"}]
["SUB-TOTAL N"]
["O","Underground Cable Installation:\ninstallation of underground cable include trenching for excavation in general trench, rail/road crossing or along the road,  directional drilling & excavation for end pits, backfilling of trench, supply of accessories includes appropriate sleeves, supply & compaction of imported bedding and blanket soil, laying of warning tape and installation of cable route markers. Laying of cable shall be in accordance with Eskom standard of laying cables. After the execution of the works, reinstatement on gardens, pavements, driveways and tarred surfaces shall be measured here "]
[1,null,"Trenching"]
[1.1,"D-DT-0854","Excavation - General Trench -  1.0m Deep and 0.45m Wide","m3",{"v":147.48,"d":"R147.48"},{"v":147.48,"d":"R147.48"}]
[1.2,"D-DT-0854","Excavation - Rail/Road Crossing Trench -  1.6m Deep and 0.45m Wide","m3",{"v":147.48,"d":"R147.48"},{"v":147.48,"d":"R147.48"}]
[1.3,"D-DT-0854","Excavation - Along The Road Trench - 1.3m Deep and 0.45m Wide","m3",{"v":147.48,"d":"R147.48"},{"v":147.48,"d":"R147.48"}]
[1.4,null,"Install Barricading ","m",{"v":41.29505615200001,"d":"R41.30"},{"v":41.29505615200001,"d":"R41.30"}]
[1.5,null,"Install Shoring","m",{"v":225,"d":"R225.00"},{"v":225,"d":"R225.00"}]
[1.6,"D-DT-0854","Compact Blanket Soil","m2",{"v":120.35,"d":"R120.35"},{"v":120.35,"d":"R120.35"}]
[1.7,"D-DT-0854","Sifted Soil - 0.25m High and 0.45m Wide","m3",{"v":120.34559221439999,"d":"R 120.35"},{"v":120.34559221439999,"d":"R 120.35"}]
[1.8,null,"Dispose of unused Excavated Material at approved disposal site","m3",{"v":245,"d":"R 245.00"},{"v":245,"d":"R 245.00"}]
[1.9,"D-DT-0854","Imported Soil - 0.25m High and 0.45m Wide","m3",{"v":383.45409284,"d":"R 383.45"},{"v":383.45409284,"d":"R 383.45"}]
[2,null,"Road & Rail Crossing"]
[2.1,null,"Directional Drilling (Supply Invoice + 5%)","m",{"v":0,"d":"R 0.00"},{"v":0,"d":"R 0.00"}]
[2.2,null,"Excavate Start and End Pits","m3",{"v":147.4823434,"d":"R 147.48"},{"v":147.4823434,"d":"R 147.48"}]
[2.3,null,"Supply and Install appropriate sleeve","Each",{"v":321.59,"d":"R 321.59"},{"v":321.59,"d":"R 321.59"}]
[2.4,null,"Rail, river and Road -pipe jacking method including access holes, shoring as well as handling of equipment-(outsourced) Supply Invoice + 5%","m",{"v":0,"d":"R 0.00"},{"v":0,"d":"R 0.00"}]
[3,null,"Road crossing trench import of backfill material and compaction"]
[3.1,"D-DT0854","Application of tar according to municipal standard - Supply Invoice + 5%","m2",{"v":0,"d":"R 0.00"},{"v":0,"d":"R 0.00"}]
[3.2,null,"Bedding soil for cable","m",{"v":13.212150187500002,"d":"R 13.21"},{"v":13.212150187500002,"d":"R 13.21"}]
[3.3,null,"Blanket soil for cable","m3",{"v":13.212150187500002,"d":"R 13.21"},{"v":13.212150187500002,"d":"R 13.21"}]
[3.4,null,"G5 filling for cable","m3",{"v":17.616200250000002,"d":"R 17.62"},{"v":17.616200250000002,"d":"R 17.62"}]
[4,null,"Compacting Bedding Soil"]
[4.1,"D-DT-0854","Sifted Soil - 0.15m High and 0.45m Wide","m2",{"v":120.34559221439999,"d":"R 120.35"},{"v":120.34559221439999,"d":"R 120.35"}]
[4.2,"D-DT-0854","Imported Soil - 0.15m High and 0.45m Wide","m2",{"v":348.05833042399996,"d":"R 348.06"},{"v":348.05833042399996,"d":"R 348.06"}]
[5,null,"Laying of Cable"]
[5.1,"D-DT-0854","Laying of 3-Core 50mm sq. MV Cable","m",{"v":17.697881208,"d":"R 17.70"},{"v":17.697881208,"d":"R 17.70"}]
[5.2,"D-DT-0854","Laying of 3-Core 95mm sq. MV Cable","m",{"v":40,"d":"R 40.00"},{"v":40,"d":"R 40.00"}]
[5.3,"D-DT-0854","Laying of 3-Core 185mm sq. MV Cable","m",{"v":65,"d":"R 65.00"},{"v":65,"d":"R 65.00"}]
[5.4,"D-DT-0854","Laying of 3-Core 300mm sq. MV Cable","m",{"v":120,"d":"R 120.00"},{"v":120,"d":"R 120.00"}]
[5.5,"D-DT-0854","Laying of 4-Core 16mm sq. LV Cable","m",{"v":17.697881208,"d":"R 17.70"},{"v":17.697881208,"d":"R 17.70"}]
[5.6,"D-DT-0854","Laying of 4-Core 25mm sq. LV Cable","m",{"v":17.697881208,"d":"R 17.70"},{"v":17.697881208,"d":"R 17.70"}]
[5.7,"D-DT-0854","Laying of 4-Core 35mm sq. LV Cable","m",{"v":17.697881208,"d":"R 17.70"},{"v":17.697881208,"d":"R 17.70"}]
[5.8,"D-DT-0854","Laying of 4-Core 50mm sq. LV Cable","m",{"v":17.697881208,"d":"R 17.70"},{"v":17.697881208,"d":"R 17.70"}]
[5.9,"D-DT-0854","Laying of 4-Core 70mm sq. LV Cable","m",{"v":35,"d":"R 35.00"},{"v":35,"d":"R 35.00"}]
[{"v":5.1,"d":"5.10"},"D-DT-0854","Laying of 4-Core 120mm sq. LV Cable","m",{"v":58,"d":"R 58.00"},{"v":58,"d":"R 58.00"}]
[5.11,"D-DT-0854","Laying of 4-Core 185mm sq. LV Cable","m",{"v":65,"d":"R 65.00"},{"v":65,"d":"R 65.00"}]
[5.12,"D-DT-0854","Laying of 4-Core 240mm sq. LV Cable","m",{"v":120,"d":"R 120.00"},{"v":120,"d":"R 120.00"}]
[6,null,"Compacting Blanket Soil"]
[6.1,"D-DT-0854","Sifted Soil -  0.25m High and 0.45m Wide","m2",{"v":120.34559221439999,"d":"R 120.35"},{"v":120.34559221439999,"d":"R 120.35"}]
[6.2,"D-DT-0854","Imported Soil - 0.25m High and 0.45m Wide","m2",{"v":348.05833042399996,"d":"R 348.06"},{"v":348.05833042399996,"d":"R 348.06"}]
[7,null,"Backfilling of the Cable Trench"]
[7.1,"D-DT-0854","General Trench - 0.6m High and 0.45m Wide","m3",{"v":120.34559221439999,"d":"R 120.35"},{"v":120.34559221439999,"d":"R 120.35"}]
[7.2,"D-DT-0854","Rail/Road Crossing Trench - 1.2m High and 0.45m Wide","m3",{"v":120.34559221439999,"d":"R 120.35"},{"v":120.34559221439999,"d":"R 120.35"}]
[7.3,"D-DT-0854","Along The Road Trench - 0.9m High and 0.45m Wide","m3",{"v":120.34559221439999,"d":"R 120.35"},{"v":120.34559221439999,"d":"R 120.35"}]
[7.4,"D-DT-0854","Laying of Warning Tape","m",{"v":2.75,"d":"R 2.75"},{"v":2.75,"d":"R 2.75"}]
[7.5,"D-DT-8012","Installation of Cable Route Markers","Each",{"v":141.583049664,"d":"R 141.58"},{"v":141.583049664,"d":"R 141.58"}]
[7.6,null,"Re-instatement of Gardens","m2",{"v":75,"d":"R 75.00"},{"v":225.4899686055,"d":"R 225.49"},"Price high see propose rate"]
[7.7,null,"Re-instatement of Pavements","m2",{"v":185,"d":"R 185.00"},{"v":271.4307185746,"d":"R 271.43"},"Price high see propose rate"]
[7.8,null,"Re-instatement of Driveways ","m2",{"v":200,"d":"R 200.00"},{"v":1728.4930646480002,"d":"R 1,728.49"},"Price high see propose rate"]
[7.9,null,"Re-instatement of Tarred surfaces","m2",{"v":180,"d":"R 180.00"},{"v":772.8074794160001,"d":"R 772.81"},"Price high see propose rate"]
["SUB-TOTAL O"]
["P",null,"MV/LV CABLE TERMINATION"]
["Termination of cable shall be done in accordance with Eskom standard of terminating cables for the termination onto air-filled cable, termination onto overhead line cable in their deferent classifications. Termination material are free issue, unless otherwise ordered and/or specified by the Project Manger to supply all accessories on an as and when required basis as cost plus fee."]
[1,null,"LV Cable Termination onto Air-Filled Cable Termination Enclosure"]
[1.1,null,"Install 2-Core 16mm sq. LV Bare Termination","Each",{"v":1250.650272032,"d":"R 1,250.65"},{"v":1250.650272032,"d":"R 1,250.65"},"Rate too high for LV cable,can't be the same as  MV cable due to less skills required for LV"]
[1.2000000000000002,null,"Install 4-Core 16mm sq. LV Bare Termination","Each",{"v":1250.650272032,"d":"R 1,250.65"},{"v":1250.650272032,"d":"R 1,250.65"},"Rate too high for LV cable,can't be the same as  MV cable due to less skills required for LV"]
[1.3,null,"Install 4-Core 25mm sq. LV Bare Termination","Each",{"v":1250.650272032,"d":"R 1,250.65"},{"v":1250.650272032,"d":"R 1,250.65"},"Rate too high for LV cable,can't be the same as  MV cable due to less skills required for LV"]
[1.4000000000000001,null,"Install 4-Core 35mm sq. LV Bare Termination","Each",{"v":1250.650272032,"d":"R 1,250.65"},{"v":1250.650272032,"d":"R 1,250.65"},"Rate too high for LV cable,can't be the same as  MV cable due to less skills required for LV"]
[1.5,null,"Install 4-Core 50mm sq. LV Bare Termination","Each",{"v":1250.650272032,"d":"R 1,250.65"},{"v":1250.650272032,"d":"R 1,250.65"},"Rate too high for LV cable,can't be the same as  MV cable due to less skills required for LV"]
[1.6,null,"Install 4-Core 70mm sq. LV Bare Termination","Each",{"v":1250.650272032,"d":"R 1,250.65"},{"v":1250.650272032,"d":"R 1,250.65"},"Rate too high for LV cable,can't be the same as  MV cable due to less skills required for LV"]
[1.7000000000000002,null,"Install 4-Core 120mm sq. LV Bare Termination","Each",{"v":1250.650272032,"d":"R 1,250.65"},{"v":1250.650272032,"d":"R 1,250.65"},"Rate too high for LV cable,can't be the same as  MV cable due to less skills required for LV"]
[1.8000000000000003,null,"Install 4-Core 185mm sq. LV Bare Termination","Each",{"v":1250.650272032,"d":"R 1,250.65"},{"v":1250.650272032,"d":"R 1,250.65"},"Rate too high for LV cable,can't be the same as  MV cable due to less skills required for LV"]
[1.9000000000000001,null,"Install 4-Core 240mm sq. LV Bare Termination","Each",{"v":1250.650272032,"d":"R 1,250.65"},{"v":1250.650272032,"d":"R 1,250.65"},"Rate too high for LV cable,can't be the same as  MV cable due to less skills required for LV"]
[{"v":1.1,"d":"1.10"},null,"Install 3-Core 50mm sq. Shrouded Termination","Each",{"v":1250.650272032,"d":"R 1,250.65"},{"v":1250.650272032,"d":"R 1,250.65"},"Rate too high for LV cable,can't be the same as  MV cable due to less skills required for LV"]
[2,null,"MV Cable Termination onto Air-Filled Cable Termination Enclosure"]
[2.1,"D-DT-8011","Install 3-Core 50mm sq. Shrouded Termination","Each",{"v":1250.650272032,"d":"R 1,250.65"},{"v":1250.650272032,"d":"R 1,250.65"},"Review rates"]
[2.2,"D-DT-8006","Install 3-Core 50mm sq. Unscreened Separable Connector Termination","Each",{"v":1592.80930872,"d":"R 1,592.81"},{"v":1592.80930872,"d":"R 1,592.81"},"Review rates"]
[2.3000000000000003,"D-DT-8006","Install 3-Core 50mm sq. Unscreened Separable Connector Extended Screen Termination","Each",{"v":1592.80930872,"d":"R 1,592.81"},{"v":1592.80930872,"d":"R 1,592.81"},"Review rates"]
[2.4000000000000004,"D-DT-8006","Install 3-Core 50mm sq. Screened Separable Connector Termination","Each",{"v":1592.80930872,"d":"R 1,592.81"},{"v":1592.80930872,"d":"R 1,592.81"},"Review rates"]
[2.5,"D-DT-8011","Install 3-Core 95mm sq. Shrouded Termination","Each",{"v":1250.650272032,"d":"R 1,250.65"},{"v":1250.650272032,"d":"R 1,250.65"},"Review rates"]
[2.6,"D-DT-8006","Install 3-Core 95mm sq. Unscreened Separable Connector Termination","Each",{"v":1592.80930872,"d":"R 1,592.81"},{"v":1592.80930872,"d":"R 1,592.81"},"Review rates"]
[2.7,"D-DT-8006","Install 3-Core 95mm sq. Unscreened Separable Connector Extended Screen Termination","Each",{"v":1592.80930872,"d":"R 1,592.81"},{"v":1592.80930872,"d":"R 1,592.81"},"Review rates"]
[2.8000000000000003,"D-DT-8006","Install 3-Core 95mm sq. Screened Separable Connector Termination","Each",{"v":1592.80930872,"d":"R 1,592.81"},{"v":1592.80930872,"d":"R 1,592.81"},"Review rates"]
[2.9000000000000004,"D-DT-8011","Install 3-Core 185mm sq. Shrouded Termination","Each",{"v":1250.650272032,"d":"R 1,250.65"},{"v":1250.650272032,"d":"R 1,250.65"},"Review rates"]
[{"v":2.1,"d":"2.10"},"D-DT-8006","Install 3-Core 185mm sq. Unscreened Separable Connector Termination","Each",{"v":1592.80930872,"d":"R 1,592.81"},{"v":1592.80930872,"d":"R 1,592.81"},"Review rates"]
[2.11,"D-DT-8006","Install 3-Core 185mm sq. Unscreened Separable Connector Extended Screen Termination","Each",{"v":1592.80930872,"d":"R 1,592.81"},{"v":1592.80930872,"d":"R 1,592.81"},"Review rates"]
[2.12,"D-DT-8006","Install 3-Core 185mm sq. Screened Separable Connector Termination","Each",{"v":1740.29165212,"d":"R 1,740.29"},{"v":1740.29165212,"d":"R 1,740.29"},"Review rates"]
[2.13,"D-DT-8011","Install 3-Core 300mm sq. Shrouded Termination","Each",{"v":1250.650272032,"d":"R 1,250.65"},{"v":1250.650272032,"d":"R 1,250.65"},"Review rates"]
[2.14,"D-DT-8006","Install 3-Core 300mm sq. Unscreened Separable Connector Termination","Each",{"v":1592.80930872,"d":"R 1,592.81"},{"v":1592.80930872,"d":"R 1,592.81"},"Review rates"]
[2.15,"D-DT-8006","Install 3-Core 300mm sq. Unscreened Separable Connector Extended Screen Termination","Each",{"v":1592.80930872,"d":"R 1,592.81"},{"v":1592.80930872,"d":"R 1,592.81"},"Review rates"]
[2.16,"D-DT-8006","Install 3-Core 300mm sq. Screened Separable Connector Termination","Each",{"v":1740.29165212,"d":"R 1,740.29"},{"v":1740.29165212,"d":"R 1,740.29"},"Review rates"]
[3,null,"MV Cable Termination onto Overhead Line from Substation "]
[3.1,"D-DT-0850","Install 50mm sq. O/D Termination","Each",{"v":892.9213136622,"d":"R 892.92"},{"v":892.9213136622,"d":"R 892.92"}]
[3.2,"D-DT-0851","Install 50mm sq. O/D Termination","Each",{"v":892.9213136622,"d":"R 892.92"},{"v":892.9213136622,"d":"R 892.92"}]
[3.3,"D-DT-0850","Install 95mm sq. O/D Termination","Each",{"v":892.9213136622,"d":"R 892.92"},{"v":892.9213136622,"d":"R 892.92"}]
[3.4,"D-DT-0851","Install 95mm sq. O/D Termination","Each",{"v":892.9213136622,"d":"R 892.92"},{"v":892.9213136622,"d":"R 892.92"}]
[3.5,"D-DT-0850","Install 185mm sq. O/D Termination","Each",{"v":892.9213136622,"d":"R 892.92"},{"v":892.9213136622,"d":"R 892.92"}]
[3.6,"D-DT-0851","Install 185mm sq. O/D Termination","Each",{"v":892.9213136622,"d":"R 892.92"},{"v":892.9213136622,"d":"R 892.92"}]
[3.7,"D-DT-0850","Install 300mm sq. O/D Termination","Each",{"v":892.9213136622,"d":"R 892.92"},{"v":892.9213136622,"d":"R 892.92"}]
[3.8,"D-DT-0851","Install 300mm sq. O/D Termination","Each",{"v":892.9213136622,"d":"R 892.92"},{"v":892.9213136622,"d":"R 892.92"}]
[3.9,"D-DT-1850","Install Equipment Links - 3-Phase ","Each",{"v":892.9213136622,"d":"R 892.92"},{"v":892.9213136622,"d":"R 892.92"}]
[{"v":3.1,"d":"3.10"},"D-DT-0261","Install Surge Arresters - 3-Phase","Each",{"v":344.7083743382001,"d":"R 344.71"},{"v":344.7083743382001,"d":"R 344.71"}]
[3.11,"D-DT-8023","Install a Steel Pipe","Each",{"v":294.9646868,"d":"R 294.96"},{"v":294.9646868,"d":"R 294.96"}]
["SUB-TOTAL P"]
["Q",null,"CABLE JOINT"]
["Cable joint bay shall be executed in accordance with Eskom standard of jointing cables in their different classifications. Joint bay materials including kits are free issue, unless otherwise ordered and/or specified by the Project Manger to supply all accessories on an as and when required basis and paid as cost plus fee. Excavations, compaction and backfilling of cable joints bay shall be measured here including supply of imported soil in bedding and blankets or sifted soil where specified. "]
[1.1,"D-DT-0854","Excavate a Joint Bay","m3",{"v":147.4823434,"d":"R 147.48"},{"v":147.4823434,"d":"R 147.48"}]
[1.2,"D-DT-0854","Compact Bedding Soil","m2",{"v":120.35,"d":"R 120.35"},{"v":120.35,"d":"R 120.35"}]
[1.3,"D-DT-0854","Sifted Soil - 0.15m High and 0.45m Wide","m3",{"v":120.34559221439999,"d":"R 120.35"},{"v":120.34559221439999,"d":"R 120.35"}]
[1.4,null,"Dispose of Excavated Material at approved disposal site","m3",{"v":245,"d":"R 245.00"},{"v":245,"d":"R 245.00"}]
[1.5,"D-DT-0854","Imported Soil -0.15m High and 0.45m Wide","m3",{"v":348.05833042399996,"d":"R 348.06"},{"v":348.05833042399996,"d":"R 348.06"}]
[1.6,"D-DT-8008","Make-Off a Cable Joint - 3-Core 16mm sq. MV Cable","Each",{"v":92.2,"d":"R 92.20"},{"v":92.2,"d":"R 92.20"},"Is make off same as install? If installation is included then the rate is low"]
[1.6,"D-DT-8008","Make-Off a Cable Joint - 3-Core 50mm sq. MV Cable","Each",{"v":92.2,"d":"R 92.20"},{"v":92.2,"d":"R 92.20"},"Is make off same as install? If installation is included then the rate is low"]
[1.6,"D-DT-8008","Make-Off a Cable Joint - 3-Core 95mm sq. MV Cable","Each",{"v":92.2,"d":"R 92.20"},{"v":92.2,"d":"R 92.20"},"Is make off same as install? If installation is included then the rate is low"]
[1.7,"D-DT-8008","Make-Off a Cable Joint - 3-Core 185mm sq. MV Cable","Each",{"v":92.2,"d":"R 92.20"},{"v":92.2,"d":"R 92.20"},"Is make off same as install? If installation is included then the rate is low"]
[1.8,"D-DT-8008","Make-Off a Cable Joint - 3-Core 300mm sq. MV Cable","Each",{"v":92.2,"d":"R 92.20"},{"v":92.2,"d":"R 92.20"},"Is make off same as install? If installation is included then the rate is low"]
[1.9,"D-DT-8014","Make-Off a Cable Joint - 4-Core 16mm sq. LV Cable","Each",{"v":92.2,"d":"R 92.20"},{"v":92.2,"d":"R 92.20"}]
[{"v":1.1,"d":"1.10"},"D-DT-8014","Make-Off a Cable Joint - 4-Core 25mm sq. LV Cable","Each",{"v":92.2,"d":"R 92.20"},{"v":92.2,"d":"R 92.20"}]
[{"v":1.1,"d":"1.10"},"D-DT-8014","Make-Off a Cable Joint - 4-Core 35mm sq. LV Cable","Each",{"v":92.2,"d":"R 92.20"},{"v":92.2,"d":"R 92.20"}]
[{"v":1.1,"d":"1.10"},"D-DT-8014","Make-Off a Cable Joint - 4-Core 50mm sq. LV Cable","Each",{"v":92.2,"d":"R 92.20"},{"v":92.2,"d":"R 92.20"}]
[1.11,"D-DT-8014","Make-Off a Cable Joint - 4-Core 70mm sq. LV Cable","Each",{"v":92.2,"d":"R 92.20"},{"v":92.2,"d":"R 92.20"}]
[1.12,"D-DT-8014","Make-Off a Cable Joint - 4-Core 120mm sq. LV Cable","Each",{"v":92.2,"d":"R 92.20"},{"v":92.2,"d":"R 92.20"}]
[1.13,"D-DT-8014","Make-Off a Cable Joint - 4-Core 185mm sq. LV Cable","Each",{"v":92.2,"d":"R 92.20"},{"v":92.2,"d":"R 92.20"}]
[1.13,"D-DT-8014","Make-Off a Cable Joint - 4-Core 240mm sq. LV Cable","Each",{"v":92.2,"d":"R 92.20"},{"v":92.2,"d":"R 92.20"}]
[1.18,"D-DT-0854","Backfill a Joint Bay","m3",{"v":120.34559221439999,"d":"R 120.35"},{"v":120.34559221439999,"d":"R 120.35"}]
[1.19,"D-DT-8012","Install a Route Marker","Each",{"v":141.583049664,"d":"R 141.58"},{"v":141.583049664,"d":"R 141.58"}]
["SUB-TOTAL Q"]
["R",null,"EQUIPMENT DISMANTLING"]
["Includes Cut Up, Coiling  And Loading But Excludes Transport To The Nearest Eskom Stores"]
[1.1,null,"Dismantle LV Conductor ","m",{"v":4.7194349888,"d":"R 4.72"},{"v":4.7194349888,"d":"R 4.72"}]
[1.2,null,"Dismantle MV Conductor","m",{"v":4.7194349888,"d":"R 4.72"},{"v":4.7194349888,"d":"R 4.72"}]
[1.3,null,"Dismantle Service Cable","m",{"v":3.15,"d":"R 3.15"},{"v":3.15,"d":"R 3.15"}]
[1.4,null,"Dismantle MV Overhead Transformers","Each",{"v":412.95056151999995,"d":"R 412.95"},{"v":412.95056151999995,"d":"R 412.95"}]
[1.5,null,"Dismantle MV Overhead Sectionaliser","Each",{"v":412.95056151999995,"d":"R 412.95"},{"v":412.95056151999995,"d":"R 412.95"}]
[1.6,null,"Dismantle MV Overhead Reclosers","Each",{"v":412.95056151999995,"d":"R 412.95"},{"v":412.95056151999995,"d":"R 412.95"}]
[1.7,null,"Dismantle MV Pole Mounted CT-VT Unit","Each",{"v":412.95056151999995,"d":"R 412.95"},{"v":412.95056151999995,"d":"R 412.95"}]
[1.8,null,"Dismantle MV Pole Mounted Shunt Capacitor Banks","Each",{"v":412.95056151999995,"d":"R 412.95"},{"v":412.95056151999995,"d":"R 412.95"}]
[1.9,null,"Dismantle MV Line Arrestor","Each",{"v":397.67,"d":"R 397.67"},{"v":397.67,"d":"R 397.67"}]
[{"v":1.1,"d":"1.10"},null,"Dismantle MV Overhead Section / Equipment Links","Each",{"v":397.67,"d":"R 397.67"},{"v":397.67,"d":"R 397.67"}]
[1.11,null,"Remove LV Pole Top Boxes","Each",{"v":355.64,"d":"R 355.64"},{"v":355.64,"d":"R 355.64"}]
[1.12,null,"Dismantle Stays","Each",{"v":261.1174889897,"d":"R 261.12"},{"v":261.1174889897,"d":"R 261.12"},"Cut off of stay or removal and backfil? Add detailed scope"]
[1.13,null,"Dismantle Poles","Each",{"v":240.3330130234,"d":"R 240.33"},{"v":240.3330130234,"d":"R 240.33"},"Cut off of stay or removal and backfil? Add detailed scope"]
[1.14,null,"Remove MV Cable, includes excavation and backfill","m",{"v":177,"d":"R 177.00"},{"v":177,"d":"R 177.00"}]
[1.15,null,"Remove LV Cable, includes excavation and backfill","m",{"v":177,"d":"R 177.00"},{"v":177,"d":"R 177.00"}]
[1.16,null,"Remove MV Cable I/D Terminations","Each",{"v":365.76,"d":"R 365.76"},{"v":365.76,"d":"R 365.76"}]
[1.17,null,"Remove MV Cable O/D Terminations","Each",{"v":365.76,"d":"R 365.76"},{"v":365.76,"d":"R 365.76"}]
[1.18,null,"Remove RMU ","Each",{"v":2949.646868,"d":"R 2,949.65"},{"v":2949.646868,"d":"R 2,949.65"}]
[1.19,null,"Remove Minisub","Each",{"v":2949.646868,"d":"R 2,949.65"},{"v":2949.646868,"d":"R 2,949.65"}]
[{"v":1.2,"d":"1.20"},null,"Remove Ground Mounted CT-VT Unit","Each",{"v":1749.6468679999998,"d":"R 1,749.65"},{"v":1749.6468679999998,"d":"R 1,749.65"}]
[1.21,null,"Remove LV Kiosks","Each",{"v":123.094557750845,"d":"R 123.09"},{"v":123.094557750845,"d":"R 123.09"}]
[1.22,null,"Remove Plinths ","Each",{"v":1849.6468679999998,"d":"R 1,849.65"},{"v":1849.6468679999998,"d":"R 1,849.65"}]
[1.23,null,"Transport Of Dismantled/Decommissioned To Eskom Stores","KM",{"v":22.05888125,"d":"R 22.06"},{"v":22.05888125,"d":"R 22.06"}]
[1.28,null,"Removal of a post / pin insulator","Each",{"v":24.4629,"d":"R 24.46"},{"v":24.4629,"d":"R 24.46"}]
[{"v":1.2999999999999998,"d":"1.30"},null,"Removal of SPU unit with rails","Each",{"v":24.4629,"d":"R 24.46"},{"v":24.4629,"d":"R 24.46"}]
[1.31,null,"Removal of LPU unit ( indoor and outdoor)","No",{"v":24.4629,"d":"R 24.46"},{"v":24.4629,"d":"R 24.46"}]
[{"v":1.3299999999999998,"d":"1.33"},null,"Moving of pre-Paid Meter (Meter Shifting)","Each",{"v":73.3887,"d":"R 73.39"},{"v":73.3887,"d":"R 73.39"}]
[1.39,null,"Removal of ED / ECU","Each",{"v":74.856474,"d":"R 74.86"},{"v":74.856474,"d":"R 74.86"}]
[1.41,null,"AP4 Meter Box + Pipe","Each",{"v":112.284711,"d":"R 112.28"},{"v":112.284711,"d":"R 112.28"}]
[1.42,null,"Removal - complete of one Regulator can/voltage regulator","Each",{"v":131.365773,"d":"R 131.37"},{"v":131.365773,"d":"R 131.37"}]
[2,null,"BIL & BONDING"]
[2.1,null,"Re-instate broken/damage bonding & BIL on existing structure ","No",{"v":48.9258,"d":"R 48.93"},{"v":48.9258,"d":"R 48.93"}]
["SUB-TOTAL R"]
["S",null,"LABELLING"]
["Allow for the following end items to be applied as per relevant Eskom \nInstructions/Bulletins/Procedures and Standards where not already allowed for in Structure Package"]
[1.1,null,"MV Pole Number","Each",{"v":17.697881208,"d":"R 17.70"},{"v":17.697881208,"d":"R 17.70"}]
[1.2,null,"LV Pole Number","Each",{"v":17.697881208,"d":"R 17.70"},{"v":17.697881208,"d":"R 17.70"}]
[1.3,null,"Meter Number","Each",{"v":17.697881208,"d":"R 17.70"},{"v":17.697881208,"d":"R 17.70"}]
[1.4,null,"House  Number\n• 100 x 240mm x 0,6mm Yellow Chromadec plate with two pre-drilled 6mm holes (rust-free metal).\n• Fixed with two 6mm x 75mm nylon anchor or 6mm Zink bolt and 2x nuts.\n• All corners rounded. Clear powder coat finish.\n• Cast vinyl with 75mm Helvetica Compact script.\n","Each",{"v":17.7,"d":"R 17.70"},{"v":17.7,"d":"R 17.70"},"New activity"]
["SUB-TOTAL S"]
["T",null,"EQUIPMENT TESTING"]
["Allowance shall be made for the complete testing and commissioning of Medium Voltage equipment.  Tests to include earth electrode resistance measurement.  Transformer to  include a LV earth electrode resistance measurement. Soil Resistivity Tests for Equipment to be performed as appropriate and to be verified by Eskom's Clerk of Works, and must be according to Eskom Standard"]
[1.1,null,"Perform Phasing Test (not required if COC option is selected)","Each",{"v":95.42,"d":"R 95.42"},{"v":95.42,"d":"R 95.42"},"Comments in red to be included in description"]
[1.2,null,"Continuity Tests (not required if COC option is selected)","Each",{"v":95.42,"d":"R 95.42"},{"v":95.42,"d":"R 95.42"},"Comments in red to be included in description"]
[1.3,null,"Earth Resistance Test (MV or LV Earth electrode test)","Each",{"v":95.42,"d":"R 95.42"},{"v":95.42,"d":"R 95.42"},"Comments in red to be included in description"]
[1.4,null,"A.C. Over-Voltage Test","Each",{"v":95.42,"d":"R 95.42"},{"v":95.42,"d":"R 95.42"}]
[1.5,null,"D.C. Insulation Test","Each",{"v":95.42,"d":"R 95.42"},{"v":95.42,"d":"R 95.42"}]
[1.6,null,"Outer Sheath Test (Serving Test)","Each",{"v":95.42,"d":"R 95.42"},{"v":95.42,"d":"R 95.42"}]
[1.7,null,"Compaction Test","Each",{"v":95.42,"d":"R 95.42"},{"v":95.42,"d":"R 95.42"}]
[1.8,null,"C.O.C Test for Certificate (20A and 60A prepaid connections) ","No",{"v":250,"d":"R 250.00"},{"v":250,"d":"R 250.00"},"Comments in red to be included in description"]
[1.9,null,"Voltage Regulator commissioning test","No",{"v":95.42,"d":"R 95.42"},{"v":95.42,"d":"R 95.42"}]
[{"v":1.1,"d":"1.10"},null,"Recloser commissioning test","No",{"v":95.42,"d":"R 95.42"},{"v":95.42,"d":"R 95.42"}]
["SUB-TOTAL T"]
["U",null,"AS - BUILTS"]
["Allow for the following end items to be applied as per relevant Eskom \nInstructions/Bulletins/Procedures and Standards where not already allowed for in Structure Package"]
[1,null,"As-built Drawings","Each",{"v":3500,"d":"R 3,500.00"},{"v":3500,"d":"R 3,500.00"},"What is included in this activity? Remove as as-built is updated by drawing office and hand over documents and marked and signed. As- builts are included in the project"]
["SUB-TOTAL U"]
["V",null,"MISCELLANEOUS"]
["Allow for the following end items to be applied as per relevant Eskom instructions/bulletins/procedures and standards where not already allowed for in structure package. Note the cross arms below are applicable for existing structures only."]
[1.1,3175,"Damper,vibrat spiral 8.29-11.71 D3175","Each",{"v":24.4629,"d":"R 24.46"},{"v":24.4629,"d":"R 24.46"}]
[1.2,3175,"Damper,vibrat spiral 11.72-14.30 D3175","Each",{"v":24.4629,"d":"R 24.46"},{"v":24.4629,"d":"R 24.46"}]
[1.3,7028,"Set: Device warning-Aircraft warning 8.87-13.55;2","SET",{"v":54.307638,"d":"R 54.31"},{"v":54.307638,"d":"R 54.31"}]
[1.4,7028,"Set: Device warning -Aircraft warning 7.35-14.16;2","SET",{"v":54.307638,"d":"R 54.31"},{"v":54.307638,"d":"R 54.31"}]
[1.5,7028,"Set: Device warning-Aircraft warning 18.13-23.88;2","SET",{"v":54.307638,"d":"R 54.31"},{"v":54.307638,"d":"R 54.31"}]
[1.6,"3029/3053","BIRD FLIGHT DIVERTERS","Each","R34 84",null,"New activity"]
[1.7,3303,"Raptor protector","Each",{"v":34.84,"d":"R 34.84"},null,"New activity"]
["SUB-TOTAL V"]
["VERIFIED BY: CLERK OF WORKS",null,null,"DATE:"]
["COST CHECK BY: QUANTITY SURVEYOR",null,null,"DATE:"]
["ACCEPTED BY: CONTRACTOR",null,null,"DATE:"]
["VERIFIED BY: QUANTITY SURVEYOR (FRANCOIS RETIEF)",null,null,"DATE:"]