{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":962,"n_cols":7,"rows_kept":962,"merged":[[1,0,1,6],[92,0,92,6],[123,0,123,6]]}
["Material nr","Description","Long Description","Rounded 5 year qty",null,"Rate per unit","Total"]
["BATCH 1   -   GENRAL CONSUMABLES"]
["0011460","TIE CBL:SELF LOCKING;50 MM;WD 4.7 MM;15","C.O.C; 0040/88Q; Q4:NSF:NC:0; CABLE TIE STRAP (BLACK); DIMEN: 200MM LG X 4.7MM WIDE; MATL: NYLON; PRICING = PER CABLE TIE; SUGGESTED PACKAGINF 1 EA = PACK OF 100 TIES; KBA:1217L00009; KBA:1215G08001, ITM:X; FUNCT.LOC:1/2LGX 000JA, 9LGX 000JA, FUNCT.LOC:1/2LGX 000JA  9LGX 000JA ***** END DETAIL DESCRIPTION ***** A.V.2002/08/08; CLC 2013/11/27; CLC 2014/03/05",230000,"EA"]
["0011461","TIE CBL:SELF LOCKING;18 MM;WD 2.5 MM;15","COC\\0040/88Q\\:Q4:NSF:NC:0 CABLE TIE STRAP P/NO: T18R DIMEN: 2,5MM WIDE X 104MM LG MATL: BLACK PLASTIC; PRICING = PER CABLE TIE; SUGGESTED PACKAGINF 1 EA = PACK OF 100 TIES; KBA:1217L00009 ITM:X   1 = SEQ:1048 KBA:1215G08001 ITM:X   2 = SEQ:1049 S/LIST:  M/MAN: / ASMT: 1 = SEQ:1048 S/LIST:  M/MAN: / ASMT: 2 = SEQ:1049 FUNCT.LOC:1/2LGX 000JA  9LGX 000JA 1 = SEQ:1048 FUNCT.LOC:1/2LGX 000JA  9LGX 000JA 2 = SEQ:1049 BOM SEQ NO:1048 = B-SER:0193921 BOM SEQ NO:1049 = B-SER:0193925***** END DETAIL DESCRIPTION ***** A.V.2002/08/08 JNF 2009/07/31 ",60000,"EA"]
["0011523","TIE CBL:SELF LOCKING;120 MM;WD 7.6 MM","C.O.C\\0040/88Q\\Q4:NSF:NC:0 ELECTRICAL CABLE TIE STRAP P/NO: T120R DIMEN: 7,6W X 385LG MM MATL: BLACK PLASTIC; PRICING = PER CABLE TIE; SUGGESTED PACKAGINF 1 EA = PACK OF 50 TIES;  ***** END DETAIL DESCRIPTION ***** JNF 2009/09/30",{"v":180000,"d":"180,000"},"EA"]
["0014413","BATT DCELL:ZN CARBON;1.5 VDC;D","COC; 0012/88Q; Q4:NSF:NC:0; SPEC DESCRIPTION CONFIRMED DRY TORCH BATTERY ZINK CARBON MNF: EVEREADY SIZE: D LARGE RATED VOLTAGE: 1.5 VOLT; SAFETY DATA SHEET TO BE SUPPLIED WITH DELIVERY; END DETAIL DESCRIPTION: YA 2023/07/13",8500,"EA"]
["0016493","TAPE ADHSV:MASKING;WD 18 MM X LG 40 M","C.O.C; 0040/88Q; Q5:NSF:NC:NEV BUFF COLOUR MASKING TAPE MATL:18MM X 40M X 75MM BORE MOISTURE OIL AND SOLVENT RESISTANT ***** END DETAIL DESCRIPTION ***** JNF 2001/12/14",700,"EA"]
["0016511","PAPER BOND:A3;WHITE;SHEET;80 G/M2;REAM","N/A\\0040/88Q\\NQL:NSF:NC:NEV DESCRIPTION CONFIRMED-SEG/COD-92/11 BOND PAPER * MNF: TYPEK; DIMEN: 420MM LG X 297MM WIDE * A3 MATL: PAPER 80GSM WHITE 500/REAM ***** END DETAIL DESCRIPTION ***** GAR 12/11/92; ML 2019/07/30",{"v":1500,"d":"1,500"},"EA"]
["0109008","HANDLE,BROOM PLATFORM","N/A\\0040/88Q\\NQL:NSF:NC:NEV DESCRIPTION CONFIRMED-SEG/COD-92/10 BROOM HANDLE FOR PLATFORM TYPE BROOM P/NO: DIMEN: MATL: KBA:  ITM: KBY: / S/LIST:  M/MAN: ASMT: TRI: ***** END DETAIL DESCRIPTION ***** GAR 27/10/92",200,"EA"]
["0144647","BATT DCELL:ALKALINE;1.5 VDC;C","C.O.C; 0012/88Q:Q4:NSF:NC:0; DRYCELL BATTERY (GOLD); MATL:ALKALINE MANGANESE; TYPE: FLAT SURFACE TERMINALS; SIZE:MEDIUM; RANGE:1,5 VOLT; SUGGESTED VENDOR: ELECTRIC CENTRE; ***** END DETAIL DESCRIPTION *****; JNF 2016/02/23",{"v":1000,"d":"1,000"},"EA"]
["0146122","TORCH:2 CELL;2D","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; 2 CELL TORCH (NOT INDUSTRIAL TYPE) WITH MAGNETIC ATTACHMENT; FUNCT LOC: 6MBI 008BG ***** END DETAIL DESCRIPTION ***** JNF 99/06/24; CLC 2016/08/30",600,"EA"]
["0159580","ENVELOPE MLNG:C5; WD 162 X LG 229 MM","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV ENVELOPE (C5) DESIGN ELEMENTS FRONT:THE PRINTED ENVELOPE FEATURES THE CORPORATE SIGNATURE POSITIONED IN THE TOP LEFT- HAND CORNER,AS INDICATED. BACK:THE ONLY INFORMATION THAT MAY APPEAR ON THE BACK OF THE ENVELOPE IS THE RETURN ADDRESS AND REGISTRATION DETAILS OF ESKOM,UNLESS OTHERWISE SPECIFIED. NOTE:DO NOT USE ANY PUNCTUATION IN THE PRE-PRINTED INFORMATION;INSERT A DOUBLE SPACE INSTEAD. INSIDE:THE ESKOM BASKET-WEAVE PATTERN IS USED IN A 20% TINT ON THE INSIDE OF THE ENVELOPE,AS ILLUSTRATED ON THE PAGE.THIS SERVES AS A SECURITY PATTERN. NOTE:THERE ARE NO DIVISIONAL ENVELOPES,EXCEPT FOR ESKOM ENTERPRISES. DIMEN:229 X 162MM PAPER SPECIFICATIONS OPAQUE BOND COLOUR SPECIFICATIONS ESKOM SIGNATURE AND ALL PRINTED TEXT: PANTONE 287 TYPE SPECIFICATIONS POSTAL ADDRESS AND REGISTRATION DETAILS: GILL SANS LIGHT - 8 PT CENTRED LEFT AND RIGHT, LEADING - 8,25 PT LANGUAGE:ENGLISH ***** END DETAIL DESCRIPTION ***** JNF 2004/06/04",500,"EA"]
["0159778","CLEANER:ANTI-FOGGER;BOTTLE 110 ML","N/A\\0040/88Q\\Q5:NSF:NC:NEV (MATERIAL DATA SHEET REQUIRED WITH EVERY DELIVERY) CRACK NON PLANT - CATEGORY 3 KEEP CLEAR ANTI-FOGGER CLEANER (110ML BOTTLE) CODE:D8241079 ***** END DETAIL DESCRIPTION ***** A.V. 2001/09/10 JNF 2005/10/28 JNF 2010/11/16",1000,"EA"]
["0159837","POLISH,FURNITURE:275 ML","C.O.C; 0040/88Q;Q4:NSF:NC:NEV; (MATERIAL DATA SHEET REQUIRED WITH EVERY DELIVERY); POLISH, FURNITURE;  TYPE: PLEDGE; CONTAINER: CAN; CAPACITY: 275 ML; PAKG: SIX IN BOX; FUNC LOC: CONSUMABLE  ***** END DETAIL DESCRIPTION ***** JNF 2009/04/09 JNF 2010/06/25; ML 2021/12/13",{"v":2100,"d":"2,100"},"EA"]
["0159848","POLISH,FLOOR SUPERCOAT               25L","N/A\\0040/88Q\\NQL:NSF:NC:NEV (MATERIAL DATA SHEET REQUIRED WITH EVERY DELIVERY) FLOOR POLISH P/NO: SUPERCOAT DIMEN:25 LITRE CONTAINER FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** GAR 21/04/93 ET 2010/06/28",1800,"EA"]
["0159868","CLEANER:HANDY ANDY;COMPOUND","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; (MATERIAL DATA SHEET REQUIRED WITH EVERY DELIVERY); HANDY ANDY CLEANING COMPOUND W/AMMONIA; SIZE: 500ML BOTTLE; ***** END DETAIL DESCRIPTION *****; JNF 2003/04/22; JNF 2010/06/25; JNF 2012/09/18",5500,"EA"]
["0160335","BAG:REFUSE;WD 750 X LG 950 MM;PLASTIC","N/A\\0040/88Q\\Q5:NSF:NC:NEV REFUSE BAG DIMEN: LTH=950 X W=750 X 40 MICRON THICK MATL: PLASTIC COLOUR:BLACK ***** END DETAIL DESCRIPTION ***** JNF 2004/03/23 BOM SEQ NO:0898",{"v":500000,"d":"500,000"},"EA"]
["0160369","BAG:WD 750 MM X LG 950 MM X THK 50 UM","N/A\\0040/88Q:Q5:NSF:NEV:NC GREY PLASTIC BAGS P/NO: DIMEN:950LX 750WX 50MICRON MATL: PLASTIC FUNCT.LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2004/03/23",{"v":110000,"d":"110,000"},"EA"]
["0160383","BAG,PLASTIC CLEAR  120LX  80W ZIPPERLOCK","N/A\\0040/88Q\\Q5:NSF:NC:NEV PLASTIC BAG W/SELF SEALING \"ZIPPERLOCK\" DIMEN: 120LG X 80W MATL: CLEAR PLASTIC X 50 MICRON THICK FUNCT.LOC: (CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2004/03/23",36500,"EA"]
["0160471","TOWEL,KIMCLOTH X50 BLUE 250MMX400M","N/A\\0040/88Q\\Q5:NSF:NC:NEV KIMCLOTH X50 JUMBO ROLL BLUE 45 GSM RAYON BASED ON DISPENSING ROLL COLOUR: BLUE   P/NO: SA081653 DIMEN: 250MM WIDE,AND 400M IN LENGTH ***** END DETAIL DESCRIPTION ***** JNF 2007/04/11",1400,"EA"]
["0161134","CLEANER,HAND:REINOL FLAX;DEGREASER","N/A\\0040/88Q\\NQL:NSF:NC:NEV DESCRIPTION CONFIRMED-SEG/COD-93/03 REINOL HAND CLEANER WITHOUT SOLVENTS (NATURAL INGREDIENTS) TO CLEAN AND CONDITION SKIN DIMEN:3KG CARTRIDGES ***** END DETAIL DESCRIPTION ***** BOM SEQ NO:0898",150,"EA"]
["0161141","SOAP:HAND,LIQUID,1 L","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; (MATERIAL DATA SHEET REQUIRED WITH EVERY DELIVERY); LIQUID TOILET SOAP; (1 EACH = 1 LITRE); COLOUR : WHITE; P/NO: CALSOAP; FUNCT.LOC: CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2006/09/14; JNF 2009/07/01; JNF 2010/06/25; JNF 2016/02/18; CLC 2016/05/12",{"v":20000,"d":"20,000"},"EA"]
["0161144","DEODORANT,AIRFRESHNER AEROSOL CAN 180ML","N/A\\0040/88Q:NQL:NSF:NEV:NC (MATERIAL DATA SHEET REQUIRED WITH EVERY DELIVERY) DEODORANT AIRFRESHNER P/NO: SIZE: 180 ML AEROSOL CAN ***** END DETAIL DESCRIPTION ***** JNF 2010/06/25",12000,"EA"]
["0161153","TOWEL,PAPER:2 PLY;WD 240 MM;LG 324 MM","N/A\\0040/88Q\\Q5:NSF:NC:NEV KLEENEX BRAND PREMIER HANDTOWELS P/NO: 285917 PACKAGING: 120 TOWELS/PACK 20PACKS/BOX DIMEN: 240MM X 324MM MATL: 2PLY PAPER ***** END DETAIL DESCRIPTION ***** JNF 2006/02/15",2500,"EA"]
["0161155","TOWEL,PAPER:2 PLY JUMBO;WD 270 MM;WHITE","N/A\\0040/88Q\\Q5:NSF:NC:NEV 2 PLY WHITE JUMBO TOWEL DIMEN: 270MM WIDE X 1500M MATL: PAPER FUNCT.LOC: 6MBI 008BG ***** END DETAIL DESCRIPTION ***** JNF 2008/07/17",{"v":8000,"d":"8,000"},"EA"]
["0161759","PLASTIC,CLING-WRAP CLEAR 300MMX1400M","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV PLASTIC CLEAR CLING-WRAPPING 300MM WIDE 1400 METRE LONG FUNCT. LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2009/07/29",30,"EA"]
["0213946","DISINFECTANT:750 ML","N/A; 0040/88Q; Q5:NSF:NC:NEV; LIQUID DISINFECTANT (GENERAL PURPOSES) DETTOL ANTISEPTIC (CONCENTRATED); MFR:N/A; P/N:N/A; PACK: 750ML CONTAINER; ***** END DETAIL DESCRIPTION ***** JNF 2003/10/20; JNF 2004/08/30; JNF 2010/11/01; CLC 2012/10/17; ML 2018/08/29",7500,"EA"]
["0217562","SOAP:BATHING","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; PROTEX SOAP (WHITE); MFR:PROTEX SOAP; TYPE: PROTEX; SIZE: 150 G; FUNCT. LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION ***** JNF 2005/06/24; CLC 2012/10/17; JNF 2015/09/28; ML 2019/06/04; ML 2021/02/24",3000,"EA"]
["0229603","HEAD,BROOM 78X305MM FIBRE","N/A\\0040/88Q\\Q5:NSF:NC:NEV SOFT DOMECTIC BROOM WITHOUT HANDLE (WITH BROOM STAY/GRIP FOR HANDLE) MATL:WOODEN TOP WITH BLACK FIBRE BRISTLES SIZE:78 X 305MM FUNCT.LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2007/11/29 JNF 2010/08/23",200,"EA"]
["0237131","MOP:GRIP;COTTON; WD 140 X LG 450 MM","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV GRIP MOP 500G WITH DETACHABLE METAL HEAD SUPPLIER:F&A DISTRIBUTORS SIZE:140MM WIDTH X 450MM LENGTH MATERIAL: COTTON FFT:SUPPLIED WITH HANDLE FUNCT.LOC: (CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2008/10/13",300,"EA"]
["0243995","PAPER BOND:A4; WD 210 X LG 297 MM;WHITE","C.O.C; 0040/88Q; Q4:NSF:NC:NEV A4 PAPER (500 SHEETS PER REAM) (CONTRACT MATERIAL NUMBER 0159154);  MNF: TYPEK; TYPE: 80GSM;PAPER, BOND: SIZE: A4; WD 210 X LG 297 MM; COLOR: WHITE; USAGE FORM: SHEETS/REAM 500; PACKAGE TYPE: REAM; PACKAGE QUANTITY: 500 PAGES; COLOUR:WHITE; FUNCT.LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2009/09/10; ML 2018/11/06; ML 2019/03/11; ML 2019/07/30",45000,"EA"]
["0248023","PAPER BOND:A4;PINK;PHOTOCOPY;BOX","C.O.C; PAPER, BOND; MNF: MONDI ROTATRIM; SIZE: A4; COLOR: PINK; SPECIFIC USE: PHOTOCOPY; PACKAGE TYPE: BOX; PACKAGE QUANTITY: 500 SHEETS PER REAM; TYPE REAM PHONE; 80G/M2, 500 SHEETS PER REAM; FUNC LOC: CONSUMABLES ***** END DETAIL DESCRIPTION ***** ML 2021/03/24",100,"EA"]
["0502922","PAGER:2028 ALPHA-NUMERIC","C.O.C; 0147/88Q; Q4:NSF:NC:0; PAGER; ALPHA NUMERIC; MFR:ITRONICS; P/NO: 2028; SIGNAL FORMAT: POCSAG 512 OR 1200BPS; CAP CODES: 8; MESSAGE CAPACITY: 19 MESSAGES UP TO 512 CHARACTERS EACH; LCD DISPLAY: 4 LINES X 20 CHARACTERS OR ZOOM TO 2 LINES X 2 CHARACTERS; LCD BACKLIGHT: WHITE LED; DIMENSION: 80MM (L) X 54MM (W) X 19MM (H); WEIGHT: 68G WITH BATTERY; FUNCT.LOC: SYSTEM 0DVT; ***** END DETAIL DESCRIPTION *****; JNF 2012/02/11; JNF 2012/02/15; CLC 2012/10/18; CLC 2014/05/16; CLC 2014/05/21; ML 2020/04/29; ML 2020/11/23; ML 2022/02/16",150,"EA"]
["0595684","TOWEL,HAND:21 CM;LG 660 SHEETS PER ROLL","N/A; NO ENG.INPUT REQ,D; SCOTT SLIMROLL HAND TOWEL; SUPPLIER:PTA AGENCY CC; CODE:6657010/1; WIDTH: 21 CM; LENGTH: 660 SHEETS PER ROLL; MATERIAL: SCOTT SLIMROLL; COLOR: WHITE; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2014/12/04; JNF 2014/12/09",150,"EA"]
["0597202","TORCH:PROTECTIVE HELMET HEADLAMP","C.O.C; 0040/88Q; Q4:NSF:NC:0:L3; TORCH; MNF: ENERGIZER; P/NO: MSHD3AA; TYPE: PROTECTIVE HELMET HEADLAMP; DIMENSIONS: SHALL BE INTRINSICALLY SAFE; ADJUSTABLE;  PROVIDE AT LEAST 400 LUMENS AT 20 METER FOR 6 HOURS AND MUST BE ABLE TO FIT ALL TYPES OF PROTECTIVE HELMETS ***** END DETAIL DESCRIPTION ***** ML 2021/01/29; ML 2021/02/22; ML 2021/05/05",300,"EA"]
["0600620","BATT DCELL:NIMH;1.2 V;AAA;FLAT TERMINALS","C.O.C; 0016/96Q; Q4:NSF:NC:1; BATTERY, DRY CELL: TYPE: RECHARGEABLE; POTENTIAL: 1.2 V; DIMENSIONS: AAA; CONNECTION: FLAT TERMINALS; MATERIAL: NIMH; FUNCT LOC:1/2 KRT 1-19 MA; 1/2 KRT 21-25 MA; ***** END DETAIL DESCRIPTION *****; CLC 2015/04/13",1500,"EA"]
["0604458","BATT:DURACELL, AA;1.5 V","N/A; 0200/87Q; Q5:NSF:NC:0; DURACELL BATTERY; TYPE: DURACELL; AA; POTENTIAL: 1.5 V; FUNCT.LOC: CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2015/06/26",{"v":4500,"d":"4,500"},"EA"]
["0607409","PAPER BOND:WD 210 X LG 297 MM;BLUE;REAM","C.O.C; 0040/88Q; Q4:NSF:NC:0; PAPER,BOND; MNF: TYPEK; SIZE: WD 210 X LG 297 MM; COLOR: BLUE; PACKAGE TYPE: REAM; PACKAGE QUANTITY: 500 PAGES; A4; REAM; COLOR: BLUE; ALL PRINTERS; ***** END DETAIL DESCRIPTION *****; JNF 2015/08/25; ML 2019/07/30",{"v":2000,"d":"2,000"},"EA"]
["0716592","DISHWASH COMP            5L","C.O.C; 0040/88Q; Q4:NSF:NEV:NC; DETERGENT; MNF: ZONE CHEMICALS; P/NO: E15DW5;TRADE NAME: DETERGENT; SPECIFIC USE: DISH WASHING; PACKAGE TYPE: CAN PLASTIC; PACKAGE WEIGHT: 5 L; PHYSICAL FORM: LIQUID; ISO 9002 SABS MATERIAL DATA SHEET REQUIRED WITH EVERY DELIVERY; FUNC LOC: CONSUMABLE ***** END DETAIL DESCRIPTION ***** JNF 2002/05/30 JNF 2009/04/19 JNF 2010/06/25; ML 2020/05/21",{"v":1300,"d":"1,300"},"EA"]
["0724197","PAPER,TOILET:ROLL;1;WHITE","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; PERFORATED, SHALL BE WOUND ON TO A CORE AND SHALL BE OF THE UNDERMENTIONED SHEET COUNT, 500 SHEETS AND MULTIPLES OF 100 SHEETS PER ROLL ABOVE 500 SHEETS, WRAPPED IN POLYTHENE BAGS CONTAINING 48 ROLLS SABS SPEC 648-1984 AS AMENDED; CORE SIZE: 40 MM; SIZE: WD 100 X LG 110 MM; FUNCT.LOC: CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2014/03/27",{"v":550000,"d":"550,000"},"EA"]
["0079224","BLADE KNF:TRIMMING;STL","C.O.C; 0040/88; NQL:NSF:NC: BLADE, KNIFE; P/NO: 1992; TYPE: TRIMMING; DIMENSIONS: WD 19 X LG 60 X THK 0.6 MM; MATERIAL: HEAVY DUTY; FUNC LOC: CONSUMABLE  ***** END DETAIL DESCRIPTION ***** BOM SEQ NO:0898; ML 2022/07/14",4500,"EA"]
["0079228","KNIFE:TRIMMING, RETRACTABLE BLADE","N/A\\0040/88Q:Q5:NSF:NC:NEV DESCRIPTION CONFIRMED-STG/COD-91/05 RETRACTABLE BLADE TRIMMING KNIFE 3-POSITION BLADE BUTTON & BLADE STORAGE FURNISHED WITH NO1992 HEAVY DUTY BLADES TYPE 99 P/NO: TH128-99 MATL: LIGHT ALUMINIUM BODY TRI: 6MBI 008BG ***** END DETAIL DESCRIPTION ***** BOM SEQ NO:0898",600,"EA"]
["0108549","PADLOCK:KEY;6 MM;WD 33 X THK 40 MM;BRASS","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; PADLOCK; TYPE: KEY; SHACKLE DIAMETER: 6 MM; CASE SIZE: WD 33 X THK 40 MM; MATERIAL: BRS; VERTICAL CLEARANCE: 20 MM; HORIZONTAL CLEARANCE: 23 MM  ***** END DETAIL DESCRIPTION ***** JNF 2012/02/10; ML 2022/08/05; ML 2022/09/08",7500,"EA"]
["0109013","TAPE:MIRROR SCOTCH;SYNTHETIC ADHESIVE","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; TAPE; MFR:3M;  TYPE: MIRROR SCOTCH; DIMENSIONS: WD 24 MM X LG 33 M X THK 3 MM; MATERIAL: SYNTHETIC ADHESIVE; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2014/09/16; ML 2021/08/05",300,"EA"]
["0160050","BRUSH PAINT:SETTER;WD 25 MM;FLAT;PLASTIC","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV FLAT PAINT BRUSH DIMEN:25MM X 48MM X 16MM ***** END DETAIL DESCRIPTION ***** A.V.2001/04/25 JNF 2009/09/03 BOM SEQ NO:0898",1500,"EA"]
["0160051","BRUSH PAINT:SETTER;WD 50 MM;FLAT;PLASTIC","SABS901-1973; 0040/88Q;Q5:NSF:NC:NEV; BRUSH, PAINT: TYPE: SETTER; WIDTH: 50 MM; MATERIAL: BRISTLE CHINESE PURE; SHAPE: FLAT; HANDLE: PLASTIC; LG 55 MM X THK 15 MM ***** END DETAIL DESCRIPTION ***** ML 2019/05/23",1500,"EA"]
["0160052","BRUSH PAINT:SETTER;WD 75 MM;FLAT;PLASTIC","SABS901-1973\\0040/88Q\\Q5:NSF:NC:NEV DESCRIPTION CONFIRMED-SEG/COD-92/12\nBRUSH, PAINT: TYPE: SETTER; WIDTH: 75 MM; MATERIAL: BRISTLE CHINESE PURE; SHAPE: FLAT; HANDLE: PLASTIC; SIZE: 65MM LG X 22MM THK; THE ITEM MUST BE PROTECTIVE PACKED",800,"EA"]
["0256629","INSECTICIDE:FLYING/CRAWLING INSECTS","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV (MATERIAL SAFETY DATA SHEET (MSDS) AND OR TECHNICAL DATE SHEET (TDS) REQUIRED WITH EVERY DELIVERY AND MUST INCLUDE MANUFACTURING DATE,EXPIRY DATE AND ALLOWABLE DEVIATION OF PRODUCT); ALL CHEMICALS WITH A SHELF-LIFE, SHALL NOT EXPIRE WITHIN ONE (1) YEAR; NEO INSEKIL AERO SPACE INSECTICIDE PACKG:ANY ACCEPTABLE FUNCT.LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2011/06/28",2000,"EA"]
["0578629","CREAM BARR:PETROLEUM JELLY WHITE;500 G","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; (MATERIAL SAFETY DATA SHEET (MSDS) AND OR TECHNICAL DATE SHEET (TDS) REQUIRED WITH EVERY DELIVERY AND MUST INCLUDE MANUFACTURING DATE,EXPIRY DATE AND ALLOWABLE DEVIATION OF PRODUCT;ALL CHEMICALS WITH A SHELF-LIFE,SHALL NOT EXPIRE WITHIN ONE (1) YEAR); WHITE VASELINE SOOTHING PETROLEUM CREAM; CRACK APPROVED - CATEGORY 1; DIMEN: 500GRAM CONTAINER; ***** END DETAIL DESCRIPTION *****; JNF 2013/11/22",330,"EA"]
["0579645","LATCH DOOR:WITH LATCH & DEADBOLT","DSG-319-008; 0086/91Q; Q4:NSF:NC:NEV; CISA HD EXIT PANIC LATCH; (LATCH, DOOR); SUPPLIER:JK HARDWARE; CODE:52840-60; TYPE: HEAVY DUTY CYLINDER MOTICE LOCK; STYLE: WITH LATCH & DEADBOLT; DIMENSIONS: WD 170 X HT 85 MM; FUNCT.LOC:1/2/9JFD; ***** END DETAIL DESCRIPTION *****; JNF 2013/12/17",70,"EA"]
["0579646","LATCH DOOR:LATCH ONLY-NO DEADBOLT","DSG-319-008; 0086/91Q; Q4:NSF:NC:NEV; CISA MORTICE LATCH/LOCK; (LATCH, DOOR); SUPPLIER:JK HARDWARE; CODE:52755-60-20; TYPE: HEAVY DUTY CYLINDER MOTICE LOCK; STYLE: LATCH ONLY-NO DEADBOLT; DIMENSIONS: WD 170 X HT 85 MM; FUNCT.LOC:1/2/9JFD; ***** END DETAIL DESCRIPTION *****; JNF 2013/12/17",200,"EA"]
["0579707","HANDLE DOOR:BLANK;SS","DSG-310-084; 0353/Q4:NSF:NC:NEV; BLANK S/S L HANDLE PER PAIR; LEFT & RIGHT HAND HANDLES; SUPPLIER:JK HARDWARE; P/N:MOLO/Q54484; TYPE: BLANK; SIZE: WD 45 X LG 245 X THK 8 MM; MATERIAL: SS; CENTRE TO CENTRE DIMENSION FOR FIXING BOLTS (BOOK BINDING SCREW) MUST BE 220M; FUNCT.LOC:1/2/9JFD; ***** END DETAIL DESCRIPTION *****; JNF 2013/12/18; ML 2018/07/27",250,"EA"]
["0728125","BATT:LITHIUM;3 V;540 AH","C.OC; Q4; BATTERY: TYPE: LITHIUM; POTENTIAL: 3 V; CURRENT CAPACITY: 540 AH; FUNC LOC: CONSUMABLE; END DETAIL DESCRIPTION: YA 2023/08/16",4000,"EA"]
["0690550","BATT:ALKALINE-MANGANESE;9 V","BATTERY: TYPE: ALKALINE-MANGANESE; POTENTIAL: 9 V; ALKALINE-MANGANESE DIOXIDE INTRINSIC SAFE 9V BATTERY (MN 1604 OR MX 1604)",200,"EA"]
["0013856","BATT DCELL:ZN CARBON;1.5 VDC;C","C.O.C; 0012/88Q;Q4:NSF:NC:0; DRYCELL BATTERY; (MEDIUM); MFR:EVEREADY; DIMEN:24MM DIA X 48MM LONG; (1,5VOLT); MATL:ZINC CARBON; FUNCT.LOC: CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2004/03/30; JNF 2016/02/18",6000,"EA"]
["0109565","PAD CLNG:TAPE, FINISHING ROLL","C.O.C; 0040/88; Q4:NSF:NC:NEV; PAD, CLEANING; TYPE: TAPE, FINISHING ROLL; DIMEN: WD 50 MM X LG 10 M; MAT: SCOTCH BRIGHT TAPE / BUFFRITE; END DETAIL DESCRIPTION: ML 2021/11/17; ML 2022/03/11; YA 2023/09/10",12000,"M"]
["0144630","BATT DCELL:ALKALINE;1.5 V;AAA;SLIM","C.O.C; 0125/89Q; Q4:NSF:NC:0; LR03 HP 16 BATTERY FOR USE IN PAGERS & COMMUNICATIONS; TYPE: AAA; MFR:DURACELL; P/NO: MN2400; DIMEN: 10.5 X 44.5MM; FUNCT.LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2004/03/30; CLC 2013/09/20; CLC 2014/04/21",35000,"EA"]
["0144646","BATT DCELL:ALKALINE;1.5 VDC;AA;FLAT PIN","BATTERY, DRY CELL: MATERIAL: ALKALINE; POTENTIAL: 1.5 VDC; DIMENSIONS: AA; CONNECTION: FLAT PIN; SUPPL P/N: MN1500; SAFETY DATA SHEETS REQUIRED ON DELIVERY HAZARDOUS SUBSTANCES, THIS PRODUCT IS CLASSIFIED AS HAZARDOUS SUBSTANCE AND SAFETY BROUCHURES MUST ACCOMPANY DELIVERY, IN ACCORDANCE WITH THE OCCUPATIONAL HEALTH AND SAFETY ACT OHSA, ACT 85 OF 1993 SECTION 10 AND 11; SIZES LR6/R6PP/AA/UM3/MN1500; DIMEN: 14X50MM LG",32000,"EA"]
["0144702","BATT DCELL:LITHIUM;3.6 V","N/A\\0125/89Q\\Q5:NSF:NC:0 LITHIUM BATTERY MFR: SAFT DIMEN: 14,3MM DIA X 25MM RANGE: 3,6V FUNCT.LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2004/03/30",10,"EA"]
["0147474","DISINFECTANT:BOTTLE PLASTIC;100 ML","N/A; 0040/88Q; Q4:NSF:NC:NEV; (MATERIAL SAFETY DATA SHEET (MSDS) AND OR TECHNICAL DATE SHEET (TDS) REQUIRED WITH EVERY DELIVERY AND MUST INCLUDE MANUFACTURING DATE,EXPIRY DATE AND ALLOWABLE DEVIATION OF PRODUCT ALL CHEMICALS WITH A SHELF-LIFE,SHALL NOT EXPIRE WITHIN ONE (1) YEAR);DISINFECTANT; MNF: BE SAFE PARAMEDICAL;TYPE: CETRIMIDE ANTISEPTIC CLEANER; UNIT PACKAGE TYPE: BOTTLE PLASTIC; PACKAGE WEIGHT: 100 ML ***** END DETAIL DESCRIPTION *****; JNF 2001/03/08; CCL.2005/06/27; JNF 2012/05/16; ML 2021/07/19",200,"EA"]
["0159426","PAPER RL:CONTINUOUS FLAT FOLD;WHITE","N/A\\0040/87Q\\Q5:NSF:NC:0 CONSOLE PAPER * PLAIN * SIZE 280MM LONG * 240MM WIDE * PERFORATED * PUNCHED HOLES ON BOTH SIDES * 2000 SHEETS = PER BOX * ** END PURCHASING ** PAPER,WHITE A4 FOR PRINTER L-ORD:10837379B-CD:",15,"EA"]
["0159552","BOOK REC:SHIFT SUPERVISORS LOG;A4;150","NA; 0040/88Q; Q5:NSF:NC:NEV;  BOOK, RECORD; P/NO: T 8971; TYPE: SHIFT SUPERVISORS LOG; SIZE: A4; PAGE QUANTITY: 150; NUMBERED PAGES: YES; MATL 3 PLY WHITE, GREEN, PINK; FUNC LOC: CONSUMABLE  ***** END DETAIL DESCRIPTION ***** ML 2022/03/24",400,"EA"]
["0159741","BRUSH SCRB:HANDY NAIL, DISPOSABLE ","N/A\\0040/88Q\\Q4:NSF:NC:NEV NAIL BRUSH HANDISCRUB PLAIN (DISPOSABLE) (25 PER BOX) ***** END DETAIL DESCRIPTION JNF 2002/10/28 JNF 2006/10/04",350,"EA"]
["0159835","CLEANER FLR:25 L","N/A\\0040/88Q\\Q5:NSF:NC:NEV (MATERIAL DATA SHEET REQUIRED WITH EVERY DELIVERY) FLOOR SELECT EASI CLEANING COMPOUND STRIP AMMONIATED CRACK NON PLANT - CATEGORY 3 DIMEN:25 LITRE CONTAINER ***** END DETAIL DESCRIPTION ***** A.V.2001/09/10 JNF 2005/10/28 ET 2010/06/28",3000,"EA"]
["0160053","BRUSH PAINT:SETTER;WD 100 MM;FLAT","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV BRUSH PAINT:TYPE SETTER SIZE:100MM WD X 79MM LG X 22MM THK MATL:PURE CHINESE BRISTLE,PLASTIC HANDLE,SHAPE FLAT FUNCT.LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2003/06/25",10,"EA"]
["0160440","BOTTLE:NAT DUMPY JAR;1 L;HDPE","C.OC; 0040/88Q; Q4:NQL:NSF:NC:NEV; BOTTLE;  POLYTHENE BOTTLE (GRIP JAR) ; MNF:PLASTIC WORLD PTY (LTD);  TYPE: NAT DUMPY JAR; CAPACITY: 1  L; MATERIAL: SEMI CLEAR WITH WHITE LID; STYLE: HDPE; SPECIFICATION: 1 EACH = 1 BOTTLE / JAR   END DETAIL DESCRIPTION ML 2017/08/24; ML 2018/01/18; ML 2021/06/21; ML 2022/07/08; ML 2022/08/11",7000,"EA"]
["0160441","BOTTLE:LIQUID AND OIL SAMPLE;100 ML;PE ","C.O.C; 0040/88Q; Q4:NSF:NC:NEV;BOTTLE: TYPE: LIQUID AND OIL SAMPLE; CAPACITY: 100 ML; MATERIAL: PE; STYLE: ROUND SCREW TOP; DIA 3.5 CM X HT 7.5 CM; END DETAIL DESCRIPTION; JP 92/07/02; BN 2022/11/18; ND 2023/11/16",12000,"EA"]
["0162637","LEAD ELECT","N/A\\0040/88Q\\:Q5:NSF:NC:NEV DESCRIPTION CONFIRMED-STG/COD-92/04 WIRE LEAD DIMEN:1MM KBA:1215G02005 ITM:X   1 = SEQ:0643 S/LIST: M/MAN: / ASMT:1781 1 = SEQ:0643 TRI:1/2LHP/LHQ 001GA 9LHS 001GA 1 = SEQ:0643 ***** END DETAIL DESCRIPTION ***** JNF 2000/07/21 A.V.2001/08/08 BOM SEQ NO:0643 = 0000MCAAA0001",50,"EA"]
["0209935","SPRAYER:BOTTLE 500 ML","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV PLASTIC 500ML SPRAY BOTTLE WITH TRIGGER MECH.(WATER) (FOR ASBESTOS USE) SUPPLIER:N/A MATL:PLASTIC RANGE:500ML FUNCT.LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2003/08/22",1000,"EA"]
["0209936","BAG:650 X 800 MM;PLASTIC","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV PLASTIC BAGS WITH ASBESTOS WARNING ON SIDE SUPPLIER:N/A DIMEN:650 X 800MM MATL:PLASTIC FUNCT.LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2003/08/22",500,"EA"]
["0214560","TAPE EMBSG:BLUE ON WHITE;24 MM;160 UM;8","C.O.C\\0040/88Q\\Q4:NSF:NEV LABELING TAPE CASSETTE MFR:BROTHER-P-TOUCH 9500 PC P/NO:TZ-253 FUNCT.LOC:6HAI 000BG ***** END DETAIL DESCRIPTION ***** JNF 2004/10/14",170,"EA"]
["0227583","CORD EXT:3;250 V;10;16 A","CORD, EXTENSION: CONDUCTOR: 3; POTENTIAL: 250 V; RECEPTACLES: 10; CURRENT: 16 A; REFERENCE NO: SK380010; ELECTRICAL; 1 POLE, MULTIPLUG DOUBLE SIDED WITH INDIVIDUAL ON/OFF SWITCHES; C/W EARTH LEAKAGE; RESET BUTTON AND 3M CABLE",50,"EA"]
["0234404","TAPE:DEMARCATION;WD 48 X HT 105 X LG 33M","C.O.C; 0040/88Q;Q4:NSF:NC:NEV; TAPE; MFR:INTEGRAL SAFETY PRODUCTS (PTY)LTD; P/NO: DT-48/Y; TYPE: DEMARCATION; DIMENSIONS: WD 48 MM X HT 105 MM X LG 33M; MATERIAL: SYNTHETIC ACRYLIC ADHESIVE; COLOR: YELLOW; CODE: FLOOR MARKING; A HIGH PERFORMANCE, CONFORMABLE TAPE IDEALLY SUITED TO COLOUR CODING AND DEMARCATION OF FACTORY/WAREHOUSE AND OTHER FLOOR AREAS; FUNCT.LOC:(VARIOUS) ***** END DETAIL DESCRIPTION ***** JNF 2008/06/27; ML 2022/08/16",150,"EA"]
["0234405","TAPE SFTY BARR:DEMARCATION;WHITE","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV DEMARCATION TAPE MFR:INTEGRAL SAFETY PRODUCTS (PTY)LTD CODE:DT-48/W COLOUR:WHITE FUNCT.LOC:(VARIOUS) ***** END DETAIL DESCRIPTION ***** JNF 2008/06/27",150,"EA"]
["0234656","TAPE ADHSV:MASKING;WD 48 MM X LG 40 M","(N/A\\0040/88Q\\Q5:NSF:NC:NEV MASKING TAPE MOISTURE OIL AND SOLVENT RESISTANT DIMEN:LTH = 40M X WTH = 48MM ***** END DETAIL DESCRIPTION ***** JNF 2008/07/02",15000,"EA"]
["0236094","BARRIER ZNR ","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV Z-BARRIER  P/NO:MTL-992-5020K LENGTH:2-4M FUNCT.LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2008/08/22",3500,"EA"]
["0236095","BARRIER ZNR","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV Z-BARRIER  P/NO:MTL-992-5030K LENGTH:3-6M FUNCT.LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2008/08/22",5000,"EA"]
["0236097","BARRICADE:POCKET BARRIER SIGN;PVC","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV BARRIER SIGN POCKET  P/NO:MTL-992-7010K MATL:PVC SIZE:A4 FUNCT.LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTIN ***** JNF 2008/08/22",5000,"EA"]
["0242383","BOTTLE:OIL SAMPLE;90 ML;PLASTIC","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV PLASTIC SAMPLE CONTAINER (90ML PLASTIC OIL SAMPLE BOTTLES WITH A BLACK PLASTIC SAFETY BOTTLE OUTER) MFR:OILWATCH RANGE:10 SAMPLES IN A BOX FUNCT.LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2009/07/02",250,"EA"]
["0584937","BATT:LEAD ACID;12 V;65 AH","BATTERY: TYPE: LEAD ACID; POTENTIAL: 12 V; CURRENT CAPACITY: 65 AH; MANUF P/N: DB12-65; BATTERY FOR MINIMAX PANEL PLANT A; 12V 65AH AGM LONG LIFE BATTERY",5,"EA"]
["0592142","TIE CBL:LOCKABLE IMS ONLY;50 MM;WD 2.6","C.O.C; 0201/87Q; Q4:NSF:NC:0; CABLE TIES FOR HIGH TEMPERATURE; SUPPLIER: TIDY CABLES; P/N:PLT1.5M-C71; TYPE: SELF LOCKING; HIGH TEMPERATURRE USE ONLY; DIAMETER RANGE: 50 MM; WIDTH: 2.6 MM; LENGTH: 147 MM; MATERIAL: POLYETHERETHERKETONE; FUNCT LOC:VVP; GCT; GSS; ***** END DETAIL DESCRIPTION *****; CLC 2014/09/10",100,"EA"]
["0595683","SOAP:LUXURY FOAM;1 L;1800 X 24 DOUBLE","N/A; NO ENG.INPUT REQ'D; KLEENEX LUXURY FOAM SOAP; SUPPLIER:PTA AGENCIES (PTY) LTD; CODE:6342020; 1LITRE; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2014/12/04; JNF 2014/12/09",15,"EA"]
["0648390","TISSUE:CLOTH LINT FREE;WD 5 X LG 10 CM","C.O.C; 0059/86Q; Q4:NSF:NC:NEV; SOLE SOURCE SUPPLIER: HANNA; P/NO: HI731318; TISSUE: TYPE: LINT FREE CLOTH; DIMENSIONS: WD 5 X LG 10 CM; CONTAINER: BOX ***** END DETAIL DESCRIPTION ***** ML 2018/03/27",5,"EA"]
["0662602","BOTTLE:STORAGE;5 L;POLYETHYLENE;WHITE","C.O.C; 0044/88Q; Q4:NSF:NC:NEV; BOTTLE; MNF: MERCK; P/NO: 130970; TYPE: STORAGE; CAPACITY: 5 L; MATERIAL: POLYETHYLENE; STYLE: ROUND, WIDE MOUTH WITH SCREW CAP AND CARRY HANDLE; COLOR: WHITE ***** END DETAIL DESCRIPTION ***** ML 2019/01/29",5,"EA"]
["0662606","BOTTLE:STORAGE;10 L;POLYETHYLENE","C.O.C; 0044/88Q; Q4:NSF:NC:NEV; BOTTLE; MNF: MERCK; P/NO: 130974; TYPE: STORAGE; CAPACITY: 10 L; MATERIAL: POLYETHYLENE; STYLE: WIDE MOUTH WITH SCREW CAP AND CARRYING HANDLE ***** END DETAIL DESCRIPTION ***** ML 2019/01/30",5,"EA"]
["0675227","WIPE:DISPOSABLE;UNIVERSAL","C.O.C.;0040/88Q;NSF:NC:Q4:NEV; WIPE; P/NO: SA081653; TYPE: DISPOSABLE; KIMCLOTH X50 JUMBO ROLL BLUE 45 GSM RAYON BASED ON DISPENSING ROLL COLOUR: BLUE;  DIMENSIONS: 250MM WIDE,AND 300M IN LENGTH, 200 SHEETS PER ROLL; RTCOVID19-010; FUNC LOC: CONSUMABLES ***** END DETAIL DESCRIPTION ***** ML 2020/05/15; ML 2020/08/13",1000,"EA"]
["0703710","LABEL:THERMAL;70.5 X 45 MM;GREEN;BLANK","C.O.C; 0040/88Q; Q4:NSF:NC:NEV:L3; LABEL; MNF: NEW WORLD DESIGN; TYPE: THERMAL; SIZE: 70.5 X 45 MM; COLOR: GREEN; DESIGNATION: BLANK; MATERIAL: THERMAL TOP COAT, HOTMELT ADHESIVE; PACKAGE SIZE: 500 LABELS PER ROLL; FUNC LOC: CONSUMABLE ****** END DETAIL DESCRIPTION ****** ML 2021/09/27",500,"EA"]
["0721581","CASST:BROTHER P -TOUCH;PLASTIC ","C.O.C; 0040/88Q; Q4:NSF:NC:0:L3; CASSETTE: TYPE: BROTHER P -TOUCH; MNF: BROTHER; P/N: TZE-231; MAT: PLASTIC; SIZE: 12 MM X 8 M; APPLICATION: LAMINATED LABEL CASSETTE; FUNC LOC: CONSUMABLE; END DESCRIPTION: YA 2023/02/10",30,"EA"]
["0721634","BATT:BUTTON;1.5 V;1.5 V","C.O.C; 0040/88Q; Q4:NSF:NC:0:L3; BATTERY; MNF: DURACELL; P/N: N/A; TYPE: BUTTON; POTENTIAL: 1.5 V; CURRENT CAPACITY: 1.5 V; PRODUCT CODE: LR44; END DESCRIPTION 2023/02/11; YA 2023/04/25",30,"EA"]
["0721639","CASST:BROTHER P -TOUCH;PLASTIC","C.O.C; 0040/88Q; Q4:NSF:NC:0:L3; CASSETTE; MNF: BROTHER; P/N: TZE-241; TYPE: BROTHER P -TOUCH; MAT: PLASTIC; SIZE: 18 MM X 8 M; APPLICATION: LAMINATED LABEL CASSETTE, BLACK ON YELLOW; FUNC LOC: CONSUMABLE; END DESCRIPTION: YA 2023/02/11",30,"EA"]
["0721727","CASST:BROTHER P -TOUCH;PLASTIC","C.O.C; 0040/88Q; Q4:NSF:NC:0:L3; CASSETTE, MNF: BROTHER; P/N: TZE-251; TYPE: BROTHER P -TOUCH; MAT: PLASTIC; SIZE: 24 MM X 8 M; APPLICATION: LAMINATED LABEL CASSETTE; BLACK ON YELLOW; FUNC LOC: CONSUMABLE; END DESCRIPTION: YA 2023/02/11",30,"EA"]
["0724839","CARTRIDGE INK:3;BLACK","C.O.C; Q4; CARTRIDGE, INK; MNF: ROTRING WEBSITE; P/N: SKU: RS0194640; CARTRIDGE TYPE: CARTRIDGE 3; COLOR: BLACK; APPLICATION: ROTRING RAPIDOGRAPH DRAWING INK ; END DETAIL DESCRIPTION: YA 2023/05/18; ND 2023/07/10; YA 2023/08/18",5,"EA"]
["BATCH 2   -   FOREIGN EXCLUSION MATERIALS"]
["0241944","CLIP:GLOVE","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV GG GLOVE CLIPS MFR:OVERSEA SUPPLIER:GREYSTOKE MECHANICAL P/NO:1-888-660-6133 COLOUR:BLUE FUNCT.LOC:(CONSUMABLE) ***** END DETAIL DESCRIPTION ***** JNF 2009/05/20",13000,"EA"]
["0244561","LANYARD:TOOL","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; TOOL LANYARD, HEAVY DUTY; SUPPLIER:BOLT & ENGINEERING DISTRIBUTORS CAPE; P/NO:MISC/004; FUNCT.LOC:(NON PART) ***** END DETAIL DESCRIPTION ***** JNF 2009/10/12; JNF 2010/03/25; CLC 2014/03/24",5000,"EA"]
["0244562","LANYARD:WRIST","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV WRIST LANYARD SUPPLIER:CAD TECHNICAL AND INDUSTRIAL SUPPLIES P/NO:3115 COLOUR:BLACK FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/10/12 JNF 2010/03/30",7000,"EA"]
["0592297","LANYARD:RETRACTABLE;PLASTIC;LG 5 IN;CLIP","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; RETRACTABLE LANYARDS WITH SWIVEL SPRING CLIP; SUPPLIER:SIYAPHAMBILI ELECTRICAL & INDUSTRIAL SUPPLIES CC; P/N:CC5-PH; MATERIAL: PLASTIC; LENGTH: 5 IN; ENDS: CLIP; FUNCT.LOC:N/A; ***** END DETAIL DESCRIPTION *****; JNF 2014/09/17",6000,"EA"]
["0592298","RETAINER:EYEGLASS;STD;COTTON 100 PCT","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; EYEGLASS RETAINER; SUPPLIER:SIYAPHAMBILI ELECTRICAL & INDUSTRIAL CC; DIMENSIONS: STANDARD; MATERIAL: 100% COTTON; FUNCT.LOC:NON-PLANT; ***** END DETAIL DESCRIPTION *****; JNF 2014/09/17",14000,"EA"]
["0597723","LANYARD:FME NECK ORANGE;LG 500 MM","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; NECK LANYARD BREAK AWAY WITH FME FOP (ORANGE); MANUCFACTURER: TY-FLOT; LOCAL SUPPLIER:SIYPHAMBILI ELECTRICAL AND INDUSTRIAL SUPPLIES; CODE:NL-PR-19-34W-OR; LENGTH:500MM; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2015/02/02 JNF 2015/02/02JNF  2015/02/02",13000,"EA"]
["0597728","CLIP:FME BADGE;30 MM;METAL","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; VERSACLAMP UNIVERSAL BADGE; CLIP; MNF: TY-FLOT;  P/NO: TETHCRRDOR; DIMENSIONS: 30 MM; MATERIAL: METAL; ORANGE; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2015/02/02; JNF 2015/02/11; ML 2020/06/15",7000,"EA"]
["0597739","RING:D;ID 18 MM;OD 20 MM;WD 2.5 IN;NYLON","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; HIGH STRENGTH NYLON WEBBING D-RING; MANUFACTURER:TY-FLOT; LOCAL SUPPLIER:SIYPHAMBILI ELECTRICAL AND INDUSTRIAL SUPPLIES; CODE:DRSM; TYPE: D; INSIDE DIAMETER: 18 MM; OUTSIDE DIAMETER: 20 MM; WIDTH: 2.5 IN; MATERIAL: NYLON; COLOUR:ORANGE; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2015/02/02; JNF 2015/02/11",1500,"EA"]
["0160381","BAG:WD 500 MM X LG 1 M X THK 250 UM","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; CLEAR PLASTIC BAG PRINTED IN BLACK:\"KOEBERG MAINTENANCE DEPARTMENT\" PRINTING ON A WHITE SQUARE 200X200MM SUITABLE FOR WRITING ON; MFR:PACKIT; P/N:N/A; DIMENSIONS: WD 500 MM X LG 1 M X THK 250 UM; MATERIAL: PLASTIC HEAVY DUTY; COLOR: ORANGE SEE-THROUGH PLASTIC; DESIGNATION: KOEBERG MAINTENANCE DEPARTMENT; DESIGNATION COLOR: BLACK ON WHITE; SQUARE 200 X 200 MM; FUNCT.LOC: CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2004/03/23; JNF 2014/04/10",40000,"EA"]
["0160360","BAG:MAINTENANCE;ORANGE;BLACK ON WHITE","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; CLEAR PLASTIC BAG PRINTED IN BLACK:\"KOEBERG MAINTENANCE DEPARTMENT\" PRINTING ON A WHITE SQUARE 200X200MM SUITABLE FOR WRITING ON; MNF:PACKIT; DIMENSIONS: WD 300 MM X LG 500 MM X THK 180 UM; MATERIAL: PLASTIC HEAVY DUTY; COLOR: ORANGE SEE-THROUGH PLASTIC; DESIGNATION: KOEBERG MAINTENANCE DEPARTMENT; DESIGNATION COLOR: BLACK ON WHITE; FUNCT.LOC: CONSUMABLE; **** END DETAIL DESCRIPTION ****; JNF 2004/03/23; JNF 2014/04/10; JNF 2015/01/14; JNF 2015/02/13",70000,"EA"]
["0568371","SHEET PLSTC:WD 1 M;LG 100 M;THK 250 UM","C.O.C;0040/88Q; Q4:NSF:NC:NEV; ORANGE COLOUR PLASTIC SHEET; MFR:N/A; P/NO:N/A; LENGTH: 100 M; WIDTH: 1 M; THICKNESS: 250 U; COLOR: ORANGE SEE-THROUGH PLASTIC; MATERIAL: PLASTIC; SHOULD BE VLAMVAS / NON-FLAMMABLE; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; GAR 21/04/93; JNF 2001/09/21; JNF 2013/04/25; JNF 2014/04/10; ML 2021/01/12",200,"EA"]
["0568370","SHEET:PLASTIC;WRAPPING;ORANGE","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; ORANGE COLOUR PLASTIC SHEET; MFR:N/A; P/N:N/A; DIMEN: 2M WIDE X 30M LONG X 250 MICRON CENTREFOLD; MATL:N/A; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JP 92/09/17; JNF 2013/04/15",250,"EA"]
["0597740","RING:D;ID 36 MM;OD 38 MM;WD 3-1/2 IN","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; HIGH STRENGTH NYLON WEBBING WITH RING; MANUFACTURER:TY-FLOT; LOCAL SUPPLIER:SIYPHAMBILI ELECTRICAL AND INDUSTRIAL SUPPLIES; CODE:DRHD; TYPE: D; INSIDE DIAMETER: 36 MM; OUTSIDE DIAMETER: 38 MM; WIDTH: 3-1/2 IN; MATERIAL: NYLON; COLOR: ORANGE; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2015/02/02; JNF 2015/02/11",700,"EA"]
["0597751","PEN:LANYARD;ORANGE","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; PEN,PENCIL,MARKER 3\" LANYARD; HEAT SHRINK STYLE (ORANGE); MANUFACTURER:TY-FLOT; LOCAL SUPPLIER:SIYPHAMBILI ELECTRICAL AND INDUSTRIAL SUPPLIES; CODE:LYATTI; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2015/02/03; JNF 2015/02/11",8000,"EA"]
["0619205","COVER:FOREIGN MATERIAL;DIA 38 IN;NYLON","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; 38 INCH NYLON FME COVER; MFR:TY-FLOT; CODE:CBFR38; FUNCT LOC: NON PLANT ITEM; ***** END DETAIL DESCRIPTION *****; CLC 2016/06/09",300,"EA"]
["0619206","COVER:FOREIGN MATERIAL;DIA 24 IN;NYLON","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; 24 INCH NYLON FME COVER; MFR:TY-FLOT; CODE:CBFR24; FUNCT LOC: NON PLANT ITEM; ***** END DETAIL DESCRIPTION*****; CLC 2016/06/09",500,"EA"]
["0619207","COVER:FOREIGN MATERIAL;DIA 18 IN;NYLON","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; 18 INCH NYLON FME COVER; MFR:TY-FLOT; CODE:CBFR18; FUNCT LOC: NON PLANT ITEM; ***** END DETAIL DESCRIPTION *****; CLC 2016/06/09",1000,"EA"]
["0619208","COVER:FOREIGN MATERIAL;DIA 12 IN;NYLON","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; 12 INCH NYLON FME COVER; MFR:TY-FLOT; CODE:CBFR12; FUNCT LOC: NON PLANT ITEM; ***** END DETAIL DESCRIPTION*****; CLC 2016/06/09",1000,"EA"]
["0619209","COVER:FOREIGN MATERIAL;DIA 9 IN;NYLON","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; 9 INCH NYLON FME COVER; MFR:TY-FLOT; CODE:CBFR9; FUNCT LOC: NON PLANT ITEM; ***** END DETAIL DESCRIPTION*****; CLC 2016/06/09",1000,"EA"]
["0619210","COVER:FOREIGN MATERIAL;DIA 6 IN;NYLON","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; 6 INCH NYLON FME COVER; MFR:TY-FLOT; CODE:CBFR6; FUNCT LOC: NON PLANT ITEM; ***** END DETAIL DESCRIPTION *****; CLC 2016/06/09",1000,"EA"]
["0619211","COVER:FOREIGN MATERIAL;DIA 4 IN;NYLON","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; 4 INCH FME COVER; MFR:TY-FLOT; CODE:CBFR4; FUNCT LOC: NON PLANT ITEM; ***** END DETAIL DESCRIPTION *****; CLC 2016/06/09",1000,"EA"]
["0619212","COVER:FOREIGN MATERIAL;DIA 2 IN;NYLON","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; 2 INCH FME COVER; MFR:TY-FLOT; CODE:CBFR2; FUNCT LOC: NON PLANT ITEM; ***** END DETAIL DESCRIPTION *****; CLC 2016/06/09",1000,"EA"]
["0619204","COVER:FOREIGN MATERIAL;DIA 1 IN;NYLON","C.O.C; 0040/88Q; Q4:NSF:NC:0; 1 INCH NYLON FME COVERS, MFR:TY-FLOT; P/N:CBFR1; FUNCT LOC: NON PLANT ITEM; ***** END DETAIL DESCRIPTION *****; CLC 2016/06/09",1000,"EA"]
["0709170","CLIP:REUSABLE DOUBLE STRAP - FME","C.O.C; 0040/88Q; Q4:NSF:NC:NEV:L3; CLIP; MNF: TY-FLOT; P/NO: VCLAMPBDGRL; TYPE: REUSABLE DOUBLE STRAP; DIMENSIONS: WD 15 X LG 90 X HT 10 MM; MATERIAL: NON METALLIC (PLASTIC); FUNC LOC: 6 HSM 000 BG ***** END DETAIL DESCRIPTION ***** ML 2022/03/08",1200,"EA"]
["0708401","CAP:FOREIGN MATERIAL EXCLUSION;1/2 IN","C.O.C; 0040/88Q; Q4:NSF:NC:0/1:L3; CAP; MNF: TY-FLOT; P/NO: SWGTC8; TYPE: FOREIGN MATERIAL EXCLUSION; DIMENSIONS: 1/2 IN; MATERIAL: LOW DENSITY POLYETHYLENE; PACKAGE: 100 PER PACK; WILL BE ISSUED IN EACH; FUNC LOC: NON PLANT ***** END DETAIL DESCRIPTION ***** ML 2022/02/21; ML 2022/03/01",50,"EA"]
["0708402","CAP:FOREIGN MATERIAL EXCLUSION;3/8 IN","C.O.C; 0040/88Q; Q4:NSF:NC:0/1:L3; CAP; MNF: TY-FLOT; PNO: SWGTC6; TYPE: FOREIGN MATERIAL EXCLUSION; DIMENSIONS: 3/8 IN; MATERIAL: LOW DENSITY POLYETHYLENE; PACKAGE: 100 PER PACK; WILL BE ISSUED IN EACH; FUNC LOC: NON PLANT ***** END DETAIL DESCRIPTION ***** ML 2022/02/21; ML 2022/03/01",50,"EA"]
["0708408","CAP:FOREIGN MATERIAL EXCLUSION;1/4 IN","C.O.C; 0040/88Q; Q4:NSF:NC:0/1:L3; CAP; MNF: TY-FLOT; P/NO: SWGTC4; TYPE: FOREIGN MATERIAL EXCLUSION; DIMENSIONS: 1/4 IN; MATERIAL: LOW DENSITY POLYETHYLENE; PACKAGE: 100 PER PACK; WILL BE ISSUED IN EACH; FUNC LOC: NON PLANT ***** END DETAIL DESCRIPTION ***** ML 2022/02/21; ML 2022/03/01",50,"EA"]
["0576143","TAG:INSTRUCTION;PLANT;WD 297 X HG 210 MM","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; FOREIGN MATERIAL EXCLUSION ZONE; ZONE OWNER; (TAG); SUPPLIER:NEW WORLD DESIGN; TYPE:INSTRUMENTION; FINISH:IVORY; WIDTH:297; HEIGHT:210MM; MATERIAL:PAPER; DESIGNATION:PLANT; COLOR:ORANGE; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2013/10/19; 2013/10/21",400,"EA"]
["0576147","TAG:INSTRUCTION;PLANT;WD 297 X HG 210 MM","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; FOREIGN MATERIAL EXCLUSION SIGNS; ZONE 1,2 & 3; (TAG); SUPPLIER:NEW WORLD DESIGN; TYPE:INSTRUMENTION; FINISH:IVORY; WIDTH:297; HEIGHT:210MM; MATERIAL:PAPER; DESIGNATION:PLANT; COLOR:ORANGE; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2013/10/19; JNF 2013/10/21",600,"EA"]
["0576151","TAG:INSTRUCTION;PLANT;WD 152 X HG 127 MM","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; FME TAGS WITH STRING; PRINTED BOTH SIDES; SUPPLIER:NEW WORLD DESIGN; TYPE:INSTRUCTION; FINISH:IVORY; MATL:PAPER; WIDTH:152MM; HEIGHT:127MM; DESIGNATION:PLANT; COLOR:ORANGE; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2013/10/21 DESCRIPTION *****; JNF 2013/10/21DESCRIPTION  *****;  JNF  2013/10/21",100,"EA"]
["BATCH 3   -   TOOLS AND EQUIPMENT"]
["0000999","BLADE SAW:HACK;COMBINATION;24;HSS;METAL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV HACKSAW BLADE DIMEN:12.5MM WD X 305 MM LG X 0.63 MM THK 24 TEETH PER INCH ***** END DETAIL DESCRIPTION ***** A.V.2001/04/24 JNF 2010/03/09 BOM SEQ NO:0898",1200,"EA"]
["0001000","BLADE SAW:HACK, JUNIOR;FINE;32;HSS;METAL","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; JUNIOR HACKSAW BLADE; DIMEN:LTH=155MM X THK=0,45 32; TEETH PER 25MM; MATL:CARBON STEEL; ***** END DETAIL DESCRIPTION *****; A.V.2001/04/24; JNF 2013/09/06",360,"EA"]
["0001015","BLADE SAW:JIG;CROSS CUT;12;HSS;HSS","BLADE, SAW: SAW TYPE: JIG; TOOTH DESIGN: CROSS CUT; TEETH PER INCH: 12; BLADE MATERIAL: HSS; CUT MATERIAL: HSS; REFERENCE NO: T118B; SIZE 8MM WD X 100MM LG X 3MM THK, FOR 1577,1578/1580, FOR BOSCH 1577, 1578 AND 1580, CUTTING DATA:MILD STEEL 3 TO 6MM,NON FERROUS METAL, ALUMINIUM 3 TO 10MM, REINFORCED PLATE STEEL:-COOL W/CUTTING OIL OR OIL EMULSION, ALUMINIUM:-COOL W/TURPINTINE OR MIXTURE TURPINTINE AND PARAFFIN",100,"EA"]
["0001779","INSERT:MATERIAL;RUBBER","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; INSERTION RUBBER-BLACK; TYPE: MATERIAL; DIMENSIONS: WD 1.2M X LG 20M X THK 3MM; MATERIAL: RUBBER; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 95/10/10; JNF 2015/09/21; CLC 2017/04/24",1600,"EA"]
["0035825","SAW HOLE:20 MM","N/A\\0040/88Q\\Q5:NSF:NC:0 DESCRIPTION CONFIRMED-SEG/COD-94-04 JAP HOLE SAW COMPLETE WITH MANDREL MFR:BELLCO ELECTRICAL P/NO:H6343 BELLCO STOCK NO.:11820200 DIMEN:20MM MATL:N/A ***** END DETAIL DESCRIPTION ***** A.V.94-04-14",10,"EA"]
["0040983","TESTER:SMOKE DETECTOR","C.O.C\\0421/87Q\\Q4:NSF:NC:NEV DESCRIPTION CONFIRMED-SEG/COD-96/09 Z-STC2 AEROSOL SMOKE DETECTOR TESTER MFR:ZITON SA (PTY) LTD P/NO:18710101 DIMEN:1 CAN = 300G ***** END DETAIL DESCRIPTION ***** A.V.96/09/16",3,"EA"]
["0079179","BLADE SAW:BAND;14 TEETH/IN","BLADE, SAW: SAW TYPE: BAND; TEETH PER INCH: 14 TEETH/IN; 10MM",5,"EA"]
["0079197","BLADE SAW:HACK HAND;FINE;32;HSS;METAL","N/A\\0040/88Q\\:Q5:NSF:NC:NEV DESCRIPTION CONFIRMED-STG/COD-91/11 BLADE HACKSAW HAND TYPE P/NO: DIMEN: 300MMLG 0,63MMTHICK 32 TEETH MATL: HIGH SPEED STEEL KBA:  ITM: KBY: / S/LIST:  M/MAN: ASMT: TRI: ***** END DETAIL DESCRIPTION ***** MANUFACTURER: SUGGESTED SUPPLIER: L/ORD:1KC49271 GAR 12/11/91",600,"EA"]
["0079362","WRENCH ALLN:6 MM;LG L; 32 X 90 MM","WRENCH, ALLEN: SIZE: 6 MM; LENGTH: L; 32 X 90 MM; MATERIAL: HTS ALLOY; HEXAGON HEAD KEY",5,"EA"]
["0079446","HAMMER:CHIPPING;STL;STL","N/A\\0040/88Q\\NQL:NSF:NC:NEV DESCRIPTION CONFIRMED-SEG/COD-94-11 WELDERS CHIPPING HAMMER MNF:LITECOR  P/NO:3450001 DIMEN:N/A MATL:STEEL KBA:  ITM: KBY: / S/LIST:  M/MAN: / ASMT: TRI: **** END DETAIL DESCRIPTION **** A.V.94-11-17",5,"EA"]
["0079516","WRENCH:TRANSFORMER NUT","N/A\\0856/57Q\\NQL:NSF:NC:NEV DESCRIPTION CONFIRMED-SEG/COD-94/02 SPANNER,FOR TRANSFORMER NUT MFR:SEREG  P/N:140-279-31B DIMEN: MATL: KBA:1216H00259 ITM: KBY:624/8802 S/LIST:624KBY8802 M/MAN:510 ASMT:0117 TRI:1/2RRI 001-004MO ***** END DETAIL DESCRIPTION ***** JNF 94/02/11",3,"EA"]
["0079520","JACK HYD HND:CLAW;20 T","JACK, HYDRAULIC HAND: UNIT TYPE: CLAW; LOAD CAPACITY: 20 T",3,"EA"]
["0079523","WRENCH ALLN","WRENCH, ALLEN: SUPPL P/N: C13567/3",5,"EA"]
["0079562","JACK:PNEUMATIC","JACK: TYPE: PNEUMATIC; MANUF P/N: DC70100PP",3,"EA"]
["0079563","JACK:DGS 40 600 PPV","JACK: PART NO: DGS 40 600 PPV, MANUFACTURER: FESTO",3,"EA"]
["0079611","BLADE SAW:JIG;FINE;20;HSS","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; JIGSAW BLADE FOR BOSCH JIGSAW; P/N:T118A; SAW: SAW TYPE: JIG; TOOTH DESIGN: FINE; TEETH PER INCH: 20; BLADE MATERIAL: HSS; CUT MATERIAL: PLYWOOD/PRE FINISHED PANEL; 1,2MM PITCH; MATL:HIGH SPEED TENSILE; PACKG: PACKED IN FIVES; FUNCT.LOC: CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2015/11/13",80,"EA"]
["0079643","CHISEL PWR:BULL POINT;HEX 32 MM;LG 550","CHISEL, POWER: TYPE: BULL POINT; SHANK: HEX 32 MM; LENGTH: 550 MM; MATERIAL: ALLOY FORGED A9260; REFERENCE NO: 4F8993; JACKHAMMER",3,"EA"]
["0079650","BLADE SAW:BAND;6-10;HTS","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV BANDSAW BLADE MFR:ECLIPS SUPPLIER:TOOLQUIP & ALLIED DIMEN:LTH=3700MM WIDTH=27MM TPI 6/10 MAT:HI-TENSILE STEEL FUNCT.LOC:(NON-PLANT - FOR TURNING MACHINE SHOP) ***** END DETAIL DESCRIPTION ***** JNF 2009/03/18",10,"EA"]
["0079743","BIT MSNRY:HAND STAR;11 MM;LG 150 MM","BIT, MASONRY: TYPE: HAND STAR; DIAMETER: 11 MM; LENGTH: 150 MM; TIP: TUNGSTEN CARBIDE; SINGLE TWIST FLUTED",2,"EA"]
["0079761","BIT TWST:24 MM;MORSE TAPER NO 3;HSS","BIT, TWIST: DIAMETER: 24 MM; SHANK: MORSE TAPER NO 3; MATERIAL: HSS; LENGTH: 281 MM; STANDARD: BS 328; DIN 345; ISO 235; 160MM FLUTE LENGTH",15,"EA"]
["0079799","BIT TWST:3 MM;HSS;LG 57 MM;CENTER DRILL","BIT, TWIST: DIAMETER: 3 MM; MATERIAL: HSS; LENGTH: 57 MM; TYPE: CENTER DRILL; STANDARD: BS 4; DOUBLE END, 7.9 MM BODY DIA, 60 DEG ANGLE BOTH ENDS",50,"EA"]
["0079800","BIT TWST:HSS;LG 76 MM;CENTER DRILL;BS 6","BIT, TWIST: MATERIAL: HSS; LENGTH: 76 MM; TYPE: CENTER DRILL; STANDARD: BS 6",50,"EA"]
["0079802","BIT MSNRY:PERCUSSION;25 MM;LG 152 MM","BIT, MASONRY: TYPE: PERCUSSION; DIAMETER: 25 MM; LENGTH: 152 MM; TIP: TUNGSTEN CARBIDE",2,"EA"]
["0079874","BIT TOOL:COUNTERSUNK;DIA 25 X LG 95 MM","BIT, TOOL: TYPE: COUNTERSUNK; DIMENSIONS: DIA 25 X LG 95 MM; MATERIAL: TIP WC; REFERENCE NO: 902210100NW20-25; SUPPL P/N: NW 20-25; COUNTERSUNK CUTTER; ANGLE: 60; FLUTES: 5; SHANK DIAMETER: 12 MM",3,"EA"]
["0137467","BRUSH WRE:CUP;140 X 14 MM","C.O.C; 0040/88Q; Q4:NSF:NC:NEV;  BRUSH, WIRE; TYPE: CUP; MNF: L-ORD; P/NO: C652142; DIMEN: 140 X14 MM; FUNC LOC: CONSUMBLE ***** END DETAIL DESCRIPTION *****  PW 27/03/92",10,"EA"]
["0190985","TESTER:AIR FLOW TEST SET","TESTER: TYPE: AIR FLOW TEST SET",10,"EA"]
["0193142","CALLIPER VRNR:DIGITAL ","CALLIPER, VERNIER: TYPE: DIGITAL; MANUF P/N: CD-12; DIGIMATIC INDICATOR IDU 25E",5,"EA"]
["0206905","WRENCH TRQ:4-20 N M","TORQUE WRENCH MFR:NORBAR RANGE:4-20NM FUNCT.LOC:6HAI 000BG ***** END DETAIL DESCRIPTION ***** JNF 2003/05/21",5,"EA"]
["0234419","INSERT THRDG:HELICOIL;2UN-8","C.O.C\\0159/92Q\\Q4:NSF:NC:NEV HELICOIL INSERTS, MFR:AREVA - NP SUPPLIER:BOLLHOFF HCFR UN 2\"-8 X 1,5 DTN REFNO:V/CDE 23A/1002006265 KBA: 1220B06031 KBY: 557/1004 FUNCT LOC: 2RCP 212VP ***** END DETAIL DESCRIPTION ***** AG 2008/07/01 JNF 2008/07/30 JNF 2008/10/06",2,"EA"]
["0235304","INSERT:LM;ID 12.4 X LG 130 MM","C.O.C\\0018/87Q\\Q4:NSF:NC:NEV CORRO-INSERT \"LM\" MFR:CORROCOAT LENGTH:130MM DIA.I/D:12,4MM FUNCT.LOC:1/2CET 001CS ***** END DETAIL DESCRIPTION ***** JNF 2008/07/29",2,"EA"]
["0243561","BIT TOOL:CRANKED KNIFE ","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED KNIFE TOOL B MFR:TOOLQUIP & ALLIED CODE:ISO6-10X10LH P25 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/08/31",5,"EA"]
["0243562","BIT TOOL:CRANKED KNIFE","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED KNIFE TOOL B MFR:TOOLQUIP & ALLIED CODE:ISO6-10X10RH P25 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/08/31",5,"EA"]
["0243563","CUTTER END MILL:10 MM;3 FLUTE SLOT DRILL ","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV THREE FLUTE SLOT DRILL MFR:TOOLQUIP & ALLIED CODE:HSS-C08 DIA O/D:10MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/08/31",30,"EA"]
["0243564","CUTTER END MILL:12 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV THREE FLUTE SLOT DRILL MFR:TOOLQUIP & ALLIED CODE:HSS-C08 DIA O/D:12MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/08/31",20,"EA"]
["0243565","CUTTER END MILL:16 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV THREE FLUTE SLOT DRILL MFR:TOOLQUIP & ALLIED CODE:HSS-C08 DIA O/D:16MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/08/31",20,"EA"]
["0243566","CUTTER END MILL:18 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV THREE FLUTE SLOT DRILL MFR:TOOLQUIP & ALLIED CODE:HSS-C08 DIA O/D:18MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/08/31",5,"EA"]
["0243567","CUTTER END MILL:22 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV THREE FLUTE SLOT DRILL MFR:TOOLQUIP & ALLIED CODE:HSS-C08 DIA O/D:22MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/08/31",5,"EA"]
["0243568","BIT TOOL:CRANKED KNIFE","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED KNIFE TOOL B MFR:TOOLQUIP & ALLIED CODE:IS06-20X20LH K20 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/08/31",5,"EA"]
["0243569","CUTTER END MILL:28 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV THREE FLUTE SLOT DRILL MFR:TOOLQUIP & ALLIED CODE:HSS-C08 DIA O/D:28MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/08/31",5,"EA"]
["0243570","BIT TOOL:PARTING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV PARTING TOOL BLADE MFR:TOOLQUIP & ALLIED CODE:SGIH 19-2 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/08/31",50,"EA"]
["0243571","BIT TOOL:PARTING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV; BIT, TOOL: MNF: TOOLQUIP;  TYPE: PARTING; DIMEN:: WD 3.2 X LG 150 X HT 32 MM; MAT: ISCAR; P/N: ALLIED CODE: SGIH 32- 4;  FUNCT .LOC: NON PLANT; END DETAIL DESCRIPTION: JNF 2009/08/31; YA 2024/01/05",50,"EA"]
["0243610","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:DNMG 150404-GMNC 3020 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/09/01",120,"EA"]
["0243611","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:SP400NCM325 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/09/01",600,"EA"]
["0243612","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:SP200NCM325 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/09/01",600,"EA"]
["0243613","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:TPCN 1603-PPR ST30A FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/09/01",70,"EA"]
["0243614","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:TNMG 160408-HMNC 3020 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/09/01",70,"EA"]
["0243615","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:KNUX 160405-R11NC 3020 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/09/01",320,"EA"]
["0243616","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:TPCN 2204 PDR ST30A FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/09/01",270,"EA"]
["0243618","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:DNMG 150408-GMNC 3020 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/09/01",70,"EA"]
["0243619","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:SP300NCM325 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/09/01",220,"EA"]
["0243620","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:TPMR 110304-FNC 3020 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/09/01",410,"EA"]
["0243650","BIT TOOL:PARTING, RH;SQ 20 MM;STL P25","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV PARTING TOOL H MFR:TOOLQUIP & ALLIED STOCK CODE:H6RP25 DESIGNATION:IS07 SHANK HEIGHT:20MM  SHANK WIDTH:20MM DIRECTION:RH GRADE:P25 TO CUT:STEEL FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/09/02",30,"EA"]
["0243651","BIT TOOL:CRANKED TURNING, LH;SQ 16 MM","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV 45¿ APPROACH CRANKED TURNING TOOL J MFR:TOOLQUIP & ALLIED STOCK CODE:J5LP25 DESIGNATION:IS02 SHANK HEIGHT:16MM  SHANK WIDTH:16MM DIRECTION:LH GRADE:P25 TO CUT:STEEL FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/09/02",5,"EA"]
["0243652","BIT TOOL:STRAIGHT RD NOSE ROUGHING;SQ 16","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV STRAIGHT ROUND NOSE ROUGHING TOOL C MFR:TOOLQUIP & ALLIED STOCK CODE:C5P25 SHANK HEIGHT:16MM SHANK WIDTH:16MM DIRECTION:NEUTRAL GRADE:P25 TO CUT:STEEL FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/09/02",2,"EA"]
["0243655","BAR BORING TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL BORING BAR P MFR:TOOLQUIP & ALLIED STOCK CODE:P3RP25 DESIGNATION:IS09 SHANK HEIGHT:10MM  SHANK WIDTH:10MM DIRECTION:RH GRADE:P25 TO CUT:STEEL FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** JNF 2009/09/02",2,"EA"]
["0244262","INSERT THRDG:INTERNAL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL THREADING INSERTS MFR:TOOLQUIP & ALLIED CODE:16IR AG60 MXC FUNCT.LOC:(NON PLANT) ***** END DETAIL DESCRIPTION ***** JNF 2009/10/01",30,"EA"]
["0244266","INSERT THRDG:INTERNAL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL THREADING INSERTS MFR:TOOLQUIP & ALLIED CODE:22 IR N 60 BMA FUNCT.LOC:(NON PLANT) ***** END DETAIL DESCRIPTION ***** JNF 2009/10/01",2,"EA"]
["0244267","INSERT THRDG:EXTERNAL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV EXTERNAL THREADING INSERTS MFR:TOOLQUIP & ALLIED CODE:16 ER AG 60 MXC FUNCT.LOC:(NON PLANT) ***** END DETAIL DESCRIPTION ***** JNF 2009/10/01",90,"EA"]
["0244268","INSERT THRDG:EXTERNAL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV EXTERNAL THREADING INSERTS MFR:TOOLQUIP & ALLIED CODE:22 ER N 60 MXC FUNCT.LOC:(NON PLANT) ***** END DETAIL DESCRIPTION ***** JNF 2009/10/01",30,"EA"]
["0244269","BIT TOOL:INTERNAL THREADING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL THREADING TOOL MFR:TOOLQUIP & ALLIED CODE:16 IR AG 55 MXC FUNCT.LOC:(NON PLANT) ***** END DETAIL DESCRIPTION ***** JNF 2009/10/01",2,"EA"]
["0244270","BIT TOOL:INTERNAL THREADING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL THREADING TOOL MFR:TOOLQUIP & ALLIED CODE:22 IR N 55 MXC FUNCT.LOC:(NON PLANT) ***** END DETAIL DESCRIPTION ***** JNF 2009/10/01",2,"EA"]
["0244271","BIT TOOL:EXTERNAL THREADING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV EXTERNAL THREADED TOOL MFR:TOOLQUIP & ALLIED CODE:16 ER AG 55 MXC FUNCT.LOC:(NON PLANT) ***** END DETAIL DESCRIPTION ***** JNF 2009/10/01",2,"EA"]
["0244272","BIT TOOL:EXTERNAL THREADING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV EXTERNAL THREADED TOOL MFR:TOOLQUIP & ALLIED CODE:22 ER N 55 MXC FUNCT.LOC:(NON PLANT) ***** END DETAIL DESCRIPTION ***** JNF 2009/10/01",2,"EA"]
["0249855","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:SNMG 120404-HFNC 3020 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",70,"EA"]
["0249857","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:CNMG 190612-B25NC330 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",70,"EA"]
["0249858","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:CNMG 120404-HANC9020 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",120,"EA"]
["0249859","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:HDCMT070204-HMP NC3020 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",320,"EA"]
["0249869","INSERT CUTNG TL","C.O.C;0040/88Q;Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP AND ALLIED; P/NO:VNMG 12T304 NF; FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",120,"EA"]
["0249870","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:CCMT060204-HMPNC3020 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",70,"EA"]
["0249871","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:TNMG 160404-HMNC3020 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",110,"EA"]
["0249872","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:16IR AG60 MXC FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",60,"EA"]
["0249873","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:16IR BAG60 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",50,"EA"]
["0249874","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:16IRB AG60BMA FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",50,"EA"]
["0249875","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:22IR N60BMA FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",70,"EA"]
["0249876","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:22ER N60MXC FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",70,"EA"]
["0249877","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:CNMG 160608-B25NC330 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",50,"EA"]
["0249878","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:TPMR 160308-PG FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",700,"EA"]
["0249879","INSERT CUTNG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CUTTING TOOL INSERT MFR:TOOLQUIP & ALLIED CODE:KNUX160405-L11NC3015 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/05",100,"EA"]
["0249881","BIT TOOL:CRANKED TURNING;SQ 10 MM","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED TURNING TOOL MFR:TOOLQUIP & ALLIED CODE:ISO2-10X10 LHP 25 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/06",20,"EA"]
["0249882","BIT TOOL:CRANKED TURNING;SQ 20","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED TURNING TOOL MFR:TOOLQUIP & ALLIED CODE:ISO2-20X20 RH K20 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/06",10,"EA"]
["0249883","BIT TOOL:CRANKED TURNING;SQ 20","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED TURNING TOOL MFR:TOOLQUIP & ALLIED CODE:ISO2-20X20 LH K20 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/06",10,"EA"]
["0249884","BIT TOOL:CRANKED TURNING;SQ 10 MM","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED TURNING TOOL MFR:TOOLQUIP & ALLIED CODE:ISO2-10X10 RH P25 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/06",25,"EA"]
["0249885","BIT TOOL:CRANKED TURNING;SQ 25 MM","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED TURNING TOOL MFR:TOOLQUIP & ALLIED CODE:ISO2-25X25 RH P25 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/06",10,"EA"]
["0249886","BIT TOOL:CRANKED TURNING;SQ 25 MM","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED TURNING TOOL MFR:TOOLQUIP & ALLIED CODE:ISO2-25X25 LH P25 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/06",10,"EA"]
["0249887","BIT TOOL:CRANKED TURNING;SQ 20","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED TURNING TOOL MFR:TOOLQUIP & ALLIED CODE:ISO2-20X20 RH P25 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",15,"EA"]
["0249888","BIT TOOL:CRANKED TURNING;SQ 20","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED TURNING TOOL MFR:TOOLQUIP & ALLIED CODE:ISO2-20X20 LH P25 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",10,"EA"]
["0249889","BIT TOOL:CRANKED TURNING;SQ 16","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED TURNING TOOL MFR:TOOLQUIP & ALLIED CODE:ISO2-16X16 RH P25 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",25,"EA"]
["0249890","BIT TOOL:CRANKED TURNING;SQ 12 MM","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED TURNING TOOL MFR:TOOLQUIP & ALLIED CODE:ISO2-12X12 RH P2 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/06",15,"EA"]
["0249891","BIT TOOL:CRANKED TURNING;SQ 16","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED TURNING TOOL MFR:TOOLQUIP & ALLIED CODE:ISO2-16X16 LH K20 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",15,"EA"]
["0249892","BIT TOOL:CRANKED TURNING;SQ 16","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED TURNING TOOL MFR:TOOLQUIP & ALLIED CODE:ISO2-16X16 LH K20 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",10,"EA"]
["0249893","BIT TOOL:CRANKED TURNING;SQ 12 MM","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED TURNING TOOL MFR:TOOLQUIP & ALLIED CODE:ISO2-12X12 LH P25 FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",10,"EA"]
["0249905","CUTTER END MILL:2 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV DRILL THREE FLUTE SLOT MFR:TOOLQUIP & ALLIED CODE:HSS-C08 2MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",30,"EA"]
["0249908","CUTTER END MILL:3 MM;SLOT;3;HSS","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV DRILL THREE FLUTE SLOT MFR:TOOLQUIP & ALLIED CODE:HSS-C08 3MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",35,"EA"]
["0249912","CUTTER END MILL:4 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV DRILL THREE FLUTE SLOT MFR:TOOLQUIP & ALLIED CODE:HSS-C08 4MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",35,"EA"]
["0249925","CUTTER END MILL:5 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV DRILL THREE FLUTE SLOT MFR:TOOLQUIP & ALLIED CODE:HSS-C08 5MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",35,"EA"]
["0249926","CUTTER END MILL:6 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV DRILL THREE FLUTE SLOT MFR:TOOLQUIP & ALLIED CODE:HSS-C08 6MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",35,"EA"]
["0249927","CUTTER END MILL:8 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV DRILL THREE FLUTE SLOT MFR:TOOLQUIP & ALLIED CODE:HSS-C08 8MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",35,"EA"]
["0249928","CUTTER END MILL:14 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV DRILL THREE FLUTE SLOT MFR:TOOLQUIP & ALLIED CODE:HSS-C08 14MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",10,"EA"]
["0249929","CUTTER END MILL:20 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV DRILL THREE FLUTE SLOT MFR:TOOLQUIP & ALLIED CODE:HSS-C08 20MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",10,"EA"]
["0249930","CUTTER END MILL:24 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV DRILL THREE FLUTE SLOT MFR:TOOLQUIP & ALLIED CODE:HSS-C08 24MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",15,"EA"]
["0249932","CUTTER END MILL:25 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV DRILL THREE FLUTE SLOT MFR:TOOLQUIP & ALLIED CODE:HSS-C08 25MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",15,"EA"]
["0249933","CUTTER END MILL:26 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV DRILL THREE FLUTE SLOT MFR:TOOLQUIP & ALLIED CODE:HSS-C08 26MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",15,"EA"]
["0249938","CUTTER END MILL:30 MM;3 FLUTE SLOT DRILL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV DRILL THREE FLUTE SLOT MFR:TOOLQUIP & ALLIED CODE:HSS-C08 30MM FUNCT.LOC:NON PLANT ***** END DETAIL DESCRIPTION ***** ET 2010/07/07",15,"EA"]
["0249961","BIT TOOL:CRANKED KNIFE","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED KNIFE TOOL B MFR:TOOLQUIP & ALLIED CODE:ISO 6-20 X 20 LH P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/19",10,"EA"]
["0249962","BIT TOOL:CRANKED KNIFE","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED KNIFE TOOL B MFR:TOOLQUIP & ALLIED CODE:ISO 6-20 X 20 RH P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/19",15,"EA"]
["0249963","BIT TOOL:CRANKED KNIFE","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED KNIFE TOOL B MFR:TOOLQUIP & ALLIED CODE:ISO 6-16 X 16 LH P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/19",10,"EA"]
["0249965","BIT TOOL:CRANKED KNIFE","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED KNIFE TOOL B MFR:TOOLQUIP & ALLIED CODE:ISO 6-16 X 16 RH P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/19",10,"EA"]
["0249967","BIT TOOL:CRANKED KNIFE","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED KNIFE TOOL B MFR:TOOLQUIP & ALLIED CODE:ISO 6-20 X 20 RH P20 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/19",10,"EA"]
["0249968","BIT TOOL:CRANKED KNIFE","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED KNIFE TOOL B MFR:TOOLQUIP & ALLIED CODE:ISO 6-16 X 16 RH K20 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/19",10,"EA"]
["0249969","BIT TOOL:CRANKED KNIFE","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV CRANKED KNIFE TOOL B MFR:TOOLQUIP &ALLIED CODE:ISO6-16 X 16 LH K20 FUNCT.LOC:CONSUMABLES **** END DETAIL DESCRIPTION ***** ET 2010/07/19",10,"EA"]
["0249971","BAR BORING TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL BORING BAR MFR:TOOLQUIP & ALLIED CODE:ISO9-12 X 12 P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/19",2,"EA"]
["0249972","BAR BORING TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL BORING BAR MFR:TOOLQUIP & ALLIED CODE:ISO9-16 X 16 P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/19",2,"EA"]
["0249973","BAR BORING TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL BORING BAR MFR:TOOLQUIP & ALLIED CODE:ISO9-10 X 10 K20 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/19",2,"EA"]
["0249974","BAR BORING TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL BORING BAR MFR:TOOLQUIP & ALLIED CODE:ISO9-16 X 16 K20 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/19",2,"EA"]
["0249975","BAR BORING TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL BORING BAR MFR:TOOLQUIP & ALLIED CODE:ISO9-25 X 25 K20 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/20",2,"EA"]
["0249981","BAR BORING TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL BORING BAR MFR:TOOLQUIP & ALLIED CODE:ISO9-25 X 25 P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/20",2,"EA"]
["0249982","BAR BORING TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL BORING BAR MFR:TOOLQUIP & ALLIED CODE:ISO9-20 X 20 P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/20",2,"EA"]
["0249986","BIT TOOL:INTERNAL THREADING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL THREADING TOOL K1 MFR:TOOLQUIP & ALLIED CODE:ISO14-16X16 RH 55¿ P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/20",15,"EA"]
["0249987","BIT TOOL:INTERNAL THREADING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL THREADING TOOL K1 MFR:TOOLQUIP & ALLIED CODE:ISO14-16X16 RH 60¿ P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/20",10,"EA"]
["0250009","BIT TOOL:INTERNAL THREADING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL THREADING TOOL K1 MFR:TOOLQUIP & ALLIED CODE:ISO14-20X20 RH 55¿ P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/20",15,"EA"]
["0250010","BIT TOOL:INTERNAL THREADING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL THREADING TOOL K1 MFR:TOOLQUIP & ALLIED CODE:ISO14-20X20 RH 60¿ P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/20",15,"EA"]
["0250062","BIT TOOL:INTERNAL THREADING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL THREADING TOOL K MFR:TOOLQUIP & ALLIED CODE:ISO13-20X22 RH 60¿ P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/20",15,"EA"]
["0250063","BIT TOOL:INTERNAL THREADING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL THREADING TOOL K MFR:TOOLQUIP & ALLIED CODE:ISO13-25X16 RH 55¿ P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/20",15,"EA"]
["0250064","BIT TOOL:INTERNAL THREADING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL THREADING TOOL K MFR:TOOLQUIP & ALLIED CODE:ISO13-25X16 RH 60¿ P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/20",10,"EA"]
["0250067","BIT TOOL:INTERNAL THREADING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV INTERNAL THREADING TOOL K MFR:TOOLQUIP & ALLIED CODE:ISO13-20X12 RH 55¿ P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/20",10,"EA"]
["0250072","BIT TOOL:STRAIGHT RD NOSE;SQ 10 MM","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV STRAIGHT ROUND NOSE TOOL C MFR:TOOLQUIP & ALLIED CODE:10 X 10 NEUTRAL P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/21",2,"EA"]
["0250074","BIT TOOL:STRAIGHT RD NOSE;SQ 25 MM","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV STRAIGHT ROUND NOSE TOOL MFR:TOOLQUIP & ALLIED CODE:25 X 25 NEUTRAL P25 FUNCT.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/21",5,"EA"]
["0250085","BIT TOOL:PARTING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV PARTING TOOL MFR:TOOLQUIP & ALLIED CODE:ISO7-16 X 16 P25 FUNTC.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/21",25,"EA"]
["0250087","BIT TOOL:PARTING","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV PARTING TOOL H MFR:TOOLQUIP & ALLIED CODE:ISO7-12 X 12 P25 FUNTC.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/21",30,"EA"]
["0250089","HOLDER MACHG TL","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV PARTING TOOL HOLDER MFR:TOOLQUIP & ALLIED CODE:SG TBN 16-2 FUNTC.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/21",5,"EA"]
["0250091","BIT TOOL:RH;TIP TUNGSTEN","C.O.C\\0040/88Q\\Q4:NSF:NC:NEV TUNGSTEN TIP TOOL MFR:TOOLQUIP & ALLIED CODE:ISO2R 25X25 P25 R/HAND FUNTC.LOC:CONSUMABLES ***** END DETAIL DESCRIPTION ***** ET 2010/07/21",25,"EA"]
["0403206","TESTER:TELEPHONE BLEEP SET;MK1","TESTER: TYPE: TELEPHONE BLEEP SET; REFERENCE NO: MK1; WITH BUILT IN SPEAKER;TONE EMITTER TONE EMITTER WHEN LINE IS BEING TESTED",5,"EA"]
["0513601","SAW HND:HACKSAW","SAW, HAND: DESIGN TYPE: HACKSAW",5,"EA"]
["0518355","GRINDER ELEC:ANGLE","GRINDER, ELECTRIC: TYPE: ANGLE",10,"EA"]
["0521344","SAW PWR:CIRCULAR","SAW, POWER: TYPE: CIRCULAR; SMALL",5,"EA"]
["0545129","BIT TWST:3.5 MM;STRAIGHT;HSS;LG 70 MM","BIT, TWIST: DIAMETER: 3.5 MM; SHANK: STRAIGHT; MATERIAL: HSS; LENGTH: 70 MM; TYPE: JOBBER DRILL",100,"EA"]
["0545302","BIT TWST:4.5 MM;STRAIGHT;HSS;LG 76 MM","BIT, TWIST: DIAMETER: 4.5 MM; SHANK: STRAIGHT; MATERIAL: HSS; LENGTH: 76 MM; TYPE: JOBBER DRILL",100,"EA"]
["0546107","BIT TWST:5.5 MM;STRAIGHT;HSS;LG 93 MM","BIT, TWIST: DIAMETER: 5.5 MM; SHANK: STRAIGHT; MATERIAL: HSS; LENGTH: 93 MM; TYPE: JOBBER DRILL",100,"EA"]
["0547094","BIT TWST:5 MM;STRAIGHT;HSS;LG 86 MM","BIT, TWIST: DIAMETER: 5 MM; SHANK: STRAIGHT; MATERIAL: HSS; LENGTH: 86 MM; TYPE: JOBBER DRILL",100,"EA"]
["0548902","BIT TWST:4 MM;STRAIGHT;HSS;LG 75 MM","BIT, TWIST: DIAMETER: 4 MM; SHANK: STRAIGHT; MATERIAL: HSS; LENGTH: 75 MM; TYPE: JOBBER DRILL",100,"EA"]
["0548904","BIT TWST:6.5 MM;STRAIGHT;HSS;LG 101 MM","BIT, TWIST: DIAMETER: 6.5 MM; SHANK: STRAIGHT; MATERIAL: HSS; LENGTH: 101 MM; TYPE: JOBBER DRILL",100,"EA"]
["0569847","ASSY:DOLPHIN WAVE 100 CB;POOL CLEANER","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; ASSEMBLY; MNF: BLSA; P/NO: 100 CB; TYPE: DOLPHIN WAVE 100 CB; APPLICATION: POOL CLEANER; (REACTOR CAVITY; CADDY); FUNCT.LOC:6HAI ***** END DETAIL DESCRIPTION *****; JNF 2013/05/30; JNF 2013/06/10; JNF 2015/07/02; ML 2020/06/02",6,"EA"]
["0570614","BLADE SAW:BAND;RAKE;6-10","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; BLADE FOR AUTOMATIC HEAVY DUTY BANDSAW; SUPPLIER:TOOLQUIP & ALLIED; CODE:BMBSB34X6-10S; SAW TYPE:BAND SAW; TEETH PER INCH:6-10; TOOTH DESIGN:RAKE; FUNCT.LOC:NON STOCK; ***** END DETAIL DESCRIPTION *****; JNF 2013/06/24",10,"EA"]
["0570774","TOOL:CUTTING;LATHE;16 X 16 MM","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; PARTING TOOL (CAST IRON); MNF:TOOLQUIP & ALLIED; CODE:H5RK20; TYPE:CUTTING TOOL; DIMEN:16 X 16 MM; STYLE:LATHE; FUNCT.LOC:NON PLANT; ***** END DETAIL DESCRIPTION *****; JNF 2013/06/26; ML 2020/08/25",15,"EA"]
["0570796","TOOL:CUTTING;LATHE;25 X 25 MM","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; PARTING TOOL (CAST IRON); SUPPLIER:TOOLQUIP & ALLIED; CODE:H5RP25; TYPE:CUTTING TOOL; MATLNO:KEY STEEL; DIMEN:25MM X 25MM; STYLE:LATHE; FUNCT.LOC:NON PLANT; ***** END DETAIL DESCRIPTION *****; JNF 2013/06/26",20,"EA"]
["0570823","TOOL:CUTTING;LATHE;20 X 20 MM","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; PARTING TOOL (CAST IRON); SUPPLIER:TOOLQUIP & ALLIED; CODE:H6RK20; TYPE:CUTTING TOOL; DIMEN:20MM X 20MM; STYLE:LATHE; FUNCT.LOC:WORKSHOP; ***** END DETAIL DESCRIPTION *****; JNF 2013/06/27",20,"EA"]
["0602758","INSERT:MILLING;DIA 4.1 MM;GR 2030","C.O.C; 0040/88Q; Q4:NSF:NC:NEV; MILLING INSERT; MFR:SANDVIK; CODE:R390-17 04 08M-MM; TYPE: MILLING; DIMENSIONS: DIA 4.1 MM; MATERIAL: GRADE 2030; FUNCT.LOC:CONSUMABLE; ***** END DETAIL DESCRIPTION *****; JNF 2015/05/21",150,"EA"]
["0616414","BLADE:ANGLE PLOUGH KIT;LG 150 MM","BLADE: TYPE: ANGLE PLOUGH KIT; DIMENSIONS: LG 150 MM; MATERIAL: POLYURATHANE; SPECIAL FEATURES: BOLT KIT; SUPPL P/N: 2/5/1500; DRAWING NO: E505-011-A REV 0; USED ON OC1/2; EC1/2 SC1/2 ASH CONVEYORS; REPLACEMENT BLADE SET TO FIT BRELKO E505; BELT WIDTH: 1500M",5,"EA"]
["0665581","INSERT FLEX CPLG:BLOCK;EPDM","C.O.C; 0052/93Q; Q4:NSF:NC:NEV; (OLD MATERIAL NO: 0043125); INSERT, FLEXIBLE COUPLING: MNF: CREPELLE & CO; TYPE: BLOCK; SIZE: WD 24 X LG 42 X THK 18 MM; MATERIAL: EPDM; KBA: 1214B02009; KBA1214B001001; ITM: FM1923011; M/MAN:002/1; ASMT: 1966; FUNC LOC: 1/2 SAP 101, 102 CO ***** END DETAIL DESCRIPTION ***** ML 2019/05/13; ML 2019/05/27; ML 2020/04/30",10,"EA"]
["0701453","BIT:JOBBER DRILL;LG 103 MM;SOLID CARBIDE","C.O.C; 0040/88Q; Q4:NSF:NC:NEV:L3; BIT; MNF: SOMTA; TYPE: JOBBER DRILL; LENGTH: 103 MM; MATERIAL: SOLID CARBIDE; DIAMETER: 10 MM; FUNC LOC: 6 HSM 000 BG ***** END DETAIL DESCRIPTION ***** ML 2021/08/31",5,"EA"]
["0701454","BIT:JOBBER DRILL;LG 118 MM;SOLID CARBIDE","C.O.C; 0040/88Q; Q4:NSF:NC:NEV:L3; BIT; MNF: SOMTA; TYPE: JOBBER DRILL; LENGTH: 118 MM; MATERIAL: SOLID CARBIDE; DIAMETER: 10.5 MM; FUNC LOC: 6 HSM 000 BG ***** END DETAIL DESCRIPTION ***** ML 2021/08/31",5,"EA"]
["0701455","BIT:JOBBER DRILL;LG 103 MM;SOLID CARBIDE","C.O.C; 0040/88Q; Q4:NSF:NC:NEV:L3; BIT; MNF: SOMTA; TYPE: JOBBER DRILL; LENGTH: 103 MM; MATERIAL: SOLID CARBIDE; DIAMETER: 8.50 MM; FUNC LOC: 6 HSM 000 BG ***** END DETAIL DESCRIPTION ***** ML 2021/08/31",5,"EA"]
["0701456","BIT:JOBBER DRILL;LG 91 MM;SOLID CARBIDE","C.O.C; 0040/88Q; Q4:NSF:BC:NEV:L3; BIT; MNF:SOMTA; TYPE: JOBBER DRILL; LENGTH: 91 MM; MATERIAL: SOLID CARBIDE; DIAMETER: 8 MM; FUNC LOC: 6 HSM 000 BG ***** END DETAIL DESCRIPTION ***** ML 2021/08/31",5,"EA"]
["0701457","BIT:JOBBER DRILL;LG 91 MM;SOLID CARBIDE","C.O.C; 0040/88Q; Q4:NSF:NC:NEV:L3; BIT; MNF:SOMTA; TYPE: JOBBER DRILL; LENGTH: 91 MM; MATERIAL: SOLID CARBIDE; DIAMETER: 6.50 MM; FUNC LOC: 6 HSM 000 BG ***** END DETAIL DESCRIPTION ***** ML 2021/08/31",5,"EA"]
["0701473","BIT:JOBBER DRILL;LG 82 MM;SOLID CARBIDE","C.O.C; 004/88Q; Q4:NSF:NC:NEV:L3; BIT; MNF:SOMTA; TYPE: JOBBER DRILL; LENGTH: 82 MM; MATERIAL: SOLID:CARBIDE; DIAMETER: 6 MM; FUNC LOC: 6 HSM 000 BG ***** END DETAIL DESCRIPTION ***** ML 2021/08/31 LOC: 6 HSM 000 BG ***** END DETAIL DESCRIPTION ***** ML 2021/08/31LOC:  6  HSM  000  BG  *****  END  DETAIL  DESCRIPTION  *****",5,"EA"]
["0701474","BIT:JOBBER DRILL;LG 82 MM;SOLID CARBIDE","C.O.C; 0040/88Q; Q4:NSF:NC:NEV:L3; BIT; MNF:SOMTA; TYPE: JOBBER DRILL; LENGTH: 82 MM; MATERIAL: SOLID CARBIDE; DIAMETER: 5 MM; FUNC LOC: 6 HSM 000 BG ***** END DETAIL DESCRIPTION ***** ML 2021/09/01",5,"EA"]
["0701475","BIT:JOBBER DRILL;LG 74 MM;SOLID CARBIDE","C.O.C; 0040/88Q;Q4:NSF:NC:NEV:L3; BIT; MNF: SOMTA;  TYPE: JOBBER DRILL; LENGTH: 74 MM; MATERIAL: SOLID CARBIDE; DIAMETER: 4 MM; FUNC LOC: 6 HSM 000 BG ***** END DETAIL DESCRIPTION ***** ML 2021/09/01",5,"EA"]
["0701476","BIT:JOBBER DRILL;LG 66 MM;SOLID CARBIDE","C.O.C; 0040/88Q; Q4:NSF:NC:NEV:L3; BIT; MNF: SOMTA; TYPE: JOBBER DRILL; LENGTH: 66 MM; MATERIAL: SOLID CARBIDE; DIAMETER: 3.50 MM; FUNC LOC: 6 HSM 000 BG ***** END DETAIL DESCRIPTION ***** ML 2021/09/01",5,"EA"]
["0701477","BIT:JOBBER DRILL;LG 66 MM;SOLID CARBIDE","C.O.C; 0040/88Q; Q4:NSF:NC:NEV:L3; BIT; MNF:SOMTA; TYPE: JOBBER DRILL; LENGTH: 66 MM; MATERIAL: SOLID CARBIDE; DIAMETER: 3 MM; FUNC LOC: 6 HSM 000 BG ***** END DETAIL DESCRIPTION ***** ML 2021/09/01",5,"EA"]
["0701538","BIT:JOBBER DRILL;LG 57 MM;SOLID CARBIDE","C.O.C; 0040/88Q; Q4:NSF:NC:NEV:L3; BIT; MNF:SOMTA; TYPE: JOBBER DRILL; LENGTH: 57 MM; MATERIAL: SOLID CARBIDE; DIAMETER: 2.50 MM; FUNC LOC: 6 HSM 000 BG ***** END DETAIL DESCRIPTION ***** ML 2021/09/01",5,"EA"]
["STM-053319","SCREWDRIVER SET:CHROME VANADIUM;4","SCREWDRIVER, SET: TYPE: DUAL GRIP - GENERAL PURPOSE; TIP TYPES: PHILLIPS AND SLOT MAGNETIC; TIP MATERIAL: CHROME VANADIUM; TIP SIZE RANGE: NO. 2, 3, 5, 8; HANDLE MATERIAL: RUBBER GRIP; QUANTITY: 4; LENGTH 75-200 MM, SHANK: ROUND, SHANK LENGTH: 5 MM, CODE: SEN-572-9100K; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5]
["STM-059627","KEY:ALLEN KEY CHROME VANADIUM;BALL HEAD","ALLEN KEY SET - BALL POINT - LONG - 9 PIECE\nKEY: TYPE: ALLEN KEY CHROME VANADIUM; STYLE: BALL HEAD; MATERIAL: CHROME VANADIUM; SPECIFICATION: 1.5-10 MM; ALLEN KEY BALL HEAD LONG SERIES SET 1.5-10MM; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5]
["STM-059629","PLIERS:COBINATION;LG 200 MM;INSULATED","PLIERS - COMBINATION - 200MM LONG - INSULATED\nMAKE: GEDORE; PLIERS: TYPE: COBINATION; LENGTH: 200 MM; HANDLE: INSULATED; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5]
[79394,"WRENCH ADJSTBL:56 MM;LG 450 MM","WRENCH, ADJUSTABLE: JAW CAPACITY: 56 MM; LENGTH: 450 MM; MATERIAL: STL DROP FORGED; SHIFTING SPANNER, HARDENED KNURLS",10,"EA"]
[80126,"TAP SET THRD CUT:M8;1 MM;HSS;3","TAP SET, THREAD CUTTING: TAP SIZE: M8; THREAD: 1 MM; MATERIAL: HSS; QUANTITY: 3; TYPE: TAPER; SECOND; BOTTOM; HAND",50,"EA"]
[206641,"CALLIPER VRNR:0-150 MM","CALLIPER, VERNIER: RANGE: 0-150 MM",50,"EA"]
[206816,"CALLIPER VRNR:STORM;0-300 MM","CALLIPER, VERNIER: TYPE: STORM; RANGE:0-300 MM\nMAKE: MITUTOYO",20,"EA"]
[701318,"CALLIPER VRNR:DIGITAL;0-150 MM;0.005 MM","MITOTOYO 150MM VERNIER CALIPER - PRODUCT CODE:MIT531-101;\nREQUIRED FOR A MECHNICAL FITTER.",10,"EA"]
[703849,"BIT TWST:3 MM;STRAIGHT;LG 61 MM;N","BIT, TWIST: DIAMETER: 3 MM; SHANK: STRAIGHT; MATERIAL: HSS; LIGHT INDUSTRIAL STEEL; LENGTH: 61 MM; TYPE: N; TIP: DRILLING",100,"EA"]
[708093,"CUTTER CABL:COPPER & ALUMINIUM;60 MM2","CUTTER, CABLE: TYPE: COPPER & ALUMINIUM; CABLE SIZE ACCOMMODATED: 60 MM2; COMMERCIAL SIZE: 60 MM2; HANDLE MATERIAL: PLASTIC",10,"EA"]
["STM-012655","CUTTER BLT:AXIAL;450 MM;STEEL;11","GEDORE BOLT CUTTER 460MM - PRODUCT CODE:GED2675137. VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-014754","BOX TOOL:TOOLBOX","KENNEDY 62 PIECE CANTILEVER TOOLBOX TOOLSET - PRODUCT CODE:KEN5950055K. VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-014961","HANDLE, SPANNER WRENCH:BA","HANDLE, SPANNER RACHET: SETS OF RACHET SPANNERS",10,"EA"]
["STM-014965","PLIERS:LONG NOSE;LG 150 MM;INSULATED;STL","PLIERS: TYPE: LONG NOSE; LENGTH: 150 MM; HANDLE: INSULATED; MATERIAL: STL; LONGNOSE PLIERS 150MM; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-017517","PUNCH:DRIVE PIN PUNCHES;3-9.5 MM","PUNCH: TYPE: DRIVE PIN PUNCHES; POINT SIZE: 3-9.5 MM; LENGTH: 200 MM; MATERIAL: METAL/STL; STARRETT 5 PIECE",5,"EA"]
["STM-017548","TAPE MEASNG:RUBBER CASE;5 M;STEEL","TAPE, MEASURING: TYPE:DIMENSIONS: 5 M; POWERLOCK TAPE MEAUSURE",10,"EA"]
["STM-018139","WRENCH CMBTN:SPANNER,;10 MM;LG 140 MM","GEDORE 10MM COMBINATION SPANNERS - PRODUCT CODE: GED600083. WRENCH, COMBINATION: TYPE: SPANNER,; SIZE: 10 MM; LENGTH: 140 MM; STYLE: FLAT; RING; MATERIAL: CR VANADIUM STL; 10MM RING AND FLAT SPANNER GEDORE. VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-024130","DRILL PWR:ROTARY HAMMER DRILL;ELECTRICAL","HILTI TE 6-A36 AVR ROTARY HAMMER DRILLS PERFORMANCE PACKAGE WITH BATTERY. DRILL, POWER: TYPE: ROTARY HAMMER DRILL; CORDLESS HILTI TE 6-A36 AVR ROTARY HAMMER DRILL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-025038","DRILL PWR:ROTARY HAMMER DRILL;230V","HILTI ROTARY HAMMER PERFORMANCE PACKAGE - CODE:03497788; DRILL, POWER: TYPE: ROTARY HAMMER DRILL; SPEED: APPROPRIATE; DRIVE SIZE: APPROPRIATE; CHUCK SIZE: APPROPRIATE; POWER: ELECTRICAL; POTENTIAL: 230V; POWER SOURCE: ELECTRICAL; FEATURE: HILTI; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-025094","TOOL:FLARING TOOL;FLARING TOOL","TOOL: TYPE: FLARING TOOL; STYLE: FLARING TOOL; DIMENSIONS: FLARING TOOL MM; SPECIFICATION: FLARING TOOL; FLARING TOOL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-025530","LADDER:STEP;LG 3M;ALUMINIUM;115KG","LADDER: TYPE: STEP; LENGTH: 3M; MATERIAL: ALUMINIUM; LOAD CAPACITY: 115KG; CROSSPIECE TYPE: AL AND RUBBER UV RESISTANT; CROSSPIECE SURFACE TYPE: AL AND RUBBER NON SLIP; SAFETY FEET: YES RUBBER; SAFETY FEET TYPE: NON-SLIP; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-026418","CRIMPER:MODULAR PLUGS;HAND CRIMPING","CRIMPER: TYPE: MODULAR PLUGS; CRIMPING RANGE: RJ11/12 (9.65MM) AND RJ45(11.68MM); JAW TYPE: HAND CRIMPING; DESIGN TYPE: THREE CRIMP CAVITIES FOR 4, 6 & 8 POSITION MODULAR PLUGS; SPECIFICATION: L=190MM; FURNISHED ITEMS: BUILT IN CUTTER AND STRIPPER.; MULTI-PURP OSE FUNCTIONS TOOL FOR TELECOM/NETWORK INSTALLERS WORKING WITH RJ11, RJ12 MODULAR PLUGS; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",10,"EA"]
["STM-028125","CALLIPER VRNR:0-200","CALLIPER, VERNIER: TYPE: DIGITAL VERNIER CALIPER MEASURING; RANGE: 0-200; DIGITAL VERNIER CALIPER MEASURING 200MM,\nWITH MM & INCH  READINGS. GROUND TIPS. IN STURDY PLASTIC CASE INCLUDING SPARE BATTERY.; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-030504","FRAME HAND HCKSW:HACKSAW LARGE","ECLIPSE HACKSAW FLAT FRAME 300MM LONG - PRODUCT CODE:ECP4150. VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",10,"EA"]
["STM-030509","CUTTER:STRAIGHT CUT TIN SNIPS","CUTTER: TYPE: STRAIGHT CUT TIN SNIPS",10,"EA"]
["STM-040481","DRILL PWR:AUTOMATIC LOCK;1100 RPM;13 MM","BOSCH CORDLESS PROFESSIONAL GSB 18-2LI PLUS DRILLING MACHINES COMPLETE WITH CARRY CASE,4/5Ah BATTERY & BATTERY CHARGER FOR EACH CORDLESS DRIILLING MACHINE. CHUCK SIZE: 13 MM; POWER: VARIOUS; POTENTIAL: 18 VDC; POWER SOURCE: BATTERY; FEATURE: VARIABLE SPEED; CORDLESS PROFESSIONAL GSB 18-2LI PLUS. VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-053319","SCREWDRIVER SET:CHROME VANADIUM;4","SCREWDRIVER, SET: TYPE: DUAL GRIP - GENERAL PURPOSE; TIP TYPES: PHILLIPS AND SLOT MAGNETIC; TIP MATERIAL: CHROME VANADIUM; TIP SIZE RANGE: NO. 2, 3, 5, 8; HANDLE MATERIAL: RUBBER GRIP; QUANTITY: 4; LENGTH 75-200 MM, SHANK: ROUND, SHANK LENGTH: 5 MM, CODE: SEN-572-9100K; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-053523","WRENCH CMBTN:COMBINATION SPANNER","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 6 AND 7MM; LENGTH: STANDARD; STYLE: BOTH OPEN ENDS; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-053524","WRENCH CMBTN:COMBINATION SPANNER","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 8 AND 9MM; LENGTH: STANDARD; STYLE: BOTH OPEN ENDS; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053525","WRENCH CMBTN:COMBINATION SPANNER","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 10 AND 11MM; LENGTH: STANDARD; STYLE: BOTH OPEN END; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053526","WRENCH CMBTN:COMBINATION SPANNER","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 12 AND 13MM; LENGTH: STANDARD; STYLE: OTH OPEN ENDS; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053527","WRENCH CMBTN:COMBINATION SPANNER","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE:  14 AND 15MM; LENGTH: STANDARD; STYLE: BOTH OPEN ENDS; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053529","WRENCH CMBTN:COMBINATION SPANNER","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 16 AND 17MM; LENGTH: STANDARD; STYLE: OTH OPEN ENDS; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053531","WRENCH CMBTN:COMBINATION SPANNER","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 20 AND 22MM; LENGTH: STANDARD; STYLE: BOTH OPEN ENDS; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053533","WRENCH CMBTN:COMBINATION SPANNER","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 18 AND 19MM; LENGTH: STANDARD; STYLE: OTH OPEN ENDS; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053534","WRENCH CMBTN:COMBINATION SPANNER","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 21 AND 23MM; LENGTH: STANDARD; STYLE: BOTH OPEN ENDS; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053536","WRENCH CMBTN:COMBINATION SPANNER","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 24 AND 26MM; LENGTH: STANDARD; STYLE: OTH OPEN ENDS; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053537","WRENCH CMBTN:COMBINATION SPANNER","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 25 AND 28MM; LENGTH: STANDARD; STYLE: TH OPEN ENDS; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053538","WRENCH CMBTN:COMBINATION SPANNER","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 27 AND 30MM; LENGTH: STANDARD; STYLE: OTH OPEN ENDS; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053540","WRENCH CMBTN:COMBINATION SPANNER","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 27 AND 32; LENGTH: STANDARD; STYLE: BOTH OPEN END; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053541","WRENCH CMBTN:COMBINATION SPANNER;9/16\"","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 9/16\"; LENGTH: STANDARD; STYLE: BOTH OPEN END; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",50,"EA"]
["STM-053542","WRENCH CMBTN:COMBINATION SPANNER;11/16\"","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 11/16\"; LENGTH: STANDARD; STYLE: BOTH OPEN ENDS; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053543","WRENCH CMBTN:COMBINATION SPANNER;5/8\"","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 5/8\"; LENGTH: STANDARD; STYLE: BOTH OPEN ENDS; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053544","WRENCH CMBTN:COMBINATION SPANNER;7/8\"","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 7/8\"; LENGTH: STANDARD; STYLE: BOTH OPEN ENDS; MATERIAL: CHROME VANADIUM STL; MAKE: GEDORE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECTDRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053563","WRENCH SET ALLN:ALLEN KEY SET;LONG ARM","WRENCH SET, ALLEN: TYPE: ALLEN KEY SET; SIZE: LONG ARM; SET QUANTITY: 25; CONTAINER: PLASTIC; RS PRO LONG ARM HEX ALLEN KEY SET 25 PIECE; METRIC & IMPERIAL",30,"EA"]
["STM-053588","PLIERS VISE GRP:VICE GRIP;40 MM;LG 25 CM","PLIERS, VISE GRIP: TYPE: VICE GRIP; CAPACITY: 40 MM; LENGTH: 25 CM; MATERIAL: STEEL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053599","PLIERS DGNL CUTNG:110MM;YES","PLIERS, DIAGONAL CUTTING: OVERALL LENGTH: 110MM; INSULATED HANDLE: YES; SIDE CUTTER; MAKE: RS PRO PART NUMBER:536420; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053603","PLIERS DGNL CUTNG:180MM;YES","PLIERS, DIAGONAL CUTTING: OVERALL LENGTH: 180MM; INSULATED HANDLE: YES; SIDE CUTTER; MANUFACTURER: RS PRO; STOCK NUMBER: 8755799; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-053674","PLIERS:WATERPUMP;LG 250 MM;INSULATED;STL","PLIERS: TYPE: WATERPUMP; LENGTH: 250MM; HANDLE: INSULATED; MATERIAL: STL; WATER PUMP PLIER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-055005","SCKT WRNCH SET:SOCKETS;CHROME VANADIUM","SOCKET, WRENCH SET: TYPE: SOCKETS; MATERIAL: CHROME VANADIUM; SIZE RANGE: 4/4.5/5/5.5/6/7/8/9/10/11/12/13 MM; SPECIAL FEATURES: 1/4 INCH DRIVE; COMPRISING: N/A; SPECIFICATION: N/A; STANDARD: N/A; 16 PIECE SOCKET SET \nMAKE:  RS PRO\nSTOCK NR:623 6413; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-055118","SCREWDRIVER SET:SCREWDRIVER SET;STEEL","SCREWDRIVER, SET: TYPE: SCREWDRIVER SET; TIP TYPES: FLAT/PHILIPS VDC; TIP MATERIAL: STEEL; TIP SIZE RANGE: 1/1.2/1.4/1.8/2.4/3MM, PH0,PH1,PH2,PH3,PH4; FEATURE: N/A; HANDLE MATERIAL: N/A PC; QUANTITY: 11 PC; PRECISION SCREWRIVE SET\nMAKE:RS PRO, STOCK NUMBER:537-883; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-055156","SCREWDRIVER SET:SCREWDRIVER SET;1000V","SCREWDRIVER, SET: TYPE: SCREWDRIVER SET; TIP TYPES: SLOTTED,PHILIPS,POZIDRIV VDC; TIP MATERIAL: CHROME VANADIUM; TIPSIZE RANGE: 2.5X75, 3X100,4X100, 5.5X125, 6.5X150MM,#0X60, #1X80, #2X100MM, PX0X60, PC1X80MM; FEATURE: 1000V; HANDLE MATERIAL: PP/TPR PC; QUANTITY: 10 PC; VDE SCREWDRIVER SET 1000V UNIOR ; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-055216","PLIERS:WATERPUMP;LG 250;INSULATED;STL","GEDORE UNIVERSAL WATERPUMP PLIERS 250MM LONG - PRODUCT CODE: GED6410650. VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-057974","DRILL:IMPACT;13 MM;DURA SHIELD HOUSING","BOSCH GSB 16RE 13MM IMPACT DRILL 700W. VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-058795","BIT TWST:2.0 MM;STRAIGHT;HSS;DRILL","BIT, TWIST: DIAMETER: 2.0 MM; SHANK: STRAIGHT; MATERIAL: HSS; LENGTH: STANDARD MM; TYPE: DRILL",100,"EA"]
["STM-059621","HANDLE, SPANNER WRENCH:8MM RING SLOGGING","HANDLE, SPANNER WRENCH: STYLE DESIGNATOR: 8MM RING SLOGGING; MATERIAL: CHROME VANADUIM; TORQUE: DESIGNED FOR HEAVY DUTY; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-059622","HANDLE, SPANNER WRENCH:10MM RING SLOG","HANDLE, SPANNER WRENCH: STYLE DESIGNATOR: 10MM RING SLOG; MATERIAL: CHROME VANADUIM; TORQUE: HEAVY DUTY APPLICATION; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-059624","HANDLE, SPANNER WRENCH:13MM RING SLOG","HANDLE, SPANNER WRENCH: STYLE DESIGNATOR: 13MM RING SLOG; MATERIAL: CHROME VANADUIM; TORQUE: DESIGNED FOR HEAVY DUTY; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-059625","HANDLE, SPANNER WRENCH:17MM RING SLOG","HANDLE, SPANNER WRENCH: STYLE DESIGNATOR: 17MM RING SLOG; MATERIAL: CHROME VANADUIM; TORQUE: DESIGNED FOR HEAVY DUTY; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-059627","KEY:ALLEN KEY CHROME VANADIUM;BALL HEAD","ALLEN KEY SET - BALL POINT - LONG - 9 PIECE\nKEY: TYPE: ALLEN KEY CHROME VANADIUM; STYLE: BALL HEAD; MATERIAL: CHROME VANADIUM; SPECIFICATION: 1.5-10 MM; ALLEN KEY BALL HEAD LONG SERIES SET 1.5-10MM; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-059629","PLIERS:COBINATION;LG 200 MM;INSULATED","PLIERS - COMBINATION - 200MM LONG - INSULATED\nMAKE: GEDORE;PLIERS: TYPE: COBINATION; LENGTH: 200 MM; HANDLE: INSULATED; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-059973","HOLDER ELECTRD WELD:OPTIMUS STYLE;400 A","HOLDER, ELECTRODE WELDING: DESIGN TYPE: OPTIMUS STYLE; OPERATING CURRENT: 400 A; ELECTRODE QUANTITY: 1; ELECTRODE TYPE: FULLY INSULATED JAWS; INSULATION: RIBBED HANDLE; FULLY INDUSTRIAL TYPE ELECTRODE HOLDER; RIBBED HANDLES FOR BETTER GRIP AND OPTIMAL COOLING; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-059980","HELMET WELDG:POLYPROPYLENE;FLIP FRONT","HELMET, WELDING: MATERIAL: POLYPROPYLENE; FACEPIECE TYPE: FLIP FRONT; DIMENSIONS: 108 X 51 MM; POLYPROPYLENE WELDING HELMET FOR MIG,TIG AND ARC WELDING; OFFERS FULL PROTECTION AND COMPLIES WITH EN 175; AFROX ITEM CODE: W053151; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-060148","LEVEL:TORPEDO;203 MM;3","LEVEL: TYPE: TORPEDO; DIMENSIONS: 203 MM; MATERIAL: MOULDED ABS BODY FPR STRENGTH; VIALS: 3; 0-42-294; LIGHTWEIGHT INJECTION MOULDED ABS BODY FOR STRENGHT; 3 VIALS HORIZONTAL, PLUMB AND 45 DEGREES; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-060150","WRENCH ALLN:LG N/A","WRENCH, ALLEN: SIZE: T10, T15, T20, T25, T27, T30, T40, T45, T50; LENGTH: N/A; MATERIAL: CHROME MOLYDBENUM / VANADIUM; ALLEN KEY SET - TRRX - CLIP 9 PIECE; SIZE: T10,T15,T20,T25,T27,T30,T40,T45,T50\nPROFFESSIONAL QUALITY KEY SET MANUFACTURED FROM CHROME MOLYDBENUM / VANADIUM STEEL,CORRECTLY HARDENEDAND TEMPERED FOR MAXIMUM TORQUE; LONG PATTTERN WITH SATIN-NICKEL FINISH; SET IN HANDY PLASTIC CASE FOR CONVENIENCE; MAKE:RACO; ITEM CODE: RIC0197; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-060830","TOOL:SPECIAL TOOL","TOOL: TYPE: SPECIAL TOOL; PAP6600-SIL. Pull Rod Assembly for installation of Pop-a-Plug® P2 sizes P2-460 to P2-500 / P2-600 to P2-680. Assembly Includes: Pull Rod, Knurled Nut, Rod & Tube Positioner, Plug Positioner & Safety Hex Nut. VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-060830","TOOL:SPECIAL TOOL","TOOL: TYPE: SPECIAL TOOL; PAP6600-SIL. Tapered Reamer 5/8\" (15.9mm), 0.400-0.580 (10.2-14.7mm). VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-064030","KEY:2- 10MM ALLEN KEYS","KEY: TYPE: 2- 10MM ALLEN KEYS; STYLE: 2- 10MM ALLEN KEYS; MATERIAL: 2- 10MM ALLEN KEYS; SPECIFICATION: 2- 10MM ALLEN KEYS; ALLEN KEYS SETS 2 -10MM",15,"EA"]
["STM-064746","SET:DRILL BITS SET 25PC;1-13 MM;HSS","SET: TYPE: DRILL BITS SET 25PC; APPLICATION: 1-13 MM; SPECIFICATION: DRILL BIT SET 25PC; QUANTITY: AS NEEDED; COMPRISING: HSS; SIZE RANGE: DRILL BIT SET 25PC; MATERIAL: HSS; DRILL BIT SET 25 PIECE HSS 1-13MM",15,"EA"]
["STM-068966","LADDER STEP:HT 1.2 M;FIBREGLASS;135 KG;4","LADDER, STEP: HEIGHT: 1.2 M; MATERIAL: FIBREGLASS; LOAD RATING: 135 KG; STEP QUANTITY: 4; CROSSPIECE SURFACE TYPE: DEEPLY SERRATED 76MM PULTRUDED FIBREGLASS; CROSSPIECE TYPE: STEPS; PLATFORM: HEAVY DUTY STRUCTURAL MOULDED TOP KEEPS TOOLS HANDY; SAFETY FEET: INCLUDED; WIDTH: 420 MM; FGS4-ALL\nHEAVY DUTY NON-CONDUCTIVE STEP-LADDER IS RECOMMENDED FOR INDUSTRIAL APPLICATIONS WHICH ENTAIL WORKING WITH OR AROUND ELECTRICAL CURRENT, FIBREGLASS CONSTRUCTION ENSURES NON-CONDUCTIVITY LIVE LINE TESTED TO 32KV, MAXIMUM STATIC LOAD RATING MSVL 175KG; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-072063","HOLDER MACHG TL:MACHINING TOOL;10 X 10","HOLDER, MACHINING TOOL: STYLE: MACHINING TOOL; HOLDER SIZE: 10mm X 10mm; MATERIAL: CARBON STEEL; INSERT MATERIAL: NA; TYPE: TOOL HOLDER; 3600884 SDJCR 1010F-07 TOOL HOLDER; PART NUMBER: 987654; VENDORS ARE RESPONSIBLE FOR ENSURINGTHAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-072064","HOLDER MACHG TL:MACHINING TOOL;NA","HOLDER, MACHINING TOOL: STYLE: MACHINING TOOL; HOLDER SIZE: 10MM X 10MM; MATERIAL: CARBON STEEL; INSERT MATERIAL: NA; TYPE: TOOL HOLDER; 3600875 SDJCL 1010F-07 TOOL HOLDER; PART NUMBER: 987654; VENDORS ARE RESPONSIBLE FOR ENSURINGTHAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-072065","HOLDER MACHG TL:MACHINING TOOL;NA","HOLDER, MACHINING TOOL: STYLE: MACHINING TOOL; HOLDER SIZE: 12MM X 12MM; MATERIAL: CARBON STEEL; INSERT MATERIAL: NA; TYPE: TOOL HOLDER; 3600885 SDJCR 1212F-11 TOOL HOLDER; PART NUMBER: 987654; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-072066","HOLDER MACHG TL:MACHINING TOOL;NA","HOLDER, MACHINING TOOL: STYLE: MACHINING TOOL; HOLDER SIZE: 12MM X 12MM; MATERIAL: CARBON STEEL; INSERT MATERIAL: NA; TYPE: TOOL HOLDER; 3600876 SDJCL 1212F-11 TOOL HOLDER; PART NUMBER: 987654; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-072067","HOLDER MACHG TL:MACHINING TOOL;NA","HOLDER, MACHINING TOOL: STYLE: MACHINING TOOL; HOLDER SIZE: 10MM X 10MM; MATERIAL: CARBON STEEL; INSERT MATERIAL: NA; TYPE: TOOL HOLDER; 3600900 SDNCN 1010F-07 TOOL HOLDER; PART NUMBER: 987654; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-072068","HOLDER MACHG TL:MACHINING TOOL;NA","HOLDER, MACHINING TOOL: STYLE: MACHINING TOOL; HOLDER SIZE: 12MM X 12MM; MATERIAL: CARBON STEEL; INSERT MATERIAL: NA; TYPE: TOOL HOLDER; 3600901 SDNCN 1212F-07 TOOL HOLDER; PART NUMBER: 987654; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-072070","LADDER:A FRAME;LG 0.90;AL;NA;NA;NA;NA;NA","LADDER: TYPE: A FRAME; LENGTH: 0.90; MATERIAL: AL; LOAD CAPACITY: NA; CROSSPIECE TYPE: NA; CROSSPIECE SURFACE TYPE: NA; SAFETY FEET: NA; SAFETY FEET TYPE: NA; LAS3 - H/DUTY A-FRAME LADDER 0.9M; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-072071","LADDER:STEP;LG 1.8;AL;NA;NA;NA;NA;NA","LADDER: TYPE: STEP; LENGTH: 1.8; MATERIAL: AL; LOAD CAPACITY: NA; CROSSPIECE TYPE: NA; CROSSPIECE SURFACE TYPE: NA; SAFETY FEET: NA; SAFETY FEET TYPE: NA; LAS6 - INDUSRIAL STEP LADDER; VENDORS ARE RESPONSIBLE FOR ENSURING THATTHEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-073911","LADDER:LG STORAGE LENGHT 2.85X0.70X0.25","LADDER: TYPE: ROLGUARD PLATFORM LADDER WITH EXTRA-LARGE SURFACE; LENGTH: STORAGE LENGHT 2.85X0.70X0.25; MATERIAL: ALUMINIUM; LOAD CAPACITY: WEIGHT:23.40; CROSSPIECE TYPE: ALUMINIUM; CROSSPIECE SURFACE TYPE: EXTRA-LARGE WORKING PLATFORM; SAFETY FEET: TELESCOPIC EXPENDABLE; SAFETY FEET TYPE: EQUIPPED WITH WHEEL FOR EASY TRANSPORT; ROLGUARD PLATFORM LADDER WITH EXTRALARGE SURFACE; ITEM NUMBER: 502136; NUMBER OF RUNGS: 6; PLATFORM HEIGHT (M): 1.39; STORAGE LENGHTS(M): 2.85 X 0.70X0.25; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-073921","TROLLEY:1143MMX630MMX410MM N","TROLLEY: TYPE: TROLLEY INDUSTRIAL FOLDING NOSE MEDIUM LIGHT DUTY; DIMENSIONS: 1143MMX630MMX410MM N; MILD STEEL, ELECTROPLATED; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-074940","CUTTER BLT:STRAIGHT;NORMAL;200 MM;3 MM","CUTTER, BOLT: HEAD TYPE: STRAIGHT; CUT TYPE: NORMAL; SIZE: 200 MM; MATERIAL ACCOMODATED DIAMETER: 3 MM; MINI BOLT CUTTER. NON SLIP MOULDED PLASTIC GRIP. SPRING RETURN; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",20,"EA"]
["STM-074944","CUTTER BLT:BENT;NORMAL;200 MM;3 MM","CUTTER, BOLT: HEAD TYPE: BENT; CUT TYPE: NORMAL; SIZE: 200 MM; MATERIAL ACCOMODATED DIAMETER: 3 MM; MINI BOLT CUTTER. NON-SLIP MOULDED PLASTIC GRIP. SPRIND LOADED; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-074951","PUNCH CENTR:SQUARE HEAD;60 DEG;MULITPLE","PUNCH, CENTER: TYPE: SQUARE HEAD; POINT DIAMETER: 60 DEG; DIAMETER: MULITPLE; OVERALL LENGTH: 100 MM; CENTRE PUNCH SET, 4 PIECE. 3.2MM, 4.0MM, 4.8MM AND 6.3MM; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-074954","SCRAPER:COMFORT GRIP;150 X 75 MM;STEEL","SCRAPER: TYPE: COMFORT GRIP; DIMENSIONS: 150 X 75 MM; MATERIAL: STEEL; HEAVY DUTY, WITH SCALE TANGS, TEMPERED FLEXIBLE STEEL BLADES AND COMFORT GRIP; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINSTTHE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-074956","EXTRACTOR SET:C-SCREW;6 PC","EXTRACTOR SET: TYPE: C-SCREW; QUANTITY: 6 PC; 6 PIECE C-SCREW EXTRACTOR SET; SIZES: 1, 2, 3, 4, 5 AND 6; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-075888","TOOL:WIRE STRIPPING;170 MM","TOOL: TYPE: WIRE STRIPPING; DIMENSIONS: 170 MM; WIRE STRIPPING TOOL FOR 1.0, 1.6,2.0,2.6,3.2MM\nBODY: ZINC ALLOY; BLADE: SS41; BLADE HARDNESS: HV450~800; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-078302","TAP THRD CUT:M6;66MM;1MM PITCH;HSS;3","TAP, THREAD CUTTING: TAP SIZE: M6; OVERALL LENGTH: 66MM; THREAD: 1MM PITCH; MATERIAL: HSS; FLUTE QUANTITY: 3; THREAD LENGTH: 19MM; FEW M6 X 1MM METRIC TAP SET, METRIC COARSE HSS GROUND THREAD TAPS; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEYARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-078303","TAP THRD CUT:M8;75MM;1.25;HSS;3;22MM","TAP, THREAD CUTTING: TAP SIZE: M8; OVERALL LENGTH: 75MM; THREAD: 1.25; MATERIAL: HSS; FLUTE QUANTITY: 3; THREAD LENGTH: 22MM; SUPPLY M8 X 1.25 METRIC TAP SET, FEW, METRIC COURSE HSS GROUND THREAD TAPS; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-078304","TAP THRD CUT:M10;80MM;1.5;HSS;3;24MM","TAP, THREAD CUTTING: TAP SIZE: M10; OVERALL LENGTH: 80MM; THREAD: 1.5; MATERIAL: HSS; FLUTE QUANTITY: 3; THREAD LENGTH: 24MM; SUPPLY FEW - M10 X 1.5 METRIC TAP SET, METRIC COARSE HSS GROUND THREAD TAPS; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-078418","TAP SET THRD CUT:M12;1.75;HSS;3;HAND;RH","TAP SET, THREAD CUTTING: TAP SIZE: M12; THREAD: 1.75; MATERIAL: HSS; QUANTITY: 3; TYPE: HAND; THREAD DIRECTION: RH; SUPPLY FEW M12 X 1.75 METRIC COURSE TAPS, HSS GROUND THREAD; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-078432","DIE SET THRD CUTNG:BOLT/PIPE;1MM METRIC","DIE SET, THREAD CUTTING: TYPE: BOLT/PIPE; THREAD: 1MM METRIC; DIMENSIONS: WD 0.71 X 6.3MM THICK; DIE QUANTITY: 5; MATERIAL: HSS; SUPPLY FEW M6 X 1.0 HSS GROUND THREAD DIE NUT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-078441","DIE SET THRD CUTNG:BOLT/PIPE;1.25MM;5","DIE SET, THREAD CUTTING: TYPE: BOLT/PIPE; THREAD: 1.25MM; DIMENSIONS: WD 0.82 X THK 9.4; DIE QUANTITY: 5; MATERIAL: HSS; SUPPLY FEW M8 X 1.25 HEX DIE NUT GROUND THREAD; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-078452","DIE SET THRD CUTNG:BOLT/PIPE;1.5MM;5","DIE SET, THREAD CUTTING: TYPE: BOLT/PIPE; THREAD: 1.5MM; DIMENSIONS: WD 0.94 X THK 9.4; DIE QUANTITY: 5; MATERIAL: HSS; SUPPLY FEW M10 X 1.5 METRIC HEX DIE NUT GROUND THREAD; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINSTTHE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-078456","DIE SET THRD CUTNG:BOLT/PIPE;1.75MM;5","DIE SET, THREAD CUTTING: TYPE: BOLT/PIPE; THREAD: 1.75MM; DIMENSIONS: WD 1.10 X THK 12.7; DIE QUANTITY: 5; MATERIAL: HSS; SUPPLY FEW M12 X 1.75 HEX DIE NUT GROUND THREAD; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-078504","REAMER:HAND TAPER PIN;M6;LG 135;3;RH;HSS","REAMER: TYPE: HAND TAPER PIN; DIAMETER: M6; LENGTH: 135; FLUTES: 3; CUT: RH; MATERIAL: HSS; SUPPLY M6 HSS STAIGHT SHANK HAND TAPER PIN REAMER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5,"EA"]
["STM-078509","REAMER:HAND TAPER PIN;M8;LG 180;5;RH;HSS","REAMER: TYPE: HAND TAPER PIN; DIAMETER: M8; LENGTH: 180; FLUTES: 5; CUT: RH; MATERIAL: HSS; SUPPLY M8 STRAIGHT SHANK HAND TAPER PIN REAMER;  VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5,"EA"]
["STM-078515","REAMER:HAND TAPER PIN;M10;LG 255;5;RH","REAMER: TYPE: HAND TAPER PIN; DIAMETER: M10; LENGTH: 255; FLUTES: 5; CUT: RH; MATERIAL: HSS; SUPPLY M10 STRAIGHT SHANK HAND TAPER PIN REAMER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5,"EA"]
["STM-078520","REAMER:HAND TAPER PIN;M12;LG 255;5;RH","REAMER: TYPE: HAND TAPER PIN; DIAMETER: M12; LENGTH: 255; FLUTES: 5; CUT: RH; MATERIAL: HSS; SUPPLY M12 STRAIGHT SHANK HAND TAPER PIN REAMER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5,"EA"]
["STM-078525","BIT:CARBIDE;LG 25MM;HSS;12MM","BIT: TYPE: CARBIDE; LENGTH: 25MM; MATERIAL: HSS; DIAMETER: 12MM; SUPPLY 12MM X 25MM CYLINDER-END CARBIDE BURR, CUT 9 CHIPBREAKER, PRODUCT CODE: KEN2100360K; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-078530","BIT:CARBIDE BIT;LG 25;HSS;12","BIT: TYPE: CARBIDE BIT; LENGTH: 25; MATERIAL: HSS; DIAMETER: 12; SUPPLY 12MM X 25MM ROUND TREE CARBIDE BURR BIT, CUT 9 CHIPBREAKER, PRODUCT CODE: KEN2103320K; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-078535","WRENCH, TAP:TAP WRENCH;3/4 INCH;480","WRENCH, TAP: TYPE: TAP WRENCH; TAP SIZE: 3/4 INCH; BODY LENGTH: 480; MATERIAL: TEMPERED STEEL; SUPPLY 19MM HAND TAP WRENCH, PRODUCT CODE: KEN5188480K; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-078540","WRENCH, TAP:TAP WRENCH;3/8 INCH;275","WRENCH, TAP: TYPE: TAP WRENCH; TAP SIZE: 3/8 INCH; BODY LENGTH: 275; MATERIAL: TEMPERED STEEL; SUPPLY 3/8 INCH TRADITIONAL TAP WRENCH, PRODUCT CODE: KEN5188470K; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-092791","INDEX, DRILL BIT:4MM;TITANIUM STEEL","INDEX, DRILL BIT: DRILL SIZE: 4MM; MATERIAL: TITANIUM STEEL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-092805","INDEX, DRILL BIT:9MM;TITANIUM STEEL","INDEX, DRILL BIT: DRILL SIZE: 9MM; MATERIAL: TITANIUM STEEL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-092807","INDEX, DRILL BIT:10MM;TITANIUM STEEL","INDEX, DRILL BIT: DRILL SIZE: 10MM; MATERIAL: TITANIUM STEEL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-092815","INDEX, DRILL BIT:3MM;MASIONARY BIT","INDEX, DRILL BIT: DRILL SIZE: 3MM; MATERIAL: MASIONARY  BIT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-092818","INDEX, DRILL BIT:4NN;NASIONARY BIT","INDEX, DRILL BIT: DRILL SIZE: 4NN; MATERIAL: NASIONARY BIT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-092820","INDEX, DRILL BIT:5MM;MASIONARY BIT","INDEX, DRILL BIT: DRILL SIZE: 5MM; MATERIAL: MASIONARY BIT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-092822","INDEX, DRILL BIT:6MM;MASIONARY BIT","INDEX, DRILL BIT: DRILL SIZE: 6MM; MATERIAL: MASIONARY BIT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-092824","INDEX, DRILL BIT:7MM;MASIONARY BIT","INDEX, DRILL BIT: DRILL SIZE: 7MM; MATERIAL: MASIONARY BIT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-092826","INDEX, DRILL BIT:8MM;MASIONARY BIT","INDEX, DRILL BIT: DRILL SIZE: 8MM; MATERIAL: MASIONARY BIT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-092832","INDEX, DRILL BIT:9MM;MASONARY BIT","INDEX, DRILL BIT: DRILL SIZE: 9MM; MATERIAL: MASONARY BIT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-092833","INDEX, DRILL BIT:10MM;MASIONARY BIT","INDEX, DRILL BIT: DRILL SIZE: 10MM; MATERIAL: MASIONARY BIT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-092836","INDEX, DRILL BIT:12MM;MASIONARY BIT","INDEX, DRILL BIT: DRILL SIZE: 12MM; MATERIAL: MASIONARY BIT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-092838","INDEX, DRILL BIT:11MM.;MASIONARY BIT","INDEX, DRILL BIT: DRILL SIZE: 11MM.; MATERIAL: MASIONARY BIT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-093206","TOOL:DEMOLITION DRILL;JACK HAMMER","TOOL: TYPE: DEMOLITION DRILL; STYLE: JACK HAMMER; DIMENSIONS: UNKNOWN; SPECIFICATION: 1500W, MAX 10.1KG; DRILL P DEMOLITION 1500W BOS. HAMMER SDS MAX 10.1KG; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWINGREVISION NUMBER (IF APPLICABLE).",5,"EA"]
["STM-093207","TOOL:BELT SANDER;1200W;100MM X 610MM","TOOL: TYPE: BELT SANDER; STYLE: 1200W; DIMENSIONS: 100MM X 610MM; MAKITA BELT SANDER 100MM X 610MM BELT 1200W WITH DUST BAG; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-093504","PLIERS:QUICK ACTION;LG NA;INSULATED","PLIERS: TYPE: QUICK ACTION; HANDLE: INSULATED; MATERIAL: PLASTICE; 1/4\" PLIER FOR HOSE ASSEMBLY\nCODE: IND4470010K; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-094253","SAW:HACK;300MM","SAW: TYPE:HACK; DIMENSIONS: 300MM; RS COMPLNENT PAST NUMBER: 442-0515; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-094585","GUN:HEAT;ELECTRICAL","GUN: TYPE: HEAT; POWER SOURCE: ELECTRICAL; HEAT GUN. RS PART NUMBER: 175-7106; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-094594","WRENCH PIPE:44;LG 305;STL","WRENCH, PIPE: CAPACITY: 44; LENGTH: 305; MATERIAL: STL; BAHCO PIPE WRENCH. RS STOCK NUMBER: 731-9402; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-095895","TAP SET THRD CUT:M3 TO M10;METRIC;40 PC","TAP SET, THREAD CUTTING: TAP SIZE: M3 TO M10; THREAD: METRIC; QUANTITY: 40 PC; TYPE: HAND; THREAD DIRECTION: CLOCKWISE; 40PC METRIC TAP AND DIE SET. RS STOCK NUMBER: 6122718; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-098268","PLIERS:GRIP;LG 250 MM;NON INSULATED;STL","PLIERS: TYPE: GRIP; LENGTH: 250 MM; HANDLE: NON INSULATED; MATERIAL: STL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-098338","TAPE MEASNG:HIGH IMPACT;STAINLESS STEEL","TAPE, MEASURING: TYPE: HIGH IMPACT; DIMENSIONS: WD 9.5 MM X LG 30 M; MATERIAL: STAINLESS STEEL; DURABLE YELLOW HIGH IMPACT ABS CASE FOR STRENGTH; FEATURES A BLADE GUARD AND ROLLERS OF SS FOR SMOOTH OPERATION; STEEL BLADE WITH 2 COLOUR GRADUATIONS FOR EASY READING IN ALL CONDITIONS; MYLAR COATING FOR MAXIMUM PROTECTION AGAINST ABRASION; HOOK WITH SPURS FOR EASE OF USE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-098348","BIT TWST:3 MM;STRAIGHT;LG 61 MM;N","BIT, TWIST: DIAMETER: 3 MM; SHANK: STRAIGHT; MATERIAL: HSS; LIGHT INDUSTRIAL STEEL; LENGTH: 61 MM; TYPE: N; TIP: DRILLING; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-098366","BIT TWST:4 MM;STRAIGHT;LG 75 MM;N","BIT, TWIST: DIAMETER: 4 MM; SHANK: STRAIGHT; MATERIAL: HSS; LIGHT INDUSTRIAL STEEL; LENGTH: 75 MM; TYPE: N; TIP: DRILLING; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-098372","BIT TWST:5 MM;STRAIGHT;LG 86 MM;N","BIT, TWIST: DIAMETER: 5 MM; SHANK: STRAIGHT; MATERIAL: HSS; LIGHT INDUSTRIAL STEEL; LENGTH: 86 MM; TYPE: N; TIP: DRILLING; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-098381","BIT TWST:6 MM;STRAIGHT;LG 93 MM;N","BIT, TWIST: DIAMETER: 6 MM; SHANK: STRAIGHT; MATERIAL: HSS; LIGHT INDUSTRIAL STEEL; LENGTH: 93 MM; TYPE: N; TIP: DRILLING; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-098407","BIT TWST:7 MM;STRAIGHT;LG 109 MM;N","BIT, TWIST: DIAMETER: 7 MM; SHANK: STRAIGHT; MATERIAL: HSS; LIGHT INDUSTRIAL STEEL; LENGTH: 109 MM; TYPE: N; TIP: DRILLING; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-098408","BIT TWST:8 MM;STRAIGHT;LG 117 MM;N","BIT, TWIST: DIAMETER: 8 MM; SHANK: STRAIGHT; MATERIAL: HSS; LIGHT INDUSTRIAL STEEL; LENGTH: 117 MM; TYPE: N; TIP: DRILLING; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",30,"EA"]
["STM-098410","BIT TWST:10 MM;STRAIGHT;LG 133 MM;N","BIT, TWIST: DIAMETER: 10 MM; SHANK: STRAIGHT; MATERIAL: HSS; LIGHT INDUSTRIAL STEEL; LENGTH: 133 MM; TYPE: N; TIP: DRILLING; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-098417","TAPE MEASNG:PROFESSIONAL;LG 5 M","TAPE, MEASURING: TYPE: PROFESSIONAL; DIMENSIONS: LG 5 M; MATERIAL: RUBBER CASE; FAST LOCK TO SECURE BLADE; STAND OUT 1.4M; NYLON BLADE COATING TWICE DURABILITY OF ACRYLIC COATING; HOOK MAGNETS, 2 RIVETS + 1 EYELET FOR MULTI-USE WITH EXTRA STRENGHT; DOUBLE SIDED BLADE FOR EASY READABILITY FROM ALL ANGLES; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-098446","COLLET WELDG:BODIES;2.4 MM;LG 47 MM","COLLET, WELDING: TYPE: BODIES; SIZE: 2.4 MM; LENGTH: 47 MM; COLLET BODIES USED TO SECURELY CLAMP THE TUNGSTEN ELECTRODE, FOR USE WITH 17/26 AND 18 SERIES TORCHES; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",100,"EA"]
["STM-098505","CHISEL COLD HND:LG 300 MM;25 MM;FLAT","CHISEL, COLD HAND: LENGTH: 300 MM; BLADE WIDTH: 25 MM; MATERIAL: HEXAGONAL TOOL STEEL; TYPE: FLAT; THE BODY IS TAPERED TO THE EDGE WHERE A PRIMARY AND SECONDARY CUTTING EDGE ARE FORMED; THESE CHISELS ARE USED BY THE CONSTRUCTION AND ENGINEERINGINDUSTRIES; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-098767","CLEANER TIP:CLEANING FILE;ALUMINIUM","CLEANER, TIP: TYPE: CLEANING FILE; HANDLE: ALUMINIUM; DIAMETER: ASSORTED SIZES; MATERIAL: STRONG ALUMINIUM CASE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-098976","TOOL:13MM CHROME VANADIUM COMB SPANNER","GEDORE 13MM COMBINATION SPANNERS - PRODUCT CODE: GED600113. VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-098994","TAPE MEASNG:PROFESSIONAL;LG 8 M","TAPE, MEASURING: TYPE: PROFESSIONAL; DIMENSIONS: LG 8 M; MATERIAL: RUBBER CASE; FAST LOCK TO SECURE BLADE; STAND OUT 1.4M; NYLON BLADE COATING TWICE DURABILITY OF ACRYLIC COATING; HOOK MAGNETS, 2 RIVETS + 1 EYELET FOR MULTI-USE WITH EXTRA STRENGHT; DOUBLE SIDED BLADE FOR EASY READABILITY FROM ALL ANGLES; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-099464","TAPE:TAPE MEASURE (3M);N/A;N/A;N/A","STANLEY POWERBLOCK MEASURING TAPE 3M X 19MM. VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-099478","SQUARE:ENGINEERS SQUARE (5);N/A","GR ENGINEERS SQUARE SSA/12 300MM - PRODUCT CODE: GRO6525. VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-099926","WRENCH IMPCT:1 IN;PNEUMATIC;400-1400 NM","WRENCH, IMPACT: DRIVE SIZE: 1 IN; POWER SOURCE: PNEUMATIC; TORQUE: 400-1400 NM; SPEED: 5100 RPM; CP6778EX-P18D H/DUTY PISTOL GRIP ATEX 1750NM; TORQUE WRENCH; SPEC:; SQUARE DRIVE-1''; NET WEIGHT - 4,6KG; LENGTH - 255MM; MAX TORQUE - 1750 NM",15,"EA"]
["STM-100135","PLIERS VISE GRP:VICE GRIP,LG 250MM MM","PLIERS, VISE GRIP: TYPE: VICE GRIP, CAPACITY: NOT APPLICCABLE MM, LENGTH: 250MM MM, MATERIAL: CVS; WRENCH, ADJUSTABLE, CURVED JAW; NICKEL PLATED;",20,"EA"]
["STM-100387","GUN AIR BLW:HAND-HELD;FNPT 1/4;NA","GUN, AIR BLOW: TYPE: HAND-HELD; FITTING TYPE: FNPT 1/4; TEMPERATURE RANGE: NA; CODE: KBE2592550K  PISTOL GRIP; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-100511","ADAPTOR WRNCH SCKT:1/2;LG NA;NA;NA","ADAPTOR, WRENCH SOCKET: DRIVE SIZE: 1/2; CODE: 987654; DESCRIPTION: ADAPTOR - 7680650 1/2\" DR RATCHET HEAD; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THECORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-100512","ADAPTOR WRNCH SCKT","ADAPTOR, WRENCH SOCKET: DRIVE SIZE: 3/4\"; CODE: 987654; DESCRIPTION:ADAPTOR - 7680730 3/4\"DR RATCHET HEAD; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THECORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-100558","SOCKET SCKT WRNCH:NA;SQUARE;3/4 IN;NA;NA","SOCKET, SOCKET WRENCH: DRIVE END SHAPE: SQUARE; DRIVE SURFACE SIZE: 3/4 IN; CODE:987654; DESCRIPTION: KEN5838831K 46MM DEEP IMPACT SOCKET 3/4\" SQUARE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-100688","PUNCH SET:PIN;.;.;6","PUNCH, SET: TYPE: PIN; SET QUANTITY: 6; CODE: 20977; DESCRIPTION: KEN5182200K SET OF 6 PARALLEL PIN PUNCHES; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",50,"EA"]
["STM-100691","TOOL DBRRNG:DUALCUT;6 MM;.;CARBIDE;HAND","TOOL, DEBURRING: TYPE: DUALCUT; DIAMETER: 6 MM; MATERIAL: CARBIDE; APPLICATION: HAND; CODE: 34226; DESCRIPTION: YRK2109920K SPEEDWAY DUALCUT 6MM SHANK 8PCECARBIDEBURR SET; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-100694","PLIERS DGNL CUTNG:.;PLASTIC;.","PLIERS, DIAGONAL CUTTING: INSULATED HANDLE: PLASTIC; CODE: 21726; DESCRIPTION: KEN5583330K 7 DIAGONAL CUTTING NIPPERS; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THECORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",30,"EA"]
["STM-100704","PLIERS RETNG RNG:INTERNAL;LG .;.;.;BENT","PLIERS, RETAINING RING: TYPE: INTERNAL; TIP STYLE: BENT; INSULATION: PLASTIC; CODE: 21788; DESCRIPTION:KEN5586510K 5 BENT NOSE INTERNAL CIRCLIP PLIERS; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-100709","PLIERS RETNG RNG:EXTERNAL;LG .;.;.;BENT","PLIERS, RETAINING RING: TYPE: EXTERNAL; TIP STYLE: BENT; INSULATION: PLASTIC; CODE:21790; DESCRIPTION: KEN5586530K 5 BENT NOSE EXTERNAL CIRCLIP PLIERS; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-100718","PLIERS:SNIPE NOSE;LG .;PLASTIC;STL","PLIERS: TYPE: SNIPE NOSE; HANDLE: PLASTIC; MATERIAL: STL; CODE:21721; DESCRIPTION: KEN5583230K 8 SNIPE NOSE PLIERS WITH SIDE CUTTER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",50,"EA"]
["STM-100727","SCRIBER:DOUBLE ENDED;.;STEEL","SCRIBER: TYPE: DOUBLE ENDED;  MATERIAL: STEEL; CODE: 21051; DESCRIPTION:KEN5184370K 7 INCH DOUBLE ENDED ENGINEERS SCRIBER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",50,"EA"]
["STM-100809","HAMMER MLLT:MALLET;16 OZ;WOOD","HAMMER, MALLET: TYPE: MALLET; HEAD WEIGHT: 16 OZ; HEAD MATERIAL: RUBBER COMPOTHANE; HANDLE: WOOD; CODE:21206; DESCRIPTION:KEN5259160K 16OZ BLACK RUBBER MALLETWOOD SHAFT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",50,"EA"]
["STM-100823","BIT SET","BIT SET: CODE:27960; DESCRIPTION:SHR0258500K SET OF 25 HSS DRILLS 113.00MM X 0.5mm; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",50,"EA"]
["STM-100864","TAPE MEASNG","TAPE,MEASURING: CODE:33469; DESCRIPTION: YMT5361490K 8M LOCKING TAPE RULE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",50,"EA"]
["STM-101852","TOOL:CHAMFERING TOOL;10MM STRAIGHT SHANK","TOOL: TYPE: CHAMFERING TOOL; STYLE: 10MM STRAIGHT SHANK; DIMENSIONS: 45 DEGREES; 45 DEGREE CHAMFERING TOOL WITH 10MM STRAIGHT SHANK; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-101860","BIT TWST:2.5 MM;STRAIGHT 2.5;HSS","BIT, TWIST: DIAMETER: 2.5 MM; SHANK: STRAIGHT 2.5; MATERIAL: HSS; LENGTH: UNKNOWN; 2.5MM STRAIGHT SHANK DRILL  BIT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",100,"EA"]
["STM-101865","BIT TWST:3.5 MM;STRAIGHT 3.5;HSS","BIT, TWIST: DIAMETER: 3.5 MM; SHANK: STRAIGHT 3.5; MATERIAL: HSS; LENGTH: UNKNOWN; 3.5MM STRAIGHT SHANK DRILL BIT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",100,"EA"]
["STM-101867","BIT TWST:4 MM;STRAIGHT 4;HSS;LG UNKNOWN","BIT, TWIST: DIAMETER: 4 MM; SHANK: STRAIGHT 4; MATERIAL: HSS; LENGTH: UNKNOWN; 4MM STRAIGHT SHANK DRILL BIT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",100,"EA"]
["STM-101869","BIT TWST:6.8 MM;STRAIGHT 6.8;HSS","BIT, TWIST: DIAMETER: 6.8 MM; SHANK: STRAIGHT 6.8; MATERIAL: HSS; LENGTH: UNKNOWN; 6.8MM STRAIGHT SHANK DRILL BIT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",100,"EA"]
["STM-101903","CHUCK:DRILL CHUCK ARBOR","CHUCK: TYPE: DRILL CHUCK ARBOR; DRILL CHUCK ARBOR B16 X MT4 C4B PORTA; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-101904","CHUCK:DRILL CHUCK KEYED","CHUCK: TYPE: DRILL CHUCK KEYED; DRILL CHECK KEYED MED. 3-16 B16 KS3 PORTA; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-102981","HAMMER:CHIPPING CHISEL AND POINT END","HAMMER: TYPE: CHIPPING CHISEL AND POINT END; HEAD WEIGHT: 0.413 KG; HEAD MATERIAL: STEEL SPRING; HANDLE: SHOCKPROOF SPRING WIRE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",50,"EA"]
["STM-104799","SET:BIT;POZI;BIT","SET: TYPE: BIT; COMPRISING: POZI; MATERIAL: BIT; POZI BIT 225MM VERMONT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",100,"EA"]
["STM-104803","BIT SCRWDRVR:BIT PHILL;2X25MM","BIT, SCREWDRIVER: TIP TYPE: BIT PHILL; TIP SIZE: 2X25MM; DRIVE SHANK TYPE:; BIT PHILL NO 2X25MM CLASSIC; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",100,"EA"]
["STM-104806","TOOL:NUT SETTER;VERMON;5/16\" X 65MM MM","SPECIFICATION:; NUT SETTER 5/16\" X 65MM VERMON; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-106191","CHISEL PWR:FLAT POINT;25;18;LG 400","BOSCH SDS MAX FLAT R-TECH CHISELS FOR CFI REFURBISHMENT PROJECT. CHISEL, POWER: TYPE: FLAT POINT; BLADE SIZE: 25; SHANK: 18; LENGTH: 400; MATERIAL: STL HARDENED; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",50,"EA"]
["STM-106216","CHISEL PWR:POINTED CHISEL;22;18;LG 400","BOSCH SDS MAX POINTED CHISELS FOR CFI REFURBISHMENT PROJECT. CHISEL, POWER: TYPE: POINTED CHISEL; BLADE SIZE: 22; SHANK: 18; LENGTH: 400; MATERIAL: STL HARDENED; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",50,"EA"]
["STM-106486","BIT MSNRY:SDS MAX;30;LG 400;DIA 10","BOSCH SDS MAX M4 CONCRETE DRILL BIT - 30MM DIAMETER X 400MM LONG -CFI PROJECT. BIT, MASONRY: TYPE: SDS MAX M4; DIAMETER: 30; LENGTH: 400; MATERIAL: TUNGSTEN TIPPED; SHANK: DIA 10; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-106503","TAPE MEASNG:STANLEY;WD 13MM X 3M;STEEL","STANLEY MEASURING TAPE - 3MX13MM - CFI PROJECT. TAPE, MEASURING: TYPE: STANLEY; DIMENSIONS: WD 13MM X 3M LONG; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",50,"EA"]
["STM-106506","TAPE MEASNG:STANLEY;WD 19MM X 5M LONG","STANLEY MEASURING TAPE - 5MX19MM -CFI PROJECT. TAPE, MEASURING: TYPE: STANLEY; DIMENSIONS: WD 19MM X 5M LONG; MATERIAL: STEEL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-107174","WRENCH TRQ","TORQUE WRENCH 20-100NM PRO 100FTH 9X12; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-107213","WRENCH TRQ:9 X 12;0-20;LINEAR;LG NA;NA","TORQUE WRENCH 0-20NM SLO FTH 9X12; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-107226","WRENCH TRQ:14X18;20-200;LINEAR;LG NA;NA","TORQUE WRENCH 20-200NM PRO 200FTH 14X18; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-107233","WRENCH TRQ:14X18;60-300;LINEAR;LG NA;NA","TORQUE WRENCH 60-300NM 300FTH 14X18; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-107244","WRENCH TRQ:14X18;40-200;LINEAR;LG NA;NA","TORQUE WRENCH 40-200NM 200FTH 14X18; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-107252","WRENCH TRQ","TORQUE WRENCH 0-360NM 400FTH 14X18; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-107264","WRENCH TRQ:16MM;4-20;LINEAR;LG NA;NA;NA","11126 - SLO TH,16MM SPIGOT 4-20NM,40-180 LBF; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-107269","WRENCH TRQ:16;10-50;LINEAR;LG NA;NA;NA","15062- PRO 50,16MM SPIGOT,10-50NM,7.5-37.5LB; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",30,"EA"]
["STM-107568","WRENCH TRQ:16;20-100;LINEAR;LG NA;NA;NA","150603 - PRO 100,16MM SPIGOT,20-100NM,15-75; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",30,"EA"]
["STM-107579","WRENCH TRQ:16;40-200;LINEAR;LG NA;NA;NA","15064 PRO 200,16MM SPIGOT,40-200NM,30-150 L; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",30,"EA"]
["STM-107598","WRENCH TRQ:16;60-300;LINEAR;LG NA;NA;NA","15065 - PRO 300,16MM SPIGOT,60-300NM,44-222 L; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",30,"EA"]
["STM-108453","TOOL:RING FLAT SPANNER MM;HAND;23MM MM","TOOL: TYPE: RING FLAT SPANNER MM; STYLE: HAND; DIMENSIONS: 23MM MM; SPECIFICATION: GEDORE; 23 MM RING FLAT",15,"EA"]
["STM-108455","TOOL:RING FLAT SPANNER MM;HAND;24 MM MM","TOOL: TYPE: RING FLAT SPANNER MM; STYLE: HAND; DIMENSIONS: 24 MM MM; SPECIFICATION: GEDORE; 24MM RING FLAT",15,"EA"]
["STM-108601","TOOL:VENIER CALIPER MICROMETER;HAND","TOOL: TYPE: VENIER CALIPER MICROMETER; STYLE: HAND; DIMENSIONS: 6 INCH/150MM MM; SPECIFICATION: STAINLESS STEEL; MEASURING TOOL FOR PRECISION MEASUREMENTS",10,"EA"]
["STM-109386","TORQUE CONVERTER:HYTORC","TORQUE CONVERTER: TYPE: HYTORC; AVANTI 5 - 1 1/2\" SQD TORQUE WRENCH; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5,"EA"]
["STM-109398","WRENCH IMPCT","WRENCH, IMPACT; IW750 3/4 DR AIR IMPACT WRENCH; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-109404","SCREWDRIVER PWR:AS PER ITEM TEXT","CORDLESS GDX 180-LI 2X3.0 COMPACT; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",25,"EA"]
["STM-109492","BAR WRNCH:SPEED BRACE;1/2\";LG 425MM","BAR, WRENCH: TYPE: SPEED BRACE; DRIVE SIZE: 1/2\"; LENGTH: 425MM; MATERIAL: CHROME VANADIUM; SPEED BRACE , RAPID WRENCH 1/2\" DRIVE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-109506","HAMMER MLLT:NYLON MALLET;3;NYLON;WOODEN","HAMMER, MALLET: TYPE: NYLON MALLET; HEAD WEIGHT: 3; HEAD MATERIAL: NYLON; HANDLE: WOODEN; NYLON MALLET WITH FIXED NYLON HEAD , NOT REMOVAL NYLON HAEDS, WOODEN HANDLE.",10,"EA"]
["STM-109517","FRAME:JUNIOR HACKSAW;LG 150 MM;STL","FRAME: TYPE: JUNIOR HACKSAW; SIZE: LG 150 MM; MATERIAL: STL; JUNIOR HACKSAW , LG 150MM , FRAMW , S/ST.",20,"EA"]
["STM-109527","PUNCH CENTR:CENTRE PUNCH SET;3.2 - 6.3MM","PUNCH, CENTER: TYPE: CENTRE PUNCH SET; POINT DIAMETER: 3.2 - 6.3MM; DIAMETER: 8 - 10MM; OVERALL LENGTH: 100MM; CENTER PUNCH SET ,",20,"EA"]
["STM-109601","WRENCH:RATCHET;10;STL;NA","WRENCH: TYPE: RATCHET; SIZE: 10MM; MATERIAL: STL; APPLICATION: NA",20,"EA"]
["STM-109605","WRENCH:RATCHET;13;STL;NA","WRENCH: TYPE: RATCHET; SIZE: 13MM; MATERIAL: STL; APPLICATION: NA",20,"EA"]
["STM-109609","WRENCH","WRENCH: TYPE: RATCHET; SIZE: 17MM; MATERIAL: STL; APPLICATION: NA",20,"EA"]
["STM-109616","WRENCH:RATCHET;19MM;STL;NA","WRENCH: TYPE: RATCHET; SIZE: 19MM; MATERIAL: STL; APPLICATION: NA",20,"EA"]
["STM-109725","TOOL:HYDRAULIC TORQUE;1 IN SQ DRIVE","TOOL: TYPE: HYDRAULIC TORQUE; STYLE: COAXIAL SQUARE DRIVE AND REACTION ARM; DIMENSIONS: 1 IN SQ DRIVE; TORQUE RANGE 604 - 4025 NM; REACTION RELEASE LEVER; TITAL 399 HIGH STRENGTH LIGHTWEIGHT BODY; HIGHEST QUALITY STEEL INTERNAL COMPONENTS",3,"EA"]
["STM-109790","TOOL:TOOL WITH SENSOR;HAND;N/A","TOOL: TYPE: TOOL WITH SENSOR; STYLE: HAND; DIMENSIONS: N/A; 8DT OEG TOOL WITH SENOR",3,"EA"]
["STM-111141","TOOL BOX PORTBL:WORKSHOP TOOLKIT;RED","SENATOR 90 PIECE WORKSHOP TOOLKIT - PRODUCT CODE: SEN-595-1000K FOR HPIC DEPARTMENT.",5,"EA"]
["STM-115194","DRILL:CORDLESS;13MM;LG AS PER ITEM TEXT","MAKITA DHB458 18V CORDLESS DRILL WITH 2 X 3AH BATTERIES & CHARGER",5,"EA"]
["STM-115226","WINCH:NON MOTORISED;2000 KG;NA","WINCH: TYPE: NON MOTORISED; CAPACITY: 2000 KG; DIMENSIONS: NA;                             HAND WINCH 2000KG WITH STEEL WIRE ROPE AND HOOK",10,"EA"]
["STM-115414","CUTTER PIPE:TUBE CUTTER;TUBE CUTTER","CUTTER, PIPE: TYPE: TUBE CUTTER; CUTTING RANGE:; FEATURES: TUBE CUTTER; CUTTING MATERIAL:; PIPE SIZE: KEN50304; TUBE CUTTER - KEN50304",10,"EA"]
["STM-115421","CUTTER PIPE:TUBE CUTTER - KEN50305","CUTTER, PIPE: TYPE: TUBE CUTTER - KEN50305; CUTTING RANGE: TUBE CUTTER; FEATURES: TUBE CUTTER - KEN50305; CUTTING MATERIAL:  KEN50305; PIPE SIZE: KEN50305; TUBE CUTTER - KEN50305",10,"EA"]
["STM-115425","CUTTER PIPE:TUBE CUTTER;PVC;0-42 MM","CUTTER, PIPE: TYPE: KEN50312 CUTTER TUBE 0-42MM PVC; CUTTING RANGE: TUBE CUTTER; FEATURES: KEN50312 CUTTER TUBE 0-42MM PVC; CUTTING MATERIAL: PVC; PIPE SIZE: 0-42 MM; KEN50312 CUTTER TUBE 0-42MM PVC",10,"EA"]
["STM-115429","TOOL KIT:CUTTER RATCHET;26-42 MM","TOOL KIT: TYPE: CUTTER RATCHET; DIMENSIONS: 26-42 MM; MATERIAL: PVC - KEN50318; CUTTER RATCHET 26-42MM PVC KEN50318",10,"EA"]
["STM-115433","RIVET:GUN;FASCOR FH10 MM;LG;RIVERT GUN","RIVET: TYPE: GUN; DIAMETER: FASCOR FH10 MM; LENGTH:; HEAD DIAMETER:; HEAD: RIVERT GUN; MATERIAL:; RIVET GUN FASCOR FH10",10,"EA"]
["STM-115440","RATCHET:SPANNER;RATCHET SPANNER;STEEL","RATCHET: TYPE: SPANNER; LOAD CAPACITY: RATCHET SPANNER; MATERIAL: STEEL; RATCHET SPANNER COMBO - 10MM KEN15510 ; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-115445","RATCHET:RATCHET SPANNER COMBO;13 MM","RATCHET: TYPE: RATCHET SPANNER COMBO; DIMENSIONS: 13 MM; MATERIAL: KEN15513; RATCHET SPANNER COMBO 13MM KEN15513; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-115446","RATCHET:RATCHET SPANNER COMBO - KEN15517","RATCHET: TYPE: RATCHET SPANNER COMBO - KEN15517; LOAD CAPACITY: KEN15517; DIMENSIONS: 17 MM; MATERIAL: RATCHET SPANNER COMBO; RATCHET SPANNER COMBO 17MM KEN15517; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-115448","RATCHET:RATCHET SPANNER COMBO 19MM","RATCHET: TYPE: RATCHET SPANNER COMBO 19MM; LOAD CAPACITY: KEN15519; DIMENSIONS: 19 MM; MATERIAL: RATCHET SPANNER COMBO 19MM KEN15519; RATCHET SPANNER COMBO 19MM KEN15519; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THECORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-115450","TOOL:SPANNER;COMB OFFSET;10 MM","TOOL: TYPE: SPANNER; STYLE: COMB OFFSET; DIMENSIONS: 10 MM; SPANNER COMBO - SPANNER COMBO 10MM OFFSE",15,"EA"]
["STM-115454","TOOL:SPANNER;COMB OFFSET;13 MM","TOOL: TYPE: SPANNER; STYLE: COMB OFFSET; DIMENSIONS: 13 MM; SPECIFICATION: SPANNER COMBO 13MM OFFSET; SPANNER COMBO 13MM OFF SET",15,"EA"]
["STM-115455","TAPE MEASNG:5 M","TAPE, MEASURING: TYPE: TAPE MEASURE 5M P/LOCK STANLEY; DIMENSIONS: 5 M; MATERIAL: TAPE MEASURE 5M P/LOCK STANLEY; TAPE MEASURE 5M P/LOCK STANLEY",15,"EA"]
["STM-115457","TOOL:PLIER CRESCENT WATER PUMP;CRE0270","TOOL: TYPE: PLIER CRESCENT WATER PUMP; STYLE: CRE0270; DIMENSIONS: 250 MM; SPECIFICATION: PLIER CRESCENT WATER PUMP 250MM; PLIER CRESCENT WATER PUMP 250MM",15,"EA"]
["STM-115463","TOOL:PLIER CRESCENT WATER PUMP;CRE0295","TOOL: TYPE: PLIER CRESCENT WATER PUMP; STYLE: CRE0295; DIMENSIONS: 406 MM; SPECIFICATION: PLIER CRESCENT WATER PUMP 406MM; PLIER CRESCENT WATER PUMP 406MM",15,"EA"]
["STM-115467","PLIERS VISE GRP:VICEGRIP;LG 180 MM","PLIERS, VISE GRIP: TYPE: VICEGRIP; CAPACITY: VICEGRIP CURVED JAW; LENGTH: 180 MM; MATERIAL: KEN11605; VICEGRIP CURVED JAW 180MM KEN11605",10,"EA"]
["STM-115472","SAW HOLE:HOLESAW STARRETT KIT MM;16-51MM","SAW, HOLE: SIZE: HOLESAW STARRETT KIT  MM; ARBOR: 16-51MM; TEETH: HOLESAW STARRETT KIT 16-51MM STT0496; BLADE MATERIAL: HSS; HOLESAW STARRETT KIT 16-51MM STT0496",10,"EA"]
["STM-116530","TAP SET THRD CUT:M6;1;HSS;3;HAND;RH","TAP SET, THREAD CUTTING: TAP SIZE: M6; THREAD: 1; MATERIAL: HSS; QUANTITY: 3; TYPE: HAND; THREAD DIRECTION: RH; CARRY CASE: PLASTIC; MAKE: SOMTA",60,"EA"]
["STM-116546","WRENCH TRQ:AS PER ITEM TEXT","15065 - PRO 300,16MM SPIGOT,60-300NM,44-222 L; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",5,"EA"]
["STM-116607","TOOL KIT:ELECTRICAL;WD 300 X 500 LG","KENNEDYS VDE 16 PIECE ELECTRICAINS TOOLKIT FOR ESTATE MAINTENANCE SECTION HEAD AND IN-HOUSE STORES.",10,"EA"]
["STM-118705","BIT TWST:4.2 MM;STRAIGHT;HSS;DRILL","BIT, TWIST: DIAMETER: 4.2 MM; SHANK: STRAIGHT; MATERIAL: HSS; LENGTH: STANDARD MM; TYPE: DRILL; 4.2MM STRAIGHT SHANK DRILL BIT",100,"EA"]
["STM-118716","PUNCH SET:LETTER PUNCH SET;A-Z;UNKNOWN","PUNCH, SET: TYPE: LETTER PUNCH SET; RANGE SIZE: A-Z; MATERIAL: UNKNOWN; SET QUANTITY: 27 PIECE SET; 6MM LETTER STAMP SET A-Z",3,"EA"]
["STM-118717","PUNCH SET:LETTER PUNCH SET;A-Z;UNKOWN","PUNCH, SET: TYPE: LETTER PUNCH SET; RANGE SIZE: A-Z; MATERIAL: UNKOWN; SET QUANTITY: 27 PIECE SET; 12MM LETTER STAMP SET, A-Z.",3,"EA"]
["STM-118718","PUNCH SET:NUMBER;1-9;UNKNOWN;9 PIECE SET","PUNCH, SET: TYPE: NUMBER; RANGE SIZE: 1-9; MATERIAL: UNKNOWN; SET QUANTITY: 9 PIECE SET; 6MM NUMBER STAMP SET, 1-9.",3,"EA"]
["STM-118720","PUNCH SET:NUMBER;1-9;UNKNOWN;9 PIECE SET","PUNCH, SET: TYPE: NUMBER; RANGE SIZE: 1-9; MATERIAL: UNKNOWN; SET QUANTITY: 9 PIECE SET; 12MM NUMBER STAMP SET, 1-9.",3,"EA"]
["STM-118746","HAMMER MLLT:DEAD BLOW;4.5 KG;RUBBER","HAMMER, MALLET: TYPE: DEAD BLOW; HEAD WEIGHT: 4.5 KG; HEAD MATERIAL: RUBBER; HANDLE: RUBBER; DEAD BLOW HAMMER, 4.5KG",15,"EA"]
["STM-118753","SCRAPER:TANG;125 X 50 MM;UNKNOWN","SCRAPER: TYPE: TANG; DIMENSIONS: 125 X 50 MM; MATERIAL: UNKNOWN; SCRAPER 125MM X 50MM",20,"EA"]
["STM-118756","SCRAPER:TANG;125MM X 75MM;UNKNOWN","SCRAPER: TYPE: TANG; DIMENSIONS: 125MM X 75MM; MATERIAL: UNKNOWN; SCRAPER 125MM X 75MM",20,"EA"]
["STM-118757","SLEEVE MRSE TAPR:DRILL;4-5;STEEL;UNKNOWN","SLEEVE, MORSE TAPER: TYPE: DRILL; DIMENSIONS: 4-5; MATERIAL: STEEL; TAPER TYPE: UNKNOWN; TAPER SIZE: UNKNOWN; MORSE TAPER DRILL SLEEVES, 4-5.",10,"EA"]
["STM-118763","TOOL:TAPER;REVOLVING CENTRE;MT4","TOOL: TYPE: TAPER; STYLE: REVOLVING CENTRE; DIMENSIONS: MT4; REVOLVING CENTRE 4MT, STANDARD DUTY",10,"EA"]
["STM-119636","ROLLER PAINT:MOHAIR","ACADEMY PAINT ROLLERS WITH HANDLE - 225MM LONG. ROLLER, PAINT: TYPE: MOHAIR; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",50,"EA"]
["STM-119641","HAMMER:SCUTCH;800;STL;RUBBER/STL","LASHER SCUTCH HAMMER 800G. HAMMER: TYPE: SCUTCH; HEAD WEIGHT: 800; HEAD MATERIAL: STL; HANDLE: RUBBER/STL;",30,"EA"]
["STM-119643","HAMMER:BRICK COMB;N/A;STL;N/A","LASHER SCUTCH HAMMER BRICK COMBS - 4 PER PACK. HAMMER: TYPE: BRICK COMB; HEAD WEIGHT: N/A; HEAD MATERIAL: STL; HANDLE: N/A;",60,"EA"]
["STM-119647","NIPPERS:CONCRETE;LG 250;STEEL","HEAVY DUTY CONCRETE NIPPERS - 250MM LONG. NIPPERS: TYPE: CONCRETE; LENGTH: 250; MATERIAL:",20,"EA"]
["STM-119653","PLIERS:FENCING;LG 250;INSULATED","GEDORE FENCING PLIERS, 250MM LONG  & PRODUCT CODE:670250 NO:8260 . PLIERS: TYPE: FENCING; LENGTH: 250; HANDLE: INSULATED; MATERIAL: HARDENED & TEMPERED;",15,"EA"]
["STM-119656","CUTTER BLT:DOUBLE CAM;DUAL ENDS;460;N/A","GEDORE BOLT CUTTERS 460MM LONG - PRODUCT CODE:2675137 NO:8178. CUTTER, BOLT: HEAD TYPE: DOUBLE CAM; CUT TYPE: DUAL ENDS; SIZE: 460; MATERIAL: DIN ISO 5743; MATERIAL ACCOMODATED DIAMETER: N/A;",10,"EA"]
["STM-119694","SPRAYER:PRESSURE;5L PLASTIC CONTAINER;5L","5L WATER BOTTLE PRESSURE SPRAYERS. SPRAYER: TYPE: MANUAL PRESSURE; DIMENSIONS: 5L PLASTIC CONTAINER; CAPACITY: 5L;",10,"EA"]
["STM-119706","PLIERS VISE GRP:GRIP JAW;20;LG 250","GEDORE VICE GRIP PLIERS 250MM LONG - PRODUCT CODE:640670 NO:137/250. PLIERS, VISE GRIP: TYPE: GRIP JAW; CAPACITY: 20; LENGTH: 250; MATERIAL: CHROME VANADIUM STEEL;",10,"EA"]
["STM-120420","BIT:LG 75","TORK CRAFT HSS TITANIUM STEP DRILL BITS - PRODUCT CODE: TC353043.",15,"EA"]
["STM-120422","WRENCH SET ALLN:HEX, L-SHAPED;10","10 PIECE HEX KEY IDLER ALLEN SET. WRENCH SET, ALLEN: TYPE: HEX, L-SHAPED; SIZE: 2.5; 3; 3.5; 4 ETC; SET QUANTITY: 10; CONTAINER: PLASTIC INDEX HOLDER;",15,"EA"]
["STM-120476","SCREWDRIVER:GP;LG 150;125;ROUND;PHILLIPS","SCHMIDT 6-PIECE SCREWDRIVER SETS - PRODUCT CODE: SCH11001. SCREWDRIVER: TYPE: GENERAL PURPOSE; LENGTH: 150; SHANK LENGTH: 125; SHANK: ROUND; TIP: PHILLIPS; TIP SIZE: 6.5; HANDLE TYPE: PLASTIC; MATERIAL: SHANK CRV; TIP TUNGSTEN CARBIDE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",15,"EA"]
["STM-120480","SAW PWR:MITRE SAW;255;SLIDING;2000","RYOBI SLIDING COMP MITRE SAW 255MM, 2000W. SAW, POWER: TYPE: MITRE SAW; BLADE SIZE: 255; STYLE: SLIDING; RATING: 2000; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",3,"EA"]
["STM-128050","TOOL:SCREW EXTRACTORS;MANUAL;4 TO 22MM","KENNEDY INDUSTRIAL SCREW EXTRACTORS, SET OF 6 - PRODUCT CODE:KEN-075-1160K. TOOL: TYPE: SCREW EXTRACTORS; STYLE: MANUAL; DIMENSIONS: 4 TO 22MM;",10,"EA"]
["STM-128053","BIT TOOL:COMBINATION DRILL;5;HSS","FB 5MM HSS TWIST DRILLS FULLY GROUND - DIN 338 FINISH. BIT, TOOL: TYPE: TWIST DRILL; DIMENSIONS: 5; MATERIAL: HSS GROUND;",150,"EA"]
["STM-128055","BIT TOOL:TWIST DRILL;6;HSS GROUND","FB 6MM HSS TWIST DRILLS FULLY GROUND - DIN 338 FINISH. BIT, TOOL: TYPE: TWIST DRILL; DIMENSIONS: 6; MATERIAL: HSS GROUND;",150,"EA"]
["STM-128056","BIT TOOL:TWIST DRILL;7MM;HSS GROUND","FB 7MM HSS TWIST DRILLS FULLY GROUND - DIN 338 FINISH. BIT, TOOL: TYPE: TWIST DRILL; DIMENSIONS: 7MM; MATERIAL: HSS GROUND;",100,"EA"]
["STM-128059","BIT TOOL:TWIST DRILL;8MM;HSS GROUND","FB 8MM HSS TWIST DRILLS FULLY GROUND - DIN 338 FINISH. BIT, TOOL: TYPE: TWIST DRILL; DIMENSIONS: 8MM; MATERIAL: HSS GROUND;",100,"EA"]
["STM-128063","BIT TOOL:TWIST DRILL;10MM;HSS GROUND","FB 10MM HSS TWIST DRILLS FULLY GROUND - DIN 338 FINISH. BIT, TOOL: TYPE: TWIST DRILL; DIMENSIONS: 10MM; MATERIAL: HSS GROUND;",100,"EA"]
["STM-128065","BIT TOOL:TWIST DRILL;11MM;HSS GROUND","FB 11MM HSS TWIST DRILLS FULLY GROUND - DIN 338 FINISH. BIT, TOOL: TYPE: TWIST DRILL; DIMENSIONS: 11MM; MATERIAL: HSS GROUND;",100,"EA"]
["STM-128067","BIT TOOL:TWIST DRILL;12MM;HSS GROUND","FB 12MM HSS TWIST DRILLS FULLY GROUND - DIN 338 FINISH. BIT, TOOL: TYPE: TWIST DRILL; DIMENSIONS: 12MM; MATERIAL: HSS GROUND;",100,"EA"]
["STM-128068","TAP THRD CUT:M5;66;0.8;HSS","HSS GROUND (M5 X 0.8) SET OF TAPS - MANUFACTURER: FEW. TAP, THREAD CUTTING: TAP SIZE: M5; OVERALL LENGTH: 66; THREAD: 0.8 PITCH; MATERIAL: HSS;",10,"EA"]
["STM-128070","TAP THRD CUT:M6;70;1.0;HSS","HSS SET OF TAPS M6 X 1.0 - MANUFACTURER:FEW. TAP, THREAD CUTTING: TAP SIZE: M6; OVERALL LENGTH: 70; THREAD: 1.0 PITCH; MATERIAL: HSS;",10,"EA"]
["STM-128184","TOOL DBRRNG:CARBIDE;12MM;70MM;HSS","KENNEDY CARBIDE BURR CUT 9; 12 X 25MM - ORDER CODE: KEN-210-0360K. TOOL, DEBURRING: TYPE: CARBIDE; DIAMETER: 12MM; OVERALL LENGTH: 70MM; MATERIAL: HSS;",10,"EA"]
["STM-128186","TOOL DBRRNG:CARBIDE BURR;12MM;75MM;HSS","KENNEDY ROUND TREE CARBIDE BURR CUT 9, 12 X 25MM - ORDER CODE:KEN-210-3320K. TOOL, DEBURRING: TYPE: CARBIDE BURR; DIAMETER: 12MM; OVERALL LENGTH:\n75MM; MATERIAL: HSS;",10,"EA"]
["STM-130451","CROWBAR:1500 X 25MM,NA,LG na","CROWBAR: TYPE: 1500 X 25MM; MATERIAL: NA; LENGTH: na",10,"EA"]
["STM-133336","SCREWDRIVER:TERMINAL,LG 180 MM,100 MM","SCREWDRIVER: TYPE: TERMINAL; LENGTH: 180 MM; SHANK LENGTH: 100 MM; SHANK: ROUND; TIP: SLOTTED; TIP SIZE: 3.5 MM; HANDLE TYPE: PLASTIC",30,"EA"]
["STM-133341","PLIERS DGNL CUTNG:115 MM,YES,YES","PLIERS, DIAGONAL CUTTING: OVERALL LENGTH: 115 MM; INSULATED HANDLE: YES; SHORT NOSE FEATURE: YES",30,"EA"]
["STM-133343","SCREWDRIVER:TERMINAL,LG 160 MM,80 MM,3","SCREWDRIVER: TYPE: TERMINAL; LENGTH: 160 MM; SHANK LENGTH: 80 MM; SHANK: ROUND; TIP: SLOTTED; TIP SIZE: 3 MM; HANDLE TYPE: PLASTIC",30,"EA"]
["STM-133345","SCREWDRIVER:TERMINAL,LG 160 MM,80 MM,1","SCREWDRIVER: TYPE: TERMINAL; LENGTH: 160 MM; SHANKLENGTH: 80 MM; SHANK: ROUND; TIP: PHILLIPS; TIP SIZE: 1 MM; HANDLE TYPE: PLASTIC",30,"EA"]
["STM-133346","KEY:UNIVERSAL SQUARE TRIANGLE KEY,STAR","KEY: TYPE: UNIVERSAL SQUARE TRIANGLE KEY; STYLE: STAR; MATERIAL: ZINC ALLOY STEEL; SPECIFICATION: SILVER SPANNER KEY",30,"EA"]
["STM-134078","CUTTER BLT:NORMAL,COMPOUND,600MM,VARIOUS","CUTTER, BOLT: HEAD TYPE: NORMAL; CUT TYPE: COMPOUND; SIZE: 600MM; MATERIAL: ALLOY STEEL; INSULATED HANDLE: SOFT GRIP STEEL; MATERIAL ACCOMODATED DIAMETER: VARIOUS",10,"EA"]
["STM-135122","SCRAPER:HEAVY DUTY PAINT SCRAPER,75 MM","SCRAPER: TYPE: HEAVY DUTY PAINT SCRAPER; DIMENSIONS: 75 MM; MATERIAL: HEAVY DUTY PAINT SCRAPER",20,"EA"]
["STM-135123","SCRAPER:HEAVY DUTY PAINT SCRAPER,38 MM","SCRAPER: TYPE: HEAVY DUTY PAINT SCRAPER; DIMENSIONS: 38 MM; MATERIAL: HEAVY DUTY PAINT SCRAPER",20,"EA"]
["STM-135479","TAPE MEASNG:5M TAPE MEASURE,5 M","TAPE, MEASURING: TYPE: 5M TAPE MEASURE; DIMENSIONS: 5 M; MATERIAL: MEASURING TAPE",10,"EA"]
["STM-137046","TOOL:FENNER BELT TENSION INDICATOR,n/a","TOOL: TYPE: FENNER BELT TENSION INDICATOR; STYLE: V-BELT; DIMENSIONS: n/a N/A; FENNER V-BELT TENSION INDICATOR TOOL",10,"EA"]
["STM-137120","WRENCH, TAP:WRENCH TAP SET","WRENCH, TAP: TYPE: WRENCH TAP SET; TAP SIZE: SQUARE SIZE: 2.8 - 5MM AND 4.0 - 12MM; TAP WRENCH SET, 2 PIECE.\nSQUARE SIZE: 2.8 - 5MM AND 4.0 - 12MM",50,"EA"]
["STM-137123","WRENCH, TAP:CHUCK STYLE,5 PIECE SET","WRENCH, TAP: TYPE: CHUCK STYLE; TAP SIZE: 5 PIECE SET; CHUCK STYLE TAP WRENCHES, 5 PIECE SET.",10,"EA"]
["STM-137125","EXTRACTOR SET:C-SCREW,6 PIECE","EXTRACTOR SET: TYPE: C-SCREW; QUANTITY: 6 PIECE; EASY OUT SCREW EXTRACTOR SET, 6 PIECE",10,"EA"]
["STM-137130","INSERT THRDG:KORLOY,UNKOWN,LG N/A N/A","INSERT, THREADING: TYPE: KORLOY; THREAD: UNKOWN; LENGTH: N/A N/A; MATERIAL: CARBIDE; TIPS FOR LATHE MACHINE TOOLS.\nSNMG120408-VM NC3120 SNMG432; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",100,"EA"]
["STM-137133","INSERT THRDG:KORLOY/CARMEX,UNKOWN,LG N/A","INSERT, THREADING: TYPE: KORLOY/CARMEX; THREAD: UNKOWN; LENGTH: N/A N/A; MATERIAL: CARBIDE; TIPS FOR LATHE MACHINE TOOLS 16 ER AG60 MXC; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",100,"EA"]
["STM-137136","INSERT THRDG:KORLOY, TRIANGLE,UNKOWN","INSERT, THREADING: TYPE: KORLOY, TRIANGLE; THREAD: UNKOWN; LENGTH: N/A N/A; MATERIAL: CARBIDE; TIPS FOR LATHE MACHINE TOOLS. TNMG 160408-VM TNMG332NC 3120; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",100,"EA"]
["STM-137138","INSERT THRDG:LAYDOWN,UNKOWN,LG N/A N/A","INSERT, THREADING: TYPE: LAYDOWN; THREAD: UNKOWN; LENGTH: N/A N/A; MATERIAL: CARBIDE; TIPS FOR LATHE MACHINE TOOLS\n16 ER AG60 BMA; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",100,"EA"]
["STM-137592","PLIERS VISE GRP:VICE GRIP,LG 175MM MM","PLIERS, VISE GRIP: TYPE: VICE GRIP; CAPACITY: NOT APPLICCABLE MM; LENGTH: 175MM MM",10,"EA"]
["STM-137647","WRENCH:DRIVE RATCHET,1/2 IN,STEEL","WRENCH: TYPE: DRIVE RATCHET; SIZE: 1/2 IN; MATERIAL: STEEL; 1/2 DRIVE RATCHET",10,"EA"]
["STM-137649","EXTENSION TOOL:DRIVE,1/2 IN,LG 250 MM","EXTENSION, TOOL: TYPE: DRIVE; DRIVE SIZE: 1/2 IN; LENGTH: 250 MM",10,"EA"]
["STM-138617","HAMMER:CLUB HAMMER,1.1 KG,UNKNOWN,WOOD","HAMMER: TYPE: CLUB HAMMER; HEAD WEIGHT: 1.1 KG; HEAD MATERIAL: UNKNOWN; HANDLE: WOOD; HAMMER CLUB 1.1KG WOOD HANDLE LAS (6) - WOODEN HANDLE",10,"EA"]
["STM-138982","FILE HND:HALF ROUND BASTARD CUT,LG 250","FILE, HAND: CUT: HALF ROUND BASTARD CUT; CUT DESIGN: BASTARD CUT; SHAPE: HALF ROUND; LENGTH: 250 MM; SIZE: 250MM; TYPE: SAKATA - COURSE - BLISTER PACK WITH HANDLE; FILE H/ROUND BASTARD 250MM SAKATA - COARSE - BLISTER PACK WITH HANDLE",10,"EA"]
["STM-139979","PLIERS VISE GRP:CRV JAW;250 MM;LG N/A","PLIERS, VISE GRIP: TYPE: CRV JAW; CAPACITY: 250 MM; LENGTH: N/A N/A; VICEGRIP CRV JAW 250MM GED - BOTTOM CURVED / TOP JAW STRAIGHT",10,"EA"]
["STM-139981","BIT:SPADE / FLAT;LG 32 x 150 MM;STEEL","BIT: TYPE: SPADE / FLAT; LENGTH: 32 x 150 MM; MATERIAL: STEEL; SPADE DRILL / FLAT DRILL BIT FOR WOOD. \nFLAT BIT 32 X 150MM FB - AMERICAN ASTM SPEC",10,"EA"]
["STM-140041","DRILL:MAKITA IMPACT DRILL 18V;0 MM","DRILL: TYPE: MAKITA IMPACT DRILL 18V; CHUCK SIZE: 0 MM; LENGTH: 22-125 MM; MATERIAL: MAKITA IMPACT DRILL",10,"EA"]
["STM-140070","SET:TORK CRAFT 12 X ROUTER BITS","SET: TYPE: TORK CRAFT 12 X ROUTER BITS; SPECIFICATION: TORK CRAFT; MATERIAL: ROUTER BITS",10,"EA"]
["STM-140071","SCREWDRIVER SET:PHILLIPS SLOTTED;10 PC","SCREWDRIVER, SET: TYPE: CRESCENT 10 PIECE SCREW DRIVER SET; TIP TYPES: PHILLIPS SLOTTED; TIP MATERIAL: CHROME VANADIUM; TIP SIZE RANGE: 10 PIECES; QUANTITY: 10 PC",15,"EA"]
["STM-140074","SET:STANLEY 0-16-159 PIECE CHISEL SET","SET: TYPE: STANLEY 0-16-159 PIECE CHISEL SET; SPECIFICATION: STANLEY; COMPRISING: WOOD CHISEL; SIZE RANGE: 0-16-159           4 PIECE",15,"EA"]
["STM-140079","BIT:TORK CRAFT 13 PIECE SPADE DRILL BITS","BIT: TYPE: TORK CRAFT 13 PIECE SPADE DRILL BITS; LENGTH: 6-25 MM; MATERIAL: STEEL",15,"EA"]
["STM-140081","SET:ALPEN HSS SUPER SET DRILL BITS;21 PC","SET: TYPE: ALPEN HSS SUPER SET DRILL BITS; SPECIFICATION: DRILLING; QUANTITY: 21 PC; MATERIAL: HSS",15,"EA"]
["STM-140086","SET:BLACKSMITH HSS DRILL BITS (1/10MM)","SET: TYPE: BLACKSMITH HSS DRILL BITS (1/10MM); SPECIFICATION: BLACKSMITH; QUANTITY: 10 PC; SIZE RANGE: 1-10 MM; MATERIAL: HSS",15,"EA"]
["STM-140103","SET:GEDORE SPANNER SET 1B/17M","SET: TYPE: GEDORE SPANNER SET 1B/17M; SPECIFICATION: GEDORE",10,"EA"]
["STM-140112","SCKT WRNCH SET:GEODRE D19TMZ SOCKET SET","SOCKET, WRENCH SET: TYPE: GEODRE D19TMZ SOCKET SET; MATERIAL: STEEL; SIZE RANGE: 8-32 MM; SPECIAL FEATURES: COMBINATION; COMPRISING: MANUAL; SPECIFICATION: 19TMZ",10,"EA"]
["STM-140241","BIT MSNRY:DRILL BIT MASONARY;M6;LG 220","BIT, MASONRY: TYPE: DRILL BIT MASONARY; DIAMETER: M6; LENGTH: 220 MM; MATERIAL: DRILL BIT; SHANK: TE-C SDS PLUS",20,"EA"]
["STM-140361","BIT:SPADE / FLAT;LG 18 x 150 MM;STEEL","BIT: TYPE: SPADE / FLAT; LENGTH: 18 x 150 MM; MATERIAL: STEEL; FLAT BIT 18 X 150MM FB - AMERICAN ASTM SPEC\nSPADE DRILL / FLAT DRILL BIT FOR WOOD",10,"EA"]
["STM-140364","BIT:SPADE / FLAT;LG 16 x 150 MM;STEEL","BIT: TYPE: SPADE / FLAT; LENGTH: 16 x 150 MM; MATERIAL: STEEL; FLAT BIT 16 X 150MM FB - AMERICAN ASTM SPEC\nSPADE DRILL / FLAT DRILL BIT FOR WOOD",10,"EA"]
["STM-140366","STONE SHRPNG:OILSTONE, COMBINATION","STONE, SHARPENING: TYPE: OILSTONE, COMBINATION; GRIT: COARSE AND FINE; DIMENSIONS: 200x50x 25 MM; MATERIAL: ALUMINIUM OXIDE;OILSTONE COMB 200X50X25MM FB - COMBINATION SHARPENING STONE",10,"EA"]
["STM-140371","SCREWDRIVER SET:MECHANICS;STEEL;6 PC","SCREWDRIVER, SET: TYPE: MECHANICS; TIP TYPES: SLOT AND CROSS-HEAD; TIP MATERIAL: STEEL; TIP SIZE RANGE: 4 - 8, PH1 - PH2 MM; QUANTITY: 6 PC; S/DRIV SET 6PC GEDORE MEC - SCREWDRIVER SET (MECH) - 6 PIECE\nPH1X80,PH2X100,4X100,5.5X100,6.5X150,8X150",15,"EA"]
["STM-140373","HAMMER:CLAW HAMMER;700 G;STEEL;VINYL","HAMMER: TYPE: CLAW HAMMER; HEAD WEIGHT: 700 G; HEAD MATERIAL: STEEL; HANDLE: VINYL; HAMMER CLAW 700G ESTWING VINYL 24OZ - VINYL GRIP - AMERICAN PATTERN",15,"EA"]
["STM-140375","SAW:HACK JUNIOR;150 MM","SAW: TYPE: HACK JUNIOR; DIMENSIONS: 150 MM; SAW HACK JUNIOR 150MM FB (F-TYPE) - JUNIOR HACK SAW (CARDED)",10,"EA"]
["STM-140379","FRAME HAND HCKSW:STEEL FRAME;STEEL","FRAME, HAND HACKSAW: TYPE: STEEL FRAME; MATERIAL: STEEL; LENGTH: 300 MM; HANDLE MATERIAL: RED KNOB; SAW HACK FRAME 300MM MIT - PROFFESSIONAL - RED KNOB",10,"EA"]
["STM-140380","TOOL:AVIATION SNIP;STRAIGHT;250 MM","TOOL: TYPE: AVIATION SNIP; STYLE: STRAIGHT; DIMENSIONS: 250 MM; AVIATION SNIP 250MM STR (6) STANLEY - STRAIGHT",15,"EA"]
["STM-140382","PLIERS:WATER PUMP;LG 250 MM;STEEL","PLIERS: TYPE: WATER PUMP; LENGTH: 250 MM; HANDLE: STEEL; PLIER WATER PUMP 250MM GEDORE - 7 POSITIONS",10,"EA"]
["STM-140385","CUTTER:TUBE;3-30MM;STEEL","CUTTER: TYPE: TUBE; SIZE: 3-30MM; MATERIAL: STEEL; TUBE CUTTER 3-30MM STAN (10) - STANLEY",10,"EA"]
["STM-140388","CHISEL SET HND:WOOD;4 PC;6 - 25 MM","CHISEL SET, HAND: TYPE: WOOD; QUANTITY: 4 PC; SIZE RANGE: 6 - 25 MM; MATERIAL: STEEL BLADE; CHISEL SET 4 PC STANLEY (2) - 6MM-12MM-18MM-25MM",10,"EA"]
["STM-140390","TROWEL:GAUGING;150 MM","TROWEL: TYPE: GAUGING; BLADE SIZE: 150 MM; TROWEL GAUGING 150MM WOOD HDLFB - WOODEN HANDLE",30,"EA"]
["STM-140396","TAPE MEASNG:STANLEY;5 x 19 MM;TYLON","TAPE, MEASURING: TYPE: STANLEY; DIMENSIONS: 5 x 19 MM; MATERIAL: TYLON; TAPE 5X19MM STANLEY TYLON",30,"EA"]
["STM-140397","HAMMER MLLT:RUBBER;675 G;RUBBER;WOOD","HAMMER, MALLET: TYPE: RUBBER;HEAD WEIGHT: 675 G; HEAD MATERIAL: RUBBER; HANDLE: WOOD; MALLET RUBBER 675G WOOD BLACK FB - WOODEN HANDLE BLACK HEAD",15,"EA"]
["STM-140403","CUTTER GLS:GLASS;DIAMOND CHIP","CUTTER, GLASS: CUTTER TYPE: GLASS; CUTTING END TYPE: DIAMOND CHIP; GLASS CUTTER C/W DIAMOND CHIP",10,"EA"]
["STM-140404","PLANE:JACK","PLANE: TYPE: JACK; PLANE JACK 355 X 50MM STAN - DWS",5,"EA"]
["STM-140555","DRILL:MAKITA IMPACT DRILL 18V;13 MM","DRILL: TYPE: MAKITA IMPACT DRILL 18V; CHUCK SIZE: 13 MM; LENGTH: 410 MM; MATERIAL: MAKITA IMPACT DRILL 18V (DHP453RYE)",5,"EA"]
["STM-140557","CUTTER:MANUAL 60CM DESKTOP TILE CUTTER","CUTTER: TYPE: MANUAL 60CM DESKTOP TILE CUTTER; SIZE: 60CM; MATERIAL: CERAMIC BLADE HEAVY DUTY",5,"EA"]
["STM-140563","POLISHER:1400 W;CONSTANT SPEED N/A","POLISHER: TYPE: BOSCH PROFESSIONAL POLISHER GPO 14 CE; POTENTIAL: 1400 W; SPEED: CONSTANT SPEED N/A; CURRENT: GPO 14 CE N/A",5,"EA"]
["STM-140564","SANDER ELEC:240 WATT;12000;MODEL M9204B","SANDER, ELECTRIC: TYPE: MAKITA RANDOM ORBITAL SANDER 240W; SIZE: 240 WATT; SPEED: 12000; RATING: MODEL M9204B",10,"EA"]
["STM-140569","SANDER:MULTI SANDER TH-OS 1016;EINHELL","SANDER: TYPE: MULTI SANDER TH-OS 1016; SIZE: TH-OS 1016; MATERIAL: EINHELL",5,"EA"]
["STM-140595","SANDER:MAKITA BELT SANDER;940W;M9400B","SANDER: TYPE: MAKITA BELT SANDER; SIZE: 940W; MATERIAL: M9400B",5,"EA"]
["STM-140596","SAW:BOSCH RECIPROCATING SAW;900 W","SAW: TYPE: BOSCH RECIPROCATING SAW; DIMENSIONS: 900 W",5,"EA"]
["STM-140599","KIT:TORCH KIT;SPEC SIEVERT","KIT: TYPE: SIEVERT ROOFING TORCH KIT - GREY/ORANGE; APPLICATION: TORCH KIT; SPECIFICATION: SIEVERT",5,"EA"]
["STM-140601","SCRAPER:245X30X70 MM","SCRAPER: TYPE: SMITH AND CO DELUX SCRAPER -  BROWN; DIMENSIONS: 245X30X70 MM; MATERIAL: SS AND WOODEN HANDLE",30,"EA"]
["STM-140602","SCRAPER:245x100x15 MM","SCRAPER: TYPE: SMITH AND CO DELUX SCRAPER -  BROWN; DIMENSIONS: 245x100x15 MM; MATERIAL: SS AND WOODEN HANDLE",30,"EA"]
["STM-140617","SCRAPER:SPACKLE SET;50/80/100/120 MM","SCRAPER: TYPE: SPACKLE SET; DIMENSIONS: 50/80/100/120 MM; MATERIAL: ALUMINIUM; APPLICATION: HAMILTONS",30,"EA"]
["STM-140621","SCRAPER:80 MM;SS AND WOODEN HANDLE","SCRAPER: TYPE: SMITH AND CO DELUX SCRAPER -  BROWN; DIMENSIONS: 80 MM; MATERIAL: SS AND WOODEN HANDLE",30,"EA"]
["STM-140623","CALLIPER VRNR:GRIP VERNIER CALIPER 150MM","CALLIPER, VERNIER: TYPE: GRIP VERNIER CALIPER 150MM; RANGE: GRIP; GRADUATIONS: GRIP VERNIER CALIPER; MATERIAL: VERNIER CALIPER",10,"EA"]
["STM-141261","BIT TWST:SET;METAL HSS;LG assortment","BIT, TWIST: DIAMETER: assortment 1.0, 1.5, 2.0, 2.5, 3.0, 3.5, 4.0, 4.5, 5.0, 5.5, 6.0, 6.5, 7.0, 7.5, 8.0, 8.5, 9.0, 9.5, 10, 10.5, 11, 11.5, 12, 12.5,13  MM; SHANK: SET; MATERIAL: METAL HSS; LENGTH: assortment",10,"EA"]
["STM-141264","CALLIPER VRNR:DIGITAL;0-150 MM","CALLIPER, VERNIER: TYPE: DIGITAL; RANGE: 0-150 MM; GRADUATIONS: 0.01 MM (2 DECIMALS); MATERIAL: STAINLESS STL",10,"EA"]
["STM-141297","SET:HOLESAW SET IN CASE;SPEC HSS","SET: TYPE: HOLESAW SET IN CASE; SPECIFICATION: HSS; SIZE RANGE: 19, 22, 29, 35, 38, 44, 51, 57, 64   MM",5,"EA"]
["STM-141471","SET","SET: TYPE: 45 PIECE METRIC STEEL TAP & DIE SET IN CASE.; APPLICATION: METRIC COURSE & METRIC FINE COMBINATION; DIE SIZES M6 x 1, M6 x 0.75, M8 x 1.25, M8 x 1, M10 x 1.5, M10 x 1.25, M12 x 1.75, M12 1.5, M14 x 2, M14 x 1.5, M16 x 2, M16 x 1.5, M18 x 2.5, M18 x 1.5, M20 x 2.5, M20 x 1.5, M22 x 2.5, M22 x 1.5, M24 x 3, M24 x 1.5; TAP SIZES 6 x 1, 8 x 1.25, 10 x 1.5, 12 x 1.75, 14 X 2, 16 X 2, 18 X 2.5, 20 x 2.5, 22 x 2.5, 24 x 3, 6 x 0.75, 8 x 1, 10 x 1.25, 12 x 1.5, 14 x 1.5, 16 x 1.5, 18 x 1.5, 20 x 1.5, 20 x 1.5, 22 x 1.5, 25 x 1.5",10,"EA"]
["STM-141627","WRENCH SET:45# CARBON STEEL","WRENCH SET: TYPE: 8 PCE GEAR WRENCH SET WITH FORWARD/REVERSE BUTTON CR-V METRIC SET; SIZE: 72-TEETH CHROME VANADIUM RATCHETING BOX END; MATERIAL: 45# CARBON STEEL; SIZE RANGE: 8, 10, 11, 12, 13, 14, 17, 19 MM",10,"EA"]
["STM-141665","DRILL:1,5/13 MM;LG N/A","DRILL: TYPE: PORTABLE CORDLESS DRILLING MACHINE BOSCH PROFESSIONAL GSB18V-50 CORDLESS IMPACT DRILL 06019H5100; CHUCK SIZE: 1,5/13 MM; LENGTH: N/A; MATERIAL: INCLUDED:2 X BATTERY GBA 18V 2.0AH , CHARGER GAL 18V-20 PROFESSIONAL , L-CASE",5,"EA"]
["STM-141705","SOCKET:1/2 INCH DRIVE DEEP SOCKET","SOCKET: TYPE: 1/2 INCH DRIVE DEEP SOCKET; SIZE: METRIC 16, 19,  23,  24, 26,  27 MM; MATERIAL: CHROME VANADIUM",10,"EA"]
["STM-142166","WRENCH CMBTN:SPANNER;46 MM;LG 440 MM","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 46 MM; LENGTH: 440 MM; STYLE: RING-OPEN END; MATERIAL: CR VANADIUM STL",10,"EA"]
["STM-142167","WRENCH CMBTN:SPANNER;36 MM;LG 420 MM","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 36 MM; LENGTH: 420 MM; STYLE: RING-OPEN END; MATERIAL: CR VANADIUM STL",10,"EA"]
["STM-142187","WRENCH CMBTN:SPANNER;50 MM;LG 505 MM","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 50 MM; LENGTH: 505 MM; STYLE: RING-OPENEND; MATERIAL: CR VANADIUM STL",10,"EA"]
["STM-142191","TOOL:SLOGGING SPANNER;24 MM","TOOL: TYPE: SLOGGING SPANNER; STYLE: HEAVY DUTY RING SLOGGING SPANNER; DIMENSIONS: 24 MM",10,"EA"]
["STM-142192","TOOL:SLOGGING SPANNER;30 MM","TOOL: TYPE: SLOGGING SPANNER; STYLE: HEAVY DUTY RING SLOGGING SPANNER; DIMENSIONS: 30 MM",10,"EA"]
["STM-142193","TOOL:SLOGGING SPANNER;32 MM","TOOL: TYPE: SLOGGING SPANNER; STYLE: HEAVY DUTY RING SLOGGING SPANNER; DIMENSIONS: 32 MM",10,"EA"]
["STM-142222","TOOL:SLOGGING SPANNER;36 MM","TOOL: TYPE: SLOGGING SPANNER; STYLE: HEAVY DUTY RING SLOGGING SPANNER; DIMENSIONS: 36 MM",10,"EA"]
["STM-142223","TOOL:SLOGGING SPANNER;46 MM","TOOL: TYPE: SLOGGING SPANNER; STYLE: HEAVY DUTY RING SLOGGING SPANNER; DIMENSIONS: 46 MM",10,"EA"]
["STM-142224","TOOL:SLOGGING SPANNER;50 MM","TOOL: TYPE: SLOGGING SPANNER; STYLE: HEAVY DUTY RING SLOGGING SPANNER; DIMENSIONS: 50 MM",10,"EA"]
["STM-142239","WRENCH TRQ:1/2 IN;10-50 N M;LINEAR","WRENCH, TORQUE: DRIVE SIZE: 1/2 IN; RATING: 10-50 N M; GRADUATIONS: LINEAR; LENGTH: 325 MM",5,"EA"]
["STM-142247","SCKT WRNCH SET:3/4 INCH;STEEL;22-50 MM","SOCKET, WRENCH SET: TYPE: 3/4 INCH; MATERIAL: STEEL; SIZE RANGE: 22-50 MM",10,"EA"]
["STM-142251","ADAPTOR WRNCH SCKT:3/8 to 1//2 IN;LG 1/2","ADAPTOR, WRENCH SOCKET: DRIVE SIZE: 3/8 to 1//2 IN; LENGTH: 1/2 IN; MATERIAL: HIGH IMPACT STEEL; WRENCH SIZE: 3/8 to 1/2 IN; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",10,"EA"]
["STM-142252","CALLIPER VRNR:DIGITAL VERNIER CALLIPET","CALLIPER, VERNIER: TYPE: DIGITAL VERNIER CALLIPET; RANGE: 0-150 MM; GRADUATIONS: 0.005 MM; MATERIAL: STAINLESS STL",10,"EA"]
["STM-142255","CALLIPER MCRMTR:0-240 MM","CALLIPER, MICROMETER: TYPE: C-35-50MM DIAL BORE GAUGE 240MM DEEP; RANGE: 0-240 MM",5,"EA"]
["STM-142262","KEY:ALLEN KEY SOCKET SET","KEY: TYPE: ALLEN KEY SOCKET SET; STYLE: GED IN19 PM-9 ALLEN KEY SET; MATERIAL: GED IN19 PM-9 ALLEN KEY SET; SPECIFICATION: MM & IN CH MM",10,"EA"]
["STM-142313","DIE:TAP/DIE SET THREADING DIE ASSORTED","DIE: TYPE: TAP/DIE SET THREADING DIE ASSORTED; CONFIGURATION: 45 PCS; DIMENSIONS: M6-M24 MM; THREAD: METRIC SET; MATERIAL: HSS; APPLICATION: TAP & DIE ASSORTED SET",10,"EA"]
["STM-142321","HAMMER:SLEDGE;1.8 KG;STL;RUBBER","HAMMER: TYPE: SLEDGE; HEAD WEIGHT: 1.8 KG; HEAD MATERIAL: STL; HANDLE: RUBBER",10,"EA"]
["STM-142330","PLIERS RETNG RNG:CIRCLIP;LG 85-165 MM","PLIERS, RETAINING RING: TYPE: CIRCLIP; LENGTH: 85-165 MM; RING RANGE: 85-165 MM; TIP STYLE: INSIDE, STRAIGHT",10,"EA"]
["STM-142333","PLIERS RETNG RNG:CIRCLIP;LG 85-165 MM","PLIERS, RETAINING RING: TYPE: CIRCLIP; LENGTH: 85-165 MM; RING RANGE: 85-165 MM; TIP STYLE: OUTSIDE, STRAIGH",10,"EA"]
["STM-142407","TOOL KIT SPEC PURP:TOOL ENGRAVER,;DREMEL","DREMEL RIGHT ANGLE ATTACHMENT (575)",10,"EA"]
["STM-143670","LADDER STEP:HT 1570;ALUMINIUM;6 STP;6","LADDER, STEP: HEIGHT: 1570; MATERIAL: ALUMINIUM; LOAD RATING: 6 STP; STEP QUANTITY: 6; CROSSPIECE TYPE: 6 STEP",15,"EA"]
["STM-143896","BIT MSNRY:HSS JOBBER;16 MM;LG UNKNOWN","BIT, MASONRY: TYPE: HSS JOBBER; DIAMETER: 16 MM; LENGTH: UNKNOWN; MATERIAL: STEEL; SHANK: UNKNOWN; HSS JOBBER DRILL 16.00MM",30,"EA"]
["STM-143897","BIT MSNRY:HSS JOBBER;13 MM;LG UNKNOWN","BIT, MASONRY: TYPE: HSS JOBBER; DIAMETER: 13 MM; LENGTH: UNKNOWN; MATERIAL: STEEL; SHANK: UNKNOWN; HSS JOBBER DRILL 13.00MM",30,"EA"]
["STM-143898","BIT MSNRY:HSS JOBBER;12 MM;LG UNKNOWN","BIT, MASONRY: TYPE: HSS JOBBER; DIAMETER: 12 MM; LENGTH: UNKNOWN; MATERIAL: STEEL; SHANK: UNKNOWN; HSS JOBBER DRILL 12.00MM",30,"EA"]
["STM-143899","BIT MSNRY:HSS JOBBER;10 MM;LG UNKNOWN","BIT, MASONRY: TYPE: HSS JOBBER; DIAMETER: 10 MM; LENGTH: UNKNOWN; MATERIAL: STEEL; SHANK: UNKNOWN; HSS JOBBER DRILL 10.00MM",30,"EA"]
["STM-143900","BIT MSNRY:HSS JOBBER;8 MM;LG UNKNOWN","BIT, MASONRY: TYPE: HSS JOBBER; DIAMETER: 8 MM; LENGTH: UNKNOWN; MATERIAL: STEEL; SHANK: UNKNOWN; HSS JOBBER DRILL 8.0MM",30,"EA"]
["STM-143901","BIT MSNRY:HSS JOBBER;6 MM;LG UNKNOWN","BIT, MASONRY: TYPE: HSS JOBBER; DIAMETER: 6 MM; LENGTH: UNKNOWN; MATERIAL: STEEL; SHANK: UNKNOWN; HSS JOBBER DRILL 6.00MM",100,"EA"]
["STM-143903","BIT MSNRY:HSS JOBBER;3 MM;LG UNKNOWN","BIT, MASONRY: TYPE: HSS JOBBER; DIAMETER: 3 MM; LENGTH: UNKNOWN; MATERIAL: STEEL; SHANK: STRAIGHT; HSS STRAIGHT SHANK JOBBER DRILL 3.00MM",100,"EA"]
["STM-143908","FILE HND:HALF ROUND SECOND ENGINEERS","FILE, HAND: CUT: HALF ROUND SECOND ENGINEERS; CUT DESIGN: SECOND ENGINEERS; SHAPE: HALF ROUND; LENGTH: 250 MM; SIZE: 250MM; TYPE: H/ROUND SECOND ENGINEERS FILE + HANDLE; 250MM (10INCH) H/ROUND SECOND ENGINEERS FILE AND HANDLE",10,"EA"]
["STM-143911","SAW:LOW PROFILE JUNIOR HACKSAW","SAW: TYPE: LOW PROFILE JUNIOR HACKSAW; DIMENSIONS: 27.4X2.3X11.5 CM; KENNEDY LOW PROFILE JUNIOR HACKSAW",10,"EA"]
["STM-143912","SAW:42X2.6X15.5 CM","SAW: TYPE: PROFESSIONAL PLUS CUSHION GRIP HACKSAW; DIMENSIONS: 42X2.6X15.5 CM; KENNEDY PROFESSIONAL PLUS CUSHION GRIP HACKSAW",10,"EA"]
["STM-143917","PLIERS:MULTIGRIP;LG UNKNOWN;145/250","PLIERS: TYPE: MULTIGRIP; LENGTH: UNKNOWN; HANDLE: 145/250; GEDORE 145 / 250 MULTIGRIP PLIERS",10,"EA"]
["STM-143918","BENDER PIPE&CNDT:PIPE BENDER;15-22MM","BENDER, PIPE AND CONDUIT: TYPE: PIPE BENDER; SIZE: 15-22MM; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",10,"EA"]
["STM-143923","CUTTER PIPE:PIPE CUTTER;26-42 MM;26-42MM","CUTTER, PIPE: TYPE: PIPE CUTTER; CUTTING RANGE: 26-42MM; CUTTING MATERIAL: PLASTIC/PVC; PIPE SIZE: 26-42MM",10,"EA"]
["STM-143924","CHISEL SET HND:MTS WOOD;4 PC;UNKNOWN","CHISEL SET, HAND: TYPE: MTS WOOD; QUANTITY: 4 PC; SIZE RANGE: 6, 13, 19, 25 MM; MATERIAL: UNKNOWN; CHISEL MTS WOOD SET 4PC +OIL STONE WZ374",10,"EA"]
["STM-143927","HAMMER MLLT:RUBBER;24 OZ;RUBBER;HICKORY","HAMMER, MALLET: TYPE: RUBBER; HEAD WEIGHT: 24 OZ; HEAD MATERIAL: RUBBER; HANDLE: HICKORY; KENNEDY 24OZ BLACK RUBBER MALLET, HICKORYHANDLE",15,"EA"]
["STM-143931","CUTTER GLS:6-WHEEL;DIAMOND TIP","CUTTER, GLASS: CUTTER TYPE: 6-WHEEL; CUTTING END TYPE: DIAMOND TIP; GLASSCUTTER MTS 6-WHEEL",10,"EA"]
["STM-143943","SCREWDRIVER SET:ENGINEERS;STEEL;UNKNOWN","SCREWDRIVER, SET: TYPE: ENGINEERS; TIP TYPES: SLOT AND CROSS-HEAD; TIP MATERIAL: STEEL; TIP SIZE RANGE: UNKNOWN; QUANTITY: 15 PC; KENNEDY 15PCE ENGINEERS SCREWDRIVER SET",10,"EA"]
["STM-144281","LADDER STEP:HT 3290;STEEL;6 STP;6;6 STEP","LADDER, STEP: HEIGHT: 3290; MATERIAL: STEEL; LOAD RATING: 6 STP; QUANTITY: 1\nEEZEEROLL MOUNT SAFETY STEP; GALVANIZED OR POWDER COATED FINISH; FOOT BRAKE LOCK MECHANISM; STABLE ROBUST CONSTRUCTION; ALL ROUND SAFETY RAILS; MOBILE WITH LOCKING SYSTEM FOR SAFETY; ALL STEEL CONSTRUCTION; NON SLIP SELF CLEANING TREADS; WIDE STAIRWAY TYPE STEPS; TOP STEP HEIGHT: 2560mmx OVERALL HEIGHT: 3290mm x LENGTH X WIDTHBASE DIMENSION: 1865x1140mm; LOCKING SYSTEM:KICK PEDALWITH HANDRAIL",10,"EA"]
["STM-145635","BIT TWST:5.0 MM;MORSE TAPER NO 1;HSS;LG","BIT, TWIST: DIAMETER: 5.0 MM; SHANK: MORSE TAPER NO 1; MATERIAL: HSS; LENGTH: 86.0 MM; TYPE: DRILL BIT; TIP: DRILL; STANDARD: DIN 338",50,"EA"]
["STM-145640","BIT TWST:6.0 MM;MORSE TAPER NO 1;HSS;LG","BIT, TWIST: DIAMETER: 6.0 MM; SHANK: MORSE TAPER NO 1; MATERIAL: HSS; LENGTH: 93.0 MM; TYPE: DRILL BIT; TIP: DRILL; STANDARD: DIN 338",50,"EA"]
["STM-145645","BIT TWST:7.0 MM;MORSE TAPER NO 1;HSS;LG","BIT, TWIST: DIAMETER: 7.0 MM; SHANK: MORSE TAPER NO 1; MATERIAL: HSS; LENGTH: 109.0 MM; TYPE: DRILL BIT; TIP: DRILL; STANDARD: DIN 338",50,"EA"]
["STM-145650","BIT TWST:8.0 MM;MORSE TAPER NO 1;HSS;LG","BIT, TWIST: DIAMETER: 8.0 MM; SHANK: MORSE TAPER NO 1; MATERIAL: HSS; LENGTH: 117.0 MM; TYPE: DRILL BIT; TIP: DRILL; STANDARD: DIN 338",50,"EA"]
["STM-145721","LEVEL:LEVEL - 3 VIAL;1000 MM;3","LEVEL: TYPE: LEVEL - 3 VIAL; DIMENSIONS: 1000 MM; MATERIAL: ALUMINIUM CONSTRUCTION; VIALS: 3",15,"EA"]
["STM-145724","LEVEL:LEVEL - 3 VIAL - FREEMANA;600 MM;3","LEVEL: TYPE: LEVEL - 3 VIAL - FREEMANA; DIMENSIONS: 600 MM; MATERIAL: ALUMINIUM; VIALS: 3",20,"EA"]
["STM-145841","TAPE MEASNG:STANLEY GRIP TAPE MEASURE","TAPE, MEASURING: TYPE: STANLEY GRIP TAPE MEASURE; DIMENSIONS: LG 5 M; MATERIAL: RUBBER CASE",20,"EA"]
["STM-145843","TAPE MEASNG:STANLEY GRIP TAPE MEASURE","TAPE, MEASURING: TYPE: STANLEY GRIP TAPE MEASURE; DIMENSIONS: LG 8 M; MATERIAL: RUBBER CASE\nME05825 MEASURING TAPE SELF LOCK 8M X 25MM S/S & RUBBER CASING MATT FINISH",30,"EA"]
["STM-146028","TOOL KIT SPEC PURP:TOOL ENGRAVER,;DREMEL","TOOL KIT, SPECIAL PURPOSE: COMPRISING: TOOL ENGRAVER,; TYPE: DREMEL; APPLICATION: REPLACEMENT CARTIDE TIP; KIT QUANTITY: 1",10,"EA"]
["STM-146087","TORCH CUTNG:LG 500 MM;BSP 3/8 IN;BRS/SS","TORCH, CUTTING: UNIT TYPE: UNIVERSAL CUTTING TORCH - 90DEG - W005803; COMMERCIAL SIZE: LG 500 MM; CONNECTION TYPE: BSP 3/8 IN; MATERIAL: BRS/SS",10,"EA"]
["STM-146366","DRILL PWR:2800 R/MIN;1.5-13 MM;13 MM;18","DRILL, POWER: TYPE: CORDLESS IMPACT DRILL BOSCH  06019G2102; SPEED: 2800 R/MIN; DRIVE SIZE: 1.5-13 MM; CHUCK SIZE: 13 MM; POWER: 18 V; POTENTIAL: 60 N M; POWER SOURCE: BATTERY",10,"EA"]
["STM-146367","GRINDER:180 LI GRINDER;115 MM","GRINDER: TYPE: CORDLESS BATTERY GRINDER 06019H9022; SIZE: 180 LI GRINDER; DISK SIZE: 115 MM",10,"EA"]
["STM-146369","SCREWDRIVER SET:CHUCK;CARBON STEEL;13 MM","SCREWDRIVER, SET: TYPE: CORDLESS BATTERY DRILL SCREWDRIVER 180-LI; TIP TYPES: CHUCK; TIP MATERIAL: CARBON STEEL; TIP SIZE RANGE: 13 MM; FEATURE: 06019F83KO; HANDLE MATERIAL: PLASTIC; QUANTITY: 1",10,"EA"]
["STM-146371","BLOWER:BLOWER CORDLESS BLOWER 06019F5100","BLOWER: TYPE: BLOWER CORDLESS BLOWER 06019F5100; CAPACITY: 18 V; POWER: 6 A; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-146388","WRNCH & SCKT SET:1;TOOLS","FILE, HAND: CUT: 1ST; CUT DESIGN: 1ST; SHAPE: FLAT FILE; LENGTH: 100 MM; SIZE: AS PER QUOTATION; PATTERN TYPE: AMERICAN; TYPE: FLAT; MANUF P/N: 11101101;",10,"EA"]
["STM-146707","STRIPPER:HAND;0.02 TO 10;1212150","STRIPPER: TYPE: HAND; RANGE: 0.02 TO 10; PHOENIX CONTACT PART NO:1212150",10,"EA"]
["STM-146709","PLIERS:CRIMPING;INSULATED","PLIERS: TYPE: CRIMPING; HANDLE: INSULATED; PHOENIX CONTACT PART NUMBER: 1212045",15,"EA"]
["STM-147050","TOOL:STRIPPING;FAST CONNECTION;N/A ACRE","TOOL: TYPE: STRIPPING; STYLE: FAST CONNECTION; DIMENSIONS: N/A ACRE; SIEMENS PART NO: 6GK1901-1GA00",15,"EA"]
["STM-147470","DEVICE:VICEGRIP;250MM","DEVICE: TYPE: VICEGRIP; APPLICATION: 250MM",10,"EA"]
["STM-150480","PLIERS:FENCING PLIER;LG 260 MM;INSULATED","PLIERS: TYPE: FENCING PLIER; LENGTH: 260 MM; HANDLE: INSULATED; MATERIAL: STEEL",10,"EA"]
["STM-147518","ROLLER PAINT:CLASSIC;225 MM","ROLLER, PAINT: TYPE: CLASSIC; DIAMETER: 225 MM; HAMILTON CLASSIC ROLLER, 225MM; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-147521","ROLLER PAINT:MOHAIR 225;225 MM","ROLLER, PAINT: TYPE: MOHAIR 225; DIAMETER: 225 MM; HAMILTON MOHAIR ROLLER, 225MM; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",30,"EA"]
["STM-147522","SCRAPER:PAINT;75 MM;STEEL","SCRAPER: TYPE: PAINT; DIMENSIONS: 75 MM; MATERIAL: STEEL; HAMILTON SCRAPER, 75MM",20,"EA"]
["STM-147561","WRENCH:OPEN END;22 MM;CHROME VANADIUM","GED7690610 - 7118-22 RECT OPEN END FITTING; WRENCH: TYPE: OPEN END; SIZE: 22 MM; MATERIAL: CHROME VANADIUM; SUPPL P/N: 987654;",20,"EA"]
["STM-147568","WRENCH:OPEN END;24 MM;CHROME VANADIUM","GED7690880 - 7118-24 RECT OPEN END FITTING; WRENCH: TYPE: OPEN END; SIZE: 24 MM; MATERIAL: CHROME VANADIUM; SUPPL P/N: 987654; ",20,"EA"]
["STM-147571","WRENCH:OPEN END;27MM;CHROME VANADIUM","GED7690960 - 7118-27 RECT OPEN END FITTING; WRENCH: TYPE: OPEN END; SIZE: 27MM; MATERIAL: CHROME VANADIUM; SUPPL P/N: 987654;",20,"EA"]
["STM-147572","WRENCH:OPEN END;30MM;CHROME VANADIUM","GED7691260 - 7118-30 RECT OPEN END FITTING; WRENCH: TYPE: OPEN END; SIZE: 30MM; MATERIAL: CHROME VANADIUM; SUPPL P/N: 987654;",20,"EA"]
["STM-147576","WRENCH:OPEN END;32MM;CHROME VANADIUM","GED7687740 - 7118-32 RECT OPEN END FITTING; WRENCH: TYPE: OPEN END; SIZE: 32MM; MATERIAL: CHROME VANADIUM; SUPPL P/N: 987654; ",20,"EA"]
["STM-147609","DRILL:13 MM;LG AS PER ITEM TEXT","BOSCH GSB 16RE 13MM IMPACT DRILL 750W 06012281K1; SUPPL P/N: 14271;",20,"EA"]
["STM-147615","DRILL:CORDLESS IMPACT DRILL;13 MM","DRILL: TYPE: CORDLESS IMPACT DRILL; CHUCK SIZE: 13 MM; BOSCH GSB 180 LI CORDLESS IMPACT DRILL + 1 X 2AH BAT; 06019F83K6; SUPPL P/N: 453935;",30,"EA"]
["STM-147622","GRINDER ELEC:ANGLE;AS PER ITEM TEXT","GRINDER, ELECTRIC: TYPE: ANGLE; BOSCH GWS 9-115 ANGLE GRINDER 900W 06013960K5; SUPPL P/N: 243096",30,"EA"]
["STM-147627","GRINDER:PENCIL;AS PER ITEM TEXT","GRINDER: TYPE: PENCIL; KBE2702543K GM5603 MICRO AIR DIE GRINDER; SUPPL P/N: 16830",35,"EA"]
["STM-147639","WRENCH IMPCT:1/2 IN;PNEUMATIC;NA","WRENCH, IMPACT: DRIVE SIZE: 1/2 IN; POWER SOURCE: PNEUMATIC; KBE2702316P IW500 1/2 INCH AIR IMPACT WRENCH; SUPPL P/N: 16825;",15,"EA"]
["STM-147641","WRENCH IMPCT:3/4 IN;PNEUMATIC;NA","WRENCH, IMPACT: DRIVE SIZE: 3/4 IN; POWER SOURCE: PNEUMATIC; KBE2702325S IW750 3/4 DR AIR IMPACT WRENCH; SUPPL P/N: 16826;",15,"EA"]
["STM-147648","WRENCH IMPCT:1 1/2 IN;PNEUMATIC;NA","WRENCH, IMPACT: DRIVE SIZE: 1 1/2 IN; POWER SOURCE: PNEUMATIC; KBE2701620A 1 DRIVE H/D PISTOL GRIPAIR IMPACT WRENCH; SUPPL P/N: 149481",15,"EA"]
["STM-147795","WHEEL WRE:CUP;ID AS PER ITEM TEXT","Steel Crimped Cup Brush 50MM",20,"EA"]
["STM-147797","WHEEL WRE:CYLINDRICAL;STEEL WIRE","Steel Crimped Cylindrical Brush 40MM",20,"EA"]
["STM-147802","WHEEL WRE:PENCIL BRUSH;STEEL WIRE","Steel Pencil Crimped Brush 22MM",20,"EA"]
["STM-147805","CALLIPER VRNR:CALIPER VERNIER 0-300","CALLIPER, VERNIER: TYPE: CALIPER VERNIER 0-300; RANGE: 0 TO 300 MM; GRADUATIONS: 0.05 MM; MATERIAL: STAINLESS STL;",20,"EA"]
["STM-147808","TOOL:EDGE FINDER;AS PER ITEM TEXT;0.375","KENNEDY EDGE FINDER 10.00MM BODY; CODE:KEN5181420K",20,"EA"]
["STM-147812","TOOL:EDGE FINDER;AS PER ITEM TEXT;0.500","KENNEDY EDGE FINDER 0.375INCH BODY; CODE: KEN5181410K",20,"EA"]
["STM-147814","TOOL:EDGE FINDER;AS PER ITEM TEXT;0.500","KENNEDY EDGE FINDER 0.500INCH BODY; CODE:KEN5181430K",20,"EA"]
["STM-147815","TOOL:EDGE FINDER;AS PER ITEM TEXT;0.500","KENNEDY COMBINATION EDGECENTRE FINDER 0.500INCH BODY; CODE: KEN5181440K",20,"EA"]
["STM-147817","TOOL:EDGE FINDER;AS PER ITEM TEXT;0.500","KENNEDY DOUBLE EDGE FINDER 0.500INCH; CODE: KEN5181460K",20,"EA"]
["STM-147818","TOOL:EDGE FINDER;AS PER ITEM TEXT;10 MM","KENNEDY PLAIN EDGE FINDER 0.500INCH BODY; CODE: KEN5181470K",20,"EA"]
["STM-147913","CALLIPER VRNR:CALIPER VERNIER;0-500 MM","CALLIPER, VERNIER: TYPE: CALIPER VERNIER; RANGE: 0-500 MM; GRADUATIONS: 0.05 MM; MATERIAL: STAINLESS STL; SUPPLIER CODE: AC126-020-11 VERNIER CALIPER",20,"EA"]
["STM-147931","PUNCH SET:CENTRE PUNCH;NA;4","PUNCH, SET: TYPE: CENTRE PUNCH ; RANGE SIZE: NA; MATERIAL: MADE FROM CARBON STEEL; SET QUANTITY: 4; SQUARE HEAD; CODE: KEN5182100K",30,"EA"]
["STM-147934","EXTRACTOR SET:AS PER ITEM TEXT;6 PIECE","EXTRACTOR SET: TYPE: AS PER ITEM TEXT; QUANTITY: 6 PIECE; SCREW EXTRACTOR SET; CODE: KEN0751160K",30,"EA"]
["STM-147937","WRNCH RTCHT DBL SCKT:REVERSAL RATCHET","WRENCH, RATCHET, DOUBLE SOCKET: TYPE: REVERSAL RATCHET; SOCKET SIZE: 1/2 IN; LENGTH: NA; MATERIAL: CHROME VANADIUM; METAL GRIP; CODE: KEN582640K",50,"EA"]
["STM-147942","BAR WRNCH:POWER BAR 1/2 INCH KENNEDY;1/2","BAR, WRENCH: TYPE: POWER BAR 1/2 INCH KENNEDY; DRIVE SIZE: 1/2 IN; LENGTH: 375 MM; MATERIAL: VALADIUM; GROZ POWERBAR",30,"EA"]
["STM-147945","HAMMER:BALL PEIN;2 LB;FIBRE GLASS HANDLE","HAMMER: TYPE: BALL PEIN; HEAD WEIGHT: 2 LB; HEAD MATERIAL: CARBON STEEL DROP-FORGED; HANDLE: FIBRE GLASS HANDLE; CODE: KEN5253500K",30,"EA"]
["STM-147947","HAMMER:DEAD BLOW;20oz OZ;POLYURETHANE","HAMMER: TYPE: DEAD BLOW; HEAD WEIGHT: 20oz OZ; HEAD MATERIAL: POLYURETHANE; HANDLE: FIBRE GLASS HANDLE; CODE: KEN5259440K",30,"EA"]
["STM-147950","HAMMER:DEAD BLOW;40 OZ;POLYURETHANE","HAMMER: TYPE: DEAD BLOW; HEAD WEIGHT: 40 OZ; HEAD MATERIAL: POLYURETHANE; HANDLE: FIBRE GLASS HANDLE; CODE: KEN5259500K",30,"EA"]
["STM-148294","BIT MSNRY:22.0 MM;LG 540 MM;STL","BIT, MASONRY: TYPE: B/S SDS DRILL BIT 22.O X 540MM Q/CUT; DIAMETER: 22.0 MM; LENGTH: 540 MM; MATERIAL: STL; SHANK: DIA 10 MM",30,"EA"]
["STM-148295","DRILL:HILTI HAMMER DRILL BIT TE-Y 20/52","DRILL: TYPE: HILTI HAMMER DRILL BIT TE-Y 20/52; CHUCK SIZE: n/a MM; LENGTH: n/a IN; MATERIAL: N/A",50,"EA"]
["STM-148296","BIT MSNRY:20 MM;LG 540 MM;STL;0","BIT, MASONRY: TYPE: B/S SDS DRILL BIT 20X540MM Q/CUT; DIAMETER: 20 MM; LENGTH: 540 MM; MATERIAL: STL; SHANK: 0",50,"EA"]
["STM-148301","HAMMER:CLAW CARPENTER 600 STEEL H;600","HAMMER: TYPE: CLAW CARPENTER 600 STEEL H; HEAD WEIGHT: 600 ACRE; HEAD MATERIAL: CARPENTRY HAMMER; HANDLE: CARPENTRY HAMMER",40,"EA"]
["STM-148304","TAPE MEASNG:LG 8 M;STANLEY","TAPE, MEASURING: TYPE: STANLEY POWERLOCK TAPE MEASURE; DIMENSIONS: LG 8 M; MATERIAL: STANLEY",40,"EA"]
["STM-148307","SAW:BOSCH JIGSAW GST 650;450 W","SAW: TYPE: BOSCH JIGSAW GST 650; DIMENSIONS: 450 W",20,"EA"]
["STM-148314","WRENCH CMBTN:SPANNER SET;6-32 MM","WRENCH, COMBINATION: TYPE: SPANNER SET; SIZE: 6-32 MM; LENGTH: VARIOUS; STYLE: RING-OPEN END; MATERIAL: GEDORE SPANNER SET",10,"EA"]
["STM-148321","KEY CHUCK:CHUCK AND SDS;13MM","KEY, CHUCK: KEY NUMBER: RUWAG KEY TYPE CHUCK AND SDS ADAPTOR; MATERIAL: CHUCK AND SDS; STYLE DESIGNATOR: 13MM; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-148322","HANDLE, SPANNER WRENCH","HANDLE, SPANNER WRENCH: STYLE DESIGNATOR: COMBINATION SPANNER SIZE: 10MM - METRIC; MATERIAL: GEDORE CHROME VANADUIM; TORQUE: HEAVY DUTY APPLICATION",20,"EA"]
["STM-148323","HANDLE, SPANNER WRENCH","HANDLE, SPANNER WRENCH: STYLE DESIGNATOR: COMBINATION SPANNER SIZE: 13MM - METRIC; MATERIAL: GEDORE CHROME VANADUIM; TORQUE: HEAVY DUTY APPLICATION",20,"EA"]
["STM-148324","HANDLE, SPANNER WRENCH","HANDLE, SPANNER WRENCH: STYLE DESIGNATOR: COMBINATION SPANNER SIZE: 17MM - METRIC; MATERIAL: GEDORE CHROME VANADUIM; TORQUE: HEAVY DUTY APPLICATION",20,"EA"]
["STM-148325","PLIERS:SIDE CUTTERS;LG 200 MM;INSULATED","PLIERS: TYPE: SIDE CUTTERS; LENGTH: 200 MM; HANDLE: INSULATED",20,"EA"]
["STM-148326","SAW HOLE:HSS","SAW, HOLE: SIZE: RS PRO HSS 16MM TO 63MM HOLE SAW SET; ARBOR: STARRETT KDP07051-N 12 PIECE FASTCUT SET; TEETH: HSS; BLADE MATERIAL: BI-METAL INDUSTRIAL HOLE SAW KIT",10,"EA"]
["STM-150469","DRIVER NUT:6 MM NUT SCREWDRIVER;LG 125","DRIVER, NUT: SIZE: 6 MM NUT SCREWDRIVER; LENGTH: 125 MM; SHAFT: SOLID; HANDLE: STEEL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5,"EA"]
["STM-150470","DRIVER NUT:8 MM;LG 125 MM;STEEL;PLASTIC","DRIVER, NUT: SIZE: 8 MM; LENGTH: 125 MM; SHAFT: STEEL; HANDLE: PLASTIC; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5,"EA"]
["STM-150472","DRIVER NUT:10 MM NUT SCREWDRIVER;LG 125","DRIVER, NUT: SIZE: 10 MM NUT SCREWDRIVER; LENGTH: 125 MM; SHAFT: SOLID; HANDLE: STEEL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5,"EA"]
["STM-150473","DRIVER NUT:12 MM NUT SCREWDRIVER;LG 125","DRIVER, NUT: SIZE: 12 MM NUT SCREWDRIVER; LENGTH: 125 MM; SHAFT: STEEL; HANDLE: PLASTIC; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5,"EA"]
["STM-150476","TAPE MEASNG:STANLEY;19 MM;STEEL","TAPE, MEASURING: TYPE: STANLEY; DIMENSIONS: 19 MM; MATERIAL: STEEL",5,"EA"]
["STM-150477","FRAME:JUNIOR HACKSAW;150 MM;STEEL","FRAME: TYPE: JUNIOR HACKSAW; SIZE: 150 MM; MATERIAL: STEEL; SPECIFICATION: HACKSAW",10,"EA"]
["STM-150483","PLIERS:LONG NOSE PLIER;LG 200 MM;STEEL","PLIERS: TYPE: LONG NOSE PLIER; LENGTH: 200 MM; HANDLE: INSULATED; MATERIAL: STEEL",10,"EA"]
["STM-150485","SET:SPANNERS;ALLOY;8-17 MM;TOOL STEEL","SET: TYPE: SPANNERS; SPECIFICATION: ALLOY; SIZE RANGE: 8-17 MM; MATERIAL: TOOL STEEL",10,"EA"]
["STM-150487","PLIERS:SIDE CUTTER;LG 250 MM;STEEL","PLIERS: TYPE: SIDE CUTTER; LENGTH: 250 MM; HANDLE: INSULATED PLASTIC; MATERIAL: STEEL",10,"EA"]
["STM-151116","TROWEL:GAUGING;280 MM","TROWEL: TYPE: GAUGING; BLADE SIZE: 280 MM",10,"EA"]
["STM-151129","TROWEL:TROWEL POINTING;175 MM;PLASTIC","TROWEL: TYPE: TROWEL POINTING; BLADE SIZE: 175 MM; MATERIAL: PLASTIC",10,"EA"]
["STM-151515","SEAL:SILICONE GUN;AS REQUIRED","BIT: TYPE: CORE DRILL; LENGTH: 320 MM; MATERIAL: HILTI; DIAMETER: 16 MM",20,"EA"]
["STM-151517","BIT:CORE DRILL (HILTI);LG 320 MM;HILT","BIT: TYPE: CORE DRILL (HILTI); LENGTH: 320 MM; MATERIAL: HILTI; DIAMETER: 18 MM",20,"EA"]
["STM-151519","BIT:HILTI CORE DRILL BIT;LG 320 MM;HILT","BIT: TYPE: HILTI CORE DRILL BIT; LENGTH: 320 MM; MATERIAL: HILTI; DIAMETER: 20 MM",20,"EA"]
["STM-151522","BIT:HILTI CORE DRILL;LG 320 MM;HILTI;22","BIT: TYPE: HILTI CORE DRILL; LENGTH: 320 MM; MATERIAL: HILTI; DIAMETER: 22 MM",20,"EA"]
["STM-151526","BIT:HILTI CORE DRILL;LG 320 MM;24 MM","BIT: TYPE: HILTI CORE DRILL; LENGTH: 320 MM; MATERIAL: HILTI - 24/320 SP-L; DIAMETER: 24 MM",20,"EA"]
["STM-151528","BIT:HILTI CORE DRILL BIT;LG 320 MM;25 MM","BIT: TYPE: HILTI CORE DRILL BIT; LENGTH: 320 MM; MATERIAL: HILTI - 25/320 SP-L; DIAMETER: 25 MM",20,"EA"]
["STM-151530","BIT:CORE DRILL BIT;LG 320 MM;HILTI;28 MM","BIT: TYPE: CORE DRILL BIT; LENGTH: 320 MM; MATERIAL: HILTI; DIAMETER: 28 MM",20,"EA"]
["STM-151536","BIT:CORE DRILL HILTI;LG 320 MM;30 MM","BIT: TYPE: CORE DRILL HILTI; LENGTH: 320 MM; MATERIAL: HILTI - 30/320 SP-L; DIAMETER: 30 MM",20,"EA"]
["STM-151537","BIT:CORE DRILL (HILTI);LG 320 MM;32 MM","BIT: TYPE: CORE DRILL (HILTI); LENGTH: 320 MM; MATERIAL: HILTI - 32/320 SP-L; DIAMETER: 32 MM",20,"EA"]
["STM-151538","BIT:CORE DRILL HILTI;LG 430 MM;37 MM","BIT: TYPE: CORE DRILL HILTI; LENGTH: 430 MM; MATERIAL: HILTI - B 37/430 P-U ABRAS; DIAMETER: 37 MM",20,"EA"]
["STM-151540","BIT:CORE DRILL (HILTI);LG 430 MM;42 MM","BIT: TYPE: CORE DRILL (HILTI); LENGTH: 430 MM; MATERIAL: HILTI - B 42/430 P-U ABRAS; DIAMETER: 42 MM",20,"EA"]
["STM-151547","BIT:CORE DRILL;LG 430 MM;47 MM","BIT: TYPE: CORE DRILL; LENGTH: 430 MM; MATERIAL: HILTI - B 47/430 P-U ABRAS; DIAMETER: 47 MM",20,"EA"]
["STM-151551","BIT:HILTI CORE DRILL BIT;LG 430 MM;52 MM","BIT: TYPE: HILTI CORE DRILL BIT; LENGTH: 430 MM; MATERIAL: HILTI - B 52/430 P-U ABRAS; DIAMETER: 52 MM",20,"EA"]
["STM-151800","GRINDER:ANGLE;115 MM","GRINDER: TYPE: ANGLE; SIZE: 115 MM",5,"EA"]
["STM-151981","BIT:HILTI HAMMER DRILL BIT;LG 14 MM","BIT: TYPE: HILTI HAMMER DRILL BIT; LENGTH: 14 MM; MATERIAL: SDS MAX",30,"EA"]
["STM-151982","BIT:HILTI HAMMER DRILL BIT;LG 18 MM","BIT: TYPE: HILTI HAMMER DRILL BIT; LENGTH: 18 MM; MATERIAL: SDS MAX",30,"EA"]
["STM-151983","BIT:HILTI HAMMER DRILL BIT;LG 20 MM","BIT: TYPE: HILTI HAMMER DRILL BIT; LENGTH: 20 MM; MATERIAL: SDS MAX",30,"EA"]
["STM-151984","BIT:HILTI HAMMER DRILL BIT;LG 22 MM","BIT: TYPE: HILTI HAMMER DRILL BIT; LENGTH: 22 MM; MATERIAL: SDS MAX",30,"EA"]
["STM-151985","BIT:HILTI HAMMER DRILL BIT;LG 24 MM","BIT: TYPE: HILTI HAMMER DRILL BIT; LENGTH: 24 MM; MATERIAL: SDS MAX",30,"EA"]
["STM-151986","BIT:HILTI HAMMER DRILL BIT;LG 28 MM","BIT: TYPE: HILTI HAMMER DRILL BIT; LENGTH: 28 MM; MATERIAL: SDS MAX",30,"EA"]
["STM-151987","CHISEL:HILTI POINTED CHISEL;TE-SX","CHISEL: TYPE: HILTI POINTED CHISEL; BLADE WIDTH: TE-SX ; LENGTH: 360 MM; MATERIAL: TE-SX SM POINTED",100,"EA"]
["STM-151988","CHISEL:HILTI POINTED CHISEL;TE-SX","CHISEL: TYPE: HILTI POINTED CHISEL; BLADE WIDTH: TE-SX ; LENGTH: 500 MM; MATERIAL: TE-SX SM POINTED",100,"EA"]
["STM-151990","WIRE:BINDING;0.9 MM;LG 50 KG","WIRE: TYPE: BINDING; DIAMETER: 0.9 MM; LENGTH: 50 KG; MATERIAL: BINDING WIRE",5,"EA"]
["STM-151994","BLOWER:BOSCH PROFESSIONAL BLOWER","BLOWER: TYPE: BOSCH PROFESSIONAL BLOWER; CAPACITY: air speed of 270 km/h ACRE; POWER: Battery voltage 18 V; VENDORS ARE RESPONSIBLE FOR ENSURINGTHAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-151995","TOOL:TWISTING FENCE TOOL HOOK REBAR;300","TOOL: TYPE: TWISTING FENCE TOOL HOOK REBAR; STYLE: HOOK TIE WIRE TWISTER; DIMENSIONS: 300 MM; SPECIFICATION: REBAR",20,"EA"]
["STM-151997","DRILL:CORDLESS ROTARY DRILL;n/a MM","DRILL: TYPE: CORDLESS ROTARY DRILL; CHUCK SIZE: n/a MM; LENGTH: n/a IN; MATERIAL: TE 6-A36 CORDLESS ROTARY HAMMER",10,"EA"]
["STM-152004","LEVEL:800 MM;LEVELS","LEVEL: TYPE: STABILA TYPE 70 STANDARD DUTY SPIRIT LEVEL; DIMENSIONS: 800 MM; VIALS: LEVELS",10,"EA"]
["STM-152005","SET:GEDORE D19TMZ SOCKET SET;GEDORE;27","SET: TYPE: GEDORE D19TMZ SOCKET SET; APPLICATION: 8 - 15, 16, 17, 19, 20, 22, 24, 27, 30, 32MM; SPECIFICATION: GEDORE; QUANTITY: 27; COMPRISING: SOCKET HEX",15,"EA"]
["STM-152008","PLIERS DGNL CUTNG:180 MM","PLIERS, DIAGONAL CUTTING: OVERALL LENGTH: 180 MM; SHORT NOSE FEATURE: STANLEY SIDE CUTTER DYNAGRIP PLIER",20,"EA"]
["STM-152009","HAMMER:ESTWING CLAW CARPENTER;E16C","HAMMER: TYPE: ESTWING CLAW CARPENTER; HEAD WEIGHT: E16C; HEAD MATERIAL: 16 OZ CURVED CLAW; HANDLE: SMOOTH FACE GENUINE LEATHER GRIP",10,"EA"]
["STM-152010","PLIERS:STANLEY STHT84113-8 PLIER;LG 200","PLIERS: TYPE: STANLEY STHT84113-8 PLIER; LENGTH: 200 MM; HANDLE: LINESMAN; MATERIAL: PLIER",20,"EA"]
["STM-152012","TAPE:STANLEY POWER LOCK;8M;POWERLOCK","TAPE: TYPE: STANLEY POWER LOCK; DIMENSIONS: 8M; MATERIAL: POWERLOCK",20,"EA"]
["STM-152014","TROWEL:GRIP PLASTERING;290 MM","TROWEL: TYPE: GRIP PLASTERING; BLADE SIZE: 290 MM",20,"EA"]
["STM-152016","PLIERS:STANLEY STHT84167-8;LG 250 MM;STL","PLIERS: TYPE: STANLEY STHT84167-8; LENGTH: 250 MM; HANDLE: CONCRETE PINCERS; MATERIAL: STL",20,"EA"]
["STM-152018","FLOAT:GRIP;float;PLASTIC","FLOAT: TYPE: GRIP; DIMENSIONS: float; MATERIAL: PLASTIC; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)",10,"EA"]
["STM-152020","LEVEL:STANLEY LEVEL BOX 400MM-10;LG 400","LEVEL: TYPE: STANLEY LEVEL BOX 400MM-10; DIMENSIONS: LG 400 MM; MATERIAL: STEEL; VIALS: HORIZONTAL AND VERTICAL",20,"EA"]
["STM-152022","CHISEL:GRIP G21055GR ELECTRICIAN BOLSTER","CHISEL: TYPE: GRIP G21055GR ELECTRICIAN BOLSTER; BLADE WIDTH: n/a; LENGTH: n/a; MATERIAL: ORANGE/BLACK",20,"EA"]
["STM-152023","SQUARE:ROSS F7750 BUILDERS, 600 X 400 MM","SQUARE: TYPE: ROSS F7750 BUILDERS, 600 X 400 MM; MATERIAL: STL",15,"EA"]
["STM-152024","JOINT:JOINTER BRICK LONG SQUARES;8 MM","JOINT: TYPE: JOINTER BRICK LONG SQUARES; DIMENSIONS: 8 MM; MATERIAL: PVC; APPLICATION: VICKERS 52.8",15,"EA"]
["STM-152030","SET:RED 21 SPIECE SPANNER SET;GEODRE","SET: TYPE: RED 21 SPIECE SPANNER SET; SPECIFICATION: GEODRE; QUANTITY: 21 PC; COMPRISING: 380X380X70MM; MATERIAL: TOOL STEEL",10,"EA"]
["STM-153028","TOOL:HUNTINGTON DRESSER HAND TOOL;N/A","TOOL: TYPE: HUNTINGTON DRESSER HAND TOOL; STYLE: N/A; DIMENSIONS: 760 MM; HUNTINGTON DRESSER HAND TOOL #1 - FB - REPAIR WHEEL DIA TO 760MM",10,"EA"]
["STM-153030","BIT MSNRY:HSS JOBBER;5 MM;LG UNKNOWN","BIT, MASONRY: TYPE: HSS JOBBER; DIAMETER: 5 MM; LENGTH: UNKNOWN; MATERIAL: STEEL; SHANK: STRAIGHT; DRILL HSS JOBBER 5.00MM FB - DIN338 - FULLYGROUND - M2 SILVER",50,"EA"]
["STM-153031","BIT MSNRY:HSS JOBBER;4 MM;LG UNKNOWN","BIT, MASONRY: TYPE: HSS JOBBER; DIAMETER: 4 MM; LENGTH: UNKNOWN; MATERIAL: STEEL; SHANK: STRAIGHT; STM-143903",50,"EA"]
["STM-153032","BIT MSNRY:HSS JOBBER;2 MM;LG UNKNOWN","BIT, MASONRY: TYPE: HSS JOBBER; DIAMETER: 2 MM; LENGTH: UNKNOWN; MATERIAL: STEEL; SHANK: STRAIGHT; DRILL HSS JOBBER 2.00MM FB - DIN338 - FULLYGROUND - M2 SILVER",50,"EA"]
["STM-153033","KIT:HOLE SAW KIT;HOLESAW","KIT: TYPE: HOLE SAW KIT; APPLICATION: HOLESAW; HOLE SAW KIT PLASTIC CASE 7PC 16-51MM - 16, 20, 25, 32, 40, 51MM + ARBOURS",10,"EA"]
["STM-153035","SAW HND:5;600 MM;POLY HANDLE;N/A;UNKNOWN","SAW, HAND: THROAT DEPTH: 5; OVERALL LENGTH: 600 MM; HANDLE MATERIAL: POLY HANDLE; DESIGN TYPE: N/A; BLADE TYPE: UNKNOWN; BLADE LENGTH: 600 MM; SAW HAND 600X 5PT RIP LAS (10) - SUPERSAW POLY HANDLE",10,"EA"]
["STM-153036","SAW HND:8;600 MM;POLY HANDLE;N/A;UNKNOWN","SAW, HAND: THROAT DEPTH: 8; OVERALL LENGTH: 600 MM; HANDLE MATERIAL: POLY HANDLE; DESIGN TYPE: N/A; BLADE TYPE: UNKNOWN; BLADE LENGTH: 600 MM; SAW HAND 600X 8PT XCUT #899 (10) - CRAFTSMAN POLY HANDLE",10,"EA"]
["STM-153037","SAW:BACK;300 MM","SAW: TYPE: BACK; DIMENSIONS: 300 MM; SAW BACK 300MM 13 PT STAN (10) - SAWS-BACK",10,"EA"]
["STM-153227","TAPE MEASNG:TAPE MEASURE 5 X 19;5 M","TAPE, MEASURING: TYPE: TAPE MEASURE 5 X 19; DIMENSIONS: 5 M; MATERIAL: STEEL WIT RUBBER GRIP\nME05519 MEASURING TAPE SELF LOCK 5M X 19MM S/S & RUBBER CASING MATT FINISH",10,"EA"]
["STM-155046","PLIERS VISE GRP:VICE GRIP 250MM GEDORE","PLIERS, VISE GRIP: TYPE: VICE GRIP 250MM GEDORE; CAPACITY: 250 MM; ",10,"EA"]
["STM-156513","SQUARE CMBTN:STL;300 MM","SQUARE, COMBINATION: MATERIAL: STL; BLADE LENGTH: 300 MM; GRADUATION UNITS: GRIP GS7651 SQUARE RULER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5,"EA"]
["STM-156532","LEVEL:SPIRIT;LG 300 MM;VERTI/HORI","LEVEL: TYPE: SPIRIT; DIMENSIONS: LG 300 MM; VIALS: VERTI/HORI",10,"EA"]
["STM-156533","SCKT WRNCH SET:GEDORE;GEDORE","SOCKET, WRENCH SET: TYPE: GEDORE RACHET SET 16 PIECE; MATERIAL: GEDORE; SIZE RANGE:  1/4 Socket Set 190 x 110 x 60 MM; SPECIFICATION: GEDORE",10,"EA"]
["STM-156535","SET:POZI BITS 37 PIECE;TORK CRAFT","SET: TYPE: POZI BITS 37 PIECE; SPECIFICATION: TORK CRAFT; COMPRISING: POZI BITS",10,"EA"]
["STM-156536","KEY:TORK CRAFT 18 PIECE ALLEN KEYS","KEY: TYPE: TORK CRAFT 18 PIECE ALLEN KEYS; STYLE: HEX AND TORX; MATERIAL: ALLEN KEYS; SPECIFICATION: 18 PIECE",15,"EA"]
["STM-156537","RIVET:STANLEY RIVET GUN;MEDIUM DUTY IN","RIVET: TYPE: STANLEY RIVET GUN; DIAMETER: MEDIUM DUTY IN; LENGTH: N/A IN; HEAD DIAMETER: N/A IN",10,"EA"]
["STM-156538","LINER:BUILDING LINE;100 M;BUILDING","LINER: TYPE: BUILDING LINE; DIMENSIONS: 100 M; MATERIAL: BUILDING; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-156540","SAW HOLE:TORK CRAFT HOLE SAW BITS SET","SAW, HOLE: SIZE: TORK CRAFT HOLE SAW BITS SET; ARBOR: 13 PIECE CARBON STEEL HOLESAW KIT",10,"EA"]
["STM-156541","TOOL BOX PORTBL:FOLD OPEN WITH HANDLE","TOOL BOX, PORTABLE: TYPE: FOLD OPEN WITH HANDLE; MATERIAL: ALUMINIUM; COLOR: N/A; SIZE: EMPTY TOOLBOX",10,"EA"]
["STM-156543","CROWBAR:LASHER WRECKING CROW BAR;STEEL","CROWBAR: TYPE: LASHER WRECKING CROW BAR; MATERIAL: STEEL; LENGTH: 19 MM",10,"EA"]
["STM-156544","CLAMP:TORK CRAFT G CLAMPS;8\"/200 MM;145","CLAMP: TYPE: TORK CRAFT G CLAMPS; CONDUCTOR SIZE: 8\"/200 MM; MATERIAL: G CLAMP; STANDARD: 240-53113927; MAXIMUM OPERATING POTENTIAL: 145 KV; SPECIFICATION: TORK CRAFT",10,"EA"]
["STM-156549","BLADE:PLANER BLADE SET;20 IN;STEEL","BLADE: TYPE: PLANER BLADE SET; DIMENSIONS: 20 IN; MATERIAL: STEEL; SPECIFICATION: MAC AFRICA; SPECIAL FEATURES: RYOBI MACHINE",10,"EA"]
["STM-156552","SAW:STANLEY HACK SAW;300 MM","SAW: TYPE: STANLEY HACK SAW; DIMENSIONS: 300 MM",10,"EA"]
["STM-156553","BLADE SAW:TORK CRAFT JIG SAW;VARIABLE","BLADE, SAW: SAW TYPE: TORK CRAFT JIG SAW; TOOTH DESIGN: VARIABLE; TEETH PER INCH: n/a; CUT MATERIAL: WOOD",10,"EA"]
["STM-156554","BLADE SAW:TORK CRAFT SKILL SAW BLADES","BLADE, SAW: SAW TYPE: TORK CRAFT SKILL SAW BLADES; TOOTH DESIGN: WOOD; TEETH PER INCH: n/a",20,"EA"]
["STM-156596","BIT:TORK CRAFT 19 X DRILL BITS;LG 110 MM","BIT: TYPE: TORK CRAFT 19 X DRILL BITS; LENGTH: 110 MM; MATERIAL: STEEL",10,"EA"]
["STM-156597","GUN:SILICON GUN","GUN: TYPE: SILICON GUN",10,"EA"]
["STM-156598","SQUARE CMBTN:STANLEY STAINLESS STEEL;300","SQUARE, COMBINATION: MATERIAL: STANLEY STAINLESS STEEL; BLADE LENGTH: 300 MM; GRADUATION UNITS: STEEL; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5,"EA"]
["STM-156602","PUNCH:TORK CRAFT CENTER PUNCHER SET;N/A","PUNCH: TYPE: TORK CRAFT CENTER PUNCHER SET;POINT SIZE: N/A; LENGTH: N/A; MATERIAL: MS",10,"EA"]
["STM-156603","INDICATOR:WATER LEVEL;N/A;N/A;500 MM;N/A","INDICATOR: TYPE: WATER LEVEL; DIMENSIONS: N/A; RANGE: N/A; SCALE: 500 MM; RATING: N/A; SPECIFICATION: STANLEY",5,"EA"]
["STM-156604","HAMMER MLLT:RUBBER;675 G;STEEL;LASHER","HAMMER, MALLET: TYPE: RUBBER; HEAD WEIGHT: 675 G; HEAD MATERIAL: RUBBER COMPOTHANE; HANDLE: STEEL; SPECIFICATION: LASHER",10,"EA"]
["STM-156605","PLIERS:COMBINATION PLIER;PLASTIC COATED","PLIERS: TYPE: COMBINATION PLIER; HANDLE: PLASTIC COATED",10,"EA"]
["STM-156606","TOOL:CUTTER SIDE;HAND;150 MM;STANLEY","TOOL: TYPE: CUTTER SIDE; STYLE: HAND; DIMENSIONS: 150 MM; SPECIFICATION: STANLEY",10,"EA"]
["STM-156607","SCISSORS:STEEL CUTTING SCISSORS SET","SCISSORS: BLADE STYLE: STEEL CUTTING SCISSORS SET; LENGTH: n/a; MATERIAL: STEEL CUTTING; HANDLE TYPE: PLASTIC",5,"EA"]
["STM-156608","SET:S/D INS.BIT SET MULTI 33PCE","SET: TYPE: S/D INS.BIT SET MULTI 33PCE; SPECIFICATION: TORK CRAFT; MATERIAL: FLAT,STAR,SQUARE BIT FOR CORDLESS",5,"EA"]
["STM-156609","DRILL PWR:18 V;N/A;13 MM;18 V;GSB180-LI","DRILL, POWER: TYPE: BOSCH CORDLESS IMPACT DRILL WITH BATTERY; SPEED: 18 V; DRIVE SIZE: N/A; CHUCK SIZE: 13 MM; POWER: 18 V; POTENTIAL: 2AH BATTERY; POWER SOURCE: GSB180-LI",5,"EA"]
["STM-156930","SET:GEDORE SPANNER SET 21 PIECE;GEDORE","SET: TYPE: GEDORE SPANNER SET 21 PIECE; SPECIFICATION: GEDORE; SIZE RANGE: 380X380X70 MM",10,"EA"]
["STM-156940","CHISEL COLD HND:LG 250 MM;25 MM","CHISEL, COLD HAND: LENGTH: 250 MM; BLADE WIDTH: 25 MM; MATERIAL: GRIP COLD CHISEL; TYPE: ORANGE/BLACK",5,"EA"]
["STM-156979","COMB:GRIP BRICK CHISEL HAMMER","COMB: TYPE: GRIP BRICK CHISEL HAMMER; MATERIAL: CODE: GH2551; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",5,"EA"]
["STM-156981","HAMMER:CLAW STEEL HANDLE;500 G;CLAW","HAMMER: TYPE: CLAW STEEL HANDLE; HEAD WEIGHT: 500 G; HEAD MATERIAL: CLAW; HANDLE: STEEL",5,"EA"]
["STM-156982","SCRAPER:50 MM;PLASTIC;BLACK HANDLE","SCRAPER: TYPE:ACADEMY BRUSHWARE SCRAPER WITH HANDLE; DIMENSIONS: 50 MM; MATERIAL: PLASTIC; APPLICATION: BLACK HANDLE",5,"EA"]
["STM-156984","SCRAPER:80 MM;PLASTIC;BLACK HANDLE","SCRAPER: TYPE: ACADEMY BRUSHWARE SCRAPER WITH HANDLE; DIMENSIONS: 80 MM; MATERIAL: PLASTIC; APPLICATION: BLACK HANDLE",5,"EA"]
["STM-156990","TROWEL:ROX TILING TROWEL CARBON;8x8x8 MM","TROWEL: TYPE: ROX TILING TROWEL CARBON; BLADE SIZE: 8x8x8 MM; MATERIAL: ROX TILING",5,"EA"]
["STM-156991","KIT:VICKERS P21 PLASTER HAWK;VICKERS","KIT: TYPE: VICKERS P21 PLASTER HAWK; APPLICATION: HAWKER PLASTER; SPECIFICATION: VICKERS",5,"EA"]
["STM-156993","LEVEL:SPIRIT TYPE 70;LG 800 MM;STEEL","LEVEL: TYPE: SPIRIT TYPE 70; DIMENSIONS: LG 800 MM; MATERIAL: STEEL; VIALS: HORIZONTAL AND VERTICAL",5,"EA"]
["STM-157480","TAPE MEASNG:POWERBLOCK;3 M;STEEL CASE","STANLEY 3M POWERBLOCK MEASURING TAPES FOR ONLINE PLUMBING MAINTENANCE. TAPE, MEASURING: TYPE: POWERBLOCK; DIMENSIONS: 3 M; MATERIAL: STEEL CASE",20,"EA"]
["STM-159561","TOOL:WIRE STRIPPER AND CRIMPER;AUTOMATIC","TOOL: TYPE: WIRE STRIPPER AND CRIMPER; STYLE: AUTOMATIC; DIMENSIONS: 210 MM; 8PK-371D :: AUTOMATIC WIRE STRIPPER & CRIMPER OAL: 21 0MM",30,"EA"]
["STM-159837","BIT:CONE CUTTER;LG 6 x 20 MM;HSS","BIT: TYPE: CONE CUTTER; LENGTH: 6 x 20 MM; MATERIAL: HSS; RS PRO HSS CONE CUTTER 6MM X 20MM; PART NO.: 221-620",5,"EA"]
["STM-159929","LADDER STEP:HT 1.2 M;ALUMINIUM;100 KG","LADDER, STEP: HEIGHT: 1.2 M; MATERIAL: ALUMINIUM; LOAD RATING: 100 KG; STEP QUANTITY: 4 STEP; CROSSPIECE TYPE: A - FRAME; PLATFORM: DOUBLE STEP",10,"EA"]
["STM-159930","LADDER STEP:HT 2 M;ALUMINIUM;120 KG","LADDER, STEP: HEIGHT: 2 M; MATERIAL: ALUMINIUM; LOAD RATING: 120 KG; STEP QUANTITY: 8 STEP; CROSSPIECE TYPE: ALUMINIUM",10,"EA"]
["STM-159931","LADDER:6 STEP LADDER;LG 1800 MM;150 KG","LADDER: TYPE: 6 STEP LADDER; LENGTH: 1800 MM; MATERIAL: ALUMINIUM; LOAD CAPACITY: 150 KG; CROSSPIECE TYPE: ALUMINIUM; CROSSPIECE SURFACE TYPE: PVC",10,"EA"]
["STM-159932","LADDER STEP:HT 1.8 M;ALUMINIUM;150 KG","LADDER, STEP: HEIGHT: 1.8 M; MATERIAL: ALUMINIUM; LOAD RATING: 150 KG; STEP QUANTITY: 6 STEP; CROSSPIECE SURFACE TYPE: ALUMINIUM; CROSSPIECE TYPE: STEPS; PLATFORM: DOUBLE SIDE STEP LADDER; SAFETY FEET: PVC; WIDTH: ±400 MM",10,"EA"]
["STM-159933","LADDER STEP:HT 4 M;ALUMINIUM;135 KG;12","LADDER, STEP: HEIGHT: 4 M; MATERIAL: ALUMINIUM; LOAD RATING: 135 KG; STEP QUANTITY: 12; CROSSPIECE TYPE: A - FRAME; WIDTH: 46.99 CM",6,"EA"]
["STM-160069","WRENCH ADJSTBL:25 MM;LG 200 MM;SHIFTING","SENATOR ADJUSTABLE WRENCH/SHIFTING SPANNER 200MM LONG, REQUIRED FOR MECHANICAL FITTER- PRODUCT CODE:SEN-501-4380K. WRENCH, ADJUSTABLE: JAW CAPACITY: 25 MM; LENGTH: 200 MM; MATERIAL: TOOL STEEL; TYPE: SHIFTING",10,"EA"]
["STM-160073","WRENCH ADJSTBL:36 MM;LG 300 MM","KENNEDY ADJUSTABLE WRENCH/SHIFTING SPANNER 300MM LONG, REQUIRED FOR MECHANICAL FITTER- PRODUCT CODE:KEN 5010-120K. WRENCH, ADJUSTABLE: JAW CAPACITY: 36 MM; LENGTH: 300 MM; MATERIAL: TOOL STEEL; TYPE: SHIFTING SPANNER",10,"EA"]
["STM-160080","PLIERS DGNL CUTNG:256 MM","GEDORE UNIVERSAL PLIERS/WATER PUMP PLIERS 250MM LONG, REQUIRED FOR MECHANICAL FITTER- PRODUCT CODE:GED 6410650.PLIERS, UNIVERSAL: OVERALL LENGTH: 256 MM",5,"EA"]
["STM-160097","WRENCH ADJSTBL:32 MM;LG 255 MM;VICE GRIP","KENNEDY STRAIGHT JAW VICE GRIP WRENCH 255MM LONG, REQUIRED FOR MECHANICAL FITTER- PRODUCT CODE:KEN 5587-100K. WRENCH, ADJUSTABLE: JAW CAPACITY: 32 MM; LENGTH: 255 MM; MATERIAL: CHROME VANADIUM; TYPE: VICE GRIP",10,"EA"]
["STM-160107","SCREWDRIVER:INSULATED;LG 100 MM;50 MM;4","GEDORE STUBBY SLOTTED/FLAT BLACK POINT SCREWDRIVER- 1.0x5.5x25; REQUIRED FOR A MECHANICAL FITTER; PRODUCT CODE:36692. SCREWDRIVER: TYPE: INSULATED; LENGTH: 85MM MM; SHANK LENGTH: 25 MM; SHANK: ROUND; TIP: SLOTTED/FLAT BLACK POINT; TIP SIZE: 1 MM; HANDLE TYPE: PLASTIC; MATERIAL: CHROME VANADIUM MOLYBDENUM STEEL",10,"EA"]
["STM-160109","SCREWDRIVER:GP;LG 85 MM;25 MM;ROUND;PH2","GEDORE STUBBY PHILLIPS BLACK POINT SCREWDRIVER- 2x25; REQUIRED FOR A MECHANICAL FITTER; PRODUCT CODE:36693. SCREWDRIVER: TYPE: GENERAL PURPOSE; LENGTH: 85 MM; SHANK LENGTH: 25 MM; SHANK: ROUND; TIP: PHILLIPS TIP; TIP SIZE: PH2 MM; HANDLE TYPE: HARDENED PLASTIC GRIP; MATERIAL: CHROME VANADIUM MOLYBDENUM STEEL",10,"EA"]
["STM-160113","RULER SCAL:MEASURE;30;1 : 10 MM;LG 300","SENATOR 300MM STEEL RULE,PRODUCT CODE:SEN 5183-620K;REQUIRED FOR A MECHANICAL FITTER. RULER, SCALE: TYPE: MEASURE; NUMBER OF SCALES: 30; SCALE 1: 1 : 10 MM; LENGTH: 300 MM; MATERIAL: STAINLESS STEEL RULER",5,"EA"]
["STM-160115","SCKT WRNCH SET:1/2 INCE DRIVE;6 -32 MM","KENNEDY 30-PIECE KENGRIP SOCKET SET 1/2 INCE DRIVE COMPLETE WITH RATCHET & EXTENTIONS; REQUIRED FOR A MECHANICAL FITTER; PRODUCT CODE:KEN 5828-820K. SOCKET, WRENCH SET: TYPE: 1/2 INCE DRIVE; MATERIAL: CHROME VANADIUM STEEL; SIZE RANGE: 6 -32 MM; SPECIFICATION: N/A",10,"EA"]
["STM-160119","SCKT WRNCH SET:SOCKETS;5-13 MM;ISO 9001","KENNEDY 19-PIECE METRIC SOCKET SET 1/4 INCE DRIVE COMPLETE WITH RATCHET & EXTENTIONS; REQUIRED FOR A MECHANICAL FITTER; PRODUCT CODE:KEN 5824-893K. SOCKET, WRENCH SET: TYPE: SOCKETS; MATERIAL: CHROME VANADIUM STEEL; ",10,"EA"]
["STM-160123","PUNCH PIN:PARALLEL;3 - 8 (5 PIECE) MM;10","SET OF SIX(6) KENNEDY PARALLEL PIN PUNCHES;PRODUCT CODE:KEN-5181-200K, REQUIRED FOR A MECHANICAL FITTER.PUNCH, PIN: TYPE: PARALLEL; POINT DIAMETER: 3 - 10 (6 PIECE) MM; DIAMETER: +- 12MM; OVERALL LENGTH: +-100 MM; MATERIAL: CHROME VANADIUM STEEL; BODY STYLE: PARALLEL PIN PUNCH",5,"EA"]
["STM-160129","CHISEL COLD HND:LG 255 MM;25 MM","KENNEDY COLD FLAT CHISEL 25MMx255MM LONG,PRODUCT CODE:KEN-5056-460K, REQUIRED FOR A MECHANICAL FITTER. CHISEL, COLD HAND: LENGTH: 255 MM; BLADE WIDTH: 25 MM; MATERIAL: STL DROP FORGED",5,"EA"]
["STM-160131","FRAME HAND HCKSW:TUBULAR FRAME;STEEL","SENATOR 300MM ADJUSTABLE HACKSAW FRAME,PRODUCT CODE:SEN-5380-390K, REQUIRED FOR A MECHANICAL FITTER. FRAME, HAND HACKSAW: TYPE: TUBULAR FRAME; MATERIAL: STEEL; LENGTH: 300 MM; HANDLE MATERIAL: ALUMINUM + ABS + TPR",10,"EA"]
["STM-160134","FRAME HAND HCKSW:JUNIOR HACKSAW;LG 150","KENNEDY 150MM JUNIOR HACKSAW FRAMES,PRODUCT CODE:KEN-5380-600K, REQUIRED FOR A MECHANICAL FITTER. FRAME, HAND HACKSAW: TYPE: JUNIOR HACKSAW; MATERIAL: STEEL FRAME; LENGTH: 150 MM; HANDLE MATERIAL: TEMPERED STEEL; STANDARD: SABS APPROVED",10,"EA"]
["STM-160156","SCRIBER:DOUBLE ENDED;180 MM;TOOL STEEL","KENNEDY 180MM DOUBLE ENDED SCRIBERS,PRODUCT CODE:KEN-518-4370K, REQUIRED FOR A MECHANICAL FITTER. SCRIBER: TYPE: DOUBLE ENDED; DIMENSIONS: 180 MM; MATERIAL: TOOL STEEL",10,"EA"]
["STM-160208","WRENCH:SPEED BRACE;1/2 INCH DRIVE","KENNEDY 400MM LONG SPEED BRACERS,PRODUCT CODE:KEN-582-6560K, REQUIRED FOR A MECHANICAL FITTER. WRENCH: TYPE: SPEED BRACE; SIZE: 1/2 INCH DRIVE; MATERIAL: CHROMIUM-VANADIUM ALLOY TOOL STEELS",10,"EA"]
["STM-160211","WRENCH CMBTN:SPANNER SET;6-32 MM","SET x GEDORE COMBINATION SPANNERS - 6 TO 32MM; PRODUCT CODE:609374 No:7//26 M, REQUIRED FOR MECHANICAL FITTER. WRENCH, COMBINATION: TYPE: SPANNER SET; SIZE: 6-32 MM; LENGTH: VARIOUS; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STL",10,"EA"]
["STM-160429","WRENCH TRQ:1/2 IN;80-400NM;0.00;LG NA","WRENCH, TORQUE: DRIVE SIZE: 1/2 IN; RATING: 80-400NM; GRADUATIONS: 0.00; LENGTH: NA;",20,"EA"]
["STM-160431","WRENCH TRQ:3/4 IN;150-800;0.00;LG NA","34662-2DG WRENCH, TORQUE: DRIVE SIZE: 3/4 IN; RATING: 150-800; GRADUATIONS: 0.00; LENGTH: NA;",10,"EA"]
["STM-160432","WRENCH TRQ:3/4 IN;200-1000;0.00;LG NA","34662-3DG WRENCH, TORQUE: DRIVE SIZE: 3/4 IN; RATING: 200-1000; GRADUATIONS: 0.00; LENGTH: NA;",10,"EA"]
["STM-160462","GRINDER ELEC:PENCIL GRINDER;220 V;NA;500","GRINDER, ELECTRIC: TYPE: PENCIL GRINDER; POTENTIAL: 220 V; POWER: 500 W BOSCH GGS 5000 L DIE GRINDER 500W UP TO 8MM",10,"EA"]
["STM-160464","HEAT GUN ELEC:ELECTRIC;220 V;1600 W;NA","HEAT GUN, ELECTRIC: TYPE: ELECTRIC; POTENTIAL: 220 V; POWER: 1600 W; MATERIAL: PLASTIC; SPECIAL FEATURES: NA; BOSCH GHG 180 HEAT GUN 1600W",5,"EA"]
["STM-160476","MACHINE:ENGRAVING;220 V;NA;NA","MACHINE: TYPE: ENGRAVING; POTENTIAL: 220 V; CURRENT: NA; POWER: NA; OSA2799810K ELECTRIC ENGRAVER KIT",15,"EA"]
["STM-160603","PUNCH HOLW:HOLLOW PUNCH SET","PUNCH, HOLLOW: TYPE: HOLLOW PUNCH SET; DIAMETER: na; HOLE DIAMETER: na; KEN5181650K 6PCE HOLLOW PUNCH SET 619MM\\",15,"EA"]
["STM-160612","SCREWDRIVER SET:SCREW DRIVER SET;B;0","SCREWDRIVER, SET: TYPE: SCREW DRIVER SET; TIP TYPES: B; TIP MATERIAL: FULLY HARDEN TIPS; TIP SIZE RANGE: 0; QUANTITY: 6 PC; WERA WER17346 SCREWDRIVER SET B,TIP 6PC CLASSIC",50,"EA"]
["STM-160613","STRAIGHTEDGE:ALUM STRAGHT EDGE RULER;MM","STRAIGHTEDGE: TYPE: ALUM STRAGHT EDGE RULER; GRADUATIONS: MM; LENGTH: 600 MM; WIDTH: 50 MM; THICKNESS: 5 MM; MATERIAL: ALUMINIUM; ME02060 ALUMINIUM STRAIGHT EDGE RULER TYPE B 600X50X5.0MM",20,"EA"]
["STM-160615","STRAIGHTEDGE:STRAIGHT EDGE RULER TYPE B","STRAIGHTEDGE: TYPE: STRAIGHT EDGE RULER TYPE B; GRADUATIONS: MM; LENGTH: 1000 MM; WIDTH: 50 MM; THICKNESS: 5 MM; MATERIAL: ALUMINIUM; ME02100 ALUMINIUM STRAIGHT EDGE RULER TYPE B;1000X50X5.0MM",20,"EA"]
["STM-160617","STRAIGHTEDGE:BUILDERS;NA;LG 2500 MM","STRAIGHTEDGE: TYPE: BUILDERS; GRADUATIONS: NA; LENGTH: 2500 MM; WIDTH: NA; THICKNESS: NA; MATERIAL: ALUMINIUM;",20,"EA"]
["STM-160619","TAPE MEASNG:TAPE MEASURE 3 X 16;3 M","TAPE, MEASURING: TYPE: TAPE MEASURE 3 X 16; DIMENSIONS: 3 M; MATERIAL: STEEL WIT RUBBER GRIP; ME05316 MEASURING TAPE SELF LOCK 3M X 16MM S/S & RUBBER CASING MATT FINISH",30,"EA"]
["STM-160626","FRAME HAND HCKSW:HACK SAW;STEEL FRAME","FRAME, HAND HACKSAW: TYPE: HACK SAW; MATERIAL: STEEL FRAME; LENGTH: 300 MM; HANDLE MATERIAL: STEEL; KENDO KEN30566 HEAVY DUTY HACKSAW 300MM",30,"EA"]
["STM-160644","WRENCH SET ALLN:ALLEN KEY SET;10 PIECES","WRENCH SET, ALLEN: TYPE: ALLEN KEY SET; SIZE: 1/16-3/8 INCH; SET QUANTITY: 10 PIECES;\nCODE: KEN6010970K",40,"EA"]
["STM-160647","SCKT WRNCH SET:SOCKET SET HEX;4 - 55 MM","SOCKET, WRENCH SET: TYPE: SOCKET SET HEX; MATERIAL: CHROME VANADIUM; SIZE RANGE: 4MM X 55MM HEX BIT SOCKET 1/2",10,"EA"]
["STM-160671","BIT DRV SCKT:ALLEN 6 MM;1/2 SQUARE DRIVE","BIT, DRIVE SOCKET: TIP: ALLEN 6 MM; DRIVE SIZE: 1/2 SQUARE DRIVE IN; LENGTH: NA;\nSOCKET BRITO IMPACT ALLENKEY\nCODE: BRI9306",10,"EA"]
["STM-160673","BIT DRV SCKT:ALLEN 24 MM;LG NA","BIT, DRIVE SOCKET: TIP: ALLEN 24 MM; DRIVE SIZE: 3/4  SQUARE DRIVE IN; LENGTH: NA;\nSOCKET BRITO IMPACT ALLENKEY\nCODE: BRI9424",10,"EA"]
["STM-160674","BIT DRV SCKT:ALLEN 27 MM;1 SQUARE DRIVE","BIT, DRIVE SOCKET: TIP: ALLEN 27 MM; DRIVE SIZE: 1 SQUARE DRIVE IN; LENGTH: NA; SOCKET BRITO IMPACT ALLENKEY\nCODE:  BRI9527",10,"EA"]
["STM-160678","LADDER:A-FRAME;LG 1800 MM;ALLUMINIUM;136","LADDER: TYPE: A-FRAME; LENGTH: 1800 MM; MATERIAL: ALLUMINIUM; LOAD CAPACITY: 136 KG; CROSSPIECE TYPE: AL;\nCODE: MTS1848",10,"EA"]
["STM-160685","PAD CSHNNG:KNEE PAD FOAM WITH STRAP","PAD, CUSHIONING: TYPE: KNEE PAD FOAM WITH STRAP; DIMENSIONS: one size fits all MM MM; CUSHIONING MATERIAL: NONSKID MATERIAL; SUPPORT MATERIAL: NONMARRING FACE;\nMTS1792 KNEE PADS MTS",20,"EA"]
["STM-160688","GUN AIR BLW","GUN, AIR BLOW: TYPE: GAV60A AIR BLOW GUN DUSTER IN BLISTER;",40,"EA"]
["STM-160695","HANDLE, SPANNER WRENCH:CHROME VANADIUM","HANDLE, SPANNER WRENCH: STYLE DESIGNATOR: ADJUSTABLE C HOOK WRENCH;1.1/43; MATERIAL: CHROME VANADIUM;",10,"EA"]
["STM-160699","HANDLE, SPANNER WRENCH:CHROME VANADIUM","HANDLE, SPANNER WRENCH: STYLE DESIGNATOR: ADJUSTABLE C HOOK WRENCH; MATERIAL: CHROME VANADIUM; 4.1/2 INCH 6.1/4 INCH (115160MM)ADJ",10,"EA"]
["STM-160717","PLIERS:COMBINATION;LG 200 MM","PLIERS: TYPE: COMBINATION; LENGTH: 200 MM; HANDLE: ALLOY STEEL INSULATED\nCODE:TC533200",40,"EA"]
["STM-160799","PLIERS DGNL CUTNG:190 MM","PLIERS, DIAGONAL CUTTING: OVERALL LENGTH: 190 MM;\nCODE: TC534190",30,"EA"]
["STM-160806","HANDLE SCKT WRNCH:CHROME VANADIUM","HANDLE, SOCKET WRENCH: STYLE DESIGNATOR: KING TONY RATCHET 1 REVERS.800MM; MATERIAL: CHROME VANADIUM;\nCODE:8779-32F",20,"EA"]
["STM-160819","HANDLE SCKT WRNCH:RATCHET 260MM 1/2 DR","HANDLE, SOCKET WRENCH: STYLE DESIGNATOR: RATCHET 260MM 1/2 DR; MATERIAL: CHROME VANADIUM; DRIVE END SHAPE: SQUARE; DRIVE SURFACE SIZE: 1/2 IN;",50,"EA"]
["STM-160821","HANDLE SCKT WRNCH:CHROME VANADIUM;SQUARE","HANDLE, SOCKET WRENCH: STYLE DESIGNATOR: KING TONY RATCHET  REVERS . 500MM; MATERIAL: CHROME VANADIUM; DRIVE END SHAPE: SQUARE; DRIVE SURFACE SIZE: 3/4 IN;",20,"EA"]
["STM-160824","HAMMER:4 LB HAMMER;4 LB;STEEL;RUBBER","HAMMER: TYPE: 4 LB HAMMER; HEAD WEIGHT: 4 LB; HEAD MATERIAL: STEEL; HANDLE: RUBBER;",20,"EA"]
["STM-160832","HANDLE SCKT WRNCH:CHROME VANADIUM;SQUARE","HANDLE, SOCKET WRENCH: STYLE DESIGNATOR: KING TONY POWER BAR 450MM; MATERIAL: CHROME VANADIUM; DRIVE END SHAPE: SQUARE; DRIVE SURFACE SIZE: 1/2 IN;",20,"EA"]
["STM-160833","HANDLE SCKT WRNCH:CHROME VANADIUM;SQUARE","HANDLE, SOCKET WRENCH: STYLE DESIGNATOR: KING TONY POWER BAR 450MM; MATERIAL: CHROME VANADIUM; DRIVE END SHAPE: SQUARE; DRIVE SURFACE SIZE: 3/4 IN;",20,"EA"]
["STM-160836","HANDLE SCKT WRNCH:CHROME VANADIUM;SQUARE","HANDLE, SOCKET WRENCH: STYLE DESIGNATOR: KING TONY POWER BAR 1000MM; MATERIAL: CHROME VANADIUM; DRIVE END SHAPE: SQUARE; DRIVE SURFACE SIZE: 1 IN;",20,"EA"]
["STM-160839","HAMMER:BALL PEIN;32 OZ","HAMMER: TYPE: BALL PEIN; HEAD WEIGHT: 32 OZ; HEAD MATERIAL: CARBON STEEL DROP-FORGED; HANDLE: FIBREGLASS HANDLE 310MM & FULL POL H EAD; CODE: TC607900",40,"EA"]
["STM-160861","HAMMER:DEAD BLOW;1.4 KG;POLYURETHANE","HAMMER: TYPE: DEAD BLOW; HEAD WEIGHT: 1.4 KG; HEAD MATERIAL: POLYURETHANE; HANDLE: FIBRE GLASS HANDLE\nCODE:7851-48",20,"EA"]
["STM-160862","HAMMER:DEAD BLOW;2 KG;POLYURETHANE","HAMMER:DEAD BLOW;2 KG;POLYURETHANE",20,"EA"]
["STM-160863","HAMMER:DEAD BLOW;16 OZ;POLYURETHANE","HAMMER: TYPE: DEAD BLOW; HEAD WEIGHT: 16 OZ; HEAD MATERIAL: POLYURETHANE; HANDLE: FIBRE GLASS HANDLE;\nCODE: TC613450",40,"EA"]
["STM-161418","WRENCH TRQ:LST-2000;1 IN;2000 FT/LBS;NA","1\" DR 2000 FT/LBS WRELESS LITHIUM SERIES II W/CALIBRATIOBN W/CASE; MANUFACTURER: HYTORC",3,"EA"]
["STM-161421","WRENCH TRQ:1 IN;AS PER ITEM TEXT","MXTP-03 1\" SQ DRIVE TORQUE WRENCH; MANUFACTURER: HYTORC",2,"EA"]
["STM-161423","WRENCH TRQ:1 1/2 IN;AS PER ITEM TEXT","MXTP-05 1 1/2\" SQ DRIVE TORQUE WRENCH; MANUFACTURER: HYTORC",2,"EA"]
["STM-161432","PUNCH KNCKOUT:CHASSIS;20 MM;3.5 MM","PUNCH, KNOCKOUT: TYPE: CHASSIS; HOLE SIZE: 20 MM; CAPACITY: 3.5 MM",5,"EA"]
["STM-164974","WRENCH SET ALLN:ALLEN KEY SET;8 PIECES","WRENCH SET, ALLEN: TYPE: ALLEN KEY SET; SIZE: 1.5MM - 8MM; QUANTITY: 8 PIECES;\nSUPPL P/N: KEN6013020K",20,"EA"]
["STM-164983","WHEEL ABRSV:A60 MEDIUM;3160 RPM;ID 31.75","WHEEL, ABRASIVE: GRIT: A60 MEDIUM; SPEED: 3160 RPM; INSIDE DIAMETER: 31.75 MM; OUTSIDE DIAMETER: 150 MM; THICKNESS: 20 MM; ABRASIVE MATERIAL: ALUMINIUM OXIDE; USAGE DESIGN: GENERAL; TYPE: TOOLPOST GRINDER;\nSUPPL P/N: YRK2352095K;",20,"EA"]
["STM-164987","TOOL:CHAMFERRING TOOL;PSSNR-2020K-12","OLDER, MACHINING TOOL: STYLE: PSSNR-2020K-12; HOLDER SIZE: 20 MM; MATERIAL: HARDENED STEEL; TYPE: 45° CHAMFER TOOL;\nMANUFACTURER: ISCAR",20,"EA"]
["STM-164991","HOLDER MACHG TL:PSSNL-2020K-12;;20 MM","HOLDER, MACHINING TOOL: STYLE: PSSNL-2020K-12;; HOLDER SIZE: 20 MM; MATERIAL: HARDENED STEEL; TYPE: 45° CHAMFER TOOL;\nMANUFACTURER: ISCAR",20,"EA"]
["STM-164993","HOLDER MACHG TL:PSSNL 2525 M12;25 MM","HOLDER, MACHINING TOOL: STYLE: PSSNL 2525 M12; HOLDER SIZE: 25 MM; MATERIAL: HARDENED STEEL; TYPE: 45° CHAMFER TOOL;\nMANUFATURER: ISCAR",20,"EA"]
["STM-166790","TOOL KIT:COMBINATION  SET;list","TOOL KIT: TYPE: COMBINATION  SET; DIMENSIONS: list; ROTORK TOOL KIT CONSIST OF:\n1 X 42T-1/8’’ GEDORE HEXAGAN ALLEN KEY (CODE2647354)\n1 X 42T-5/32’’ GEDORE HEXAGAN ALLEN KEY (CODE2647362)\n1 X 42T-3/16’’ GEDORE HEXAGAN ALLEN KEY (CODE2647370)\n1 X 42T-7/32’’ GEDORE HEXAGAN ALLEN KEY (CODE2647388)\n1 X REVERSIBLE RATCHET (1/4’’ KENNEDY ORDER CODE KEN-582-4020K)\n1 X SLIDING T HANDLE ¼’’ (KENNEDY ORDER CODE KEN-582-4040K)\n1 X 50MM EXTENSION BAR (1/4’’ KENNEDY ORDER CODE KEN-582-4060K)\n1 X 250MM EXTENSION BAR (1/4’’ KENNEDY ORDER CODE KEN-582-4120K)\n1 X 1/8’’ HEXAGON SCREWDRIVER BIT 1/4’’ DRIVE (KENNEDY ORDER CODE KEN-582-4840K)\n1 X 5/32’’ HEXAGON SCREWDRIVER BIT 1/4’’ DRIVE (KENNEDY ORDER CODE KEN-582-4850K)\n1 X 3/16’’ HEXAGON SCREWDRIVER BIT 1/4’’DRIVE (KENNEDY ORDER CODE KEN-582-4860K)\n1 X 7/32’’ HEXAGON SCREWDRIVER BIT 1/4’’ DRIVE (KENNEDY ORDER CODE KEN-582-4870K\n1 X BALL DRIVER L-WRENCH 9 PIECE SET INCH (ALLAN KEY SET) (KENNEDY ORDER CODE KEN-602-5730K)",40,"EA"]
["STM-166827","TOOL KIT, GENERAL PURPOSE:CIRCLIP PLIERS","TOOL KIT, GENERAL PURPOSE: TYPE: CIRCLIP PLIERS; COMPRISING: COMBINATION; TOOL KIT CONSIST OF:\nEXTERNAL AND INTERNAL CIRCLIP PLIERS (GEDORE)\n1 X STRAIGHT EXTERNAL CIRCLIP PLIERS GEDORE (CODE: 6701380 NO: 8000-A0)\n1 X STRAIGHT EXTERNAL CIRCLIP PLIERS GEDORE (CODE: 6701460 NO: 8000-A1)\n1 X STRAIGHT EXTERNAL CIRCLIP PLIERS GEDORE (CODE: 6701540 NO: 8000-A2)\n1 X STRAIGHT EXTERNAL CIRCLIP PLIERS GEDORE (CODE: 6701620 NO: 8000-A3)\n1 X STRAIGHT EXTERNAL CIRCLIP PLIERS GEDORE (CODE: 6701700 NO: 8000-A4)\n1 X ANGLED EXTERNAL CIRCLIP PLIERS GEDORE (CODE: 6702270 NO: 8000-A 01)\n1 X ANGLED EXTERNAL CIRCLIP PLIERS GEDORE (CODE: 6702350 NO: 8000 -A 11)\n1 X ANGLED EXTERNAL CIRCLIP PLIERS GEDORE (CODE: 6702430 NO: 8000-A 21)\n1 X ANGLED EXTERNAL CIRCLIP PLIERS GEDORE (CODE: 6702510 NO: 8000-A 31)\n1 X ANGLED EXTERNAL CIRCLIP PLIERS GEDORE (CODE: 6702780 NO: 8000-A 41)\n1 X STRAIGHT INTERNAL CIRCLIP PLIERS GEDORE (CODE: 6703240 NO: 8000-J 0)\n1 X STRAIGHT INTERNAL CIRCLIP PLIERS GEDORE (CODE: 6703320 NO 8000-J 1)\n1 X STRAIGHT INTERNAL CIRCLIP PLIERS GEDORE (CODE: 6703400 NO: 8000-J 2)\n1 X STRAIGHT INTERNAL CIRCLIP PLIERS GEDORE (CODE: 6703590 NO: 8000-J 3)\n1 X STRAIGHT INTERNAL CIRCLIP PLIERS GEDORE (CODE: 6703670 NO: 8000-J 4)\n1 X ANGLE INTERNAL CIRCLIP PLIERS GEDORE (CODE: 6704130 NO: 8000-J01)\n1 X ANGLE INTERNAL CIRCLIP PLIERS GEDORE (CODE: 6704210 NO: 8000-J 11)\n1 X ANGLE INTERNAL CIRCLIP PLIERS GEDORE (CODE: 6704480 NO: 8000-J21)\n1 X ANGLE INTERNAL CIRCLIP PLIERS GEDORE (CODE: 6704560 NO: 8000-J 31)\n1 X ANGLE INTERNAL CIRCLIP PLIERS GEDORE (CODE: 6704640 NO: 8000-J 41)",4,"EA"]
["STM-166828","TOOL KIT, GENERAL PURPOSE:COMBINATION","TOOL KIT, GENERAL PURPOSE: TYPE: REDUCERS AND EXTENSIONS; COMPRISING: COMBINATION; REDUCERS AND EXTENSIONS KIT CONSIST OF:\n1 X REDUCER 3/8’’ TO 1/4’’ (GEDORE CODE 6236280 NO: 3020)\n1 X REDUCER 1/2’’ TO 3/8’’ (GEDORE CODE 6143000 NO: 1930)\n1 X EXTENTION 3/8’’ GEDORE CODE: 6236600 NO:3090/75\n1 X EXTENTION 3/8’’ GEDORE CODE: 6236790 NO: 3090/125\n1 X EXTENTION 3/8’’ GEDORE CODE: 6236870 NO: 3090/250",5,"EA"]
["STM-166829","TOOL:MAGNETC;LIFTER;12 MM","TOOL: TYPE: MAGNETC; STYLE: LIFTER; DIMENSIONS: 12 MM; MAGNATIC LIFTER (GEDORE CODE: 6531280 NO: 640)",5,"EA"]
["STM-166830","PUNCH SET:PUNCHES;6  MM;HARDEND STEEL","PUNCH, SET: TYPE: PUNCHES; RANGE SIZE: 6  MM; MATERIAL: HARDEND STEEL; PUNCH SETS CONSIS OF:\n1 X NUMBER SET GEDORE (CODE – 8605140 NO: 2200-6)\n1 X LETTER SET GEDORE (CODE – 8605220NO: 2201-6)",5,"EA"]
["STM-166832","TOOL:ALLEN KEY 14MM GEDORE;14MM;14 MM","TOOL: TYPE: ALLEN KEY 14MM GEDORE; STYLE: 14MM; DIMENSIONS: 14 MM; ALLEN KEY 14MM GEDORE CODE NUMBER 012214 42L-14",10,"EA"]
["STM-166833","TOOL:ALLEN KEY 17MM GEDORE;17 MM;17 MM","TOOL: TYPE: ALLEN KEY 17MM GEDORE; STYLE: 17 MM; DIMENSIONS: 17 MM; ALLEN KEY 17MM GEDORE CODE 099323 42L-17",10,"EA"]
["STM-166835","PUNCH SET:PUNCHES;various MM","PUNCH, SET: TYPE: PUNCHES; RANGE SIZE: various MM; MATERIAL: HARDEND AND TEMPERED STEEL; PUNCHE SETS CONSIST OF:\n1 X CHISEL AND PUNCH SET IN PVC STAND – 6 PIECES GEDORE (CODE: 8725200 NO: 106)\n1 X DRIFT PUNCH SET IN PVC STAND – 6 PIECES GEDORE (CODE: 8753680 NO: 113)\n1 X PIN PUNCH SET IN PVC STAND – 6 PIECES GEDORE (CODE: 8757670 NO 116A)",10,"EA"]
["STM-166836","TOOL KIT:COMBINATION RATCHET SPANNER SET","TOOL KIT: TYPE: COMBINATION RATCHET SPANNER SET; DIMENSIONS: VARIOUS MM; COMBINATION RATCHET SPANNER GEDORE SET CONSIST OF:\n1 X 8MM COMBINATION RATCHET SPANNER GEDORE CODE 2297051\n1 X 10MM COMBINATION RATCHET SPANNER GEDORE CODE 2297086\n1 X 13MM COMBINATION RATCHET SPANNER GEDORE CODE 2297116\n1 X 15MM COMBINATION RATCHET SPANNER GEDORE CODE2297132\n1 X 17MM COMBINATION RATCHET SPANNER GEDORE CODE 2297159\n1 X 19MM COMBINATION RATCHET SPANNER GEDORE CODE 2297175",10,"EA"]
["STM-167111","TOOL KIT:N/A","TOOL KIT: TYPE: 83 PC MECHANICAL/ ELECTRICAL TOOL KIT; DIMENSIONS: N/A\nSTOCK NUMBER: RSA 1000MB ( DRAPER )\nSUPPLIER: CHRISTENSEN TOOLS",20,"EA"]
["STM-168116","SCREWDRIVER SET:SLOTTED SCREW HOLDING;2","SCREWDRIVER, SET: TYPE: SLOTTED SCREW HOLDING; TIP TYPES: SLOTTED; TIP MATERIAL: STEEL; TIP SIZE RANGE: 3/16 and 1/4 IN; QUANTITY: 2; KLEIN TOOLS 85153K SLOTTED SCREW-HOLDING SCREWDRIVER SET, 3/16-INCH, 1/4-INCH SPLIT-BLADE FLAT HEAT DRIVER,POSITIVE GRIPPING ACTION, 2-PIECE",10,"EA"]
["STM-169786","LADDER STEP:HT 2.4 M;ALUMINIUM;125 KG;8","LADDER, STEP: HEIGHT: 1.2 M; MATERIAL: ALUMINIUM; LOAD RATING: 125 KG; STEP QUANTITY: 4 STEP; CROSSPIECE TYPE: 4 STEP\nMODEL: DASG 4",10,"EA"]
["STM-169787","LADDER STEP:HT 1.8 M;ALUMINIUM;125 KG","LADDER, STEP: HEIGHT: 1.8 M; MATERIAL: ALUMINIUM; LOAD RATING: 125 KG; STEP QUANTITY: 6 STEP; CROSSPIECE TYPE: 6 STEP\nMODEL: DASG 6",10,"EA"]
["STM-169788","LADDER STEP:HT 1.2 M;ALUMINIUM;125 KG","LADDER, STEP: HEIGHT: 2.4 M; MATERIAL: ALUMINIUM; LOAD RATING: 125 KG; STEP QUANTITY: 8; CROSSPIECE TYPE: 8  STEP\nMODEL: DASG 8",10,"EA"]
["STM-170070","TRAY:CLEAN OIL;450x345x50 L","TRAY: TYPE: CLEAN OIL; DIMENSIONS: 450x345x50 L; MATERIAL: ALUMINUIM OR STEEL,NON PLANT\nthe pliers for the inner rings must have straight pins!\nThe pliers for the outer rings must have angled pins\nBuyer to contact me for quote assistant",10,"EA"]
["STM-170071","PLIERS:LG 300 MM;INSULATED LEVER HANDLE","PLIERS: TYPE: OPEN CIRCLIP PLIER; LENGTH: 300 MM; HANDLE: INSULATED LEVER HANDLE; MATERIAL: STL; OPEN CIRCLIP PLIER EXTERNAL,HEAVY DUTY",10,"EA"]
["STM-170072","PLIERS:OPEN CIRCLIP PLIER;LG 300 MM;STL","PLIERS: TYPE: OPEN CIRCLIP PLIER; LENGTH: 300 MM; HANDLE: INSULATED LEVER HANDLE; MATERIAL: STL; OPEN CIRCLIP PLIER EXTERNAL,HEAVY DUTY",10,"EA"]
["STM-170313","TOOL:DUST REMOVAL;MANUAL OPERATED;10 CM","HILTI DUST REMOVAL SYSTEM TE DRS-4-A BOX, REQUIRED FOR CONCRETE DRILLING. TOOL: TYPE: DUST REMOVAL; STYLE: MANUAL OPERATED; DIMENSIONS: 10 CM",10,"EA"]
["STM-170314","HAMMER RTRY:18-22 SQUARE;1700 W;25;MOTOR","SUPPLY 1 x HILTI CORDLESS ROTARY HAMMER TE 4-A22 CASE, REQUIRED FOR CONCRETE DRILLING.",10,"EA"]
["STM-060944","TOOL:SPECIAL TOOL","TOOL: TYPE: SPECIAL TOOL; Fluke ii900 Sonic Industrial Imager",2,"EA"]
["STM-060944","TOOL:SPECIAL TOOL","TOOL: TYPE: SPECIAL TOOL; PAP6600-SIL. SMALL RAM PACKAGE. CONFORMS TO THE MACHINERY DIRECTIVE 2006/42/EC, OPERATING INSTRUCTION WITH CERTIFICATION INCLUDED. INCLUDES AIR ACTIVATED HYDRAULIC PUMP, 10FT (3M) OF HYDRAULIC HOSE W/QUICK CONNECTS, PRESSURE GAGE, CABLE ASSEMBLY, 5 TON (44.5 KN) CAPACITY RAM, AND METAL TOOL BOX. VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",2,"EA"]
["STM-100566","SOCKET SCKT WRNCH","SOCKET, SOCKET WRENCH: DRIVE END SHAPE: SQUARE; DRIVE SURFACE SIZE: 1 IN; CODE:459456; DESCRIPTION: KEN5838850K 46MM DEEP IMPACT SOCKET 1\" SQUARE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-100566","SOCKET SCKT WRNCH","SOCKET, SOCKET WRENCH: DRIVE END SHAPE: SQUARE; DRIVE SURFACE SIZE: 1 IN; CODE:411297; DESCRIPTION: KEN5838851K 50MM DEEP IMPACT SOCKET 1\" SQUARE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-100566","SOCKET SCKT WRNCH","SOCKET, SOCKET WRENCH: DRIVE END SHAPE: SQUARE; DRIVE SURFACE SIZE: 1 IN; CODE:987654; DESCRIPTION: KEN5838853K 55MM DEEP IMPACT SOCKET 1\" SQUARE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-100566","SOCKET SCKT WRNCH","SOCKET, SOCKET WRENCH: DRIVE END SHAPE: SQUARE; DRIVE SURFACE SIZE: 1 IN; CODE:24151; DESCRIPTION: KEN5836630K 60MM DEEP IMPACT SOCKET 1\" SQUARE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-100566","SOCKET SCKT WRNCH","SOCKET, SOCKET WRENCH: DRIVE END SHAPE: SQUARE; DRIVE SURFACE SIZE: 1 IN; CODE:987654; DESCRIPTION: KEN5838856K 65MM DEEP IMPACT SOCKET 1\" SQUARE; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",10,"EA"]
["STM-100779","WRENCH PIPE:.;LG .;STL","WRENCH, PIPE: MATERIAL: STL; CODE:24243; DESCRIPTION:KEN5882180K 18 STILLSON WRENCH; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-100779","WRENCH PIPE:.;LG .;STL","WRENCH, PIPE: MATERIAL: STL; CODE:24242; DESCRIPTION:KEN5882180K 18 STILLSON WRENCH; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",20,"EA"]
["STM-100827","WRENCH CMBTN:SPANNER;AS PER ITEM TEXT","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 10MM; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STL; CODE:23056; DESCRIPTION:KEN5822610K 10MM CHROME VANADIUM COMB SPANNER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100827","WRENCH CMBTN:SPANNER;AS PER ITEM TEXT","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 13MM; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STL; CODE:23059; DESCRIPTION:KEN5822660K 13MM CHROME VANADIUM COMB SPANNER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100827","WRENCH CMBTN:SPANNER;AS PER ITEM TEXT","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 17MM; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STL; CODE:23063; DESCRIPTION:KEN5822700K 17MM CHROME VANADIUM COMB SPANNER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100827","WRENCH CMBTN:SPANNER;AS PER ITEM TEXT","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 21MM; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STL; CODE:23067; DESCRIPTION:KEN5822740K 21MM CHROME VANADIUM COMB SPANNER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100827","WRENCH CMBTN:SPANNER;AS PER ITEM TEXT","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 19MM; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STL; CODE:23065; DESCRIPTION:KEN5822720K 19MM CHROME VANADIUM COMB SPANNER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100827","WRENCH CMBTN:SPANNER;AS PER ITEM TEXT","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 22MM; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STL; CODE:23068; DESCRIPTION:KEN5822750K 22MM CHROME VANADIUM COMB SPANNER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100827","WRENCH CMBTN:SPANNER;AS PER ITEM TEXT","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 24MM; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STL; CODE:23070; DESCRIPTION:KEN5822770K 24MM CHROME VANADIUM COMB SPANNER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100827","WRENCH CMBTN:SPANNER;AS PER ITEM TEXT","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 36MM; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STL; CODE:23077; DESCRIPTION:KEN5822840K 36MM CHROME VANADIUM COMB SPANNER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100827","WRENCH CMBTN:SPANNER;AS PER ITEM TEXT","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 41MM; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STL; CODE:23080; DESCRIPTION:KEN5822870K 41MM CHROME VANADIUM COMB SPANNER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100827","WRENCH CMBTN:SPANNER;AS PER ITEM TEXT","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 46MM; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STL; CODE:23081; DESCRIPTION:KEN5822880K 46MM CHROME VANADIUM COMB SPANNER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE)..",40,"EA"]
["STM-100827","WRENCH CMBTN:SPANNER;AS PER ITEM TEXT","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 50MM; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STL; CODE:23082; DESCRIPTION:KEN5822890K 50MM CHROME VANADIUM COMB SPANNER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100827","WRENCH SET ALLN:BALL END;9;PLASTIC CASE","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 24MM; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STL; CODE:23070; DESCRIPTION:KEN5822770K 24MM CHROME VANADIUM COMB SPANNER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100827","WRENCH SET ALLN:BALL END;9;PLASTIC CASE","WRENCH, COMBINATION: TYPE: SPANNER; SIZE: 36MM; STYLE: RING-OPEN END; MATERIAL: CHROME VANADIUM STL; CODE:23077; DESCRIPTION:KEN5822840K 36MM CHROME VANADIUM COMB SPANNER; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100904","SOCKET:AS PER ITEM TEXT;AS PER ITEM TEXT","SOCKET: TYPE: AS PER ITEM TEXT; SIZE: AS PER ITEM TEXT; MATERIAL: AS PER ITEM TEXT; CODE:384051; DESCRIPTION:KEN5832050K 13MM IMPACT SOCKET 1/2 INCH SQ DR; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100904","SOCKET:AS PER ITEM TEXT;AS PER ITEM TEXT","SOCKET: TYPE: AS PER ITEM TEXT; SIZE: AS PER ITEM TEXT; MATERIAL: AS PER ITEM TEXT; CODE:23852; DESCRIPTION:KEN5832090K 17MM IMPACT SOCKET 1/2 INCH SQ DR; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100904","SOCKET:AS PER ITEM TEXT;AS PER ITEM TEXT","SOCKET: TYPE: AS PER ITEM TEXT; SIZE: AS PER ITEM TEXT; MATERIAL: AS PER ITEM TEXT; CODE:23854; DESCRIPTION:KEN5832110K 19MM IMPACT SOCKET 1/2 INCH SQ DR; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100904","SOCKET:AS PER ITEM TEXT;AS PER ITEM TEXT","SOCKET: TYPE: AS PER ITEM TEXT; SIZE: AS PER ITEM TEXT; MATERIAL: AS PER ITEM TEXT; CODE:23859; DESCRIPTION:KEN5832160K 24MM IMPACT SOCKET 1/2 INCH SQ DR; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-100904","SOCKET:AS PER ITEM TEXT;AS PER ITEM TEXT","SOCKET: TYPE: AS PER ITEM TEXT; SIZE: AS PER ITEM TEXT; MATERIAL: AS PER ITEM TEXT; CODE:384057; DESCRIPTION:KEN5832140K 22MM IMPACT SOCKET 1/2 INCH SQ DR; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).",40,"EA"]
["STM-160642","WRENCH SET ALLN:ALLEN KEY SET;1.5 - 10MM","WRENCH SET, ALLEN: TYPE: SET; SIZE: 5/64 - 1/4; SET QUANTITY: 9 PIECE; SUPPL P/N: KEN6011020K",20,"EA"]
["STM-160642","WRENCH SET ALLN:ALLEN KEY SET;1.5 - 10MM","WRENCH SET, ALLEN: TYPE: ALLEN KEY SET; SIZE: 1.5 - 10MM; SET QUANTITY: 9 PIECES; CODE: KEN6012970K",40,"EA"]
["STM-160676","CHISEL COLD HND:LG ASPER ITEM TEXT","KEN5051600K 6 X 100MM FLAT COLD CHISEL",30,"EA"]
["STM-160676","CHISEL COLD HND:LG ASPER ITEM TEXT","KEN5053260K 12 X 255MM FLAT COLD CHISEL",30,"EA"]
["STM-160692","WRENCH CMBTN:COMBINATION SPANNER;NA","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 10MM; LENGTH: NA; STYLE: OFFSET; MATERIAL: CHROME VANADUIM;",50,"EA"]
["STM-160692","WRENCH CMBTN:COMBINATION SPANNER;NA","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 13MM; LENGTH: NA; STYLE: OFFSET; MATERIAL: CHROME VANADUIM;",50,"EA"]
["STM-160692","WRENCH CMBTN:COMBINATION SPANNER;NA","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 17MM; LENGTH: NA; STYLE: DEEP OFFSET; MATERIAL: CHROME VANADUIM;",50,"EA"]
["STM-160692","WRENCH CMBTN:COMBINATION SPANNER;NA","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 19MM; LENGTH: NA; STYLE: DEEP OFFSET; MATERIAL: CHROME VANADUIM;",50,"EA"]
["STM-160692","WRENCH CMBTN:COMBINATION SPANNER;NA","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 24MM; LENGTH: NA; STYLE: DEEP OFFSET; MATERIAL: CHROME VANADUIM;",50,"EA"]
["STM-160692","WRENCH CMBTN:COMBINATION SPANNER;NA","WRENCH, COMBINATION: TYPE: COMBINATION SPANNER; SIZE: 27MM; LENGTH: NA; STYLE: DEEP OFFSET; MATERIAL: CHROME VANADUIM;",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","32mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","36mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","40mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","41mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","46mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","14 X 18-32mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 643",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","14 X 18-34mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 643",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","14 X 18-36mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 643",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","14 X 18-38mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 643",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","14 X 18-41mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 643",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","19mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","20mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","21mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","22mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","23mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","24mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","26mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","27mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","28mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","30mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 642",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","32mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 644",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","34mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 644",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","36mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 644",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","41mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 644",50,"EA"]
["STM-161779","WRENCH OPN END:CHROME VANADIUM STEEL","46mm-OPEN JAW WRENCHES FOR TORQUE BARS TYPE: 644",50,"EA"]
["STM-147953","CROWBAR:TOMMY BAR;HEAVY DUTY STEEL;LG","CROWBAR: TYPE: TOMMY BAR; MATERIAL: HEAVY DUTY STEEL; LENGTH: 600 MM; CODE: AFT0205",50,"EA"]
["STM-147953","CROWBAR:TOMMY BAR;HEAVY DUTY STEEL;LG","CROWBAR: TYPE: TOMMY BAR; MATERIAL: HEAVY DUTY STEEL; LENGTH: 450 MM; CODE: AFT0200",20,"EA"]