{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["0638563","Deviation Schedules","Test Schedules"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"0638563","index":0,"n_rows":71,"n_cols":7,"rows_kept":71,"merged":[[0,0,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,1,4,6],[5,1,5,6],[7,2,7,3],[8,2,8,3],[9,3,9,4],[18,3,18,4],[27,3,27,4],[40,3,40,4],[45,3,45,4],[49,2,49,4],[50,2,50,4],[51,3,51,4],[54,3,54,4],[62,1,62,6],[63,0,63,6],[64,1,64,6],[66,0,66,1],[67,5,67,6],[70,2,70,3],[70,5,70,6]]}
["ESKOM TENDER E2719DXLIMOU"]
[null,"NOTE:  The application of Bird Diverters to the network are installed in alternating colours.  The procurement must be in equal numbers per colour, therefore via both SAP numbers."]
[null,"Technical Schedules A and B for"]
[null,"BIRD DIVERTER: FLAPPER; BLK; SQ-CENT - D3053"]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No",null,{"v":638563,"d":"0638563"},"xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer's Name",null,"xxxxxxxxxx"]
[null,"1.1.3",null,"Manufacturer's Product Code",null,"xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Drawing number & Revision number",null,"xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's Physical identification mark on product",null,"xxxxxxxxxx"]
[null,"1.1.6",null,"Compliance to all dimensions and requirements of Eskom Buyer's Guide drawing","D-DT 3053","YES"]
[null,"1.1.7",null,"Item sample required, upon request from Eskom. (As per the Technical Criteria Document)",null,"YES","xxxxxxxxxx"]
[]
[null,"1.2","·","Mechanical Properties - Clamp"]
[null,"1.2.1",null,"Material Grade - Main body",null,"UV Stable High impact PVC"]
[null,"1.2.2",null,"Material Grade - All Steel Components",null,"SS Grade 304"]
[null,"1.2.3",null,"Conductor range - Squirrel to Centipede","mm","6.33 - 26.46"]
[null,"1.2.4",null,"Jaws of Clamp secured with two Stainless Steel Springs",null,"Comply"]
[null,"1.2.5",null,"Neoprene Pad situated on inside of Clamp Jaws",null,"Comply"]
[null,"1.2.6",null,"Clamp Movement on conductor",null,"Fixed, No Movement"]
[null,"1.2.7",null,"Application via Link Stick using a standard attachment",null,"YES"]
[]
[null,"1.3","·","Mechanical Properties - Flapper"]
[null,"1.3.1",null,"Material Grade - Flapper",null,"UV Stable High impact PVC"]
[null,"1.3.2",null,"Material Grade - All Steel Components",null,"SS Grade 304"]
[null,"1.3.3",null,"Flapper size - Outside diameter","mm","130-150"]
[null,"1.3.4",null,"Reflective tape on both sides of flapper (Polymeric or Vinyl Tape)",null,"Comply"]
[null,"1.3.5",null,"Flapper Movement below Clamping Device",null,"One Directional"]
[null,"1.3.6",null,"Flapper Movement Restriction - Remain below Clamp, cannot Flip over line",null,"Comply"]
[null,"1.3.7",null,"Flapper to Clamp attachment - Stainless steel bolt",null,"Yes"]
[null,"1.3.8",null,"Flapper to Clamp attachment - Stainless steel bolt size","mm",5]
[null,"1.3.9",null,"Flapper to Clamp attachment - Stainless steel Nylock nut",null,"Yes"]
[null,"1.3.10",null,"Flapper - Grommet for bolt",null,"Yes"]
[null,"1.3.11",null,"Flapper Colour - (SAP 0638563)",null,"BLACK"]
[]
[null,"1.4","·","Material Dimensions"]
[null,"1.4.1",null,"Overall size - Effective visual area","cm2",200]
[null,"1.4.2",null,"Flapper size - Outside diameter","mm","130-150"]
[null,"1.4.3",null,"Overall Weight - Flapper and Clamping mechanism","g","≤500"]
[]
[null,"1.5","·","Marking and Packaging"]
[null,"1.5.1",null,"Indellible manufacuterers code on both Clamp and Flapper",null,"Yes"]
[null,"1.5.2",null,"Preferred method of packing",null,"Individual or collective"]
[]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to be provided in electronic format."]
[null,"2.1","·","General"]
[null,"2.1.1",null,"Outline drawings of item","Sets",1]
[null,"2.1.2",null,"Material grade certification","Certification submitted","YES"]
[null,"2.2","·","Test Reports (where applicable)",null,"Required","Report Number"]
[null,"2.2.1",null,"Visual examination\n[SANS61284]","Test report submitted","YES"]
[null,"2.2.2",null,"Dimensional and material verification \n[SANS61284]","Test report submitted","YES"]
[null,"2.2.3",null,"Slip Test\n[240-170000340 and SANS61284]","Test report submitted","YES"]
[null,"2.2.4",null,"Salt fog test for 1000 hours\n[240-170000340 and SANS9227]","Test report submitted","YES"]
[null,"2.2.5",null,"UV Stability\n[240-170000340 and ISO4892-3]","Test report submitted","YES"]
[null,"2.2.6",null,"Season Cycle trial - Mechanical and Environmental\n[240-170000340 and 240-119185951]","Test report submitted","YES"]
[]
[null,"NOTE:  DEVIATION SCHEDULE CONTINUE ON NEXT PAGE.\n             IF NO DEVIATIONS ARE MENTIONED ON THE DEVIATION SCHEDULE IT WILL BE ACCEPTED THAT THE SUPPLIER\n              AND MANUFACTURER FULLY COMPLIES WITH THE REQUIREMENTS OF THE ESKOM SPECIFICATON(S)."]
["ESKOM TENDER E2719DXLIMOU"]
[null,"SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company Name"]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Deviation Schedules","index":1,"n_rows":45,"n_cols":5,"rows_kept":45,"merged":[[0,0,0,6],[1,0,1,6],[4,2,4,3],[5,0,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[34,2,34,6],[35,2,35,6],[36,2,36,6],[37,0,37,6],[38,0,38,6],[40,0,40,1],[41,0,41,1],[41,4,41,5],[44,4,44,5]]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation schedule D-DT 3053 "]
["Description:",null,"                          BIRD DIVERTER: FLAPPER; BLK; SQ-CENT - D3053"]
["SAP No:",null,{"v":638563,"d":"0638563"}]
[]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":30}
["ESKOM TENDER E2719DXLIMOU"]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[null,null,"Name (Print)",null,"Company Name"]
[]
[null,null,"         "]
[null,null,"Sign",null,"Date"]

{"sheet":"Test Schedules","index":2,"n_rows":22,"n_cols":6,"rows_kept":22,"merged":[[0,0,0,7],[2,1,2,6],[5,2,5,3],[13,1,13,6],[14,0,14,6],[16,0,16,1],[17,5,17,6],[21,2,21,3],[21,5,21,6]]}
["ESKOM TENDER E2719DXLIMOU"]
[]
[null,"Test Report Schedule D-DT 3053  (Insert item description below)"]
[null,"Description:",null,"                          BIRD DIVERTER: FLAPPER; BLK; SQ-CENT - D3053"]
[null,"SAP No:",null,{"v":638563,"d":"0638563"}]
[]
[null,"2.2.1",null,"Visual examination","Type","SANS61284"]
[null,"2.2.2",null,"Dimensional and material verification ","Type","SANS61284"]
[null,"2.2.3",null,"Slip Test","Type","240-170000340\nSANS61284"]
[null,"2.2.4",null,"Salt fog test for 1000 hours","Type","240-170000340\nSANS9227"]
[null,"2.2.5",null,"UV Stability","Type","240-170000340\nISO 4892-3"]
[null,"2.2.6",null,"Season Cycle trial - Mechanical and Environmental","Type","240-170000340\n240-119185951"]
[]
[null,"ESKOM TENDER E2719DXLIMOU"]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company Name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]