{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":64,"n_cols":7,"rows_kept":64,"merged":[[11,0,11,5],[32,0,32,4],[49,0,49,4]]}
[]
[null,null,"SUPPLY AND INSTALLATION THE VANDALIZED P6 TRU, STEEL HOUSING AND THE CLEARVU FENCE"]
[]
[null,"SCHEDULE  1: PRELIMINARY AND GENERAL"]
[]
["ITEM NO.","PAYMENT REF.","ITEM DESCRIPTION","UNIT","QTY","RATE (R) ","AMOUNT(R) "]
[1,"SABS 1200A","PRELIMINARY AND GENERAL"]
[null,"8.3.2","Establish Facilities on the Site :"]
[1.1,null,"Provision and compliance with health and safety plan and requirements for the duration of the work, including safety file and Covid 19 Compliance","sum",1]
[1.2,null,"Plant","sum",1]
[1.3,"8.4.3","Supervision for the duration of construction work, i.e. Engineer, safety officer, foreman, etc.","sum",1]
["TOTAL AMOUNT, Excluding 14% VAT"]
[]
[]
[null,"SCHEDULE 2: Supply and Installation of the AC Cable and Kiosk   "]
["                                               "]
["ITEM NO.","PAYMENT REF.","ITEM DESCRIPTION","UNIT","QTY","RATE (R) ","AMOUNT(R) "]
[2.1,null,"Detection of underground foreign services using a suitable machine / tools up to 1m depth","m",100]
[2.2,null,"Excavate, trench, backfill and compaction ","m3",23]
[2.3,null,"Install four core 4 x 16 mm2 ac cable (Rand Water to supply cable)","m",100]
[2.7,null,"Excavate, trench, backfill and compaction ","m3",2]
[2.8,null,"Installation of kiosk plinth (1.5m x 1m x 0.5m deep)","No.",1]
[2.9,null,"Supply and install a kiosk ","No.",1]
[2.1,null,"Supply Փ110mm PVC pipe (conduit)","m",32]
[2.11,null,"Install Փ110mm PVC pipe (conduit) inside the kiosk","m",2]
[2.13,null,"Supply 15MPA ready mix concrete","m3",8]
[2.14,null,"Apply 15MPA ready mix concrete over 100m trench of 300mm width","No.",1]
[2.15,null,"Supply 3 phase 80A circuit breaker complete with holder","No.",1]
[2.16,null,"Install 3 phase 80A circuit breaker complete with circuit breaker holder","No.",1]
[2.17,null,"Supply 3 phase 60A circuit breaker complete with circuit  breaker holder","No.",1]
[2.18,null,"Install 3 phase 60A circuit breaker complete with circuit breaker holder","No.",1]
[]
["TOTAL, Excluding 15% VAT"]
[]
[null,"SCHEDULE 3: Supply and Install 100A/100V Rectifier, the steel enclosure and the ClearVU fence"]
[]
["ITEM NO.","PAYMENT REF.","ITEM DESCRIPTION","UNIT","QTY","RATE (R) ","AMOUNT(R) "]
[]
[null,null,"The supply of the TRU (100A/100V), TRU steel enclosure and the ClearVU fence shall be supplied and installed as per RAND WATER CATHODIC PROTECTION SYSTEM TECHNICAL SPECIFICATION – Revision 7.5 Rev 3 RW ELS 00001 TS, so as to make sure that the installed system eliminates or combat vandalism and theft.  "]
[2.1,null,"Detection of underground foreign services using a suitable machine / tools up to 1m depth","m",100]
[2.2,null,"Excavate, trench, backfill and compaction (0.3m width X 1.5m depth X 30m length) for the pipe cable connection","m3",14]
[null,null,"Supply and install the 35mm² by 40m length black PVC/PVC cable for pipe connection ","m",40]
[2.3,null,"Supply and install the PRE and coupon  with extended cable of 40 meters to reach the TRU location.","No.",1]
[2.7,null,"Supply and install the steel plate TRU housing as per CP Installation specification 7.5 rev 3 to combat vandalism on rectifiers.","No.",1]
[2.8,null,"Supply and install a ClearVu fence around the TRU and Eskom/Municipality transformer to prevent un-authorised entry as per RW CP Installation Specification 7.5 rev 3.  ","No.",1]
[2.1,null,"Supply and install two kicker pipes of 110mm diameter PVC pipe (conduit) for pipe and power cables insertion inside the steel enclosure.","m",3]
[2.13,null,"Supply 15MPA ready mix concrete","m3",4]
[2.14,null,"Apply 15MPA ready mix concrete over 30m length trench X 0.3m width X 0.2m breadth","No.",1]
[]
["TOTAL, Excluding 15% VAT"]
[]
["                             "]
[]
[]
[]
[null,null,"SUMMARY OF SCHEDULES"]
[]
[null,null,"ITEM DESCRIPTION",null,null,"Amount"]
[null,null,"Schedule 1",null,null,"R "]
[null,null,"Schedule 2",null,null,"R "]
[null,null,"Schedule 3",null,null,"R "]
[null,null,"TOTAL, Excl. VAT",null,null,"R "]
[null,null,"VAT (15%)",null,null,"R "]
[null,null,"TOTAL, Incl. VAT",null,null,"R"]