{"text_format":"3","workbook":"xls","n_sheets":10,"sheets":["1.P&G","2.SITE CLEARANCE","3.EARTHWORKS SMALL WORKS","4.EARTHWORKS PIPE TRENCHES","5.CONCRETE","6.MEDIUM PRESS. PIPELINE","7.BEDDING","8.ELECTRICAL","9.SUNDRIES","Summary"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1.P&G","index":0,"n_rows":204,"n_cols":8,"rows_kept":204,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7],[62,0,63,0],[62,1,63,1],[62,2,63,2],[62,3,63,3],[62,4,63,4],[62,5,63,5],[62,6,63,6],[62,7,63,7],[115,0,116,0],[115,1,116,1],[115,2,116,2],[115,3,116,3],[115,4,116,4],[115,5,116,5],[115,6,116,6],[115,7,116,7],[165,0,166,0],[165,1,166,1],[165,2,166,2],[165,3,166,3],[165,4,166,4],[165,5,166,5],[165,6,166,6],[165,7,166,7]],"flags":["formulas_cached_only"]}
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"SANS\r\n1200A",null,"SECTION 1 : \nPRELIMINARY GENERAL"]
[]
[null,"PSA 8.2.1",null,"Fixed-Charge Items"]
[]
["1.1","8.3.1",null,"Contractual Requirements","Sum",{"v":1,"d":" 1.00"}]
[]
[null,"8.3.2",null,"Establish Facilities on the Site"]
[]
["1.2","8.3.2.1",null,"Facilities for Engineer (SANS 1200AB)"]
[]
["1.2.1","8.3.2.1  PSAB 3.1 & 3.2",null,"a) Two contract nameboards, furnished offices and meeting room, printer, toilet and covered parking bays.","Sum",{"v":1,"d":" 1.00"}]
[]
["1.2.2","PSAB 4.1",null,"b) Telephone","No.",{"v":2,"d":" 2.00"}]
[]
["1.2.3","PSAB 4.3",null,"c) Computer","No.",{"v":1,"d":" 1.00"}]
[]
["1.2.4","PSAB 4.4",null,"d) Vehicle","No.",{"v":1,"d":" 1.00"}]
[]
["1.3","8.3.2.2",null,"Facilities for Contractor"]
[]
["1.3.1",null,null,"a) Offices and storage sheds","Sum",{"v":1,"d":" 1.00"}]
[]
["1.3.2",null,null,"b) Workshops","Sum",{"v":1,"d":" 1.00"}]
[]
["1.3.3",null,null,"c) Laboratories, testing equipment and facilities","Sum",{"v":1,"d":" 1.00"}]
[]
["1.3.4",null,null,"d) Living accommodation","Sum",{"v":1,"d":" 1.00"}]
[]
["1.3.5",null,null,"e) Ablution and latrine facilities","Sum",{"v":1,"d":" 1.00"}]
[]
["1.3.6",null,null,"f) Tools and equipment","Sum",{"v":1,"d":" 1.00"}]
[]
["1.3.7",null,null,"g) Water supply, electric power communications, dealing with water and access","Sum",{"v":1,"d":" 1.00"}]
[]
["1.3.8","PSA 8.4.2.2",null,"h) Dealing with water, inclusive of stormwater management plan for construction purposes","Sum",{"v":1,"d":" 1.00"}]
[]
["1.4","8.3.3",null,"Other fixed-charge obligations","Sum",{"v":1,"d":" 1.00"}]
[]
["1.5","8.3.4",null,"Remove Engineer's and Contractors site establishment on completion of works","Sum",{"v":1,"d":" 1.00"}]
[]
["1.6",null,null,"Compliance with OHS Act (Act 85 of 1993) and Construction Regulations 2014 requirements:"]
[]
["1.6.1",null,null,"Preparation of risk assessments, safe work procedures, the project H&S File and the H&S plan","Sum",{"v":1,"d":" 1.00"}]
[]
["1.6.2",null,null,"The provision of PPE(exclude EPWP) and protective clothing, and all other H&S matters that the contractor deems necessary","Sum",{"v":1,"d":" 1.00"}]
[]
["1.6.3",null,null,"Completing and checking the Project H&S File and handing over to the Client on completion of the Works","Sum",{"v":1,"d":" 1.00"}]
[]
["1.6.4",null,"PE","Contractor's responsibility in terms of Quality Assurance, Construction Records and Construction Dossier","Sum",{"v":1,"d":" 1.00"}]
[]
[" TOTAL CARRIED FORWARD"]
[{"$nulls":7},"PD7"]
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["BROUGHT FORWARD"]
["1.6.5",null,null,"Contractors responsibility in terms of Record of Decision and Environmental Management Plan","Sum",{"v":1,"d":" 1.00"}]
[]
["1.6.6",null,null,"Contractors Responsibility in terms of 24 hour security","Sum",{"v":1,"d":" 1.00"}]
[]
[null,"PSA 8.2.2 & 8.4",null,"Time-Related Items"]
[]
["1.7","8.4.1",null,"Contractual Requirements","Sum",{"v":1,"d":" 1.00"}]
[]
["1.8","8.4.2",null,"Operate and maintain facilities on Site","Sum",{"v":1,"d":" 1.00"}]
[]
["1.9","8.2.2",null,"Facilities for Engineer for duration of construction (SANS 1200AB)"]
[]
["1.9.1","PSA 8.2.2 ",null,"a) Two contract nameboards, furnished offices and meeting room, printer, toilet and covered parking bays.","Sum",{"v":1,"d":" 1.00"}]
[]
["1.9.2","PSAB 4.1",null,"b) Telephone","Sum",{"v":1,"d":" 1.00"}]
[]
["1.10","8.4.2.2",null,"Facilities for Contractor, for duration of construction except where otherwise stated"]
[]
["1.10.1",null,null,"a) Offices and storage sheds","Sum",{"v":1,"d":" 1.00"}]
[]
["1.10.2",null,null,"b) Workshops","Sum",{"v":1,"d":" 1.00"}]
[]
["1.10.3",null,null,"c) Laboratories, materials, testing equipment and facilities","Sum",{"v":1,"d":" 1.00"}]
[]
["1.10.4",null,null,"d) Living accommodation","Sum",{"v":1,"d":" 1.00"}]
[]
["1.10.5",null,null,"e) Ablution and latrine facilities","Sum",{"v":1,"d":" 1.00"}]
[]
["1.10.6",null,null,"f) Tools and equipment","Sum",{"v":1,"d":" 1.00"}]
[]
["1.10.7",null,null,"g) Water supply, electric power, communications dealing with water and access","Sum",{"v":1,"d":" 1.00"}]
[]
["1.10.8","PSA 8.4.2.2",null,"h) Dealing with water","Sum",{"v":1,"d":" 1.00"}]
[]
["1.10.9",null,null,"i) Dealing with water, inclusive of stormwater management plan for construction purposes","Sum",{"v":1,"d":" 1.00"}]
[]
["1.10.10","PSA 8.8.2",null,"j) Dealing with traffic","Sum",{"v":1,"d":" 1.00"}]
[]
["1.11","8.4.3\n",null,"Supervision","Sum",{"v":1,"d":" 1.00"}]
[]
["1.12","8.4.4",null,"Company and head office over head costs","Sum",{"v":1,"d":" 1.00"}]
[]
[]
[]
[" TOTAL CARRIED FORWARD"]
[{"$nulls":7},"PD8"]
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["BROUGHT FORWARD"]
["1.13",null,null,"Compliance with OHS Act (Act 85 of 1993) and Construction Regulations 2003 requirements:"]
[]
["1.13.1",null,null,"Updating and amending the risk assessments, safe work procedures, the project H&S File and the H&S plan","Sum",{"v":1,"d":" 1.00"}]
[]
["1.13.2",null,null,"The provision of PPE and protective clothing, and any other H&S matters that the contractor deems necessary for EPWP","Sum",{"v":1,"d":" 1.00"}]
[]
["1.13.3",null,null,"Compliance with SANS 1921 Part 6 HIV/Aids Awareness during the contract","Sum",{"v":1,"d":" 1.00"}]
[]
["1.13.4",null,null,"Full compliance with all H&S matters during the construction of the works under the contract","Sum",{"v":1,"d":" 1.00"}]
[]
["1.13.5",null,null,"Full compliance with EMP","Sum",{"v":1,"d":" 1.00"}]
[]
["1.14","8.4.5",null,"Other time-related obligations","Sum",{"v":1,"d":" 1.00"}]
[]
["1.15","C3.3.3.2",null,"Contractors commission for the provision of appointing and management of the specialist subcontractors. ","sum",{"v":1,"d":" 1.00"}]
[]
["1.16",null,null,"PROVISIONAL SUMS"]
[]
["1.16.1","PSAB 8.2.2 (a)",null,"Laboratory Testing (Required by the Engineer)","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":50000,"d":"50,000.00"}]
[]
["1.16.2",null,null,"Contractor's Commission on Item 1.16.1","%",{"v":50000,"d":"50 000.00"}]
[]
["1.16.3","PSDB 8.3.10",null,"Relocation of existing services where ordered by the Engineer","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":20000,"d":"20,000.00"}]
[]
["1.16.4",null,null,"Provision of tools and equipment as specified by the Employer","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":10000,"d":"10,000.00"}]
[]
["1.16.5","PSA 8.5 (c)",null,"Provision for Community Liaison Officer","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":84000,"d":"84,000.00"}]
[]
["1.16.6",null,null,"Contractor's Commission on Item 1.16.3 - 1.16.5","%",{"v":114000,"d":"114 000.00"}]
[]
["1.16.7",null,null,"Stationary and other consumables for the Engineer and his/her Representative","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":20000,"d":"20,000.00"}]
[]
["1.16.8",null,null,"Contractor's Commission on Item 1.16.7","%",{"v":20000,"d":"20 000.00"}]
[]
["1.17","PA 5.1",null,"DAYWORKS"]
[]
["1.17.1",null,null,"Labour"]
[]
["1.17.1.1",null,"LI","a) Foreman","Hr",{"v":20,"d":" 20.00"}]
[]
["1.17.1.2",null,"LI","b) Unskilled : labourer","Hr",{"v":30,"d":" 30.00"}]
[" TOTAL CARRIED FORWARD"]
[{"$nulls":7},"PD9"]
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["BROUGHT FORWARD"]
["1.17.1.3",null,"LI","c) Semi-skilled : pipelayer, section leader, survey assistant","Hr",{"v":30,"d":" 30.00"}]
[]
["1.17.1.4",null,null,"d) Skilled: artisan","Hr",{"v":10,"d":" 10.00"}]
[]
["1.17.1.5",null,null,"e) Surveyor including assistants and equipment","Hr",{"v":5,"d":" 5.00"}]
[]
["1.17.2","PA 5.2",null,"Plant"]
[]
["1.17.2.1",null,null,"a) Back-acting excavator","Hr",{"v":9,"d":" 9.00"}]
[]
["1.17.2.2",null,null,"b) Compactors","Hr",{"v":3,"d":" 3.00"}]
[]
["1.17.2.3",null,null,"c) Compressor with hoses, hand tools and bits (min air output 7m3/min)","Hr",{"v":10,"d":" 10.00"}]
[]
["1.17.2.4",null,null,"d) Tiptruck (6m3)","Hr",{"v":9,"d":" 9.00"}]
[]
["1.17.2.5",null,null,"e) Pedestrian roller (Bomag 60 or similar)","Hr",{"v":18,"d":" 18.00"}]
[]
["1.18","PSA8.5 (d) C3.5.10",null,"Provisional Sum for skills training and EPWP requirements","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":20000,"d":"20,000.00"}]
[]
["1.18.1",null,null,"E/O Item 1.18 for Contractor's overheads, charges and profit","%",{"v":20000,"d":"20 000.00"}]
[]
["1.19",null,null,"Provisional Sum for PSC Requirements","Sum",{"v":1,"d":" 1.00"},null,{"v":20000,"d":"20,000.00"}]
[]
["1.19.1",null,null,"E/O Item 1.19 for Contractor's overheads, charges and profit","%",{"v":20000,"d":"20 000.00"}]
{"$rows_empty":9}
[" TOTAL CARRIED FORWARD"]
[{"$nulls":7},"PD10"]

{"sheet":"2.SITE CLEARANCE","index":1,"n_rows":45,"n_cols":8,"rows_kept":45,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7]],"flags":["formulas_cached_only"]}
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[" ","SANS \n1200C",null,"SECTION 2:\nSITE CLEARANCE"]
[]
[{"$nulls":3},"Note: Particular Specification PI: Employer's Environmental Management Specification for Environmental Management of construction projects"]
[]
[" "," ",null,"Clearing and Grubbing & Stripping"]
[]
["2.1"," ",null,"Clear and grub and strip topsoil:"]
[]
["2.1.1","8.2.2 & PSC 8.2.10","LI","a) Strip clearing vegetation and 150mm thick topsoil, stockpile, maintain and reinstate on completion of pipeline (By hand)","m",{"v":15000,"d":"15 000.00"}]
[]
["2.1.2",null,"LI","b) Clear and grub vegetation and 150 mm thick topsoil, stockpile, maintain and reinstate on completion for tank bases and isolating valve chambers (By hand)","m²",{"v":350,"d":" 350.00"}]
[]
["2.2","8.2.2",null,"Remove and grub large trees and tree stumps of girth:"]
[]
["2.2.1",null,"LI","a) over 1m and up to and including 2m","No.",{"v":15,"d":" 15.00"}]
[]
["2.2.2",null,"LI","b) over 2m and up to and including 3m ","No.",{"v":10,"d":" 10.00"}]
[]
["2.2.3",null,null,"c) over 3m","No.",{"v":5,"d":" 5.00"}]
[]
["2.3","PSC 8.2.11",null,"Dismantle existing fencing, move to storage and later reinstate as directed by the Employer's Agent:"]
[]
["2.3.2",null,null,"Welded mesh wire fencing with straining posts","m",{"v":100,"d":" 100.00"}]
[]
["2.3.3",null,null,"Wire fencing with straining posts","m",{"v":500,"d":" 500.00"}]
[]
["2.4",null,null,"Remove and re-erect Structures"]
[]
["2.4.1","PSC 8.2.12",null,"Demarcation staking of pipeline servitude with wooden stakes","m",{"v":20,"d":" 20.00"}]
[]
["2.4.2","PSC 8.2.13",null,"Fencing pipeline servitude in populated area","m",{"v":600,"d":" 600.00"}]
[]
["2.4.3","PSC 8.2.14",null,"Removing and re-erecting of Structures","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":20000,"d":"20,000.00"}]
[]
[]
[]
[]
[" TOTAL CARRIED FORWARD TO SUMMARY"]
[{"$nulls":7},"PD11"]

{"sheet":"3.EARTHWORKS SMALL WORKS","index":2,"n_rows":41,"n_cols":8,"rows_kept":41,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7]],"flags":["formulas_cached_only"]}
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"SANS \r\n1200D",null,"SECTION 3:\nEARTHWORKS SMALL STRUCTURES"]
[]
["3.1","PSD 8.3.3"," ","Restricted excavation, beyond the limits of the pipe trench, in all materials to net outline of structures and to underside of blinding layers, including for disposal of material.",""]
[]
["3.1.1","","LI","Excavate material for tank bases","m³",{"v":60,"d":" 60.00"}]
[]
["3.1.2",null,"LI","Excavate materials for isolating valve chambers","m³",{"v":25,"d":" 25.00"}]
[]
["3.1.3","","LI","Excavate material for package water treatment plant","m³",{"v":50,"d":" 50.00"}]
[]
["3.1.4","","LI","Excavate material for pumpstation","m³",{"v":60,"d":" 60.00"}]
[]
["3.2","8.3.3(b)",null,"Extra over Items 3.1.1 to 3.1.4 for excavation in: "]
[]
["3.2.1",null,null,"Intermediate material (Prov.)","m³",{"v":150,"d":" 150.00"}]
[]
["3.2.2","8.3.3(b)(2)",null,"Hard rock (Prov.)","m³",{"v":40,"d":" 40.00"}]
[]
["3.2.3","8.3.3(b)(3)",null,"Boulder excavation Class A (Prov.)","m³",{"v":30,"d":" 30.00"}]
[]
["3.2.4","8.3.3(b)(4)",null,"Boulder excavation Class B (Prov.)","m³",{"v":10,"d":" 10.00"}]
[]
["3.3","PSD 8.3.15","LI","Extra over Items 3.2.1 to 3.2.4 for backfill stabilised with 8 % cement where directed by the Engineer","m³",{"v":20,"d":" 20.00"}]
[]
["3.4","8.3.4(a)",null,"Import G2 fill material to use for backfill underside of blinding level of tank bases compacted to 96% MOD AASHTO","m³",{"v":100,"d":" 100.00"}]
{"$rows_empty":8}
[" TOTAL CARRIED FORWARD TO SUMMARY"]
[{"$nulls":7},"PD12"]

{"sheet":"4.EARTHWORKS PIPE TRENCHES","index":3,"n_rows":93,"n_cols":8,"rows_kept":93,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7],[47,0,48,0],[47,1,48,1],[47,2,48,2],[47,3,48,3],[47,4,48,4],[47,5,48,5],[47,6,48,6],[47,7,48,7],[49,0,49,6]],"flags":["formulas_cached_only"]}
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"SANS\r\n1200DB",null,"SECTION 4 :\nEARTHWORKS PIPE TRENCHES"]
[]
[{"$nulls":3},"Pipeline Trench Excavations:"]
[]
["4.1","PSDB 8.3.2(a)",null,"Excavate, in all materials for trenches, backfill, compact and dispose of surplus unsuitable material, for DN 50 - DN 100 pipes for the following depths:  Rates are to include for all temporary works including trimming, shoring and dewatering where necessary:"]
[]
[{"$nulls":3},"        Over            Up to and including"]
[]
["4.1.1",null,null,"         0 m                      1,5 m","m³",{"v":14000,"d":"14 000.00"}]
[]
["4.1.2",null,null,"      1,5 m                      2,0 m ","m³",{"v":200,"d":" 200.00"}]
[]
["4.1.3",null,null,"      2,0 m                      3,0 m ","m³",{"v":60,"d":" 60.00"}]
[{"$nulls":4}," "]
["4.2",null,null,"Extra over Items in 4.1 for excavation in: "]
[]
["4.2.1","PSDB 8.3.2(c)(1)",null,"Hard rock (Prov.)","m³",{"v":1200,"d":"1 200.00"}]
[]
["4.2.2","PSDB 8.3.2(c)(2)",null,"Boulder excavation Class A (Prov.)","m³",{"v":500,"d":" 500.00"}]
[]
["4.2.3","PSDB 8.3.2(c)(3)",null,"Boulder excavation Class B (Prov.)","m³",{"v":200,"d":" 200.00"}]
[]
["4.3","PSDB 8.3.2(e)",null,"Extra over Items for 4.2.1 to 4.2.3 for backfill stabilised with 8 % cement where directed by the Engineer as per PSDB 3.5c (Prov.)","m³",{"v":50,"d":" 50.00"}]
[null," "]
["4.4","8.3.2 (c) ","LI","Excavate and dispose of unsuitable material from trench bottom (Prov.)","m³",{"v":500,"d":" 500.00"}]
[]
["4.5",null,null,"Excavation ancillaries"]
[]
["4.5.1","PSDB 8.3.3.1",null,"Make up deficiency in backfill material from designated borrowpits ","m³",{"v":1500,"d":"1 500.00"}]
[]
["4.6","8.3.3.3",null,"Compaction in road reserves","m³",{"v":100,"d":" 100.00"}]
[]
["4.7","8.3.4(b)",null,"Control of underground water seepage at stream crossings","m",{"v":50,"d":" 50.00"}]
[]
[]
[" TOTAL CARRIED FORWARD"]
[{"$nulls":7},"PD13"]
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["BROUGHT FORWARD"]
["4.8",null,null,"Existing Services"]
[]
["4.8.1","8.3.5(a)",null,"Protect, maintain, repair services that intersect a pipe trench","No",{"v":20,"d":" 20.00"}]
[]
["4.8.2","8.3.5(b)",null,"Protect, maintain, repair services that adjoin a pipe trench","m",{"v":500,"d":" 500.00"}]
[]
["4.9","PSDB 8.3.5(c)","LI","Excavate by hand to expose existing services","m³",{"v":100,"d":" 100.00"}]
[]
["4.10","PSDB 8.3.6.2",null,"Grassing where directed by Engineer (Prov)","m2",{"v":100,"d":" 100.00"}]
[]
["4.11","PSDB 8.3.8",null,"Sack Breakers where directed by Engineer (Prov)","No",{"v":10,"d":" 10.00"}]
{"$rows_empty":30}
[" TOTAL CARRIED FORWARD TO SUMMARY"]
[{"$nulls":7},"PD14"]

{"sheet":"5.CONCRETE","index":4,"n_rows":52,"n_cols":8,"rows_kept":52,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7]],"flags":["formulas_cached_only"]}
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"SANS\n1200GA",null,"SECTION 5 :\nCONCRETE (SMALL WORKS)"]
[]
["5.1","8.2",null,"FORMWORK"]
[]
["5.1.1",null,"LI","a) Rough horizontal","m²",{"v":20,"d":" 20.00"}]
[]
["5.1.2",null,"LI","b) Rough vertical","m²",{"v":40,"d":" 40.00"}]
[]
["5.1.3",null,"LI","c) Smooth horizontal","m²",{"v":20,"d":" 20.00"}]
[]
["5.1.4",null,"LI","d) Smooth vertical","m²",{"v":20,"d":" 20.00"}]
[]
["5.2","8.3",null,"REINFORCEMENT"]
[]
["5.2.1","8.3.1","LI","a) High tensile","kg",{"v":400,"d":" 400.00"}]
[]
["5.2.2","8.3.1","LI","b) Mild steel","kg",{"v":300,"d":" 300.00"}]
[]
["5.2.3","8.3.2","LI","c) Weldmesh Ref 245","m²",{"v":200,"d":" 200.00"}]
[]
["5.2.4","8.3.3","LI","d) Weldmesh Ref 345","m²",{"v":25,"d":" 25.00"}]
[]
["5.3","8.4",null,"CONCRETE"]
[]
["5.3.1","8.4.2","LI","Blinding concrete Class 15/19 50 mm thick","m²",{"v":200,"d":" 200.00"}]
[]
["5.3.2",null,"LI","Concrete Class 25/19 to package water treatment plants, pump stations and jojo water tank concrete bases."]
[]
["5.3.2.1",null,"LI","Concrete bases","m³",{"v":70,"d":" 70.00"}]
[]
["5.3.3",null,null,"Concrete Class 25/19 to concrete pedestals, plinths and other minor concrete work, including all formwork."]
[]
["5.3.3.1",null,null,"Concrete pedestals, plinths, etc","m³",{"v":10,"d":" 10.00"}]
[]
["5.4",null,null,"UNFORMED SURFACE FINISHING"]
[]
["5.4.1","8.4.4(a)","LI","a) Wood-floated finish","m²",{"v":150,"d":" 150.00"}]
[]
["5.4.2","8.4.4(b)","LI","b) Steel-floated finish","m²",{"v":10,"d":" 10.00"}]
[]
[]
[]
[]
[]
[" TOTAL CARRIED FORWARD"]
[{"$nulls":7},"PD15"]

{"sheet":"6.MEDIUM PRESS. PIPELINE","index":5,"n_rows":146,"n_cols":8,"rows_kept":146,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7],[61,0,62,0],[61,1,62,1],[61,2,62,2],[61,3,62,3],[61,4,62,4],[61,5,62,5],[61,6,62,6],[61,7,62,7],[63,0,63,6],[116,0,117,0],[116,1,117,1],[116,2,117,2],[116,3,117,3],[116,4,117,4],[116,5,117,5],[116,6,117,6],[116,7,117,7],[118,0,118,6]],"flags":["formulas_cached_only"]}
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"SANS\r\n1200L",null,"SECTION 6 :\nMEDIUM PRESSURE PIPELINES"]
[{"$nulls":3},"Note: Particular Specification PB: Pipelines Valves has reference.                               Particular Specification PC: HDPE Pipes and Fittings has reference.                               Particular Specification PD: Disinfection of Pipelines and Fittings has reference."]
[]
["6.1",null,null,"PIPES"]
[]
[null,"PSL 8.2.1",null,"Supply, handle, lay, test, disinfect, join PVC pipes on bedding for flexible pipe"]
[]
["6.1.1",null,"LI","DN110 Class 16 uPVC","m",{"v":2000,"d":"2 000.00"}]
[]
["6.1.2",null,"LI","DN90 Class 16 uPVC","m",{"v":1000,"d":"1 000.00"}]
[]
["6.1.3",null,"LI","DN75 Class 16 uPVC","m",{"v":1500,"d":"1 500.00"}]
[]
[{"$nulls":3},"Supply, handle, lay, test, disinfect, join HDPE pipes on bedding for flexible pipe"]
["6.2",null,null,"HDPE Pipe PE80 (PN12) SDR 11"]
[]
["6.2.1",null,null,"DN110","m",{"v":1000,"d":"1 000.00"}]
[]
["6.2.2",null,null,"DN90","m",{"v":1500,"d":"1 500.00"}]
[]
["6.2.3",null,null,"DN75","m",{"v":7500,"d":"7 500.00"}]
[]
[{"$nulls":3},"HDPE Compression Fittings and Specials PE100 (PN16) SDR 11"]
[]
[{"$nulls":3},"Supply, handle, lay, bed, test and disinfect pipe fittings and specials (including specified bolts, nuts and gaskets)"]
[]
["6.3",null,null,"Flange adaptors"]
[]
["6.3.1",null,null,"DN110","No.",{"v":15,"d":" 15.00"}]
[]
["6.3.2",null,null,"DN90","No.",{"v":10,"d":" 10.00"}]
[]
["6.3.3",null,null,"DN75","No.",{"v":15,"d":" 15.00"}]
[]
["6.4",null,null,"90 degree bend"]
[]
["6.4.1",null,null,"DN110","No.",{"v":2,"d":" 2.00"}]
[]
["6.4.2",null,null,"DN90","No.",{"v":2,"d":" 2.00"}]
[]
["6.4.3",null,null,"DN75","No.",{"v":2,"d":" 2.00"}]
[]
["6.5",null,null,"Equal tees"]
[]
["6.5.1",null,null,"DN110","No.",{"v":2,"d":" 2.00"}]
[]
["6.5.2",null,null,"DN90","No.",{"v":2,"d":" 2.00"}]
[]
["6.5.3",null,null,"DN75","No.",{"v":2,"d":" 2.00"}]
[" TOTAL CARRIED FORWARD"]
[{"$nulls":7},"PD16"]
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["BROUGHT FORWARD"]
[6.6,null,null,"Reducing tees"]
[]
["6.6.1",null,null,"DN110","No.",{"v":5,"d":"5.00"}]
[]
["6.6.2",null,null,"DN90","No.",{"v":5,"d":"5.00"}]
[]
["6.6.3",null,null,"DN75","No.",{"v":2,"d":"2.00"}]
[]
["6.7",null,null,"Steel Pipes And Fittings"]
[]
[{"$nulls":3},"NOTE:  In accordance with SABS 62: Part 1, 3,3 mm thick steel pipes up to and including DN150 and 4,5mm thick Grade B steel plate for manufacture of DN200 and larger. Pipes up to and including DN150 hot dipped galvanised. "]
[]
[null,"PSL 8.2.1 ",null,"Supply, handle, lay, bed, test and disinfect pipe fittings and specials (including specified bolts, nuts and gaskets)"]
[]
["6.7.1",null,null,"Pipes"]
[]
["6.7.1.1",null,"LI","DN110 x 5 000mm long d/fl pipe","No.",{"v":1,"d":"1.00"}]
[]
["6.7.1.2",null,"LI","DN110 x 2 500mm long d/fl pipe","No.",{"v":1,"d":"1.00"}]
[]
["6.7.1.3",null,"LI","DN75 x 1 500mm long d/fl pipe","No.",{"v":1,"d":"1.00"}]
[]
["6.7.1.4",null,"LI","DN75 x 5 000mm long d/fl pipe","No.",{"v":2,"d":"2.00"}]
[]
["6.7.2",null,null,"Tees"]
[]
["6.7.2.1",null,"LI","DN100 FL Equal Tee","No.",{"v":1,"d":" 1.00"}]
[]
["6.7.2.2",null,"LI","DN80 FL Equal Tee ","No.",{"v":1,"d":" 1.00"}]
[]
["6.7.2.3",null,"LI","DN100 x DN80 FL Reducing Tee ","No.",{"v":1,"d":" 1.00"}]
[]
["6.7.3",null,null,"Reducers"]
[]
["6.7.3.1",null,"LI","DN150 x DN100 d/fl reducer","No.",{"v":1,"d":" 1.00"}]
[]
["6.7.3.2",null,"LI","DN100 x DN80 d/fl reducer","No.",{"v":1,"d":" 1.00"}]
[]
["6.7.4",null,null,"Flange Adaptors"]
[]
["6.7.4.1",null,"LI","DN100","No.",{"v":1,"d":" 1.00"}]
[]
["6.7.4.2",null,"LI","DN80","No.",{"v":1,"d":" 1.00"}]
[]
[]
[]
[" TOTAL CARRIED FORWARD"]
[{"$nulls":7},"PD17"]
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["BROUGHT FORWARD"]
[null,"PSL 3.10 & 8.2.3",null,"Supply, handle, install and test SABS approved waterworks pattern, flanged valves (SABS 1123, Table 1600 unless otherwise specified):"]
[]
["6.7.5",null,null,"Valves"]
[]
["6.7.5.1"," ","LI","DN80 d/fl wedge gate valve with square cap","No.",{"v":5,"d":" 5.00"}]
[]
["6.7.5.2",null,"LI","DN50 d/fl wedge gate valve with square cap","No.",{"v":1,"d":" 1.00"}]
[]
["6.7.5.3",null,"LI","DN50 Ball-O-Stop valve","No.",{"v":10,"d":" 10.00"}]
[]
["6.7.5.4",null,"LI","DN25 Ball-O-Stop valve","No.",{"v":5,"d":" 5.00"}]
{"$rows_empty":14}
[" TOTAL CARRIED FORWARD"]
[{"$nulls":7},"PD18"]

{"sheet":"7.BEDDING","index":6,"n_rows":48,"n_cols":8,"rows_kept":48,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7]],"flags":["formulas_cached_only"]}
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[null,"SABS    1200LB",null,"SECTION 7 :\nBEDDING (PIPES)"]
[]
[{"$nulls":3},"PROVISION OF BEDDING"]
[]
[null,"PSLB 8.2.1(1)",null,"Provision of bedding from trench excavation"]
[]
["7.1",null,null,"Without the need for screening:"]
[]
["7.1.1","PSLB 8.2.1(1)(a)","LI","Selected granular material","m³",{"v":2200,"d":"2 200.00"}]
[]
["7.1.2","PSLB 8.2.1(1)(b)","LI","Selected fill material","m³",{"v":1600,"d":"1 600.00"}]
[]
["7.2","PSLB 8.2.1(2)","LI","Including for screening"]
[]
["7.2.1","PSLB 8.2.1(2)(a)","LI","Selected granular material","m³",{"v":550,"d":" 550.00"}]
[]
["7.2.2","PSLB 8.2.1(2)(b)","LI","Selected fill material","m³",{"v":400,"d":" 400.00"}]
[]
["7.3","8.2.2.2 & 8.2.2.3",null,"Provision of bedding by importation from commercial or off-site sources, including for screening and/or other treatment:"]
[]
["7.3.1","PSLB 8.2.1(2)(b)","LI","Selected granular material","m³",{"v":550,"d":" 550.00"}]
[]
["7.3.2","PSLB 8.2.1(2)(b)","LI","Selected fill material","m³",{"v":400,"d":" 400.00"}]
[]
["7.4","PSLB 8.2.6","LI","13 mm Drianage layer","m³",{"v":10,"d":" 10.00"}]
{"$rows_empty":15}
[" TOTAL CARRIED FORWARD TO SUMMARY"]
[{"$nulls":7},"PD19"]

{"sheet":"8.ELECTRICAL","index":7,"n_rows":51,"n_cols":8,"rows_kept":51,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7]],"flags":["formulas_cached_only"]}
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[{"$nulls":3},"SECTION 8 :\nELECTRICAL AND ELECTRONIC EQUIPMENT AND INSTALLATION"]
[]
["8.1",null,null,"Electrical Installation"]
[]
["8.1.1",null,null,"Provision for Eskom Power Supply to 7No. New Stations","Prov Sum",{"v":1,"d":" 1.00"},{"v":1000000,"d":"1000 000.00"},{"v":1000000,"d":"1000 000.00"}]
[]
["8.1.2",null,null,"Contractor's mark-up on items 9.1.1","%",{"v":1000000,"d":"1000 000.00"}]
[]
["8.1.3",null,null,"Trenching and cabling from Eskom connection points (7No. Stations)","m",{"v":170,"d":" 170.00"}]
[]
["8.1.4",null,null,"Supply, install, commission and test new Electric Borehole Pumps.","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":800000,"d":"800 000.00"}]
[]
["8.1.5",null,null,"Provision for installation of electrical control system for all Boreholes","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":80000,"d":"80 000.00"}]
[]
["8.1.6",null,null,"Provision for supply, install, commission and test an Electric Pumps","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":100000,"d":"100 000.00"}]
[]
["8.1.7",null,null,"Contractor's mark-up on items 9.1.4 - 9.1.6","%",{"v":980000,"d":"980 000.00"}]
{"$rows_empty":26}
[" TOTAL CARRIED FORWARD TO SUMMARY"]
[{"$nulls":7},"PD20"]

{"sheet":"9.SUNDRIES","index":8,"n_rows":159,"n_cols":8,"rows_kept":159,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[4,5,5,5],[4,6,5,6],[4,7,5,7],[52,0,53,0],[52,1,53,1],[52,2,53,2],[52,3,53,3],[52,4,53,4],[52,5,53,5],[52,6,53,6],[52,7,53,7],[54,0,54,6],[102,0,103,0],[102,1,103,1],[102,2,103,2],[102,3,103,3],[102,4,103,4],[102,5,103,5],[102,6,103,6],[102,7,103,7],[104,0,104,6]],"flags":["formulas_cached_only"]}
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[{"$nulls":3},"SECTION 10 :\nSUNDRIES"]
[]
["9.1",8.4,null,"CONCRETE"]
[]
["9.1.1","PSL 8.2.11","LI","Anchor/Thrust blocks, inclusive of formwork and additional excavation Class 25/19","m³",{"v":2,"d":" 2.00"}]
[]
["9.1.2","PSL 8.2.12","LI","Concrete Encasing at Stream Crossings, including formwork and additional excavation Class 25/19","m",{"v":10,"d":" 10.00"}]
[]
["9.1.3","PSL 8.2.18","LI","Concrete marker posts. Rates are to include for base concrete, installation & painting","No.",{"v":150,"d":" 150.00"}]
[]
["9.2","PSL 8.2.15",null,"Denso wrapping bolted fittings located underground"]
[]
["9.2.1",null,"LI","DN150 ","No.",{"v":5,"d":" 5.00"}]
[]
["9.2.2",null,"LI","DN100","No.",{"v":10,"d":" 10.00"}]
[]
["9.2.3",null,"LI","DN80 to DN50 ","No.",{"v":20,"d":" 20.00"}]
[]
["9.3",null,"LI","Supply and install 50mm Discus 0370 keyed alike padlocks with 3 keys as supplied by Multi Locking","No.",{"v":25,"d":" 25.00"}]
[]
["9.4",null,null,"JOJO TANKS"]
[]
["9.4.1",null,null,"Supply, erect and testing of 10 000L x 4.5m high elevated JoJo water tank and structural steel stand (hot dipped galvanised)","No.",{"v":6,"d":" 6.00"}]
[]
["9.4.2",null,null,"Supply and erect 10 000L standard vertical JoJo Water Tanks on existing concrete footing stands","No.",{"v":6,"d":" 6.00"}]
[]
["9.5",null,null,"STANDPIPES"]
[]
["10.5.1",null,null,"Supply and construct complete Standpipes including concrete tray, plinth and meter boxes with ball valves and fittings (refer DWG No. P0023-SD-01)","No.",{"v":10,"d":" 10.00"}]
[]
["9.6",null,null,"VALVE CHAMBER"]
[]
["9.6.1",null,null,"Supply and construct isolating valve chamber complete as per drawing P0023/SD/02 (pipework measured elsewhere)","No.",{"v":5,"d":" 5.00"}]
{"$rows_empty":7}
[" TOTAL CARRIED FORWARD"]
[{"$nulls":7},"PD21"]
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["BROUGHT FORWARD"]
["9.7",null,null,"CONNECT TO EXISTING PIPELINES"]
[]
[null,"PSL 8.2.17","LI","Connect to existing pipelines in the following areas (Rate to include exposing of existing pipe, supervision, liaison with Operator, preparation of method statements, dealing with water from the existing pipelines and any other operation to successfully complete the tie in):"]
[]
["9.7.1",null,null,"Connect to DN50 pipe","No.",{"v":2,"d":" 2.00"}]
[]
["9.7.2",null,null,"Connect to DN63 pipe","No.",{"v":2,"d":" 2.00"}," "]
[]
["9.7.3",null,"LI","Connect to DN90 pipe","No.",{"v":2,"d":" 2.00"}]
[]
["9.7.4",null,"LI","Connect to DN110 pipe","No.",{"v":2,"d":" 2.00"}]
[]
["9.7.5",null,"LI","Connect to DN160 pipe","No.",{"v":1,"d":" 1.00"}]
[]
["9.8",null,null,"CATTLE DRINKING BASINS"]
[]
["9.8.1",null,null,"Supply and erect 250 litre Jojo cattle drinking trough onto the existing concrete slabs.  Rate to include bolting onto the slab.  ","No.",{"v":10,"d":" 10.00"}]
[]
["9.9",null,null,"PACKAGE WATER TREATMENT PLANT"]
[]
["9.9.1",null,null,"Supply, erect and testing of a 2 x 100kl package water treatment plants","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":4000000,"d":"4,000,000.00"}]
[]
["9.9.2",null,null,"Supply, erect and testing of a 200kl package water treatment plant","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":3000000,"d":"3,000,000.00"}]
[]
["9.10",null,null,"BOREHOLE"]
[]
["9.10.1",null,null,"Provision for testing of existing boreholes on yielding and water quality.","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":400000,"d":"400,000.00"}]
[]
["9.10.2",null,null,"Provision for drilling and equipping of new electric boreholes pumps including casing","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":1200000,"d":"1,200,000.00"}]
[]
["9.10.3",null,null,"Contractor's mark-up on items 10.9.1 - 10.10.2","%",{"v":8600000,"d":"8600 000.00"}]
[]
["9.11",null,null,"BRICKWORK"]
[]
[{"$nulls":3},"Engineering brick walls brickforce every 5 courses and above first and below last course, face brick finish exposed external.  "]
[]
["9.11.1",null,null,"115mm thick","m²",{"v":60,"d":" 60.00"}]
[]
["9.11.2",null,null,"230mm thick","m²",{"v":90,"d":" 90.00"}]
[]
[]
[" TOTAL CARRIED FORWARD"]
[{"$nulls":7},"PD22"]
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["ITEM\nNO","PAYMENT","LIC","DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
["BROUGHT FORWARD"]
["9.11.3",null,null,"Internal Walls Plaster (not less than 10mm and not more than 15mm thick) and 2 Coats white PVA paint","m²",{"v":90,"d":" 90.00"}]
[]
["9.12",null,null,"PUMP STATION"]
[]
["9.12.1",null,null,"Provision to build three pump stations including all internal fittings and electrical components","Prov Sum",{"v":1,"d":" 1.00"},null,{"v":3550000,"d":"3,550,000.00"}]
[]
["9.12.2",null,null,"Contractor's mark-up on items 10.12.1","%",{"v":3550000,"d":"3550 000.00"}]
{"$rows_empty":45}
[" TOTAL CARRIED FORWARD TO SUMMARY"]
[{"$nulls":7},"PD23"]

{"sheet":"Summary","index":9,"n_rows":63,"n_cols":3,"rows_kept":63,"merged":[[4,0,5,0],[4,1,5,1],[4,2,5,2],[61,0,61,1]],"flags":["formulas_cached_only"]}
["MHLATHUZE WATER"]
["BIG 5 HLABISA LM - REFURBISHMENT AND AUGMENTATION OF WATER SUPPLY SCHEME IN WARD 1,2,3 & 4"]
[]
["SCHEDULE OF QUANTITIES"]
["SECTION","DESCRIPTION","AMOUNT"]
[]
["1.","PRELIMINARY AND GENERAL"]
[]
["2.","SITE CLEARANCE"]
[]
["3.","EARTHWORKS"]
[]
["4.","EARTHWORKS (PIPE TRENCHES)"]
[]
["5.","CONCRETE (SMALL WORKS)"]
[]
["6.","MEDIUM PRESSURE PIPELINES"]
[]
["7.","BEDDING (PIPES)"]
[]
["8.","ELECTRICAL AND ELECTRONIC EQUIPMENT AND INSTALLATION"]
[]
["9.","SUNDRIES"]
[]
[]
[null,"SUBTOTAL"]
[]
[null,"CONTINGENCIES - 10%"]
[]
[null,"SUBTOTAL"]
[]
[null,"VALUE ADDED TAX - 15%"]
{"$rows_empty":29}
["SUMMARY OF BILL OF QUANTITIES"]
[null,null,"PD24"]