{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["RFP161.2023"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"RFP161.2023","index":0,"n_rows":39,"n_cols":6,"rows_kept":39,"merged":[[0,0,0,5],[1,1,1,5],[34,0,34,4],[36,0,36,4],[38,0,38,4]]}
["RFP161/2023:\nTHE SUPPLY AND DELIVERY OF FORMWORK AND PLATFORMS TO THE DEPARTMENT OF WATER AND SANITATION, TZANEEN DAM RAISING PROJECT IN LIMPOPO PROVINCE "]
[null,"Supply and delivery of Formwork and Working Accesses "]
["Item","Description","Unit","Quantity","Rate","Total"]
[1,"\tLabyrinth Base slab & Walls formwork "]
[null,"(Refer Drawing 9368 – 301, 308, 309, 310, 311 & 312)"]
[null,"Formwork design, Rental, supply and deliver including anchors and accessories for"]
[1.1,"Complete set of one Base Slab formwork system (Two Moulds)","Sum",1,null,{"$f":"D7*E7","v":{"v":0,"d":"R0.00"}}]
[1.2,"Complete set of one Walls formwork system (Two moulds)","Sum",1,null,{"$f":"D8*E8","v":{"v":0,"d":"R0.00"}}]
[2,"Ogee outgoing channel & inner outgoing channel formwork "]
[null,"(Refer Drawing 9368 – 301, 308, 309, 310, 311 & 312)"]
[null,"Formwork design, Rental, supply and deliver including anchors and accessories for"]
[2.1,"Complete set of one Ogee outgoing channel formwork system","Sum",1,null,{"v":0,"d":"R0.00"}]
[2.2,"Complete set of one inner outgoing channel formwork system","Sum",1,null,{"v":0,"d":"R0.00"}]
[3,"Retaining wall formwork ((Refer to drawing no. 9368 – 211 & 212)"]
[null,"Formwork design,Rental, supply and deliver including anchors and accessories for"]
[3.1,"Complete set of one Retaining wall formwork mould MKD. RW – 1R & MKD. RW ","Sum",1,null,{"v":0,"d":"R0.00"}]
[3.3,"Complete set of Retaining wall formwork mould MKD. RW – STD ","Sum",1,null,{"v":0,"d":"R0.00"}]
[null,"(Six moulds are required)"]
[4,"Spillway Sidewalls (Refer to Drawing no. 9368 – 351, 9368 – 352, 9368 – 353 & 9368 – 354) "]
[null,"Formwork design,Rental, supply and deliver including anchors and accessories for"]
[4.1,"Formwork system for inclined spillway sidewalls","Sum",1,null,{"v":0,"d":"R0.00"}]
[5,"Working, access and working platforms (Refer Drawing 9368 – 301, 308, 309 & 310, 311, 312)"]
[null,"Access, stairways, Walkways and work platforms design,Rental, supply and deliver including anchors and accessories for"]
[5.1,"Work platforms for spillway, Tongue walls, Training wall and Intake tower along the full length of the upstream and downstream faces of the dam wall ","Sum",1,null,{"v":0,"d":"R0.00"}]
[6,"INTAKE TOWER (Refer to Drawing no. 9368 – 401, 9368 – 402, 9368 – 403, 9368 – 405, 9368 – 406, 9368 – 407)"]
[null,"Formwork design,Rental, supply and deliver including anchors and accessories for"]
[6.1,"Formwork system for the walls","Sum",1,null,{"v":0,"d":"R0.00"}]
[6.2,"Formwork system for the roof ","Sum",1,null,{"v":0,"d":"R0.00"}]
[7,"Man cages for using with when working on Heights"]
[null,"Man cage Designing, Manufacturing, Supply and delivery including accessories for "]
[7.1,"Man cage","No.",3,null,{"v":0,"d":"R0.00"}]
[7.2,"One combined sling with 4-legged slings must be attached with a D shape shackle to the cage","No.",3,null,{"v":0,"d":"R0.00"}]
[7.3,"set of safety chains to attach working people’s safety harnesses to the crane hook ","No.",6,null,{"v":0,"d":"R0.00"}]
[8,"On - site Training Services of personnel","No.",30,null,{"v":0,"d":"R0.00"}]
["SUB TOTAL A",{"$nulls":4},{"$f":"SUM(F7:F34)","v":{"v":0,"d":"R0.00"}}]
["CONTIGENCY @15%",null,"%",{"v":0.15,"d":"15%"},null,{"$f":"F35*D36","v":{"v":0,"d":"R0.00"}}]
["SUB - TOTAL B",{"$nulls":4},{"$f":"SUM(F35:F36)","v":{"v":0,"d":"R0.00"}}]
["VAT @ 15%",null,"%",{"v":0.15,"d":"15%"},null,{"$f":"F37*D38","v":{"v":0,"d":"R0.00"}}]
["TOTAL",{"$nulls":4},{"$f":"F38+F37","v":{"v":0,"d":"R0.00"}}]