{"text_format":"3","workbook":"xlsx","n_sheets":10,"sheets":["Sheet1","Cover Page ","Air-Con Spares","Chemical Spares","Electrical Spares","Fire Systems","General Spares","Handyman Spares","Mechanical Spares","Plumbing Spares"],"not_rendered":{"images":1,"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":3,"n_cols":1,"rows_kept":3,"hidden":true}
["Bidder Must Indicate  Compliance to Specification"]
["YES"]
["NO"]

{"sheet":"Cover Page ","index":1,"n_rows":29,"n_cols":5,"rows_kept":29,"merged":[[13,0,13,5],[23,0,23,5],[25,0,25,5],[26,0,26,5],[27,0,27,5],[28,0,28,5]]}
{"$rows_empty":13}
["TECHNICAL SPECIFICATIONS"]
[]
[]
["RFP NO:",{"$nulls":3},"RFP No. 3662/28/11/2024"]
[]
["RFP NAME:",{"$nulls":3},"Supply and delivery of Various Spares on an “as and when” required basis to the CSIR for a period of Five (5) years"]
[]
["BIDDER NAME"]
[]
[]
[" INSTRUCTIONS"]
[]
["STRUCTURE OF THE TENDER"]
["The bidder/s may give a proposal on the exact specification outlined by the CSIR or propose an equivalent alternative."]
[]
["Failure to comply with specifications will be disqualified"]

{"sheet":"Air-Con Spares","index":2,"n_rows":25,"n_cols":6,"rows_kept":25,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,1],[3,1,3,2]]}
["Supply and delivery of Various Spares on an “as and when” required basis for five (5) years.  "]
["RFP: 0000/00/00/2024"]
["Bidder's Name",null,{"$f":"'Cover Page '!E21","v":0}]
["Note: ","The bidders may give a proposal on the exact specification outlined by the CSIR or propose an equivalent alternative."]
[]
["Category","CSIR Part Code","Product technical specifications ","Bidder Must Indicate  Compliance to Specification YES/N0","Any alternative offered compatible to this specification shall be listed below with full functional specification.","Indicate the quality standard the part complies with "]
["Air-con",600882,"Coupling 20mm PVC Blue - Material:Polyvinyl chloride (PVC)"]
["Air-Con",600100,"Acidic cleaner 5 Litre; Potassium or sodium hydroxide"]
["Air-Con",600146,"Capacitor 25MF - Aluminium"]
["Air-Con",600147,"Capacitor 30MF - Aluminium"]
["Air-Con",600151,"Capacitor 50MF - Aluminium"]
["Air-Con",600240,"Fan Extracto G X9\" Window/Surface Wall Fan 220- 240V White"]
["Air-con",600275,"Flux Silver Solder 30F potassium salts or fluorides and borates in a water base"]
["Air-Con",600286,"Gas Bottle Disposable R134A - 13.6KG Disposable"]
["Air-Con",600287,"Gas Bottle Disposable R22 Starke Refrigerant Gas Cylinder (13.6kg)"]
["Air-Con",600288,"Gas Bottle Disposable R404A - 10.9KG Disposable"]
["Air-Con",600289,"Gas Bottle Disposable R407C Disposable Cyl 13kg"]
["Air-Con",600290,"Gas Bottle Disposable R408 - 13.6KG Disposable"]
["Air-con",600291,"Gas Bottle Disposable R410A Disposable Cyl 11.3kg"]
["Air-Con",600464,"Pencil dryer - Domestic Refrigeration Dryers 25 Gram Pencil Drier "]
["Air-Con",600493,"Pressure Switch_KP 15 Hp/ LP  Alarm - KP15 Pressure Switch HP/LP HP Manual Reset"]
["Air-Con",600591,"Tape insulation cork 1 roll -1/8\" X2 X 30' - 2\" Prestite Tacky Tar-Cork Insulation Tape"]
["Air-Con",600643,"Valve Schrader long - A/C R12 R134a Refrigeration Schrader Valve"]
["Air-Con",600701,"York Box 4X2 Waterproof - Silicone Moulds."]
["Air-con",600702,"York Box 4X4 Waterproof - Silicone Moulds."]

{"sheet":"Chemical Spares","index":3,"n_rows":11,"n_cols":6,"rows_kept":11,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,1],[3,1,3,2]]}
["Supply and delivery of Various Spares on an “as and when” required basis for five (5) years.  "]
["RFP: 0000/00/00/2024"]
["Bidder's Name",null,{"$f":"'Cover Page '!E21","v":0}]
["Note: ","The bidders may give a proposal on the exact specification outlined by the CSIR or propose an equivalent alternative."]
[]
["Category","CSIR Part Code ","Product technical specifications ","Bidder Must Indicate  Compliance to Specification YES/N0","Any alternative offered compatible to this specification shall be listed below with full functional specification.","Indicate the quality standard the part complies with "]
["Chemical","600195","Degreaser Engine wash 5L heavy-duty cleaner that removes dirt, grease"]
["Chemical","600339","Hand Cleaner 5 Litre - HANDCLEANER MTS WITH GRIT 5KG"]
["Chemical","600443","Paint sprayon electric orange 250MM - Fast Drying Spray Paint Electric Orange 250ml "]
["Chemical","600565","Paint Sprayon Grey 250MM - Fast Drying Spray Paint Electric Grey 250ml "]
["Chemical","600526","Shampoo car 500ML - pH neutral vehicle shampoo"]

{"sheet":"Electrical Spares","index":4,"n_rows":124,"n_cols":6,"rows_kept":124,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,1],[3,1,3,2]]}
["Supply and delivery of Various Spares on an “as and when” required basis for five (5) years.  "]
["RFP: 0000/00/00/2024"]
["Bidder's Name",null,{"$f":"'Cover Page '!E21","v":0}]
["Note: ","The bidders may give a proposal on the exact specification outlined by the CSIR or propose an equivalent alternative."]
[]
["Category","CSIR Part Code","Product technical specifications ","Bidder Must Indicate  Compliance to Specification YES/N0","Any alternative offered compatible to this specification shall be listed below with full functional specification.","Indicate the quality standard the part complies with "]
["Electrical","600827","Circuit breaker 5 AMP single phase QA-1 1 POLE 3KA 5AMP CIRCUIT BREAKER"]
["Electrical","600757","38mm Top Toilet Flusher Double, dual flush toilets with a 38mm hole in the cistern lid"]
["Electrical","600117","Battery AA - Alkaline Zinc-manganese Dioxide Cell · Battery voltage: 1.5Vh"]
["Electrical","600118","Battery AAA - Alkaline Zinc-manganese Dioxide Cell · Battery voltage: 1.5Vh"]
["Electrical","600119","Battery DD Alkaline Batteries, 1.5V LR20 MN1300"]
["Electrical","600120","Battery Rechargeable NIMH9V 2509V 250mah NiMH Rechargeable. H 48 mm × L 25 mm × W 15"]
["Electrical","600766","Butterfly M6  Normal Galvanised"]
["Electrical","600138","Cable Surfix 1.5MM  2XE /1M - SABS Approved"]
["Electrical","600139","Cable Surfix 2.5MM 2XE/M - SABS Approved"]
["Electrical","600140","Cable Surfix 2.5MM 4XE /M - SABS Approved"]
["Electrical","600141","Cable Surfix 4mm 2XE - SABS Approved"]
["Electrical","600142","Cable Surfix 4mm 4XE/M - SABS Approved"]
["Electrical","600786","CBI adapter plate - Steel Adapter plate for DB Boards"]
["Electrical","600154","Circuit breaker 10 AMP Single phase 3KA CBI, QA-1 1 POLE 3KA 10AMP CIRCUIT BREAKER"]
["Electrical","600155","Circuit breaker 20 AMP Single  phase 3KA CBI, QA-1 1 POLE 3KA 20AMP CIRCUIT BREAKER. "]
["Electrical","600156","Circuit breaker 30 AMP Single phase 3KA CBI,  QA-1 1 POLE 3KA 30AMP CIRCUIT BREAKER"]
["Electrical","600204","Earth leakage 63A with overload 3KA Single Phase - QF17ASingle Phase with Overload ProtectionDual Mount"]
["Electrical","600237","Extension box 4X2 Closed White - Steel white coated"]
["Electrical","600238","Extension Box 4X4 Closed White - Steel white coated"]
["Electrical","600239","Extension Box PVC 4X4 Closed White - PVC (Polyvinyl Chloride)"]
["Electrical","600241","Ferrules Wire 10mm - Aluminium Stainless Steel Tinned Copper."]
["Electrical","600242","Ferrules Wire 16mm - Aluminium Stainless Steel Tinned Copper."]
["Electrical","600243","Ferrules Wire 4mm - Aluminium Stainless Steel Tinned Copper."]
["Electrical","600244","Ferrules Wire 6mm - Aluminium Stainless Steel Tinned Copper."]
["Electrical","600266","Fitting centurion Slimline Bulkhead 2D 16Watts - Suitable for compact fluorescent lamps E27, 2 x PL9 and 16watt 2D"]
["Electrical","600267","Fitting downlight tilt with twist lock - Downlight Fitting Tilt Twistlock 80mm Steel White"]
["Electrical","600768","Floodlight 150watt, 20-240 150W COOL WHITE LED ALUM. FLOOD LIGHT IP65"]
["Electrical","600270","Fluorescent tube 16W 2D SQUARE 2 Pin - Fluorescent Lamp 2D Square 16W/835 2-Pin Gr8 Cool White"]
["Electrical","600271","Fluorescent tube 16W 2D SQUARE 4 Pin - 2D 16 Watt 4 Pin Fluorescent Lamp Features Energy Saving"]
["Electrical","600336","Grease Di- Electric NSF1 (284g) CRC Di-Electric Grease Food Grade 284g (3082"]
["Electrical","600357","Insulation Tape Black 0.2mm X 18mmX 20mm - PVC Fire retardant "]
["Electrical","600358","Insulation Tape Blue 0.2mm X 18mmX 20mm - PVC Fire retardant  "]
["Electrical","600359","Insulation Tape Red 0.2mm X 18mmX 20mm - PVC Fire retardant "]
["Electrical","600360","Insulation Tape White 0.2mm X 18mmX 20mm - PVC Fire retardant "]
["Electrical","600841","Isolator 60A 100X100mm Universal Yoke (must be approved for sale by the South African Bureau of Standards)"]
["Electrical","600361","Isolator 60A Triple Pole 100X50mm crabtree (must be approved for sale by the South African Bureau of Standards)"]
["Electrical","600363","Isolator stove ISO Double Pole 30A 100X50mm WHT Cr (must be approved for sale by the South African Bureau of Standards)"]
["Electrical","600364","Isolator Triple Pole 60A  4X4mm Plastic White (must be approved for sale by the South African Bureau of Standards)"]
["Electrical","600300","Light 11/840 Dulux Sta 220-240V cool WHT  E27 600, lifetime of >8,000 hours, this energy-saving light bulb Cool white"]
["Electrical","600808","Light 13W/840 G24q-1 4 pin, Life Time (h):. 20000 ; Dimmable:.Cool white"]
["Electrical","600301","Light 14/840 Dulux Star 220-240V cool WHT B22d 600, lifetime of >8,000 hours, this energy-saving light bulb Cool white"]
["Electrical","600302","Light 26w/840 Dulux G24D-3 2 pin, Average lifespan · 8000 hours. ; Light colour Cool white"]
["Electrical","600305","Light 85W E40 Spiral,  E40 · Daylight 865 · 6000 Hours"]
["Electrical","600307","Light Bulkhead 2XPL9 Clear; 9W Colour: Cool White Lamp Life Hours: 10000"]
["Electrical","600315","Light dimmable LED MR16 12V 6.5W 6500k 60 Deg; MR16 7.5W/865 GU5.3 Dimmable Day Light ; LED · 6500K · 720lm "]
["Electrical","600310","Light GY22TG-20W cool white LED Flood- Led Flood Light Cool White 20W 220V. Lumen 1500 lm ; Wattage 20W ; Body Material Aluminium "]
["Electrical","600805","Light LED 6W E14 - 6W LED (240lm), AC100-240VAC, 160° Beam angle, COOL WHITE (±6000K )"]
["Electrical","600311","Light LED Candle Non dimmable 4W E14; LAMP TYPE: LED FLAME CANDLE; WATTAGE: 4W; VOLTAGE: 220 -240V "]
["Electrical","600312","Light LED Open Channel 1200mm DOUBLE 4 FT - Open channel Empty Body LED Fitting. 4FT 1200mm. Double fitting"]
["Electrical","600313","Light LED Open Channel 1500mm DOUBLE 5 FT - Open channel Empty Body LED Fitting. 5FT 1200mm. Double fitting"]
["Electrical","600809","Light LED Tube 9w/900L 2FT - 230VAC 9W COOL WHITE, FROSTED, 550mm (2Ft) LED T8 TUBE"]
["Electrical","600314","Light non dimmable LED GU10 3W 6500k  110 Deg 450 (GU10 LED Reflector Lamp 4.3 W(50W), 4000K, Cool White)"]
["Electrical","600319","Light pin Dulux  D 18w/840  G24D-2 2 (12000 hours average lifetime. Wattage 18w. Pins 2 pins)"]
["Electrical","600373","Light Switch 1 way 2 Lever Crabtree (must be approved for sale by the South African Bureau of Standards)"]
["Electrical","600321","Tube 549mm 14W T5 840 Cool White. Light Color: 4000 K ; lumens: 1200."]
["Electrical","600418","Lugs wire 4mm X 6mm - (for use in a heavy duty electrical power or grounding application)"]
["Electrical","600779","M8 GALV NUT PKT/100 - Galvanised"]
["Electrical","600421","Masking Tape 18mm X 40m (Tough and stretchable plastic)"]
["Electrical","600807","Motion Sensor PIR32Infrared Motion Sensor 360deg Pir32"]
["Electrical","600806","Motion Sensor PIR361100W 360° Ceiling Mount Eco-Friendly Motion Sensor PIRInfrared Motion Sensor"]
["Electrical","600434","Osram L30W/640 Cool WhiteT8 L 30W/640 G13 Cool White Non-Dimmable"]
["Electrical","600438","Osram ST8V-1.2m-18W-840-EM 16W G13 A+ Cool white1500 life hours"]
["Electrical","600439","Osram ST8V-1.5m-20W-840-EM 20W G13 A+ Cool white1500 life hours"]
["Electrical","600468","Pipe conduit PVC 20mmPVC (Polyvinyl Chloride)"]
["Electrical","600475","Plug crabtree double socket 6881/001 16A 4X4approved for sale by the South African Bureau of Standards"]
["Electrical","600476","Plug Crabtree single socket 6861 16A 4X4approved for sale by the South African Bureau of Standards"]
["Electrical","600477","Plug double switched socket D 4X4mm 16A Red CBIapproved for sale by the South African Bureau of Standards"]
["Electrical","600478","Plug Sockets single  16A 4X4  plastic whiteapproved for sale by the South African Bureau of Standards"]
["Electrical","600479","Plug top dedicated red 16 AMP PVC (must be approved for sale by the South African Bureau of Standards)"]
["Electrical","600480","Plug top Normal black 16 AMP PVC (must be approved for sale by the South African Bureau of Standards)"]
["Electrical","600495","PVC Gland NO 0 - PVC (Polyvinyl Chloride)"]
["Electrical","600496","PVC round box 1 way  20mm - PVC (Polyvinyl Chloride)"]
["Electrical","600497","PVC round box 2 way 20mm - PVC (Polyvinyl Chloride)"]
["Electrical","600782","PVC round box 3 way 20mm - PVC (Polyvinyl Chloride)"]
["Electrical","600498","PVC Trunking 16X16- 2M - PVC (Polyvinyl Chloride)"]
["Electrical","600499","PVC trunking 25X16- 3M - PVC (Polyvinyl Chloride)"]
["Electrical","600500","PVC trunking 40X40 - 3M - PVC (Polyvinyl Chloride)"]
["Electrical","600769","Round Box PVC cover - PVC (Polyvinyl Chloride)"]
["Electrical","600767","Spring washer M8 - DIN 127 B, ZINC"]
["Electrical","600775","Steel coupling 20mm (Solid 20mm Galvanized Steel 76-201-101)"]
["Electrical","600776","Steel pipe 20mm x 1.5mm Mild Steel (ERW) Tube - 250mm Long"]
["Electrical","600774","Steel saddles 20mmMaterial: Steel; Diameter: 20mm; Saddles"]
["Electrical","600773","Steel saddles 25mmMaterial: Steel; Diameter: 25mm; Saddles"]
["Electrical","600576","Switch 1 lever double pole industrial crabtree (must be approved for sale by the South African Bureau of Standards)"]
["Electrical","600577","Switch 20A 1Lever  one way classic Crabtree (must be approved for sale by the South African Bureau of Standards)"]
["Electrical","600578","Switch cover Plate STL 1 lever switch 4x2mm WHT (must be approved for sale by the South African Bureau of Standards)"]
["Electrical","600579","Switch cover plate STL 16A Single socket 4X4 WHT (must be approved for sale by the South African Bureau of Standards)"]
["Electrical","600581","Switch cover plate STL Stove ISO 2X4mm WHT (must be approved for sale by the South African Bureau of Standards)"]
["Electrical","600582","Switch Day/Night LS-20C 15A Day-Night Switch. 230V 15A"]
["Electrical","600585","Switch Pull 1 way  10 AMP; X Rated 1 Way White Ceiling Pull Cord Light Switch"]
["Electrical","600616","Timer programmable 24H Touch screen TRDM; Graphical display on home screen of 24h program schedule "]
["Electrical","600770","Tork craft Hole Saw HSS 20MM; bi-metal and tungsten carbide"]
["Electrical","600771","Tork craft Hole Saw HSS 25MM; bi-metal and tungsten carbide"]
["Electrical","600842","Transfomer 20W-50W; Class : 2 ; Height : 45mm ; Width : 110mm ; Depth : 25mm"]
["Electrical","600675","Wire GP house 1.5mm Black - SABS Approved"]
["Electrical","600676","Wire GP house 1.5mm Earth Green/ Yellow - SABS Approved"]
["Electrical","600678","Wire GP house 10mm Black - SABS Approved"]
["Electrical","600679","Wire GP house 10mm Blue - SABS Approved"]
["Electrical","600680","Wire GP house 10mm Earth Green / yellow - SABS Approved"]
["Electrical","600681","Wire GP house 10mm Red - SABS Approved"]
["Electrical","600682","Wire GP house 10mm White - SABS Approved"]
["Electrical","600683","Wire GP house 2.5mm Black - SABS Approved"]
["Electrical","600811","Wire GP house 2.5mm Blue - SABS Approved"]
["Electrical","600684","Wire GP house 2.5mm Earth Green / Yellow - SABS Approved"]
["Electrical","600685","Wire GP house 2.5mm Red - SABS Approved"]
["Electrical","600686","Wire GP house 4mm Black - SABS Approved"]
["Electrical","600687","Wire GP house 4mm Blue - SABS Approved"]
["Electrical","600688","Wire GP house 4mm Erth Green / Yellow - SABS Approved"]
["Electrical","600689","Wire GP house 4mm Red - SABS Approved"]
["Electrical","600690","Wire GP house 4mm White - SABS Approved"]
["Electrical","600691","Wire GP house 6mm Black - SABS Approved"]
["Electrical","600692","Wire GP house 6mm Blue - SABS Approved"]
["Electrical","600693","Wire GP house 6mm Earth Green / Yellow - SABS Approved"]
["Electrical","600694","Wire GP house 6mm Red - SABS Approved"]
["Electrical","600695","Wire GP house 6mm White - SABS Approved"]
["Electrical","600697","Wire Silicone 4mm Blue - SABS Approved"]
["Electrical","600698","Wire Silicone 4mm Red - SABS Approved"]
["Electrical","600699","Wire Silicone 4mm White - SABS Approved"]

{"sheet":"Fire Systems","index":5,"n_rows":8,"n_cols":6,"rows_kept":8,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,1],[3,1,3,2]]}
["Supply and delivery of Various Spares on an “as and when” required basis for five (5) years.  "]
["RFP: 0000/00/00/2024"]
["Bidder's Name",null,{"$f":"'Cover Page '!E21","v":0}]
["Note: ","The bidders may give a proposal on the exact specification outlined by the CSIR or propose an equivalent alternative."]
[]
["Category","CSIR Part Code ","Product technical specifications ","Bidder Must Indicate  Compliance to Specification YES/N0","Any alternative offered compatible to this specification shall be listed below with full functional specification.","Indicate the quality standard the part complies with "]
["Fire Systems","600750","Battery 12 V 7.2 AH12 (Volt 7.2Amp rechargeable backup battery)"]
["Fire Systems","600747","XP95 Optical Smoke Detector (XP95 Fixed Temperature Heat Detector; Class C/S (90°C))"]

{"sheet":"General Spares","index":6,"n_rows":9,"n_cols":6,"rows_kept":9,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,1],[3,1,3,2]]}
["Supply and delivery of Various Spares on an “as and when” required basis for five (5) years.  "]
["RFP: 0000/00/00/2024"]
["Bidder's Name",null,{"$f":"'Cover Page '!E21","v":0}]
["Note: ","The bidders may give a proposal on the exact specification outlined by the CSIR or propose an equivalent alternative."]
[]
["Category","CSIR Part Code ","Product technical specifications ","Bidder Must Indicate  Compliance to Specification YES/N0","Any alternative offered compatible to this specification shall be listed below with full functional specification.","Indicate the quality standard the part complies with "]
["General","600111","Bung for Flush pipe MK2 - Rubber Bung for Flush Pipe Connector."]
["General","600822","Cleaning Rags 5kg - Cleaning Rags Wrapped (5kg) "]
["General","600196","Degreaser heavy duty 5 litre - WATER BASED DEGREASER (HEAVY DUTY)"]

{"sheet":"Handyman Spares","index":7,"n_rows":72,"n_cols":6,"rows_kept":72,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,1],[3,1,3,2]]}
["Supply and delivery of Various Spares on an “as and when” required basis for five (5) years.  "]
["RFP: 0000/00/00/2024"]
["Bidder's Name",null,{"$f":"'Cover Page '!E21","v":0}]
["Note: ","The bidders may give a proposal on the exact specification outlined by the CSIR or propose an equivalent alternative."]
[]
["Category","CSIR Part Code ","Product technical specifications ","Bidder Must Indicate  Compliance to Specification YES/N0","Any alternative offered compatible to this specification shall be listed below with full functional specification.","Indicate the quality standard the part complies with "]
["Handyman","600801","Adapter female 32mm - HDPE (High-Density Polyethylene)"]
["Handyman","600130","Brush paint size 12mm - Polyester brush for Wall and trim"]
["Handyman","600131","Brush paint size 25mm - Polyester brush for Wall and trim"]
["Handyman","600132","Brush paint size 50mm - Polyester brush for Wall and trim"]
["Handyman","600133","Brush paint size 75mm - Polyester brush for Wall and trim"]
["Handyman","600197","Door closer QS700/1, EN1154 fire rated, size 2-3 with designer arm"]
["Handyman","600851","Door name sliders - Aluminium"]
["Handyman","600852","Door name sliders - Boardroom aluminium"]
["Handyman","600198","Door stop 165mm foot action - Heavy duty "]
["Handyman","600260","Fischer Plug 5X36 100 Per Box (high-quality nylon plug and a zinc-plated nail screw)"]
["Handyman","600261","Fischer Plug 6X42mm 100/box (high-quality nylon plug and a zinc-plated nail screw)"]
["Handyman","600262","Fischer Plug 6X70mm (high-quality nylon plug and a zinc-plated nail screw)"]
["Handyman","600263","Fischer Plug 8X60mm 100 Per box (high-quality nylon plug and a zinc-plated nail screw)"]
["HandyMan","600276","Foam filla spray 500ml - Power polyurethane foam "]
["Handyman","600278","Furniture dove blank on rose union AL6D66-13ASnFinish. Anodised Silver."]
["Handyman","600330","Glue contact genkem 500ml Litre (ADHESIVE GENKEM CLEAR 25ML HAN472)"]
["Handyman","600331","Glue wood 500M (Lunique low VOC formula)"]
["Handyman","600341","Handle aluminium black window Right (Aluminium Window Handle Virage Black)"]
["Handyman","600342","Handle door chrome C2692-13CH Oval Union (Gower Handle CZ682-13CH)"]
["Handyman","600343","Handle door profile chromed unionBackplate size: 152 x 41; Centres: 57mm; Finish: Satin Chrome"]
["Handyman","600351","Hinge aluminium fast fixed 100x75x3.5MM (Medium Duty Butt Hinge 100x75x3.5mm; Fixed Pin)"]
["Handyman","600352","Hinge aluminium fast fixed black (Heavy Duty Fast Fix Hinge with face fix flanges)"]
["Handyman","600353","Hinge But 100MM And screws Brass (BUTT HINGE 100M X 60MM, PAIR, SOLID BRASS)"]
["Handyman","600376","Lock bol barrel 100MM - Chrome finished"]
["Handyman","600377","Lock bolt barrel 150MM - Chrome finished"]
["Handyman","600378","Lock bolt barrel 200MM - Chrome finished"]
["Handyman","600381","Lock cam 16MM - Chrome finished"]
["Handyman","600382","Lock cam 16mm Hook - Chrome finished"]
["Handyman","600384","Lock cam 20MM - Chrome finished"]
["Handyman","600385","Lock cam 20MM Hook - Chrome finished"]
["Handyman","600386","Lock cam 25MM Hook - Chrome finished"]
["Handyman","600388","Lock cylinder cupboard 50MM 5 pin - Brass finished"]
["Handyman","600389","Lock cylinder double oval Union (must meet EN 1303:2015)"]
["Handyman","600391","Lock door mechanism 3 Lever (must meet EN 1303:2015)"]
["Handyman","600392","Lock double euro profile cylinder 2X18SC (must meet EN 1303:2015)"]
["Handyman","600798","Lock knob cylinder euro (must meet EN 1303:2015)"]
["HandyMan","600397","Lock knob cylinder oval 2X13SC Union (must meet EN 1303:2015)"]
["Handyman","600398","Lock latch + strike CT 1178 (must meet EN 1303:2015)"]
["Handyman","600816","Lock Latch bolt (must meet EN 1303:2015)"]
["Handyman","600400","Lock narrow stile aluminium Q35x85 Union (must meet EN 1303:2015)"]
["Handyman","600401","Lock narrow stile mortice Q25x85 Union (must meet EN 1303:2015)"]
["HandyMan","600402","Lock night latch 60mm (must meet EN 1303:2015)"]
["Handyman","600403","Lock oval door mechanisim 8L/12241/78 SS Union  (must meet EN 1303:2015)"]
["Handyman","600404","Lock pad Yale 40MM - Brass Padlock"]
["Handyman","600406","Lock padlock 38MM triicircle (hardenned pad lock)"]
["Handyman","600408","Lock profile door mechanism Union (must meet EN 1303:2015)"]
["Handyman","600409","Lock profile door mechanism Union (must meet EN 1303:2015)"]
["Handyman","600411","Lock waldo hasp + staple brass 115MM - Brass "]
["Handyman","600871","Padlock 50mm - Brass Padlock"]
["Handyman","600884","Padlock 60mm - Brass Padlock"]
["HandyMan","600460","Pattex No more nail 250G synthetic rubber-based adhesive"]
["Handyman","600481","Plugs drywall 30mm (Drywall Plug Nylon 1Fin 30mm)"]
["Handyman","600482","Plugs drywall 40mm (Drywall Plug Nylon 1Fin 40mm)"]
["Handyman","600490","Polyfilla 500G Calcium carbonate in a styrene-acrylate based polymer"]
["Handyman","600799","Push Lock Chrome- Cabinet  Cupboard Push Lock Chrome Plated"]
["Handyman","600494","Putty Standard 125 Gram (SURFACE PREPERATION:​​ dried teak putty)"]
["Handyman","600506","Reflector Yellow 5X300C MFD1403 (M82) Marine Microprismatic Retroreflective Conspicuity Tape"]
["Handyman","600511","Roller paint 225mm (Mohair Roller 225mm)"]
["Handyman","600547","Silicone Soudal Clear 280M - Lacetoxy cure silicon"]
["Handyman","600548","Silicone Soudal White 280M - Lacetoxy cure silicon"]
["Handyman","600588","Tape double sided 120 kg - Heavy duty double sided tape 3mm thick x 24mm wide"]
["Handyman","600589","Tape duct 48MM X 25M   Black (PE Coated cloth as backing with rubber resin adhesive coated)"]
["Handyman","600590","Tape duct 48MM X 25M Silver (PE Coated cloth as backing with rubber resin adhesive coated)"]
["HandyMan","600592","Tape masking 48mmX40m (Thin saturated crepe paper backing)"]
["Handyman","600593","Tape reflective barrier 70X500 Red/WhiteTough and stretchable plastic"]
["Handyman","600594","Tape safety & floor marking 75X35 yellow blackPVC based floor demarcation tape"]

{"sheet":"Mechanical Spares","index":8,"n_rows":30,"n_cols":6,"rows_kept":30,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,1],[3,1,3,2]]}
["Supply and delivery of Various Spares on an “as and when” required basis for five (5) years.  "]
["RFP: 0000/00/00/2024"]
["Bidder's Name",null,{"$f":"'Cover Page '!E21","v":0}]
["Note: ","The bidders may give a proposal on the exact specification outlined by the CSIR or propose an equivalent alternative."]
[]
["Category","CSIR Part Code ","Product technical specifications ","Bidder Must Indicate  Compliance to Specification YES/N0","Any alternative offered compatible to this specification shall be listed below with full functional specification.","Indicate the quality standard the part complies with "]
["Mechanical","600110","Antifreeze & Summer Coolant Concentrate 1 Litre "]
["Mechanical","600836","Ball bearing 6207-2RS Single Row Deep Groove Ball Bearing"]
["Mechanical","600129","Brake Fluide 500ML (Oil Grade. DOT-4)"]
["Mechanical","600135","Bulbs automotive 12V Double 21/5w  P21/5W 24V 21/5W Bay15D"]
["Mechanical","600257","Cable Tie 100mm x 2.5 Black - polyamides (Nylon 6/6)"]
["Mechanical","600259","Cable Tie 150 x 3.6 Black - polyamides (Nylon 6/6)"]
["Mechanical","600277","Cable Tie 200mm x 4.8 Black - polyamides (Nylon 6/6)"]
["Mechanical","600448","Cable Tie 400mm x 4.8 Black - polyamides (Nylon 6/6)"]
["Mechanical","600764","Eclipse Hacksaw Blades 24T carbon steel or high speed steel strip rolls. 24 Teeth"]
["Mechanical","600236","Engine Oil - Pretrol 1 Litre (20w40 Specification)"]
["Mechanical","600711","Multi-Purpose Q20 sprayon 400ml (lubricant"]
["Mechanical","600445","Paint sprayon Silver 250MM (Fast Drying Spray Paint Electric Silver 250ml )"]
["Mechanical","600446","Paint sprayon White 250MM (Fast Drying Spray Paint Electric White 250ml )"]
["Mechanical","600488","Pneumatic trolley Wheel 200mm Rubber Wheel"]
["Mechanical","600256","Rawl Bolt M10 (medium carbon or alloy steel)"]
["Mechanical","600125","Rawl Bolts M8 (medium carbon or alloy steel)"]
["Mechanical","600508","Rods copper brazing 2mm x50mm (Copper Brazing Rods Square 2mm 94% Copper 6% Phosphor. Degussa)"]
["Mechanical","600510","Rods welding 6013 2.5MM (5kg) carbonmanganese steels having a carbon equivalent below 0,28%."]
["Mechanical","600781","Thin cutting Disk 115 x 1.0 x 22 Industrial 2-1 Stainless & Carbon Steel) cutting discs"]
["Mechanical","600638","Valve none return Inline compressed Air 25MM - Brass spring loaded non return valve 1\" female BSP threads "]
["Mechanical","600651","V-Belt VB13NX1000 (rubber, neoprene, and urethane synthetic material)"]
["Mechanical","600662","Wheel trolley swivel brake bracket 100MM - CASTOR WHEEL GREY 100MM PL/BRAKE 50KGS "]
["Mechanical","600672","Wipers Size 16 - durable rubber"]
["Mechanical","600674","Wipers Size 19 - durable rubber"]

{"sheet":"Plumbing Spares","index":9,"n_rows":152,"n_cols":6,"rows_kept":152,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,1],[3,1,3,2]]}
["Supply and delivery of Various Spares on an “as and when” required basis for five (5) years.  "]
["RFP: 0000/00/00/2024"]
["Bidder's Name",null,{"$f":"'Cover Page '!E21","v":0}]
["Note: ","The bidders may give a proposal on the exact specification outlined by the CSIR or propose an equivalent alternative."]
[]
["Category","CSIR Part Code ","Product technical specifications ","Bidder Must Indicate  Compliance to Specification YES/N0","Any alternative offered compatible to this specification shall be listed below with full functional specification.","Indicate the quality standard the part complies with "]
["Plumbing","600705","1 inch Cascade Clamp (CASCADE'S Stainless Steel Repair Clamp)"]
["Plumbing","600709","20mm plason adaptor - HDPE (High-Density Polyethylene)"]
["Plumbing","600706","25mm male plason coupling- HDPE (High-Density Polyethylene)"]
["Plumbing","600704","3/4 inch  Cascade clamp (CASCADE'S Stainless Steel Repair Clamp)"]
["Plumbing","600756","38mm Top Toilet Flusher Single (38MM Toilet Tank Button Single Push Flushing Toilet Button)"]
["Plumbing","600792","Adapter plasson female 63mm - HDPE (High-Density Polyethylene)"]
["Plumbing","600101","Adapter plasson male 32mm - HDPE (High-Density Polyethylene)"]
["Plumbing","600103","Adapter plasson male 75mm - HDPE (High-Density Polyethylene)"]
["Plumbing","600173","Adapter plasson straight 25mm - HDPE (High-Density Polyethylene)"]
["Plumbing","600175","Adapter plasson straight 40mm - HDPE (High-Density Polyethylene)"]
["Plumbing","600176","Adapter plasson straight 50mm - HDPE (High-Density Polyethylene)"]
["Plumbing","600177","Adapter plasson straight 63mm - HDPE (High-Density Polyethylene)"]
["Plumbing","600178","Adapter plasson straight 75mm - HDPE (High-Density Polyethylene)"]
["Plumbing","600104","Adapter PVC female 50mm - PVC (Polyvinyl Chloride)"]
["Plumbing","600105","Adapter PVC Male 50mm - PVC (Polyvinyl Chloride)"]
["Plumbing","600112","Ball cock brass 2 ways  1/2\" Lever (Valve Ball Lever Full Bore FxF 1/2\"Brass 1's)"]
["Plumbing","600113","Ball cock brass 2 ways 3/4\" Lever (Valve Ball Lever Full Bore FxF 3/4\"Brass 1's)"]
["Plumbing","600115","Basin Waste WITH Plug 32mm (BASIN WASTE & PLUG UNSLOTTED CP 32mm) "]
["Plumbing","600122","Bend PVC SV 75X45mm PlainPVC (Polyvinyl Chloride)"]
["Plumbing","600128","Bottle Trap PVC anti-vac 40X40PVC (Polyvinyl Chloride)"]
["Plumbing","600137","Bush galvanized 1/2 X 3/4\"Normal Galvanised"]
["Plumbing","600795","Clamp Cascade 150mm CASCADE'S Stainless Steel Repair Clamp"]
["Plumbing","600793","Clamp Cascade 15mm CASCADE'S Stainless Steel Repair Clamp"]
["Plumbing","600794","Clamp Cascade 50mm CASCADE'S Stainless Steel Repair Clamp"]
["Plumbing","600157","Clamps holderbart 110MM - Holderbat Aluminium Agriney"]
["Plumbing","600158","Clamps holderbart 50MM - Holderbat Aluminium Agriney"]
["Plumbing","600162","Conex Male Coupling 28MM meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600163","Connector flexible 15X350MM"]
["Plumbing","600269","Connector flexible 15X450MM"]
["Plumbing","600164","Connector flush pipe white PF 50 (Colour, White. Material, Rubber. Range)"]
["Plumbing","600165","Connector pan PVC 110mm - PVC (Polyvinyl Chloride)"]
["Plumbing","600166","Copper Elbow 22MM - class 1"]
["Plumbing","600172","Coupler Johnson 3/4\" - Normal Galvanised"]
["Plumbing","600179","Coupling conex female 15mm; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600180","Coupling conex female 22mm; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600181","Coupling conex female 28mm; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600182","Coupling conex male 15mm; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600183","Coupling conex male 22mm; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600184","Coupling conex straight 15mm; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600185","Coupling conex straight 22mm; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600186","Coupling conex straight 28mm; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600187","Coupling copper 15mm - class 1"]
["Plumbing","600189","Coupling solded female 15mmx 3/4\" Brass"]
["Plumbing","600199","Drain Cleaner 5kg - Granules  Material"]
["Plumbing","600200","Drain Cleaner Acid 1 litre (Liquid)"]
["Plumbing","600205","Elbow conex 15MM 90 DEG; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600206","Elbow conex 22MM 90 DEG; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600207","Elbow conex 28MM 90 Deg; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600209","Elbow conex female 15MM 90 DEG; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600210","Elbow conex female 22MM 90DEG; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600211","Elbow conex male 15MM 90DEG; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600212","Elbow conex male 22MM 90DEG; meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600213","Elbow copper 1/2\" - a high purity alloy C12200"]
["Plumbing","600214","Elbow copper 22mm 45 deg - a high purity alloy C12200"]
["Plumbing","600216","Elbow copper 45 degrees 15mm - a high purity alloy C12200"]
["Plumbing","600223","Elbow galvanized 2\" Normal Galvanised"]
["Plumbing","600224","Elbow galvanized 3/4\" Normal Galvanised"]
["Plumbing","600226","Elbow plasson 32MM - HDPE (High-Density Polyethylene)"]
["Plumbing","600230","Elbow PVC 50mm IE - PVC (Polyvinyl Chloride)"]
["Plumbing","600232","Elbow PVC drain plain 75MM - PVC (Polyvinyl Chloride)"]
["Plumbing","600233","Elbow PVC E45 Degrees IE 50MM - PVC (Polyvinyl Chloride)"]
["Plumbing","600272","Flushing mechanism toilet Low level Flash (Pan Connector Agrinet Wirquin Extendable with Fins 110mm)"]
["Plumbing","600274","Flux plumbers 100g (Zinc Chloride and Ammonium Chloride.)"]
["Plumbing","600777","GARDEN TAP 15MM (Crutch heavy-pattern, standard head part, 1/2, rough brass)"]
["Plumbing","600785","GARDEN TAP 20MM (Crutch heavy-pattern, standard head part, 1/2, rough brass)"]
["Plumbing","600293","Gas Ro 2000 360ml/210g - C2000 Oil (CBD 40mg/mL) - 50ml, Cannrix Duo 15:15 ... 210g"]
["Plumbing","600294","Flange Gasket Spiral Element FLG337"]
["Plumbing","600295","Geyser 100 litre - SABS Approved"]
["Plumbing","600297","Geyser 200 Litre - SABS Approved"]
["Plumbing","600299","Geyser vacuum Breaker 22MM (APEX VRV-22CXC 22mm VACUUM CONTROL VALVE CXC.)"]
["Plumbing","600328","Glue Cement Non Pressure PVC 200 - Mlfast setting solvent-based cementing adhesive"]
["Plumbing","600329","Glue Cement Pressure PVC  200Ml (PVC Weld Pipe Cement Adhesive High Pressure)"]
["Plumbing","600338","Gyser underbasin 10 Liter - SABS Approved"]
["Plumbing","600347","Head Part Crossn Converter 5/8\"Cachet Cross Converter Headpart Hot 5/8″ M/P"]
["Plumbing","600349","Headpart with handle 15MM light  pattern taps1/2\" euro head part, chrome-plated"]
["Plumbing","600350","Hemps plumbing 200GFine, long-fibre flax/hemp, which comes from the stem of the flax plant"]
["Plumbing","600355","Hydroboil 10 Liter - SABS Approved"]
["Plumbing","600367","Junction Tee PVC 50MM - PVC (Polyvinyl Chloride)"]
["Plumbing","600368","Junction Tee PVC IE 50MM - PVC (Polyvinyl Chloride)"]
["Plumbing","600370","Junction Y PVC drain pipe 50MM - PVC (Polyvinyl Chloride)"]
["Plumbing","600422","Mixer basin 15MM (Heavy Pattern Medical elbow action sink mixer, chrome)"]
["Plumbing","600423","Mixer sink 1TH Stella # 3396 Star Wall Mount Swivel Sink Mixer Tap"]
["Plumbing","600424","Mixer spout CP swivel (SINK MIXER SPOUT CP LIGHT PATTERN 0305)"]
["Plumbing","600426","Nipple galvanized 1\" - Normal Galvanised"]
["Plumbing","600427","Nipple galvanized 1/2\" - Normal Galvanised"]
["Plumbing","600429","Nipple galvanized 2\" - Normal Galvanised"]
["Plumbing","600817","Nipple Galvanized 3\" - Normal Galvanised"]
["Plumbing","600430","Nipple galvanized 3/4\" - Normal Galvanised"]
["Plumbing","600467","Pillar Tap 15MM Star 211Tap Pillar Cobra Star 15mm Chrome"]
["Plumbing","600470","Pipe drain PVC 50MMX6M PVC (Polyvinyl Chloride)"]
["Plumbing","600472","Pipe galvanised 15MM- Normal Galvanised"]
["Plumbing","600473","Pipe galvanised 22MM - Normal Galvanised"]
["Plumbing","600483","Plugs galvanised 1/2\" - Normal Galvanised"]
["Plumbing","600484","Plugs galvanized 1 1/4\" - Normal Galvanised"]
["Plumbing","600487","Plugs galvanized 3/4\" - Normal Galvanised"]
["Plumbing","600501","Reducer conex 22MMX15MM meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600502","Reducer conex 22MMX28MM meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600503","Reducer copper 22MMx15MM - Class 1"]
["Plumbing","600505","Reducer PVC eccentric 110X50MM PVC (Polyvinyl Chloride)"]
["Plumbing","600512","Rubber S Trap 32X40 MM (S-Trap Reseal Rubber 32 x 40 mm)"]
["Plumbing","600524","Seal Ring toilet Wax Pan (High-quality wax material for superior sealing performance)"]
["Plumbing","600525","Seat Wooden Delux Regal White (024454- WOODEN TOILET SEAT with NYLON HINGE WHITE.)"]
["Plumbing","600797","Shower armS - TAINLESS STEEL SQUARE SHOWER ARM LONG 15x400mm"]
["plumbing","600543","Shower Rose ifunetion minta 95mm diameter. Swivel knuckle. 15mm inner thread"]
["Plumbing","600549","Sink Waste - Unslotted Basin Waste · Height: 74.2mm. Diameter: 63mm."]
["Plumbing","600550","Socket copper 28MM - class 1"]
["Plumbing","600551","Socket double PVC 50mm - PVC (Polyvinyl Chloride)"]
["Plumbing","600823","Socket galvanized 1 &1/4\" - Normal Galvanised"]
["Plumbing","600553","Socket galvanized 1\" - Normal Galvanised"]
["Plumbing","600554","Socket galvanized 1/2\" - Normal Galvanised"]
["Plumbing","600557","Socket galvanized 3/4\" - Normal Galvanised"]
["Plumbing","600560","Solded Male coupling 22mmx3/4\" - Brass"]
["Plumbing","600561","Solder Wire 97/3 2,00MMX250g;  Material, Solder Wire. Range, Copcal. Size, 0.0."]
["Plumbing","600563","Spiral Element 3KW (Spiral Geyser Element – 3Kw)"]
["Plumbing","600572","Stop-end Plain female  PVC 110MM PVC (Polyvinyl Chloride)"]
["Plumbing","600573","Stop-end PVC 50MM White PVC (Polyvinyl Chloride)"]
["Plumbing","600574","Straight adapater copper 22MM - Class 1"]
["Plumbing","600575","Straight male coupling copper 28MM X 22MM - Class 1"]
["Plumbing","600596","Tee Piece conex 15MM meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600597","Tee Piece conex 22MM meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600598","Tee piece copper 15MM class 1"]
["Plumbing","600599","Tee piece copper 22MM class 1"]
["Plumbing","600600","Tee piece galvanized 1/2\" - Normal Galvanised"]
["Plumbing","600608","Tee piece plasson 75MM - HDPE (High-Density Polyethylene)"]
["Plumbing","600610","Thermostat 20AMP Round Geyser Thermostat 20A"]
["Plumbing","600614","Thread tape 19mmX.1mmX30m ."]
["Plumbing","600618","Trap P 40x40 Plain Mini Rubber Reseal"]
["Plumbing","600619","Tube copper 15MMX5.5M Copper pipe Class 1"]
["Plumbing","600620","Tube copper 22MMX5.5M Copper pipe Class 1"]
["Plumbing","600621","Tube copper 28MMX5.5M Copper pipe Class 1"]
["Plumbing","600622","Tube copper tube 42MMX6M Copper pipe Class 1"]
["Plumbing","600623","Union galvanized 1\" - Normal Galvanised"]
["Plumbing","600626","Union galvanized 2\" - Normal Galvanised"]
["Plumbing","600788","Urinal Cartridge 10204 330  WALCRO 102 (S-10204 SPARE CARTRIDGE FOR 330 & 102 VALVES)"]
["Plumbing","600629","Urinal Flush Master - Push Button J6.00 (Spare FJ Push button assembly TLT)"]
["Plumbing","600790","Urinal spreader large - Chrome finished"]
["Plumbing","600635","Valve inlet fill master (Bottom and side inlet valve)"]
["Plumbing","600636","Valve lacto pressure control 100 Kpa (LAT25 LATCO STANDARD CONTROL VALVE 100kPa)"]
["Plumbing","600637","Valve mini ball 15mm (MxF 15mm x 15mm Mini Chrome)"]
["Plumbing","600639","Valve pressure Control 400KPA 22mm (CXC 400KPA Pressure Control Valve (22mm)) "]
["Plumbing","600641","Valve safety female 600 KPA 2mm (406CX FEMALE TEMP & PRESSURE SAFETY VALVE 600kPa 20mm)"]
["Plumbing","600649","Valve Urinal piston (Urinal Piston for Flush Valve Chrome)"]
["Plumbing","600654","Wall Plate 15MM meta-aramid fibers resistant to temperatures of 100-250°C (212-482°F)"]
["Plumbing","600660","Washer Tap 22mm - Vulcanised fibre"]
["Plumbing","600661","Washers Tap 15mm - Vulcanised fibre"]
["plumbing","600671","White Foxy fit Pan connector foxy 01 (Clour White 110mm)"]