{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["Annex A ","Technical returnables","Evaluation Criteria","Sheet3"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"Annex A ","index":0,"n_rows":14,"n_cols":4,"rows_kept":14,"merged":[[0,0,0,3]]}
["AnnexureA – Schedule of Compliance = 100%  compliance"]
[null,"Description and Specification","Schedule A (Eskom’s requirement statement)","COMPLIANT/NON-COMPLIANT"]
[1,"Steel brush (wire brush): Engineering, general cleaning Wire brass and steel hand brushes can be used in a range of applications such as within engineering for rust removal and debris cleaning ","State Compliance & Provide Evidence"]
[2,"Silicon clothes: The silicone courted clothe wipes are so easy to use. Just zip open a foil packet, pull out the silicone-saturated 8″ x 10″ lint-free towel and wipe down a hotstick.","State Compliance & Provide Evidence"]
[3,"Shifting spanner (580mm): Universal adjustable shifting wrench. Forged from high grade steel. Heat treated. Available in various sizes. What's in the box 1x Adjustable Wrench …","State Compliance & Provide Evidence"]
[4,"Nylon sling (3-Ton, 1m): 3 Ton (3000Kg) flat webbing sling 1m wide can be used for many lifting modes. Our webbing lifting slings are made from 100% polyester with reinforced eyes","State Compliance & Provide Evidence"]
[5,"Nylon sling (3-Ton, 500mm): 3 Ton (3000Kg) flat webbing sling 500mm wide can be used for many lifting modes. Our webbing lifting slings are made from 100% polyester with reinforced eyes","State Compliance & Provide Evidence"]
[6,"Karabiners: Oval shaped Karabiner made of round Steel Bar. Self closing & manual locking type Karabiner. Locking by screw locking nut. Alloy Steel. OPEN CONDITION.","State Compliance & Provide Evidence"]
[7,"Pylon hooks (Red): Alloy Steel · Gate opening: 50 mm · Min breaking strength: 23kN · Gate mechanism: Double action/self locking · Weight: 473gm · En std: 362:2004 ·","State Compliance & Provide Evidence"]
[8,"Pylon hooks (Silver): Alloy Steel · Gate opening: 50 mm · Min breaking strength: 23kN · Gate mechanism: Double action/self locking · Weight: 473gm · En std: 362:2004 ·","State Compliance & Provide Evidence"]
[9,"Pylon hooks (Yellow): Alloy Steel · Gate opening: 50 mm · Min breaking strength: 23kN · Gate mechanism: Double action/self locking · Weight: 473gm · En std: 362:2004 ·","State Compliance & Provide Evidence"]
[10,"Polly Dacron rope 12mm 1 drum: Poly Dacron rope is made from polypropylene and Dacron plastic fibers. Fibers are twisted into strands and then the strands are braided into various types","State Compliance & Provide Evidence"]
[11,"Polly Dacron rope16mm 1 drum: Poly Dacron rope is made from polypropylene and Dacron plastic fibers. Fibers are twisted into strands and then the strands are braided into various types","State Compliance & Provide Evidence"]
[12,"Slicon Wipes (Disposable): The disposable wipes are so easy to use. Just zip open a foil packet, pull out the silicone-saturated 8″ x 10″ lint-free towel and wipe down a hotstick.","State Compliance & Provide Evidence"]

{"sheet":"Technical returnables","index":1,"n_rows":8,"n_cols":4,"rows_kept":8}
["Item Number","Technical returnable for evaluation","SUBMITTED","NOT SUBMITTED"]
[1,"Annexure A – Schedule of Compliance to: Specification"]
["a)","Submission of completed Annexure A – Schedule of Compliance (100% Compliance)"]
[2,"Submission of Supporting Certificate or Datasheet"]
["a)","Long Range OTDR  with OLTS Module"]
["a)","Product as per Eskom specification 362:2004"]
["b)"]
["C)"]

{"sheet":"Evaluation Criteria","index":2,"n_rows":8,"n_cols":5,"rows_kept":8,"merged":[[0,0,0,4]]}
["Mandatory Criteria "]
["Item Number","Technical returnable for evaluation","Weighting (%)","Score","COMPLIANT/ NON COMPLIANT"]
[1,"Submission of completed Annexure A – Schedule of Compliance ",{"v":0.9,"d":"90%"}]
[2,"Product as per Eskom specification 362:2004",{"v":0.1,"d":"10%"}]
[]
[]
[]
[null,null,{"$f":"SUM(C3:C7)","v":{"v":1,"d":"100%"}}]

{"sheet":"Sheet3","index":3,"n_rows":9,"n_cols":1,"rows_kept":9,"hidden":true}
["COMPLIANT"]
["NON-COMPLIANT"]
[]
[]
["SUBMITTED"]
["NOT SUBMITTED"]
[]
["COMPLIANT"]
["NON-COMPLIANT"]