{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["A&B Schedules","Deviation Schedule","Test Schedule"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"A&B Schedules","index":0,"n_rows":95,"n_cols":7,"rows_kept":95,"merged":[[0,0,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,1,4,6],[6,4,6,5],[7,4,7,5],[9,1,9,6],[10,1,10,6],[13,2,13,3],[14,2,14,3],[15,3,15,4],[21,3,21,4],[38,3,38,4],[44,3,44,4],[55,3,55,4],[61,3,61,4],[65,3,65,4],[72,2,72,4],[73,2,73,4],[74,3,74,4],[76,3,76,4],[78,3,78,4],[82,0,82,6],[83,1,84,6],[85,1,85,3],[87,0,87,6],[89,0,89,1],[94,2,94,3]]}
["ESKOM TENDER E2719DXLIMOU"]
[null,"Technical Schedules A and B for"]
[null," D-DT-3153 - TAP CONN,TOFF"]
[null,"NB. UNIQUE SCHEDULES ARE TO BE COMPLETED PER SAP NUMBER LISTED BELOW "]
[null,"NB. SUPPLIERS TO CONFIRM ADHERENCE TO THE LATEST PUBLISHED REVISION OF ALL APPLICABLE ESKOM DRAWINGS"]
[]
[{"$nulls":3},"SAP Number","Technical Description "]
[{"$nulls":3},"0175985","TAP CONN,TOFF 9.0-15.0 I/C D3153"]
[]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No",175985,"xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer","Manufacturer name","xxxxxxxxxx"]
[null,"1.1.3",null,"Manufacturer's Product Code","Specify Code","xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Drawing number & Revision number","Specify No and Rev","xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's physical unique identifier indelibly marked. According to clause 5 in the Eskom standard","240-75883110\nClause 5.1","YES"]
[null,"1.1.6","·","Compliance to Eskom Buyer's Guide Drawings"]
[null,"1.1.6.1",null,"T-Off\n - For use according to SAP nr"," Eskom D-DT-3153","YES"]
[null,"1.1.6.2",null,"T-Off\n - Compliance to critical dimensions accoring to SAP number","Eskom D-DT-3153","YES"]
[null,"1.1.6.3",null,"T-Off\n - Tolerances for dimensions up to and including 35mm","±0.7mm","YES"]
[null,"1.1.6.4",null,"T-Off\n - Tolerances for dimensionsabove 35mm","±2% of dimension","YES"]
[null,"1.1.6.5",null,"T-Off\n- Range of system according to SAP number\n- Designed according to Table 1 in the Eskom standard","240-75883110\nClause 3.1.4","YES"]
[{"$nulls":3},"- Conductor diameter range - identified by the colour code given for each fitting. (According to 240-75883110 - table 1) colour codes shall be displayed on the surface of the fitting & names of the standard conductors within the range of the fitting shall be engraved on each fitting.",null,"YES"]
[{"$nulls":3},"- The range and maximum internal diameter of the tubes if Acacia/Magpie/Squirrel/35/Fox conductors","mm",9]
[{"$nulls":3},"- The range and maximum internal diameter of the tubes if Pine/Mink/Oak/Hare conductors","mm",15]
[{"$nulls":3},"Full tension joints will be two piece joints. Full tension fittings will have a smaller range taking ability. The standard range to be covered for mid span full tension joints is:","Magpie; Acacia/Squirrel; 35/Fox ; Pine/Mink; Oak/Hare","xxxxxxxxxx"]
[null,"1.1.6.6",null,"Workmanship shall be according to the Eskom standard","240-75883110\nClause 3.1.1","YES"]
[null,"1.1.6.7",null,"General principles of the design shall be according to the Eskom standard","240-75883110\nClause 3.1.5","YES"]
[null,"1.1.6.8",null,"Materials and fabrication shall be according to the Eskom standard","240-75883110\nClause 3.1.9","YES"]
[null,"1.1.6.9",null,"Bimetallic fittings shall be according to the Eskom standard","240-75883110\nClause 3.1.10"]
[{"$nulls":3},"- Friction welded with the friction weld coated with an approved epoxy compound sealing the weld interface.","Yes/No","xxxxxxxxxx"]
[{"$nulls":3},"- Aluminium lugs with forged copper inserts sealed with an epoxy compound sealing the material interface.","Yes/No","xxxxxxxxxx"]
[null,"1.1.6.10",null,"Item sample required, upon request from Eskom  (As per the Technical Criteria Document)",null,"YES","xxxxxxxxxx"]
[null,1.2,"·","Electrical Properties"]
[{"$nulls":3},"The compression fittings shall:"]
[null,"1.2.1",null,"Provide satisfactory distribution of current in the jointed conductors,","240-75883110\nClause 3.1.6","YES"]
[null,"1.2.2",null,"Sustain the passage of service current and short-circuit current without excessive heating,","240-75883110\nClause 3.1.6","YES"]
[null,"1.2.3",null,"Not increase the resistance of the elements of the circuit in which they are incorporated relative to the resistance of the reference conductor","240-75883110\nClause 3.1.6","YES"]
[null,"1.2.4",null,"They shall provide the lowest possible emission of radio interference voltage, and shall not contribute to corona levels.","240-75883110\nClause 3.1.6","YES"]
[null,1.3,"·","Mechanical Properties"]
[null,"1.3.1",null,"The mounted compression fittings shall comply to the Eskom standard","240-75883110\nClause 3.1.7","YES"]
[null,"1.3.2",null,"Extruded or seam free",null,"xxxxxxxxxx"]
[null,"1.3.3",null,"Alloy used & any treatment material",null,"xxxxxxxxxx"]
[null,"1.3.4",null,"Outside diameter","mm","xxxxxxxxxx"]
[null,"1.3.5",null,"Inside diameter","mm","xxxxxxxxxx"]
[null,"1.3.6",null,"Wall thickness and tolerance","mm","xxxxxxxxxx"]
[null,"1.3.7",null,"Overal length","mm","xxxxxxxxxx"]
[null,"1.3.8",null,"Fitting to compressed by: Die-less 4-pointshallow indentation (approved tool)","Yes/No","xxxxxxxxxx"]
[null,"1.3.9",null,"Number of crimps per connection",null,"xxxxxxxxxx"]
[null,"1.3.10",null,"Do crimps overlap?","Yes/No","xxxxxxxxxx"]
[null,1.4,"·","Classification of fittings"]
[null,"1.4.1",null,"The mounted compression fittings shall comply to the Eskom standard as classified in Table 3","240-75883110\nClause 3.1.8","YES"]
[{"$nulls":3},"- Mechanical",null,"xxxxxxxxxx"]
[{"$nulls":3},"- Functional",null,"xxxxxxxxxx"]
[{"$nulls":3},"- Principle of shape",null,"xxxxxxxxxx"]
[{"$nulls":3},"- Principle of application",null,"xxxxxxxxxx"]
[null,1.5,"·","Electrical jointing compound"]
[null,"1.5.1",null,"The jointing compound shall comply to the Eskom standard","240-75883110\nClause 3.2","YES"]
[null,"1.5.2",null,"Trade name","","xxxxxxxxxx"]
[null,"1.5.3",null,"Type of compound",null,"xxxxxxxxxx"]
[null,"1.5.4",null,"Recommended quantitiy per fitting",null,"xxxxxxxxxx"]
[null,"1.5.5",null,"Are compression sleeves pre-filled and sealed before dispatch?",null,"YES"]
[null,"1.5.6",null,"Source of supply",null,"xxxxxxxxxx"]
[null,"1.5.7",null,"Temperature rating:",null,"xxxxxxxxxx"]
[{"$nulls":3},"- Continous","°C",120]
[{"$nulls":3},"- Max. under short-circuit conditions","°C",150]
[null,"1.5.8",null,"Method of marketing i.e. tube/canister/drum. etc.",null,"per tube"]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to also be provided in electronic format."]
[null,2.1,"·","General"]
[null,"2.1.1",null,"Approved Manufacturer Drawings showing markings and dimensions","1 Set submitted","YES"]
[null,2.2,"·","Test Reports (where applicable)",null,"Required"]
[null,"2.2.1",null,"Has the relevant signed mandatory test schedule been submitted.","Signed Test Schedule Submitted ","YES"]
[null,3,null,"Packaging"]
[null,3.1,null,"Packaging as per the Eskom standard","240-75883110\nClause 5","YES"]
[null,3.2,null,"Installation instructions provided in packaging",null,"YES"]
[]
["ESKOM TENDER E2719DXLIMOU"]
[null,"Deviations to any of the stated requirements are to be captured on the Deviation Schedule."]
[]
[]
[]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":43,"n_cols":6,"rows_kept":43,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[2,7,2,13],[2,14,2,20],[2,21,2,27],[2,28,2,34],[2,35,2,41],[2,42,2,48],[2,49,2,55],[2,56,2,62],[2,63,2,69],[2,70,2,76],[2,77,2,83],[2,84,2,90],[2,91,2,97],[2,98,2,104],[2,105,2,111],[2,112,2,118],[2,119,2,125],[2,126,2,132],[2,133,2,139],[2,140,2,146],[2,147,2,153],[2,154,2,160],[2,161,2,167],[2,168,2,174],[2,175,2,181],[2,182,2,188],[2,189,2,195],[2,196,2,202],[2,203,2,209],[2,210,2,216],[2,217,2,223],[2,224,2,230],[2,231,2,237],[2,238,2,244],[2,245,2,251],[2,252,2,255],[3,0,3,6],[3,7,3,13],[3,14,3,20],[3,21,3,27],[3,28,3,34],[3,35,3,41],[3,42,3,48],[3,49,3,55],[3,56,3,62],[3,63,3,69],[3,70,3,76],[3,77,3,83],[3,84,3,90],[3,91,3,97],[3,98,3,104],[3,105,3,111],[3,112,3,118],[3,119,3,125],[3,126,3,132],[3,133,3,139],[3,140,3,146],[3,147,3,153],[3,154,3,160],[3,161,3,167],[3,168,3,174],[3,175,3,181],[3,182,3,188],[3,189,3,195],[3,196,3,202],[3,203,3,209],[3,210,3,216],[3,217,3,223],[3,224,3,230],[3,231,3,237],[3,238,3,244],[3,245,3,251],[3,252,3,255],[4,0,4,6],[5,2,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[34,0,34,6],[35,0,35,6],[37,0,37,1],[38,2,38,3],[42,2,42,3]]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation schedule"]
[" D-DT-3153 - TAP CONN,TOFF"]
["SAP No: 0175985"]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":28}
["ESKOM TENDER E2719DXLIMOU"]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[null,null,"Name (Print)",null,null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Test Schedule","index":2,"n_rows":28,"n_cols":5,"rows_kept":28,"merged":[[0,0,0,5],[1,0,1,6],[2,0,2,6],[3,1,3,4],[4,0,4,6],[17,1,17,2],[18,1,18,2],[19,1,19,7],[20,1,20,7],[23,1,23,2],[27,1,27,2]]}
["ESKOM TENDER E2719DXLIMOU"]
["Test Report Schedule"]
[" D-DT-3153 - TAP CONN,TOFF"]
[null,"The test reports are required for the selected SAP number listed on this sheet"]
["SAP No: 0175985"]
[]
[null,1,2,3,4]
[null,"Item ","Description","Standard","Report No."]
[null,"2.2.1","General","240-75883110\nClause 4"]
[null,"2.2.2","Qualifying tests:\n1. Type\n2. Sample\n3. Routine\n4. Quantity","240-75883110\nClause 4"]
[null,"2.2.3","Visual inspection and verification of dimensions","240-75883110\nClause 4"]
[null,"2.2.4","Material verification test","240-75883110\nClause 4"]
[null,"2.2.5","Mechanical tension tests","240-75883110\nClause 4"]
[null,"2.2.6","Heat cycle test","240-75883110\nClause 4"]
[null,"2.2.7","Corrosion test","240-75883110\nClause 4"]
[null,"2.2.8","Drift test","240-75883110\nClause 4"]
[null,"2.2.8","Test certificates and samples","240-75883110\nClause 4"]
[]
[]
[]
[null,"SUPPLIER SIGNATURES"]
[]
[]
[null,"Name (Print)",null,null,"Company name"]
[]
[]
[]
[null,"Sign",null,null,"Date"]