{"text_format":"3","workbook":"xls","n_sheets":11,"sheets":["VVVVa","1 P&G","2MV transformers, etc","3 MV overhead","4 Overhead support","5 LV Overhead","6 House connection","7 Dismantling","8 Line Clearing","Summary","Sheet1"],"not_rendered":{"external_links":2,"defined_names":15},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"VVVVa","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"1 P&G","index":1,"n_rows":164,"n_cols":7,"rows_kept":164,"merged":[[1,0,1,6],[2,0,3,0],[2,1,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[21,1,21,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[27,1,27,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[81,1,81,2],[96,1,96,2],[101,1,101,2],[118,1,118,2],[119,1,119,2],[138,1,138,2],[146,1,146,2]],"flags":["formulas_cached_only"]}
["BILL NO 1 - PRELIMINARY AND GENERAL"]
["GUGULETHU PHASE 2 ELECTRIFICATION"]
["Item","Discription",null,"Unit","Qty","Rate","Total Price"]
[]
[]
[1.1,"Condition of Contract"]
[]
["1.1.1","Compliance with all the contractual requirements of the contract,"]
[null,"including providing necessary insurances required to adequately to"]
[null,"cover the works, outage management, weekly progress reporting,"]
[null,"materials management, meetings and quality & environmental"]
[null,"management.",null,"Item",1]
[]
[1.2,"Site Store and Office"]
[]
[null,"Establish facilities on site. The Contractor shall provide "]
[null,"fenced space with fence at least 1.8m high with"]
[null,"a lockable gate for a temporary Site Office and Stores"]
[null,"where all drawings and Specifications will be kept, as"]
[null,"well as the provision of safe and Facilities for Contractor:"]
[]
[null,"a)  Offices & storage sheds",null,"sum",1]
[]
[null,"b)  Establishment of staff accommodation, office "]
[null,"accommodation on site for site meetings and a Clerk "]
[null,"of Works including office furniture and telephone / "]
[null,"telefax as specified and facilities.",null,"sum",1]
[]
[null,"c)  Ablution & latrine facilities",null,"sum",1]
[]
[null,"d)  Tools & equipment",null,"sum",1]
[]
[null,"e)  Water supplies, electric power & communications",null,"sum",1]
[]
["1.2.1","Other fixed charge obligations such as compliance to Covid-19"]
[null,"regulations and other health related disaster management processes",null,"sum",1]
[]
["1.2.2","Removal of all items indicated above upon completion "]
[null,"of construction and making good and restoring of the Site"]
[null,"to the satisfaction of the Consultant.",null,"sum",1]
[]
["1.2.3","Provision of \"As Built\" drawings.",null,"sum",1]
[]
["1.2.4","Construction Name Board  - The Contractor shall place "]
[null,"an order and collect from Eskom and  maintain one"]
[null,"project signboard bearing the name of the project,"]
[null,"the name and logo of Eskom, and the Contractor.",null,"sum",1]
[]
["1.2.5","Provision of samples of materials to be used "]
[null,"(only materials supplied by contractor).",null,"sum",1]
[]
["1.2.6","Provision for the compilation of the Construction"]
[null,"Programme, to be done in MS Project and updated on "]
[null,"a fortnight basis and Quality Assurance Programme for"]
[null,"the works.",null,"sum",1]
[]
[1.3,"Compliance with OHS Act & Construction Regulation"]
[]
["1.3.1","Provision for Legal and Contractual Compliance.",null,"sum",1]
[]
["1.3.2","Provision of personal protective equipment and clothing"]
[null,"for all the contractor's staff, including sub-contractors.",null,"sum",1]
[]
["1.3.3","Provision of safety measures, e.g.. Fall arrest systems, "]
[null,"shoring for safety purposes etc.",null,"sum",1]
[]
["1.3.4","Compliance with OH&S Act & Construction Regulations.",null,"sum",1]
[]
["1.3.5","Orange PVC netting with supports to barricade all excavation,"]
[null,"STOP-GO & danger signs, chevron markers, cones, etc",null,"sum",1]
{"$rows_empty":9}
[null,"Amount carried over to next page"]
[]
["Item","Discription",null,"Unit","Qty","Rate","Total Price"]
[]
[null,"Amount brought forward from previous page"]
[]
[]
[1.4,"Compliance with the Requirements for the "]
[null,"Expanded Public Works Programme (EPWP)."]
[]
[null,"Note: The reports are to be submitted with the"]
[null,"contractors monthly invoice."]
[]
["1.4.1","Compliance with the Requirements for the Expanded "]
[null,"Public Works Programme (incl. monthly reports).",null,"Item",1]
[]
[1.5,"Material Management"]
[]
["1.5.1","The Contractor shall make allowance to receive, transport to site"]
[null,"off load and stack the free-issue materials supplied to the contract."]
[null,"The rate shall also include the implementation and maintenance"]
[null,"Management System for the duration of the contract.",null,"sum",1]
[]
["1.5.2","On Completion of the project, all unused materials"]
[null,"supplied free issue materials shall be reconciled and"]
[null,"qualified.  Once authorised by the Consultant/Project "]
[null,"Co-ordinator, the unused materials shall be transported"]
[null,"to Eskom New Germany stores using the correct",null,"sum",1]
[]
[1.6,"Time Related Items (To maintain site for the"]
[null,"project)"]
[]
["1.6.1","Operate and Maintain Facilities on Site"]
[null,"Facilities for Contractor:"]
[]
[null,"a)  Offices & storage sheds",null,"months",3]
[]
[null,"b)  Ablution & latrine facilities",null,"months",3]
[]
[null,"c)  Tools & equipment",null,"months",3]
[]
[null,"d)  Water supplies, electric power & communications",null,"months",3]
[]
[null,"e)  Health and Safety (Service provider directly accountable to client",null,"months",3]
[null,"for Health and Safety Services)"]
[]
["1.6.2","Social Facilitation Fees ( Service provider directly accountable to client"]
[null,"for ISD Services)",null,"months",3]
[]
["1.6.3","Contract management and full time supervision of the"]
[null,"works.",null,"months",3]
[]
["1.6.4","Overhead costs",null,"months",3]
[]
["1.6.5","Provision for a trainee in electrical engineering - client to appoint student",null,"months",3]
[]
["1.6.6","Community Liaison Officer conversant in Zulu and local "]
[null,"cultural norms.",null,"months",3]
[]
[1.7,"Security"]
[]
["1.7.1","Contractor shall provide security guard/s to ensure the "]
[null,"substation site including offices, storage sheds and all Free"]
[null,"issue material are protected from theft or any damage. The"]
[null,"Contractor needs to ensure that the above mentioned is"]
[null,"guarded 24hrs a day.",null,"months",3]
[]
[1.8,"Special Engineering Services"]
[]
["1.8.1","Provisional sum for additional Engineering Services Inclusive of"]
[null,"Pre-Marketing, Detailed Markerting, Survey, Environmental Assessment &",null,"Prov Sum",1]
[null,"Wayleaves and AMAFA documentation."]
[]
["1.8.2","Allowance for handling and profit in respect of item 1.8.1",null,null,"%"]
[]
["1.8.3","Provisional sum for providing Technical Support on site to the contractor"]
[null,"(Clerk of Works) and Quality Assurance",null,"Prov Sum",1]
[]
["1.8.4","Allowance for handling and profit in respect of item 1.8.3",null,null,"%"]
[]
[]
[]
[]
[]
[null,"TOTAL: Carried forward to summary"]

{"sheet":"2MV transformers, etc","index":2,"n_rows":165,"n_cols":23,"rows_kept":165,"merged":[[1,0,1,8],[2,0,3,0],[2,1,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[2,21,3,21],[2,22,3,22],[16,1,16,2],[17,1,17,2],[19,1,19,2],[21,1,21,2],[23,1,23,2],[25,1,25,2],[27,1,27,2],[32,1,32,2],[82,1,82,2]],"flags":["formulas_cached_only"]}
["BILL NO 2 - MEDIUM VOLTAGE SWITCHGEAR, SECTIONALISERS, TRANSFORMERS, ETC"]
["GUGULETHU PHASE 2 ELECTRIFICATION"]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price",{"$nulls":12},"Total Supply","Total Install"]
[]
[]
[null,"Transformers (Coastal Spec) - Pole Mounted"]
[]
[null,"Installation of existing or new"]
[null,"transformers on an ppropriate structure and secure"]
[null,"as required including the termination of cables"]
[null,"and conductors, the provision of suitable lugs"]
[null,"for 35, 50 or 70mm conductor as required and"]
[null,"all accessories. Excluding cable conductors, and"]
[null,"the transformer structure. Include transport, "]
[null,"offloading / loading, safe storage from appropriate "]
[null,"Eskom store.",{"$nulls":7},"supply","install"]
[{"$nulls":13},"cual","voltex","sgew","cual","voltex","sgew"]
[2.1,"New Transformer 16kVA, 22kV/+240V",null,3021,"No",{"$nulls":4},0,0,{"$nulls":3},{"v":18000,"d":"R 18,000.00"},null,0,{"v":19800,"d":"R 19,800.00"},{"$nulls":3},0,0]
[{"$nulls":16},0,0]
[2.2,"New Transformer 32kVA, 22kV/+240V/-240V",null,3021,"No",{"$nulls":4},0,0,{"$nulls":3},{"v":18600,"d":"R 18,600.00"},null,0,{"v":20460,"d":"R 20,460.00"},{"$nulls":3},0,0]
[{"$nulls":16},0,0]
[2.3,"New Transformer 64kVA, 22kV/415V",null,3021,"No",{"$nulls":4},0,0,{"$nulls":3},{"v":21000,"d":"R 21,000.00"},null,0,{"v":23100.000000000004,"d":"R 23,100.00"},{"$nulls":3},0,0]
[{"$nulls":16},0,0]
[2.4,"New Transformer 50kVA, 22kV/415V",null,3021,"No",{"$nulls":4},0,0,{"$nulls":3},{"v":53000,"d":"R 53,000.00"},null,0,{"v":58300.00000000001,"d":"R 58,300.00"},{"$nulls":3},0,0]
[{"$nulls":16},0,0]
[2.5,"New Transformer 100kVA, 22kV/415V",null,3021,"No",3,{"$nulls":10},0,0,{"$nulls":3},0,0]
[{"$nulls":16},0,0]
[2.6,"New Transformer 200kVA, 22kV/415V",null,3021,"No",{"$nulls":11},0,0,{"$nulls":3},0,0]
[{"$nulls":16},0,0]
[2.7,"Existing transformers to be moved out of line as well as ",{"$nulls":14},0,0]
[null,"upgrading to present standard",null,3021,"No",{"$nulls":11},0,0,{"$nulls":3},0,0]
[{"$nulls":16},0,0]
[2.8,"DATA CONCENTRATOR UNIT,INTERFACE DC450 MODEM",null,621052,"No",3,{"$nulls":10},0,0,{"$nulls":3},0,0]
[null,"G3 PLC DC 230 V (INTERNAL MODEM)",{"$nulls":14},0,0]
[{"$nulls":16},0,0]
[null,"Medium Voltage Surge Arrestors",{"$nulls":14},0,0]
[{"$nulls":16},0,0]
[null,"Supply, deliver, off load on site and safely store",{"$nulls":14},0,0]
[null,"on site the following surge arrestors, complete",{"$nulls":7},0,0,{"$nulls":3},{"v":700,"d":"R 700.00"},null,null,{"v":770.0000000000001,"d":"R 770.00"}]
[null,"with galvanised steel mounting brackets",{"$nulls":15},0]
[null,"for securing the surge arrestor, nuts, bolts, washers",{"$nulls":15},0]
[null,"and lock washers as specified. Secure the surge",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":3},{"v":850,"d":"R 850.00"},null,null,{"v":935.0000000000001,"d":"R 935.00"}]
[null,"arrestor and brackets to the transformer as",{"$nulls":15},0]
[null,"specified including the termination of conductors",{"$nulls":15},0]
[null,"the termination of conductors. Excluding the",{"$nulls":15},0]
[null,"conductors and transformer. Discharge current 10kA.",{"$nulls":15},0]
[{"$nulls":17},0]
[2.9,"22kV, MCOV 19.2kV Surge arrestor, ",{"$nulls":15},0]
[null,"31mm/kV, coastal. NB: Double Surge Arrestors",null,3100,"No",18,{"$nulls":11},0,{"$nulls":3},0,0]
[{"$nulls":17},0]
[{"$nulls":17},0]
[null,"Medium Voltage Sectionalisers and Links",{"$nulls":7},0,0,{"$nulls":3},{"v":2918,"d":"R 2,918.00"},null,null,{"v":3209.8,"d":"R 3,209.80"}]
[{"$nulls":17},0]
[null,"Supply and install link isolators as detailed ",{"$nulls":7},0,0,{"$nulls":3},{"v":4377,"d":"R 4,377.00"},null,null,{"v":4814.700000000001,"d":"R 4,814.70"}]
[null,"including the installation of crossarm brackets",{"$nulls":15},0]
[null,"and the termination of conductors and including",{"$nulls":15},0]
[null,"the drilling of holes in wooden poles as required",{"$nulls":7},0,0,{"$nulls":3},{"v":3058,"d":"R 3,058.00"},null,null,{"v":3363.8,"d":"R 3,363.80"}]
[null,"15k fused links.",{"$nulls":15},0]
[{"$nulls":17},0]
[{"v":2.1,"d":"2.10"},"22kV, Solid links,Single Pole (2.5 X-am) (dual phase).",null,"1848/1849","Set",{"$nulls":4},0,0,{"$nulls":3},{"v":4587,"d":"R 4,587.00"},null,null,{"v":5045.700000000001,"d":"R 5,045.70"},{"$nulls":3},0,0]
[{"$nulls":17},0]
[2.11,"22kV, Solid links,Single Pole Mount (dual phase).",null,3086,"Set",{"$nulls":4},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":3},{"v":4377,"d":"R 4,377.00"},null,null,{"v":4814.700000000001,"d":"R 4,814.70"},{"$nulls":3},0,0]
[{"$nulls":17},0]
[2.12,"22kV, Solid links,Single Pole (2.5 X-am) (three phase).",null,"1848/1849","Set",{"$nulls":12},0,{"$nulls":3},0,0]
[{"$nulls":9},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":3},{"v":3058,"d":"R 3,058.00"},null,null,{"v":3363.8,"d":"R 3,363.80"}]
[2.13,"22kV, Solid links,Single Pole Mount (three phase).",null,3086,"Set",{"$nulls":12},0,{"$nulls":3},0,0]
[{"$nulls":17},0]
[2.14,"22kV, Fuse links,Single Pole (2.5m X-am)",{"$nulls":15},0]
[null,"(dual phase).",null,"1848/1849","Set",{"$nulls":12},0,{"$nulls":3},0,0]
[{"$nulls":17},0]
[2.15,"22kV, Fuse links,Single Pole Mount (dual phase).",null,3086,"Set",{"$nulls":12},0,{"$nulls":3},0,0]
[{"$nulls":17},0]
[2.16,"22kV, Fuse links, Single Pole (2.5m X-am)",{"$nulls":15},0]
[null,"(three phase).",null,"1848/1849","Set",4,{"$nulls":11},0,{"$nulls":3},0,0]
[{"$nulls":17},0]
[2.17,"22kV, Fuse links,Single Pole Mount (three phase).",null,3086,"Set",2,{"$nulls":11},0,{"$nulls":3},0,0]
[{"$nulls":17},0]
[2.18,"22kV, Solid links, Single Pole (3.5m / 4.5m X-arm) / H- Pole ",null,1847,"Set",{"$nulls":4},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":6},0,{"$nulls":3},0,0]
[null,"(three phase).",{"$nulls":15},0]
[{"$nulls":17},0]
[null,"Amount carried over to next page",{"$nulls":15},0,{"$nulls":3},0,0]
[{"$nulls":17},0]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price ",{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":6},0]
[{"$nulls":17},0]
[null,"Amount brought forward from previous page",{"$nulls":15},0,{"$nulls":3},0,0]
[{"$nulls":17},0]
[]
[2.19,"22kV, Fuse links,Single Pole / H- Pole Mount (three phase).",null,1850,"Set",{"$nulls":16},0,0]
[]
[{"v":2.2,"d":"2.20"},"22kV, Fuse links,H- Pole Mount / (2.5m X-arm) (three phase).",null,1851,"Set",{"$nulls":16},0,0]
[]
[2.21,"22kV, Solid links,H- Pole Mount / (3.5m / 4.5m X-arm) ",null,1852,"Set",{"$nulls":16},0,0]
[null,"(three phase)."]
[]
[2.22,"22kV, Fuse links,H- Pole Mount / (2x2.5m X-arm)",null,1853,"Set",{"$nulls":16},0,0]
[null,"(three phase)."]
[]
[{"$nulls":17},0]
[null,"Neutral Surge Arrestor",{"$nulls":15},0]
[{"$nulls":17},0]
[null,"Supply and install a LV surge arrestor including",{"$nulls":15},0]
[null,"lugs and galvanised bolts.",{"$nulls":7},0,0,{"$nulls":3},{"v":350,"d":"R 350.00"},null,null,{"v":385.00000000000006,"d":"R 385.00"}]
[{"$nulls":17},0]
[2.23,"6kV, 10kA Surge Arrestor",null,3088,"No",3,{"$nulls":11},0,{"$nulls":3},0,0]
[{"$nulls":17},0]
[null,"MV Section Breaker\\Voltage Regulator",{"$nulls":15},0]
[{"$nulls":9},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":6},0]
[{"$nulls":17},0]
[2.24,"New Section Breaker 11+22kV, 400A, 8kA with IRTU/Modem.",{"$nulls":15},0]
[null,"(includes the cabling and control box). Allow for transport from",{"$nulls":15},0]
[null,"the supplier, loading/offloading, safe storage.",null,"DDT-30177","Unit",{"$nulls":12},0,{"$nulls":3},0,0]
[{"$nulls":17},0]
[2.25,"New Voltage Regulator, 11 + 22kV 100A/200A 8kA with IRTU ",{"$nulls":15},0]
[null,"(includes the cabling and control box). Allow for transport from",{"$nulls":15},0]
[null,"the supplier, loading/offloading, safe storage.",null,"DDT-3119","Unit",{"$nulls":12},0,{"$nulls":3},0,0]
[{"$nulls":17},0]
[null,"Transformer & Equipment Earthing",{"$nulls":15},0]
[{"$nulls":17},0]
[null,"Supply and install all materials for the complete",{"$nulls":15},0]
[null,"earthing of transformer structures for ABC networks",{"$nulls":15},0]
[null,"as specified. Included in the rate shall be all required",{"$nulls":7},0,0,null,null,{"v":1550,"d":"R 1,550.00"},{"v":1787.18,"d":"R 1,787.18"},null,null,{"v":1965.8980000000001,"d":"R 1,965.90"}]
[null,"spikes, insulated copper conductor, excavations,",{"$nulls":15},0]
[null,"backfilling, etc. The rate shall allow for all required",{"$nulls":15},0]
[null,"MV earth electrodes, consisting of four earth spikes",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":6},0]
[null,"in accordance with the Distribution specification,",{"$nulls":15},0]
[null,"Part 2. Additional earth spikes / conductor shall",{"$nulls":15},0]
[null,"be measuresd alsewhere if required.",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":6},0]
[]
[2.26,"MV Earth (per transformer)",null,"1860/1","No",3,{"$nulls":15},0,0]
[]
[2.27,"MV Earth Section Breaker Earthing",null,"1829B","No",{"$nulls":16},0,0]
[]
[2.28,"MV M/SUB EARTHING w/o continuous earth cond to"]
[null,"source sub (per voltage regulator)",null,"DDT-0855","No",{"$nulls":16},0,0]
{"$rows_empty":30}
[null,"TOTAL: Carried forward to summary",{"$nulls":19},0,0]

{"sheet":"3 MV overhead","index":3,"n_rows":412,"n_cols":18,"rows_kept":412,"merged":[[0,0,0,3],[1,0,1,8],[2,0,3,0],[2,1,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[2,16,3,16],[2,17,3,17],[18,1,18,2],[20,1,20,2],[22,1,22,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[56,1,56,2],[57,1,57,2],[59,1,59,2],[60,1,60,2],[62,1,62,2],[63,1,63,2],[65,1,65,2],[66,1,66,2],[81,1,81,2],[164,1,164,2],[186,1,186,2],[246,1,246,2],[266,1,266,2],[267,1,267,2],[268,1,268,2],[269,1,269,2],[282,1,282,2],[283,1,283,2],[284,1,284,2],[285,1,285,2],[287,1,287,2],[289,1,289,2],[291,1,291,2],[293,1,293,2],[295,1,295,2],[296,1,296,2],[297,1,297,2],[299,1,299,2],[300,1,300,2],[301,1,301,2],[303,1,303,2],[305,1,305,2],[306,1,306,2],[307,1,307,2],[308,1,308,2],[309,1,309,2],[311,1,311,2],[312,1,312,2],[313,1,313,2],[314,1,314,2],[319,1,319,2],[320,1,320,2],[321,1,321,2],[322,1,322,2],[323,1,323,2],[324,1,324,2],[329,1,329,2],[334,1,334,2],[336,1,336,2],[337,1,337,2],[338,1,338,2],[340,1,340,2],[342,1,342,2],[344,1,344,2]],"flags":["formulas_cached_only"]}
["BILL NO 3 - MEDIUM VOLTAGE OVERHEAD DISTRIBUTION SYSTEM"]
["GUGULETHU PHASE 2 ELECTRIFICATION"]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price",{"$nulls":7},"Total Supply","Total Install"]
[]
[]
[null,"CONDUCTOR"]
[]
[null,"Supply, safely store on sealed drums with ends "]
[null,"adequately secured and transport to site conductor"]
[null,"as specified. String conductor as specified "]
[null,"including splices, jumper conductor ties, strain"]
[null,"clamps, suspension clamps, tensioning, "]
[null,"sagging, etc."]
[]
[null,"The following dimensions will all be"]
[null,"Conductor Length with 10% is allowed for "]
[null,"slack & wastage. Additional wastage/slack"]
[null,"Additional wastage/slack is for Contractor's ",{"$nulls":9},"cual","voltex","sgew"]
[null,"account.",{"$nulls":7},"supply","install"]
[]
["3.1","COND,ACSR FOX     8.37D UNGRS   ",null,3136,"m",6522,{"$nulls":3},0,null,{"v":12.2,"d":"R 12.20"},{"v":12.5,"d":"R 12.50"},null,{"v":13.750000000000002,"d":"R 13.75"},null,0,0]
[{"$nulls":14},0]
["3.2","COND, ACSR HARE",null,3136,"m",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[null,"MV STRUCTURES",{"$nulls":12},0]
[{"$nulls":14},0]
[null,"Allow for the  following structures and insulator",{"$nulls":12},0]
[null,"assemblies in accordance with the",{"$nulls":12},0]
[null,"specifications as shown in the drawings.",{"$nulls":12},0]
[null," Include the specified crossarms, drilling of",{"$nulls":12},0]
[null,"holes and treating of such holes, the provision",{"$nulls":12},0]
[null,"of the U-nails and earthwire in accordance ",{"$nulls":12},0]
[null,"with Eskom specifications. All jumpers to",{"$nulls":12},0]
[null,"links and transformers to be installed with",{"$nulls":12},0]
[null,"PVC black pipe.  Supply and installation ",{"$nulls":12},0]
[null,"of 15m of 3/3.35x1100MPa steel wire for a ",{"$nulls":12},0]
[null,"BIL for each pole structure as per Eskom ",{"$nulls":12},0]
[null,"specification. Exclude the supply and planting",{"$nulls":12},0]
[null,"of poles, stays and struts which are measured",{"$nulls":12},0]
[null,"elsewhere. Insulators as per EI090SS. Include",{"$nulls":12},0]
[null,"BIL insulation co-ordination for shared",{"$nulls":12},0]
[null,"MV & LV structures as per 03TB-34 or later",{"$nulls":12},0]
["Note","approved Eskom standard.",{"$nulls":12},0]
[{"$nulls":14},0]
[null,"Supply and install all material as specified for",{"$nulls":12},0]
[null," the construction of the following MV structures.",{"$nulls":12},0]
[null,"Including bonding of hardware and earthing.",{"$nulls":12},0]
[null,"All excavations, poles, crossarms and stay",{"$nulls":12},0]
[null,"are measured elsewhere.  ",{"$nulls":12},0]
[{"$nulls":14},0]
[null,"Note: RX refers to statutory road crossings",{"$nulls":12},0]
[null,"with the relevant DDT0257-10kN-31mm/kV",{"$nulls":12},0]
[null,"post insulator, full wrap tie (suspension ",{"$nulls":12},0]
[null,"structures) or DDT0251 - 40KN-31mm/KV",{"$nulls":12},0]
[null,"longrod with pistolgrips (strain structures).",{"$nulls":12},0]
[{"$nulls":14},0]
["3.3","Delta / 2,5m Wood X-arm - Intermediate - ",{"$nulls":12},0]
[null,"0° Deviation",null,"1340B","No",{"$nulls":4},0,0,{"v":1227,"d":"R 1,227.00"},{"v":1502.78,"d":"R 1,502.78"},null,{"v":1653.058,"d":"R 1,653.06"},null,0,0]
[{"$nulls":14},0]
["3.4","Delta / 2,5m Wood X-arm - Intermediate - ",{"$nulls":12},0]
[null,"0° Deviation (RX).",null,"1340B-RX","No",{"$nulls":4},0,0,{"v":1424.5,"d":"R 1,424.50"},{"v":1573.36,"d":"R 1,573.36"},null,{"v":1730.6960000000001,"d":"R 1,730.70"},null,0,0]
[{"$nulls":14},0]
["3.5","Delta / 2,5m Wood X-arm - Strain - ",{"$nulls":12},0]
[null,"0° Deviation",null,1343,"No",{"$nulls":4},0,0,{"v":1799.7,"d":"R 1,799.70"},{"v":2182.68,"d":"R 2,182.68"},null,{"v":2400.948,"d":"R 2,400.95"},null,0,0]
[{"$nulls":14},0]
["3.6","Delta / 2,5m Wood X-arm - Strain -",{"$nulls":12},0]
[null,"0° Deviation (RX).",null,"1343-RX","No",{"$nulls":4},0,0,{"v":1895,"d":"R 1,895.00"},{"v":2262.68,"d":"R 2,262.68"},null,{"v":2488.948,"d":"R 2,488.95"},null,0,0]
[{"$nulls":14},0]
["3.7","Delta / 2,5m Wood X-arm - Strain - Medium",{"$nulls":12},0]
[null,"(1°- 60°) Deviation.",null,1344,"No",{"$nulls":4},0,0,{"v":1901.65,"d":"R 1,901.65"},{"v":2182.68,"d":"R 2,182.68"},null,{"v":2400.948,"d":"R 2,400.95"},null,0,0]
[{"$nulls":14},0]
["3.8","Delta / 2,5m Wood X-arm - Strain - Medium",{"$nulls":12},0]
[null,"(1°- 60°) Deviation (RX).",null,"1344-RX","No",{"$nulls":4},0,0,null,{"v":2262.68,"d":"R 2,262.68"},null,{"v":2488.948,"d":"R 2,488.95"},null,0,0]
[]
[3.9,"Delta / 2,5m Wood X-arm - Strain - Terminal ",null,1346,"No",{"$nulls":11},0,0]
[{"$nulls":14},0]
[{"v":3.1,"d":"3.10"},"Delta / 2,5m Wood X-arm - Strain - Terminal(RX) ",null,"1346-RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[{"$nulls":14},0]
[null,"Amount carried over to next page",{"$nulls":7},0,0,{"$nulls":3},0,null,0,0]
[{"$nulls":14},0]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price ",{"$nulls":5},0]
[{"$nulls":14},0]
[null,"Amount brought forward from previous page",{"$nulls":12},0,null,0,0]
[{"$nulls":9},0,0,{"$nulls":3},0]
[{"$nulls":14},0]
[3.11,"Delta - H-Pole / 4,5m Wood X-arm - Intermediate",{"$nulls":12},0]
[null,"0° Deviation",null,1370,"No",{"$nulls":4},0,0,{"v":1295.3,"d":"R 1,295.30"},{"v":1427.39,"d":"R 1,427.39"},null,{"v":1570.1290000000001,"d":"R 1,570.13"},null,0,0]
[{"$nulls":14},0]
[3.12,"Delta - H-Pole / 4,5m Wood X-arm - Intermediate",{"$nulls":7},0,0,{"v":1550.3,"d":"R 1,550.30"},{"v":1567.39,"d":"R 1,567.39"},null,{"v":1724.1290000000004,"d":"R 1,724.13"}]
[null,"0° Deviation (RX).",null,"1370-RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.13,"Delta - H-Pole / 4,5m Wood X-arm - Intermediate",{"$nulls":7},0,0,{"$nulls":3},0]
[null,"1°- 10° Deviation",null,1371,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.14,"Delta - H-Pole / 4,5m Wood X-arm - Intermediate",{"$nulls":7},0,0,{"v":3398.55,"d":"R 3,398.55"},{"v":2012.42,"d":"R 2,012.42"},null,{"v":2213.6620000000003,"d":"R 2,213.66"}]
[null,"1°- 10° Deviation",null,"1371-RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.15,"Delta - H-Pole / 4,5m Wood X-arm - Strain",{"$nulls":12},0]
[null,"0° Deviation",null,1373,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":9},0,0,{"v":2310.45,"d":"R 2,310.45"},{"v":2554.54,"d":"R 2,554.54"},null,{"v":2809.994,"d":"R 2,809.99"}]
[3.16,"Delta - H-Pole / 4,5m Wood X-arm - Strain",{"$nulls":12},0]
[null,"0° Deviation (RX).",null,"1373-RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":9},0,0,{"v":2630.4,"d":"R 2,630.40"},{"v":2856.89,"d":"R 2,856.89"},null,{"v":3142.579,"d":"R 3,142.58"}]
[3.17,"Delta – H-Pole / 4,5m Wood X-arm - Strain - Medium",{"$nulls":12},0]
[null,"(1°-60°) Deviation.",null,1374,"No",{"$nulls":4},0,0,{"v":3189,"d":"R 3,189.00"},{"v":3572.09,"d":"R 3,572.09"},null,{"v":3929.2990000000004,"d":"R 3,929.30"},null,0,0]
[{"$nulls":14},0]
[3.18,"Delta – H-Pole / 4,5m Wood X-arm - Strain - Medium",{"$nulls":12},0]
[null,"(1°-60°) Deviation (RX).",null,"1374-RX","No",{"$nulls":4},0,0,{"v":3324,"d":"R 3,324.00"},{"v":3763.86,"d":"R 3,763.86"},null,{"v":4140.246,"d":"R 4,140.25"},null,0,0]
[{"$nulls":14},0]
[3.19,"Delta – H-Pole / 4,5m Wood X-arm - Strain - Terminal",null,1376,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":9},0,0,{"v":3330.5,"d":"R 3,330.50"},{"v":3572.09,"d":"R 3,572.09"},null,{"v":3929.2990000000004,"d":"R 3,929.30"}]
[{"v":3.2,"d":"3.20"},"Delta – H-Pole / 4,5m Wood X-arm - Strain - Terminal (RX).",null,"1376-RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[null,"3 PHASE STRUCTURES GENERAL ARRANGEMENT",{"$nulls":7},0,0,{"v":3540,"d":"R 3,540.00"},{"v":3763.86,"d":"R 3,763.86"},null,{"v":4140.246,"d":"R 4,140.25"}]
[{"$nulls":14},0]
[3.21,"Delta / 2,5m Wood X-arm - Intermediate - ",{"$nulls":7},0,0,{"v":1577,"d":"R 1,577.00"},{"v":1787.39,"d":"R 1,787.39"},null,{"v":1966.1290000000004,"d":"R 1,966.13"}]
[null,"0° Deviation",null,"1740B","No",9,{"$nulls":8},0,null,0,0]
[{"$nulls":14},0]
[3.22,"Delta / 2,5m Wood X-arm - Intermediate - ",{"$nulls":9},{"v":1674.43,"d":"R 1,674.43"},{"v":1907.39,"d":"R 1,907.39"},null,{"v":2098.1290000000004,"d":"R 2,098.13"}]
[null,"0° Deviation (RX).",null,"1740B-RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.23,"Delta / 2,5m Wood X-arm - Strain - 0° Deviation",null,1743,"No",4,{"$nulls":3},0,0,{"$nulls":3},0,null,0,0]
[{"$nulls":14},0]
[3.24,"Delta / 2,5m Wood X-arm - Strain - 0° Deviation (RX).",null,"1743-RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":9},0,0,{"v":1983,"d":"R 1,983.00"},{"v":2998.12,"d":"R 2,998.12"},null,{"v":3297.9320000000002,"d":"R 3,297.93"}]
[3.25,"Delta / 2,5m Wood X-arm - Strain - Medium",{"$nulls":12},0]
[null,"(1°-60°) Deviation",null,1744,"No",7,{"$nulls":8},0,null,0,0]
[{"$nulls":9},0,0,{"v":1983,"d":"R 1,983.00"},{"v":2998.12,"d":"R 2,998.12"},null,{"v":3297.9320000000002,"d":"R 3,297.93"}]
[3.26,"Delta / 2,5m Wood X-arm - Strain - Medium",{"$nulls":12},0]
[null,"(1°-60°) Deviation (RX).",null,"1744-RX","No",{"$nulls":4},0,0,{"v":1735,"d":"R 1,735.00"},{"v":1783.76,"d":"R 1,783.76"},null,{"v":1962.1360000000002,"d":"R 1,962.14"},null,0,0]
[{"$nulls":14},0]
[3.27,"Delta / 2,5m Wood X-arm - Strain - Terminal",null,1746,"No",3,{"$nulls":8},0,null,0,0]
[{"$nulls":9},0,0,{"v":2140,"d":"R 2,140.00"},{"v":2896.01,"d":"R 2,896.01"},null,{"v":3185.6110000000003,"d":"R 3,185.61"}]
[3.28,"Delta / 2,5m Wood X-arm - Strain - Terminal (RX).",null,"1746-RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.29,"3 Phase - Delta / 2x2,5m Wood X-arm – Strain",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},{"v":1924.5,"d":"R 1,924.50"},{"v":2895.34,"d":"R 2,895.34"},null,{"v":3184.8740000000003,"d":"R 3,184.87"}]
[null,"Intermediate - 0° Deviation ",null,1747,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[{"v":3.3,"d":"3.30"},"3 Phase - Delta / 2x2,5m Wood X-arm – Strain",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":3},0]
[null,"Intermediate - 0° Deviation RX",null,"1747-RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.31,"3 Phase - Delta / 2x2,5m Wood X-arm – Strain",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},{"v":2100,"d":"R 2,100.00"},{"v":2927.81,"d":"R 2,927.81"},null,{"v":3220.5910000000003,"d":"R 3,220.59"}]
[null,"Medium(1°-60°) Deviation",null,1748,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.32,"3 Phase - Delta / 2x2,5m Wood X-arm – Strain",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},{"v":2256.4,"d":"R 2,256.40"},{"v":2927.81,"d":"R 2,927.81"},null,{"v":3220.5910000000003,"d":"R 3,220.59"}]
[null,"Medium(1°-60°) Deviation RX",null,"1748-RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.33,"3 Phase - Delta / 2x2,5m Wood X-arm – Strain",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},{"v":4120.34,"d":"R 4,120.34"},{"v":4707.91,"d":"R 4,707.91"},null,{"v":5178.701,"d":"R 5,178.70"}]
[null,"Medium(60°-90°) Deviation",null,1745,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.34,"3 Phase - Delta / 2x2,5m Wood X-arm – Strain",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},{"v":4120.2,"d":"R 4,120.20"},{"v":4707.91,"d":"R 4,707.91"},null,{"v":5178.701,"d":"R 5,178.70"}]
[null,"Terminal",null,1749,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.35,"3 Phase - Delta / 4,5m Wood X-arm - Intermediate – 0°",{"$nulls":12},0]
[null,"Deviation",null,1750,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.36,"3 Phase - Delta / 4,5m Wood X-arm - Intermediate – 0°",{"$nulls":12},0]
[null,"Deviation",null,"1750RX","No",{"$nulls":11},0,0]
[]
[{"$nulls":14},0]
[{"$nulls":14},0]
[null,"Amount carried over to next page",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":3},0,null,0,0]
[{"$nulls":14},0]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price ",{"$nulls":5},0]
[{"$nulls":14},0]
[null,"Amount brought forward from previous page",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":3},0,null,0,0]
[{"$nulls":14},0]
[{"$nulls":14},0]
[3.37,"3 Phase - Delta / 3,5m Wood X-arm - Intermediate – 0°",{"$nulls":12},0]
[null,"Deviation",null,1760,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.38,"3 Phase - Delta / 4,5m Wood X-arm - Strain – 0°",{"$nulls":12},0]
[null,"Deviation",null,"1753RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.39,"3 Phase - Delta / 4,5m Wood X-arm - Strain - Medium  ",{"$nulls":12},0]
[null,"(1°-60°) Deviation",null,1754,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[{"v":3.4,"d":"3.40"},"3 Phase - Delta / 4,5m Wood X-arm - Strain",{"$nulls":12},0]
[null,"Terminal",null,1756,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.41,"3 Phase - H-Pole / 3,5m Wood X-arm - Strain – 0°",{"$nulls":12},0]
[null,"Deviation",null,1763,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.42,"3 Phase - H-Pole / 3,5m Wood X-arm - Strain – Medium",{"$nulls":12},0]
[null,"(1°-60°) Deviation",null,1764,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.43,"3 Phase - H-Pole / 3,5m Wood X-arm - Strain – Medium",{"$nulls":12},0]
[null,"(1°-60°) Deviation",null,"1764RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.44,"3 Phase - H-Pole / 3,5m Wood X-arm - Strain –  Terminal",null,1766,"No",3,{"$nulls":8},0,null,0,0]
[{"$nulls":14},0]
[3.45,"3 Phase - H-Pole / 3,5m Wood X-arm - Strain –  Terminal",null,"1766RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.46,"3 Phase - H-Pole / 2x3,5m Wood X-arm - Strain –  ",{"$nulls":12},0]
[null,"0° Deviation ",null,1767,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.47,"3 Phase - H-Pole / 2x3,5m Wood X-arm - Strain –  ",{"$nulls":12},0]
[null,"0° Deviation ",null,"1767RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":9},0,0,{"v":1940.2,"d":"R 1,940.20"},{"v":1971.11,"d":"R 1,971.11"},null,{"v":2168.221,"d":"R 2,168.22"}]
[3.48,"3 Phase - H-Pole / 2x3,5m Wood X-arm - Strain - Medium",{"$nulls":12},0]
[null,"(1°-60°) Deviation",null,1768,"No",{"$nulls":4},0,0,{"v":2192,"d":"R 2,192.00"},{"v":2037.65,"d":"R 2,037.65"},null,{"v":2241.4150000000004,"d":"R 2,241.42"},null,0,0]
[{"$nulls":14},0]
[3.49,"3 Phase - H-Pole / 2x3,5m Wood X-arm - Strain - Terminal",null,1769,"No",{"$nulls":4},0,0,{"v":1779.2,"d":"R 1,779.20"},{"v":1764.89,"d":"R 1,764.89"},null,{"v":1941.3790000000004,"d":"R 1,941.38"},null,0,0]
[{"$nulls":14},0]
[{"v":3.5,"d":"3.50"},"3 Phase - H-Pole / 4,5m Wood X-arm - Intermediate – 0°",{"$nulls":7},0,0,{"v":1340,"d":"R 1,340.00"},{"v":1519.18,"d":"R 1,519.18"},null,{"v":1671.0980000000002,"d":"R 1,671.10"}]
[null,"Deviation",null,1770,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":9},0,0,{"v":1460,"d":"R 1,460.00"},{"v":1566.76,"d":"R 1,566.76"},null,{"v":1723.4360000000001,"d":"R 1,723.44"}]
[3.51,"3 Phase - H-Pole / 4,5m Wood X-arm - Intermediate",{"$nulls":12},0]
[null,"Small (1°-10°) Deviation",null,1771,"No",{"$nulls":4},0,0,{"v":7945,"d":"R 7,945.00"},{"v":586.94,"d":"R 586.94"},null,{"v":8739.5,"d":"R 8,739.50"},null,0,0]
[{"$nulls":14},0]
[3.52,"3 Phase - H-Pole / 4,5m Wood X-arm - Strain – 0°",{"$nulls":7},0,0,{"$nulls":3},0]
[null,"Deviation",null,1773,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.53,"3 Phase - H-Pole / 4,5m Wood X-arm - Strain – 0°",{"$nulls":12},0]
[null,"Deviation",null,"1773RX","No",{"$nulls":4},0,0,{"v":9730,"d":"R 9,730.00"},{"v":4749.29,"d":"R 4,749.29"},null,{"v":5224.219,"d":"R 5,224.22"},null,0,0]
[{"$nulls":14},0]
[3.54,"3 Phase - H-Pole / 4,5m Wood X-arm - Strain - Medium",{"$nulls":12},0]
[null,"(1°-60°) Deviation",null,1774,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":9},0,0,{"$nulls":3},0]
[3.55,"3 Phase - H-Pole / 4,5m Wood X-arm - Strain - Medium",{"$nulls":12},0]
[null,"(1°-60°) Deviation",null,"1774RX","No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.56,"3 Phase - H-Pole / 4,5m Wood X-arm - Strain - Terminal",null,1776,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.57,"3 Phase - H-Pole / 2x4,5m Wood X-arm - Strain – 0°"]
[null,"Deviation",null,1777,"No",{"$nulls":11},0,0]
[]
[3.58,"3 Phase - H-Pole / 2x4,5m Wood X-arm - Strain - Medium"]
[null,"(1°-60°) Deviation",null,1778,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.59,"3 Phase - H-Pole / 2x4,5m Wood X-arm - Strain - Medium",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":3},0]
[null,"(1°-60°) Deviation",null,"1778RX","No",{"$nulls":9},0,null,0,0]
[]
[{"v":3.6,"d":"3.60"},"3 Phase - H-Pole / 2x4,5m Wood X-arm - Strain - Large",{"$nulls":12},0]
[null,"(61°-90°) Deviation",null,1873,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.61,"3 Phase - H-Pole / 2x4,5m Wood X-arm - Strain - Terminal",null,1779,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.62,"3 Phase - Trips - Strain - 0° Deviation",null,1783,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[3.63,"3 Phase - Trips - Strain - Large (01°-90°) Deviation",null,1784,"No",{"$nulls":9},0,null,0,0]
[{"$nulls":14},0]
[{"$nulls":14},0]
[null,"Amount carried over to next page",{"$nulls":12},0,null,0,0]
[{"$nulls":9},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":3},0]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price ",{"$nulls":5},0]
[{"$nulls":14},0]
[null,"Amount brought forward from previous page",{"$nulls":12},0,null,0,0]
[{"$nulls":14},0]
[{"$nulls":9},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":3},0]
[null,"MV STRUCTURES",{"$nulls":12},0]
[{"$nulls":14},0]
[null,"Allow for the  following structures and insulator",{"$nulls":12},0]
[null,"assemblies in accordance with the",{"$nulls":12},0]
[null,"specifications as shown in the drawings.",{"$nulls":12},0]
[null," Include the specified crossarms, drilling of",{"$nulls":12},0]
[null,"holes and treating of such holes, the provision",{"$nulls":12},0]
[null,"of the U-nails and earthwire in accordance ",{"$nulls":12},0]
[null,"with Eskom specifications. All jumpers to",{"$nulls":7},0,0,{"$nulls":3},0]
[null,"links and transformers to be installed with",{"$nulls":12},0]
[null,"PVC black pipe.  Supply and installation ",{"$nulls":7},0,0,{"$nulls":3},0]
[null,"of 15m of 3/3.35x1100MPa steel wire for a ",{"$nulls":12},0]
[null,"BIL for each pole structure as per Eskom ",{"$nulls":12},0]
[null,"specification. Exclude the supply and planting",{"$nulls":12},0]
[null,"of poles, stays and struts which are measured",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":3},0]
[null,"elsewhere. Insulators as per EI090SS. Include",{"$nulls":12},0]
[null,"BIL insulation co-ordination for shared MV & LV"]
[null,"structures as per 03TB-34 or later approved"]
["Note","Eskom standard."]
[]
[null,"Supply and install all material as specified for"]
[null," the construction of the following MV structures."]
[null,"Including bonding of hardware and earthing."]
[null,"All excavations, poles, crossarms and"]
[null,"stays are measured elsewhere.  "]
[]
[null,"Note: RX refers to statutory road crossings"]
[null,"with the relevant DDT0257-10kN-31mm/kV"]
[null,"post insulator, full wrap tie (suspension"]
[null,"structures) or DDT0251-40kN-31mm/kV"]
[null,"longrod with pistolgrips (strain structures)."]
[]
[3.64,"3-Phase, Take off (2.5m X-arm)",null,1804,"No",4,{"$nulls":10},0,0]
[]
[3.65,"3-Phase, Take off (2.5m X-arm) (RX)",null,"1804-RX","No",{"$nulls":11},0,0]
[]
[3.66,"3-Phase, Take off (2x2.5m X-arm) ",null,1805,"No",{"$nulls":11},0,0]
[]
[3.67,"3-Phase, Take off - H-Pole (3.5m X-arm) ",null,1806,"No",{"$nulls":11},0,0]
[]
[3.68,"3-Phase, Take off - H-Pole (2x3.5m X-arm) ",null,1807,"No",{"$nulls":11},0,0]
[]
[3.69,"2-Phase, Take off (2.5m X-arm)",null,1814,"No",{"$nulls":11},0,0]
[]
[{"v":3.7,"d":"3.70"},"2-Phase, Take off (2.5m X-arm) (RX)",null,"1814-RX","No",{"$nulls":11},0,0]
[]
[3.71,"2-Phase, Take off - 2x2.5m X-arm",null,1815,"No",{"$nulls":11},0,0]
[]
[3.72,"2-Phase, Take off - H-Pole (3.5m X-arm)",null,1816,"No",{"$nulls":11},0,0]
[]
[3.73,"2-Phase, Take off - H-Pole (2x3.5m X-arm)",null,1817,"No",{"$nulls":11},0,0]
[]
[3.74,"Transformer - Single Pole mount (16 -100kVA).",null,1860,"No",{"$nulls":11},0,0]
[]
[3.75,"Transformer - 2 Pole platform mount(H-Pole) - 100 -200kVA",null,1861,"No",2,{"$nulls":10},0,0]
[]
[3.76,"Transformer - Pole mounting out-of-line "]
[null,"(16-100kVA) includes 1860 module, etc… as "]
[null,"per EI067-MVL) and excludes transformer.",null,"1866B","No",{"$nulls":11},0,0]
[]
[3.77,"Transformer - Pole mounting out-of-line "]
[null,"(100-200kVA) includes 1860 module, etc… as "]
[null,"per EI067-MVL) and excludes transformer.",null,"1865B","No",2,{"$nulls":10},0,0]
[]
[3.78,"NEW Recloser Structure, (exclusive of poles, stays, "]
[null,"crossarms, links, excavations, approved anticlimbing "]
[null,"device, etc… as per EI070-MVL.)",null,"1829B","No",{"$nulls":11},0,0]
[]
[3.79,"NEW Voltage Regulator Structure, "]
[null,"(exclusive of poles, stays, crossarms, links,"]
[null,"excavations, approved anticlimbing device, etc… as"]
[null,"per El-124-MVL. Recloser supplied by Eskom)"]
[null,"Allow for transport, loading/offloading, safe storage"]
[null,"from Eskom stores to site.",null,"1833B","No",{"$nulls":11},0,0]
[]
[]
[null,"Amount carried over to next page",{"$nulls":14},0,0]
[]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price "]
[]
[null,"Amount brought forward from previous page",{"$nulls":14},0,0]
[]
[]
[null,"Testing"]
[]
[null,"Allowance shall be made for the complete"]
[null,"testing and commissioning of the Medium Voltage "]
[null,"overhead distribution system."]
[]
[{"v":3.8,"d":"3.80"},"MV Test (per transformer installation)  ",null,null,"No",3,{"$nulls":10},0,0]
[]
[3.81,"MV Test (per Auto-recloser installation) ",null,null,"No",{"$nulls":11},0,0]
[]
[3.82,"MV Test (Voltage Regulator installation) ",null,null,"No",{"$nulls":11},0,0]
[]
[]
[3.83,"Supply the  MV cable includingg transport to site and"]
[null,"install as per Eskom Standards and DDT 0854."]
[]
[null,"Cable 11kV 3C 95SQ Cu  (XLPE Type A) ",null,"0855","m",{"$nulls":11},0,0]
[]
[3.84,"Soft & intermediate material (Excavate by pick & shovel "]
[null,"machine",null,"0855","m",{"$nulls":12},0]
[]
[3.85,"Cable Termination onto Overhead Line. Included is a "]
[null,"termination kit 3C 11kV 90-185SQ OD XLPE, post"]
[null,"insulators, steel pipe, surge arrestor earthing, equip. links "]
[null,"cut/outs or disc etc. Surge arrestors, barbed wire and"]
[null,"danger sign are measured elsewhere.",null,"0851","No",{"$nulls":11},0,0]
{"$rows_empty":51}
[null,"TOTAL: Carried forward to summary",{"$nulls":14},0,0]

{"sheet":"4 Overhead support","index":4,"n_rows":250,"n_cols":19,"rows_kept":250,"merged":[[0,0,0,3],[1,0,1,8],[2,0,3,0],[2,1,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[13,1,13,2],[15,1,15,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[23,1,23,2],[25,1,25,2],[27,1,27,2],[29,1,29,2],[31,1,31,2],[33,1,33,2],[35,1,35,2],[40,1,40,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[83,1,83,2],[115,1,115,2],[116,1,116,2],[118,1,118,2],[119,1,119,2],[121,1,121,2],[122,1,122,2],[124,1,124,2],[125,1,125,2],[127,1,127,2],[128,1,128,2],[146,1,146,2],[147,1,147,2],[148,1,148,2],[149,1,149,2],[151,1,151,2],[158,1,158,2],[163,1,163,2],[182,1,182,2],[183,1,183,2],[184,1,184,2],[185,1,185,2],[186,1,186,2],[187,1,187,2],[188,1,188,2],[190,1,190,2],[191,1,191,2],[193,1,193,2],[194,1,194,2],[196,1,196,2],[197,1,197,2],[199,1,199,2],[200,1,200,2],[215,1,215,2],[216,1,216,2],[217,1,217,2],[218,1,218,2],[219,1,219,2],[220,1,220,2],[221,1,221,2],[222,1,222,2],[223,1,223,2],[224,1,224,2],[225,1,225,2],[226,1,226,2],[227,1,227,2],[228,1,228,2],[229,1,229,2],[230,1,230,2],[231,1,231,2],[232,1,232,2],[234,1,234,2],[236,1,236,2],[240,1,240,2],[241,1,241,2]],"flags":["formulas_cached_only"]}
["BILL NO 4 - SUPPORT FOR OVERHEAD RETICULATION"]
["GUGULETHU PHASE 2 ELECTRIFICATION",{"$nulls":11},"cual","voltex","ttp"]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price"]
[]
[]
[null,"POLES AND CROSSARMS"]
[]
[null,"Supply and safely store the following poles."]
[null,"Transport to site of works and install pole in"]
[null,"excavated hole, including cutting and scafing,"]
[null,"kicking blocks, bonding, treating, etc. Excavations"]
[null,"and compaction are measured elsewhere.",{"$nulls":7},"supply","install"]
[]
[4.1,"7m Pole, 120-139mm top diameter ",null,"0050","No",8,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.2,"9m Pole, 140-159mm top diameter",null,"0055","No",114,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.3,"9m Pole, 160-179mm top diameter",null,"0055","No",{"$nulls":4},0,0,{"$nulls":6},0,0]
[]
[4.4,"10m Pole, 200-219mm top diameter",null,"0052","No",17,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.5,"11m Pole, 160-179mm top diameter",null,"0051","No",{"$nulls":4},0,0,{"$nulls":6},0,0]
[]
[4.6,"11m Pole, 180-199mm top diameter",null,"0051","No",12,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.7,"11m Pole, 200-219mm top diameter",null,"0051","No",{"$nulls":4},0,0,{"$nulls":6},0,0]
[]
[4.8,"12m Pole, 160-180mm top diameter",null,"0053","No",{"$nulls":4},0,0,{"$nulls":6},0,0]
[]
[4.9,"12m Pole, 180-199mm top diameter",null,"0053","No",9,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[{"v":4.1,"d":"4.10"},"12m Pole, 200-219mm top diameter",null,"0053","No",3,{"$nulls":11},0,0]
[]
[4.11,"13m Pole, 160-180mm top diameter",null,"0056","No",{"$nulls":12},0,0]
[{"$nulls":9},0,0]
[4.12,"13m Pole, 180-200mm top diameter",null,"0056","No",{"$nulls":12},0,0]
[{"$nulls":9},0,0]
[null,"Supply, off load and install the following"]
[null,"wooden cross arms.",{"$nulls":7},0,0]
[]
[4.13,"2.5m, 140 -159mm Diameter",null,"0061","No",27,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.14,"3.5m, 140 -159mm Diameter",null,"0063","No",6,{"$nulls":11},0,0]
[]
[4.15,"4.5m, 160 -179mm Diameter",null,"0064","No",4,{"$nulls":11},0,0]
[]
[4.16,"6m, 160 -179mm Diameter",null,"0064","No",3,{"$nulls":11},0,0]
[]
[null,"Stays, Flying Stays and Anti-Climbing Devices"]
[null,"The unit price for a standard stay and an aerial"]
[null,"stay shall exclude the wooden poles, but"]
[null,"include the stay wire, stay rods, insulators,"]
[null,"stay plate, stay guards, bitumastic paint, guy"]
[null,"grip dead end, earthing of stay, line splice,"]
[null,"precast concrete slabs, pole clamp, nuts bolts",{"$nulls":7},0,0,null,null,1076.47]
[null,"and washers etc. "]
[{"$nulls":9},0,0,null,null,571.76]
[null,"The following stays shall be in accordance"]
[null,"with the specifications and shall include stay plate."]
[]
[4.17,"MV Stay (DDT0341 rev 9, BIL 40kV & 150kV)",null,"0341","No",39,{"$nulls":11},0,0]
[]
[4.18,"LV Stay",null,"0341","No",358,{"$nulls":3},0,0,null,null,1699.41,{"$nulls":3},0,0]
[]
[null,"The following flying stays shall be in ",{"$nulls":7},0,0,null,null,1021.18]
[null,"accordance with the specifications and shall"]
[null,"include poles & excavation."]
[]
[4.19,"MV Flying Stay",null,"0343","No",{"$nulls":12},0,0]
[]
[{"v":4.2,"d":"4.20"},"LV Flying Stay",null,"0343","No",{"$nulls":4},0,0,null,null,1372.24,{"$nulls":3},0,0]
[]
[null,"The following struts shall be in accordance with",{"$nulls":7},0,0,null,null,934.59]
[null,"the specifications and shall include poles"]
[null,"& excavation."]
[]
[4.21,"MV Strut",null,"0342","No",4,{"$nulls":11},0,0]
[]
[4.22,"LV Strut",null,1167,"No",14,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[]
[null,"Amount carried over to next page",{"$nulls":15},0,0]
[]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price ",0,0]
[]
[null,"Amount brought forward from previous page",{"$nulls":15},0,0]
[]
[]
[null,"EXCAVATIONS AND COMPACTION"]
[]
[null,"The excavations for service connections are"]
[null,"measured elsewhere."]
[]
[null,"Determination of pole positions, excavate, and "]
[null,"supply a mechanical boring device if required."]
[null,"The rate shall include backfilling, compaction"]
[null,"to 93% MOD AASHTO density, and where necessary "]
[null," the supply and transportation of suitable ground "]
[null,"as may be required to receive the desired "]
[null,"compaction, except where cement is specified. "]
[null,"Any damage to existing services shall be made"]
[null,"good by the Contractor at his own expense and to"]
[null,"the approval or the PM(C)."]
[]
[null,"Before excavation work begins the Contractor "]
[null,"shall evaluate the stability of the ground before"]
[null,"excavation begins. Contractor shall use "]
[null,"warning signs, positioned next to an excavation "]
[null,"within which persons are working or carrying "]
[null,"out inspections.  Ref CR (11).",{"$nulls":7},0,0]
[]
[4.23,"Hole for 7m pole - 1.3m deep",null,"0332","No",8,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.24,"Hole for 9m pole - 1.5m deep",null,"0332","No",114,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.25,"Hole for 10m pole - 1.6m deep",null,"0332","No",17,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.26,"Hole for 11m pole - 1.8m deep",null,"0332","No",12,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.27,"Hole for 12m pole - 2.0m deep",null,"0332","No",12,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.28,"Hole for 13m pole - 2.2m deep",null,"0332","No",0,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.29,"Hole for MV stay - 1.5m deep",null,"0350","No",39,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[{"v":4.3,"d":"4.30"},"Hole for LV stay - 1.4m deep",null,"0350","No",358,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.31,"Hole for MV strut - 1.8m deep",null,"0342","No",4,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.32,"Hole for LV strut - 1.3m deep",null,"0342","No",14,{"$nulls":11},0,0]
[]
[4.33,"Trenching & Back Filling for MV Earth for transformers"]
[null,"(0.5m width x0.5m depth x20m length)",null,null,"No",3,{"$nulls":11},0,0]
[]
["4.34","Provisional blasting  - Up to 2,2m deep.  "]
[null,"Each hole to be verified by Clerk of Works."]
[null,"Develop a method statement in accordance"]
[null,"with explosives legislation, by an appointed",{"$nulls":7},0,0]
[null,"person who is competant in the use of"]
[null,"explosives for excavation work and that the "]
[null,"procedures therein are followed. Ref CR (11)",null,null,"No",{"$nulls":12},0,0]
[]
[4.35,"Rock excavation (the contractor is to provide "]
[null,"adequate measures to ensure a rock hole be"]
[null,"exacavated to the correct depth to faciliate"]
[null,"the correct infrastructure, this may include"]
[null,"the excavation per rock hole by mechanical "]
[null,"means viz. Compressors dependent on diesel ",{"$nulls":7},0,0]
[null,"fuel to accommodate Jackhammer drilling). "]
[null,"These Rock Holes to be verified by the relevant "]
[null,"Clerk of Works. Ref CR (11)",null,null,"No",20,{"$nulls":11},0,0]
{"$rows_empty":10}
[null,"Amount carried over to next page",{"$nulls":15},0,0]
[]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price "]
[]
[null,"Amount brought forward from previous page",{"$nulls":15},0,0]
[]
[{"$nulls":9},0,0]
[null,"POLE LABES"]
[]
[null,"Supply and install labels on all poles in "]
[null,"accordance with the specifications including the "]
[null,"provision of all fixing materials.  Allow for pick-up, ",{"$nulls":7},0,0]
[null,"loading/offloading, transport from appropriate "]
[null,"Eskom store.   Labels to the Eskom Standard "]
[null,"SCSSCAAP5, TQGHSP05 and TQCSS005. "]
[null,"Dynatape, masking tape or Hand written with"]
[null,"permanent marker type labels are not to be"]
[null,"considered for operational labelling under any "]
[null,"circumstances."]
[]
[4.36,"Equipment labels ",null,null,"No",6,{"$nulls":11},0,0]
[]
[4.37,"Mosdorfer fuse rating labels (transformers)",null,null,"No",2,{"$nulls":11},0,0]
[]
[4.38,"Fuse - \"Warning. Open all fuses before"]
[null,"working on line\"",null,null,"No",2,{"$nulls":11},0,0]
[]
[4.39,"Transformer Max fuse notification label",null,null,"No",2,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[{"v":4.4,"d":"4.40"},"Feeder Max Fuse notification label",null,null,"No",2,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.41,"Danger Labels (transformers, links,"]
[null,"anti-climbings)",null,3202,"No",20,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.42,"LV Feeder Labels",null,null,"No",102,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.43,"House Connections Labels",null,null,"No",68,{"$nulls":3},0,0,{"$nulls":6},0,0]
[]
[4.44,"Pole Top Box Phase Labels",null,null,"No",66,{"$nulls":11},0,0]
[{"$nulls":9},0,0]
[null,"GENERAL ITEMS"]
[{"$nulls":9},0,0]
[null,"Supply and install labels Spiral Vibration Dampers"]
[null,"as per the DT Standards",{"$nulls":7},0,0]
[]
[4.45,"Spiral Vibration Dampers (Fox)",null,3175,"ea",{"$nulls":4},0,0,{"$nulls":6},0,0]
[]
[4.46,"Bird Flappers",null,3175,"ea",{"$nulls":12},0,0]
[]
[null,"Supply and Install Anti-Climbing Devices as per "]
[null,"the latest DDT Standards."]
[]
[4.47,"Anti-Climbing Device as per 05TI09. ",{"$nulls":7},0,0,null,null,135]
[null,"Including the removal of existing spikes. "]
[null,"Galvanised wire per DDT3170.  Galvanises ",{"$nulls":7},0,0,null,null,100]
[null,"staples per DDT3129. Install on trfr strs,"]
[null,"struts, parallel MV stay wires, recloser str, "]
[null,"OOL trfr strs, etc, structures where meter "]
[null,"boxes or equipment is installed <2m "]
[null,"above ground, any str having cable secured "]
[null,"by means of strapping <0.5m apart, any"]
[null,"climbable pole str, apparatus etc as per"]
[null,"DDT standard.",null,"0399","per srt",9,{"$nulls":11},0,0]
[]
[4.48,"Supply and Install, where MV & LV Earths "]
[null,"are on the same structure, UV protected black "]
[null,"PVC pipe of length 1.2m on each earth"]
[null,"downwire, cutting the top and bottom of the"]
[null,"pipe at 45deg, split the pipe so as to insert the "]
[null,"MV/LV earth and installing clout nails at the ",{"$nulls":7},0,0,null,null,399]
[null,"bottom and top. ",null,null,"per srt",2,{"$nulls":11},0,0]
[]
[]
[]
[]
[]
[]
[{"$nulls":9},0,0,null,null,60]
[]
[]
[]
[]
[]
[null,"TOTAL: Carried forward to summary",{"$nulls":15},0,0]
[]
[]
[]
[]
[{"$nulls":9},0,0]

{"sheet":"5 LV Overhead","index":5,"n_rows":413,"n_cols":19,"rows_kept":413,"merged":[[0,0,0,2],[1,0,1,8],[2,0,3,0],[2,1,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[27,1,27,2],[28,1,28,2],[29,1,29,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[71,1,71,2],[73,1,73,2],[75,1,75,2],[81,1,81,2],[98,1,98,2],[99,1,99,2],[100,1,100,2],[102,1,102,2],[103,1,103,2],[105,1,105,2],[106,1,106,2],[108,1,108,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[114,1,114,2],[115,1,115,2],[117,1,117,2],[118,1,118,2],[121,1,121,2],[122,1,122,2],[124,1,124,2],[130,1,130,2],[132,1,132,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[138,1,138,2],[139,1,139,2],[141,1,141,2],[142,1,142,2],[145,1,145,2],[162,1,162,2],[206,1,206,2],[207,1,207,2],[208,1,208,2],[209,1,209,2],[210,1,210,2],[211,1,211,2],[212,1,212,2],[213,1,213,2],[214,1,214,2],[227,1,227,2],[228,1,228,2],[229,1,229,2],[230,1,230,2],[231,1,231,2],[242,1,242,2],[246,1,246,2],[250,1,250,2],[251,1,251,2],[252,1,252,2],[253,1,253,2],[254,1,254,2],[255,1,255,2],[256,1,256,2],[257,1,257,2],[258,1,258,2],[322,1,322,2]],"flags":["formulas_cached_only"]}
["BILL NO 5 - OVERHEAD DISTRIBUTION LINES"]
["GUGULETHU PHASE 2 ELECTRIFICATION"]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price"]
[]
[]
[null,"LV ABC (insulated neutral)"]
[]
["Note","The LV insulated aerial bundle conductor system"]
[null,"shall be in accordance with SABS 1418 and"]
[null,"insulated in accordance with SABS 0198 and the"]
[null,"Distribution Standard Part 3.  Ref. EI-092-LVL"]
[]
["Note","The unit rate per meter shall include the tensioning"]
[null,"and stringing of the bundle in accordance with the "]
[null,"sag and stress tables provided by the manufacturer"]
[null,"with all plant, equipment and accessories required "]
[null,"to erect an LV overhead bundled distribution"]
[null,"line i.e. Drum trailer, winch, wind-off pulleys, pulling "]
[null,"rope/cable with connection, dynamometer, "]
[null,"slide-lock, sheathed synthetic-fibre belt, woven "]
[null,"snatch belt, snatch block, tackle, shackle, etc."]
[]
["Note","Measured lengths for stringing shall be net line "]
[null,"route lengths and unit rates shall include for sag,"]
[null,"off-cuts, etc."]
[]
[null,"Supply, safely store and transport to site and "]
[null,"string. The conductor will be delivered on sealed "]
[null,"drums and adequate allowance shall be made for"]
[null,"the correct handling thereof.  "]
[]
[null,"Ensure correct tooling - D 51 Hydraulic "]
[null,"Crimping Tool and dies, a 13mm tube spanner "]
[null,"with T – bar, Phase separators, Slings, Wide "]
[null,"Grooved Pulleys, Steel Pulling Socks, Pulling "]
[null,"Swivels, Rickie, Come-along and"]
[null,"Dynamometers."]
[{"$nulls":9},"supply","install",null,"Cual","Voltex","SGEW"]
[5.1,"Single phase ABC (35mm2,  2 core) - insulated"]
[null,"neutral.",null,3141,"m",{"$nulls":4},0,0,null,null,39,null,42.900000000000006,null,0,0]
[{"$nulls":15},0]
[5.2,"Dual phase ABC (35mm2, 3 core) - insulated",{"$nulls":13},0]
[null,"neutral.",null,3141,"m",{"$nulls":4},0,0,null,null,49,null,53.900000000000006,null,0,0]
[{"$nulls":15},0]
[5.3,"Three phase ABC (35mm2, 4 core) - insulated",{"$nulls":13},0]
[null,"neutral.",null,3141,"m",8000,{"$nulls":3},0,0,null,null,63.5,null,69.85000000000001,null,0,0]
[{"$nulls":15},0]
[5.4,"Dual phase ABC (70mm2, 3 core) - insulated",{"$nulls":13},0]
[null,"neutral.",null,3141,"m",{"$nulls":4},0,0,null,null,99,null,108.9,null,0,0]
[]
[5.5,"Three phase ABC (70mm2, 4 core) - insulated"]
[null,"neutral.",null,3141,"m",{"$nulls":12},0,0]
[{"$nulls":15},0]
[null,"LV STRUCTURES",{"$nulls":13},0]
[{"$nulls":15},0]
[null,"Allow for the assembly of the following LV strain ",{"$nulls":13},0]
[null,"and suspension assemblies in accordance with the ",{"$nulls":13},0]
[null,"specifications shown in the drawings. Including ",{"$nulls":13},0]
[null,"all earthing, drilling of holes and treating of drilled ",{"$nulls":13},0]
[null,"holes. All LV ABC hardware, line connectors, ",{"$nulls":13},0]
[null,"PVC cable ties, nuts, bolts, washers, lock washers ",{"$nulls":13},0]
[null,"shall be allowed for in the appropriate item below.",{"$nulls":13},0]
[null,"Excluding the supply and planting of poles, stays ",{"$nulls":13},0]
[null,"and struts, which are measured elsewhere. ",{"$nulls":13},0]
[null,"Use strain assembly when crossing roads.",{"$nulls":13},0]
[{"$nulls":15},0]
[null,"Supply and install all the materials as specified for ",{"$nulls":13},0]
[null,"following:",{"$nulls":13},0]
[{"$nulls":15},0]
[5.5,"Single Phase ABC Intermediate Assembly",null,1153,"No",{"$nulls":4},0,0,null,null,80.35,null,88.385,null,0,0]
[{"$nulls":15},0]
[5.6,"Single Phase ABC Terminal Assembly",null,1154,"No",{"$nulls":4},0,0,null,null,191.88,null,211.068,null,0,0]
[{"$nulls":15},0]
[5.7,"Single Phase ABC Strain Assembly (0-60 deg)",null,1155,"No",{"$nulls":4},0,0,null,null,340.94,null,375.03400000000005,null,0,0]
[{"$nulls":15},0]
[5.8,"Single Phase ABC Strain Assembly (60-90 deg)",null,1156,"No",{"$nulls":4},0,0,null,null,348.6,null,383.46000000000004,null,0,0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[null,"Amount carried over to next page",{"$nulls":7},0,0,{"$nulls":4},0,null,0,0]
[{"$nulls":15},0]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price ",{"$nulls":6},0]
[{"$nulls":15},0]
[null,"Amount brought forward from previous page",{"$nulls":13},0,null,0,0]
[{"$nulls":9},0,0,{"$nulls":4},0]
[{"$nulls":15},0]
[5.9,"Single Phase ABC Tee from Intermediate",null,1157,"No",{"$nulls":10},0,null,0,0]
[{"$nulls":9},0,0,null,null,209.41,null,230.35100000000003]
[{"v":5.1,"d":"5.10"},"Single Phase ABC  X Suspensionn Assembly",null,1158,"No",{"$nulls":10},0,null,0,0]
[{"$nulls":9},0,0,null,null,364.94,null,401.434]
[5.11,"Single Phase ABC Tee from Strain",null,1159,"No",{"$nulls":10},0,null,0,0]
[{"$nulls":9},0,0,null,null,284.71,null,313.181]
[5.12,"Single Phase ABC  X Intermediate Strain",{"$nulls":13},0]
[null,"Assembly.",null,1160,"No",{"$nulls":10},0,null,0,0]
[{"$nulls":9},0,0,null,null,490.59,null,539.649]
[5.13,"Dual Phase ABC Intermediate Assembly",null,1145,"No",{"$nulls":10},0,null,0,0]
[{"$nulls":9},0,0,null,null,80.35,null,88.385]
[5.14,"Dual Phase ABC Terminal Assembly",null,1146,"No",{"$nulls":10},0,null,0,0]
[{"$nulls":9},0,0,null,null,195.06,null,214.56600000000003]
[5.15,"Dual Phase ABC Strain Assembly (0-60 deg)",null,1147,"No",{"$nulls":10},0,null,0,0]
[{"$nulls":9},0,0,null,null,340.94,null,375.03400000000005]
[5.16,"Dual Phase ABC Strain Assembly (60-90 deg)",null,1148,"No",{"$nulls":10},0,null,0,0]
[{"$nulls":9},0,0,null,null,343.41,null,377.75100000000003]
[5.17,"Dual Phase ABC Tee from Intermediate",null,1149,"No",{"$nulls":10},0,null,0,0]
[{"$nulls":9},0,0,null,null,287.18,null,315.898]
[5.18,"Dual Phase ABC  X Suspensionn Assembly",null,1150,"No",{"$nulls":4},0,0,{"$nulls":4},0,null,0,0]
[{"$nulls":9},0,0,null,null,435.53,null,479.083]
[5.19,"Dual Phase ABC Tee from Strain",null,1151,"No",{"$nulls":4},0,{"$nulls":5},0,null,0,0]
[{"$nulls":9},0,0,null,null,316.94,null,348.634]
[{"v":5.2,"d":"5.20"},"Dual Phase ABC  X Intermediate Strain",{"$nulls":7},0,{"$nulls":5},0]
[null,"Assembly",null,1152,"No",{"$nulls":4},0,{"$nulls":5},0,null,0,0]
[{"$nulls":9},0,0,null,null,472.94,null,520.234]
[5.21,"Thee Phase ABC Suspension Assembly 0-30",null,1100,"No",62,{"$nulls":3},0,{"$nulls":5},0,null,0,0]
[{"$nulls":9},0,0,null,null,80.35,null,88.385]
[5.22,"Thee Phase ABC Terminal Assembly",null,1120,"No",43,{"$nulls":3},0,{"$nulls":5},0,null,0,0]
[{"$nulls":9},0,0,null,null,196.59,null,216.24900000000002]
[5.23,"Thee Phase ABC Strain Assembly (0-60 deg)",null,1121,"No",23,{"$nulls":3},0,{"$nulls":5},0,null,0,0]
[{"$nulls":9},0,0,null,null,340.94,null,375.03400000000005]
[5.24,"Three Phase ABC Strain Assembly (60-90 deg)",null,1122,"No",14,{"$nulls":3},0,{"$nulls":5},0,null,0,0]
[{"$nulls":9},0,0,null,null,348,null,382.8]
[5.25,"Three Phase ABC Tee from Intermediate ",{"$nulls":7},0,{"$nulls":5},0]
[null,"Assembly",null,1140,"No",17,{"$nulls":3},0,{"$nulls":5},0,null,0,0]
[{"$nulls":9},0,0,null,null,277.41,null,305.15100000000007]
[5.26,"Three Phase Intermediate Suspension",{"$nulls":7},0,{"$nulls":5},0]
[null,"Assembly",null,1141,"No",2,{"$nulls":3},0,{"$nulls":5},0,null,0,0]
[{"$nulls":9},0,0,null,null,509.18,null,560.0980000000001]
["5.27","Three Phase ABC Tee from Strain",null,1142,"No",7,{"$nulls":3},0,{"$nulls":5},0,null,0,0]
[{"$nulls":9},0,0,null,null,356.82,null,392.502]
[5.28,"Three Phase ABC  X Intermediate Strain",{"$nulls":7},0,{"$nulls":5},0]
[null,"Assembly.",null,1143,"No",{"$nulls":4},0,{"$nulls":5},0,null,0,0]
[{"$nulls":9},0,0,null,null,505.53,null,556.083]
[{"$nulls":9},0,{"$nulls":5},0]
[{"$nulls":9},0,{"$nulls":5},0]
[{"$nulls":9},0,{"$nulls":5},0]
[{"$nulls":9},0,{"$nulls":5},0]
[{"$nulls":9},0,{"$nulls":5},0]
[{"$nulls":9},0,{"$nulls":5},0]
[{"$nulls":9},0,{"$nulls":5},0]
[{"$nulls":9},0,{"$nulls":5},0]
[{"$nulls":9},0,{"$nulls":5},0]
[{"$nulls":9},0,{"$nulls":5},0]
[{"$nulls":9},0,{"$nulls":5},0]
[{"$nulls":9},0,{"$nulls":5},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[null,"Amount carried over to next page",{"$nulls":13},0,null,0,0]
[{"$nulls":9},0,0,{"$nulls":4},0]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price ",{"$nulls":6},0]
[{"$nulls":15},0]
[null,"Amount brought forward from previous page",{"$nulls":13},0,null,0,0]
[{"$nulls":15},0]
[{"$nulls":9},0,0,{"$nulls":4},0]
[null,"LV FUSE SWITCHES UNITS",{"$nulls":13},0]
[{"$nulls":15},0]
[null,"Supply, deliver to site, off load on site and safely ",{"$nulls":13},0]
[null,"store. The fused switch shall be supplied complete",{"$nulls":13},0]
[null,"with the pole mounting bracket, nuts, bolts,",{"$nulls":13},0]
[null,"washers, etc. for securing the unit to the wooden",{"$nulls":13},0]
[null,"pole. The fuses shall be supplied with the fuse ",{"$nulls":13},0]
[null,"switch unit. Fuse ratings shall be as shown on the ",{"$nulls":13},0]
[null,"drawings. Install the on load fused disconnecting ",{"$nulls":13},0]
[null,"switch on the transformer structure including ",{"$nulls":13},0]
[null,"the drilling of holes as required, including the",{"$nulls":13},0]
[null,"termination of the LV ABC to the unit.  Fuse ratings",{"$nulls":13},0]
[null,"below allow for 120% overload.",{"$nulls":13},0]
[{"$nulls":15},0]
[null,"One fuse unit is for the transformer and one unit",{"$nulls":13},0]
[null,"per LV feeder for isolation/protection.",{"$nulls":13},0]
[{"$nulls":15},0]
[5.29,"63A Dual Phase Load disconnecting switch ",{"$nulls":13},0]
[null,"MORSDORPHER. ",null,"0309","No",{"$nulls":10},0,null,0,0]
[{"$nulls":15},0]
[{"v":5.3,"d":"5.30"},"80A Three Phase Load disconnecting switch ",{"$nulls":7},0,0,null,null,729.41,null,802.351]
[null,"MORSDORPHER. ",null,"0309","No",{"$nulls":10},0,null,0,0]
[{"$nulls":15},0]
[5.31,"100A Three Phase Load disconnecting switch ",{"$nulls":7},0,0,null,null,1023.53,null,1125.883]
[null,"MORSDORPHER. ",null,"0309","No",{"$nulls":10},0,null,0,0]
[{"$nulls":15},0]
[5.32,"160A Three Phase Load disconnecting switch ",{"$nulls":7},0,0,{"$nulls":4},0]
[null,"MORSDORPHER. ",null,"0309","No",8,{"$nulls":9},0,null,0,0]
[{"$nulls":15},0]
[{"$nulls":9},0,0,null,680,1023.53,null,1125.883]
[null,"EARTHING OF LV NETWORK",{"$nulls":13},0]
[{"$nulls":15},0]
["Note","All MV transformer earthing is measured elsewhere",{"$nulls":13},0]
[null,"and all LV earths per structure are measured with",{"$nulls":13},0]
[null,"the structure. This section is intended for LV earths",{"$nulls":13},0]
[null,"at transformers.",{"$nulls":13},0]
[{"$nulls":15},0]
[null,"Allowance shall be made for the testing",{"$nulls":13},0]
[null,"(including earth loop impedance) of the earth ",{"$nulls":13},0]
[null,"resistance for the entire reticulation system in",{"$nulls":13},0]
[null,"accordance with the TN-C-S earthing system as",{"$nulls":13},0]
[null,"defined in the Distribution Standard Part 2 and any ",{"$nulls":13},0]
[null,"earth tests which may be required in terms of the",{"$nulls":13},0]
[null,"standard and detailed specifications. ",{"$nulls":13},0]
[null,"Use 2 x H-Crimps - neutral connection point.",{"$nulls":13},0]
[{"$nulls":15},0]
[5.33,"LV Earth ",null,"0627","No",3,{"$nulls":9},0,null,0,0]
[{"$nulls":15},0]
[null,"LV Pole Mounted Service Boxes (Outdoor)",{"$nulls":7},0,0,null,1450,1776.59,null,1954.249]
[{"$nulls":15},0]
[null,"Supply and install on a wooden and/or concrete",{"$nulls":13},0]
[null,"pole a pole mounted distribution box as specified",{"$nulls":13},0]
[null,"complete with pole mounting brackets, cable ties, ",{"$nulls":13},0]
[null,"PG clamps, miniture circuit breaker(s), neutral,",{"$nulls":13},0]
[null,"phase and earth bars, insulated copper tails for",{"$nulls":13},0]
[null,"connecting to LV ABC, insulation piercing ",{"$nulls":13},0]
[null,"connectors and factory installed cable openings.",{"$nulls":13},0]
[null,"Included shall be the stainless steel strapping and",{"$nulls":13},0]
[null,"buckles and terminations of the tails onto the",{"$nulls":13},0]
[null,"LV ABC.  Allow for required space on DIN rail for ",{"$nulls":13},0]
[null,"appropriate no of EMU's.  Supply and install",{"$nulls":13},0]
[null,"5kA, 5kV rating surge protection between ",{"$nulls":13},0]
[null,"phase-neutral.  To comply with NRS032 and",{"$nulls":13},0]
[null,"DSP0018.",{"$nulls":13},0]
[{"$nulls":15},0]
[5.34,"1-2 Way 1x50A MCB Split Box in ABC Split Box onto ",{"$nulls":13},0]
[null,"Insulated Neutral ABC ",null,3055,"No",62,{"$nulls":9},0,null,0,0]
[{"$nulls":15},0]
[5.35,"1-4 Way 1x50A MCB Split Box in ABC Split Box onto",{"$nulls":13},0]
[null,"Insulated Neutral ABC",null,3055,"No",4,{"$nulls":9},0,null,0,0]
[{"$nulls":9},0,0,null,480,565.29,null,621.819]
[{"$nulls":15},0]
[{"$nulls":15},0]
[null,"Amount carried over to next page",{"$nulls":13},0,null,0,0]
[{"$nulls":15},0]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price ",0,0,{"$nulls":4},0]
[{"$nulls":15},0]
[null,"Amount brought forward from previous page",{"$nulls":13},0,null,0,0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[5.36,"5-8 Way 1x50A MCB Split Box in ABC Split Box onto ",{"$nulls":7},0,0,{"$nulls":4},0]
[null,"Insulated Neutral ABC",null,3055,"No",{"$nulls":10},0,null,0,0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[null,"TESTING",{"$nulls":13},0]
[{"$nulls":15},0]
[null,"Allowance shall be made for the testing of each ",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},null,490,594.71,null,654.181]
[null,"LV ABC distributor on accordance with the project ",{"$nulls":13},0]
[null,"specification. Included shall be the provision of ",{"$nulls":13},0]
[null,"test certificates and all documentation as required.",{"$nulls":13},0]
[{"$nulls":15},0]
[5.37,"LV Test, per zone.  Ref. SCSASABZ1",null,null,"No",3,{"$nulls":3},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":4},0,null,0,0]
[{"$nulls":15},0]
{"$rows_empty":62}
[{"$nulls":15},0]
[{"$nulls":15},0]
[null,"TOTAL: Carried forward to summary",{"$nulls":13},0,null,0,0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":9},0,0,{"$nulls":4},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":9},{"$error":"#REF!"},{"$error":"#REF!"},{"$nulls":4},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]
[{"$nulls":15},0]

{"sheet":"6 House connection","index":6,"n_rows":166,"n_cols":17,"rows_kept":166,"merged":[[0,0,0,2],[1,0,1,8],[2,0,3,0],[2,1,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[5,1,5,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[29,1,29,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[65,1,65,2],[77,1,77,2],[81,1,81,2],[98,1,98,2],[99,1,99,2],[158,1,158,2]],"flags":["formulas_cached_only"]}
["BILL NO 6 - HOUSE CONNECTIONS"]
["GUGULETHU PHASE 2 ELECTRIFICATION"]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price"]
[]
[]
[null,"House Connections"]
[]
[null,"House Connections , test and commissioning "]
[null,"complete. Poles and excavation are measured "]
[null,"elsewhere.",{"$nulls":7},"supply ","install","cual","voltex","sgew"]
[]
[6.1,"Type A",null,"D-DT-0360","No",{"$nulls":4},0,0,{"$nulls":4},0,0]
[]
[6.2,"Type B - (Service pole 100%)",null,"D-DT-0361","No",68,null,null,0,0,0,null,177,null,null,0,0]
[]
[null,"Supply and install, transport to site, offloading and "]
[null,"safely store on the site the following Passive Base "]
[null,"Units, ECU's , complete with rail, galvanised steel"]
[null,"mounting brackets for securing to the dwelling, nuts,"]
[null,"bolts, washers and lock washers as required. "]
[null,"Secure the passive base, "]
[null,"ECU and brackets to the dwelling as required"]
[null,"including the termination of conductors. Excluding"]
[null,"the conductors."]
[]
[6.3,"READYBOARD, 20A,SPLIT METER 2x16A SKTS  D3176",null,null,"No",68,{"$nulls":3},0,0,null,400,null,null,0,0]
[{"$nulls":12},1150]
[6.4,"METER, 20A, SPLIT POWER-RAIL PLC D3145",null,null,"No",68,{"$nulls":3},0,0,{"$nulls":4},0,0]
[]
[6.5,"CIU",null,null,"No",68,{"$nulls":3},0,0,{"$nulls":4},0,0]
[]
[6.6,"Commissioning, testing and supply of certificate of ",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"}]
[null,"compliance",null,null,"No",68,{"$nulls":9},0,0]
[]
[null,"CONDUCTOR"]
[]
["Note","Measured lengths for stringing shall be net line route"]
[null,"lengths and unit rates shall include for sag, "]
[null,"cut-offs etc."]
[]
[null,"Contractor to supply, safely store, transport to site"]
[null,"and string. Installation includes all glands, lugs,"]
[null,"shrouds, termination and connections as required."]
[{"$nulls":9},0,0,null,63]
[6.7,"Cable 1KV 2C 6mm SQ Concentric CU",null,null,"m",4080,{"$nulls":9},0,0]
[{"$nulls":9},0,0]
[6.8,"Cable 1KV 2C 10mm SQ Concentric CU",null,null,"m"]
[]
[6.9,"Submit populated Control Sheet and PCS "]
[null,"CorDaptix information to the Project Engineer"]
[null,"upon the successful energising  of a customer."]
[null,"Payment will only be made upon the successful"]
[null,"loading of the Data onto Eskom's CorDaptix"]
[null,"software system.  Resolve queries raised by",{"$nulls":7},0,0]
[null,"Eskom and the Engineer.",null,null,"No",68,{"$nulls":9},0,0]
[]
[null,"SUNDRY ITEMS"]
[]
[null,"Supply and install pole in excavated hole, including"]
[null,"cutting and scafing, kicking bolts, bonding,"]
[null,"treating, etc. Excavations and compaction are "]
[null,"measured elsewhere."]
[{"$nulls":9},0,0]
[{"v":6.1,"d":"6.10"},"5m Pole, 80-99mm top diameter",null,"0058A","No",68,{"$nulls":9},0,0]
[null,null,"`",{"$nulls":6},0,0]
[6.11,"7m Pole, 100-120mm top diameter",null,"0058B","No",5,{"$nulls":9},0,0]
{"$rows_empty":13}
[null,"Amount carried over to next page",{"$nulls":13},0,0]
[{"$nulls":9},{"$error":"#REF!"},{"$error":"#REF!"}]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price "]
[]
[null,"Amount brought forward from previous page",{"$nulls":13},0,0]
[]
[{"$nulls":9},{"$error":"#REF!"},{"$error":"#REF!"}]
[null,"Determination of pole positions, excavate in all"]
[null,"ground conditions as necessary, and supply a"]
[null,"mechanical boring device if required. The rate shall"]
[null,"include backfilling, compaction to 93% MOD AASHTO"]
[null,"density, and where necessary the supply and "]
[null,"transportation of suitable ground as may be"]
[null,"required to receive the desired compaction, except"]
[null,"where cement is specified. Any damage to existing"]
[null,"services shall be made good by the Contractor"]
[null,"at his own expense and to the approval or the PM(C)."]
[]
[6.12,"Hole for 5m service pole - 1m deep",null,null,"No",68,{"$nulls":9},0,0]
[]
[6.13,"Hole for 7m service pole - 1.3m deep",null,null,"No",5,{"$nulls":3},0,0,{"$nulls":4},0,0]
{"$rows_empty":61}
[{"$nulls":9},0,0]
[]
[null,"TOTAL: Carried forward to summary",{"$nulls":13},0,0]
[]
[{"$nulls":9},{"$error":"#REF!"},{"$error":"#REF!"}]

{"sheet":"7 Dismantling","index":7,"n_rows":82,"n_cols":9,"rows_kept":82,"merged":[[0,0,0,8],[1,0,1,8],[2,0,3,0],[2,1,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[5,1,5,2],[6,1,6,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[22,1,22,2],[24,1,24,2],[26,1,26,2],[79,1,79,2]],"flags":["formulas_cached_only"]}
["BILL NO 7 - DISMANTLING & REMOVAL"]
["GUGULETHU PHASE 2 ELECTRIFICATION"]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price"]
[]
[]
[null,"Recovering of Transformers, Structures,"]
[null,"Insulators and Line Hardware."]
[]
[null,"Allow for the disassembly , removal  transport to "]
[null,"site store & to New Germany and booked back to"]
[null,"stores with the relevant documentation.  Include"]
[null,"the backfilling consolidation and levelling of soil"]
[null,"from excavation at the site of recovery."]
[]
[7.1,"MV Route.",null,null,"m"]
[]
[7.2,"Cable",null,null,"m"]
[]
[7.3,"LV Route",null,null,"m"]
[]
[7.4,"Woodpoles 7m.",null,null,"No"]
[]
[7.5,"Woodpoles 9m.",null,null,"No"]
[]
[7.6,"Woodpoles 10m.",null,null,"No"]
[]
[7.7,"Woodpoles 11m.",null,null,"No"]
[]
[7.8,"Woodpoles 12m.",null,null,"No"]
[]
[7.9,"Stay assemblies complete - MV",null,null,"No"]
[]
[{"v":7.1,"d":"7.10"},"Stay assemblies complete - LV",null,null,"No"]
[]
[7.11,"Struts - MV & LV",null,null,"No"]
[]
[7.12,"Single Pole Structures - MV",null,null,"No"]
[]
[7.13,"Single Pole Structures - LV",null,null,"No"]
[]
[7.14,"H-pole Structures - MV",null,null,"No"]
[]
[7.15,"Cross Arms",null,null,"No"]
[]
[7.16,"Transformers & Equipment (existing)",null,null,"No"]
{"$rows_empty":36}
[null,"TOTAL: Carried forward to summary"]

{"sheet":"8 Line Clearing","index":8,"n_rows":83,"n_cols":10,"rows_kept":83,"merged":[[0,0,0,8],[1,0,1,8],[2,0,3,0],[2,1,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,3,8],[5,1,5,2],[6,1,6,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2]],"flags":["formulas_cached_only"]}
["BILL NO 8 - LINE ROUTE CLEARING"]
["GUGULETHU PHASE 2 ELECTRIFICATION"]
["Item","Description",null,"DDT Ref","Unit","Qty","Supply Rate","Install Rate","Total Price"]
[]
[]
[null,"Line Route Clearing"]
[]
[null,"Clearing of trees from a servitude, including "]
[null,"the stacking or disposal of cuttings and debris"]
[null,"as directed by Eskom, and the poisoning of "]
[null,"stumps with an approved poison/herbicide as "]
[null,"per OHS Act & Eskom Regs.  Cut bush & trees "]
[null,"to be cut into 1-2m strips and removed from"]
[null,"the MV/LV servitude.  Allow for Security for"]
[null,"working in the area where appropriate.  "]
[null,"Contractor to have certificates for ORHVS,"]
[null,"Environmental Awareness, Plant Identification, "]
[null,"Safe Working Procedures & Correct use of"]
[null,"herbicides.  "]
[]
[null,"The CoW must audit quantities below and sign "]
[null,"off as being corrrect, on notification from the "]
[null,"Contractor to do so.  "]
[]
[8.1,"Dense bush (thin dense blackwattles, "]
[null,"thornbush or brambles - not possible to walk"]
[null,"through) MV strip (12m either side of the"]
[null,"centre line) to be cleared and poisoned",null,null,"No",{"$nulls":4},0]
[]
[8.2,"Ditto, but for LV (1m either side of the centre"]
[null,"line or as per Eskom Regulations & TSC"]
[null,"request) and no poisoning required.",null,null,"No",{"$nulls":4},0]
[]
[8.3,"Small trees (less than 30cm diameter"]
[null,"scattered bush or plantation - accessible on"]
[null,"foot) MV strip (12m on either side of the line)"]
[null,"to be cleared and poisoned.",null,null,"No",{"$nulls":4},0]
[]
[8.4,"Ditto, but for LV (1m either side of the centre"]
[null,"line or as per Eskom Regulations & TSC "]
[null,"request) and no poisoning required.",null,null,"No",{"$nulls":4},0]
[]
[8.5,"Large trees (greater than 30cm diameter) "]
[null,"including poisoning/herbicides. Trees to be "]
[null,"cut down as close as possible to the ground,"]
[null,"but not higher than 50mm from ground level.  "]
[null,"Special equipment & expertise to be"]
[null,"accommodated for where required for trees "]
[null,"close to houses, roads, sensitive areas etc...",null,null,"No",{"$nulls":4},0]
[]
[8.6,"Appointment of the Botanist to assess and apply"]
[null,"for Tree-Cutting Permit",null,null,"Prov. Sum",{"$nulls":4},0]
[]
[8.7,"Submission of the approval of the Water Use Licence"]
[null,"for MV/LV lines crossing any rivers",null,null,"Prov. Sum",{"$nulls":4},0]
{"$rows_empty":27}
[null,"TOTAL: Carried forward to summary",{"$nulls":7},0]

{"sheet":"Summary","index":9,"n_rows":61,"n_cols":5,"rows_kept":61,"merged":[[0,0,1,4],[2,0,3,4],[4,0,5,0],[4,1,5,1],[4,2,5,2],[4,3,5,3],[4,4,5,4],[31,2,31,3],[32,2,32,3],[33,1,33,3],[34,1,34,3],[37,2,37,3],[38,2,38,3],[40,2,40,3],[41,2,41,3],[43,1,43,3]],"flags":["formulas_cached_only"]}
["FINAL SUMMARY"]
[]
["GUGULETHU PHASE 2 ELECTRIFICATION"]
[]
["ITEM","DESCRIPTION","TOTAL SUPPLY","TOTAL INSTALL","TOTAL PRICE "]
[]
[]
["1","PRELIMINARY AND GENERAL."]
[]
[]
["2","MEDIUM VOLTAGE SWITCHGEAR, SECTIONALISERS, "]
[null,"TRANSFORMERS, ETC."]
[]
["3","MEDIUM VOLTAGE OVERHEAD DISTRIBUTION SYSTEM."]
[]
[]
["4","SUPPORT FOR OVERHEAD RETICULATION."]
[]
[]
["5","LOW VOLTAGE OVERHEAD DISTRIBUTION LINES."]
[]
[]
["6","CUSTOMER SERVICES AND GENERAL."]
[]
[]
["7","DISMANTLING."]
[]
[]
["8","LINE CLEARING."]
[]
[]
[null,null,"SUB TOTAL A="]
[]
[]
[null,"Add: Contingencies ( % of SUBTOTAL A )="]
[]
[]
[null,null,"SUBTOTAL B="]
[]
[]
[null,null,"Add: VAT (15% of SUBTOTAL B)="]
[]
[]
[null,"TOTAL CARRIED FORWARD TO FORM OF OFFER="]
[]
[]
[]
[]
[]
["Signed on behalf of the Tenderer….......................................................................................................( Signature)"]
[]
[]
[]
[]
["Date: …........................................................................................................................"]
[]
[]
[]
[]
[]
["Tenderer's Name:…...........................................................................................................................( Company Name)"]

{"sheet":"Sheet1","index":10,"n_rows":59,"n_cols":4,"rows_kept":59,"hidden":true,"flags":["formulas_cached_only"]}
{"$rows_empty":58}
[{"$nulls":3},"mkkkjjjjbgghjk"]