{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["0402501","Deviation Schedule","Test Schedule","Eskom Drawing"],"not_rendered":{"images":1,"external_links":2,"defined_names":4},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"0402501","index":0,"n_rows":60,"n_cols":7,"rows_kept":60,"merged":[[1,1,1,6],[2,1,2,6],[3,1,3,6],[6,1,6,6],[7,1,7,6],[10,2,10,3],[11,2,11,3],[12,3,12,4],[18,1,19,1],[28,3,28,4],[33,3,33,4],[39,3,39,5],[41,3,41,5],[48,1,49,6],[50,1,50,6],[52,0,52,6],[54,0,54,1],[59,2,59,3]],"flags":["formulas_cached_only"]}
[]
[null,"ESKOM TENDER E2719DXLIMOU"]
[null,"Technical Schedules A and B for"]
[null," CLAMP,SUSP CRADLE CON 8,0-18,0 D3008"]
[null,"NB. SUPPLIERS TO CONFIRM ADHERENCE TO THE LATEST PUBLISHED REVISION OF ALL APPLICABLE ESKOM DRAWINGS"]
[]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,3,4,5]
[null,"Item ","Description",null,"Requirement","Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No",null,{"v":402501,"d":"0402501"},"xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer","Manufacturer name","xxxxxxxxxx"]
[null,"1.1.3",null,"Country of origin",null,"xxxxxxxxxx"]
[null,"1.1.4",null,"Trade name of fitting",null,"xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's Product Code",null,"xxxxxxxxxx"]
[null,"1.1.6",null,"Fitting suitable for main conductor (code names)",null,"xxxxxxxxxx","xxxxxxxxxx"]
[{"$nulls":3},"Main conductor (code names)","Up to Fox","YES"]
[null,"1.1.7",null,"Trade name of the fitting",null,"xxxxxxxxxx"]
[null,"1.1.8",null,"Manufacturer’s part number",null,"xxxxxxxxxx"]
[null,"1.1.9",null,"Catalogue reference number",null,"xxxxxxxxxx"]
[null,"1.1.10",null,"Drawing number & Revision number",null,"xxxxxxxxxx"]
[null,"1.1.11",null,"Physical identification mark on product",null,"specify "]
[null,"1.1.12",null,"Compliance to critical dimensions on Buyer's Guide","D-DT 3008","YES"]
[{"$nulls":3},"Body manufactured from galvanised steel , Millage cast iron or die cast aluminium","D-DT 3009","Specify"]
[null,1.2,null,"Colour coding",null,"Orange"]
[null,2,null,"Mechanical and electrical properties"]
[null,"2.1.",null,"Mechanical and electrical properties",null,null,"xxxxxxxxxx"]
[null,"2.1.3",null,"Minimum diameter","mm","8mm"]
[null,"2.1.4",null,"Maximum diameter","mm","18mm"]
[null,"2.1.5",null,"Minimum failing load","Kn",40]
[null,2.2,null,"Packaging"]
[null,2.2,null,"All fittings shall be clearly and permanently marked with the following:",null,null,"xxxxxxxxxx"]
[null,"2.2.1",null,"a) the manufacturer’s name or identification mark;"]
[null,"2.2.2",null,"b) the manufacturer’s item batch number;"]
[null,"2.2.3",null,"c) the joint reference number;"]
[null,"2.2.4",null,"d) the code name/s of the conductor for which they are intended;",null,"YES/NO"]
[null,3,null,"Test Authority"]
[null,3.1,null,"Approved person/organisation",null,"SABS/CSIR","xxxxxxxxxx"]
[null,4,null,"Documentation (to be submitted with tender)"]
[{"$nulls":3},"Note: All documentation to be provided in electronic format.",null,null,"xxxxxxxxxx"]
[null,4.1,null,"General",null,null,"xxxxxxxxxx"]
[null,"4.1.1",null,"Outline drawings of item","Sets",1]
[null,"4.1.2",null,"Are there detailed installation instructions of the fitting provided?",null,"YES/NO"]
[null,"4.1.3",null,"Material grade certification",null,"YES"]
[]
[null,"Deviations to any of the stated requirements are to be captured on the Deviation Schedule."]
[]
[null,"ESKOM TENDER E2719DXLIMOU"]
[]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":48,"n_cols":6,"rows_kept":48,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[2,7,2,13],[2,14,2,20],[2,21,2,27],[2,28,2,34],[2,35,2,41],[2,42,2,48],[2,49,2,55],[2,56,2,62],[2,63,2,69],[2,70,2,76],[2,77,2,83],[2,84,2,90],[2,91,2,97],[2,98,2,104],[2,105,2,111],[2,112,2,118],[2,119,2,125],[2,126,2,132],[2,133,2,139],[2,140,2,146],[2,147,2,153],[2,154,2,160],[2,161,2,167],[2,168,2,174],[2,175,2,181],[2,182,2,188],[2,189,2,195],[2,196,2,202],[2,203,2,209],[2,210,2,216],[2,217,2,223],[2,224,2,230],[2,231,2,237],[2,238,2,244],[2,245,2,251],[2,252,2,255],[4,0,4,6],[4,7,4,13],[4,14,4,20],[4,21,4,27],[4,28,4,34],[4,35,4,41],[4,42,4,48],[4,49,4,55],[4,56,4,62],[4,63,4,69],[4,70,4,76],[4,77,4,83],[4,84,4,90],[4,91,4,97],[4,98,4,104],[4,105,4,111],[4,112,4,118],[4,119,4,125],[4,126,4,132],[4,133,4,139],[4,140,4,146],[4,147,4,153],[4,154,4,160],[4,161,4,167],[4,168,4,174],[4,175,4,181],[4,182,4,188],[4,189,4,195],[4,196,4,202],[4,203,4,209],[4,210,4,216],[4,217,4,223],[4,224,4,230],[4,231,4,237],[4,238,4,244],[4,245,4,251],[4,252,4,255],[5,0,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[34,2,34,6],[35,2,35,6],[36,2,36,6],[38,0,38,6],[40,0,40,6],[42,0,42,1],[43,2,43,3],[47,2,47,3]],"flags":["formulas_cached_only"]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation schedule"]
[" CLAMP,SUSP CRADLE CON 8,0-18,0 D3008"]
[]
["SAP No: 0402501"]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":31}
["ESKOM TENDER E2719DXLIMOU"]
[]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[null,null,"Name (Print)",null,null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Test Schedule","index":2,"n_rows":29,"n_cols":6,"rows_kept":29,"merged":[[0,0,0,5],[1,0,1,6],[2,0,2,6],[3,1,3,5],[4,0,4,6],[19,1,19,2],[20,1,20,7],[21,1,21,7],[24,1,24,2],[28,1,28,2]],"flags":["formulas_cached_only"]}
["ESKOM TENDER E2719DXLIMOU"]
["Test Report Schedule"]
["CLAMP,SUSP CRADLE CON 8,0-18,0 D3008"]
[null,"The test reports are required for the selected SAP number listed on this sheet."]
["SAP No: 0402501"]
[]
[null,1,2,3,4,5]
[null,"Item ","Description","Standard","Clause No.","Report No."]
[null,1,"Verification of general dimensions","240-75883154",4.3]
[null,2,"Verification of material type","240-75883154",4.4]
[null,3,"Sample and visual test","240-75883154",4.5]
[null,4,"Damage and failure load test","240-75883154","4.5.1"]
[null,5,"Tensile test (SANS 61284)","240-75883154","4.5.2"]
[null,6,"Heat cycle test (SANS 61284)","240-75883154",4.6]
[null,7,"Short-circuit test","240-75883154",4.6]
[null,8,"Corrosion test (SANS 61284)","240-75883154",4.7]
[null,9,"Drift test (DSP 34-1659)","240-75883154",4.8]
[null,10,"Torque test (DSP 34-1659)","240-75883154",4.9]
[null,11,"Magnetic particle test (ASTM E709 )","240-75883154",4.1]
[]
[null,"ESKOM TENDER E2719DXLIMOU"]
[null,"SUPPLIER SIGNATURES"]
[]
[]
[null,"Name (Print)",{"$nulls":3},"Company name"]
[]
[]
[]
[null,"Sign",{"$nulls":3},"Date"]

{"sheet":"Eskom Drawing","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}