{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":[" Functional evaluation"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":" Functional evaluation","index":0,"n_rows":24,"n_cols":35,"rows_kept":24,"merged":[[6,2,6,24],[7,2,7,3],[8,2,10,3],[11,2,12,3],[13,19,13,20],[13,23,13,24],[14,2,14,6],[14,19,14,20],[14,23,14,24],[15,2,15,6],[15,11,15,12],[15,15,15,16],[15,19,15,20],[15,23,15,24],[16,2,16,6],[16,11,16,12],[16,15,16,16],[17,2,17,6],[17,11,17,12],[17,13,17,14],[17,15,17,16],[22,2,23,9],[22,11,22,12],[22,15,22,16],[23,11,23,12],[23,15,23,16]],"flags":["formulas_cached_only"]}
[{"$nulls":3},0,"Do Not Meet",{"$nulls":23},"MAX",null,"Not applicable",{"v":0,"d":"0%"},{"v":0.69,"d":"69%"},"NOT MEET","0-69"]
[{"$nulls":3},1,"Partial Meet (large gap) ",{"$nulls":23},{"v":0,"d":"0%"},0,"Do Not Meet",{"v":0.7,"d":"70%"},{"v":0.79,"d":"79%"},"PARTIAL MEET","70-79"]
[{"$nulls":3},2,"Partial Meet (small gap)",{"$nulls":23},{"v":0.75,"d":"75%"},1,"Partial Meet",{"v":0.8,"d":"80%"},{"v":1,"d":"100%"},"MEET","80-100"]
[{"$nulls":3},3,"Meet",{"$nulls":23},{"v":1,"d":"100%"},2,"Meet",{"v":1.01,"d":"101%"},110,"EXCEED","101-110"]
[{"$nulls":28},{"v":1.1,"d":"110%"},3,"Exceed"]
[{"$nulls":28},{"v":1,"d":"100%"},"X","Not applicable"]
[null,null,"Technical  Evaluation Criteria for Enquiry "]
[{"$nulls":4},"Requirements",null,null,"Criteria ","Deliverables","Weighting",null," Rating","% Rating","% Score",null,"[ Supplier Name ] Response","Eskom Comments"]
[null,null,"1. COMPANY PROFILE",null,"Company must be able to supply the correct or equivalent Pump, centrifugal D6D-4 1450rpm, 110Kw.","The structure needs to show the function areas from CEO/MD down to the site management and the roles each member plays in delivering the scope.","Provide organisational structure highlighting key positions and how they will interface with Employer","Company to provide detailed Quote referencing the correct reference of the item which we can purchase.","Detailed quote",{"v":0.5,"d":"50%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"},{"$nulls":3},{"v":0,"d":"0.0%"},{"$nulls":7},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"Quantitative & practical experience of Company.","The supplier needs to have more than 5 years experience in similar projects.","Quantitative & practical experience of Company","The supplier needs to have more than 5 years experience in supplying similar equipment.","Submit a portfolio of previous similar item supplied that demonstrates that the Tenderer has the appropriate abilities. Submit a list of contactable references that the Employer can contact during tender evaluations or any previous PO's indicating similar products supplied to Eskom",{"v":0.5,"d":"50%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"}]
[{"$nulls":4},"TOTAL WEIGHTING",{"$nulls":4},{"v":1,"d":"100%"},null,false,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":7},{"$error":"#REF!"}]
[null,null,"2. TECHNICAL REQUIREMENTS",null,"Company to have the capacity to supply the correct Pump, centrifugal, Manufacturer: Rateau, Part number D6D-4, Type: NPSS 4m, Capacity:200 m/hr, Total Head: 120m, Size: FM 39-1-04, Speed: 1450rpm, Stage: 4, Power: 110Kw. The Supplier shall demonstrate the ability supply and deliver the equipement to the requirements and specifications of KNPS and provide all the relevant documentation.","CV's including references of previous experience of personnel who shall execute the scope","Appropriately qualified and skilled personnel","Compilance to KNPS Technical Specification as outlined in Invitation.","Submit technical datasheet and delivery scheduled ",{"v":1,"d":"100%"},null,null,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":7},{"$error":"#REF!"}]
[{"$nulls":4},"TOTAL WEIGHTING",{"$nulls":4},{"v":1,"d":"100%"},null,false,{"v":0,"d":"0%"},{"v":0,"d":"0.0%"},{"$nulls":3},{"$error":"#REF!"},{"$nulls":7},{"$error":"#REF!"}]
[]
[null,null,"Final Analysis"]
[null,null,"1. COMPANY PROFILE",{"$nulls":6},{"v":0.35,"d":"35%"},null,{"v":0,"d":"0.0%"}]
[null,null,"2. TECHNICAL REQUIREMENTS",{"$nulls":6},{"v":0.35,"d":"35%"},null,{"v":0,"d":"0.0%"}]
[null,null,"TOTAL",{"$nulls":6},{"v":0.7,"d":"70%"},null,{"v":0,"d":"0.0%"}]
[{"$nulls":3},"RECOMMENDED"]
[{"$nulls":3},"NOT RECOMMENDED"]
[{"$nulls":3},"RE-EVALUATE",{"$nulls":7},{"$error":"#REF!"},{"$error":"#REF!"},null,null,{"$error":"#REF!"},{"$error":"#REF!"}]
[]
[null,null,"The scoring of the Functional Evaluation is conducted as follows:\nA supplier is given a score in each of the sub-categories. These sub-categories are requirements detailed in the specification or contract. Scores are allocated as follows:\n0 - 0% -    Does not meet \n1 - 75% -  Partial meet  \n2 -100% - Meet \n\nThe overall score for functionality criteria is  analysed as follows:\n0%     - 79%   - Does not meet\n80%   - 100% - Meet\n\n                                                                                   ",{"$nulls":8},"NOT MEET",{"$nulls":3},"CONCLUSION"]
[{"$nulls":15},"COMPILED BY:    T Nkopane                           REVIEWED BY:   H Ferreira                                                                                                                                                                                                                                                                                          "]