{"text_format":"3","workbook":"xls","n_sheets":11,"sheets":["P&G(1)","Distribution Boards(2)","Cables Building 9(3)","Sleeves (4)","Earthing (5)","Fire Alarm (11)","Auditorium Equipment(13)","Bulk Electrical (6)","Decommissioning (7)","Diesel Tank (8)","Summary"],"not_rendered":{"images":8,"external_links":1,"defined_names":9,"comments":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"P&G(1)","index":0,"n_rows":74,"n_cols":8,"rows_kept":74,"merged":[[2,5,2,7],[5,5,5,6],[30,5,30,6]],"flags":["formulas_cached_only"]}
[]
[null,"CSIR GENERATOR INSTALLATION"]
[null,"BILL OF QUANTITIES AND SUMMARY OF PRICES"]
[null,"PRELIMINARY AND GENERAL CHARGES"]
[null,"BILL NO. 1"]
[null,"ITEM","DESCRIPTION","UNIT","QTY","RATE",null,"   TOTAL"]
[{"$nulls":5},"MATERIAL","LABOUR"]
[null,null,"FIXED CHARGE ITEMS"]
[null,1.1,"GENERAL"]
[null,null,"Preliminaries and general required to comply with the conditions of contract and all regulations governing this contract","Sum",1,null,0,0]
[null,1.2,"Site establishment and de-establishment ","Sum",1,null,0,0]
[null,1.3,"OCCUPATIONAL HEALTH & SAFETY"]
[null,null,"Allowamce for Compliance with Construction Regulations, as detailed in Occupational Health & Safety Act (OHS), Act 85 of 1993, Submission of a (OHS) plan and all applicable documentation, to the client's satisfaction","Sum",1,null,0,0]
[]
[null,1.4,"PERMITS AND NOTICES"]
[null,null,"Allow for obtaining all necessary permits and giving of notices and co-operation with other Trades","Sum",1,null,0,0]
[null,1.5,"DEFECTS LIABILITY"]
[null,null,"Allow for a defects liability period of 12 months against defects in Equipment, Material and Workmanship as set out elsewhere, but excluding abuse, wear and tear and normal maintenance.","Sum",1,null,0,0]
[]
[]
[]
[]
[{"$nulls":7},{"v":0,"d":"R 0.00"}]
[]
[]
[]
[null,"CSIR GENERATOR INSTALLATION"]
[null,"BILL OF QUANTITIES AND SUMMARY OF PRICES"]
[null,"PRELIMINARY AND GENERAL CHARGES"]
[]
[null,"ITEM","DESCRIPTION","UNIT","QTY","RATE",null,"   TOTAL"]
[{"$nulls":5},"MATERIAL","LABOUR"]
[]
[null,null,"CARRIED OVER",{"$nulls":4},{"v":0,"d":"R 0.00"}]
[]
[null,null,"TIME RELATED ITEMS"]
[null,1.6,"STORAGE"]
[null,null,"Provide for storage of Plant, Equipment and Material on site including protection and insurance thereof","Mnth",3,null,{"v":0,"d":"R 0.00"},{"v":0,"d":"R 0.00"}]
[]
[null,1.7,"SUPERVISION"]
[null,null,"Allow for qualified site supervision during the construction period","Mnth",3,null,{"v":0,"d":"R 0.00"},{"v":0,"d":"R 0.00"}]
[]
[null,1.8,"TRANSPORT"]
[null,null,"Allow for Transportation of Generators","Sum",1,null,{"v":0,"d":"R 0.00"},{"v":0,"d":"R 0.00"}]
[null,null,"Allow for transport cost during the construction period ","Mnth",3,null,{"v":0,"d":"R 0.00"},{"v":0,"d":"R 0.00"}]
[null,1.9,"OTHER TIME RELATED ITEMS"]
[null,null,"Specify and cost all other time related items"]
[null,null,"not listed elsewhere as well as the period for"]
[null,null,"which these items will be applicable"]
[null,null,"Bond Costs","Sum",1,null,{"v":0,"d":"R 0.00"},{"v":0,"d":"R 0.00"}]
[]
[null,{"v":1.1,"d":"1.10"},"PROVISIONAL AMOUNTS"]
[null,null,"Allow for a Provisional Amount for the works"]
[null,null,"to be used as directed by the Engineer for"]
[null,null,"items not allowed for in the Bill of Quantities"]
[null,null,"Provisional Amount for Day works"]
[null,null,"Allow for Procurement, Transport to site and ","Sum",1,null,{"v":0,"d":"R 0.00"},{"v":0,"d":"R 0.00"}]
[null,null,"Profit:__12__%"]
[null,null,"(Tenderer to indicate profit margin and price"]
[null,null,"accordingly to day works amount)"]
[]
[]
[]
[null,1.2,"ADDITIONAL ITEMS"]
[null,null,"Any additional Items that the tenderer would wish to specify and not listed elsware"]
[]
[null,"1.2.1","Allowance for Factorty Acceptance Test (FAT) to include Client Representative and Engineer","ea",4,null,{"v":0,"d":"R 0.00"},{"v":0,"d":"R 0.00"}]
[null,"1.2.2",null,"Sum"]
[null,"1.2.3",null,"Sum"]
[null,"1.2.4",null,"Sum"]
[null,"1.2.5",null,"Sum"]
[]
[]
[null,null,"TOTAL OF SECTION  CARRIED TO SUMMARY",{"$nulls":4},{"v":0,"d":"R 0.00"}]

{"sheet":"Distribution Boards(2)","index":1,"n_rows":23,"n_cols":8,"rows_kept":23,"merged":[[2,5,2,7],[5,5,5,6]],"flags":["formulas_cached_only"]}
[]
[null,"CSIR GENERATOR INSTALLATION"]
[null,"BILL OF QUANTITIES AND SUMMARY OF PRICES"]
[null,"PRELIMINARY AND GENERAL CHARGES"]
[null,"BILL NO. 2"]
[null,"ITEM","DESCRIPTION","UNIT","QTY","RATE",null,"   TOTAL"]
[{"$nulls":5},"MATERIAL","LABOUR"]
[null,2,"DISTRIBUTION BOARDS"]
[null,null,"GENERAL"]
[null,null,"For the supply and installation of distribution boards, complete with sheet metal trays, frames, sub-frames, bus bars, lockable doors and provision for 30% future circuit breakers as per specification and drawings. Allow 30% spare space for future BMS Installation."]
[null,null,"Site establishment and de-establishment "]
[null,2.1,"Distribution Boards"]
[null,null,"For the supply and installation of the following distribution boards as per the specification and drawings. Similar or equal to ABB switch gear. "]
[]
[null,"2.1.1","Main LV Distribution Board Board (MDB 9) with Change over switch (ATS). The Board to have online thermal scanning functionality and some of the MCCB’s to have micro logics to enable Client to monitor power quality and consumption.","ea",1,0,0,0]
[null,"2.1.2","DATA Center Distribution Board. The Board to have online thermal scanning functionality and some of the MCCB’s to have micro logics to enable Client to monitor power quality and consumption.","ea",1,0,0,0]
[]
[null,2.2,"For the supply and installation of labels and a legend cards as per the standard and specification documents"]
[null,"2.2.1","Labelling of distribution boards - legend cards","sum",1,0,0,{"v":0,"d":"R 0.00"}]
[null,2.3,"Certificate of compliance (COC)"]
[null,null,"For the testing, commissioning and submission of a COC document for each Distribution Board. as per the  specification documents"]
[null,"2.3.1","COC Document","ea",4,null,{"v":0,"d":"R 0.00"},{"v":0,"d":"R 0.00"}]
[{"$nulls":7},{"v":0,"d":"R 0.00"}]

{"sheet":"Cables Building 9(3)","index":2,"n_rows":71,"n_cols":11,"rows_kept":71,"merged":[[2,5,2,7],[5,5,5,6],[36,5,36,6]],"flags":["formulas_cached_only"]}
[]
[null,"CSIR GENERATOR INSTALLATIONS"]
[null,"BILL OF QUANTITIES AND SUMMARY OF PRICES"]
[null,"CABLES AND CONDUCTORS"]
[null,"BILL NO. 3"]
[null,"ITEM","DESCRIPTION","UNIT","QTY","RATE",null,"   TOTAL"]
[{"$nulls":5},"MATERIAL","LABOUR"]
[]
[null,3.1,"LOW VOLTAGE CABLES (MV) TERMINATIONS - Building 9"]
[null,null,"For the delivery to site, supply and installation of 0.4kV Four Core Cables, Terminations and Joints for PILC Cable, as per specification."]
[null,"3.1.1","Contractor to allow for Tracing  of existing 0.4kV XLPE Cable  and other services in the area and provide layout drawing of services","Sum",1,null,0,0,null,null,594.91]
[null,"3.1.2","Disconnect existing 6 x 150mm² XLPE 0.4kV, 4 core Cable from the existing MDB 9 and connect to new LV Board","Sum",1,null,0,0,null,null,594.91]
[null,"3.1.3","Supply and installations of 4 x 120mm², XLPE, 4-Core CU, insulated PVC embeded, steel wire armoured Cable from new Generator 1 & 2 to each ground mounted change over panels ","m",80,0,0,0]
[null,"3.1.4","Supply and installations of 4 x 120mm², XLPE, 4-Core CU, insulated PVC embeded, steel wire armoured Cable from the Transformer to Generator 1 ground mounted change over panel (ATS)","m",60,0,0,0]
[null,"3.1.5","Supply and installations of 4 x 120mm², XLPE, 4-Core CU, insulated PVC embeded, steel wire armoured Cable from the new Generator 1 ground mounted  change over panel to Generator 2 ground mounted change over panel","m",40,0,0,0]
[null,"3.1.6","Supply and installations of 4 x 120mm², XLPE, 4-Core CU, insulated PVC embeded, steel wire armoured Cable from the new Generator 2 ground mounted  change over panel to Data centre Main distribution board","m",110,0,0,0]
[null,"3.1.7","Terminations for 120mm² x 4 Core, XLPE cables  and Preparation kits for  terminations, complete with screened connectors.","ea",32,0,0,0]
[null,"3.1.8","Re-routing of the existing 2 x 185mm² XLPE Cables from the existing MDB 9 DB to Data Center Main distribution Board","m",15,0,0,0]
[null,"3.1.9","Terminations for 185mm² x 4 Core, XLPE cables  and Preparation kits for  terminations, complete with screened connectors.","ea",4,0,0,0]
[]
[null,3.2,"Bare Copper Earth Wire installed with cable."]
[null,null,"For the supply and instalation of the following BCEW  with the 4 Core PVC insulated PVC Bedded SWA PVC sheathed 600/1000V copper cables as specified."]
[null,"3.2.1","95mm² CU bare earth wire, complete with joints.","m",360,0,0,0,null,null,39.78]
[null,"3.2.2","Terminations for the 95mm² CU bare earth wire","Ea",10,0,0,0]
[]
[null,3.3,"LV Cable Terminations and Connection"]
[]
[null,"3.3.1","Contractor to allow for Tracing and re-termination of existing LV Cables from the existing MDB 9 to the newly installed Distribution Board   circuit","sum",1,null,0,0]
[null,"3.3.2","Contractor to allow for labelling of all circuits on new Board","sum",1,0,0,0]
[{"$nulls":7},0]
[]
[]
[null,"CSIR GENERATOR INSTALLATIONS"]
[null,"BILL OF QUANTITIES AND SUMMARY OF PRICES"]
[null,"CABLES AND CONDUCTORS"]
[null,"BILL NO. 3"]
[null,"ITEM","DESCRIPTION","UNIT","QTY","RATE",null,"   TOTAL"]
[{"$nulls":5},"MATERIAL","LABOUR"]
[null,null,"Carried Over",{"$nulls":4},0]
[]
[]
[null,"3.3.3","Supply and installations of 2 x 95mm², XLPE, 4-Core CU, insulated PVC embeded, steel wire armoured Cable ","m",85,0,0,0]
[null,"3.3.4","Supply off Termination kits for 95mm², XLPE, 4-Core CU, cables","Ea",116,0,0,0]
[null,"3.3.5","Supply and installations of 4 x 70mm², XLPE, 4-Core CU, insulated PVC embeded, steel wire armoured Cable ","m",35,0,0,0]
[null,"3.3.6","Supply 4 off Termination kits for 70mm², XLPE, 4-Core CU, cables","Ea",8,0,0,0]
[null,"3.3.7","Supply and installations of 3 x 50mm², XLPE, 4-Core CU, insulated PVC embeded, steel wire armoured Cable ","m",15,0,0,0]
[null,"3.3.8","Supply 3 off Termination kits for 50mm², XLPE, 4-Core CU, cables","Ea",24,0,0,0]
[null,"3.3.9","Supply and installations of 4 x 50mm²,  4-Core CU, PVC insulated PVC embeded, Cable ","m",50,0,0,0]
[null,"3.3.10","Supply 4 off Termination for 50mm², PVC, 4-Core CU, cables","Ea",4,0,0,0]
[null,"3.3.11","Supply and installations of 4 x 35mm²,  4-Core CU, PVC insulated PVC embeded, Cable ","m",30,0,0,0]
[null,"3.3.12","Supply 4 off Termination kits for 35mm², PVC, 4-Core CU, cables","Ea",4,0,0,0]
[null,"3.3.13","Supply and installations of 4 x 25mm²,  4-Core CU, PVC insulated PVC embeded, Cable ","m",35,0,0,0]
[null,"3.3.14","Supply 4 off Termination kits for 25mm², PVC, 4-Core CU, cables","Ea",4,0,0,0]
[null,"3.3.15","Supply and installations of 4 x 16mm²,  4-Core CU, PVC insulated PVC embeded, Cable ","m",20,0,0,0]
[null,"3.3.16","Supply 4 off Termination kits for 16mm², PVC, 4-Core CU, cables","Ea",4,0,0,0]
[null,"3.3.17","Supply and installations of 4 x 10mm²,  4-Core CU, PVC insulated PVC embeded, Cable ","m",50,0,0,0]
[null,"3.3.18","Supply and installations of 6 x 6mm²,  4-Core CU, PVC insulated PVC embeded, Cable ","m",60,0,0,0]
[null,3.4,"GROUND WORKS FOR BUILDING 9"]
[null,null,"The Contractor shall do the setting out, excavation, removal of excavated material and backfilling of the following trenches:"]
[null,"3.4.1","GROUND WORKS FOR LV CABLES"]
[null,"3.4.2","Excavate 1m deep x 450mm wide x 20m length in trenches","/m³",9,null,0,0]
[null,"3.4.3","Bedding as per specification","m³",9,null,0,0]
[null,"3.4.4","Backfilling and compaction of excavated trenches","/m",20,null,0,0]
[null,"3.4.5","Lay 120mm², 0.4kV, XLPE, CU, SWA, Cable","m",250,null,0,0]
[null,"3.4.6","Cable pressure Testing","Ea",8,null,0,0]
[]
[]
[null,3.5,"Rehabilitation of groundworks"]
[null,null,"For the rehabilitation of groundworks where the contractor excavated through existing paved areas, gardens, road crossings etc.","sum",1,null,{"v":0,"d":"0.00"},0]
[]
[{"$nulls":7},0]

{"sheet":"Sleeves (4)","index":3,"n_rows":26,"n_cols":11,"rows_kept":26,"merged":[[2,5,2,7],[5,5,5,6]],"flags":["formulas_cached_only"]}
[]
[null,"CSIR GENERATOR INSTALLATIONS"]
[null,"BILL OF QUANTITIES AND SUMMARY OF PRICES"]
[null,"SLEEVES"]
[null,"BILL NO. 4"]
[null,"ITEM","DESCRIPTION","UNIT","QTY","RATE",null,"   TOTAL"]
[{"$nulls":5},"MATERIAL","LABOUR"]
[]
[null,4.1,"SLEEVING"]
[null,null,"For the supply and installation of the following sleeves"]
[null,"4.1.1","110mm dia sleeves in trench","m",120,0,0,0,null,null,42.63]
[null,"4.1.2","50mm dia sleeves in trench","m",0,{"$nulls":5},56.88]
{"$rows_empty":12}
[{"$nulls":7},0]
[null,null,"(Unit prize required for each item)"]

{"sheet":"Earthing (5)","index":4,"n_rows":31,"n_cols":8,"rows_kept":31,"merged":[[2,5,2,7],[3,1,3,6],[5,5,5,6]],"flags":["formulas_cached_only"]}
[]
[null,"CSIR GENERATOR INSTALLATIONS"]
[null,"BILL OF QUANTITIES AND SUMMARY OF PRICES"]
[null,"EARTHING , BONDING AND LIGHTNING PROTECTION"]
[null,"BILL NO. 5"]
[null,"ITEM","DESCRIPTION","UNIT","QTY","RATE",null,"   TOTAL"]
[{"$nulls":5},"MATERIAL","LABOUR"]
[]
[null,5.1,"Earthing and lightning protection:"]
[null,null,"Measuring of earth resistance by an earthing specialist and issuing of a report"]
[null,"5.1.1","Measuring of earth resistivity over the site","Sum",1,null,0,0]
[null,"5.1.2","Issuing of a report","Sum",1,null,0,0]
[]
[null,5.2,"Earthing and lightning protection:"]
[null,null,"Design, supply and install lightning protection and earthing system as per general and detail specifications document."]
[null,"5.2.1","Design supply and installation of the full earthing system for the site","Sum",1,null,0,0]
[null,"5.2.2","Installation of complete earthing and lightning protection system for the site based on SANS 10199/ 10313/ 62305 and IEC 62305 and as per drawings issued","Sum",1,0,0,0]
[null,"5.2.3","Issuing of earthing Certificates","Sum",1,null,0,0]
{"$rows_empty":12}
[{"$nulls":7},0]

{"sheet":"Fire Alarm (11)","index":5,"n_rows":43,"n_cols":11,"rows_kept":43,"hidden":true,"merged":[[1,0,1,7],[1,8,1,10]],"flags":["formulas_cached_only"]}
["BILL NO. 11:"]
["FIRE ALARM INSTALLATION"]
[]
["Item","Description","Unit","Qty","Genl","Basement ","Ground Floor","First Floor","Material Rate","Labour Rate","Total"]
[11,"Supply, Install and commision fire alarm/protection system , simmular to Fire Class 500 System or approved."]
[]
["11.1.1","Fire Control Panel (2 loop panel (Slave))","Ea",2,0,1,0,1,{"v":23106,"d":"23106.00"},{"v":120,"d":"120.00"},{"v":46452,"d":"46452.00"}]
["11.1.2","Fire Control Panel (1 loop panel (Master))","Ea",1,0,0,1,0,{"v":18060,"d":"18060.00"},{"v":120,"d":"120.00"},{"v":18180,"d":"18180.00"}]
["11.1.3","Indoor Call Point / Class break unit","Ea",20,0,4,11,5,{"v":1292,"d":"1292.00"},{"v":120,"d":"120.00"},{"v":28240,"d":"28240.00"}]
["11.1.4","Call point surface mount back box","Ea",20,0,4,11,5,{"v":81.6,"d":"81.60"},{"v":120,"d":"120.00"},{"v":4032,"d":"4032.00"}]
["11.1.5","FC loop -service tool- program detectors","Ea",1,1,0,0,0,{"v":5326,"d":"5326.00"},{"v":87,"d":"87.00"},{"v":5413,"d":"5413.00"}]
["11.1.6","Universal Mounting Base for detectors","Ea",111,0,34,34,43,{"v":56,"d":"56.00"},{"v":87,"d":"87.00"},{"v":15873,"d":"15873.00"}]
["11.1.7","Heat detector - 25ºC to 70ºC","Ea",30,0,27,3,0,{"v":652,"d":"652.00"},{"v":120,"d":"120.00"},{"v":23160,"d":"23160.00"}]
["11.1.8","Photo Electric smoke detector","Ea",79,0,5,31,43,{"v":788,"d":"788.00"},{"v":87,"d":"87.00"},{"v":69125,"d":"69125.00"}]
["11.1.9","Sounder Base","Ea",14,0,2,5,7,{"v":799,"d":"799.00"},{"v":120,"d":"120.00"},{"v":12866,"d":"12866.00"}]
["11.1.10","Loop Power Beacon","Ea",13,0,1,5,7,{"v":850,"d":"850.00"},{"v":210,"d":"210.00"},{"v":13780,"d":"13780.00"}]
["11.1.11","Loop Isolator ","Ea",5,0,1,2,2,{"v":680,"d":"680.00"},{"v":120,"d":"120.00"},{"v":4000,"d":"4000.00"}]
["11.1.12","2 core fire cable","m",1075,300,250,260,265,{"v":8,"d":"8.00"},7.75,16931.25]
["11.1.13","3 Pair Twisted mylar screened cable","Ea",3,3,0,0,0,{"v":970,"d":"970.00"},{"v":8,"d":"8.00"},{"v":2934,"d":"2934.00"}]
["11.1.14","Fireclass software 2.0 ","Ea",3,3,0,0,0,{"v":970,"d":"970.00"},{"v":8,"d":"8.00"},{"v":2934,"d":"2934.00"}]
[]
[11.2,"Supply, Install and commision fire protection system for the kitchen canopy, simmular to the Piranha R-102","Ea",1,0,1,0,0,{"v":25000,"d":"25000.00"},{"v":5000,"d":"5000.00"},{"v":30000,"d":"30000.00"}]
[]
[11.3,"PVC Conduit, Boxes and acccessories"]
["11.3.1","50 mm² Round PVC conduit box with cover","Ea",111,0,34,34,43,3.33,{"v":25,"d":"25.00"},{"v":3144.6299999999997,"d":"3,144.63"}]
["11.3.2","100 x 50 x 50 mm² Deep galvanized box","Ea",15,0,5,5,5,3.71,{"v":25,"d":"25.00"},{"v":430.65000000000003,"d":"430.65"}]
["11.3.3","50 x 50 x 50 mm² Deep galvanized box","Ea",20,0,4,11,5,3.71,{"v":25,"d":"25.00"},{"v":574.2,"d":"574.20"}]
["11.3.4","50 x 50 x 50 mm² Deep galvanized box","Ea",20,0,4,11,5,3.71,{"v":25,"d":"25.00"},{"v":574.2,"d":"574.20"}]
["11.3.5","300 x 300 x 100 mm² Deep galvanized box","m",1,0,0,1,0,{"v":4.5,"d":"4.50"},{"v":25,"d":"25.00"},{"v":29.5,"d":"29.50"}]
["11.3.6","20 mm² PVC Conduit in concrete or fixed in ceilings","m",775,0,250,260,265,2.38,{"v":12.5,"d":"12.50"},{"v":11532,"d":"11,532.00"}]
{"$rows_empty":11}
[null,"(Unit prize required for each item)"]
[null,"Total Bill No. 11 carried forward to Summary",{"$nulls":8},{"v":310205.43000000005,"d":"R 310,205.43"}]

{"sheet":"Auditorium Equipment(13)","index":6,"n_rows":48,"n_cols":6,"rows_kept":48,"hidden":true,"merged":[[1,0,1,5]],"flags":["formulas_cached_only"]}
["BILL NO. 13:"]
["SUPPLY, INSTALLATION AND COMMISIONING OF SOUND AND VIDEO EQUIPMENT FOR THE AUDITORIUM"]
[]
["Item","Description","Unit","Qty","Material Rate","Total"]
[13,"For the supply, installation and commissioning of Audio, Control and Video equipment:"]
[13.1,"Video Equipment"]
["13.1.1","6000 Lumen, XGA Data Projector",null,1]
["13.1.2","Standard Lens Option",null,1]
["13.1.3","Custom Made Presentation Points",null,2]
["13.1.4","Professional DVD Player",null,1]
["13.1.5","Professional Rack Mount CD Player",null,1]
[]
[13.2,"Audio Equipment"]
["13.2.1","12In 8Out Digital Sound Processor",null,1]
["13.2.2","8In Echo Cancellation with Hybrid",null,1]
["13.2.3","500W Continuous line Array Element",null,2]
["13.2.4","Extension Subwoofer Module for 70J",null,2]
["13.2.5","50 cm Straight Line Array Module(Side Fill)",null,2]
["13.2.6","Sound Delay Speakers",null,2]
["13.2.7","Professional Power Amplifier",null,1]
["13.2.8","Professional Power Amplifier (Control29AV)",null,1]
["13.2.9","Professional Power Amplifier (CBT-50LA)",null,1]
["13.2.10","Wireless UHF Radio Microphones",null,2]
["13.2.11","Professional Lapel Microphone System",null,1]
["13.2.12","Headworm Radio Microphone System",null,2]
["13.2.13","4Channel Active Antennae Combiner/Splitter",null,2]
["13.2.14","Professional Gooseneck Microphone",null,1]
["13.2.15","Feedback Suppression Devices",null,2]
["13.2.16","Custom Panels for 3 Point Access",null,3]
[]
[13.3,"Control System"]
["13.3.1","Central Control System",null,1]
["13.3.2","Wireless Touch Panel",null,1]
["13.3.3","Docking Station for Touch Panel",null,1]
["13.3.4","Automatic VGA Switcher",null,1]
["13.3.5","Audio Distribution Amplifier",null,1]
[]
[13.4,"Installation and Cabling","Sum",1]
[13.5,"Programming, Commisioning and Testing","Sum",1]
[13.6,"Training and Handover.","Sum",1]
[13.7,"6 months Support and maintanance contract","Sum",1]
[]
[]
[]
[]
[]
[null,"(Unit prize required for each item)"]
[null,"Total Bill No. 12 carried forward to Summary",{"$nulls":3},{"v":414000,"d":"R 414,000.00"}]

{"sheet":"Bulk Electrical (6)","index":7,"n_rows":29,"n_cols":8,"rows_kept":29,"merged":[[2,5,2,7],[3,1,3,6],[5,5,5,6]],"flags":["formulas_cached_only"]}
[]
[null,"CSIR GENERATOR INSTALLATIONS"]
[null,"BILL OF QUANTITIES AND SUMMARY OF PRICES"]
[null,"BULK ELECTRICAL EQUIPMENT"]
[null,"BILL NO. 6"]
[null,"ITEM","DESCRIPTION","UNIT","QTY","RATE",null,"   TOTAL"]
[{"$nulls":5},"MATERIAL","LABOUR"]
[]
[null,6.1,"ELECTRICAL EQUIPMENT"]
[null,null,"This is the bill to cover the supply, delivery installation, testing, cable termination and commissioning of all electrical equipment required for the Main Electrical supply as per Design Specification supplied. Detailed specification to be supplied for all equipment offered.  Contractor to indicate period for Warranty and Gaurantee as per supplied Techical Schedules A and B"]
[null,"6.1.1","650kVA 415/380V, @50Hz 1500rpm 3 phase  DIESEL GENERATOR  SILENT WAETHER PROOF, SOUND ATTENUATED CANOPY . With Onboard Deep sea - DSE 7320 controller and Gateway 890, Automatic changeover (ATS), maintenance free batteries and trickle charger included,  Mild Steel Powder Coated Base Integrated Fuel Tank with Sender Unit. High Residential Mild Steel Silencer                               (Section 4 - Schedule of Technical Information to be completed and submitted with Tender)","ea",2,0,0,0]
[]
[null,"6.1.2","Upgrade of the existing generator Off board Deep sea - with DSE 7320 controller and Gateway 890,  and production of new drawings","Sum",1,0,0,0]
[]
[null,"6.1.3","All notices and signs as per the OHAS act","Sum",1,0,0,0]
{"$rows_empty":13}
[{"$nulls":7},0]

{"sheet":"Decommissioning (7)","index":8,"n_rows":26,"n_cols":8,"rows_kept":26,"merged":[[2,5,2,7],[3,1,3,6],[5,5,5,6]],"flags":["formulas_cached_only"]}
[]
[null,"CSIR TRANSFORMER REPLACEMENTS"]
[null,"BILL OF QUANTITIES AND SUMMARY OF PRICES"]
[null,"DECOMMISSIONING OF ELECTRICAL EQUIPMENT"]
[null,"BILL NO. 7"]
[null,"ITEM","DESCRIPTION","UNIT","QTY","RATE",null,"   TOTAL"]
[{"$nulls":5},"MATERIAL","LABOUR"]
[]
[null,7.1,"DECOMMISSIONING OF ELECTRICAL EQUIPMENT"]
[null,null,"The Contractor to Decommision the following"]
[null,"7.1.1","The existing MDB 9 Distribution Board and associated equipment and Buy as Scrap material","each",1,null,0,0]
[null,"7.1.2",null,"each"]
[null,"7.1.3",null,"each"]
[null,"7.1.4",null,"Sum"]
[]
[null,7.2,"REDUNDANT EQUIPMENT"]
{"$rows_empty":9}
[{"$nulls":7},0]

{"sheet":"Diesel Tank (8)","index":9,"n_rows":25,"n_cols":8,"rows_kept":25,"merged":[[2,5,2,7],[3,1,3,6],[5,5,5,6]],"flags":["formulas_cached_only"]}
[]
[null,"CSIR TRANSFORMER REPLACEMENTS"]
[null,"BILL OF QUANTITIES AND SUMMARY OF PRICES"]
[null,"DECOMMISSIONING OF ELECTRICAL EQUIPMENT"]
[null,"BILL NO. 8"]
[null,"ITEM","DESCRIPTION","UNIT","QTY","RATE",null,"   TOTAL"]
[{"$nulls":5},"MATERIAL","LABOUR"]
[]
[null,8.1,"Diesel Tank"]
[null,null,"Supply, Installation, testing of Aboveground Storage Tanks -SANS10131"]
[null,"8.1.1","Supply, Delivery,  Installation, pressure testing of 9000L Diesel Tank","each",1,0,0,0]
[null,"8.1.2","Supply of Diesel","L",100]
[null,"8.1.3",null,"each"]
[null,null,"Supply of "]
[null,8.2,"REDUNDANT EQUIPMENT"]
{"$rows_empty":9}
[{"$nulls":7},0]

{"sheet":"Summary","index":10,"n_rows":17,"n_cols":3,"rows_kept":17,"merged":[[0,0,0,2],[1,0,1,1],[12,0,12,1],[13,0,13,1],[14,0,14,1],[15,0,15,1],[16,0,16,1]],"flags":["formulas_cached_only"]}
[]
["CSIR GENERATOR INSTALLATION",null,"Sub Total"]
[]
["BILL 01","P&G",{"v":0,"d":"R 0.00"}]
["BILL 02","Distribution Boards",{"v":0,"d":"R 0.00"}]
["BILL 03","LV Cables",{"v":0,"d":"R 0.00"}]
["BILL 04","Sleeves",{"v":0,"d":"R 0.00"}]
["BILL 05","Earthing",{"v":0,"d":"R 0.00"}]
["BILL 06","Bulk Electrical Equipment",{"v":0,"d":"R 0.00"}]
["BILL 07","Decommissioning",{"v":0,"d":"R 0.00"}]
["Bill 08","Diesel Tank",{"v":0,"d":"R 0.00"}]
["Bill 09","Civil Works",{"v":0,"d":"R 0.00"}]
["SUB TOTAL",null,{"v":0,"d":"R 0.00"}]
["10% Contingency",null,{"v":0,"d":"R 0.00"}]
["SUB TOTAL",null,{"v":0,"d":"R 0.00"}]
["15% Vat",null,{"v":0,"d":"R 0.00"}]
["TOTAL",null,{"v":0,"d":"R 0.00"}]