{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Supply of FAS Equipment BOQ "],"not_rendered":{"external_links":25,"defined_names":778},"read":"whole","date_system":"1900"}

{"sheet":"Supply of FAS Equipment BOQ ","index":0,"n_rows":11,"n_cols":7,"rows_kept":11,"merged":[[0,0,0,6]]}
["SUPPLY, SERVICING AND CERTIFICATION OF FAS EQUIPMENT IN THE ERI CONSTRUCTION SERVICES BUSINESS UNIT, AT VARIOUS POWER STATIONS FOR A PERIOD OF 3 YEARS"]
[]
["Item No","Bill Description","SAP Description","Unit of measurements","Total Qty","Rate","Total"]
[]
["0001","Supply or replace Safety Harnesses as per PERSONAL PROTECTIVE EQUIPMENT FOR WORK AT HEIGHTS SPECIFICATION 240-100979499","HARNESS, SAFETY INDUSTRIAL: TYPE: FALL ARREST, FULL BODY; PPE","ea",1000,null,{"$f":"E5*F5","v":{"v":0,"d":"R0.00"}}]
["0002","Recertification of Safety Harnesses","CERTIFICATE: TYPE: CALIBRATION/TEST REPORT; DIMENSIONS: A4; MATERIAL: PAPER; VENDOR TO SUPPLY INSTRUMENT CALIBRATION CERTIFICATE OR TEST REPORT; TO HAVE LOGO OF ACCREDITATION (SANAS) OR OEM","ea",2500,null,{"$f":"E6*F6","v":{"v":0,"d":"R0.00"}}]
["0003","Replacement of Safety Harness Lanyards","LANYARD:TOOL,Tool Lanyards for Working at Heights, LANYARD: TYPE: TOOL; SUPPL P/N: MISC/004; (C.O.C; Q4:NSF:NC:NEV); HEAVY DUTY; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE).","ea",5000,null,{"v":0,"d":"R0.00"}]
["0004","Supply Tool Lanyards for Working at Heights","LANYARD:SHOCK ABSORBING LANSAE;LG 2 M;2,  LANYARD: TYPE: SHOCK ABSORBING LANSAE; LENGTH: 2 M; ENDS: 2; LANYARD DOUBLE LEG WEBBING, 2 METER TOTAL LENGHT, SHOCK ABSORBING WITH TERMINATING PYLAN HOOKS; VENDORS ARE RESPONSIBLE FOR ENSURING THAT THEY ARE PERFORMING AGAINST THE CORRECT DRAWING REVISION NUMBER (IF APPLICABLE). LOAD RATING: 250KG, DIMENSIONS: 58MM X 3700MM,  SCAFFOLD HOOK, NYLON","ea",2500,null,{"v":0,"d":"R0.00"}]
["0005","Transportation ",null,"sum",1,null,{"v":0,"d":"R0.00"}]
[]
[{"$nulls":5},"Total of Prices:",{"$f":"SUM(G5:G10)","v":{"v":0,"d":"R0.00"}}]