{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Fire"],"not_rendered":{"defined_names":41},"read":"whole","date_system":"1900"}

{"sheet":"Fire","index":0,"n_rows":155,"n_cols":7,"rows_kept":155,"merged":[[1,1,1,4]]}
[]
[null,"Rosherville Oil Depot Refurbishment  "]
[null,"Item No.","Description","Unit","Quantity"," Rate","Amount "]
[null,null,"FIRE WORKS "]
[]
[null,null,"PREAMBLES"]
[]
[null,null,"General Preamble For Trades – 2017 as published by The Association of South African Quantity Surveyors as well as the Supplementary preambles under the section “Works Information-Specifications, standards & workmanship” "]
[]
[null,null,"ALL MATERIALS, EQUIPMENT AND INSTALLATION METHODS TO BE IN STRICT COMPLIANCE WITH AUTOMATIC SPRINKLER INSTALLATION FOR FIRE FIGHTING PURPOSES (SANS 10287) AND HYDRANTS (SANS 1128)"]
[]
[null,null,"PRELIMINARY AND GENERAL"]
[]
[null,null,"CONTRACTOR'S ESTABLISHMENT ON SITE AND GENERAL OBLIGATIONS"]
[]
[null,null,"FIXED CHARGES ITEMS"]
[]
[null,null,"Contractual Requirements","Sum",1]
[]
[null,null,"Site Establishment : Site Offices and Storage Sheds including temporary fencing.","Sum",1]
[]
[null,null,"Ablution and latrine facilities","Sum",1]
[]
[null,null,"Tools and Equipment","Sum",1]
[]
[null,null,"Remove contractor's site establishment","Sum",1]
[]
[null,null,"TIME RELATED ITEMS"]
[]
[null,null,"Site Offices and Storage Sheds","Month",5]
[]
[null,null,"Ablution and latrine facilities","Month",5]
[]
[null,null,"Tools and Equipment","Month",5]
[]
[null,null,"Company/head office overhead cost.","Month",5]
[]
[null,null,"Supervision","Month",5]
[]
[null,null,"Quality management","Month",5]
[]
[null,null,"HEALTH AND SAFETY"]
[]
[null,null,"Prepare, submit and obtain approval of safety plan/file and lodge same on site.","Sum",1]
[]
[null,null,"Personal Protective Equipment","Sum",1]
[]
[null,null,"Transportation of Employees","Month",5]
[]
[]
[null,null,"Environmental management","Month ",5]
[]
[]
[null,null,"Preliminary and General "]
[]
[]
[null,null,"Upgrade of a Foam Protection System "]
[]
[null,null,"Foam System"]
[null,1,"4000L Foam tank - 11 bar, internally coated 4 times M3 Scotch ","Item",1]
[]
[null,2,"GB6  150mm Foam Dosing Unit - 3%","No ",1]
[]
[]
[null,null,"Detection and Control "]
[null,3,"Extinguishing Panel ","No",3]
[]
[null,4,"LHGC Controllers ","No ",8]
[]
[null,5,"24V Power supply 5amp - including batteries ","No ",2]
[]
[null,6,"Sirens ","No ",2]
[]
[null,7,"Bells ","No ",2]
[]
[]
[null,null,"Cabling "]
[null,8,"LHGC stainless steel braided detection cable 90 degrees.","m",1960]
[]
[null,9,"PH 30 Fire Cable ","m",1200]
[]
[]
[null,null,"Accessories"]
[null,10,"Waterproof enclosures ","No ",2]
[]
[]
[null,null,"Piping "]
[]
[null,11,"3' Galvanized pipe ","m",64]
[]
[null,12,"2' Galvanized pipe ","m",252]
[]
[null,13,"1½' Galvanized pipe ","m",132]
[]
[null,14,"1¼' Galvanized pipe ","m",132]
[]
[]
[null,null,"Pipe Fittings "]
[null,15,"2''Monitors ","No",4]
[]
[null,16,"High pressure 300 Bar 2 Port Manifold - ¾","No ",2]
[]
[null,17,"High flow regulator - 300 Bar","No",2]
[]
[null,18,"High capacity 150mm strainer ","No ",1]
[]
[null,19,"5 way stainless steel Nozzles ","No ",204]
[]
[null,20,"Bosal Conduit ","No ",160]
[]
[]
[null,null,"Valves "]
[]
[null,21,"80I 300 Bar culindres C/W Meuler Valve ","No ",4]
[]
[null,22,"Electric Valve C/W SS Ball Valves ","No ",2]
[]
[null,23,"Pnumatic Actuator C/W SS Ball Valves ","No ",2]
[]
[null,24,"Pilot Cylinder for Deluge Valve ","No ",2]
[]
[null,25,"Ugrade of a Foam Protection System - Installation and commission ","No ",30]
[]
[]
[null,null,"UPGRADING "]
[]
[null,null,"Drizit Oil Separator "]
[]
[null,25,"Upgrading drizit oil separator ","Item ",1]
[]
[]
[null,null,"FIRE HOSE REELS "]
[]
[null,26,"Supply of hose reels ","No ",5]
[]
[null,27,"Instal and Move Fire Equipment ","Item ",1]
[]
[]
[null,null,"FOAM "]
[]
[null,28,"Spare foam","L",500]
[]
[null,29,"250L Foam Trolleys","No ",2]
[]
[null,null,"Provisional sum for Firedos foam proportioning system (One Million Two hundred Thousand.)","sum",1,null,{"$f":"E145*F145","v":0}]
[]
[null,null,"Profisional Sum for water tank Storage (Two hundred thousand)","sum",1,null,{"$f":"E147*F147","v":0}]
[]
[]
[null,null,"SUB-TOTAL carried forward to Bill Summary Page"]
[]
[{"$nulls":3},{"v":0.05,"d":"5%"},"Contigency Allowance"]
[{"$nulls":4},"Sub-Total 1"]
[{"$nulls":3},{"v":0.15,"d":"15%"},"VAT "]
[{"$nulls":4},"TOTAL INCL. VAT"]