{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["MECHANICAL","ELECTRICAL"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"MECHANICAL","index":0,"n_rows":20,"n_cols":7,"rows_kept":20,"merged":[[0,0,0,6],[2,0,2,6],[30,0,30,6]]}
["BURGERSFORT MATERIALS LIST "]
["ITEM","DISCRIPTION  Techncial Data Specification","BRAND ","QUANTITY","SERIAL NUMBER","Installed","Not installed"]
[]
[1,"Visolid 700IQ sn2211037-sn22110378: TSS meter for Reactor","Water Skills",2,"22110378; 2211037",null,"✔                 d"]
[2,"TSS Meters connecting cables in box sn22110614-sn22130924","Water Skills",2,"22110614; 22130924",null,"✔                 d"]
[3,"Single electrode holder and cable for probes, incl 50m cable connection to TSS meters","Water Skills",2,"N/A",null,"✔                 d"]
[4,"E&H DO meters, cables and probes, incl controller for above","Water Skills",2,"N/A",null,"✔                 d"]
[5,"Residual chlorine analyzer (0-5ppm) incl flow probe, flow cell and cable complete",null,6,null,null,"✔                 d"]
[6,"Chlorine pigtails 1.5m for 70 kg Cylinders",null,1,"11G70 04-0039","✔                 "]
[7,"Chlorine cyclinder scale ",null,1,"C15/00296/4/2","✔                 "]
[8,"Chlorine Vacuum Regulators 0-5 kg/h",null,1,"220232; 220231","✔                 "]
[9,"Chlorine manifold",null,null,76011411503,"✔                "]
[10,"Chlorine Emergency kit A ",null,1,16011911502,null,"✔                "]
[11,"Full face gas mask ",null,6,10031285,null,"✔                "]
[12,"Chlorine Safety kit",null,1,"FMX24866 06/2016","✔                "]
[13,"Chlorine booster pumps 5m3/h at 5Bar",null,2]
[null,"Ultrasonic flow meter and brackets PTU51 for final outlet at chlorine contact channels",null,1,"mu0122105171"]
[14,"0-100 kPA Pressure transmitter",null,4,null,null,"✔                "]
[15,"Axial flow pump impellers, draft tubes, drive frames, weir boxes. Excluding structural steel and platform for mounting above the TWL of the Reactor. Motors excluded. ",null,4,null,null,"✔                "]
[16,"Tertiary Drum filters with 20micron filtration (3300 m3/d capacity). No wash water systems included, no pipe connections included",null,2,null,null,"✔                "]

{"sheet":"ELECTRICAL","index":1,"n_rows":28,"n_cols":7,"rows_kept":28,"merged":[[0,0,0,6],[2,0,2,6],[19,0,19,6],[33,0,33,6],[38,0,38,6],[42,0,42,6]]}
["BURGERSFORT MATERIALS LIST "]
["ITEM","DISCRIPTION  Techncial Data Specification","BRAND","QUANTITY","SERIAL NUMBER","Installed","Not installed"]
["instruments and switches"]
[1,"Motor control centre complete including all switchgear, pump starters, metering: MCC 4 Chlorination","Water Skills",1,"N/A",null,"✔                 d"]
[2,"Distribution boards complete including all switchgear, metering: Dosing System MCC, complete","Water Skills",1,"N/A",null,"✔                 d"]
[3,"600/1000V PVC PVC SWA PVC cable installed in cable sleeves, trenches or on cable support:",{"$nulls":4},"✔                 d"]
[4,"50mm² 4 core","N/A","80m","N/A",null,"✔                 d"]
[5,"10mm² 3 core","N/A","75m","N/A",null,"✔                 d"]
[6,"6mm2 3-core","N/A","45m","N/A",null,"✔                 d"]
[7,"Instrumentation cable:"]
[8,"1mm 2 Pair APL","N/A","40m","N/A",null,"✔                 d"]
[9,"1mm 4 Pair APL","N/A","30m","N/A",null,"✔                 d"]
[null,"Automation:"]
[11,"MCC1: Inlet Works: LAN Switch complete with fibre convertors","Water Skills",1,"N/A",null,"✔                 d"]
[12,"MCC2: BNR 1: LAN Switch complete with fibre convertors","Water Skills",1,"N/A",null,"✔                 d"]
[13,"MCC3: BNR2: LAN Switch complete with fibre convertors","Water Skills",1,"N/A",null,"✔                 d"]
[null,"Complete SCADA IT Rack with Server & Client PC, licensing to be renewed, Approx R 220 000","Water Skills",1,"N/A",null,"✔                 d"]
[14,"PC Worx ","Endress + Houser",1,"N/A",null,"✔"]
[]
["BURGERSFORT MATERIALS LIST "]
["ITEM","DISCRIBTION","BRAND","QUANTITY","SERIAL NUMBER","Installed","Not installed"]
[15,"10kVA UPS for control & instrumentation","Rhomberg ",1,"N/A",null,"✔                 d"]
[16,"Lightning and Surge protection on Analog inputs","Rhomberg ",1,"N/A",null,"✔                 d"]
[17,"LAN Switch complete with fibre convertors","Water Skills",1,"N/A",null,"✔                 d"]
[]
[18,"Combined old and new plant Power Factor Correction complete installation incl cables and terminations (Quote B103190122). NOTE: No Cables have been procured for the PFC unit","Water Skills",1,"N/A",null,"✔                 d"]
[]
[19,"6x 2.2kW VSD Drievs to be built into MCC5 - Dewatering MCC which is not built yet","Water Skills",6,"N/A",null,"✔"]