{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["5 Year Fire Detection Contract","Year Fire Detection Contr Rates"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"5 Year Fire Detection Contract","index":0,"n_rows":100,"n_cols":20,"rows_kept":100,"merged":[[1,0,1,19],[95,0,95,1],[97,0,97,1],[99,0,99,1],[101,0,101,1],[103,0,103,1],[105,0,105,1]]}
[]
["CSIR RFQ No: 3733/31/07/2026 For the Provision of  Fire Detection, Gas Fire Suppression Systems and Sprinkler Systems, for a period of five (5) years at the CSIR Gauteng & KwaZulu Natal Sites."]
["ITEM NO","DESCRIPTION","TYPES OF FIRE CONTROL PANELS/SYSTEMS","UNIT","NUMBER OF PANELS","NUMBER OF DETECTORS","NUMBER OF BEAM DETECTORS","NUMBER OF SOUNDERS","NUMBER OF MANUAL CALL POINTS","QUATERLY SCHEDULE MAINTENANCE","RATE","TOTAL YEAR 1","RATE","TOTAL YEAR 2","RATE","TOTAL YEAR 3","RATE","TOTAL YEAR 4","RATE","TOTAL YEAR 5"]
[]
[null,"PRETORIA"]
[]
[1,"Building 1","Ziton 2-loop addressable fire alarm panel","No",1,3,0,2,2,4,0,{"$f":"(F7+G7+I7)*J7*K7","v":0},0,{"$f":"(F7+G7+I7)*J7*M7","v":0},0,{"$f":"(F7+G7+I7)*J7*O7","v":0},0,{"$f":"(F7+G7+I7)*J7*Q7","v":0},0,{"$f":"(F7+G7+I7)*J7*S7","v":0}]
[{"$f":"A7+1","v":2},"Building 2","Ziton 2-loop addressable fire alarm panel","No",1,119,1,38,40,4,0,0,0,0,0,0,0,0,0,0]
[{"$f":"A8+1","v":3},"Building 3 ","Ziton 2-loop addressable fire alarm panel","No",1,110,0,30,25,4,0,0,0,0,0,0,0,0,0,0]
[4,"Building 3 Archives","C-Tec Panel - gas suppresssion system","No",2,16,0,4,4,4,0,0,0,0,0,0,0,0,0,0]
[5,"Building 4","Aritech FP2000 2 Loop adressable panel,expandable to 4 Loops","No",1,96,0,34,37,4,0,0,0,0,0,0,0,0,0,0]
[6,"Building 5","Aritech , Conventional","No",1,140,0,15,12,4,0,0,0,0,0,0,0,0,0,0]
[7,"Building 6","Ziton, Conventional","No",1,82,0,7,6,4,0,0,0,0,0,0,0,0,0,0]
[8,"Building 7","Aritech, Conventional","No",1,31,0,8,5,4,0,0,0,0,0,0,0,0,0,0]
[9,"Building 8","Ziton 2-loop addressable fire alarm panel","No",1,30,0,10,11,4,0,0,0,0,0,0,0,0,0,0]
[10,"Building 9","Aritech FP2000 2 Loop adressable panel,expandable to 4 Loops","No",1,70,0,8,8,4,0,0,0,0,0,0,0,0,0,0]
[11,"Building 9 Data Centre","Pyroshield gas suppression","No",3,42,0,6,4,4,0,0,0,0,0,0,0,0,0,0]
[12,"Building 9 SANREN Server room","C-Tec Panel - gas suppresssion system","No",1,8,0,1,1,4,0,{"$f":"(F18+G18+I18)*J18*K18","v":0},0,{"$f":"(F18+G18+I18)*J18*M18","v":0},0,{"$f":"(F18+G18+I18)*J18*O18","v":0},0,{"$f":"(F18+G18+I18)*J18*Q18","v":0},0,{"$f":"(F18+G18+I18)*J18*S18","v":0}]
[{"$f":"A18+1","v":13},"Building 10","Ziton/Aritech 2-loop addressable fire alarm panel","No",2,146,0,34,43,4,0,0,0,0,0,0,0,0,0,0]
[14,"Building 11","Ziton 4-loop addressable fire alarm panel","No",1,123,0,18,18,4,0,0,0,0,0,0,0,0,0,0]
[15,"Building 11","Thefirebeam","No",1,0,2,7,2,4,0,0,0,0,0,0,0,0,0,0]
[16,"Building 12","Ziton 4-loop addressable fire alarm panel","No",1,135,0,20,12,4,0,0,0,0,0,0,0,0,0,0]
[17,"Building 13","Aritech, Conventional","No",1,25,0,3,4,4,0,0,0,0,0,0,0,0,0,0]
[18,"Building 14","Aritech, Conventional","No",2,380,0,30,20,4,0,0,0,0,0,0,0,0,0,0]
[19,"Building 15","Aritech, Addressable","No",1,58,0,12,14,4,0,0,0,0,0,0,0,0,0,0]
[20,"Building 16","Ziton 2-loop addressable fire alarm panel","No",1,21,0,15,8,4,0,0,0,0,0,0,0,0,0,0]
[21,"Building 17A","Aritech, Addressable","No",1,69,0,7,7,4,0,0,0,0,0,0,0,0,0,0]
[22,"Building 17A","Thefirebeam","No",1,0,2,2,0,4,0,0,0,0,0,0,0,0,0,0]
[23,"Building 17 B","Aritech, Addressable","No",1,53,0,7,8,4,0,0,0,0,0,0,0,0,0,0]
[24,"Building 18","Aritech, Technoswitch Addressable & Ziton","No",3,125,0,15,15,4,0,0,0,0,0,0,0,0,0,0]
[25,"Building 19","Aritech, Addressable/Ziton addressable ","No",2,161,0,15,15,4,0,0,0,0,0,0,0,0,0,0]
[26,"Building 19C","Fire beams","No",1,0,2,4,0,4,0,0,0,0,0,0,0,0,0,0]
[27,"Building 20","Aritech addressable /2 x Ziton Conventional","No",1,105,0,22,20,4,0,0,0,0,0,0,0,0,0,0]
[28,"Building 21","Ziton 2-loop addressable fire alarm panel","No",1,70,0,14,13,4,0,0,0,0,0,0,0,0,0,0]
[{"$f":"A34+1","v":29},"Building 22","Ziton 2-loop addressable fire alarm panel","No",1,165,0,20,23,4,0,0,0,0,0,0,0,0,0,0]
[30,"Building 22 Archives North","HFC 227 gas suppression system","No",2,24,0,6,4,4,0,0,0,0,0,0,0,0,0,0]
[]
[]
[{"$f":"A36+1","v":31},"Building 23","Ziton 2-loop addressable fire alarm panel","No",1,85,0,30,30,4,0,0,0,0,0,0,0,0,0,0]
[32,"Building 23","Fire beams","No",0,0,2,2,0,4,0,0,0,0,0,0,0,0,0,0]
[33,"Building 26","Technoswitch Conventional","No",1,5,0,1,1,4,0,0,0,0,0,0,0,0,0,0]
[34,"Building 33","Ziton 2-loop addressable fire alarm panel","No",1,67,0,30,30,4,0,{"$f":"(F42+G42+I42)*J42*K42","v":0},0,{"$f":"(F42+G42+I42)*J42*M42","v":0},0,{"$f":"(F42+G42+I42)*J42*O42","v":0},0,{"$f":"(F42+G42+I42)*J42*Q42","v":0},0,{"$f":"(F42+G42+I42)*J42*S42","v":0}]
[35,"Building 34","Ziton 2-loop addressable fire alarm panel","No",1,18,0,5,8,4,0,0,0,0,0,0,0,0,0,0]
[36,"Building 35","Ziton 2-loop addressable fire alarm panel","No",1,16,0,6,6,4,0,0,0,0,0,0,0,0,0,0]
[37,"Building 36","Ziton 2-loop addressable fire alarm panel","No",1,12,0,5,7,4,0,0,0,0,0,0,0,0,0,0]
[38,"Building 36 Data Centre","Pyroshield gas suppression","No",1,4,0,2,2,4,0,0,0,0,0,0,0,0,0,0]
[39,"Building 37","Aritech Addressable","No",1,27,0,4,6,4,0,0,0,0,0,0,0,0,0,0]
[40,"Building 38","Ziton 2-loop addressable fire alarm panel","No",1,13,0,7,7,4,0,0,0,0,0,0,0,0,0,0]
[41,"Building 38","Fire beams","No",1,0,1,1,1,4,0,0,0,0,0,0,0,0,0,0]
[42,"Building 39","Aritech Addressable","No",1,142,5,18,12,4,0,0,0,0,0,0,0,0,0,0]
[43,"Building 39","Vesda system X 4 VENUES","Sum",1,1,1,1,1,4,0,0,0,0,0,0,0,0,0,0]
[44,"Building 40","Ziton 2-loop addressable fire alarm panel","No",1,8,0,2,2,4,0,0,0,0,0,0,0,0,0,0]
[45,"Building 41","Ziton 2-loop addressable fire alarm panel","No",1,29,0,10,8,4,0,0,0,0,0,0,0,0,0,0]
[46,"Building 42 North/South","Ziton 2-loop addressable fire alarm panel","No",1,49,0,12,14,4,0,0,0,0,0,0,0,0,0,0]
[{"$f":"A54+1","v":47},"Building 43","Aritech addressable & TC804 Conventional","No",2,310,0,40,25,4,0,0,0,0,0,0,0,0,0,0]
[48,"Building 43","Gas suppression system","No",3,16,0,3,3,4,0,0,0,0,0,0,0,0,0,0]
[49,"Building 44","Kiddy x 1 & Ziton ZP2 x 3 & 1 x conventional Technoswitch","No",4,1150,0,68,30,4,0,0,0,0,0,0,0,0,0,0]
[50,"Building 44","Basement archive room gas suppression system","No",4,22,0,3,6,4,0,0,0,0,0,0,0,0,0,0]
[51,"Building 44","Block D server room gas suppression system","No",1,6,0,2,2,4,0,{"$f":"(F59+G59+I59)*J59*K59","v":0},0,{"$f":"(F59+G59+I59)*J59*M59","v":0},0,{"$f":"(F59+G59+I59)*J59*O59","v":0},0,{"$f":"(F59+G59+I59)*J59*Q59","v":0},0,{"$f":"(F59+G59+I59)*J59*S59","v":0}]
[{"$f":"A57+1","v":50},"Building 45","Aritech FP2000 2 Loop adressable panel,expandable to 4 Loops","No",1,86,2,12,9,4,0,0,0,0,0,0,0,0,0,0]
[51,"Building 46 A/B/C/D","Ziton 2-loop addressable fire alarm panel","No",1,125,0,30,32,4,0,0,0,0,0,0,0,0,0,0]
[52,"Building 46 E","Ziton 2-loop addressable fire alarm panel","No",1,18,0,3,6,4,0,0,0,0,0,0,0,0,0,0]
[53,"Building 46 F","Aritech Addressable","No",1,111,0,28,18,4,0,0,0,0,0,0,0,0,0,0]
[54,"Building 46 F","Fire beams","No",2,0,4,3,4,4,0,0,0,0,0,0,0,0,0,0]
[55,"Building 50","Aritech Addressable","No",1,20,1,8,6,4,0,0,0,0,0,0,0,0,0,0]
[56,"Safety File",null,"Item",{"$nulls":6},0,0,0,0,0,0,0,0,0,0]
[57,"Conduct inspections and maintenance of sprinkler system at building 9 (Data Centre) as per SANS10287 requirements",null,"Sum",{"$nulls":6},0,0,0,0,0,0,0,0,0,0]
[]
[]
[null,"PAARDENFONTEIN"]
[]
[{"$f":"A67+1","v":58},"Building 2","Technoswicth conventional","No",1,12,0,4,3,4,0,{"$f":"(F72+G72+I72)*J72*K72","v":0},0,{"$f":"(F72+G72+I72)*J72*M72","v":0},0,{"$f":"(F72+G72+I72)*J72*O72","v":0},0,{"$f":"(F72+G72+I72)*J72*Q72","v":0},0,{"$f":"(F72+G72+I72)*J72*S72","v":0}]
[]
[null,"JOHANNESBURG"]
[]
[{"$f":"A72+1","v":59},"Cottesloe admin building","Ziton addressable panel","No",1,3,0,6,2,4,0,{"$f":"(F76+G76+I76)*J76*K76","v":0},0,{"$f":"(F76+G76+I76)*J76*M76","v":0},0,{"$f":"(F76+G76+I76)*J76*O76","v":0},0,{"$f":"(F76+G76+I76)*J76*Q76","v":0},0,{"$f":"(F76+G76+I76)*J76*S76","v":0}]
[{"$f":"A76+1","v":60},"Cottesloe mechanical workshop","Ziton addressable panel","No",1,8,0,4,2,4,0,{"$f":"(F77+G77+I77)*J77*K77","v":0},0,{"$f":"(F77+G77+I77)*J77*M77","v":0},0,{"$f":"(F77+G77+I77)*J77*O77","v":0},0,{"$f":"(F77+G77+I77)*J77*Q77","v":0},0,{"$f":"(F77+G77+I77)*J77*S77","v":0}]
[{"$f":"A77+1","v":61},"Cottesloe corrosion test lab","Ziton addressable panel","No",1,8,0,2,2,4,0,0,0,0,0,0,0,0,0,0]
[62,"Cottesloe rope test lab","Ziton addressable panel","No",1,15,0,6,3,4,0,0,0,0,0,0,0,0,0,0]
[63]
[64,"Carlow Road building 1","Ziton addressable panel","No",1,21,0,6,7,4,0,{"$f":"(F81+G81+I81)*J81*K81","v":0},0,{"$f":"(F81+G81+I81)*J81*M81","v":0},0,{"$f":"(F81+G81+I81)*J81*O81","v":0},0,{"$f":"(F81+G81+I81)*J81*Q81","v":0},0,{"$f":"(F81+G81+I81)*J81*S81","v":0}]
[65,"Carlow Road building 2","Ziton addressable panel","No",1,18,0,6,7,4,0,0,0,0,0,0,0,0,0,0]
[66,"Carlow Road building 3","Ziton addressable panel","No",1,7,0,4,2,4,0,0,0,0,0,0,0,0,0,0]
[67,"Carlow Road building 4","Ziton addressable panel","No",1,7,0,2,3,4,0,0,0,0,0,0,0,0,0,0]
[]
[null,"KWAZULU NATAL"]
[]
[{"$f":"A84+1","v":68},"Building 1","Aritec/Kidde ZP2 2-4-loop addressable fire alarm panel","No",2,260,0,38,32,4,0,{"$f":"(F88+G88+I88)*J88*K88","v":0},0,{"$f":"(F88+G88+I88)*J88*M88","v":0},0,{"$f":"(F88+G88+I88)*J88*O88","v":0},0,{"$f":"(F88+G88+I88)*J88*Q88","v":0},0,{"$f":"(F88+G88+I88)*J88*S88","v":0}]
[{"$f":"A88+1","v":69},"BIDF","Ziton ZP3 2-4-loop addressable fire alarm panel","No",1,38,2,12,14,4,0,0,0,0,0,0,0,0,0,0]
[]
[]
[]
[null," SUB-TOTAL 1 (Excl. VAT)",{"$nulls":9},{"$f":"SUM(L6:L91)","v":0},null,{"$f":"SUM(N6:N91)","v":0},null,{"$f":"SUM(P6:P91)","v":0},null,{"$f":"SUM(R6:R91)","v":0},null,{"$f":"SUM(T6:T91)","v":0}]
[]
[]
["ADD 15% VAT",{"$nulls":10},{"$f":"L93*15%","v":0},null,{"$f":"N93*15%","v":0},null,{"$f":"P93*15%","v":0},null,{"$f":"R93*15%","v":0},null,{"$f":"T93*15%","v":0}]
[]
["SUB-TOTAL 2 (INCL VAT)",{"$nulls":10},{"$f":"SUM(L93,L96)","v":0},null,{"$f":"SUM(N93,N96)","v":0},null,{"$f":"SUM(P93,P96)","v":0},null,{"$f":"SUM(R93,R96)","v":0},null,{"$f":"SUM(T93,T96)","v":0}]
[]
["GRAND TOTAL",{"$nulls":18},{"$f":"SUM(L98,N98,P98,R98,T98)","v":0}]

{"sheet":"Year Fire Detection Contr Rates","index":1,"n_rows":21,"n_cols":8,"rows_kept":21,"merged":[[1,0,1,7]]}
[]
["CSIR RFQ No: 3733/31/07/2026 For the Provision of  Fire Detection, Gas Fire Suppression Systems and Sprinkler Systems, for a period of five (5) years at the CSIR Gauteng & KwaZulu Natal Sites."]
[]
[null,"AD-HOC SERVICES","UNIT","YEAR 1","YEAR 2","YEAR 3","YEAR 4","YEAR 5"]
[]
[1,"Call out fee during normal hour working hours (Monday to Friday, 08:00 to 16:30)","Rate per hour",0,0,0,0,0]
[{"$f":"A6+1","v":2},"Call out fee during weekends and public holidays","Rate per hour",0,0,0,0,0]
[{"$f":"A7+1","v":3},"Supervisor\nTotal cost per hour to supervise and manage crafts perform fire systems repairs during normal working hours","Rate per hour",0,0,0,0,0]
[{"$f":"A8+1","v":4},"Supervisor\nTotal cost per hour to supervise and manage crafts perform fire systems repairs during weekends and public holidays","Rate per hour",0,0,0,0,0]
[5,"Artisan\nTotal cost per hour per artisan to perform fire systems repairs during normal working hours","Rate per hour",0,0,0,0,0]
[6,"Artisan\nTotal cost per hour per artisan to perform fire systems repairs during weekends and public holidays","Rate per hour",0,0,0,0,0]
[7,"Assistant Artisan\nTotal cost per hour per artisan to perform fire systems repairs during normal working hours","Rate per hour",0,0,0,0,0]
[]
[]
[{"$f":"A12+1","v":8},"Assistant Artisan\nTotal cost per hour per artisan to perform fire systems repairs during weekends and public holidays","Rate per hour",0,0,0,0,0]
[{"$f":"A15+1","v":9},"Laborer\nTotal cost per hour per artisan to perform fire systems repairs during normal working hours","Rate per hour",0,0,0,0,0]
[10,"Laborer\nTotal cost per hour per artisan to perform fire systems repairs during weekends and public holidays","Rate per hour",0,0,0,0,0]
[11,"Transport costs light vehicle","Rate per kilometer",0,0,0,0,0]
[12,"Transport costs heavy vehicle","Rate per kilometer",0,0,0,0,0]
[13,"Spare parts, materials, goods, services, large equipment hire and other general costs not made up by the contract","Mark up (percentage)","%","%","%","%","%"]
[14,"Rigging equiment (Crane, Scaffolding, Cherry Picker)","Rate per hour",0,0,0,0,0]