{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Technical Schedule XLPE Cable","Deviation Schedule","Drwg & Type Tests"],"not_rendered":{"external_links":1,"defined_names":19},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Technical Schedule XLPE Cable","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"merged":[[0,1,0,7],[1,1,1,7],[2,1,2,7],[3,6,3,7],[4,1,4,7],[5,1,5,7],[8,3,8,4],[9,3,9,4],[18,3,18,4],[32,1,32,4],[35,1,35,2],[38,1,38,2],[41,1,41,2]],"flags":["formulas_cached_only"]}
[null,"TECHNICAL SCHEDULES A & B FOR CRIMP FERRULES"]
[]
[null,"Ferrule, Crimp CU "]
[]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B: Guarantees and technical particulars of equipment offered"]
[]
[null,1,2,null,3,null,4,5]
[null,"Item ","NRS 074-2\nSANS 1803-1\nSANS 61238-1","Description",null,null,"Schedule A","Schedule B"]
[null,1,null,"Item and system description"]
[{"$nulls":4},"LUG, CRIMPING CU"]
[null,1.1,null,"·","SAP No",null,"Item specific","____________"]
[null,1.2,null,"·","Buyers Guide Drawing",null,"D-DT-8020","xxxxxxxxxx"]
[null,"1.3",null,"·","Symmetrical fault level rating","kA","Item specific","xxxxxxxxxx"]
[null,"1.4",null,"·","Nominal system voltage","kV","11, 22, 33kV","xxxxxxxxxx"]
[null,"1.5","NRS 074-2 4.6","·","Earth fault level rating","kA",10,"xxxxxxxxxx"]
[]
[]
[null,2,null,"Ratings"]
[null,2.1,null,"·","Rated voltage (Ur)","kV","0-36 kV","____________"]
[null,"2.2","D-DT-8020","·","Conductor Size","mmsq","Item specific","____________"]
[null,"2.4","NRS 074-2 \n","·","Are the ferrule sizing marked in square millimetres to indicate the conductor size?",null,"Yes","____________"]
[null,"2.5","D-DT-8020","·","Are the lugs and ferrules made in an electrolytic grade copper material",null,"Yes","____________"]
[null,2.6,"NRS 074-2 \n","·","Is the surface cleaned, free of defects and polished to a mirror finish?",null,"Yes","____________"]
[null,2.7,"NRS 074-2 \n","·","Does marking comply with NRS 074-2?",null,"Yes","____________"]
[null,2.8,"NRS 074-2 \nD-DT-8020","·","Do the dimensions of the ferrule comply with D-DT-8020 and SANS 1803-1? ",null,"Yes","____________"]
[null,2.9,"NRS 074-2 ","·","Are the crimping die requirements as per NRS 074-2?",null,"Yes","____________"]
[null,2.1,null,"·","Rated frequency (fr)","Hz",50,"____________"]
[null,2.11,"NRS 074-2 \n5.1 a)","·","Availability of catalogue with required information?",null,"Yes","____________"]
[null,2.12,"NRS 074-2 \n","·","Catalogue to be provided with tender documentation\ndocumentation?",null,"Yes","____________"]
[null,2.13,"NRS 074-2 \n","·","Copy of type tests report and where applicable certificates to be provided with tender documentation.",null,"Yes","____________"]
[]
[null,"SIGNATURES"]
[]
[{"$nulls":4},"         "]
[null,"Supplier",null,null,"Name (Print)",null,"Sign","Date"]
[]
[{"$nulls":4},"         "]
[null,"Factory",null,null,"Name (Print)",null,"Sign","Date"]
[]
[{"$nulls":4},"         "]
[null,"Eskom",null,null,"Name (Print)",null,"Sign","Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":6,"n_cols":3,"rows_kept":6,"merged":[[0,0,0,2],[2,0,2,2]],"flags":["formulas_cached_only"]}
["Deviation schedule"]
[null,null,"Ferrule, Crimp Cu"]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Proposed deviation"]
[]
[null,null,"NO DEVIATIONS TO SPECIFICATION"]

{"sheet":"Drwg & Type Tests","index":2,"n_rows":13,"n_cols":10,"rows_kept":13,"merged":[[0,1,0,9],[1,1,1,9],[2,1,2,9],[5,1,5,4],[6,2,6,4],[7,1,7,4],[11,1,11,4]],"flags":["formulas_cached_only"]}
[null,"Drawing and Type Test Report Schedule for lugs and ferrules"]
[]
[null,"Ferrule, Crimp CU "]
[]
[null,1,2,3,4,5,6,7,8,9]
[null,"Drawings",{"$nulls":3},"Drawing/ Instruction number ","Revision number","Unique product model/ type/ code offered","Product rating / size offered ","Manufacturing location (Name, Address and Country)"]
[null,"1","Cable joint kit manufacturer drawing"]
[null,"Type Test Reports and certificates as required in SANS 1803-1",{"$nulls":3},"Report Number","Test facility and date tested","Unique product model/type type tested","Product rating offered ","Manufacturing location of type tested unit (Name, Address and Country)"]
[null,"Component","Test property","Test method","Requirement"]
[null,"Crimping ferrule","Electrical tests","SANS 61238-1",6]
[null,null,"Mechanical tests","SANS 61238-1",7]
[null,"Routine Test reports and certificates generic copies as required in SANS 61238-1",{"$nulls":3},"Report Number","Test facility and date tested","Unique product model/type type tested","Product rating offered ","Manufacturing location of type tested unit (Name, Address and Country)"]
[null,"Component","Test property","Test method","Requirement"]