{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Summary","Electrified Fences"],"not_rendered":{"external_links":3,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Summary","index":0,"n_rows":35,"n_cols":2,"rows_kept":35,"merged":[[0,0,2,1],[3,0,3,1]],"flags":["formulas_cached_only"]}
["Sentech STP"]
[]
[]
["RFQ SUMMARY"]
["Description","TOTAL"]
[]
["ELECTRIFIED FENCE  1400m -3M Electrified fixed to ClearVu fence.. RE-MEASURABLE",0]
[]
["CONTINGENCY ","R"]
[]
["PROJECT MANAGEMENT ","R"]
[]
["PRELIMINARIES AND GENERAL (P & G)","R"]
[]
["TOTAL FOR ELECTRONIC SERVICES"]
["NOTE !"]
[]
[]
[]
[]
[]
["SERVICE LEVEL AGREEMENT (SLA) 3 YEARS"]
["YEAR 1 (WARRANTEE PERIOD) FULLY COMPREHENSIVE",0]
[]
["YEAR 2 FULLY COMPREHENSIVE",0]
[]
["YEAR 3 FULLY COMPREHENSIVE",0]
[]
["YEAR 4 FULLY COMPREHENSIVE",0]
[]
[]
[]
["TOTAL COST OF SERVICE OVER A 3 YEAR PERIOD",0]
[]
["Tenderer to supply service contract with the RFQ document"]

{"sheet":"Electrified Fences","index":1,"n_rows":103,"n_cols":5,"rows_kept":103,"merged":[[0,1,2,4]],"flags":["formulas_cached_only"]}
[null,"SENTECH STP"]
[]
[]
[null,"Electrified Fence Equipment"]
[null,"Licences"]
[null,"Command Centre"]
[null,"Supply",1,null,0]
[null,"Install",1,null,0]
[]
[null,"Fence Zone License"]
[null,"Supply",13,null,0]
[null,"Install",13,null,0]
[]
[null,"Workstation License (per Workstation)"]
[null,"Supply",1,null,0]
[null,"Install",1,null,0]
[]
[null,"Equipment"]
[null,"T20 Alarms Terminal, Black"]
[null,"Supply",9,null,0]
[null,"Install",9,null,0]
[]
[null,"F32 Fence Controller"]
[null,"Supply",9,null,0]
[null,"Install",9,null,0]
[]
[null,"Sign Warning Security PK 10"]
[null,"Supply",330,null,0]
[null,"Install",330,null,0]
[]
[null,"Lightning Diverter"]
[null,"Supply",36,null,0]
[null,"Install",36,null,0]
[]
[null,"Cable U/Gate 1.6Mmx50M Soft"]
[null,"Supply",9,null,0]
[null,"Install",9,null,0]
[]
[null,"Earth Clamp Galv PK 3"]
[null,"Supply",137,null,0]
[null,"Install",137,null,0]
[]
[null,"Wire HI Conductive M.T 2X1609M"]
[null,"Supply",70,null,0]
[null,"Install",70,null,0]
[]
[null,"Bracket Offset Block Blk PK 50"]
[null,"Supply",3300,null,0]
[null,"Install",3300,null,0]
[]
[null,"Switch Gate High Voltage"]
[null,"Supply",4,null,0]
[null,"Install",4,null,0]
[]
[null,"F3 Cable Manager"]
[null,"Supply",9,null,0]
[null,"Install",9,null,0]
[]
[null,"Power Supply - 3.5A"]
[null,"Supply",9,null,0]
[null,"Install",9,null,0]
[]
[null,"Controller 6000, 2 Door Variant"]
[null,"Supply",9,null,0]
[null,"Install",9,null,0]
[]
[null,"K20 Pivot Mount Bracket ( PK 25)"]
[null,"Supply",2500,null,0]
[null,"Install",2500,null,0]
[]
[null,"K20 Mount Screw Anti-Tamper  ( PK 25)"]
[null,"Supply",2500,null,0]
[null,"Install",2500,null,0]
[]
[null,"K20 Spring Indicator - 15Kg ( PK 25)"]
[null,"Supply",1250,null,0]
[null,"Install",1250,null,0]
[]
[null,"K20 Pivot Mount Tensioner ( PK 25)"]
[null,"Supply",2500,null,0]
[null,"Install",2500,null,0]
[]
[null,"K20 Wire Link 91P 182 MM- 60H ( PK 25)"]
[null,"Supply",2500,null,0]
[null,"Install",2500,null,0]
[]
[null,"Hardware"]
[null,"POST 3.0M STRAIGHT 33 WIRE - 2MM  Steel"]
[null,"Supply",null,null,0]
[null,"Install",null,null,0]
[]
[null,"INSULATOR : IN-LINE BLACK HARD CLAW (PK 100)"]
[null,"Supply",39000,null,0]
[null,"Install",39000,null,0]
[]
[null,"EARTH ROD 1.5M COMPLETE INCL LINE CLAMP"]
[null,"Supply",137,null,0]
[null,"Install",137,null,0]
[]
[null,"Other"]
[null,"Supply",null,null,0]
[null,"Install",null,null,0]
[null,"Total Cost Carried to summary sheet",null,null,0]