{"text_format":"3","workbook":"xlsx","n_sheets":14,"sheets":["Notes","Summary","SECTION A P&G's"," Section B Civil","Section C Earth Grid","Section D Foundations","Section E Steel Work","Section F Equipment & Lighting","Section G Miscellanous & Clamps","Section H Cable & Stringing","Section I Labelling","Section J Dismantling","SECTION K Control Plant","SECTION L OTHER "],"not_rendered":{"images":1,"external_links":2,"defined_names":14,"comments":2},"read":"whole","date_system":"1900"}

{"sheet":"Notes","index":0,"n_rows":67,"n_cols":2,"rows_kept":67,"merged":[[1,0,1,1],[6,0,6,1],[36,0,36,1],[37,0,37,1],[38,0,38,1],[39,0,39,1],[40,0,40,1],[41,0,41,1],[42,0,42,1],[43,0,43,1],[44,0,44,1],[62,0,62,1],[63,0,63,1],[64,0,64,1],[65,0,65,1],[66,0,66,1]]}
[]
["NOTES"]
[]
["1.           Measurement and payment"]
["1.1.        Symbols"]
[]
["The units of measurement described in the Bill of Quantities are metric units abbreviated as follows:"]
[]
["Abbreviation","Unit"]
["%","percent"]
["h","hour"]
["ha","hectare"]
["kg","kilogram"]
["kl","kilolitre"]
["km","kilometre"]
["km-pass","kilometre-pass"]
["kPa","kilopascal"]
["kW","kilowatt"]
["l","litre"]
["m","metre"]
["mm","millimetre"]
["m2","square metre"]
["m2-pass","square metre pass"]
["m3","cubic metre"]
["m3-km","cubic metre-kilometre"]
["MN","meganewton"]
["MN.m","meganewton-metre"]
["MPa","megapascal"]
["No.","number"]
["Prov sum[1]","provisional sum"]
["PC-sum","prime cost sum"]
["R/only","Rate only"]
["sum","Lump sum"]
["t","ton (1000kg)"]
["W/day","Work day"]
[]
["1.2.        General assumptions"]
["1.2.1.               Unless otherwise stated, items are measured net in accordance with the drawings, and no allowance has been made in the quantities for waste."]
["1.2.2.               The Prices and rates stated for each item in the Bill of Quantities shall be treated as being fully inclusive of all work, risks, liabilities, obligations, overheads, profit and everything necessary as incurred or required by the Contractor in carrying out or providing that item.    "]
["1.2.3.               An item against which no Price is entered will be treated as covered by other Prices or rates in the bill of quantities.  "]
["1.2.4.               The quantities contained in the Bill of Quantities may not be final and do not necessarily represent the actual amount of work to be done.  The quantities of work assessed and certified for payment by the Project Manager at each assessment date will be used for determining payments due."]
["1.2.5.               The short descriptions of the items of payment given in the bill of quantities are only for the purposes of identifying the items.  Detail regarding the extent of the work entailed under each item is provided in the Works Information."]
["1.2.6.      The handling fee shall be deemed to include transportation and all logistical arrangements associated with the sourcing and provisioning of the material item."]
["1.2.7.    When claiming for Sleeping out ,attendance reigister must be submitted."]
["1.2.8.   For all transport claims google map to be atached."]
[]
["1.3.    Basic PPE "]
[]
[]
["Hard hat with chin strap"]
["Goggles"]
["Ear Plug"]
["Dust masks"]
["Gloves"]
["2 Piece overall cotton"]
["Reflective waistcoat "]
["Rainsiut "]
["Safety boots with steel cap"]
["Gumboots with steel  toe"]
["Soft hat"]
[]
["1.4 TRANSPORT"]
[".. The following shall apply:"]
["1.     Once off trip for all required transport equipment/ plant to and fro base   office. "]
["2.     Office – Site – Office  : transport for employees twice a month in a Kombi or Bakkie."]
["3.     Site camp – Site – Site camp : Daily trip to and fro for the employee transport (Kombi/ Bakkie) within a 10km radius."]
["4.     Site Camp to be within 10km’s of construction site. Special cases where the 10km’s radius is not practical will be looked unto by the responsible PM."]

{"sheet":"Summary","index":1,"n_rows":64,"n_cols":5,"rows_kept":64,"merged":[[0,2,0,4],[1,3,1,4],[2,3,2,4],[3,3,3,4],[4,3,4,4],[5,0,5,2],[8,0,10,0],[8,1,10,1],[8,2,10,2],[8,3,10,3],[8,4,10,4],[11,0,13,0],[11,1,13,1],[11,2,13,2],[11,3,13,3],[11,4,13,4],[14,0,16,0],[14,1,16,1],[14,2,16,2],[14,3,16,3],[14,4,16,4],[17,0,19,0],[17,1,19,1],[17,2,19,2],[17,3,19,3],[17,4,19,4],[20,0,22,0],[20,1,22,1],[20,2,22,2],[20,3,22,3],[20,4,22,4],[23,0,25,0],[23,1,25,1],[23,2,25,2],[23,3,25,3],[23,4,25,4],[26,0,28,0],[26,1,28,1],[26,2,28,2],[26,3,28,3],[26,4,28,4],[29,0,30,0],[29,1,30,1],[29,2,30,2],[29,3,30,3],[29,4,30,4],[31,0,33,0],[31,1,33,1],[31,2,33,2],[31,3,33,3],[31,4,33,4],[34,0,35,0],[34,1,35,1],[34,2,35,2],[34,3,35,3],[34,4,35,4],[36,0,37,0],[36,1,37,1],[36,2,37,2],[36,3,37,3],[36,4,37,4],[38,0,39,0],[38,1,39,1],[40,0,42,0],[40,1,42,1],[40,2,42,2],[40,3,42,3],[40,4,42,4]]}
[null,"GEMMA CLUSTER"]
["Project Name:",null,"Template Identifier:"]
["Project ID:",null,"Effective Date:"]
["Job Name:",null,"Review Date:"]
["Job ID:"]
["SUMMARY OF SCHEDULE OF QUANTITIES SUBSTATION BOQ"]
[]
[null,null,"SUPPLY","INSTALL","Total"]
["SECTION A","PRELIMINARY & GENERAL"]
[]
[]
["SECTION B"," CIVIL WORK, FACILITIES & SUBSTATION FENCING"]
[]
[]
["SECTION C","EARTH GRID"]
[]
[]
["SECTION D","FOUNDATION, TRFR BUND AREA & SLIPWAY, CABLE TRENCHES  AND KERBING & YARD STONE"]
[]
[]
["SECTION E","STEELWORK"]
[]
[]
["SECTION F","SUBSTATION EQUIPMENT AND SUBSTATION LIGHTING"]
[]
[]
["SECTION G","MISCELLANEOUS AND CLAMPS"]
[]
[]
["SECTION H","CABLE & STRINGERS "]
[]
["SECTION I","SUBSTATION LABELS AND SIGNS"]
[]
[]
["SECTION J","DISMANTLING"]
[]
["SECTION K","SUBSTATION SECONDARY PLANT"]
[]
["SECTION L","OTHER ADDITIONAL  ITEMS"]
[]
["TOTAL SCHEDULE OF QUANTITIES"]
[]
[]
[]
[]
[]
[]
["BOQ ISSUED BY :"]
[]
[]
[]
["PRINT NAME","Snr PROJECT ENGINEER - Control Plant","DATE"]
[]
[]
["PRINT NAME","Snr PROJECT ENGINEER - Primary Plant","DATE"]
[]
[]
["PRINT NAME","Snr PROJECT ENGINEER - Civil","DATE"]
[]
[]
["PRINT NAME","QUANTITY SURVEYOR","DATE"]
[]
[]
["PRINT NAME","PROJECT MANAGER","DATE"]

{"sheet":"SECTION A P&G's","index":2,"n_rows":73,"n_cols":11,"rows_kept":73,"merged":[[0,0,0,10],[1,0,1,10],[2,9,2,10],[3,9,3,10],[4,9,4,10],[6,0,6,10],[7,0,7,10],[8,0,8,10],[9,1,9,3],[10,0,11,0],[10,1,11,1],[10,2,11,2],[10,3,11,3],[10,4,10,5],[10,6,10,7],[10,8,10,9],[10,10,11,10],[18,0,18,3],[20,0,21,0],[20,1,21,1],[20,2,21,2],[20,3,21,3],[20,4,20,5],[20,6,20,7],[20,8,20,9],[20,10,21,10],[37,0,37,3],[39,0,40,0],[39,1,40,1],[39,3,40,3],[39,4,39,5],[39,6,39,7],[39,8,39,9],[39,10,40,10],[54,0,54,3],[57,0,57,3],[65,8,65,9],[66,8,66,9],[67,8,67,9]]}
[]
["GEMMA CLUSTER"]
["Project Name:",{"$nulls":6},"Template Identifier:"]
["Project ID:",{"$nulls":6},"Effective Date:"]
["Job Name:",{"$nulls":6},"Review Date:"]
["Job ID:"]
["SCHEDULE OF QUANTITIES - SECTION A"]
["PRELIMINARIES & GENERAL"]
[]
["A","PRELIMINARIES & GENERAL"]
["Item No.","Description of the item","Contracted Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
[{"$nulls":4},"Supply","Install","Supply Rate","Labour Rate","Supply","Install"]
["A.1","Site Establishment"]
["A1..1","Site Yard 30m x 35m =1050m2 ",null,"Item",{"$nulls":3},{"v":12745.346956521738,"d":"12,745.35"}]
["A1..2","Fencing incl dropper poles every 3m and access gate 6m wide.",null,"Item",{"$nulls":3},{"v":13670.218730434783,"d":"13,670.22"}]
["A1..3","Security Guard house and sanitation ( As per Security risk assesment)",null,"Item",{"$nulls":3},0]
["A1..4","Transportation of of  all site establishment facilities ,plant, tools etc. ",null,"Item",{"$nulls":3},{"v":17750.064347826086,"d":"17,750.06"}]
["A1..5","Site De-establishment",null,"Item",{"$nulls":3},{"v":24739.154751304348,"d":"24,739.15"}]
["Subtotal carried to Item A of Summary"]
[]
["Item No.","Description of the item","Contracted Description of the item","Unit","Rate",null,"Rate",null,"Total",null,"Price (R)"]
[{"$nulls":4},"Supply","Install","Supply","Install","Supply","Install"]
["A.2","Contractor’s time related items:"]
["A2.1","Site office 6m x 3m steel container (including maintenance)",null,"monthly",{"$nulls":3},{"v":6356.95773102989,"d":"6,356.96"}]
["A2.2","Site storage 6m x 3m steel container (including maintencance and site storeperson costs)",null,"monthly",{"$nulls":3},{"v":7792.934696795643,"d":"7,792.93"}]
["A2.3","Sanitary facilities (including Maintenance) (R2520/Toilet)",null,"monthly",{"$nulls":3},{"v":2669.9222470325535,"d":"2,669.92"}]
["A2.4","Sleeping out allowance (Accomodation & meals for Employees) (per person/30days)",null,"monthly",{"$nulls":3},{"v":8726.173913043478,"d":"8,726.17"}]
["A2.5","Communication ",null,"monthly",{"$nulls":3},{"v":2397.054652305165,"d":"2,397.05"}]
["A2.6","clean water (Jojo Tanks, including maintenace)",null,"monthly",{"$nulls":3},{"v":4841.881291573068,"d":"4,841.88"}]
["A2.7","Electricity",null,"monthly",{"$nulls":3},{"v":3305.6180201355423,"d":"3,305.62"}]
["A2.8","Site Security (As per Eskom proposed site specific requirements) (As per qoute(PSIRA RATE) + handling fee of 10%)",null,"monthly",{"$nulls":3},"cost+5%"]
["A2.9","compliance reporting (EPWP, etc.)",null,"monthly",{"$nulls":3},{"v":1852.5234321176272,"d":"1,852.52"}]
["A2.10","Community Liason Officer (CLO)",null,"monthly",{"$nulls":3},{"v":5297.4647758582405,"d":"5,297.46"}]
["A2.11","Project Steering Committee (PSC)",null,"monthly",{"$nulls":3},{"v":4237.971820686593,"d":"4,237.97"}]
["A2.12","Supervision",null,"monthly",{"$nulls":3},{"v":42219.34275824159,"d":"42,219.34"}]
["A2.13","Safety Officer",null,"monthly",{"$nulls":3},{"v":25242.56533724586,"d":"25,242.57"}]
["A2.14","1. Contractor's insurance.                                                                 2. Company & head office overhead costs.                                              3. Personal Protective Equipment .                                                 4. Plant, tools and equipment .                                                        5. Risk Assessment Procedure, QM, Quality Management System, Health and Safety Specification, Environmental Plan, Safety Inspections, OHSA appointments, etc.                                                  6. Environmental Compliance & Site maintenance (waste management, site habitability etc.) .                                                7. Safety Compliance & Site maintenance (first aid, fire extinguisher, medical tests, inductions, signage etc).            (10% of Total Labour Cost)",null,"%",{"$nulls":3},{"v":0.07,"d":"7%"}]
["Subtotal carried to Item B of Summary",{"$nulls":7},{"$f":"SUM(I24:I37)","v":0},{"$f":"SUM(J24:J37)","v":0},{"$f":"SUM(K24:K37)","v":0}]
[]
["Item No.","Description of the item",null,"Unit","Rate",null,"Rate",null,"Total",null,"Price (R)"]
[{"$nulls":4},"Supply","Install","Supply","Install","Supply","Install"]
["A.3","Transport "]
["A3.1","LDV Transport 4 x 2",null,"km",{"$nulls":3},{"v":7.023153482161257,"d":"7.02"}]
["A3.2","LDV Transport 4 x 4",null,"km",{"$nulls":3},{"v":8.411186153223383,"d":"8.41"}]
["A3.3","Transport for labour (minibus 13)",null,"km",{"$nulls":3},{"v":10.019125860818852,"d":"10.02"}]
["A3.4","Transport for labour (minibus 23)",null,"km",{"$nulls":3},{"v":13.508239108917355,"d":"13.51"}]
["A3.5","6 m³ Tipper Truck",null,"km",{"$nulls":3},{"v":22.430728693067596,"d":"22.43"}]
["A3.6","10m³ Tipper Truck",null,"km",{"$nulls":3},{"v":28.055349436399222,"d":"28.06"}]
["A3.7","Transport Truck 2-4 ton",null,"km",{"$nulls":3},{"v":12.585315939985112,"d":"12.59"}]
["A3.8","Transport Truck 5-8 ton",null,"km",{"$nulls":3},{"v":18.87797390997767,"d":"18.88"}]
["A3.9","Transport Truck 5-8 ton with crane",null,"km",{"$nulls":3},{"v":23.204176264347552,"d":"23.20"}]
["A3.10","Transport Truck 9-14 ton",null,"km",{"$nulls":3},{"v":28.70592008586532,"d":"28.71"}]
["A3.11","Transport Truck 9-14 ton with crane",null,"km",{"$nulls":3},{"v":35.66125546236842,"d":"35.66"}]
["A3.12","Transport truck >22 ton",null,"km",{"$nulls":3},{"v":53.78125011686972,"d":"53.78"}]
["Subtotal carried to Item C of Summary",{"$nulls":7},{"$f":"SUM(I43:I54)","v":0},{"$f":"SUM(J43:J54)","v":0},{"$f":"SUM(K43:K54)","v":0}]
[]
[]
["PRELIMINARIES & GENERAL"]
[]
["Item\nNo.","Description of the item","Contracted Description of the item","Page","Install","PRICE (R)",null,null,"Supply","Install","PRICE (R)"]
["A.1","Site Establishment"]
["A.2","Contractor’s time related items"]
["A.3","Transport "]
[]
["Total of the prices Excluding VAT"]
[{"$nulls":8},"Please initial"]
[{"$nulls":8},"Compiler/Designer:"]
[{"$nulls":8},"Quantity Surveyor"]
[null,".. The following shall apply:"]
[null,"1.     Once off trip for all required transport equipment/ plant to and fro base office. "]
[null,"2.     Office – Site – Office  : transport for employees twice a month in a Kombi or Bakkie."]
[null,"3.     Site camp – Site – Site camp : Daily trip to and fro for the employee transport (Kombi/ Bakkie) within a 10km radius."]
[null,"4.     Site Camp to be within 10km’s of construction site. Special cases where the 10km’s radius is not practical will be looked unto by the responsible PM."]

{"sheet":" Section B Civil","index":3,"n_rows":220,"n_cols":11,"rows_kept":220,"merged":[[1,0,1,10],[2,0,2,1],[2,9,2,10],[3,0,3,1],[3,9,3,10],[4,0,4,1],[4,9,4,10],[5,0,5,1],[6,0,6,10],[7,0,7,10],[8,1,8,3],[9,1,10,1],[9,2,10,2],[9,3,10,3],[9,4,9,5],[9,6,9,7],[9,8,9,9],[9,10,10,10],[64,8,64,9],[65,1,66,1],[65,2,66,2],[65,3,66,3],[65,4,65,5],[65,6,65,7],[65,8,65,9],[65,10,66,10],[131,1,132,1],[131,2,132,2],[131,3,132,3],[131,4,131,5],[131,6,131,7],[131,8,131,9],[131,10,132,10],[217,8,217,9],[218,8,218,9],[219,8,219,9]]}
[]
["GEMMA CLUSTER"]
["Project Name:",{"$nulls":6},"Template Identifier:"]
["Project ID:",{"$nulls":6},"Effective Date:"]
["Job Name:",{"$nulls":6},"Review Date:"]
["Job ID:"]
["SCHEDULE OF QUANTITIES - SECTION B"]
["CIVIL WORK, FACILITIES & SUBSTATION FENCING"]
["B1","CIVIL WORK"]
["Item","Refer","Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,null,"Supply the material, transport to site, excavate into all material, backfill, compact and construct"]
["B1.1",null,"EARTHWORKS (SANS 1200 D)"]
["B1.1.1",null,"Setting-out of earthworks ","Sum",null,null,{"v":6304.139358482194,"d":"6,304.14"},{"v":3804.4979362940326,"d":"3,804.50"}]
["B1.2",null,"SITE CLEARANCE (SANS 1200 C and 1200 D)"]
[null,null,"The Contractor shall detect for the presence of underground services (electric cables, sewerage & stormwater)"]
["B1.2.1",null,"1.5x1.5x2m Trial Hole","each",null,null,{"v":2781.1690073255763,"d":"2,781.17"},{"v":1158.3966225369215,"d":"1,158.40"}]
["B1.2.2",null,"Substation site to be cleared of all trees up to 300mm girth, vegetation and topsoil to a nominal depth of 150mm, including disposal and free haul. ","m²",{"$nulls":3},{"v":72.72727272727272,"d":"72.73"}]
["B1.2.3",null,"Long haul 2 - 10km load radius","m³",{"$nulls":3},{"v":48,"d":"48.00"}]
["B1.3",null,"BULK EXCAVATION (SANS 1200 D)"]
[null,null,"Excavate in all material.(this is measured in compacted density as per SANS 1200 D-1980, the Project Engineer shall decide what is to happen with the in-situ material)"]
["B1.3.1",null,"Stock Piling of excavated material","m³",null,null,"Cost plus 5%",{"v":33.585926678941256,"d":"33.59"}]
["B1.3.2",null,"Cart away excavated material","m³",null,null,"Cost plus 5%",{"v":161.74219453650383,"d":"161.74"}]
["B1.4",null,"Extra over excavation for"]
["B1.4.1",null,"Soil Excavation in Pickable Soil ","m³",null,null,"Cost plus 5%",{"v":77.55488431856466,"d":"77.55"}]
["B1.4.2",null,"Compact Soil to 95% Mod AASHTO","m²",null,null,"Cost plus 5%",{"v":36.23465906687037,"d":"36.23"}]
["B1.4.3",null,"Cast concrete to 25 Mpa density","m³",null,null,"Cost plus 5%",{"v":737.193211659142,"d":"737.19"}]
["B1.4.4",null,"Block Retaining wall","m²",null,null,"Cost plus 5%",{"v":349.9649019261585,"d":"349.96"}]
["B1.4.5",null,"Grassing Retaining wall","m²",null,null,"Cost plus 5%",{"v":43.86300834410624,"d":"43.86"}]
["B1.4.6",null,"Precast water channel","m",null,null,"Cost plus 5%",{"v":151.21991593028483,"d":"151.22"}]
["B1.4.7",null,"Water diversion berm","m",null,null,"Cost plus 5%",{"v":164.48628129039838,"d":"164.49"}]
["B1.4.8",null,"1) intermediate excavation","m³",null,null,"Cost plus 5%",{"v":52.12705339444509,"d":"52.13"}]
["B1.4.9",null,"2) hard rock excavation","m³",null,null,"Cost plus 5%",{"v":116.22637718232981,"d":"116.23"}]
["B1.4.10",null,"3) boulder excavation, Class A","m³",null,null,"Cost plus 5%",{"v":526.2854672655967,"d":"526.29"}]
["B1.4.11",null,"4) boulder excavation, Class B","m³",null,null,"Cost plus 5%",{"v":273.4198152979634,"d":"273.42"}]
["B1.4.12",null,"5) Excavation of hard rock by means of chemical method ","m³",null,null,"Cost plus 5%",{"v":551.6779817578773,"d":"551.68"}]
["B1.4.13",null,"Backfill and compact with excavated  material(stockpile)  in layers of 200mm thick to 95% of Mod. AASHTO density up to final level.","m³",null,null,"Cost plus 5%",{"v":182.46587673966127,"d":"182.47"}]
["B1.4.14",null,"Backfill and compact with imported G5/G6 material from commercial sources in layers of 200mm thick to 95% of Mod. AASHTO density to final level, including final cutting and levelling","m³",null,null,"Cost plus 5%",{"v":185.0669319446077,"d":"185.07"}]
["B1.4.15",null,"Soil cement backfill(1:5) in layers of 200mm where required/necessary","m³",null,null,"Cost plus 5%",{"v":361.50959123411803,"d":"361.51"}]
["B1.4.16",null,"Backfill all the pits to full capacity, level to ground and hand compact. (Note: Supply and transport the material from the nearest borrow pit. Pits include that of foundations, plinth, Curbing, fencing and control room foundations)","m³",null,null,"Cost plus 5%",{"v":185.0669319446077,"d":"185.07"}]
["B1.5",null,"Embarkment protection"]
["B1.5.1",null,"Supply and install stone pitching as per the drawing around the embankment to avoid erosion, 1.5m wide","m²",null,null,"Cost plus 5%",{"v":113,"d":"113.00"}]
["B1.6",null,"Brick retaining wall"]
["B1.6.1",null,"Build a berm wall using the existing soil as per the drawing","m²",null,null,"Cost plus 5%",{"v":164.48628129039838,"d":"164.49"}]
["B1.6.2",null,"Remove retaining blocks and reposition at embankment","m²",null,null,"Cost plus 5%",{"v":169.92148015042895,"d":"169.92"}]
["B1.6.3",null,"Build a brick retaining wall as per the drawing (units is in m)","m²",null,null,"Cost plus 5%",{"v":1817.1681522035492,"d":"1,817.17"}]
["B1.7",null,"Drainage/Stormwater management"]
["B1.7.1",null,"Supply, delivery and construction of a concrete V-drain as per the drawing","m",null,null,"Cost plus 5%",{"v":228.85047831707604,"d":"228.85"}]
["B1.7.2",null,"Build a subsurface drain as per the drawing","m",null,null,"Cost plus 5%",{"v":2593,"d":"2,593.00"}]
["B1.8",null,"Access road"]
["B1.8.1",null,"Build paving access road to the substation, as per the drawing.","m",null,null,"Cost plus 5%",{"v":195.02616572322114,"d":"195.03"}]
["B1.8.2",null,"Build gravel access road to the substation, as per the drawing.","m",null,null,"Cost plus 5%",{"v":195.02616572322114,"d":"195.03"}]
["B1.8.3",null,"Supply and install 300mm concrete pipe to divert storm water and to prevent ponding","m",null,null,"Cost plus 5%",{"v":190.7087319308967,"d":"190.71"}]
["B1.8.4",null,"300mm Diameter concrete pipe Shale","m",null,null,"Cost plus 5%",{"v":190.7087319308967,"d":"190.71"}]
["B1.8.5",null,"300mm Diameter concrete pipe Soft Rock","m",null,null,"Cost plus 5%",{"v":190.7087319308967,"d":"190.71"}]
["B1.8.6",null,"Supply and install Culvert as per the drawing","each",null,null,"Cost plus 5%",{"v":833.3971585380185,"d":"833.40"}]
["B1.9",null,"DRAINAGE CHANNEL, YARDSTONE AND EXISTING DRAINAGE SYSTEM"]
[null,null,"SETTING-OUT: SANS 1200 AA."]
["B1.9.1",null,"Setting-out of drainage channel, yard stone","sum",null,null,"Cost plus 5%",{"v":1060.3935241835443,"d":"1,060.39"}]
["B1.9.2",null,"1. Supply and transport all building material required for the complete construction of the concrete lined gutter with grating as indicated on the Foundation plan and as per the detail drawing 0.54/390 sheet 6.","m",null,null,"Cost plus 5%",{"v":459.34105172875775,"d":"459.34"}]
["B1.9.3",null,"2. Supply, transport and completely install all materials required to construct a outlet with wing walls as indicated on site plan.","sum",null,null,"Cost plus 5%",{"v":1287.2839405335526,"d":"1,287.28"}]
["B.1.10",null,"Neutralizing of substation yard"]
["B1.10.1",null,"Treating of yard surface with Eskom approved herbicides, insecticides, etc.","m²",null,null,"Cost plus 5%",{"v":9.206993780441621,"d":"9.21"}]
[null,null,"                                                                Total carried to Item of Summary"]
["B2.",null,"FACILITIES"]
["Item","Refer","Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,null,"Supply the material, transport to site, excavate into all material, backfill, compact and install"]
["B.2.1","Drawing No.","CONTROL ROOM"]
["B2.1.1","D-ST 1287 R0","Build 220mm Brick Retaining Wall ","m²",null,null,"Cost plus 5%",{"v":573.5918277140108,"d":"573.59"}]
["B2.1.2","D-DT 5239 S1-4 R4","Build Control/Relay Room","m²",null,null,"Cost plus 5%",{"v":2860.6309789634506,"d":"2,860.63"}]
["B2.1.3","D-DT 5238 S1-4 R1 / D-DT 5238 S13-14 R0 / D-DT 5238 S15-16 R1","Build Switch Room with sloping steel roof as per drawing","m²",null,null,"Cost plus 5%",{"v":2860.6309789634506,"d":"2,860.63"}]
["B2.1.4","D-DT 5238 S5-12 R1 / D-DT 5238 S13-14 R0 / D-DT 5238 S16 R1","Build Switch Room with conventional roof as per drawing","m²",null,null,"Cost plus 5%",{"v":2860.6309789634506,"d":"2,860.63"}]
["B2.1.5","D-DT 5238 S1-4 R1 / D-DT 5238 S13-14 R0 / D-DT 5238 S15-16 R1","Build Switch Room with sloping steel roof as per drawing with cavity wall filled with concrete","m²",null,null,"Cost plus 5%",{"v":2860.6309789634506,"d":"2,860.63"}]
["B2.1.6","D-DT 5238 S5-12 R1 / D-DT 5238 S13-14 R0 / D-DT 5238 S16 R1","Build Switch Room with conventional roof as per drawing with cavity wall filled with concrete","m²",null,null,"Cost plus 5%",{"v":2860.6309789634506,"d":"2,860.63"}]
["B2.1.7",null,"AIR CONDITIONER 12000 BTU","each",null,null,"Cost plus 5%",{"v":380,"d":"380.00"}]
["B2.1.8",null,"AIR CONDITIONER 18000 BTU","each",null,null,"Cost plus 5%",{"v":380,"d":"380.00"}]
["B2.1.9",null,"AIR CONDITIONER 24000 BTU","each",null,null,"Cost plus 5%",{"v":380,"d":"380.00"}]
["B2.1.10",null,"Replace gutters and down pipes of Control/battery room.","m",null,null,"Cost plus 5%",{"v":90.39064147046918,"d":"90.39"}]
["B2.1.11",null,"Repair door lintel and paint.","item",null,null,"Cost plus 5%",{"v":156.18250525424057,"d":"156.18"}]
["B2.1.12",null,"Paint Control / Battery room on inside and outside completely","m2",null,null,"Cost plus 5%",{"v":75.94277264284139,"d":"75.94"}]
["B2.1.13",null,"Neatly break out and remove windows","each",null,null,"Cost plus 5%",{"v":487.3667593789582,"d":"487.37"}]
["B2.1.14",null,"Supply & install fibre cement covers for cable entry to control room ","each",null,null,"Cost plus 5%",{"v":238.38591491362087,"d":"238.39"}]
["B2.1.15",null,"Replace door at toilet with galvanised door with 4 level lock and door handle as per Eskom standard","each",null,null,"Cost plus 5%",{"v":1381.6847628393464,"d":"1,381.68"}]
["B2.1.16",null,"Provide vastrap / Chequer plates covers & supports in switch room ","m²",null,null,"Cost plus 5%",{"v":1782.0671505987125,"d":"1,782.07"}]
["B2.1.17",null,"Neatly break out and remove 2400 x 1524mm double door and prepare for new door installation. ","Each",null,null,"Cost plus 5%",{"v":4000,"d":"4,000.00"}]
["B2.1.18","D-DT-5238s13r1","Supply and install 2600 x 1524mm double door as per D-DT-5238s13r1.","Each",null,null,"Cost plus 5%",{"v":2700,"d":"2,700.00"}]
["B2.1.19",null,"Supply and install Vimba Locks","Each",null,null,"Cost plus 5%",{"v":2700,"d":"2,700.00"}]
["B2.1.20",null,"Breakdown a 220mm wall, make a 1000x600mm opening, trim the opening, plaster and paint along with the wall","item",null,null,"Cost plus 5%",{"v":4050,"d":"4,050.00"}]
["B2.1.21",null,"Demolish concrete floor to allow for the extension cable trench extension including disposal of concrete rubble and insitu material. ","m²",{"$nulls":3},{"v":4989.43,"d":"4,989.43"}]
["B2.1.22",null,"Supply necessary material and build a 230mm supporting wall and re-inforced concrete floor (mesh ref. 395) to extend cable trench ","m²",null,null,"Cost plus 5%",{"v":4224.261190786614,"d":"4,224.26"}]
["B2.1.23",null,"Paint the building inside walls, ceiling, floors and outside upper walls (Rate to include scrapping of old paint)","m²",null,null,"Cost plus 5%",{"v":71.67841208584338,"d":"71.68"}]
["B2.1.24",null,"Rewire existing switch room light circuit to accommodate emergency lighting including Control Room. ","item",null,null,"Cost plus 5%",{"v":9500,"d":"9,500.00"}]
["B2.1.25",null,"Fluorescent light fitting complete with 2 x 58W T8 Fluorescent tubes each. ","each",null,null,"Cost plus 5%",{"v":150,"d":"150.00"}]
["B2.1.26",null,"15W LED Bulkhead fittings with cast aluminium base and polycarbonate diffuser ","each",null,null,"Cost plus 5%",{"v":150,"d":"150.00"}]
["B2.1.27",null,"Photo cell - Day night switch ","each",null,null,"Cost plus 5%",{"v":177,"d":"177.00"}]
["B2.1.28",null,"Remove batteries and dispose according to environmental regulations","ea",null,null,"Cost plus 5%",{"v":29166.666666666664,"d":"29,166.67"}]
["B2.1.29",null,"Remove1.5m 2xtubes flourescent light fittings","ea",null,null,"Cost plus 5%",{"v":150,"d":"150.00"}]
["B2.1.30",null,"Remove Bulkhead light fittings.","ea",null,null,"Cost plus 5%",{"v":50,"d":"50.00"}]
["B2.1.17",null,"Supply and install Air-filter","each",null,null,"Cost plus 5%",{"v":175.01310058071098,"d":"175.01"}]
["B2.1.18",null,"Install burglars bars outside of wind blocks","each",null,null,"Cost plus 5%",{"v":191.3757870599603,"d":"191.38"}]
["B2.1.19",null,"Neatly brick up window openning. Bricks to match the existing wall, including wall tiers","m²",null,null,"Cost plus 5%",{"v":1363.5488921791957,"d":"1,363.55"}]
["B2.1.20",null,"Install 200mm dia. concrete drain pipe from Control room entrance sump to water trench out side yard","m",null,null,"Cost plus 5%",{"v":279.78162903837114,"d":"279.78"}]
["B2.1.21",null,"Install interlocking paving at Control room entrance","m²",null,null,"Cost plus 5%",{"v":184.7437865932803,"d":"184.74"}]
["B2.1.22",null,"Remove existing broken paving as per instruction","m²",null,null,"Cost plus 5%",{"v":113.05243900090846,"d":"113.05"}]
["B2.1.23",null,"Remove retaining blocks and reposition at embankment","m²",null,null,"Cost plus 5%",{"v":169.92148015042895,"d":"169.92"}]
["B2.1.24",null,"Build a 440mm wide double brick retaining wall high at embankment.","m²",null,null,"Cost plus 5%",{"v":1817.1716838467332,"d":"1,817.17"}]
["B2.1.25","2-ET/14904","Acid Evaporation dam","item",null,null,"Cost plus 5%",{"v":520,"d":"520.00"}]
["B2.1.26","D-DT-5239s3","Install whirly birds fans as per drawings","item",null,null,"Cost plus 5%",{"v":520,"d":"520.00"}]
["B2.1.27","D-DT-5239s3","Install lights according to the drawing","each",null,null,"Cost plus 5%",{"v":50,"d":"50.00"}]
["B2.1.28",null,"Install Enviro Loo or water borne sewerage toilet if water is available","each",null,null,"Cost plus 5%",{"v":8500,"d":"8,500.00"}]
["B2.1.29",null,"The contractor shall allow for the supply and installation of an outdoor type waterproof switch for the yard lighting; this will be wired to a contactor in the yard box via a 4mm-4core cable","item",null,null,"Cost plus 5%",{"v":1126.664808529531,"d":"1,126.66"}]
["B2.1.30",null,"Alterations to existing steel plates and frames to accommodate all panels and cables in the control rooms and switch room.","m²",null,null,"Cost plus 5%",{"v":178.78943618521566,"d":"178.79"}]
["B2.1.31",null,"Acid Evaporation dam painting","m²",null,null,"Cost plus 5%",{"v":75.94277264284139,"d":"75.94"}]
["B2.1.32",null,"Electrical installation and wiring for the  Control/Battery  Room including lighting","item",null,null,"Cost plus 5%",{"v":8500,"d":"8,500.00"}]
["B2.1.33",null,"Supply and install Plates for Cable Rack","item",null,null,"Cost plus 5%",{"v":1566,"d":"1,566.00"}]
["B2.1.34",null,"Acid Resistance Paint for the Battery Room","m²",null,null,"Cost plus 5%",{"v":75.94277264284139,"d":"75.94"}]
["B2.1.35",null,"Supply and install Yard AC for NEC and Oildam","item",null,null,"Cost plus 5%",{"v":1984.44725692378,"d":"1,984.45"}]
["B2.1.36",null,"Supply & Install Handrails","m",null,null,"Cost plus 5%",{"v":95.5,"d":"95.50"}]
["B2.1.37"]
["B2.2",null,"OVERHEAD RACKING"]
["B2.2.1",null,"Overhead Cable Rack","m",null,null,"Cost plus 5%",{"v":170.0067104726005,"d":"170.01"}]
["B2.3",null,"CONTROL ROOM FURNITURE AND ACCESSORIES"]
["B2.3.1","2-ET/14905 S5","Desk and Lockable Bin for Portable Earths","each",null,null,"Cost plus 5%",{"v":126,"d":"126.00"}]
["B2.3.2","D-DT 6101","Desk and Lockable Bin for Portable Earths","each",null,null,"Cost plus 5%",{"v":126,"d":"126.00"}]
["B2.3.3","D-DT 6101","Chair, Steel Frame arm/rest desk","each",null,null,"Cost plus 5%",{"v":60.3,"d":"60.30"}]
["B2.3.4","D-DT 6100","Board, Notice Pin 1200x900mm","each",null,null,"Cost plus 5%",{"v":60.3,"d":"60.30"}]
["B2.3.5","D-DT 6103","Netting, Barrier 50m L x 2m H Nylon","each",null,null,"Cost plus 5%",{"v":60.3,"d":"60.30"}]
["B2.3.6","D-DT 6082","Earth Kit, Work Assy Sub YL 21kA Up","each",null,null,"Cost plus 5%",{"v":113,"d":"113.00"}]
[null,null,"                                                                Total carried to Item of Summary"]
["B3",null,"SUBSTATION FENCING"]
["Item","Refer","Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,null,"Supply the material, transport to site, excavate into all material, dispose of excavated material, backfill, compact, install and pour complete support foundations with holding down bolts and earth connections as detailed in the drawings. Civil Engineer to clarify the soil type:"]
["B3.1",null,"Boundary Fence"]
["B3.1.1","D-DT 5237 S1A ","1.24m High Double Leaf Gate (6m Wide)","each",null,null,"Cost plus 5%",{"v":590.7322164516982,"d":"590.73"}]
["B3.1.2","D-DT 5237 S1A ","1.24m High x 1m Wide Gate","each",null,null,"Cost plus 5%",{"v":485.68746304501116,"d":"485.69"}]
["B3.1.3","D-DT 5237 S1A ","1.24m High Fence Hard Rock with Posts Hard Rock","m",null,null,"Cost plus 5%",{"v":108.22014208441605,"d":"108.22"}]
["B3.1.4","D-DT 5237 S1A ","1.24m High Fence Hard Rock with Posts Shale","m",null,null,"Cost plus 5%",{"v":93.2035952664499,"d":"93.20"}]
["B3.1.5","D-DT 5237 S1A ","1.24m High Fence Hard Rock with Posts Soft Rock","m",null,null,"Cost plus 5%",{"v":93.20889273122575,"d":"93.21"}]
["B3.2",null,"1.8m Diamond Mesh No Overhang"]
["B3.2.1","D-DT 5237 S2A ","1.8m High Double Leaf Gate (6m Wide)","each",null,null,"Cost plus 5%",{"v":2811.831696623658,"d":"2,811.83"}]
["B3.2.2","D-DT 5237 S2A ","1.8m High x 1m Wide Gate","each",null,null,"Cost plus 5%",{"v":1381.6847628393464,"d":"1,381.68"}]
["B3.2.3","D-DT 5237 S2A ","1.8m High x 1,5m Wide Gate","each",null,null,"Cost plus 5%",{"v":1381.6847628393464,"d":"1,381.68"}]
["B3.2.4","D-DT 5237 S2A ","1.8m High Diamond Mesh Fence Hard Rock","m",null,null,"Cost plus 5%",{"v":205.96543048536842,"d":"205.97"}]
["B3.2.5","D-DT 5237 S2A ","1.8m High Diamond Mesh Fence Shale","m",null,null,"Cost plus 5%",{"v":228.85047831707604,"d":"228.85"}]
["B3.2.6","D-DT 5237 S2A ","1.8m High Diamond Mesh Fence Soft Rock","m",null,null,"Cost plus 5%",{"v":220.4861889332863,"d":"220.49"}]
["B3.3",null,"1.8m Diamond Mesh With Overhang"]
["B3.3.1","D-DT 5237 S3A ","1.8m High Double Leaf Gate (6m Wide)","each",null,null,"Cost plus 5%",{"v":2860.6309789634506,"d":"2,860.63"}]
["B3.3.2","D-DT 5237 S3A ","1.8m High x 1m Wide Gate","each",null,null,"Cost plus 5%",{"v":1381.6847628393464,"d":"1,381.68"}]
["B3.3.3","D-DT 5237 S3A ","1.8m High x 1,5m Wide Gate","each",null,null,"Cost plus 5%",{"v":1381.6847628393464,"d":"1,381.68"}]
["B3.3.4","D-DT 5237 S3A ","1.8m High Diamond Mesh Fence Hard Rock","m",null,null,"Cost plus 5%",{"v":341.59165342336865,"d":"341.59"}]
["B3.3.5","D-DT 5237 S3A ","1.8m High Diamond Mesh Fence Shale","m",null,null,"Cost plus 5%",{"v":325.39359537822696,"d":"325.39"}]
["B3.3.6","D-DT 5237 S3A ","1.8m High Diamond Mesh Fence Soft Rock","m",null,null,"Cost plus 5%",{"v":330.11681497238214,"d":"330.12"}]
["B3.4",null,"1.8m Diamond Mesh With Double Overhang"]
["B3.4.1","D-DT 5237 S4A ","1.8m High Double Leaf Gate (6m Wide)","each",null,null,"Cost plus 5%",{"v":3132.9047760482363,"d":"3,132.90"}]
["B3.4.2","D-DT 5237 S4A ","1.8m High x 1m Wide Gate","each",null,null,"Cost plus 5%",{"v":1599.8025775205338,"d":"1,599.80"}]
["B3.4.3","D-DT 5237 S4A ","1.8m High x 1,5m Wide Gate","each",null,null,"Cost plus 5%",{"v":1595.1533297981578,"d":"1,595.15"}]
["B3.4.4","D-DT 5237 S4A ","1.8m High Diamond Mesh Fence Hard Rock","m",null,null,"Cost plus 5%",{"v":384.7501578130055,"d":"384.75"}]
["B3.4.5","D-DT 5237 S4A ","1.8m High Diamond Mesh Fence Shale","m",null,null,"Cost plus 5%",{"v":366.25900919952846,"d":"366.26"}]
["B3.4.6","D-DT 5237 S4A ","1.8m High Diamond Mesh Fence Soft Rock","m",null,null,"Cost plus 5%",{"v":329.8122107477702,"d":"329.81"}]
["B3.5",null,"2.4m Diamond Mesh With Flatwrap"]
["B3.5.1","D-DT 5237 S5A ","2.4m High Double Leaf Gate (5m Wide)","each",null,null,"Cost plus 5%",{"v":3877.9384563033477,"d":"3,877.94"}]
["B3.5.2","D-DT 5237 S5A ","2.4m High x 1m Wide Gate","each",null,null,"Cost plus 5%",{"v":1760.4711525291304,"d":"1,760.47"}]
["B3.5.3","D-DT 5237 S5A ","2.4m High x 1,5m Wide Gate","each",null,null,"Cost plus 5%",{"v":1611.7624871628295,"d":"1,611.76"}]
["B3.5.4","D-DT 5237 S5A ","2.4m High Diamond Mesh Fence Hard Rock","m",null,null,"Cost plus 5%",{"v":467.09914073423147,"d":"467.10"}]
["B3.5.5","D-DT 5237 S5A ","2.4m High Diamond Mesh Fence Shale","m",null,null,"Cost plus 5%",{"v":459.6297154002714,"d":"459.63"}]
["B3.5.6","D-DT 5237 S5A ","2.4m High Diamond Mesh Fence Soft Rock","m",null,null,"Cost plus 5%",{"v":448.8303518669775,"d":"448.83"}]
["B3.6",null,"2.4m Weld Mesh With Double Overhang & Razor Coil Wire"]
["B3.6.1","D-DT 5237 S6A ","2.4m High Double Leaf Gate (6.5m Wide)","each",null,null,"Cost plus 5%",{"v":5428.034333224806,"d":"5,428.03"}]
["B3.6.2","D-DT 5237 S6A ","2.4m High x 1m Wide Gate","each",null,null,"Cost plus 5%",{"v":1737.0780525993953,"d":"1,737.08"}]
["B3.6.3","D-DT 5237 S6A ","2.4m High x 1,5m Wide Gate","each",null,null,"Cost plus 5%",{"v":1869.9319608640524,"d":"1,869.93"}]
["B3.6.4","D-DT 5237 S6A ","2.4m High Weld Mesh Fence Hard Rock","m",null,null,"Cost plus 5%",{"v":476.77182982724173,"d":"476.77"}]
["B3.6.5","D-DT 5237 S6A ","2.4m High Weld Mesh Fence Shale","m",null,null,"Cost plus 5%",{"v":476.77182982724173,"d":"476.77"}]
["B3.6.6","D-DT 5237 S6A ","2.4m High Weld Mesh Fence Soft Rock","m",null,null,"Cost plus 5%",{"v":476.77182982724173,"d":"476.77"}]
["B3.6.7","D-DT 5237 S6D ","2.4m High Motorised (6.5m Wide) Gate ","each",null,null,"Cost plus 5%",{"v":7666.3941556947175,"d":"7,666.39"}]
["B3.7",null,"2.4m Steel Palisade Panel Fence",{"$nulls":3},0,0]
["B3.7.1","D-DT 5237 S7E ","2.4m High Double Leaf Gate (5m Wide)","each",null,null,"Cost plus 5%",{"v":4244.964474190725,"d":"4,244.96"}]
["B3.7.2","D-DT 5237 S7E ","2.4m High Double Leaf Gate (4m Wide)","each",null,null,"Cost plus 5%",{"v":4251.111299152313,"d":"4,251.11"}]
["B3.7.3","D-DT 5237 S7E ","2.4m High x 1m Wide Gate","each",null,null,"Cost plus 5%",{"v":1397.8332012977544,"d":"1,397.83"}]
["B3.7.4","D-DT 5237 S7E ","2.4m High x 1,5m Wide Gate","each",null,null,"Cost plus 5%",{"v":1405.1631267259502,"d":"1,405.16"}]
["B3.7.5","D-DT 5237 S7E ","2.4m High x 2m Wide Gate","each",null,null,"Cost plus 5%",{"v":2498.882245033736,"d":"2,498.88"}]
["B3.7.6","D-DT 5237 S7E ","2.4m High x 2,5m Wide Gate","each",null,null,"Cost plus 5%",{"v":2553.1396360487583,"d":"2,553.14"}]
["B3.7.7","D-DT 5237","6m Sliding gate","each",null,null,"Cost plus 5%",{"v":946.6741722063892,"d":"946.67"}]
["B3.7.8","2-ET/14610","6m Sliding gate","each",null,null,"Cost plus 5%",{"v":946.6741722063892,"d":"946.67"}]
["B3.8","2-ET/14899","Supply and install 150x150mm square tubing galvanised poles 3m tall for gates. Plant 650mm deep with  concrete footing. Add locking hooks to keep gate in place once opened."]
["B3.8.1","2-ET/14899","2.4m High Personnel Gate 1m Wide","each",null,null,"Cost plus 5%",{"v":643.7068642102805,"d":"643.71"}]
["B3.8.2","2-ET/14899","2.4m High Double Leaf Gate 5m Wide","each",null,null,"Cost plus 5%",{"v":644.7663571654522,"d":"644.77"}]
["B3.8.3","2-ET/14899","2.4m High Steel Palisade Fence","each",null,null,"Cost plus 5%",{"v":645.8258501206238,"d":"645.83"}]
["B3.8.4","D-DT 5237","2.4m High Personnel Gate 1m Wide","each",null,null,"Cost plus 5%",{"v":1397.8332012977544,"d":"1,397.83"}]
["B3.8.5","D-DT 5237","2.4m High Double Leaf Gate 5m Wide","each",null,null,"Cost plus 5%",{"v":4244.964474190725,"d":"4,244.96"}]
["B3.8.6","D-DT 5237","2.4m High Steel Palisade Fence","each",null,null,"Cost plus 5%",{"v":1397.8332012977544,"d":"1,397.83"}]
["B3.8.7","D-DT 5237 S7A & S7C ","2.4m High Steel Palisade Fence Hard Rock","m",null,null,"Cost plus 5%",{"v":572.12619579269,"d":"572.13"}]
["B3.8.8","D-DT 5237 S7A & S7C ","2.4m High Steel Palisade Fence Shale","m",null,null,"Cost plus 5%",{"v":572.12619579269,"d":"572.13"}]
["B3.8.9","D-DT 5237 S7A & S7C ","2.4m High Steel Palisade Fence Soft Rock","m",null,null,"Cost plus 5%",{"v":510.3676892526377,"d":"510.37"}]
["B3.8.10","D-DT 5237 S7G & S7H ","2.4m High Electric (4m Wide) Gate ","each",null,null,"Cost plus 5%",{"v":3051.3397108943473,"d":"3,051.34"}]
["B3.8.11","D-DT 5237 S7G & S7I ","2.4m High Electric (5m Wide) Gate ","each",null,null,"Cost plus 5%",{"v":3051.3397108943473,"d":"3,051.34"}]
["B3.8.12","D-DT 5237 S7J ","Electric Fence on Top of Steel Palisade","m",null,null,"Cost plus 5%",{"v":310.6851844280566,"d":"310.69"}]
["B3.8.13","D-DT 5237 S7K & S7L ","Electric Fence Behind Steel Palisade","m",null,null,"Cost plus 5%",{"v":283.73448373701416,"d":"283.73"}]
["B3.9",null,"2.4m Concrete Wall Fence With Double Overhang & Razor Coil Wire"]
["B3.9.1","D-DT 5237 S8A ","2.4m Concrete Wall Fence With Double Overhang & Razor Coil Wire Hard Rock","m",null,null,"Cost plus 5%",{"v":499.0675347026351,"d":"499.07"}]
["B3.9.2","D-DT 5237 S8A ","2.4m Concrete Wall Fence With Double Overhang & Razor Coil Wire Shale","m",null,null,"Cost plus 5%",{"v":405.0138855348305,"d":"405.01"}]
["B3.9.3","D-DT 5237 S8A ","2.4m Concrete Wall Fence With Double Overhang & Razor Coil Wire Soft Rock","m",null,null,"Cost plus 5%",{"v":356.2847774037574,"d":"356.28"}]
["B3.9.4","D-DT 5237 ","2.4m High and 6.5m Wide Gate","each",null,null,"Cost plus 5%",{"v":5572.5091470208,"d":"5,572.51"}]
["B3.9.5","D-DT 5237 ","2.4m High and 1m Wide Gate","each",null,null,"Cost plus 5%",{"v":5259.599999999999,"d":"5,259.60"}]
["B3.9.6","D-DT 5237 ","2.4m High and 5m Wide Gate","each",null,null,"Cost plus 5%",{"v":5259.599999999999,"d":"5,259.60"}]
["B3.10",null,"3m Concrete Wall Fence With Double Overhang & Razor Coil Wire"]
["B3.10.1","D-DT 5237 S8A ","3m Concrete Wall Fence With Double Overhang & Razor Coil Wire Hard Rock","m",null,null,"Cost plus 5%",{"v":463.5281678875961,"d":"463.53"}]
["B3.10.2","D-DT 5237 S8A ","3m Concrete Wall Fence With Double Overhang & Razor Coil Wire Shale","m",null,null,"Cost plus 5%",{"v":441.6672965792211,"d":"441.67"}]
["B3.10.3","D-DT 5237 S8A ","3m Concrete Wall Fence With Double Overhang & Razor Coil Wire Soft Rock","m",null,null,"Cost plus 5%",{"v":399.5347933952285,"d":"399.53"}]
["B3.10.4","D-DT 5237 S8B ","3m High and 6.5m Wide Gate","each",null,null,"Cost plus 5%",{"v":5819.80657490181,"d":"5,819.81"}]
["B3.10.5","D-DT 5237 S8B ","3m High and 1m Wide Gate","each",null,null,"Cost plus 5%",{"v":5819.80657490181,"d":"5,819.81"}]
["B3.10.6","D-DT 5237 S8B ","3m High and 5m Wide Gate","each",null,null,"Cost plus 5%",{"v":5819.80657490181,"d":"5,819.81"}]
["B3.11",null,"Brick wall"]
["B3.11.1",null,"Brick wall 2.4m high as per drawing ","m",null,null,"Cost plus 5%",{"v":573.5918277140108,"d":"573.59"}]
["B3.11.2",null,"Brick wall 3m high as per drawing ","m",null,null,"Cost plus 5%",{"v":573.5918277140108,"d":"573.59"}]
[null,null,"                                                                Total carried to Item of Summary"]
[{"$nulls":8},"Please initial"]
[{"$nulls":8},"Compiler/Designer:"]
[{"$nulls":8},"Quantity Surveyor"]

{"sheet":"Section C Earth Grid","index":4,"n_rows":42,"n_cols":11,"rows_kept":42,"merged":[[0,0,0,10],[1,0,1,1],[1,9,1,10],[2,0,2,1],[2,9,2,10],[3,0,3,1],[3,9,3,10],[4,0,4,1],[5,0,5,10],[6,0,6,10],[7,2,7,10],[8,1,9,1],[8,2,9,2],[8,3,9,3],[8,4,8,5],[8,6,8,7],[8,8,8,9],[8,10,9,10],[39,8,39,9],[40,8,40,9],[41,8,41,9]]}
["GEMMA CLUSTER"]
["Project Name:",{"$nulls":6},"Template Identifier:"]
["Project ID:",{"$nulls":6},"Effective Date:"]
["Job Name:",{"$nulls":6},"Review Date:"]
["Job ID:"]
["SCHEDULE OF QUANTITIES - SECTION C"]
["EARTH GRID"]
["C",null,"EARTH GRID"]
["Item","Refer","Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,"D-DT 5240","Supply the material, transport to site, excavate into all material, backfill, compact and install"]
["C1",null,"EARTH GRID"]
[null,null,"Earth grid Installation as per the earth mat drawings.                                                                                                                                   NB: Annealed, Round 10mm Cu (1kg=1.41m), Flat Cu 3.0x50mm (1kg = 0.723m)"]
["C1.1",null,"10 mm Round Copper earthmat 1m deep","m",null,null,"Cost plus 5%",{"v":25.652973177093532,"d":"25.65"}]
["C1.2",null,"10mm round copper for earth tails connected from reinforcement of trfr plinths, slipways and runway to main earth grid","m",null,null,"Cost plus 5%",25.65]
["C1.3",null,"50 mm x 3 mm flat copper for earth tails connected to the earth grid from equipment foundations, transformer and fence (to the fence and fence corner gate post CGP)","m",null,null,"Cost plus 5%",{"v":95.35436596544835,"d":"95.35"}]
["C1.4",null,"50 mm x 3 mm flat to 50 mm x 3 mm flat, Earth tail to Earth tail for joining foundations  ","m",null,null,"Cost plus 5%",{"v":95.35436596544835,"d":"95.35"}]
["C1.5",null,"80 x 6 mm x 1.2 m long galvanised steel strap bolted to trfr tank and connected to trfr holding down bolts for earthing of transformers.\nNote: This is to be measured on site once the transformers have been installed","each",null,null,"Cost plus 5%",{"v":115,"d":"115.00"}]
["C1.6",null,"50 mm x 3 mm flat copper for earth tails for building earthing of panels. This earthing should run on cable rack.","m",null,null,"Cost plus 5%",{"v":112.77243014847025,"d":"112.77"}]
["C1.7",null,"50 mm x 3 mm flat copper for battery room","m",null,null,"Cost plus 5%",{"v":112.77243014847025,"d":"112.77"}]
["C1.8",null,"10 mm round copper from main earth grid to sacrificial earth anode","m",null,null,"Cost plus 5%",112.77]
["C2","D-DT-5240","SACRIFICIAL EARTH ANODES"]
["C2.1",null,"Sacrificial earth mat anodes","each",null,null,"Cost plus 5%",112.77]
["C3","D-DT-3059s1 & D-DT-5240","EQUI-POTENTIAL EARTH GRIDS"]
["C3.1",null,"Equip-potential earth grids 700x700x50 for Isolator control boxes, Junction boxes, Breaker mechanism boxes, AC/DC Box\nNote: Must be positioned for the operator to stand on.","each",null,null,"Cost plus 5%",{"v":560,"d":"560.00"}]
["C4",null,"JOINTS/BONDING"]
[null,"D-DT-5240","Bond all foundation copper to main earth grid of the substation as per the earthing standard for earth mat and foundation drawings. (Note: Earth tails from one foundation should never be connected on the same side of the eart mat. Earth tails from same foundation should prefferably be joined on opposite sides of the eath mat)"]
["C4.1",null,"Main earth grid brazing: 10 mm round to 10 mm round","each",null,null,"Cost plus 5%",{"v":49.75568112656626,"d":"49.76"}]
["C4.2",null,"Main earth grid brazing to earth tails (foundations and control room) ; 10 mm round to 50 mm x 3 mm flat. Note: Two earth tails per foundation to be installed!!","each",null,null,"Cost plus 5%",{"v":49.75568112656626,"d":"49.76"}]
["C4.3",null,"Main earth grid brazing to earth tails (reinforcing of trfr plinths, slipways and runway); 10 mm round to 10mm round","each",null,null,"Cost plus 5%",{"v":49.75568112656626,"d":"49.76"}]
["C4.4",null,"Earth tail to foundation / plinth copper brazing; 50 mm x 3 mm flat to 50 mm x 3 mm flat.\nNote: Copper quantified in the main BOM is for the earth grid only, and not for the earthing of the hold-down bolts. Copper for the holding down bolts to be priced and allowed for with the foundations.","each",null,null,"Cost plus 5%",{"v":49.75568112656626,"d":"49.76"}]
["C4.5",null,"50 mm x 3 mm flat copper bolted to corner gate posts, intermediate posts and fence","each",null,null,"Cost plus 5%",{"v":112.77243014847025,"d":"112.77"}]
["C4.6",null,"Silbralloy brazing for connecting 10mm round to rail (sacrificial earth)","each",null,null,"Cost plus 5%",{"v":49.75568112656626,"d":"49.76"}]
["C4.7",null,"80 x 6 mm x 1.2 m long galvanised steel strap bolted to trfr tank and connected to trfr holding down bolts for earthing of trfr's. (2 connections per strap)","each",null,null,"Cost plus 5%",{"v":190.7087319308967,"d":"190.71"}]
["C4.8",null,"Equip-potential earth grids connections. 30mm2 stranded copper cable (0.5m each) with luggs for bolted connection","each",null,null,"Cost plus 5%",{"v":1907.087319308967,"d":"1,907.09"}]
["C5",null,"TESTING:",{"$nulls":3},0,0]
["C5.1",null,"The substation Contractor must test the earth-grid resistance on completion of project. Tests to be done by an approved person. The results shall be compared to the design results, as submitted by Eskom Design Eng","each",null,null,{"v":8980.059218551816,"d":"8,980.06"},{"v":2966.580274480615,"d":"2,966.58"}]
["C5.2",null,"Do continuity tests on all equipments on completion of project. Tests to be done by an approved person. The results shall be compared to the design results, as submitted by Eskom Design Eng","each",null,null,{"v":8980.059218551816,"d":"8,980.06"},{"v":2966.580274480615,"d":"2,966.58"}]
[null,null,"Total carried to Item of Summary"]
[{"$nulls":8},"Please initial"]
[{"$nulls":8},"Compiler/Designer:"]
[{"$nulls":8},"Quantity Surveyor"]

{"sheet":"Section D Foundations","index":5,"n_rows":201,"n_cols":11,"rows_kept":201,"merged":[[0,0,0,10],[1,0,1,1],[1,9,1,10],[2,0,2,1],[2,9,2,10],[3,0,3,1],[3,9,3,10],[4,0,4,1],[5,0,5,10],[6,0,6,10],[7,2,7,10],[8,1,9,1],[8,2,9,2],[8,3,9,3],[8,4,8,5],[8,6,8,7],[8,8,8,9],[8,10,9,10],[96,2,96,10],[97,1,98,1],[97,2,98,2],[97,3,98,3],[97,4,97,5],[97,6,97,7],[97,8,97,9],[97,10,98,10],[142,2,142,10],[143,1,144,1],[143,2,144,2],[143,3,144,3],[143,4,143,5],[143,6,143,7],[143,8,143,9],[143,10,144,10],[174,2,174,10],[175,1,176,1],[175,2,176,2],[175,3,176,3],[175,4,175,5],[175,6,175,7],[175,8,175,9],[175,10,176,10],[198,8,198,9],[199,8,199,9],[200,8,200,9]]}
["GEMMA CLUSTER"]
["Project Name:",{"$nulls":6},"Template Identifier:"]
["Project ID:",{"$nulls":6},"Effective Date:"]
["Job Name:",{"$nulls":6},"Review Date:"]
["Job ID:"]
["SCHEDULE OF QUANTITIES - SECTION D"]
["FOUNDATION, TRFR BUND AREA & SLIPWAY, CABLE TRENCHES  AND KERBING & YARD STONE"]
["D1",null,"FOUNDATIONS "]
["Item","Refer","Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,null,"Supply the material, transport to site, excavate into all material, dispose of excavated material, backfill, compact, install and pour complete support foundations with holding down bolts and earth connections as detailed in the drawings. Civil Engineer to clarify the soil type:"]
["D1.1",null,"HV CABLE TERMINATION FOUNDATION"]
["D1.1.1","D-DT 5271 S1","HV Cable Termination End Support Foundation Soft Rock","each",null,null,"Cost plus 5%",{"v":2373.6117332737876,"d":"2,373.61"}]
["D1.1.2","D-DT 5272 S1 ","HV Cable Termination End Support Foundation (Alternative for 44kV Only) Soft Rock","each",null,null,"Cost plus 5%",{"v":2561.020144649325,"d":"2,561.02"}]
["D1.2",null,"MV CABLE END SUPPORT FOUNDATION"]
["D1.2.1","D-DT-5213 s1A ","MV Cable Sealing End Lattice Support Foundation Details (Soil Type 1 & 2) ","each",null,null,"Cost plus 5%",{"v":2090.9090909090905,"d":"2,090.91"}]
["D1.2.2","D-DT-5213 s1B","MV Cable Sealing End - Piled Lattice Support Foundation Details (Soil Type 3) ","each",null,null,"Cost plus 5%",{"v":2090.9090909090905,"d":"2,090.91"}]
["D1.2.3","D-DT-5213 s1C","MV Cable Sealing End - A & B Tubular Support Foundation Details  (Soil Type 1 & 2)","each",null,null,"Cost plus 5%",{"v":2090.9090909090905,"d":"2,090.91"}]
["D.1.3",null,"ISOLATOR SUPPORT FOUNDATION"]
["D.1.3.1","2-ET/14936s2","Isolator 132kV Transverse Isolator Support Shale","each",null,null,"Cost plus 5%"]
["D.1.3.2","D-DT 5202 S1C ","Isolator 132kV - 2.4m Phase CRS Tubular Soft Rock","each",null,null,"Cost plus 5%",{"v":1858.7712620742745,"d":"1,858.77"}]
["D.1.3.3","D-DT 5202 S1D ","Isolator 132kV - 2.4m Phase CRS Lattice Soft Rock","each",null,null,"Cost plus 5%",{"v":1852.9323963983234,"d":"1,852.93"}]
["D.1.3.4","D-DT 5202 S1E ","Isolator 132kV - 2.4m Phase CRS Lattice Soft Rock","each",null,null,"Cost plus 5%",{"v":1844.986199234536,"d":"1,844.99"}]
["D.1.3.5","D-DT 5202 S1A ","Isolator 132kV - 3 & 3,6m Phase CRS Soft Rock","each",null,null,"Cost plus 5%",{"v":1867.2355512931404,"d":"1,867.24"}]
["D.1.3.6","D-DT 5202 S1B","Isolator 132kV - 3 & 3,6m Phase CRS Lattice Soft Rock","each",null,null,"Cost plus 5%",{"v":1854.5215395135392,"d":"1,854.52"}]
["D.1.3.7","2-ET/14936s2","Isolator 132kV Transverse Isolator Support Soft Rock","each",null,null,"Cost plus 5%",{"v":1854.5215395135392,"d":"1,854.52"}]
["D.1.3.8","D-DT 5203 S1A","Isolator 66kV (TYPE 1 & 2)  Soft Rock","each",null,null,"Cost plus 5%",{"v":1802.3799849781421,"d":"1,802.38"}]
["D.1.3.9","D-DT 5203 S1B","Isolator 66kV  (TYPE 3) Soft Rock","each",null,null,"Cost plus 5%",{"v":1640.8449801750942,"d":"1,640.84"}]
["D.1.3.10","D-DT 5204 S1A","Isolator 33kV Lattice Soft Rock","each",null,null,"Cost plus 5%",{"v":1236.5268115301444,"d":"1,236.53"}]
["D.1.3.11","D-DT 5204 S1B","Isolator 33kV Tubular Soft Rock","each",null,null,"Cost plus 5%",{"v":1315.4664531411186,"d":"1,315.47"}]
["D.1.3.12","D-DT 5205 S1A","Isolator 22kV Lattice Soft Rock","each",null,null,"Cost plus 5%",{"v":1402.367389690491,"d":"1,402.37"}]
["D.1.3.13","D-DT 5205 S1B","Isolator 22kV Tubular Soft Rock","each",null,null,"Cost plus 5%",{"v":1377.4350188747135,"d":"1,377.44"}]
["D1.4",null,"BREAKER's FOUNDATION"]
["D1.4.1","D-DT 5200 S1A ","Breakers 132kV Cable Pipe Soft Rock","each",null,null,"Cost plus 5%",{"v":3200.7176226439974,"d":"3,200.72"}]
["D1.4.2","D-DT 5200 S1B ","Breakers 132kV Cable Cutout Soft Rock","each",null,null,"Cost plus 5%",{"v":3194.360664912968,"d":"3,194.36"}]
["D1.4.3","D-DT 5200 S1C ","Breakers 132kV Separate Soft Rock","each",null,null,"Cost plus 5%",{"v":2961.95134975947,"d":"2,961.95"}]
["D1.4.4","D-DT 5200 S1D ","Breakers 132kV Cable Pipe (Type 3) Soft Rock","each",null,null,"Cost plus 5%",{"v":3465.0325086495336,"d":"3,465.03"}]
["D1.4.5","D-DT 5201 S1A ","Breakers 66kV Cable Pipe Soft Rock","each",null,null,"Cost plus 5%",{"v":2072.214593837244,"d":"2,072.21"}]
["D1.4.6","D-DT 5201 S1B ","Breakers 66kV Cable Cutout Soft Rock","each",null,null,"Cost plus 5%",{"v":2069.9889964482863,"d":"2,069.99"}]
["D1.4.7","D-DT 5201 S1C ","Breakers 66kV Separate Soft Rock","each",null,null,"Cost plus 5%",{"v":2079.474475008959,"d":"2,079.47"}]
["D1.4.8","D-DT 5201 S1D ","Breakers 66kV Cable Pipe (TYPE 3) Soft Rock","each",null,null,"Cost plus 5%",{"v":1940.3478302945337,"d":"1,940.35"}]
["D1.4.9","D-DT 5214 S1A ","22kV KIOSK & ME Lattice Soft Rock ","each",null,null,"Cost plus 5%",{"v":1771.5666122375476,"d":"1,771.57"}]
["D1.4.10","D-DT 5214 S1B ","22kV KIOSK & ME Tubular Soft Rock ","each",null,null,"Cost plus 5%",{"v":1829.357137065092,"d":"1,829.36"}]
["D1.4.11","D-DT 5214 S1C ","33kV KIOSK & ME Lattice Soft Rock ","each",null,null,"Cost plus 5%",{"v":2022.2202997615598,"d":"2,022.22"}]
["D1.4.12","D-DT 5216 S1A ","Breakers 11kV KIOSK Soft Rock","each",null,null,"Cost plus 5%",{"v":1771.5122463364135,"d":"1,771.51"}]
["D1.4.13","D-DT 5216 S1B ","Breakers 22kV KIOSK Soft Rock","each",null,null,"Cost plus 5%",{"v":1757.2844331628528,"d":"1,757.28"}]
["D1.5",null,"RECLOSERS FOUNDATION"]
["D1.5.1","D-DT 5222 S1A ","11kV Foundation Soft Rock","each",null,null,"Cost plus 5%",{"v":1573.3470384298976,"d":"1,573.35"}]
["D1.5.2","D-DT 5222 S1B ","22kV Foundation Soft Rock","each",null,null,"Cost plus 5%",{"v":1573.3470384298976,"d":"1,573.35"}]
["D1.5.3","D-DT 5222 S1C ","33kV Foundation Soft Rock","each",null,null,"Cost plus 5%",{"v":1573.3470384298976,"d":"1,573.35"}]
["D1.5.4","D-DT 5222 S1D ","Recloser/VT 11/22kV Foundation Soft Rock","each",null,null,"Cost plus 5%",{"v":1731.635285932542,"d":"1,731.64"}]
["D1.6",null,"NECRT's FOUNDATION"]
["D1.6.1","D-DT 5207 S1A ","NECRT Soft Rock","each",null,null,"Cost plus 5%",{"v":1900.930488025025,"d":"1,900.93"}]
["D1.6.2","D-DT 5207 S1B ","NECRT (TYPE 3) Soft Rock","each",null,null,"Cost plus 5%",{"v":1995.3330761524107,"d":"1,995.33"}]
["D1.6.3","D-DT 5207 S2 ","NECRT Soft Rock","each",null,null,"Cost plus 5%",{"v":2009.0025953993159,"d":"2,009.00"}]
["D1.6.4","D-DT 5207s1b","Aux.TRFR 22kV Lattice Support Foundation Details","each",null,null,"Cost plus 5%",{"v":1900.930488025025,"d":"1,900.93"}]
["D1.7",null,"MEDIUM EQUIPMENT FOUNDATION"]
["D.1.7.1","D-DT 5206 S1A ","Medium Equipment foundation, Lattice (CT, VT, Surge Arrestors and Post Insulators) Soft Rock","each",null,null,"Cost plus 5%",{"v":1740.131477661503,"d":"1,740.13"}]
["D.1.7.2","D-DT 5206 S1B ","Medium Equipment foundation, Lattice (CT, VT, Surge Arrestors and Post Insulators)  - (TYPE 3) Soft Rock","each",null,null,"Cost plus 5%",{"v":1486.3637263032606,"d":"1,486.36"}]
["D.1.7.3","D-DT 5206 S1C ","Medium Equipment foundation, Tubular (CT, VT, Surge Arrestors and Post Insulators) Soft Rock","each",null,null,"Cost plus 5%",{"v":1434.0851654162261,"d":"1,434.09"}]
["D.1.7.4","D-DT 5206 S1D ","Medium Equipment foundation 1.83m CRS, Lattice (CT, VT, Surge Arrestors and Post Insulators)  - (TYPE 3) Soft Rock","each",null,null,"Cost plus 5%",{"v":1473.5263210512035,"d":"1,473.53"}]
["D.1.7.5","D-DT 5206 S1E ","Medium Equipment foundation 2.5m CRS, Lattice (CT, VT, Surge Arrestors and Post Insulators)  - (TYPE 3) Soft Rock","each",null,null,"Cost plus 5%",{"v":1351.8993887467425,"d":"1,351.90"}]
["D.1.7.6","D-DT 5206 S1F ","Medium Equipment foundation 3m CRS, Lattice (CT, VT, Surge Arrestors and Post Insulators)  - (TYPE 3) Soft Rock","each",null,null,"Cost plus 5%",{"v":1288.0267628165675,"d":"1,288.03"}]
["D.1.7.7","D-DT 5210s1","6m Terminal Support Pad Type Foundation","each",null,null,"Cost plus 5%",{"v":1288.0267628165675,"d":"1,288.03"}]
["D1.8",null,"132KV BUSBAR TUBULAR SUPPORT  FOUNDATION"]
["D1.8.1","D-DT 5220 S1A ","Foundation Soft Rock","each",null,null,"Cost plus 5%",{"v":1842.4767901702119,"d":"1,842.48"}]
["D1.9",null,"132KV BUSBAR TUBULAR TWIN SUPPORT  FOUNDATION"]
["D1.9.1","D-DT 5225 S1A ","Foundation Soft Rock","each",null,null,"Cost plus 5%",{"v":3499.751563044031,"d":"3,499.75"}]
["D1.10",null,"66KV BUSBAR TUBULAR SUPPORT  FOUNDATION"]
["D1.10.1","D-DT 5208 S1A ","Foundation Soft Rock","each",null,null,"Cost plus 5%",{"v":2852.3999411936375,"d":"2,852.40"}]
["D1.11",null,"33KV BUSBAR TUBULAR SUPPORT  FOUNDATION"]
["D1.11.1","D-DT 5226 S1C ","Foundation Soft Rock","each",null,null,"Cost plus 5%",{"v":2262.282332530262,"d":"2,262.28"}]
["D1.12",null,"22KV BUSBAR TUBULAR SUPPORT  FOUNDATION"]
["D1.12.1","D-DT 5226 S1B ","Foundation Soft Rock","each",null,null,"Cost plus 5%",{"v":2205.0697129509927,"d":"2,205.07"}]
["D1.13",null,"11KV BUSBAR TUBULAR SUPPORT  FOUNDATION"]
["D1.13.1","D-DT 5226 S1A ","Foundation Soft Rock","each",null,null,"Cost plus 5%",{"v":2169.3118257139495,"d":"2,169.31"}]
["D1.14",null,"ROAD CROSSING TUBULAR FOUNDATION"]
["D.1,14.1","D-DT 5209 S1A ","Foundation 1.2m Phase CRS Soft Rock","each",null,null,"Cost plus 5%",{"v":1907.087319308967,"d":"1,907.09"}]
["D.1,14.2","D-DT 5209 S1B ","Foundation 1.8m Phase CRS Soft Rock","each",null,null,"Cost plus 5%",{"v":1907.087319308967,"d":"1,907.09"}]
["D1.15",null,"OVERHEAD BUSBARS FOUNDATION"]
["D1.15.1","D-DT 5252 S1A ","Columns 132kV Soft Rock","each",null,null,"Cost plus 5%",{"v":4624.686749324244,"d":"4,624.69"}]
["D1.15.2","D-DT 5252 S1B ","Columns 132kV (Rock Pinned) Soft Rock","each",null,null,"Cost plus 5%",{"v":4004.8833705488305,"d":"4,004.88"}]
["D1.15.3","D-DT 5252 S1C ","Columns 132kV (Piled) Soft Rock","each",null,null,"Cost plus 5%",{"v":4624.686749324244,"d":"4,624.69"}]
["D1.15.4","D-DT 5265 S1A ","Columns 88kV Soft Rock","each",null,null,"Cost plus 5%",{"v":4133.116451645642,"d":"4,133.12"}]
["D1.15.5","D-DT 5260 S1A ","Columns 66kV Soft Rock","each",null,null,"Cost plus 5%",{"v":4314.616718278105,"d":"4,314.62"}]
["D1.15.6","D-DT 5257 S1A ","Columns 6.6 - 44kV Soft Rock","each",null,null,"Cost plus 5%",{"v":2775.6924882402946,"d":"2,775.69"}]
["D1.15.7","D-DT 5223 S1A ","Columns 22 (Box Structure) Soft Rock","each",null,null,"Cost plus 5%",{"v":2660.33383578825,"d":"2,660.33"}]
["D1.15.8","D-DT 5270 S1B ","A Frame Structure Soft Rock","each",null,null,"Cost plus 5%",{"v":4268.935502301484,"d":"4,268.94"}]
["D1.16",null,"LIGHTNING & LIGHTING MASTS FOUNDATIONS"]
["D1.16.1","D-DT 5217 S1A ","8 Metre mast (TYPE 1 & 2) ","each",null,null,"Cost plus 5%",{"v":1871.3294320719237,"d":"1,871.33"}]
["D1.16.2","D-DT 5217 S1D ","8 Metre mast (TYPE 3) ","each",null,null,"Cost plus 5%",{"v":2420.2382845151474,"d":"2,420.24"}]
["D1.16.3","D-DT 5217 S1B ","14 Metre mast (TYPE 1 & 2) ","each",null,null,"Cost plus 5%",{"v":2109.7153469855443,"d":"2,109.72"}]
["D1.16.4","D-DT 5217 S1E ","14 Metre mast (TYPE 3) ","each",null,null,"Cost plus 5%",{"v":2109.7153469855443,"d":"2,109.72"}]
["D1.16.5","D-DT 5217 S1C ","21 Metre mast (TYPE 1 & 2) ","each",null,null,"Cost plus 5%",{"v":2355.252839346574,"d":"2,355.25"}]
["D1.16.6","D-DT 5217 S1F ","21 Metre mast (TYPE 3) ","each",null,null,"Cost plus 5%",{"v":2355.252839346574,"d":"2,355.25"}]
[null,null,"                                                                Total carried to Item of Summary"]
["D2",null,"TRANSFORMER BUND AREA & SLIPWAY"]
["Item","Refer","Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,null,"Supply the material, transport to site, excavate into all material, dispose of excavated material, backfill, compact, install and pour complete support foundations with holding down bolts and earth connections as detailed in the drawings. Civil Engineer to clarify the soil type:"]
["D2.1",null,"TRANSFORMER PLINTH                                                                                                                                           "]
["D2.1.1","D-DT 5232 S1A-S1D","Drainage and self- contained Oil contain area with manual water release (Max 5 MVA ) ","each",null,null,"Cost plus 5%",{"v":26172.89144486287,"d":"26,172.89"}]
["D2.1.2","D-DT 5232 S2A-S2D","Drainage and self- contained Oil contain area with manual water release (Max 10-20 MVA ) ","each",null,null,"Cost plus 5%",{"v":23064.482675684678,"d":"23,064.48"}]
["D2.1.3","D-DT 5232 S3A-S3D","Drainage and Oil catchment Area connected to Oil Dam with Self Drainage  (Max 20-40 MVA ) ","each",null,null,"Cost plus 5%",{"v":28252.921388483934,"d":"28,252.92"}]
["D2.1.4","D-DT 5232 S4A-S4D","Drainage and Oil catchment Area connected to Oil Dam with Self Drainage  (Max 40-80 MVA ) ","each",null,null,"Cost plus 5%",{"v":33415.984008931715,"d":"33,415.98"}]
["D2.1.5","D-DT 5232 S5A-S5D","Drainage and Oil catchment Area connected to Oil Dam with Self Drainage  (Max 40-80 MVA ) ","each",null,null,"Cost plus 5%",{"v":41724.97519541269,"d":"41,724.98"}]
["D2.1.6","D-DT 5232 S6A-S6D","Drainage and Oil catchment Area connected to Oil Dam with Self Drainage  (Max 80-160 MVA ) ","each",null,null,"Cost plus 5%",{"v":37408.82864998355,"d":"37,408.83"}]
["D2.1.7","2-ET/14900","4500mm x 3000mm x 250mm thick reinforced concrete for additional slipway / entrance and runway ramps as per design drawing. Reinforcing to be mesh ref. 245 top and bottom","each",null,null,"Cost plus 5%",{"v":38530.8,"d":"38,530.80"}]
["D2.2",null,"OIL CATCHMENT DAM  "]
["D2.2.1","D-DT 5234 ","Oil Dam  ( 32000 liter 20 - 40MVA ) Brick build with concrete cover ","each",null,null,"Cost plus 5%",{"v":17000,"d":"17,000.00"}]
["D2.2.2","D-DT 5234 ","Oil Dam  ( 32000 liter 20 - 40MVA ) Brick build with steel cover ","each",null,null,"Cost plus 5%",{"v":17000,"d":"17,000.00"}]
["D2.2.3","D-DT 5234 ","Oil Dam  ( 32000 liter 20 - 40MVA ) Concrete Build with concrete cover ","each",null,null,"Cost plus 5%",{"v":17000,"d":"17,000.00"}]
["D2.2.4","D-DT 5234 ","Oil Dam  ( 32000 liter 20 - 40MVA ) Concrete Build with steel cover ","each",null,null,"Cost plus 5%",{"v":17000,"d":"17,000.00"}]
["D2.2.5","D-DT 5234 ","Oil Dam  ( 42000 liter 40 - 80MVA ) Brick build with concrete cover ","each",null,null,"Cost plus 5%",{"v":25000,"d":"25,000.00"}]
["D2.2.6","D-DT 5234","Oil Dam  ( 42000 liter 40 - 80MVA ) Brick build with Steel cover ","each",null,null,"Cost plus 5%",{"v":25000,"d":"25,000.00"}]
["D2.2.7","D-DT 5234","Oil Dam  ( 42000 liter 40 - 80MVA ) Brick build with concrete cover ","each",null,null,"Cost plus 5%",{"v":25000,"d":"25,000.00"}]
["D2.2.8","D-DT 5234","Oil Dam  ( 42000 liter 40 - 80MVA ) Concrete build with concrete cover ","each",null,null,"Cost plus 5%",{"v":25000,"d":"25,000.00"}]
["D2.2.9","D-DT 5234 ","Oil Dam  ( 52000 liter 40 - 160MVA ) Brick build with concrete cover ","each",null,null,"Cost plus 5%",{"v":28000,"d":"28,000.00"}]
["D2.2.10","D-DT 5234 ","Oil Dam  ( 52000 liter 40 - 160MVA ) Brick build with Steel cover ","each",null,null,"Cost plus 5%",{"v":28000,"d":"28,000.00"}]
["D2.2.11","D-DT 5234","Oil Dam  ( 52000 liter 40 - 160MVA ) Concrete build with concrete cover ","each",null,null,"Cost plus 5%",{"v":28000,"d":"28,000.00"}]
["D2.2.12","D-DT 5234","Oil Dam  ( 52000 liter 40 - 160MVA ) Concrete build with Stee cover ","each",null,null,"Cost plus 5%",{"v":28000,"d":"28,000.00"}]
["D2.3",null,"OIL DRAINAGE SYSTEM "]
["D2.3.1","D-DT 5234 S1, S2 ","300mm Diameter concrete pipe Hard Rock","m",null,null,"Cost plus 5%",{"v":228.85047831707604,"d":"228.85"}]
["D2.3.2","D-DT 5234 S1, S2 ","300mm Diameter concrete pipe Shale","m",null,null,"Cost plus 5%",{"v":190.7087319308967,"d":"190.71"}]
["D2.3.3","D-DT 5234 S1, S2 ","300mm Diameter concrete pipe Soft Rock","m",null,null,"Cost plus 5%",{"v":190.7087319308967,"d":"190.71"}]
["D2.4",null,"MAN HOLES"]
["D2.4.1","0.54/390 S1 R2","Man Holes Hard Rock","each",null,null,"Cost plus 5%",{"v":2643.5112066460347,"d":"2,643.51"}]
["D2.4.2","0.54/390 S1  R2","Man Holes Shale","each",null,null,"Cost plus 5%",{"v":2615.62911915198,"d":"2,615.63"}]
["D2.4.3","0.54/390 S1  R2","Man Holes Soft Rock","each",null,null,"Cost plus 5%",{"v":2523.494434555859,"d":"2,523.49"}]
["D2.4.4","D-DT 5231","Man Holes Hard Rock","each",null,null,"Cost plus 5%",{"v":2643.5112066460347,"d":"2,643.51"}]
["D2.4.5","D-DT 5231","Man Holes Shale","each",null,null,"Cost plus 5%",{"v":2615.62911915198,"d":"2,615.63"}]
["D2.4.6","D-DT 5231","Man Holes Soft Rock","each",null,null,"Cost plus 5%",{"v":2523.494434555859,"d":"2,523.49"}]
["D2.5",null,"OIL INTERCEPTOR TRAP"]
["D2.5.1","D-DT 5231 ","Oil Interceptor Trap Hard Rock","each",null,null,"Cost plus 5%",{"v":7009.3002574445345,"d":"7,009.30"}]
["D2.5.2","D-DT 5231 ","Oil Interceptor Trap Shale","each",null,null,"Cost plus 5%",{"v":6090.663005855455,"d":"6,090.66"}]
["D2.5.3","D-DT 5231 ","Oil Interceptor Trap Soft Rock","each",null,null,"Cost plus 5%",{"v":5724.326011553257,"d":"5,724.33"}]
["D2.6",null,"GALVANISED STEEL & BRICKWALL FIRE BARRIER "]
["D2.6.1","D-DT 5218 S1A ","Foundation Soil Type 1 and 2 Hard Rock ","each",null,null,"Cost plus 5%",{"v":2671.6211439861713,"d":"2,671.62"}]
["D2.6.2","D-DT 5218 S1A ","Foundation Soil Type 1 and 2 Shale","each",null,null,"Cost plus 5%",{"v":2860.6309789634506,"d":"2,860.63"}]
["D2.6.3","D-DT 5218 S1A ","Foundation Soil Type 1 and 2 Soft Rock","each",null,null,"Cost plus 5%",{"v":2124.460310442672,"d":"2,124.46"}]
["D2.6.4","D-DT 5275 S1 ","Brick fire wall 5m high","m²",null,null,"Cost plus 5%",{"v":1243.4209321894464,"d":"1,243.42"}]
[null,null,"                                                                Total carried to Item of Summary"]
["D3",null,"CABLE TRENCHES "]
["Item","Refer","Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,null,"Supply the material, transport to site, excavate into all material, dispose of excavated material, backfill, compact, install and pour complete support foundations with holding down bolts and earth connections as detailed in the drawings. Civil Engineer to clarify the soil type:"]
["D3.1",null,"CABLE TRENCHES AND COVERS"]
["D3.1.1","D-DT 5254 ","Single (covers)","m",null,null,"Cost plus 5%",{"v":46.05615876131155,"d":"46.06"}]
["D3.1.2","D-DT 5254 ","Double (covers)","m",null,null,"Cost plus 5%",{"v":71.51577447408626,"d":"71.52"}]
["D3.1.3","D-DT 5254 ","Concrete Trench Cover","m",null,null,"Cost plus 5%",{"v":46.05615876131155,"d":"46.06"}]
["D3.1.4","D-DT 5254 ","Complete 0.6m wide cable trenches ","m",null,null,"Cost plus 5%",{"v":74.58830404408404,"d":"74.59"}]
["D3.1.5","D-DT 5254 ","Complete 0.9m wide cable trenches ","m",null,null,"Cost plus 5%",{"v":468,"d":"468.00"}]
["D3.1.6","D-DT 5254 ","Complete 1.2m wide cable trenches ","m",null,null,"Cost plus 5%",{"v":323.60093329807654,"d":"323.60"}]
["D3.1.7","D-DT 5254 ","Complete 1.5m wide cable trenches ","m",null,null,"Cost plus 5%",{"v":323.60093329807654,"d":"323.60"}]
["D3.1.8",null,"Cable trench crossing under the road","m",null,null,"Cost plus 5%",{"v":388.7385601820295,"d":"388.74"}]
["D3.1.9",null,"Screeding 100mm thick including river sand (Note: Refer to Civil Specifications)","m²",null,null,"Cost plus 5%",198.46]
["D3.2",null,"POWER CABLE TRENCH "]
["D3.2.1","D-DT 0854 S1-8 ","±450mm x 800mm Cable Trench Soft Rock","m",null,null,"Cost plus 5%",{"v":64.0919704351809,"d":"64.09"}]
["D3.2.2","D-DT 0854 S1-8 ","±600mm x 800mm Cable Trench Soft Rock","m",null,null,"Cost plus 5%",{"v":64.0919704351809,"d":"64.09"}]
["D3.2.3","D-DT-5254s5J","Concrete Trench Cover","each",null,null,"Cost plus 5%",{"v":46.05615876131155,"d":"46.06"}]
["D3.2.4",null,"Supply & Install 160mm diameter PVC Sleeves","m",null,null,"Cost plus 5%",{"v":146.39955933122368,"d":"146.40"}]
["D3.2.5",null,"Supply and install concrete culvert as per civil drawing","m",null,null,"Cost plus 5%",{"v":833.3971585380185,"d":"833.40"}]
["D3.3",null,"MISCELLENIOUS TRENCHING & CONCRETE"]
["D3.3.1",null,"Chemical bonded bolts","each",null,null,"Cost plus 5%",{"v":308.01692205332046,"d":"308.02"}]
["D3.3.2",null,"50mm wide cable tray","m",null,null,"Cost plus 5%",{"v":151.55146154718534,"d":"151.55"}]
["D3.3.3",null,"Re-instate concrete screed to trenches","m",null,null,"Cost plus 5%",{"v":67.46003544168919,"d":"67.46"}]
["D3.3.4",null,"Breaking & removing of concrete screed to trenches","m",null,null,"Cost plus 5%",{"v":73.20914692872346,"d":"73.21"}]
["D3.3.5",null,"Chemical Bolts (M20x400mm)",4,null,null,"Cost plus 5%",{"v":370.78197086550745,"d":"370.78"}]
["D3.3.6",null,"Chemical Cement ","ml",null,null,"Cost plus 5%",{"v":361.5113842221961,"d":"361.51"}]
["D3.3.7",null,"Setting of Isolators","each",null,null,"Cost plus 5%",{"v":5075.174677919588,"d":"5,075.17"}]
["D3.3.8",null,"Modification to Isolator bases","each",null,null,"Cost plus 5%",{"v":7541.665095286907,"d":"7,541.67"}]
["D3.3.9",null,"600mm wide cable tray","m",null,null,"Cost plus 5%",{"v":151.55146154718534,"d":"151.55"}]
[null,null,"                                                                Total carried to Item of Summary"]
[]
["D4",null,"KERBING & YARD STONE"]
["Item","Refer","Description of the item","Unit","Qty",null,"Rate"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install"]
[null,null,"Supply the material, transport to site, excavate into all material, dispose of excavated material, backfill, compact, install and pour complete support foundations with holding down bolts and earth connections as detailed in the drawings. Civil Engineer to clarify the soil type:"]
["D4.1",null,"CONCRETE KERBING \n"]
["D.4.1.1",null,"Pre-Cast Kerbing","m",null,null,"Cost plus 5%",{"v":81.14656543659655,"d":"81.15"}]
["D.4.1.2",null,"Kerbing Cast on Site","m",null,null,"Cost plus 5%",{"v":81.14656543659655,"d":"81.15"}]
["D4.2",null,"CONCRETE RUNWAY.                                                                                                            "]
[null,null,"250mm thick reinforced concrete runway as detailed on drawing. Reinforce concrete at cable trench crossings. Connect reinforcement to earth grid as per earthing standard.   Reinforcing to be mesh ref. 245 top and bottom. (Note: Transformer slip ways are part of the Transformer plinth and are detailed on those drawings)"]
["D4.2.1",null,"3.5 m wide as per design drawing","m",null,null,"Cost plus 5%",{"v":405.7328271829827,"d":"405.73"}]
["D4.2.2",null,"4.5 m wide as per design drawing","m",null,null,"Cost plus 5%",{"v":1229.7428781381805,"d":"1,229.74"}]
["D4.2.3",null,"6 m wide as per design drawing","m",null,null,"Cost plus 5%",{"v":2040.0242548231429,"d":"2,040.02"}]
["D4.2.4"]
["D4.2.5"]
["D4.3",null,"GATE AND RUNWAY RAMP "]
[null,null,"For substation entrance and offramps inside the substation on the runway"]
["D.4.3.1",null,"4500mm x 1000mm x 250mm thick reinforced concrete entrance. Reinforcing to be mesh ref. 245 top and bottom.","each",null,null,"Cost plus 5%",{"v":1017.2191862602996,"d":"1,017.22"}]
["D.4.3.2",null,"5500mm x 3000mm x 250mm thick reinforced concrete entrance. Reinforcing to be mesh ref. 245 top and bottom.","each",null,null,"Cost plus 5%",{"v":1017.2191862602996,"d":"1,017.22"}]
["D.4.3.3",null,"70000mm x 3000mm x 250mm thick reinforced concrete entrance. Reinforcing to be mesh ref. 245 top and bottom.","each",null,null,"Cost plus 5%",{"v":1017.2191862602996,"d":"1,017.22"}]
["D4.4",null,"YARD STONE"]
["D4.4.1",null,"Yard stone to a 150mm thick layer of 25mm-38mm diameter crusher stones.","M³",null,null,"Cost plus 5%",{"v":210.96506001938394,"d":"210.97"}]
["D4.4.2",null,"Remove and Reinstate Yard Stone 25-35mm Diameter","m²",null,null,"Cost plus 5%",{"v":101.85369306232943,"d":"101.85"}]
["D4.4.3",null,"Apply Weed Killer ","m²",null,null,"Cost plus 5%",{"v":9.21123175226231,"d":"9.21"}]
[null,null,"Total carried to Item of Summary"]
[{"$nulls":8},"Please initial"]
[{"$nulls":8},"Compiler/Designer:"]
[{"$nulls":8},"Quantity Surveyor"]

{"sheet":"Section E Steel Work","index":6,"n_rows":197,"n_cols":11,"rows_kept":197,"merged":[[1,0,1,10],[2,0,2,1],[2,9,2,10],[3,0,3,1],[3,9,3,10],[4,0,4,1],[4,9,4,10],[5,0,5,1],[6,0,6,10],[7,0,7,10],[8,2,8,10],[9,1,10,1],[9,2,10,2],[9,3,10,3],[9,4,9,5],[9,6,9,7],[9,8,9,9],[9,10,10,10],[194,8,194,9],[195,8,195,9],[196,8,196,9]]}
[]
["GEMMA CLUSTER"]
["Project Name:",{"$nulls":6},"Template Identifier:"]
["Project ID:",{"$nulls":6},"Effective Date:"]
["Job Name:",{"$nulls":6},"Review Date:"]
["Job ID:"]
["SCHEDULE OF QUANTITIES - SECTION E"]
["STEELWORK"]
["E","SANS\n1200A","STEELWORK"]
["Item","Refer","Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,null,"Supply the material, transport to site, excavate into all material, backfill, compact and install the steelwork support for the equipment"]
["E1.1",null,"BREAKER SUPPORT"]
["E1.1.1","D-DT 5200 S2A ","132kV Circuit Breaker Support","each",null,null,"Cost plus 5%",{"v":572.12619579269,"d":"572.13"}]
["E1.1.2","D-DT 5201 S2A ","66kV Circuit Breaker Support","each",null,null,"Cost plus 5%",{"v":572.12619579269,"d":"572.13"}]
["E1.1.3","D-DT 5216","33kV Breaker Support","each",null,null,"Cost plus 5%",{"v":605.784167992583,"d":"605.78"}]
["E1.1.4","D-DT 5216","6.6/11/22kV Kiosk Breaker Support","each",null,null,"Cost plus 5%",{"v":528.7936402548064,"d":"528.79"}]
["E1.2",null,"132KV ISOLATOR SUPPORT"]
["E1.2.1","D-DT-5202 s2A r17","Isolator Std - 132KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 3m Phase CRS ","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.2","D-DT-5202 s2A r18","Isolator Std - 132KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 3m Phase CRS ","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.3","D-DT-5202 s2A r19","Isolator Std LH E/S - 132KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 3m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.4","D-DT-5202 s2A r20","Isolator Std RH E/S - 132KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 3m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.5","D-DT-5202 s2A r21","Isolator Std L/RH E/S - 132KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 3m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.6","D-DT-5202 s2A r22","Isolator Std LH E/S - 132KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 3m Phase CRS ","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.7","D-DT-5202 s2A r23","Isolator Std RH E/S - 132KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 3m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.8","D-DT-5202 s2A r24","Isolator Std L/RH E/S - 132KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 3m Phase CRS ","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.9","D-DT-5202 s2A r25","Isolator Inline - 132KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 3.6m Phase CRS ","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.10","D-DT-5202 s2A r26","Isolator Inline - 132KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 3.6m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.11","D-DT-5202 s2A r27","Isolator Std - 132KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 2.4m Phase CRS ","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.12","D-DT-5202 s2A r28","Isolator Std - 132KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 2.4m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.13","D-DT-5202 s2A r29","Isolator Std LH E/S - 132KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 2.4m Phase CRS ","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.14","D-DT-5202 s2A r30","Isolator Std RH E/S - 132KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 2.4m Phase CRS ","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.15","D-DT-5202 s2A r31","Isolator Std L/RH E/S - 132KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 2.4m Phase CRS ","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.16","D-DT-5202 s2A r32","Isolator Std LH E/S - 132KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 2.4m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.17","D-DT-5202 s2A r33","Isolator Std RH E/S - 132KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 2.4m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.18","D-DT-5202 s2A r34","Isolator Std L/RH E/S - 132KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 2.4m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.19","2ET/14891s3","132KV Isolator Support - Manufacturing Details","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.2.20","2ET/14936s2","132KV Transverse Isolator Support Manufacturing Details","each",null,null,"Cost plus 5%",{"v":1107.8376187161307,"d":"1,107.84"}]
["E1.3","D-DT-5203","66KV ISOLATOR SUPPORT:","each"]
["E1.3.1","D-DT-5203 s2A r12","Isolator Std - 66KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 2m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.3.2","D-DT-5203 s2B r0","Isolator Std - 66KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 2m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.3.3","D-DT-5203 s2C r0","Isolator Std LH E/S - 66KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 2m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.3.4","D-DT-5203 s2D r0","Isolator Std RH E/S - 66KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 2m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.3.5","D-DT-5203 s2E r0","Isolator Std LH/RH E/S - 66KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 2m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.3.6","D-DT-5203 s2F r0","Isolator Std LH E/S - 66KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 2m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.3.7","D-DT-5203 s2G r0","Isolator Std RH E/S - 66KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 2m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.3.8","D-DT-5203 s2H r0","Isolator Std L/RH E/S - 66KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 2m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.3.9","D-DT-5203 s2I r0","Isolator Inline - 66KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 2.4m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.3.10","D-DT-5203 s2J r0","Isolator Inline - 66KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 2.4m Phase CRS","each",null,null,"Cost plus 5%",{"v":953.5436596544835,"d":"953.54"}]
["E1.3.11","D-DT-5204 s2A r11","Isolator Std - 33KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 1.2m Phase CRS ","each",null,null,"Cost plus 5%",{"v":928.1985938270974,"d":"928.20"}]
["E1.4","D-DT-5205s2A","6.6/11/22KV ISOLATOR SUPPORT"]
["E1.4.1","D-DT-5205 s2A r9","Isolator Std - 22KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 1m Phase CRS  ","each",null,null,"Cost plus 5%",{"v":1026.7010249779357,"d":"1,026.70"}]
["E1.4.2","2ET/14933s2","22kV Isolator Support Tubular","each",null,null,"Cost plus 5%",{"v":1026.7010249779357,"d":"1,026.70"}]
["E1.4.3",null,"22KV Surge Arrestor Bracket Mounted on Isolator",{"$nulls":3},"Cost plus 5%",{"v":496.37810012701146,"d":"496.38"}]
["E1.4.4","2-WT/918s3 and 2-WT/918s1","Knife Link Isol Support","each",null,null,"Cost plus 5%",{"v":496.37810012701146,"d":"496.38"}]
["E1.5",null,"EARTH SWITCH SUPPORT"]
["E1.5.1","D-DT-5212 s2A r2","Earth Switch - 132KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 3m Phase CRS","each",null,null,"Cost plus 5%",{"v":680,"d":"680.00"}]
["E1.5.2","D-DT-5212 s2B r2","Earth Switch - 132KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 3m Phase CRS","each",null,null,"Cost plus 5%",{"v":680,"d":"680.00"}]
["E1.5.3","D-DT-5211 s2A r0","Earth Switch - 66KV Manual Lattice Support Steelwork Manufacturing Details and Assembly - 1.8m Phase CRS","each",null,null,"Cost plus 5%",{"v":630.622153846154,"d":"630.62"}]
["E1.5.4","D-DT-5211 s2B r0","Earth Switch - 66KV Motor Lattice Support Steelwork Manufacturing Details and Assembly - 1.8m Phase CRS","each",null,null,"Cost plus 5%",{"v":630.622153846154,"d":"630.62"}]
["E1.6",null,"MEDIUM EQUIPMENT SUPPORT"]
["E1.6.1","2ET/14927s2","Medium Equipment Support - Manufacturing details","each",null,null,"Cost plus 5%",{"v":297.9273000083571,"d":"297.93"}]
["E1.6.2","D-DT 5206 S2A ","Medium Equipment - 1.5m Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":371.91136707016096,"d":"371.91"}]
["E1.6.3","D-DT 5206 S2B ","Medium Equipment - 2m Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":371.20274092484703,"d":"371.20"}]
["E1.6.4","D-DT 5206 S2C ","Medium Equipment - 2.5m Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":376.36686094449016,"d":"376.37"}]
["E1.6.5","D-DT 5206 S2D ","Medium Equipment - 3m Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":384.79028400651407,"d":"384.79"}]
["E1.6.6","D-DT 5206 S2E","Medium Equipment - 3.5m Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":406.7360855120722,"d":"406.74"}]
["E1.6.7","D-DT 5206 S2F ","Medium Equipment - 4m Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":384.4846959670152,"d":"384.48"}]
["E1.6.8","D-DT 5206 S2G ","Medium Equipment - 6m Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":405.6679862141262,"d":"405.67"}]
["E1.6.9","D-DT 5206 S2H ","Medium Equipment - Cap M1 Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":152.1999771850459,"d":"152.20"}]
["E1.6.10","D-DT 5206 S2I ","Medium Equipment - Cap M2 Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":147.25068533854497,"d":"147.25"}]
["E1.6.11","D-DT 5206 S2J ","Medium Equipment - Cap M3 Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":154.43263491733515,"d":"154.43"}]
["E1.6.12","D-DT 5215 S2 ","33/22/11KV V.T., C.T. & P.I. Support CAP","each",null,null,"Cost plus 5%",{"v":151.27487502516578,"d":"151.27"}]
["E1.6.13","D-DT 5215 S3 ","33/22/11KV V.T. & C.T. Support CAP","each",null,null,"Cost plus 5%",{"v":151.27487502516578,"d":"151.27"}]
["E1.6.14","D-DT 5207 S2A ","Necrt - Aux Trfr - 1.5m Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":418.05261126571867,"d":"418.05"}]
["E1.6.15","2ET/14927s4","Medium Equipment Support Short Cap","each",null,null,"Cost plus 5%",{"v":151.27487502516578,"d":"151.27"}]
["E1.6.16","2ET/14927s5","MV Medium Equipment Support, Long Cap","each",null,null,"Cost plus 5%",{"v":151.27487502516578,"d":"151.27"}]
["E1.7",null,"OPERATING FOOT PLATES"]
["E1.7.1",null,"Operating Footplates at every Isolator","each",null,null,"Cost plus 5%",{"v":739.4140791688353,"d":"739.41"}]
["E1.7.2",null,"Removed as not necessary","each",null,null,"Cost plus 5%",{"v":2249.098237638985,"d":"2,249.10"}]
["E1.8",null,"INSTALLATION OF PI SUPPORT STEELWORK"]
["E1.8.1","D-DT-5221 s2 r7","6.6-44KV Post Insulator 1.2m Phase Centres, High Level Lipped Channel Support","each",null,null,"Cost plus 5%",{"v":199.99999999999997,"d":"200.00"}]
["E1.9",null,"INSTALLATION OF BRACKET CAP - SURGE ARRESTOR"]
["E1.9.1","D-DT-5219 s1 r3","Surge Arrestor Bracket 11/22KV Mounted on Isolator Support","each",null,null,"Cost plus 5%",532.95]
["E1.9.2","D-DT-5219 s2 r2","Surge Arrestor Bracket 33KV Mounted on Isolator Support","each",null,null,"Cost plus 5%",532.95]
["E1.9.3","D-DT-5219 s3 r4","66KV Surge Arrestor Bracket Mounted on Isolator Support","each",null,null,"Cost plus 5%",532.95]
["E1.9.4","D-DT-5219 s4 r4","132KV Surge Arrestor Bracket Mounted on Isolator","each",null,null,"Cost plus 5%",532.95]
["E1.9.5","2-ET/14891 s4","132KV Surge Arrestor Bracket Mounted on Isolator","each",null,null,"Cost plus 5%",{"v":1042.992714600078,"d":"1,042.99"}]
["E1.10",null,"BUSBAR TUBULAR SUPPORT"]
["E1.10.1","2-ET/14942s2","132KV Busbar Support Tubular 2.5m Spacing","each",null,null,"Cost plus 5%",{"v":982.821082553151,"d":"982.82"}]
["E1.10.2","D-DT 5225 S2A ","Tubular Busbar - 132KV Twin Tubular Support Steelwork Manufacturing Details and Assembly - 3m CRS","each",null,null,"Cost plus 5%",{"v":982.821082553151,"d":"982.82"}]
["E1.10.3","D-DT 5208 S2A ","Tubular Busbar - 66KV Single Tubular Support Steelwork Manufacturing Details and Assembly - 2.5m Phase CRS","each",null,null,"Cost plus 5%",{"v":886.1771623051224,"d":"886.18"}]
["E1.10.4","D-DT-5226 s2C r0","Tubular Busbar - 33KV Single Tubular Support Steelwork Manufacturing Details and Assembly - 1.2m Phase CRS ","each",null,null,"Cost plus 5%",{"v":672.7504797171622,"d":"672.75"}]
["E1.10.5","D-DT-5226 s2B r0","Tubular Busbar - 22KV Single Tubular Support Steelwork Manufacturing Details and Assembly - 1.5m Phase CRS ","each",null,null,"Cost plus 5%",{"v":610.0807008784282,"d":"610.08"}]
["E1.10.6","D-DT-5226 s2A r0","Tubular Busbar - 11KV Single Tubular Support Steelwork Manufacturing Details and Assembly - 1.5m Phase CRS ","each",null,null,"Cost plus 5%",{"v":499.87654586498826,"d":"499.88"}]
["E1.10.7","2-ET/14947s2","Road Crossing Support Manufacturing Details","each",null,null,"Cost plus 5%",{"v":946.2395152215303,"d":"946.24"}]
["E1.10.8","D-DT 5221 s2","Road Crossing Support Manufacturing Details","each",null,null,"Cost plus 5%",{"v":946.2395152215303,"d":"946.24"}]
["E1.10.9","D-DT 5209 S2A ","Tubular Busbar Road Crossing Single Tubular Support Steelwork Manufacturing Details and Assembly - 1.2m Phase CRS","each",null,null,"Cost plus 5%",{"v":855.8142131958132,"d":"855.81"}]
["E1.10.10","D-DT 5209 S2B ","Tubular Busbar Road Crossing Single Tubular Support Steelwork Manufacturing Details and Assembly - 1.85m Phase CRS","each",null,null,"Cost plus 5%",{"v":857.6740774005488,"d":"857.67"}]
["E1.11",null,"132KV BUSBAR COLUMN & BEAM SUPPORT"]
["E1.11.1","D-DT 5252 S2A ","132kV Column - 132/C Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":6696.970916532212,"d":"6,696.97"}]
["E1.11.2","D-DT 5252 S2B ","132kV Beam - 132/50/1 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":5959.039145979005,"d":"5,959.04"}]
["E1.11.3","D-DT 5252 S2C ","132kV Beam - 132/50/2 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":6020.065940196893,"d":"6,020.07"}]
["E1.11.4","D-DT 5252 S2D ","132kV Beam - 132/40/1 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":5877.82419508803,"d":"5,877.82"}]
["E1.11.5","D-DT 5252 S2E ","132kV Earth Wire Support"," each",null,null,"Cost plus 5%",{"v":950.2677074370927,"d":"950.27"}]
["E1.12","D-DT-5225","88KV BUSBAR COLUMN & BEAM SUPPORT"]
["E.1.12.1","D-DT-5265 2A","COLUMN - 88kV - CH8 LATTICE STEEL STEELWORK MANUFACTURING DETAILS AND ASSEMBLEY","each",null,null,"Cost plus 5%",{"v":6658.3570709518035,"d":"6,658.36"}]
["E.1.12.2","D-DT-5265 2B","BEAM - 88kV - B822 LATTICE STEEL STEELWORK MANUFACTURING DETAILS AND ASSEMBLEY","each",null,null,"Cost plus 5%",{"v":4250.696331078205,"d":"4,250.70"}]
["E.1.12.3","D-DT-5265 2C","BEAM - 88kV - B831 LATTICE STEEL STEELWORK MANUFACTURING DETAILS AND ASSEMBLEY","each",null,null,"Cost plus 5%",{"v":4557.675938895548,"d":"4,557.68"}]
["E.1.12.4","D-DT-5265 2D","BEAM - 88kV - B840 LATTICE STEEL STEELWORK MANUFACTURING DETAILS AND ASSEMBLEY","each",null,null,"Cost plus 5%",{"v":4564.773694100834,"d":"4,564.77"}]
["E.1.12.5","D-DT-5265 2E","BEAM - 88kV - B841 LATTICE STEEL STEELWORK MANUFACTURING DETAILS AND ASSEMBLEY","each",null,null,"Cost plus 5%",{"v":4593.591902481504,"d":"4,593.59"}]
["E.1.12.6","D-DT-5265 2F","BEAM - 88kV - B842 LATTICE STEEL STEELWORK MANUFACTURING DETAILS AND ASSEMBLEY","each",null,null,"Cost plus 5%",{"v":4593.591902481504,"d":"4,593.59"}]
["E.1.12.7","D-DT-5265 2G","COLUMN - 88kV - EW8 EARTHWIRE SUPPORT STEELWORK MANUFACTURING DETAILS AND ASSEMBLEY","each",null,null,"Cost plus 5%",{"v":4593.591902481504,"d":"4,593.59"}]
["E.1.12.8","D-DT-5265 2H","COLUMN - 88kV - AC8 ANTI - CLIMBING DEVICE STEELWORK MANUFACTURING DETAILS AND ASSEMBLEY","each",null,null,"Cost plus 5%",{"v":4593.591902481504,"d":"4,593.59"}]
["E1.13",null,"66KV BUSBAR COLUMN & BEAM SUPPORT"]
["E1.13.1","D-DT 5260 S2A ","66kV Column - 66/27/1 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":5982.233084165917,"d":"5,982.23"}]
["E1.13.2","D-DT 5260 S2B1 ","66kV Beam - 66/50/1 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":2285.352117406335,"d":"2,285.35"}]
["E1.13.3","D-DT 5260 S2B2 ","66kV Beam - 66/50/1 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":2342.982851432731,"d":"2,342.98"}]
["E1.13.4","D-DT 5260 S2C ","66kV Beam - 66/32/1 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":2310.4564177089615,"d":"2,310.46"}]
["E1.13.5","D-DT 5260 S2D ","66kV Beam - 66/25/1 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":2296.5594017802937,"d":"2,296.56"}]
["E1.13.6","D-DT 5260 S2E ","66kV Earth Wire Support","each",null,null,"Cost plus 5%",{"v":760.1756004061058,"d":"760.18"}]
["E1.14",null,"6.6/44KV BUSBAR COLUMN & BEAM SUPPORT"]
["E1.14.1","D-DT 5257 S2A ","6.6/44kV Column - C1 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":2247.5974952983443,"d":"2,247.60"}]
["E1.14.2","D-DT 5257 S2B ","6.6/44kV Column - C2 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":2245.9420375558884,"d":"2,245.94"}]
["E1.14.3","D-DT 5257 S2C ","6.6/44kV Column - C3 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":2265.926723422813,"d":"2,265.93"}]
["E1.14.4","D-DT 5257 S2D ","6.6/44kV Column - C4 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":2264.6023572288486,"d":"2,264.60"}]
["E1.14.5","D-DT 5257 S2E ","66/44kV Beam - B1 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":2412.6126578137487,"d":"2,412.61"}]
["E1.14.6","D-DT 5257 S2F ","66/44kV Beam - B2 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":1492.2804647114165,"d":"1,492.28"}]
["E1.14.7","D-DT 5257 S2G ","6.6/44kV Column - B3 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":1977.7867544610936,"d":"1,977.79"}]
["E1.14.8","D-DT 5257 S2H ","6.6/44kV Column - B4 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":1988.2757347172926,"d":"1,988.28"}]
["E1.14.9","D-DT 5257 S2I ","6.6/44kV Column - B5 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":1988.2757347172926,"d":"1,988.28"}]
["E1.14.10","D-DT 5257 S2J ","6.6/44kV Column - B6 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":2135.218498227023,"d":"2,135.22"}]
["E1.14.11","D-DT 5257 S2K ","6.6/44kV Column - B7 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":1975.9254902120958,"d":"1,975.93"}]
["E1.14.12","D-DT 5257 S2L ","6.6/44kV Column - B8 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":2135.218498227023,"d":"2,135.22"}]
["E1.14.13","D-DT 5257 S2M ","6.6/44kV Column - B9 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":2073.524056496973,"d":"2,073.52"}]
["E1.14.14","D-DT 5257 S2N ","6.6/44kV Column - B10 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":2256.6865145382276,"d":"2,256.69"}]
["E1.14.15","D-DT 5257 S2O ","6.6/44kV Column - B11 Lattice Steelwork","each",null,null,"Cost plus 5%",{"v":1986.6434344637146,"d":"1,986.64"}]
["E1.14.16","D-DT 5257 S2P ","6.6/44kV Earth Wire Support - E1","each",null,null,"Cost plus 5%",{"v":719.9521017191507,"d":"719.95"}]
["E1.14.17","D-DT 5257 S2Q ","6.6/44kV Earth Wire Support - E2","each",null,null,"Cost plus 5%",{"v":719.9521017191507,"d":"719.95"}]
["E1.14.18","D-DT 5257 S2R ","6.6/44kV Earth Wire Support - E3","each",null,null,"Cost plus 5%",{"v":668.1397293751716,"d":"668.14"}]
["E1.15",null,"MV CABLE END SUPPORT"]
["E1.15.1","D-DT 5213 S2A ","MV CES - 1 X 3 Core Cable Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":921.1231752262311,"d":"921.12"}]
["E1.15.2","D-DT 5213 S2B ","MV CES - 1 X 3 Core & 1 - 2 Single Core Cables / Phase Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":921.1231752262311,"d":"921.12"}]
["E1.15.3","D-DT 5213 S2C ","MV CES - 1 - 2 Single Core Cables / Phase Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":1063.9852053015761,"d":"1,063.99"}]
["E1.15.4","D-DT 5213 S2D ","MV CES - 2 - 4 Single Core Cables / Phase Lattice Support Steelwork Manufacturing Details and Assembly","each",null,null,"Cost plus 5%",{"v":1063.9852053015761,"d":"1,063.99"}]
["E1.16",null,"HV CABLE TERMINATION SUPPORT"]
[]
["E1.16.1","D-DT 5271 S1 R0","HV Cable Termination End Support Foundation Hard Rock","Each",null,null,"Cost plus 5%",{"v":2774.640411735809,"d":"2,774.64"}]
["E1.16.2","D-DT 5271 S1 R0","HV Cable Termination End Support Foundation Shale","Each",null,null,"Cost plus 5%",{"v":2508.2261404395995,"d":"2,508.23"}]
["E1.16.3","D-DT 5271 S1 R0","HV Cable Termination End Support Foundation Soft Rock","Each",null,null,"Cost plus 5%",{"v":2373.6117332737876,"d":"2,373.61"}]
["E1.16.4","D-DT 5272 S1 R0","HV Cable Termination End Support Foundation (Alternative for 44kV Only) Hard Rock","Each",null,null,"Cost plus 5%",{"v":2839.1762466212244,"d":"2,839.18"}]
["E1.16.5","D-DT 5272 S1 R0","HV Cable Termination End Support Foundation (Alternative for 44kV Only) Shale","Each",null,null,"Cost plus 5%",{"v":2587.0312264452673,"d":"2,587.03"}]
["E1.16.6","D-DT 5272 S1 R0","HV Cable Termination End Support Foundation (Alternative for 44kV Only) Soft Rock",{"$nulls":3},"Cost plus 5%",{"v":2561.020144649325,"d":"2,561.02"}]
["E1.16.7","D-DT 5271 S2 ","HV Cable Termination End Support","each",null,null,"Cost plus 5%",{"v":921.1231752262311,"d":"921.12"}]
["E1.16.8","D-DT 5271 S3 ","HV Cable Termination End Support (CAP Modified to suit PCD - 450)","each",null,null,"Cost plus 5%",{"v":1226.0282958373484,"d":"1,226.03"}]
["E1.16.9","D-DT 5272 S2 ","HV Cable Termination End Support NON SELF-SUPPORTING (Alternative for 44kV Only) ","each",null,null,"Cost plus 5%",{"v":1253.898502521513,"d":"1,253.90"}]
["E1.16.10","D-DT 5272 S3 ","HV Cable Termination End Support NON SELF-SUPPORTING, Surge Arrestor Mounting Plate (Alternative for 44kV Only)","each",null,null,"Cost plus 5%",{"v":1362.1630346441023,"d":"1,362.16"}]
["E1.17",null,"INSTALLATION OF MV BOX STRUCTURE STEELWORK"]
["E.1.17.1","D-DT-5223 s2 r3","MV Box Structure C1 Column Detail (Light) Standard Steelwork","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.2","D-DT-5223 s3 r3","MV Box Structure C2 Column Detail (Heavy) Standard Steelwork","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.3","D-DT-5223 s4 r3","MV Box Structure Beam Details Standard Steelwork 22/33KV Beam MK XB1","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.4","D-DT-5223 s4 r3","MV Box Structure Beam Details Standard Steelwork 22/33KV Beam MK XB2","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.5","D-DT-5223 s4 r3","MV Box Structure Beam Details Standard Steelwork 22/33KV Beam MK XB3","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.6","D-DT-5223 s4 r3","MV Box Structure Beam Details Standard Steelwork 22/33KV Cleat MK CLC","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.7","D-DT-5223 s5 r3","MV Box Structure Beam Details Standard Steelwork 22/33KV Beam MK LC1","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.8","D-DT-5223 s5 r3","MV Box Structure Beam Details Standard Steelwork 22/33KV Beam MK LC2","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.9","D-DT-5223 s5 r3","MV Box Structure Beam Details Standard Steelwork 22/33KV Beam MK Cb1&Cla","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.10","D-DT-5223 s5 r3","MV Box Structure Beam Details Standard Steelwork 22/33KV Cleat Bt/B MK Bpb","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.11","D-DT-5223 s6 r1","MV Box Structure Beam Details Standard Steelwork - Basic 1 X Bull","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.12","D-DT-5223 s6 r1","MV Box Structure Beam Details Standard Steelwork - Basic 2 X Bull","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.13","D-DT-5223 s6 r1","MV Box Structure Beam Details Standard Steelwork - Extension 1 X Bull","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.14","D-DT-5223 s6 r1","MV Box Structure Beam Details Standard Steelwork - Extension 2 X Bull ","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.15","2ET/114957s2","MV Box Busbar C1 Column Light","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.16","2ET/114957s3","MV Box Busbar C2 Column Heavy","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.17","2ET/114957s4","MV Box Busbar Beam Details","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E.1.17.18","2ET/14943s2","MV Cable Support Details","each",null,null,"Cost plus 5%",{"v":655.6778102375263,"d":"655.68"}]
["E1.18",null,"INSTALLATION OF A-FRAME SUPPORT STEELWORK"]
["E1.18.1","D-DT-5270 s5 r3","11/22KV A Frame End/Intermediate Feeder Structure Assembly and Details","each",null,null,"Cost plus 5%",{"v":1200,"d":"1,200.00"}]
["E1.18.2","D-DT-5270 s6 r3","11/22KV A Frame Busbar Section/Support Structure Assembly and Details","each",null,null,"Cost plus 5%",{"v":1200,"d":"1,200.00"}]
["E1.18.3","D-DT-5270 s7 r3","11/22KV A Frame Busbar, End/Intermediate Feeder, Bus Section & Busbar Support Structural Details","each",null,null,"Cost plus 5%",{"v":1200,"d":"1,200.00"}]
["E1.18.4","D-DT-5270 s8 r1","11/22KV A Frame Surge Arrester Adapter Plate Layout and Details","each",null,null,"Cost plus 5%",{"v":1200,"d":"1,200.00"}]
["E1.19",null,"YARD-AC SUPPORT STEELWORK"]
["E1.19","D-DT-5276 s2A r1","Yard AC Distribution Board Steelwork Manufacturing Details And Assembly","each",null,null,"Cost plus 5%",{"v":1984.44725692378,"d":"1,984.45"}]
["E1.20",null,"AUX. TRFR 22KV LATTICE SUPPORT"]
["E.1.20.1","D-DT 5207s2A","Aux. TRFR 22kV Lattice Support - 1.5m","each",null,null,"Cost plus 5%",{"v":2909.090909090909,"d":"2,909.09"}]
["E1.21",null,"FIRE BARRIER SUPPORT"]
["E.1.21.1","D-DT 5218 S2A ","6m Lattice Support","each",null,null,"Cost plus 5%",{"v":2045.351149958867,"d":"2,045.35"}]
["E.1.21.2","D-DT 5218 S2A ","Module A","each",null,null,"Cost plus 5%",{"v":2860.6309789634506,"d":"2,860.63"}]
["E.1.21.3","D-DT 5218 S2A ","Module B","each",null,null,"Cost plus 5%",{"v":2860.6309789634506,"d":"2,860.63"}]
["E1.22",null,"LIGHTING/LIGHTNING MAST"]
["E.1.22.1","D-DT 5217 S2A ","8m Lighting Mast","each",null,null,"Cost plus 5%",{"v":1310.714980401492,"d":"1,310.71"}]
["E.1.22.2","D-DT 5217 S2B ","14m Lighting Mast","each",null,null,"Cost plus 5%",{"v":1463.147763505221,"d":"1,463.15"}]
["E.1.22.3","D-DT 5217 S2C ","21m Lighting Mast","each",null,null,"Cost plus 5%",{"v":1724.359934778723,"d":"1,724.36"}]
[null,null," Total carried to Item of Summary"]
[{"$nulls":8},"Please initial"]
[{"$nulls":8},"Compiler/Designer:"]
[{"$nulls":8},"Quantity Surveyor"]

{"sheet":"Section F Equipment & Lighting","index":7,"n_rows":152,"n_cols":11,"rows_kept":152,"merged":[[1,0,1,10],[2,0,2,1],[2,9,2,10],[3,0,3,1],[3,9,3,10],[4,0,4,1],[4,9,4,10],[5,0,5,1],[6,0,6,10],[7,0,7,10],[8,2,8,10],[9,1,10,1],[9,2,10,2],[9,3,10,3],[9,4,9,5],[9,6,9,7],[9,8,9,9],[9,10,10,10],[28,3,29,3],[28,4,28,5],[28,6,28,7],[28,8,28,9],[28,10,29,10],[59,3,60,3],[59,4,59,5],[59,6,59,7],[59,8,59,9],[59,10,60,10],[122,1,123,1],[135,0,136,0],[135,1,136,1],[135,2,136,10],[137,1,138,1],[137,2,138,2],[137,3,138,3],[137,4,137,5],[137,6,137,7],[137,8,137,9],[137,10,138,10],[149,8,149,9],[150,8,150,9],[151,8,151,9]]}
[]
["GEMMA CLUSTER"]
["Project Name:",{"$nulls":6},"Template Identifier:"]
["Project ID:",{"$nulls":6},"Effective Date:"]
["Job Name:",{"$nulls":6},"Review Date:"]
["Job ID:"]
["SCHEDULE OF QUANTITIES - SECTION F"]
["SUBSTATION EQUIPMENT AND LIGHTING"]
["F1",null,"SUBSTATION EQUIPMENT"]
["Item","Refer","Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,null,"Transport to site from Eskom stores and Install the following equipment supplied by Eskom:"]
["F1.1",null,"BREAKER:"]
[null,null,"Note: All Circuit Breakers and Isolators are to be erected and commissioned by the Original Equipment Supplier. Only accredited equipment installers as defined by the OEM will be allowed to erect and commission the above. On completion of the installation the equipment test results are to be handed over to the Eskom project engineer."]
["F.1.1.1","D-DT- 6250","132kV Breaker ","each",{"$nulls":3},{"v":3483.7823554772067,"d":"3,483.78"}]
["F.1.1.2","D-DT- 6251","66kV breaker","each",{"$nulls":3},{"v":3070.4105840874367,"d":"3,070.41"}]
["F.1.1.3","D-DT-6266","6.6/11/22/33 kV Kiosk","each",{"$nulls":3},{"v":2114.2630253258603,"d":"2,114.26"}]
["F.1.1.4","D-DT-6252","11/22/33kV Combo Breaker","each",{"$nulls":3},{"v":1922.9286225318147,"d":"1,922.93"}]
["F.1.1.5","D-DT- 6269","Installation of Indoor Switch Gear","each",{"$nulls":3},{"v":1035.6056270043482,"d":"1,035.61"}]
["F.1.1.6",null,"Switchgear Base frames ","each",{"$nulls":3},{"v":1611.488784816077,"d":"1,611.49"}]
["F1.2",null,"SURGE ARRESTOR"]
["F1.2.1","D-DT-6210","132kV","each",{"$nulls":3},{"v":572.12619579269,"d":"572.13"}]
["F1.2.2","D-DT-6211","88kV","each",{"$nulls":3},{"v":546.1281222158092,"d":"546.13"}]
["F1.2.3","D-DT-6212","66kV","each",{"$nulls":3},{"v":460.7650102605085,"d":"460.77"}]
["F1.2.4","D-DT-6214","33/44kV","each",{"$nulls":3},{"v":286.063097896345,"d":"286.06"}]
["F1.2.5","D-DT-6215","22kV ","each",{"$nulls":3},{"v":286.063097896345,"d":"286.06"}]
["F1.2.6","D-DT-6216","11kV","each",{"$nulls":3},{"v":277.4890754785502,"d":"277.49"}]
["F1.2.7","D-DT-6217","6.6kV","each",{"$nulls":3},{"v":271.9349106952676,"d":"271.93"}]
["F1.3",null,"ISOLATOR","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
[null,null,"Note: All Circuit Breakers and Isolators are to be erected and commissioned by the Original Equipment Supplier. Only accredited equipment installers as defined by the OEM will be allowed to erect and commission the above. On completion of the installation the equipment test results are to be handed over to the Eskom project engineer.",null,"Supply","Install","Supply","Install","Supply","Install"]
["F1.3.1","D-DT- 6302","132kV Isolator","each",{"$nulls":3},{"v":2495.053715460493,"d":"2,495.05"}]
["F1.3.2","D-DT- 6152","66kV Isolator","each",{"$nulls":3},{"v":2203.6405127172534,"d":"2,203.64"}]
["F1.3.3","D-DT- 6208","33kV Isolator","each",{"$nulls":3},{"v":1884.3561767696947,"d":"1,884.36"}]
["F1.3.4","D-DT- 6305","6.6/11/22kV Isolator","each",{"$nulls":3},{"v":1615.8168693007406,"d":"1,615.82"}]
["F1.4",null,"CURRENT TRANSFORMER"]
["F1.4.1","D-DT 6190","132kV Current transformer","each",{"$nulls":3},{"v":603.5111318065577,"d":"603.51"}]
["F1.4.2","D-DT 6198","66kV Current Transformer","each",{"$nulls":3},{"v":538.4769114350295,"d":"538.48"}]
["F1.4.3","D-DT 6191","33kV Current Transformer","each",{"$nulls":3},{"v":305.0362328643201,"d":"305.04"}]
["F1.4.4","D-DT6192","6.6/11/22kV Current Transformer","each",{"$nulls":3},{"v":226.856512575443,"d":"226.86"}]
["F1.5",null,"VOLTAGE TRANSFORMER / POWER VT"]
["F1.5.1","D-DT 6170 / 6315","132kV VT","each",{"$nulls":3},{"v":597.1059789182115,"d":"597.11"}]
["F1.5.2","D-DT 6171 / 6315","88kV VT","each",{"$nulls":3},{"v":570.3782678595358,"d":"570.38"}]
["F1.5.3","D-DT 6176 / 6315","66kV VT","each",{"$nulls":3},{"v":514.907007357099,"d":"514.91"}]
["F1.5.4","D-DT 4777 ","44kV VT","each",{"$nulls":3},{"v":413.08740348060223,"d":"413.09"}]
["F1.5.5","D-DT 6172","33kV VT","each",{"$nulls":3},{"v":315.3545464636572,"d":"315.35"}]
["F1.5.6","D-DT 6173","22kV VT","each",{"$nulls":3},{"v":268.4724540830696,"d":"268.47"}]
["F1.5.7","D-DT 6174","11kV VT","each",{"$nulls":3},{"v":266.5182781879752,"d":"266.52"}]
["F1.5.8","D-DT 6178","6.6kV VT","each",{"$nulls":3},{"v":261.87981803023376,"d":"261.88"}]
["F1.6",null,"NECRT"]
["F1.6.1","D-DT- 6145","44kV","each",{"$nulls":3},{"v":801.840223191346,"d":"801.84"}]
["F1.6.2","D-DT 6142","33kV","each",{"$nulls":3},{"v":776.1031698997924,"d":"776.10"}]
["F1.6.3","D-DT 6141","22kV","each",{"$nulls":3},{"v":658.0005013267172,"d":"658.00"}]
["F1.6.4","D-DT 6140","11kV","each",{"$nulls":3},{"v":602.5176334903493,"d":"602.52"}]
["F1.6.5","D-DT 6143","6.6kV","each",{"$nulls":3},{"v":586.8506050864836,"d":"586.85"}]
["F1.7",null,"POST INSULATORS"]
["F1.7.1","D-DT 6230","132kV","each",{"$nulls":3},{"v":388.1783238516226,"d":"388.18"}]
["F1.7.2","D-DT 6232","44/66kV","each",{"$nulls":3},{"v":228.85047831707604,"d":"228.85"}]
["F1.7.3","D-DT 6234","33kV","each",{"$nulls":3},{"v":228.85047831707604,"d":"228.85"}]
["F1.7.4","D-DT 6235","6.6/11/22kV","each",{"$nulls":3},{"v":209.01677019626277,"d":"209.02"}]
["F1.8",null,"TRANSFORMERS","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
[null,null,"Note: All Power Transformers are to be installed and commissioned by the Original Equipment Supplier. Only accredited equipment installers as defined by the OEM will be allowed to erect and commission the above. On completion of the installation the equipment test results are to be handed over to the Eskom project engineer.",null,"Supply","Install","Supply","Install","Supply","Install"]
["F1.8.1","D-DT-4600","Transformer 132/11KV 10MVA OLTC Cent To Bull","each"]
["F1.8.2","D-DT-4601","Transformer 132/11KV 20MVA OLTC Cent To Bull","each"]
["F1.8.3","D-DT-4678","Transformer 132/11KV 40MVA OLTC Cent To Twin Bull","each"]
["F1.8.4","D-DT-4602","Transformer 132/22KV 10MVA OLTC Cent To Bull","each"]
["F1.8.5","D-DT-4603","Transformer 132/22KV 20MVA OLTC Cent To Bull","each"]
["F1.8.6","D-DT-4604","Transformer 132/22KV 40MVA OLTC Cent To Bull","each"]
["F1.8.7","D-DT-4679","Transformer 132/33KV 10MVA OLTC Cent To Bull","each"]
["F1.8.8","D-DT-4680","Transformer 132/33KV 20MVA OLTC Cent To Bull","each"]
["F1.8.9","D-DT-4681","Transformer 132/33KV 40MVA OLTC Cent To Bull","each"]
["F1.8.10","D-DT-4605","Transformer 132/33KV 80MVA OLTC Cent To Twin Bull","each"]
["F1.8.11","D-DT-4690","Transformer 132/44/22KV 20MVA OLTC Cent To Bull","each"]
["F1.8.12","D-DT-4691","Transformer 132/44/22KV 40MVA OLTC Cent To Bull","each"]
["F1.8.13","D-DT-4692","Transformer 132/44/22KV 80MVA OLTC Cent To Bull","each"]
["F1.8.14","D-DT-4676","Transformer 132/6.6KV 10MVA OLTC Cent To Bull","each"]
["F1.8.15","D-DT-4677","Transformer 132/6.6KV 20MVA OLTC Cent To Twin Bull","each"]
["F1.8.16","D-DT-4693 ","Transformer 132/66/22KV 20MVA OLTC Cent To Bull","each"]
["F1.8.17","D-DT-4694","Transformer 132/66/22KV 40MVA OLTC Cent To Bull","each"]
["F1.8.18","D-DT-4695","Transformer 132/66/22KV 80/10MVA OLTC Bull To Bull","each"]
["F1.8.19","D-DT-4696","Transformer 132/88/22KV 40MVA OLTC Cent To Bull","each"]
["F1.8.20","D-DT-4697","Transformer 132/88/22KV 80/10MVA OLTC Cent To Bull","each"]
["F1.8.21","D-DT-4699","Transformer 66/6.6KV 10MVA OLTC Cent To Bull","each"]
["F1.8.22","D-DT-4698","Transformer 66/6.6KV 5MVA OLTC Cent To Bull","each"]
["F1.8.23","D-DT-4606","Transformer 88/11KV 10MVA OLTC Cent To Bull","each"]
["F1.8.24","D-DT-4607","Transformer 88/11KV 20MVA OLTC Cent To Bull","each"]
["F1.8.25","D-DT-4686","Transformer 88/11KV 40MVA OLTC Cent To Twin Bull","each"]
["F1.8.26","D-DT-4685","Transformer 88/11KV 5MVA OLTC Cent To Bull","each"]
["F1.8.27","D-DT-4608","Transformer 88/22KV 10MVA OLTC Cent To Bull","each"]
["F1.8.28","D-DT-4609","Transformer 88/22KV 20MVA OLTC Cent To Bull","each"]
["F1.8.29","D-DT-4610","Transformer 88/22KV 40MVA OLTC Cent To Bull","each"]
["F1.8.30","D-DT-4687","Transformer 88/22KV 5MVA OLTC Cent To Bull","each"]
["F1.8.31","D-DT-4675","Transformer 88/33KV 10MVA OLTC Cent To Bull","each"]
["F1.8.32","D-DT-4688","Transformer 88/33KV 20MVA OLTC Cent To Bull","each"]
["F1.8.33","D-DT-4689","Transformer 88/33KV 40MVA OLTC Cent To Bull","each"]
["F1.8.34","D-DT-4611","Transformer 88/33KV 80MVA OLTC Cent To Twin Bull","each"]
["F1.8.35","D-DT-4683","Transformer 88/6.6KV 10MVA Otlc Cent To Bull","each"]
["F1.8.36","D-DT-4684","Transformer 88/6.6KV 20MVA OLTC Cent To Twin Bull","each"]
["F1.8.37","D-DT-4682","Transformer 88/6.6KV 5MVA OLTC Cent To Bull","each"]
["F1.8.38","D-DT-4700","TRANSFORMER 66/6.6kV 20MVA OLTC CENT TO TWIN BULL","each"]
["F1.8.39","D-DT-4701","TRANSFORMER 66/11kV 5MVA OLTC CENT TO BULL","each"]
["F1.8.40","D-DT-4702","TRANSFORMER 66/11kV 10MVA OLTC CENT TO BULL","each"]
["F1.8.41","D-DT-4703","TRANSFORMER 66/11kV 20MVA OLTC CENT TO BULL","each"]
["F1.8.42","D-DT-4704","TRANSFORMER 66/11kV 40MVA OLTC CENT TO TWIN BULL","each"]
["F1.8.43","D-DT-4705","TRANSFORMER 66/22kV 5MVA OLTC CENT TO BULL","each"]
["F1.8.44","D-DT-4706","TRANSFORMER 66/22kV 10MVA OLTC CENT TO BULL","each"]
["F1.8.45","D-DT-4707","TRANSFORMER 66/22kV 20MVA OLTC CENT TO BULL","each"]
["F1.8.46","D-DT-4708","TRANSFORMER 66/22kV 40MVA OLTC CENT TO BULL","each"]
["F1.8.47","D-DT-4709","TRANSFORMER 44/6.6kV 5MVA OLTC CENT TO BULL","each"]
["F1.8.48","D-DT-4710","TRANSFORMER 44/6.6kV 10MVA OLTC CENT TO BULL","each"]
["F1.8.49","D-DT-4711","TRANSFORMER 44/6.6kV 20MVA OLTC CENT TO TWIN BULL","each"]
["F1.8.50","D-DT-4712","TRANSFORMER 44/11kV 5MVA OLTC CENT TO BULL","each"]
["F1.8.51","D-DT-4713","TRANSFORMER 44/11kV 10MVA OLTC CENT TO BULL","each"]
["F1.8.52","D-DT-4714","TRANSFORMER 44/11kV 20MVA OLTC CENT TO BULL","each"]
["F1.8.53","D-DT-4715","TRANSFORMER 44/22kV 5MVA OLTC CENT TO BULL","each"]
["F1.8.54","D-DT-4716","TRANSFORMER 44/22kV 10MVA OLTC CENT TO BULL","each"]
["F1.8.55","D-DT-4717","TRANSFORMER 44/22kV 20MVA OLTC CENT TO BULL","each"]
["F1.8.56","D-DT-4718","TRANSFORMER 33/11kV 2.5MVA OCTS CENT TO BULL","each"]
["F1.8.57","D-DT-4719","TRANSFORMER 33/11kV 5MVA OCTS CENT TO BULL","each"]
["F1.8.58","D-DT-4720","TRANSFORMER 33/11kV 10MVA OCTS CENT TO BULL","each"]
["F1.8.59","D-DT-4721","TRANSFORMER 33/11kV 20MVA OCTS CENT TO BULL","each"]
["F1.8.60","D-DT-4722",null,"each"]
["F1.8.61","D-DT-4723","TRANSFORMER 33/22kV 5MVA OCTS CENT TO BULL","each"]
["F1.8.62","D-DT-4724","TRANSFORMER 22/11kV 2.5MVA OCTS CENT TO BULL","each"]
["F1.8.63",null,"TRANSFORMER 22/11kV 2.5MVA OCTS CENT TO BULL","each"]
["F1.8.64","D-DT-4725","TRANSFORMER 22/11kV 5MVA OCTS CENT TO BULL","each"]
["F1.8.65","D-DT-4726","TRANSFORMER 22/11kV 10MVA OCTS CENT TO BULL","each"]
["F1.8.66","D-DT-4727","TRANSFORMER 22/11kV 20MVA OCTS CENT TO BULL","each"]
["F1.8.67","D-DT 3192","33KV I/L 3PH 200KVA","each",{"$nulls":3},{"v":820,"d":"820.00"}]
["F1.8.68","D-DT 3021","11KV I/L 3PH 100KVA","each",{"$nulls":3},{"v":820,"d":"820.00"}]
["F1.8.69","D-DT 3021","11KV I/L 3PH 200KVA","each",{"$nulls":3},{"v":820,"d":"820.00"}]
["F1.8.70","D-DT 3021","22KV I/L 3PH 100KVA","each",{"$nulls":3},{"v":820,"d":"820.00"}]
["F1.8.71","D-DT 3021","22KV I/L 3PH 200KVA","each",{"$nulls":3},{"v":820,"d":"820.00"}]
["F1.8.72","D-DT 3192","33KV 3PH 100KVA 3.5M","each",{"$nulls":3},{"v":820,"d":"820.00"}]
[null,null,"                                                                Total carried to Item of Summary"]
[]
["F2",null,"SUBSTATION LIGHTING"]
[]
["Item",null,"Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,null,"Supply the material, transport to site, excavate into all material, backfill, compact and install"]
["F2.1",null,"FLOOD LIGHTS"]
["F2.1.1","D-DT-6105","Lamp, Flood light - 400W/230V HPS","each",null,null,"Cost plus 5%",{"v":1684.785920112125,"d":"1,684.79"}]
["F2.1.2","D-DT-6104","Holder Floodlight Lamp - 400/250W                                                            \nNote: All masts to be supplied complete with wiring and circuit breaker etc.","each",null,null,"Cost plus 5%",312.55]
["F2.1.3","D-DT-3128","Cable to power the flood lights. (Cable 4core 4mm² 1kV Cu BVX4ECV)\nNote:\nLights 1, 2, 3 looped together \nLights 4, 5, 6 looped together \nLights 7, 8 & 9 looped together etc,,","each",null,null,"Cost plus 5%",{"v":28.606309789634505,"d":"28.61"}]
["F2.1.4","D-DT-3070","Glands for flood light cables.\n(Cable Gland Adjust No. 1)","each",null,null,"Cost plus 5%",137.76]
["F2.1.5",null,"Photo cell - Day night switch to be installed for all yard lights","each",null,null,"Cost plus 5%",137.76]
["F2.2",null,"CONDUIT FOR LIGHTING MAST CABLES:"]
["F2.2.1","D-DT-5217 s6","50mm Ø PVC Pipes for running cables for lighting masts (used in foundations, 3m per foundation)","m",null,null,"Cost plus 5%",{"v":20.9,"d":"20.90"}]
[null," ","                                                                Total carried to Item of Summary"]
[{"$nulls":8},"Please initial"]
[{"$nulls":8},"Compiler/Designer:"]
[{"$nulls":8},"Quantity Surveyor"]

{"sheet":"Section G Miscellanous & Clamps","index":8,"n_rows":256,"n_cols":11,"rows_kept":256,"merged":[[1,0,1,10],[2,0,2,1],[2,9,2,10],[3,0,3,1],[3,9,3,10],[4,0,4,1],[4,9,4,10],[5,0,5,1],[6,0,6,10],[7,0,7,10],[8,2,8,10],[9,1,10,1],[9,2,10,2],[9,3,10,3],[9,4,9,5],[9,6,9,7],[9,8,9,9],[9,10,10,10],[32,2,32,10],[33,1,34,1],[33,2,34,2],[33,3,34,3],[33,4,33,5],[33,6,33,7],[33,8,33,9],[33,10,34,10],[253,8,253,9],[254,8,254,9],[255,8,255,9]]}
[]
["GEMMA CLUSTER"]
["Project Name:",{"$nulls":6},"Template Identifier:"]
["Project ID:",{"$nulls":6},"Effective Date:"]
["Job Name:",{"$nulls":6},"Review Date:"]
["Job ID:"]
["SCHEDULE OF QUANTITIES - SECTION G"]
["MISCELLANEOUS AND CLAMPS"]
["G1",null,"MISCELLANEOUS ITEMS"]
["Item","Refer","Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,null,"Supply the material, transport to site, excavate into all material, backfill, compact, complete the required finishing and install"]
["G1.1",null,"MISCELLANEOUS"]
["G.1.1.1","D-DT 6292","Tape Elect EPR 18mm W x 0.76mm Thk","each",null,null,"cost plus 5%",{"v":89.84625000000001,"d":"89.85"}]
["G.1.1.2","D-DT 6292","Putty Scotchfill 38mm W Roll","each",null,null,"cost plus 5%",{"v":89.84625000000001,"d":"89.85"}]
["G.1.1.3","D-DT 6065","Bracket Control Cable ","each",null,null,"cost plus 5%",{"v":89.84625000000001,"d":"89.85"}]
["G.1.1.4","D-DT 6081","Ball Joint Portable Earth","each",null,null,"cost plus 5%",{"v":89.84625000000001,"d":"89.85"}]
["G.1.1.5","D-DT 6097","Bolt HX Galv M16x45mm W/HxNUT","each",null,null,"cost plus 5%",{"v":52.79625,"d":"52.80"}]
["G.1.1.6","D-DT 3014","Washer, RD Flat M16 29.6D 18.25DIA HL","each",null,null,"cost plus 5%",{"v":39.82875,"d":"39.83"}]
["G.1.1.7","D-DT 3014","Washer, Taper Galv M16 38SQ 18.25DIA HL","each",null,null,"cost plus 5%",{"v":39.82875,"d":"39.83"}]
["G.1.1.8","D-DT-6055","Cover Acrylic 480x160mm ACC4","each",null,null,"cost plus 5%",2.99]
["G.1.1.9","D-DT-3082s2","Set Screw, Hx Galv M16x65 Nut+Wash","each",null,null,"cost plus 5%",18.61]
["G.1.1.10","D-DT-3031s2","Strap, Tie St Galv 910x50x6","each",null,null,"cost plus 5%",{"v":97.25625,"d":"97.26"}]
["G.1.1.11",null,"Barbed Wire ","m",null,null,"cost plus 5%",{"v":161.1660796613505,"d":"161.17"}]
["G.1.1.12",null,"Handrails","m",null,null,"cost plus 5%",{"v":388.80667044343335,"d":"388.81"}]
["G.1.1.13",null,"Split Sleeves","m",null,null,"cost plus 5%",{"v":158.6424208619445,"d":"158.64"}]
["G.1.1.14",null,"10mm Copper Clad Rods","each",null,null,"cost plus 5%",{"v":213.24414708739766,"d":"213.24"}]
["G.1.1.15",null,"Cable Support Cap for LV Termination","each",null,null,"cost plus 5%",{"v":2238.3262550423156,"d":"2,238.33"}]
["G.1.1.16",null,"Operating Locks (North West O/U)","each",null,null,"cost plus 5%",{"v":18.589627948562814,"d":"18.59"}]
["G.1.1.17",null,"Prohibited Locks (North West O/U)","each",null,null,"cost plus 5%",{"v":18.589627948562814,"d":"18.59"}]
[null,null,"                                                                Total carried to Item of Summary"]
[]
["G2",null,"CLAMPS "]
["Item","Refer","Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,null,"Supply the material, transport to site and install the clamps and connectors as per the design and the clamp schedule documents"]
["G2.1",null,"CLAMPS"]
["G.2.1.1","D-DT-6037","Clamp, BUS STUD INLINE TBSI-120/26/C D6037","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.2","D-DT-6037","Clamp, BUS STUD INLINE TBSI-120/38/C D6037","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.3","D-DT-6037","Clamp, BUS STUD INLINE TBSI-80/26/C D6037","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.4","D-DT-6037","Clamp, BUS STUD INLINE TBSI-80/38/C D6037","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.5","D-DT-6118","Clamp, TUBE TBSFS 120/127 D6118","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.6","D-DT-6118","Clamp, TUBE TBSFS 120/76 D6118","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.7","D-DT-6118","Clamp, TUBE TBSS 120/127 D6118","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.8","D-DT-6118","Clamp, TUBE TBSS 120/76 D6118","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.9","D-DT-6068","Clamp, CLAMPEX 13mm DIA GALV STEEL D6068","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.10","D-DT-6068","Clamp, CLAMPEX 19mm DIA GALV STEEL D6068","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.11","D-DT-6068","Clamp, CLAMPEX 25mm DIA GALV STEEL D6068","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.12","D-DT-6068","Clamp, CLAMPEX 32mm DIA GALV STEEL D6068","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.13","D-DT-6068","Clamp, CLAMPEX 40mm DIA GALV STEEL D6068","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.14","D-DT-6039","Clamp, F/BUS SUPP TYPE TBFS120-127 D6039","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.15","D-DT-6040","Clamp, F/BUS SUPP TYPE TBFS120-76 D6039","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.16","D-DT-6040","Clamp, F/BUS SUPP TYPE TBFS80-127 D6039","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.17","D-DT-6040","Clamp, F/BUS SUPP TYPE TBFS80-76 D6039","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.18","D-DT-6025","Clamp, F/SUPT 26.5mm P26/76/150 C/C D6025","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.19","D-DT-6025","Clamp, F/SUPT 38.3mm P38/127/150 C/C D6025","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.20","D-DT-6025","Clamp, F/SUPT 38.3mm P38/76/150 C/C D6025","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.21","D-DT-6029","Clamp, FIX/SUPP 26.5mm KCP 26/127 D6029","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.22","D-DT-6029","Clamp, FIX/SUPP 26.5mm KCP 26/76 D6029","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.23","D-DT-6029","Clamp, FIX/SUPP 38.3mm KCP 38/127 D6029","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.24","D-DT-6029","Clamp, FIX/SUPP 38.3mm KCP 38/76 D6029","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.25","D-DT-6115","Clamp, PEG AL BULL 38.3mm EPC-38 D6115","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.26","D-DT-6115","Clamp, PEG AL CENT 26.5mm EPC-26 D6115","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.27","D-DT-6115","Clamp, PEG AL HORN 16.3mm EPC-14-40 D6115","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.28","D-DT-6042","Clamp, PISTOL 4B 20mm-30mm D6042","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.29","D-DT-6042","Clamp, PISTOL 4B 30mm-40mm D6042","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.30","D-DT-6027","Clamp, STUD PALM BOLT 26.5mm EXP-A  D6027","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.31","D-DT-6010","Clamp, T/COMP 38.3mm-38.3mm 0DG ETC-K D6010","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.32","D-DT-6080","Clamp, TUBULAR EARTHING PEG TBEP120 D6080","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.33","D-DT-6080","Clamp, TUBULAR EARTHING PEG TBEP80 D6080","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.34","D-DT-6054","Clamp, BI-MET R6-11mm - T26.5mm 0DG D6054","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.35","D-DT-6317","Clamp, HOR/VER STUDMTEXPTBHXS120/26 D6317","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.36","D-DT-6317","Clamp, HOR/VER STUDMTEXPTBHXS120/38 D6317","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.37","D-DT-6092","Clamp, LOOP:TBTO120;TUBULAR PALM TAP-OFF ","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.38","D-DT-6092","Clamp, LOOP:TBTO80;TUBULAR PALM TAP-OFF ","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.39","D-DT-6090","Clamp, S/COMP TBCT120/26/C1 0DEG D6090","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.40","D-DT-6090","Clamp, S/COMP TBCT120/38/C1 0DEG D6090","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.41","D-DT-6090","Clamp, S/COMP TBCT80/26/C1 0 DEG D6090","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.42","D-DT-6090","Clamp, S/COMP TBCT80/26/C1 45 DEG D6090","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.43","D-DT-6090","Clamp, S/COMP TBCT80/26/C1 90 DEG D6090","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.44","D-DT-6090","Clamp, S/COMP TBCT80/38/C1 0 DEG D6090","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.45","D-DT-6090","Clamp, S/COMP TBCT80/38/C1 45 DEG D6090","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.46","D-DT-6090","Clamp, S/COMP TBCT80/38/C1 90 DEG D6090","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.47","D-DT-6316","Clamp, SLIDING SUPPORT TBFSS D6316","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.48","D-DT-6018","Clamp, STRAIN:EPC-F;38.3MM PALM 90DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.49","D-DT-6099","Clamp, STRAIN:EUT-B ;AL TO AL; BOLTED T","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.50","D-DT-6099","Clamp, STRAIN:EUT-C ;AL TO AL; BOLTED T","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.51","D-DT-6099","Clamp, STRAIN:EUT-C MOD ;AL TO AL","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.52","D-DT-6099","Clamp, STRAIN:EUT-D ;AL TO AL; BOLTED T","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.53","D-DT-6099","Clamp, STRAIN:EUT-E ;AL TO AL; BOLTED T","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.54","D-DT-6027","Clamp, STUD PALM BOLT 38.3mm EXP-B D6027","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.55","D-DT-6090","Clamp, T/COMP TBCT120/26/C2 0DEG D6090","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.56","D-DT-6090","Clamp, T/COMP TBCT120/38/C2 0DEG D6090","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.57","D-DT-6090","Clamp, T/COMP TBCT80/26/C2 D6090","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.58","D-DT-6090","Clamp, T/COMP TBCT80/38/C2 D6090","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.59","D-DT-6119","Clamp, TUB  TAP-OFF TBTC120/C1-26  D6119","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.60","D-DT-6119","Clamp, TUB  TAP-OFF TBTC120/C1-38  D6119","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.61","D-DT-6119","Clamp, TUB  TAP-OFF TBTC120/C2-26  D6119","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.62","D-DT-6119","Clamp, TUB  TAP-OFF TBTC120/C2-38  D6119","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.63","D-DT-6119","Clamp, TUB  TAP-OFF TBTC120/C3-26  D6119","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.64","D-DT-6119","Clamp, TUB  TAP-OFF TBTC120/C3-38  D6119","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.65","D-DT-6119","Clamp, TUB  TAP-OFF TBTC80/C1-26   D6119","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.66","D-DT-6119","Clamp, TUB  TAP-OFF TBTC80/C1-38   D6119","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.67","D-DT-6119","Clamp, TUB  TAP-OFF TBTC80/C2-38   D6119","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.68","D-DT-6119","Clamp, TUB  TAP-OFF TBTC80/C-26   D6119","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.69","D-DT-6119","Clamp, TUB  TAP-OFF TBTC80/C3-26   D6119","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.70","D-DT-6119","Clamp, TUB  TAP-OFF TBTC80/C3-38   D6119","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.71","D-DT-6117","Clamp, TUBE BUS/PALM T/OFF TBPT120  D6117","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.72","D-DT-6117","Clamp, TUBE BUS/PALM T/OFF TBPT80   D6117","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.73","D-DT-6086","Clamp, TUBE:ECC-PI-F-A;80/80/76;FIX","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.74","D-DT-6086","Clamp, TUBE:ECC-PI-F-B;80/80/127;FIX","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.75","D-DT-6086","Clamp, TUBE:ECC-PI-F-E;120/120/76;FIX","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.76","D-DT-6086","Clamp, TUBE:ECC-PI-F-F;120/120/127;FIX","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.77","D-DT-6086","Clamp, TUBE:ECC-PI-S-A;80/80/76;SLIDE","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.78","D-DT-6086","Clamp, TUBE:ECC-PI-S-B;80/80/127;SLIDE","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.79","D-DT-6086","Clamp, TUBE:ECC-PI-S-E;120/120/76;SLIDE","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.80","D-DT-6086","Clamp, TUBE:ECC-PI-S-F;120/120/127;SLIDE","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.81","D-DT-6086","Clamp, TUBE:ECC-PI-S-J;200/200/225;SLIDE","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.82","D-DT-6086","Clamp, TUBE:ECC-PI-S-K;250/250/225;SLIDE","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.83","D-DT-6086","Clamp, TUBE:ECC-PI-S-L;200/200/127;SLIDE","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.84","D-DT-6035","Clamp, TUBE:ECC-T-ST-A;80/26STEM;TEE","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.85","D-DT-6035","Clamp, TUBE:ECC-T-ST-B;80/38STEM;TEE","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.86","D-DT-6035","Clamp, TUBE:ECC-T-ST-E;120/26STEM;TEE","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.87","D-DT-6035","Clamp, TUBE:ECC-T-ST-F;120/38STEM;TEE","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.88","D-DT-6116","Clamp, TUBE:ECC-TT-C;120/120;COUPLER","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.89","D-DT-6116","Clamp, TUBE:ECC-TT-F;200/200;COUPLER","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.90","D-DT-6116","Clamp, TUBE:ECC-TT-G;250/250;COUPLER","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.91","D-DT-6093","Clamp, TUBE:EEC-PI-FS-A;80/76;FIX/SLD","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.92","D-DT-6093","Clamp, TUBE:EEC-PI-FS-B;80/127;FIX/SLD","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.93","D-DT-6093","Clamp, TUBE:EEC-PI-FS-E;120/76;FIX/SLD","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.94","D-DT-6093","Clamp, TUBE:EEC-PI-FS-F;120/127;FIX/SLD","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.95","D-DT-6093","Clamp, TUBE:EEC-PI-FS-P;200/127;FIX/SLD","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.96","D-DT-6093","Clamp, TUBE:EEC-PI-FS-Q;200/225;FIX/SLD","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.97","D-DT-6093","Clamp, TUBE:EEC-PI-FS-R;250/225;FIX/SLD","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.98","D-DT-6093","Clamp, TUBE:EEC-PI-SS-A;80/76;SLD/SLD","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.99","D-DT-6093","Clamp, TUBE:EEC-PI-SS-B;80/127;SLD/SLD","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.100","D-DT-6093","Clamp, TUBE:EEC-PI-SS-E;120/76;SLD/SLD","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.101","D-DT-6093","Clamp, TUBE:EEC-PI-SS-F;120/127;SLD/SLD","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.102","D-DT-6093","Clamp, TUBE:EEC-PI-SS-Q;200/225;SLD/SLD","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.103","D-DT-6018","Clamp, EPC-A;COMP/PALM ODG;26.5 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.104","D-DT-6018","Clamp, EPC-B;COMP/PALM 45DG;26.5 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.105","D-DT-6018","Clamp, EPC-C;COMP/PALM 90DG;26.5 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.106","D-DT-6018","Clamp, EPC-D;COMP/PALM ODG;38.3 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.107","D-DT-6018","Clamp, EPC-E;COMP/PALM 45DG;38.3 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.108","D-DT-6018","Clamp, EPC-G;COMP/PALM ODG;26.5 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.109","D-DT-6018","Clamp, EPC-H;COMP/PALM 45DG;26.5 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.110","D-DT-6018","Clamp, EPC-J;COMP/PALM 90DG;26.5 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.111","D-DT-6018","Clamp, EPC-K;COMP/PALM ODG;38.3 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.112","D-DT-6018","Clamp, EPC-L;COMP/PALM 45DG;38.3 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.113","D-DT-6018","Clamp, EPC-M;COMP/PALM 90DG;38.3 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.114","D-DT-6018","Clamp, EPC-N;COMP/PALM ODG;80MM X 90MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.115","D-DT-6018","Clamp, EPC-P;COMP/PALM ODG;125MM X 125MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.116","D-DT-6018","Clamp, EPC-Q;COMP/PALM ODG;16.3 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.117","D-DT-6018","Clamp, EPC-R;COMP/PALM 45DG;16.3 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.118","D-DT-6018","Clamp, EPC-S;COMP/PALM 90DG;16.3 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.119","D-DT-6010","Clamp, ETC-A;T/COMP; RUN 23.5 TAP 26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.120","D-DT-6010","Clamp, ETC-B;T/COMP; RUN 23.5 TAP 38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.121","D-DT-6010","Clamp, ETC-C;T/COMP; RUN 26.5 TAP 26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.122","D-DT-6010","Clamp, ETC-D;T/COMP; RUN 26.5 TAP 38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.123","D-DT-6010","Clamp, ETC-E;T/COMP; RUN 28.6 TAP 26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.124","D-DT-6010","Clamp, ETC-F;T/COMP; RUN 28.6 TAP 38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.125","D-DT-6010","Clamp, ETC-G;T/COMP; RUN 35.6 TAP 26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.126","D-DT-6010","Clamp, ETC-H;T/COMP; RUN 35.6 TAP 38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.127","D-DT-6010","Clamp, ETC-J;T/COMP; RUN 38.3 TAP 26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.128","D-DT-6010","Clamp, ETC-K;T/COMP; RUN 38.3 TAP 38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.129","D-DT-6010","Clamp, ETC-L;T/COMP; RUN 18.1 TAP 26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.130","D-DT-6010","Clamp, ETC-M;T/COMP; RUN 18.1 TAP 18.1","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.131","D-DT-6010","Clamp, ETC-N;T/COMP; RUN 26.5 TAP 18.1","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.132","D-DT-6010","Clamp, ETC-P;T/COMP; RUN 38.3 TAP 18.1","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.133","D-DT-6010","Clamp, ETC-Q;T/COMP; RUN 38.3 TAP 16","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.134","D-DT-6002","Clamp, EX-A;BOLT/BOLT; STEM 26 COND 16.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.135","D-DT-6002","Clamp, EX-B;BOLT/BOLT; STEM 26 COND 26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.136","D-DT-6002","Clamp, EX-C;BOLT/BOLT; STEM 38 COND 16.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.137","D-DT-6006","Clamp, EXC-A;BOLT/COMP; STEM 26 COND26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.138","D-DT-6006","Clamp, EXC-B;BOLT/COMP; STEM 38 COND26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.139","D-DT-6006","Clamp, EXC-C;BOLT/COMP; STEM 38 COND38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.140","D-DT-6006","Clamp, EXC-D;BOLT/COMP; STEM 38 COND38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.141","D-DT-6006","Clamp, EXC-E;BOLT/COMP; STEM 38 COND38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.142","D-DT-6006","Clamp, EXC-F;BOLT/COMP; STEM 38 COND26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.143","D-DT-6006","Clamp, EXC-G;BOLT/COMP; STEM 38 COND26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.144","D-DT-6006","Clamp, EXC-H;BOLT/COMP; STEM 38 COND18.1","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.145","D-DT-6006","Clamp, EXC-J;BOLT/COMP; STEM 35 COND26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.146","D-DT-6006","Clamp, EXC-K;BOLT/COMP; STEM 35 COND38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.147","D-DT-6006","Clamp, EXC-L;BOLT/COMP; STEM 26 COND26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.148","D-DT-6006","Clamp, EXC-M;BOLT/COMP; STEM 26 COND18.1","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.149","D-DT-6006","Clamp, EXC-N;BOLT/COMP; STEM 40 COND26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.150","D-DT-6006","Clamp, EXC-P;BOLT/COMP; STEM 60 COND38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.151","D-DT-6006","Clamp, EXC-Q;BOLT/COMP; STEM 60 COND38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.152","D-DT-6006","Clamp, EXC-R;BOLT/COMP; STEM 60 COND38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.153","D-DT-6002","Clamp, EX-D;BOLT/BOLT; STEM 38 COND 26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.154","D-DT-6002","Clamp, EX-E;BOLT/BOLT; STEM 38 COND 38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.155","D-DT-6002","Clamp, EX-F;BOLT/BOLT; STEM 38 COND 19","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.156","D-DT-6002","Clamp, EX-G;BOLT/BOLT; STEM 35 COND 26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.157","D-DT-6002","Clamp, EX-H;BOLT/BOLT; STEM 35 COND 38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.158","D-DT-6002","Clamp, EX-J;BOLT/BOLT; STEM 26 COND 19","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.159","D-DT-6002","Clamp, EX-K;BOLT/BOLT; STEM 26 COND 21","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.160","D-DT-6022","Clamp, EY-A;Y/BOLT; STEM 38 COND X2 26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.161","D-DT-6022","Clamp, EY-B;Y/BOLT; STEM 38 COND X2 38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.162","D-DT-6022","Clamp, EY-C;Y/BOLT; STEM 38 COND X2 26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.163","D-DT-6013","Clamp, EYC-A;2X26.5 COMP 38 BOLTED 0DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.164","D-DT-6013","Clamp, EYC-AA;2X26.5 COMP 60 BOLTED 0DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.165","D-DT-6013","Clamp, EYC-AB;2X26.5 COMP 60 BOLTED 45DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.166","D-DT-6013","Clamp, EYC-AC;2X26.5 COMP 26 BOLTED 90DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.167","D-DT-6013","Clamp, EYC-B;2X38.3 COMP 38 BOLTED 0DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.168","D-DT-6013","Clamp, EYC-C;2X26.5 COMP 38 BOLTED 45DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.169","D-DT-6013","Clamp, EYC-D;2X38.3 COMP 38 BOLTED 45DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.170","D-DT-6013","Clamp, EYC-E;2X26.5 COMP 38 BOLTED 90DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.171","D-DT-6013","Clamp, EYC-F;2X38.3 COMP 38 BOLTED 90DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.172","D-DT-6013","Clamp, EYC-G;2X38.3 COMP 60 BOLTED 0DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.173","D-DT-6013","Clamp, EYC-H;2X38.3 COMP 60 BOLTED 45DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.174","D-DT-6013","Clamp, EYC-J;2X38.3 COMP 60 BOLTED 90DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.175","D-DT-6013","Clamp, EYC-K;2X26.5 COMP 26 BOLTED 0DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.176","D-DT-6013","Clamp, EYC-L;2X26.5 COMP 26 BOLTED 45DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.177","D-DT-6013","Clamp, EYC-M;2X26.5 COMP 26 BOLTED 90DG","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.178","D-DT-6109","Clamp, EYC-N;COMP/PALM ODG;2X38.3 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.179","D-DT-6109","Clamp, EYC-P;COMP/PALM 45DG;2X38.3 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.180","D-DT-6109","Clamp, EYC-Q;COMP/PALM 90DG;2X38.3 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.181","D-DT-6109","Clamp, EYC-R;COMP/PALM ODG;2X38.3 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.182","D-DT-6109","Clamp, EYC-S;COMP/PALM 45DG;2X38.3 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.183","D-DT-6109","Clamp, EYC-T;COMP/PALM 90DG;2X38.3 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.184","D-DT-6109","Clamp, EYC-U;COMP/PALM ODG;2X26.5 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.185","D-DT-6109","Clamp, EYC-V;COMP/PALM 45DG;2X26.5 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.186","D-DT-6109","Clamp, EYC-W;COMP/PALM 90DG;2X26.5 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.187","D-DT-6109","Clamp, EYC-X;COMP/PALM ODG;2X26.5 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.188","D-DT-6109","Clamp, EYC-Y;COMP/PALM 45DG;2X26.5 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.189","D-DT-6109","Clamp, EYC-Z;COMP/PALM 90DG;2X26.5 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.190","D-DT-6022","Clamp, EY-D;Y/BOLT; STEM 38 COND X2 38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.191","D-DT-6022","Clamp, EY-E;Y/BOLT; STEM 26 COND X2 26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.192","D-DT-6022","Clamp, EY-F;Y/BOLT; STEM 26 COND X2 26.5","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.193","D-DT-6022","Clamp, EY-G;Y/BOLT; STEM 26 COND X2 38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.194","D-DT-6022","Clamp, EY-H;Y/BOLT; STEM 26 COND X2 38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.195","D-DT-6022","Clamp, EY-J;Y/BOLT; STEM 60 COND X2 38.3","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.196","D-DT-6003","Clamp, EESP-A;STEM PALM;38 MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.197","D-DT-6059","Clevis Ball 16mm 16L 100CL 120kN D6059","each",null,null,"cost plus 5%",{"v":83,"d":"83.00"}]
["G.2.1.198","D-DT-6059","Clevis Ball 16mm 16L 80CL 120kN D6059","each",null,null,"cost plus 5%",{"v":83,"d":"83.00"}]
["G.2.1.199","D-DT-6059","Clevis Ball 16mm 19L 80CLG 120kN D6059","each",null,null,"cost plus 5%",{"v":83,"d":"83.00"}]
["G.2.1.200","D-DT-6084","CLEV-TONG, TWIST 19L 210kN D6084","each",null,null,"cost plus 5%",{"v":83,"d":"83.00"}]
["G.2.1.201","D-DT-6084","CLEV-TONG,TWIST 16L 120kN D6084","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.202","D-DT-6040","End Cap, TBEC 120 COND WITH F/CLAMP D6040","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.203","D-DT-6040","End Cap, TBEC 120 PLAIN NO F/CLAMP D6040","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.204","D-DT-6040","End Cap, TBEC 80 COND WITH F/CLAMP D6040","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.205","D-DT-6040","End Cap, TBEC 80 PLAIN NO F/CLAMP D6040","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.206","D-DT-6087","Spacer, ES-A;COND 2X26.5MM;150MM CRS","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.207","D-DT-6087","Spacer, ES-B;COND 2X38.3MM;150MM CRS","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.208","D-DT-6087","Spacer, ES-C;COND 2X26.5MM;330MM CRS","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.209","D-DT-6087","Spacer, ESC-A;COND 2X26.5MM;150MM CRS","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.210","D-DT-6087","Spacer, ESC-B;COND 2X38.3MM;150MM CRS MM","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.211","D-DT-6087","Spacer, ESC-C;COND 2X26.5MM;330MM CRS","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.212","D-DT-6087","Spacer, ESC-D;COND 2X38.3MM;330MM CRS","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.213","D-DT-6087","Spacer, ESC-E;COND 3X38.3MM;165MM CRS","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.214","D-DT-6087","Spacer, ES-D;COND 2X38.3MM;330MM CRS","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
["G.2.1.215","D-DT-6087","Spacer, ES-E;COND 3X38.3MM;165MM CRS","each",null,null,"cost plus 5%",{"v":260,"d":"260.00"}]
[null,null,"                                                                Total carried to Item of Summary"]
[{"$nulls":8},"Please initial"]
[{"$nulls":8},"Compiler/Designer:"]
[{"$nulls":8},"Quantity Surveyor"]

{"sheet":"Section H Cable & Stringing","index":9,"n_rows":54,"n_cols":11,"rows_kept":54,"merged":[[1,0,1,10],[2,0,2,1],[2,9,2,10],[3,0,3,1],[3,9,3,10],[4,0,4,1],[4,9,4,10],[5,0,5,1],[6,0,6,10],[7,0,7,10],[9,0,10,0],[9,1,10,1],[9,2,10,10],[11,1,12,1],[11,2,12,2],[11,3,12,3],[11,4,11,5],[11,6,11,7],[11,8,11,9],[11,10,12,10],[51,8,51,9],[52,8,52,9],[53,8,53,9]]}
[]
["GEMMA CLUSTER"]
["Project Name:",{"$nulls":6},"Template Identifier:"]
["Project ID:",{"$nulls":6},"Effective Date:"]
["Job Name:",{"$nulls":6},"Review Date:"]
["Job ID:"]
["SCHEDULE OF QUANTITIES - SECTION H"]
["CABLING & STRINGING"]
[]
["H1",null,"CABLING & STRINGING"]
[]
["Item",null,"Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,null,"Supply the material, transport to site, install the cable, stringers, tube and conductor"]
["H1.1",null,"Conductor & Stringers"]
["H1.1.1","D-DT-6000","Aluminium Tube (120mm x 4mm x 12m)","each",{"$nulls":3},{"v":160.28700884396915,"d":"160.29"}]
["H1.1.2","D-DT-6000","Aluminium Tube (80mm x 8mm x 12m)","each",{"$nulls":3},160.29]
["H1.1.3","D-DT-3136","Bull (38.25mm Diameter AAC) Ungrs","m",{"$nulls":3},{"v":143.90563063618913,"d":"143.91"}]
["H1.1.4","D-DT-3136","Insulated Bull (38.25mm Diameter AAC) Ungrs","m",{"$nulls":3},{"v":146.3927903484546,"d":"146.39"}]
["H1.1.5","D-DT-3136","Centipede (26.46mm Diameter AAC) Ungrs","m",{"$nulls":3},{"v":135.04509105208865,"d":"135.05"}]
["H1.1.6","D-DT-3136","Insulated Centipede (26.46mm Diameter AAC) Ungrs","m",{"$nulls":3},{"v":127.0773300905078,"d":"127.08"}]
["H1.1.7","D-DT-3136","Hornet (16.25 mm Diameter AAC) Ungrs","m",{"$nulls":3},{"v":28.16099675063005,"d":"28.16"}]
["H1.1.8","D-DT-3136","Insulated Hornet (16.25 mm Diameter AAC) Ungrs","m",{"$nulls":3},{"v":28.117530372981975,"d":"28.12"}]
["H1.1.9","D-DT-3136","Hare (14.16mm Diameter ACSR) Ungrs","m",{"$nulls":3},{"v":92.63462433862435,"d":"92.63"}]
["H1.1.10","D-DT-3136","Hare (14.16mm Diameter ACSR) Grs","m",{"$nulls":3},{"v":95.63462433862435,"d":"95.63"}]
["H1.1.11","D-DT-3136","Steel Wire (7/3.35mm) (for high strung shielding)","m",{"$nulls":3},{"v":32.3,"d":"32.30"}]
["H1.1.12","D-DT-3136","Steel Wire (19/2.65mm) (for high strung shielding)","m",{"$nulls":3},{"v":32.3,"d":"32.30"}]
["H1.2",null,"POWER CABLE INSTALLATION"]
["H1.2.1","D-DT 0854","Trenching 1m x 1m","m",null,null,"Cost plus 5%",{"v":1168.7032387566137,"d":"1,168.70"}]
["H1.2.2","D-DT 0854","River Sand Bedding","m",null,null,"Cost plus 5%",{"v":160.18329005993652,"d":"160.18"}]
["H1.2.3","D-DT 8018/19","sleeves across runway","m",null,null,"Cost plus 5%",{"v":236.15833097537245,"d":"236.16"}]
["H1.2.4",null,"Install Poly Prop Clamps","each",null,null,"Cost plus 5%",{"v":388.74067916793985,"d":"388.74"}]
["H1.2.5","D-DT 0854","Installation of danger tape","each",null,null,"Cost plus 5%",{"v":40.88159516825322,"d":"40.88"}]
["H1.2.6","D-DT 0854","Laying Of Single Core MV Cable Trefoil ","m",null,null,"Cost plus 5%",{"v":19.008379431216934,"d":"19.01"}]
["H1.2.7","D-DT 0854","Laying Of Three Core MV Cable","m",null,null,"Cost plus 5%",{"v":26.611731203703705,"d":"26.61"}]
["H1.2.8","D-DT 8005/6","95-185 mm2 Cable Termination (Outdoor)","each",null,null,"Cost plus 5%",{"v":1403.6162670113997,"d":"1,403.62"}]
["H1.2.9","D-DT 8005/6","95-185 mm2 Shrouded Cable Termination","each",null,null,"Cost plus 5%",{"v":19.070873193089668,"d":"19.07"}]
["H1.2.10","D-DT 8005/6","95-185 mm2 Screened Separable Connectors  Termination","each",null,null,"Cost plus 5%",{"v":1386.6961645173085,"d":"1,386.70"}]
["H1.2.11","D-DT 8005/6","185-300 mm2 Cable Termination (Outdoor)","each",null,null,"Cost plus 5%",{"v":1403.6162670113997,"d":"1,403.62"}]
["H1.2.12","D-DT 8005/6","85-300 mm2 Shrouded Cable Termination","each",null,null,"Cost plus 5%",{"v":19.070873193089668,"d":"19.07"}]
["H1.2.13","D-DT 8005/6","185-300 mm2 Screened Separable Connectors  Termination","each",null,null,"Cost plus 5%",{"v":1386.6961645173085,"d":"1,386.70"}]
["H1.2.14","D-DT 8005/6","630 mm2 Shrouded Cable Termination","each",null,null,"Cost plus 5%",{"v":19.070873193089668,"d":"19.07"}]
["H1.2.15","D-DT 8005/6"," 630 mm2  Cable Termination (Outdoor)","each",null,null,"Cost plus 5%",{"v":1403.6162670113997,"d":"1,403.62"}]
["H1.2.16","D-DT 8005/6"," 630 mm2 Screened Separable Connectors  Termination","each",null,null,"Cost plus 5%",{"v":1386.6961645173085,"d":"1,386.70"}]
["H1.2.17","D-DT 8004"," Trifur Kit,Scr MV 2.5M Xlpe 95-300 mm2  ","each",null,null,"Cost plus 5%",{"v":1177.777021164021,"d":"1,177.78"}]
["H1.2.18","D-DT 8008","Make Off 95-185mm2 MV Cable Joint","each",null,null,"Cost plus 5%",{"v":1177.777021164021,"d":"1,177.78"}]
["H1.2.19","D-DT 8008","Make Off 185-300mm2 MV Cable Joint","each",null,null,"Cost plus 5%",{"v":1177.777021164021,"d":"1,177.78"}]
["H1.2.20","D-DT 8008","Make Off 630mm2 MV Cable Joint","each",null,null,"Cost plus 5%",{"v":1177.777021164021,"d":"1,177.78"}]
["H.1.3",null,"TESTING","each"]
["H1.3.1",null,"VLF Test for MV Cables","each",null,null,"Cost plus 5%",{"v":2118.9859103432964,"d":"2,118.99"}]
[null,null,"                                                                Total carried to Item of Summary"]
[{"$nulls":8},"Please initial"]
[{"$nulls":8},"Compiler/Designer:"]
[{"$nulls":8},"Quantity Surveyor"]

{"sheet":"Section I Labelling","index":10,"n_rows":43,"n_cols":11,"rows_kept":43,"merged":[[1,0,1,10],[2,0,2,1],[2,9,2,10],[3,0,3,1],[3,9,3,10],[4,0,4,1],[4,9,4,10],[5,0,5,1],[6,0,6,10],[7,0,7,10],[8,2,8,10],[9,1,10,1],[9,2,10,2],[9,3,10,3],[9,4,9,5],[9,6,9,7],[9,8,9,9],[9,10,10,10],[40,8,40,9],[41,8,41,9],[42,8,42,9]]}
[]
["GEMMA CLUSTER"]
["Project Name:",{"$nulls":6},"Template Identifier:"]
["Project ID:",{"$nulls":6},"Effective Date:"]
["Job Name:",{"$nulls":6},"Review Date:"]
["Job ID:"]
["SCHEDULE OF QUANTITIES - SECTION I"]
["SUBSTATION LABELS AND SIGNS"]
["I",null,"SUBSTATION LABELS AND SIGNS"]
["Item","Refer","Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,"DISASAAN0\nDSP 34-254\nD-DT-5273","Supply the material, transport to site, and install (attach to equipment, fence, gates and building) according to Eskom specification. Contractor to ensure that labels are attached at the correct positions  as per the Labelling Schedule and the substation drawing documents. Refer to SCSASABK3 Rev.0 p26-28"]
["I.1.1",null,"EQUIPMENT LABELLING"]
["I1.1","D-DT-5047s1\nD-DT-5273s4","Large substation Name Label","each",null,null,"Cost plus 5%",242.35]
["I1.2",null,"Outdoor Equipment labels","each",null,null,"Cost plus 5%",{"v":205.01188682571393,"d":"205.01"}]
["I1.3",null,"Supply and Install Station Equipment Labels Brackets","each",null,null,"Cost plus 5%",{"v":193.49143131693532,"d":"193.49"}]
["I1.4","D-DT-5237 sheet 14","Attachment Materials For Fence Labels: ","each",null,null,"Cost plus 5%",61.18]
["I1.5",null,"Back Plates (size acc. to label size needed for and as per Eskom spec. Contractor to calculate and confirm quantity needed)","each",null,null,"Cost plus 5%",61.18]
["I1.6",null,"Angle Iron (size and lengths acc. to label size needed for and as per Eskom spec. Contractor to calculate and confirm quantity needed)","each",null,null,"Cost plus 5%",61.18]
["I1.2","D-DT-6114","PHASE LABELS"]
["I1.2.1","D-DT-6114","Phase marker plate Blue","each",null,null,"Cost plus 5%",{"v":57,"d":"57.00"}]
["I1.2.2","D-DT-6114","Phase marker plate Red","each",null,null,"Cost plus 5%",{"v":57,"d":"57.00"}]
["I1.2.3","D-DT-6114","Phase marker plate White","each",null,null,"Cost plus 5%",{"v":57,"d":"57.00"}]
["I1.2.4","D-DT-5273s3","Phase marker plate bracket","each",null,null,"Cost plus 5%",{"v":38,"d":"38.00"}]
["I1.3",null,"SIGNS & LABELS ON FENCE"]
["I1.3.1",null,"Unauthorised Labels on Fence","each",null,null,"Cost plus 5%",{"v":46.63636363636363,"d":"46.64"}]
["I1.3.2",null,"Internal Labeling","each",null,null,"Cost plus 5%",{"v":39.55636363636363,"d":"39.56"}]
["I1.3.3",null,"Supply  and Install Station Equipment Labels","each",null,null,"Cost plus 5%",{"v":39.55636363636363,"d":"39.56"}]
["I1.3.4","D-DT-5015","Sign, ABC - Unauthorised Entry & Interfering","each",null,null,"Cost plus 5%",{"v":46.63636363636363,"d":"46.64"}]
["I1.3.5","D-DT-5016","Sign, DE - Sign Fire First Aid","each",null,null,"Cost plus 5%",{"v":63.75272727272727,"d":"63.75"}]
["I1.3.6","D-DT-5017","Sign, F - Prohibitive Fence and Gate","each",null,null,"Cost plus 5%",50.35]
["I1.3.7","D-DT-5018","Sign, G - Hard Hat Area","each",null,null,"Cost plus 5%",50.35]
["I1.3.8","D-DT-5047","Gate number 1 to 5","each",null,null,"Cost plus 5%",{"v":49.58181818181818,"d":"49.58"}]
["I1.4",null,"INTERNAL LABELING","each"]
["I.4.1","D-DT 5022s1","Sign, DCSS 1 – Battery Room","each",null,null,"Cost plus 5%",50.35]
["I.4.2","D-DT-5022s2","Sign, DCSS 2 – Battery Cabinet","each",null,null,"Cost plus 5%",50.35]
["I.4.3","D-DT-5023s1","Sign, GA 20 – Informative – Emergency Shower","each",null,null,"Cost plus 5%",50.35]
["I.4.4","D-DT-5023s2","Sign, GA 19 – Informative - Eye Wash","each",null,null,"Cost plus 5%",50.35]
["I.4.5","D-DT-5023s3","Sign, PV 5 – Drinking Water Prohibitive","each",null,null,"Cost plus 5%",50.35]
[null,null,"                                                                Total carried to Item of Summary"]
[{"$nulls":8},"Please initial"]
[{"$nulls":8},"Compiler/Designer:"]
[{"$nulls":8},"Quantity Surveyor"]

{"sheet":"Section J Dismantling","index":11,"n_rows":115,"n_cols":11,"rows_kept":115,"merged":[[1,0,1,10],[2,0,2,1],[2,9,2,10],[3,0,3,1],[3,9,3,10],[4,0,4,1],[4,9,4,10],[5,0,5,1],[6,0,6,10],[7,0,7,10],[8,2,8,10],[9,1,10,1],[9,2,10,2],[9,3,10,3],[9,4,9,5],[9,6,9,7],[9,8,9,9],[9,10,10,10],[112,8,112,9],[113,8,113,9],[114,8,114,9]]}
[]
["GEMMA CLUSTER"]
["Project Name:",{"$nulls":6},"Template Identifier:"]
["Project ID:",{"$nulls":6},"Effective Date:"]
["Job Name:",{"$nulls":6},"Review Date:"]
["Job ID:"]
["SCHEDULE OF QUANTITIES - SECTION J"]
["DISMANTLING"]
["J",null,"DISMANTLING"]
["Item",null,"Description of the item","Unit","Qty",null,"Rate",null,"Total",null,"Price (R)"]
["No.",{"$nulls":3},"Supply","Install","Supply","Install","Supply","Install"]
[null,null,"Supply the material, transport to site, excavate into all material, dismantle the existing installation, level-off as required, collect the material as required and do the finishing as per  the environmental requirements "]
["J1.1",null,"ISOLATOR"]
["J1.1.1",null,"132kV","each",{"$nulls":3},{"v":1376.6823947328974,"d":"1,376.68"}]
["J1.1.2",null,"88kV","each",{"$nulls":3},{"v":1353.0813527146422,"d":"1,353.08"}]
["J1.1.3",null,"66kV","each",{"$nulls":3},{"v":1306.0639550290541,"d":"1,306.06"}]
["J1.1.4",null,"44kV","each",{"$nulls":3},{"v":796.6194033823272,"d":"796.62"}]
["J1.1.5",null,"33kV","each",{"$nulls":3},{"v":686.9645256781707,"d":"686.96"}]
["J1.1.6",null,"22kV","each",{"$nulls":3},{"v":574.9875331002903,"d":"574.99"}]
["J1.1.7",null,"11kV","each",{"$nulls":3},{"v":432.47843190045694,"d":"432.48"}]
["J1.1.8",null,"6.6kV","each",{"$nulls":3},{"v":413.8407736045929,"d":"413.84"}]
["J1.2",null,"SURGE ARRESTORS"]
["J1.2.1",null,"132kV","each",{"$nulls":3},{"v":610.5351698464516,"d":"610.54"}]
["J1.2.2",null,"88kV","each",{"$nulls":3},{"v":498.6449441653209,"d":"498.64"}]
["J1.2.3",null,"66kV","each",{"$nulls":3},{"v":478.7497162052021,"d":"478.75"}]
["J1.2.4",null,"44kV","each",{"$nulls":3},{"v":393.296263432299,"d":"393.30"}]
["J1.2.5",null,"33kV","each",{"$nulls":3},{"v":317.6873422072284,"d":"317.69"}]
["J1.2.6",null,"22kV","each",{"$nulls":3},{"v":252.70976108262144,"d":"252.71"}]
["J1.2.7",null,"11kV","each",{"$nulls":3},{"v":244.91737736667906,"d":"244.92"}]
["J1.2.8",null,"6.6kV","each",{"$nulls":3},{"v":227.67755729258602,"d":"227.68"}]
["J1.3",null,"BREAKERS"]
["J1.3.1",null,"132kV","each",{"$nulls":3},{"v":1911.19137122012,"d":"1,911.19"}]
["J1.3.2",null,"88kV","each",{"$nulls":3},{"v":2022.5177056663879,"d":"2,022.52"}]
["J1.3.3",null,"66kV","each",{"$nulls":3},{"v":1948.8951606125001,"d":"1,948.90"}]
["J1.3.4",null,"44kV","each",{"$nulls":3},{"v":1365.8479330311989,"d":"1,365.85"}]
["J1.3.5",null,"33kV","each",{"$nulls":3},{"v":1067.8224533423288,"d":"1,067.82"}]
["J1.3.6",null,"22kV","each",{"$nulls":3},{"v":1045.7037720815288,"d":"1,045.70"}]
["J1.3.7",null,"11kV","each",{"$nulls":3},{"v":1038.5164904140097,"d":"1,038.52"}]
["J1.3.8",null,"Removal of indoor switch gear","each",{"$nulls":3},{"v":2409.874063803723,"d":"2,409.87"}]
["J1.4",null,"JUNCTION BOXES"]
["J.1.4.1",null,"VT JB with insert","each",{"$nulls":3},{"v":189.07234506163408,"d":"189.07"}]
["J.1.4.2",null,"CT JB with insert","each",{"$nulls":3},{"v":189.07234506163408,"d":"189.07"}]
["J.1.5",null,"CURRENT TRANSFORMER",{"$nulls":4},0]
["J1.5.1",null,"132kV","each",{"$nulls":3},{"v":603.5111318065577,"d":"603.51"}]
["J1.5.2",null,"88kV","each",{"$nulls":3},{"v":570.6670620948277,"d":"570.67"}]
["J1.5.3",null,"66kV","each",{"$nulls":3},{"v":538.4769114350295,"d":"538.48"}]
["J1.5.4",null,"44kV","each",{"$nulls":3},{"v":431.4899485175696,"d":"431.49"}]
["J1.5.5",null,"33kV","each",{"$nulls":3},{"v":305.0362328643201,"d":"305.04"}]
["J1.5.6",null,"22kV","each",{"$nulls":3},{"v":277.0060812297799,"d":"277.01"}]
["J1.5.7",null,"11kV","each",{"$nulls":3},{"v":231.4926183043952,"d":"231.49"}]
["J1.5.8",null,"6.6kV","each",{"$nulls":3},{"v":226.856512575443,"d":"226.86"}]
["J1.6",null,"VOLTAGE TRANSFORMER"]
["J1.6.1",null,"132kV","each",{"$nulls":3},{"v":597.1059789182115,"d":"597.11"}]
["J1.6.2",null,"88kV","each",{"$nulls":3},{"v":570.3782678595358,"d":"570.38"}]
["J1.6.3",null,"66kV","each",{"$nulls":3},{"v":514.907007357099,"d":"514.91"}]
["J1.6.4",null,"44kV","each",{"$nulls":3},{"v":413.08740348060223,"d":"413.09"}]
["J1.6.5",null,"33kV","each",{"$nulls":3},{"v":315.3545464636572,"d":"315.35"}]
["J1.6.6",null,"22kV","each",{"$nulls":3},{"v":268.4724540830696,"d":"268.47"}]
["J1.6.7",null,"11kV","each",{"$nulls":3},{"v":266.5182781879752,"d":"266.52"}]
["J1.6.8",null,"6.6kV","each",{"$nulls":3},{"v":261.87981803023376,"d":"261.88"}]
["J1.7",null,"NECRT",{"$nulls":4},0]
["J1.7.1",null,"44kV","each",{"$nulls":3},{"v":801.8402231913456,"d":"801.84"}]
["J1.7.2",null,"33kV","each",{"$nulls":3},{"v":776.1031698997924,"d":"776.10"}]
["J1.7.3",null,"22kV","each",{"$nulls":3},{"v":658.0005013267172,"d":"658.00"}]
["J1.7.4",null,"11kV","each",{"$nulls":3},{"v":602.5176334903493,"d":"602.52"}]
["J1.7.5",null,"6.6kV","each ",{"$nulls":3},{"v":586.8506050864836,"d":"586.85"}]
["J1.8",null,"POST ISOLATORS",{"$nulls":4},0]
["J1.8.1",null,"132kV","each",{"$nulls":3},{"v":597.1059789182115,"d":"597.11"}]
["J1.8.2",null,"88kV","each",{"$nulls":3},{"v":570.3782678595358,"d":"570.38"}]
["J1.8.3",null,"66kV","each",{"$nulls":3},{"v":514.907007357099,"d":"514.91"}]
["J1.8.4",null,"44kV","each",{"$nulls":3},{"v":413.08740348060223,"d":"413.09"}]
["J1.8.5",null,"33kV","each",{"$nulls":3},{"v":315.3545464636572,"d":"315.35"}]
["J1.8.6",null,"22kV","each",{"$nulls":3},{"v":268.4724540830696,"d":"268.47"}]
["J1.8.7",null,"11kV","each",{"$nulls":3},{"v":266.5182781879752,"d":"266.52"}]
["J1.8.8",null,"6.6kV","each",{"$nulls":3},{"v":261.87981803023376,"d":"261.88"}]
["J1.9",null,"STRINGERS (INCLUDING CLAMPS)",{"$nulls":4},0]
["J1.9.1",null,"Tubular B/Bars","m",{"$nulls":3},{"v":159.03291969399348,"d":"159.03"}]
["J1.9.2",null,"Bull Conductor","m",{"$nulls":3},{"v":118.01956900895786,"d":"118.02"}]
["J1.9.3",null,"Centipede Conductor","m",{"$nulls":3},{"v":105.17668065447042,"d":"105.18"}]
["J1.9.4",null,"Hornet","m",{"$nulls":3},{"v":21.860669500193076,"d":"21.86"}]
["J1.9.5",null,"Disconnect Jumpers","each",{"$nulls":3},{"v":89.48295872015998,"d":"89.48"}]
["J1.9.6",null,"Indoor Switchgear Terminations","each",{"$nulls":3},{"v":183.89301375027748,"d":"183.89"}]
["J.1.10",null,"TRANSFORMERS"]
["J1.10.1",null,"Trfr (All MVA's)","each"]
["J1.11",null,"STEELWORK"]
["J1.11.1","D-DT-5200","Circuit Breaker Support","each",{"$nulls":3},{"v":469.23671593006094,"d":"469.24"}]
["J1.11.2","D-DT-5202","Isolator Support","each",{"$nulls":3},{"v":541.9425899454292,"d":"541.94"}]
["J1.11.3","2-ET/14927s2","Me Support","each",{"$nulls":3},{"v":297.9273000083571,"d":"297.93"}]
["J1.11.4","2-ET/14942s2","Busbar Support","each",{"$nulls":3},{"v":510.95222837157564,"d":"510.95"}]
["J1.11.5","DT-5213","Cable End Support","each",{"$nulls":3},{"v":487.1107858809889,"d":"487.11"}]
["J1.11.6","DT-5218","Fire Barrier Support","each",{"$nulls":3},{"v":1999.6348439377916,"d":"1,999.63"}]
["J1.11.7","D-DT 5252s2B","Beam - 132/50/1 Lattice Steel Steelwork Manufacturing Details And Assembly","each",{"$nulls":3},{"v":1900,"d":"1,900.00"}]
["J1.11.8","D-DT 5252s2A","Column - 132/C Lattice Steel Steelwork Manufacturing Details And Assembly","each",{"$nulls":3},{"v":1900,"d":"1,900.00"}]
["J1.11.9","D-DT-5212s2B","132Kv Earth Switch Support","each",{"$nulls":3},{"v":1887.3507692307694,"d":"1,887.35"}]
["J1.11.10","D-DT-5217s5&7","21M Lighting Mast","each",{"$nulls":3},{"v":1887.3507692307694,"d":"1,887.35"}]
["J1.11.11","D-DT-5217s5&7","14M Lightning/Lighting Mast","each",{"$nulls":3},{"v":1887.3507692307694,"d":"1,887.35"}]
["J1.11.12","D-DT-5217s5&7","8M Lightning/Lighting Mast","each",{"$nulls":3},{"v":1887.3507692307694,"d":"1,887.35"}]
["J1.11.13",null,"Cap Bank Unit Inclunding Fence","each",{"$nulls":3},{"v":1193.72,"d":"1,193.72"}]
["J1.11.14",null,"2.4M Steel Palisade Fence","m",{"$nulls":3},{"v":1193.72,"d":"1,193.72"}]
["J1.11.15",null,"2.4M Mesh Wire Fence","m",{"$nulls":3},101.73]
["J1.11.16",null,"Personnel Gate","each",{"$nulls":3},101.73]
["J1.12",null,"BRICKWORK & CONCRETE","each"]
["J1.12.1",null,"Break Down And Remove Foundations","m³",{"$nulls":3},{"v":1907.087319308967,"d":"1,907.09"}]
["J1.12.2",null,"Cable Trench And Covers","m",{"$nulls":3},{"v":90,"d":"90.00"}]
["J1.12.3",null,"Break Down And Remove Concrete Runway","m²",{"$nulls":3},{"v":1907.087319308967,"d":"1,907.09"}]
["J1.12.4",null,"Break Down Of Switchroom/ Control Room","m²",{"$nulls":3},{"v":2011.97712187096,"d":"2,011.98"}]
["J1.12.5",null,"Breakdown Asbestos Room","m²"]
["J1.12.6",null,"Removal Of Rubbles From Site","m³",{"$nulls":3},{"v":488.2143537430955,"d":"488.21"}]
["J1.13",null,"CABLES"]
["J1.13.1",null,"Power Cables","m",{"$nulls":3},10.84]
["J1.13.2",null,"Control Cables","m",{"$nulls":3},10.84]
[null,null,"                                                                Total carried to Item of Summary"]
[{"$nulls":8},"Please initial"]
[{"$nulls":8},"Compiler/Designer:"]
[{"$nulls":8},"Quantity Surveyor"]

{"sheet":"SECTION K Control Plant","index":12,"n_rows":73,"n_cols":12,"rows_kept":73,"merged":[[0,0,0,11],[1,0,1,1],[1,2,1,3],[1,4,4,5],[1,8,1,11],[2,0,2,1],[2,2,2,3],[2,8,2,11],[3,0,3,1],[3,2,3,3],[3,8,3,11],[4,0,4,1],[4,2,4,3],[4,6,4,7],[4,8,4,11],[5,0,5,11],[6,3,7,3],[6,5,6,6],[6,7,6,8],[6,9,6,10],[31,3,31,11],[41,3,41,11],[45,3,45,11],[52,3,52,11],[65,2,65,6],[65,9,65,11],[66,2,66,6],[66,9,66,11],[67,2,67,6],[67,9,67,11],[68,2,68,6],[68,9,68,11],[69,2,69,6],[69,9,69,11],[70,2,70,6],[70,9,70,11],[71,2,71,6],[71,9,71,11],[72,2,72,6],[72,9,72,11]]}
["GEMMA CLUSTER CONTROL PLANT BOQ"]
["Project Name:",{"$nulls":5},"Template Identifier:"]
["Project ID:",{"$nulls":5},"Effective Date:"]
["Job Name:",{"$nulls":5},"Review Date:"]
["Job ID:"]
["Please note: The quantities provided in the schedules are estimated figures and are subject to change, if no quantities are given the contractor must provide estimated figures. "]
["Item","Description of the item","Unit","Contracted BOQ","Qty",{"$nulls":4},"Total",null,"Total"]
[{"$nulls":5},"Supply","Labour",null,null,"Supply","Labour","Price"]
[1,"Decommission and remove Protection Panel.","ea","Protection Panels",0,null,{"v":3095.391184338244,"d":"R 3,095.39"},null,null,{"$f":"E9*F9","v":0},{"$f":"E9*G9","v":0},{"$f":"J9+K9","v":0}]
[2,"Decommission and remove Metering Panel.","ea","Metering Panels",0,null,{"v":3085.170193476588,"d":"R 3,085.17"},null,null,{"$f":"E10*F10","v":0},{"$f":"E10*G10","v":0},{"$f":"J10+K10","v":0}]
[3,"Decommission and remove AC/DC panel.","ea","AC/DC Panel deconission",0,null,{"v":3085.170193476588,"d":"R 3,085.17"},null,null,0,0,0]
[4,"Decommission and remove Charger and battery cabinet.","ea","Battery & Chargers",0,null,{"v":2638.969796042987,"d":"R 2,638.97"},null,null,0,0,0]
[5,"Install HV Feeder Protection Panel.","ea","Protection Panels",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[6,"Install Transformer and Tap Change Protection Panel.","ea","Protection Panels",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[7,"Install MV Rural Feeder Protection Panel.","ea","Protection Panels",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[8,"Install Cable Feeder Protection Panel.","ea","Protection Panels",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[9,"Install Buszone Protection Panel.","ea","Protection Panels",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[10,"Install MV Busbar Arc Detection Protection Panel.","ea","Protection Panels",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[11,"Install Bus-coupler Protection Panel.","ea","Protection Panels",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[12,"Install Under Frequency Load Shedding Protection Panel.","ea","Protection Panels",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[13,"Install Capacitor Bank Protection Panels.","ea","Protection Panels",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[14,"Install Yard AC Board.","ea","Protection Panels",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[15,"Install AC/DC Distribution Panel.","ea","Yard AC board",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[16,"Install Cordex HF, Switchmode Sub-rack battery charger in the AC/DC panel.","ea","AC/DC Panel",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[17,"Install Metering Panel.","ea","Metering Panel",0,null,{"v":2347.8418980237398,"d":"R 2,347.84"},null,null,0,0,0]
[18,"Install Intermediate Distribution Frame (IDF). (Including the backmount frames)","ea","IDF",0,null,{"v":1420.9080396341649,"d":"R 1,420.91"},null,null,0,0,0]
[19,"Install RTU Panel.","ea","RTU Panel",0,null,{"v":1611.4794612780713,"d":"R 1,611.48"},null,null,0,0,0]
[20,"Install CT Junction Box.","ea","CT Junction Box",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[21,"Install VT Junction Box.","ea","VT Junction Box",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[22,"Install Isolator Junction Box.","ea","Isolator Junction Box ",0,null,{"v":1984.44725692378,"d":"R 1,984.45"},null,null,0,0,0]
[{"$nulls":4},0,{"$nulls":4},0,0,0]
[null,"INSTALLATION AND TERMINATION OF CABLES "]
[1,"4 Core - 2.5mm (no.1) Armoured","m","Contracted is split in 3 different items ",0,null,{"v":7.423796504024061,"d":"R 7.42"},null,null,0,0,0]
[2,"4 Core - 4mm (no.1) Armoured","m","Contracted is split in 3 different items ",0,null,{"v":6.768888592000627,"d":"R 6.77"},null,null,0,0,0]
[3,"4 Core - 16mm (no.2) Armoured","m","Contracted is split in 3 different items ",0,null,{"v":6.6920400363188435,"d":"R 6.69"},null,null,0,0,0]
[4,"4 Core - 35mm (no.3) Armoured","m","Not Included in Contract",0,null,{"v":6.7,"d":"R 6.70"},null,null,0,0,0]
[5,"12 Core - 2.5mm (no.2) Armoured","m","Contracted is split in 3 different items ",0,null,{"v":8.607320767814471,"d":"R 8.61"},null,null,0,0,0]
[6,"19 Core 2.5mm (no.3) Armoured","m","Contracted is split in 3 different items ",0,null,{"v":6.983612497582079,"d":"R 6.98"},null,null,0,0,0]
[7,"10 Pair - 0.6mm (no.1) Armoured","m","Contracted is split in 3 different items ",0,null,{"v":7.0058383053527935,"d":"R 7.01"},null,null,0,0,0]
[8,"25 Pair - 0.6mm (no.1) Armoured","m","Contracted is split in 3 different items ",0,null,{"v":7.485200006848232,"d":"R 7.49"},null,null,0,0,0]
[9,"50 Pair - 0.6mm (no.2) Armoured","m","Contracted is split in 3 different items ",0,null,{"v":8.190586872113624,"d":"R 8.19"},null,null,0,0,0]
[null,"GLANDS & SHROUDS"]
[10,"No.1 Gland & Shroud (4ECV)","ea","Armour Glands No. 1 and Shroud ",0,null,{"v":174.7073832005137,"d":"R 174.71"},null,null,0,0,0]
[11,"No.2 Gland & Shroud (12DCV)","ea","Armour Glands No. 2 and Shroud ",0,null,{"v":214.65270765486656,"d":"R 214.65"},null,null,0,0,0]
[12,"No.3 Gland & Shroud (19DCV)","ea","Armour Glands No. 3 and Shroud ",0,null,{"v":385.0061783995509,"d":"R 385.01"},null,null,0,0,0]
[null,"MISCELLANEOUS"]
[13,"Terminal - Klippon RSF 1","ea","Klippon terminals",0,null,{"v":36.678233450768936,"d":"R 36.68"},null,null,0,0,0]
[14,"Mounting Rail - Klippon TS32 (2M)","ea","Not Included in Contract ",0,null,{"v":35.94,"d":"R 35.94"},null,null,0,0,0]
[15,"Terminal Fuse - Klippon","ea","Not Included in Contract ",0,null,{"v":35.94,"d":"R 35.94"},null,null,0,0,0]
[16,"RS 485 cable (with SWA)","m","4 Pair Belden Cable (Armoured RS 485)",0,null,{"v":6.983612497582084,"d":"R 6.98"},null,null,0,0,0]
[17,"Installation accessories (eg, lugs, cable markers, cable ties, bandit straps etc)","lot","Not Included in Contract ",0,null,{"v":1500,"d":"R 1,500.00"},null,null,0,0,0]
[18,"Labels (for panels, junction boxes etc)","lot","Not Included in Contract ",0,null,{"v":1500,"d":"R 1,500.00"},null,null,0,0,0]
[null,"DECOMMISION AND REMOVALOF OLD CABLE"]
[1,"4 Core - 2.5mm (no.1) Armoured","m","4 Core - 2.5mm (no.1) Armoured",0,null,{"v":11.432053632532106,"d":"R 11.43"},null,null,0,0,0]
[2,"4 Core - 4mm (no.1) Armoured","m","4 Core - 4mm (no.1) Armoured",0,null,{"v":12.260452477246314,"d":"R 12.26"},null,null,0,0,0]
[3,"4 Core - 16mm (no.2) Armoured","m","4 Core - 16mm (no.2) Armoured",0,null,{"v":11.246580042262057,"d":"R 11.25"},null,null,0,0,0]
[4,"4 Core - 35mm (no.3) Armoured","m","Not Included in Contract ",0,null,{"v":25,"d":"R 25.00"},null,null,0,0,0]
[5,"12 Core - 2.5mm (no.2) Armoured","m","12 Core - 2.5mm (no.2) Armoured",0,null,{"v":11.342806931837647,"d":"R 11.34"},null,null,0,0,0]
[6,"19 Core 2.5mm (no.3) Armoured","m","19 Core 2.5mm (no.3) Armoured",null,null,{"v":11.171293719329862,"d":"R 11.17"},null,null,0,0,0]
[7,"10 Pair - 0.6mm (no.1) Armoured","m","10 Pair - 0.6mm (no.1) Armoured",null,null,{"v":11.789507858672518,"d":"R 11.79"},null,null,0,0,0]
[8,"25 Pair - 0.6mm (no.1) Armoured","m","25 Pair - 0.6mm (no.1) Armoured",0,null,{"v":11.848309717684545,"d":"R 11.85"},null,null,0,0,0]
[9,"50 Pair - 0.6mm (no.2) Armoured",null,"50 Pair - 0.6mm (no.2) Armoured",null,null,{"v":13.765119442935084,"d":"R 13.77"},null,null,0,0,0]
[null,"Total of the Prices excluding VAT","R",{"$nulls":6},{"$f":"SUM(J9:J62)","v":0},{"$f":"SUM(K9:K62)","v":0},{"$f":"SUM(L9:L62)","v":0}]
[]
[]
[]
[null,"COMPILED BY","SIGNATURE",{"$nulls":6},"DATE"]
[]
[null,"CHECKED","SIGNATURE",{"$nulls":6},"DATE"]
[]
[null,"SENIOR ELECTRICAL ENGINEER","SIGNATURE",{"$nulls":6},"DATE"]
[]
[null,"QUANTITY SURVEY","SIGNATURE",{"$nulls":6},"DATE"]

{"sheet":"SECTION L OTHER ","index":13,"n_rows":30,"n_cols":11,"rows_kept":30,"merged":[[0,0,0,10],[1,0,1,1],[1,2,1,3],[1,7,1,8],[1,9,1,10],[2,0,2,1],[2,2,2,3],[2,7,2,8],[2,9,2,10],[3,0,3,1],[3,2,3,3],[3,7,3,8],[3,9,3,10],[4,0,4,1],[4,2,4,3],[5,0,5,7],[6,0,6,7],[7,4,7,5],[7,6,7,7],[7,8,7,9],[7,10,8,10],[10,1,10,10],[11,1,11,2],[27,7,27,8],[28,7,28,8],[29,7,29,8]]}
["GEMMA CLUSTER"]
["Project Name:",{"$nulls":6},"Template Identifier:"]
["Project ID:",{"$nulls":6},"Effective Date:"]
["Job Name:",{"$nulls":6},"Review Date:"]
["Job ID:"]
["SCHEDULE OF QUANTITIES - SECTION L"]
["OTHER ADDITIONAL ACTIVITIES"]
["Item","Reference","Description of the item","Unit","Qty",null,"Rates",null,"Totals",null,"Price (R)"]
[{"$nulls":4},"Supply","Install","Supply","Install","Supply","Install"]
["M1",null,"Additional Items"]
[null,"Add any other additional activities "]
[]
["M1.1"]
["M1.2"]
["M1.3"]
["M1.4"]
["M1.5"]
["M1.6"]
["M1.7"]
["M1.8"]
["M1.9"]
["M1.10"]
["M1.11"]
["M1.12"]
["M1.13"]
["M1.14"]
["Subtotal carried to Item M  of Summary"]
[{"$nulls":7},"Please initial"]
[{"$nulls":7},"Compiler/Designer:"]
[{"$nulls":7},"Quantity Surveyor"]