{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Schedules A&B 0241918 ","Deviation Schedule","Test Report Schedule"],"read":"whole","date_system":"1900"}

{"sheet":"Schedules A&B 0241918 ","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"merged":[[0,0,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,1,4,6],[7,2,7,3],[8,2,8,3],[9,3,9,4],[18,3,18,4],[21,3,21,4],[26,3,26,4],[30,2,30,4],[31,2,31,4],[34,3,34,4],[40,2,40,4],[43,1,43,6],[45,0,45,6],[46,0,46,6],[48,0,48,1],[53,2,53,3]]}
["ESKOM TENDER E2719DXLIMOU"]
[null,"Technical Schedules A and B for"]
[null,"WASHER,SPRING M20  D3014"]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"SAP No",null,"Eskom SAP No: 0241918","xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer",null,"xxxxxxxxxx"]
[null,"1.1.3",null,"Manufacturer's Product Code",null,"xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Drawing number & Revision number",null,"xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's Physical identification mark on product",null,"xxxxxxxxxx"]
[null,"1.1.6",null,"Compliance to all dimensions AND REQUIREMENTS of Eskom Buyer's Guide Drawings",null,"Eskom D-DT-3014"]
[null,"1.1.7",null,"Item sample required, upon request from Eskom. (As per the Technical Criteria Document)",null,"YES","xxxxxxxxxx"]
[]
[null,1.2,"·","Mechanical Properties"]
[null,"1.2.2",null,"Material Grade",null,"S355JR"]
[]
[null,1.3,"·","Dimension"]
[null,"1.3.1",null,"Thickness (s)","mm","4.5  +0.2"]
[null,"1.3.2",null,"Height (h)","mm","9.0   8.25"]
[null,"1.3.3",null,"Bolt hole diameter (d1)","mm","20.2 +1.0"]
[null,"1.3.4",null,"Overall diameter (d2)","mm","30.6"]
[]
[null,1.4,"·","Galvanising (where applicalbe)"]
[null,"1.4.1",null,"Average minimum galvanising thickness on product body to SANS 121",null,"YES"]
[]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to be provided in electronic format."]
[null,2.1,"·","General"]
[null,"2.1.1",null,"Outline drawings of item","Sets",1]
[null,"2.1.2",null,"Material grade certification",null,"YES"]
[null,2.2,"·","Test Reports (where applicable)",null,"Required","Report\nNumber"]
[null,"2.2.1",null,"Verification of general dimensions",null,"YES"]
[null,"2.2.2",null,"Verification of material type & hardness",null,"YES"]
[null,"2.2.3",null,"Galvanising certificate of product body",null,"YES"]
[]
[null,3,"Packaging"]
[null,3.1,"·","Packaging material, method and maximum quantity, not exceeding 50 units or 800kg (as per clause 4.18 of Eskom 240-60777474)","Wooden Boxes, Crates or Pallets, Hessian / Cloth Bags ","YES"]
[]
[null,"NOTE:  DEVIATION SCHEDULE CONTINUE ON NEXT PAGE.\n             IF NO DEVIATIONS ARE MENTIONED ON THE DEVIATION SCHEDULE IT WILL BE ACCEPTED\n             THAT THE SUPPLIER AND MANUFACTURER FULLY COMPLIES WITH THE REQUIREMENTS OF\n             THE ESKOM SPECIFICATON(S)."]
[]
["ESKOM TENDER E2719DXLIMOU"]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,null,"Company Name"]
[]
[]
[]
[null,null,"Sign",{"$nulls":3},"Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":47,"n_cols":7,"rows_kept":47,"merged":[[0,0,0,6],[1,0,1,6],[3,0,3,6],[4,2,4,6],[5,2,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[34,2,34,6],[36,0,36,6],[39,0,39,1],[40,0,40,1],[42,0,42,1],[43,0,43,1],[45,0,45,1],[46,0,46,1]]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation Schedule  -  WASHER,SPRING M20  D3014"]
[null,null,"Eskom SAP No: 0241918"]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":31}
["ESKOM TENDER E2719DXLIMOU"]
["SIGNATURES"]
[]
["Supplier"]
[null,null,"Name (Print)",null,"Sign",null,"Date"]
[]
["Manufacture"]
[null,null,"Name (Print)",null,"Sign",null,"Date"]
[]
["Eskom"]
[null,null,"Name (Print)",null,"Sign",null,"Date"]

{"sheet":"Test Report Schedule","index":2,"n_rows":26,"n_cols":7,"rows_kept":26,"merged":[[0,0,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[5,1,5,6],[14,1,14,3],[17,0,17,6],[18,0,18,7],[21,0,21,3],[21,6,21,7],[25,0,25,3],[25,6,25,7]]}
["ESKOM TENDER E2719DXLIMOU"]
[null,"Test Report Schedule"]
[null,"WASHERS, D3014"]
[null,"Below test requirements, and compliance, in accordance with SANS 1700 (Specification for Fasteners) and D-DT-3014"]
[{"$nulls":5},"SANS 61284"]
[]
[null,1,null,2,null,3,4]
[null,"Item ",null,"Description","Test","Specification","Report No."]
[null,1,null,"Visual examination","Type","SANS 1700"]
[null,2,null,"Dimensional and material verification","Type","SANS 61284 & SANS 1700 & D-DT-3014","xxxxxxxxxx"]
[null,2.1,null,"Dimensions","Type","D-DT-3014 & SANS 1700"]
[null,"2.2.",null,"Verification of material type and hardness","Type","SANS 61284 & SANS 1700 ","xxxxxxxxxx"]
[null,3,null,"Hot Dip Galvanising certificate of product body","Sample","SANS 121"]
[]
[]
[]
[]
["ESKOM TENDER E2719DXLIMOU"]
["SUPPLIER SIGNATURES"]
[]
["         "]
["Name (Print)",{"$nulls":5},"Company Name"]
[]
[]
[]
["Sign",{"$nulls":5},"Date"]