{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Refractory Materials ","Sheet1"],"not_rendered":{"comments":2},"read":"whole","date_system":"1900"}

{"sheet":"Refractory Materials ","index":0,"n_rows":20,"n_cols":7,"rows_kept":20}
[]
["FURNACE TYPE","CONSUMABLES FOR SMELTER","Specification ","MONTHLY CONSUMPTION (as and when required)**","12 MONTHS CONSUMPTION (as and when required)**","Item quantities/Description","Industry"]
[]
["Test Smelter Furnace","Refractory lining material","Alumina Spinel ",4,{"$f":"+D4*12","v":48},"bag","Refractory suppliers"]
["Test Smelter Furnace","Refractory lining material installation (labour)","Labour",1,{"$f":"+D5*12","v":12},"labour - 1 day","Refractory suppliers"]
["Test Smelter Furnace","Coil Grout material ","Alumina Special Induction Coil refractory",25,300,"bags","Refractory suppliers"]
["Test Smelter Furnace","Coil Grout installation (labour )","Labour ",1,12,"labour - 1 day","Refractory suppliers"]
["Test Smelter Furnace","Steel former (made of carbon/mild steel)","Steel former for a 125kg induction furnace (made of carbon/mild steel)",1,12,"former","Refractory suppliers"]
["4 ton Furnace Ferrous Metals","Refractory lining material","Alumina Spinel ",2125,{"$f":"+D9*12","v":25500},"Mass in kg -bags","Refractory suppliers"]
["4 ton Furnace Ferrous Metals","Refractory lining material installation (labour)","Labour",1,12,"labour","Refractory suppliers"]
["4 ton Furnace Ferrous Metals","Coil Grout material","Alumina Special Induction Coil refractory",500,6000,"Mass in kg - bags","Refractory suppliers"]
["4 ton Furnace Ferrous Metals","Castable refractory lining materials for lining the 4 ton ladle","Quick cast 62 ZA",{"$f":"1525*2","v":3050},36600,"Mass in kg -bags","Refractory suppliers"]
["4 ton Furnace Ferrous Metals","Custable refractory lining materials for lining 1 ton ladle","Quick cast 62 ZA",{"$f":"325*2","v":650},7800,"Mass in kg -bags","Refractory suppliers"]
["4 ton Furnace Ferrous Metals","Steel former   (made of carbon/mild steel)","Steel former for a 4 ton furnace induction furnace (made of carbon/mild steel)",1,12,"Former  ","Refractory suppliers"]
["4 ton Furnace Non-Ferrous","Refractory lining material","Magnesia–chrome (MgCr2O4",2125,25500,"Mass in kg -bags","Refractory suppliers"]
["4 ton Furnace Non-Ferrous","Refractory lining material installation (labour)","Labour",1,12,"labour","Refractory suppliers"]
["4 ton Furnace Non-Ferrous","Coil Grout material","Alumina Special Induction Coil refractory",500,{"$f":"+D17*12","v":6000},"Mass in kg - bags","Refractory suppliers"]
["4 ton Furnace Non-Ferrous","Castable refractory lining materials for lining the 4 ton ladle","Quick cast 62 ZA",1,12,"LABOUR AND MIXING EQUIPMENT ONLY","Refractory suppliers"]
["4 ton Furnace Non-Ferrous","Custable refractory lining materials for lining 1 ton ladle","Quick cast 62 ZA",1,12,"LABOUR AND MIXING EQUIPMENT ONLY","Refractory suppliers"]
["4 ton Furnace Non-Ferrous","Steel former (made of carbon/mild steel)","Steel former for a 4 ton furnace induction furnace (made of carbon/mild steel)",1,12,"Former  ","Refractory suppliers"]

{"sheet":"Sheet1","index":1,"n_rows":107,"n_cols":10,"rows_kept":107,"hidden":true}
[]
["FURNACE TYPE",null,"CONSUMABLES FOR SMELTER","MONTHLY CONSUMPTION (as and when required)**","36 MONTHS CONSUMPTION (as and when required)**","Price per unit ","Total price per month ","Total cost  for 36 months ","Item quantities/Description","Industry"]
[{"$nulls":9},"Refractory suppliers"]
["Test Smelter Furnace",1,"Refractory lining material",4,{"$f":"+D4*36","v":144},{"$f":"15000/D4","v":{"v":3750,"d":"R3,750.00"}},{"v":15000,"d":"R15,000.00"},{"$f":"G4*36","v":{"v":540000,"d":"R540,000.00"}},"bag","Refractory suppliers"]
[null,2,"Refractory lining material installation (labour)",1,{"$f":"+D5*36","v":36},{"v":8652,"d":"R8,652.00"},{"$f":"F5*D5","v":{"v":8652,"d":"R8,652.00"}},{"v":311472,"d":"R311,472.00"},"labour - 1 day","Refractory suppliers"]
[null,3,"Coil Grout material ",25,{"$f":"+D6*36","v":900},{"v":44.72,"d":"R44.72"},{"$f":"F6*D6","v":{"v":1118,"d":"R1,118.00"}},{"v":40248,"d":"R40,248.00"},"bags","Refractory suppliers"]
[null,4,"Coil Grout installation (labour )",1,{"$f":"+D7*36","v":36},{"v":8652,"d":"R8,652.00"},{"$f":"F7*D7","v":{"v":8652,"d":"R8,652.00"}},{"v":311472,"d":"R311,472.00"},"labour - 1 day","Refractory suppliers"]
[null,5,"Steel former (made of carbon/mild steel)",1,{"$f":"+D8*36","v":36},{"v":4390,"d":"R4,390.00"},{"$f":"F8*D8","v":{"v":4390,"d":"R4,390.00"}},{"v":158040,"d":"R158,040.00"},"former","Refractory suppliers"]
[null,6,"Electrode panels(SAVEWAY ELECTRODE PANEL SET. 125KG TEST FURNACE. 3 PER SET (1xB-PANEL, 2xC-PANELS,H:470)",1,{"$f":"+D9*36","v":36},{"v":9816.86,"d":"R9,816.86"},{"$f":"F9*D9","v":{"v":9816.86,"d":"R9,816.86"}},{"v":353406.96,"d":"R353,406.96"}," 3 PER SET (1xB-PANEL","Sole supplier (Saveway)"]
[null,7,"SAVEWAY TECHNICIAN. NORMAL HOURS. 865t1 (labour)",1,{"$f":"D10*36","v":36},{"v":650,"d":"R650.00"},{"$f":"650*8*2","v":{"v":10400,"d":"R10,400.00"}},{"$f":"G10*36","v":{"v":374400,"d":"R374,400.00"}},"labour","Sole supplier (Saveway)"]
[null,8,"Earth detector/Spider",1,36,{"v":1500,"d":"R1,500.00"},{"v":1500,"d":"R1,500.00"},{"$f":"G11*36","v":{"v":54000,"d":"R54,000.00"}},"spider (Per furnace reline )","Sole supplier (Saveway)"]
[null,9,"Copper coil",1,1,{"v":100000,"d":"R100,000.00"},{"$f":"F12*D12","v":{"v":100000,"d":"R100,000.00"}},{"$f":"+G12","v":{"v":100000,"d":"R100,000.00"}},"coil (once-off purchase)","Furnace supliers"]
[null,10,"Thermocouple S-Type",4,{"$f":"+D13*36","v":144},{"v":5200,"d":"R5,200.00"},{"v":20800,"d":"R20,800.00"},{"v":748800,"d":"R748,800.00"},"thermocouple","Instrumentation suppliers"]
[null,11,"Thermocouple K-Type",4,{"$f":"+D14*36","v":144},{"v":639,"d":"R639.00"},{"v":2556,"d":"R2,556.00"},{"v":92016,"d":"R92,016.00"},"thermocouple","Instrumentation suppliers"]
[null,12,"Thermocouple S-Type 2 meter extention cables",4,{"$f":"+D15*36","v":144},{"v":159,"d":"R159.00"},{"$f":"F15*D15","v":{"v":636,"d":"R636.00"}},{"$f":"G15*36","v":{"v":22896,"d":"R22,896.00"}},"Cables","Instrumentation suppliers"]
[null,13,"Thermocouple K-Type 2 meter extention cables",4,{"$f":"+D16*36","v":144},{"v":149,"d":"R149.00"},{"v":596,"d":"R596.00"},{"v":21456,"d":"R21,456.00"},"Cables","Instrumentation suppliers"]
[null,14,"Steel former (made of carbon/mild steel)",1,36,{"v":11087,"d":"R11,087.00"},{"$f":"+F17","v":{"v":11087,"d":"R11,087.00"}},{"$f":"+G17*E17","v":{"v":399132,"d":"R399,132.00"}},"former","Refractory suppliers"]
[]
[]
["4 ton Furnace Ferrous Metals",1,"Refractory lining material",2125,{"$f":"+D20*36","v":76500},{"v":34.2,"d":"R34.20"},{"$f":"F20*D20","v":{"v":72675,"d":"R72,675.00"}},{"$f":"G20*36","v":{"v":2616300,"d":"R2,616,300.00"}},"Mass in kg -bags","Refractory suppliers"]
[null,2,"Refractory lining material installation (labour)",1,{"$f":"+D21*36","v":36},{"v":24636,"d":"R24,636.00"},{"$f":"F21*D21","v":{"v":24636,"d":"R24,636.00"}},{"$f":"G21*36","v":{"v":886896,"d":"R886,896.00"}},"labour","Refractory suppliers"]
[null,3,"Coil Grout material",500,{"$f":"+D22*36","v":18000},{"v":44.72,"d":"R44.72"},{"$f":"F22*D22","v":{"v":22360,"d":"R22,360.00"}},{"$f":"G22*36","v":{"v":804960,"d":"R804,960.00"}},"Mass in kg - bags","Refractory suppliers"]
[null,4,"Refractory lining installation for 4 ton  ladle (labour)",1,36,{"v":36954,"d":"R36,954.00"},{"$f":"F23*D23","v":{"v":36954,"d":"R36,954.00"}},{"$f":"G24*36","v":{"v":556200,"d":"R556,200.00"}},"LABOUR AND MIXING EQUIPMENT ONLY","Refractory suppliers"]
[null,5,"Refractory lining installation for 1 tons  ladle (labour)",1,36,{"v":15450,"d":"R15,450.00"},{"$f":"F24*D24","v":{"v":15450,"d":"R15,450.00"}},{"$f":"G23*36","v":{"v":1330344,"d":"R1,330,344.00"}},"LABOUR AND MIXING EQUIPMENT ONLY","Refractory suppliers"]
[null,6,"Steel former (made of carbon/mild steel)",1,36,{"v":38912,"d":"R38,912.00"},{"$f":"F25*D25","v":{"v":38912,"d":"R38,912.00"}},{"v":1400832,"d":"R1,400,832.00"},"Former  ","Refractory suppliers"]
[null,7,"SAVEWAY ELECTRODE PANEL SET. 4T PILLAR FURNACE. 7 PER SET (7xA-PANELS. H:1400)",1,{"$f":"D26*36","v":36},{"v":44854.4,"d":"R44,854.40"},{"$f":"F26*D26","v":{"v":44854.4,"d":"R44,854.40"}},{"$f":"G26*36","v":{"v":1614758.4000000001,"d":"R1,614,758.40"}},"Set = Each(Use for every reline)","Sole supplier (Saveway)"]
[null,8,"SAVEWAY FOIL:RF 4;25MX1MX0.42MM;PGP0042 25m/1x1000mm",1,{"$f":"D27*36","v":36},{"v":27163.90827130532,"d":"R27,163.91"},{"v":27163.90827130532,"d":"R27,163.91"},{"$f":"G27*36","v":{"v":977900.6977669916,"d":"R977,900.70"}},"Roll = 25m(Minor amount utilised per reline)","Sole supplier (Saveway)"]
[null,9,"SAVEWAY FOIL:RF 4;25MX500MMX0.42MM;PGP0042 25m/2x500mm",1,36,{"v":27571.3668953749,"d":"R27,571.37"},{"v":27571.3668953749,"d":"R27,571.37"},{"v":992569.2082334964,"d":"R992,569.21"},"Roll = 25m(Minor amount utilised per reline)","Sole supplier (Saveway)"]
[null,10,"SAVEWAY FOIL:RF 4;25MX330X0.42MM;PGP0042 25m/3x330mm",1,36,{"v":27978.825519444483,"d":"R27,978.83"},{"v":27978.825519444483,"d":"R27,978.83"},{"$f":"G29*36","v":{"v":1007237.7187000014,"d":"R1,007,237.72"}},"Roll = 25m(Minor amount utilised per reline)","Sole supplier (Saveway)"]
[null,11,"SAVEWAY SILICONE: E-PANEL; 300ML TUBE. 701",1,36,{"v":8717.907383343756,"d":"R8,717.91"},{"v":8717.907383343756,"d":"R8,717.91"},{"v":313844.6658003752,"d":"R313,844.67"},"Box = 20 tubes(Use for every reline)","Sole supplier (Saveway)"]
[null,12,"SAVEWAY GREASE:CERAMIC,ANTI-SEIZE;500ML;CAN. 2202",1,36,{"v":3415.8626064546743,"d":"R3,415.86"},{"v":3415.8626064546743,"d":"R3,415.86"},{"v":122971.05383236827,"d":"R122,971.05"},"Each(Minor amount utilised per reline)","Sole supplier (Saveway)"]
[null,13,"SAVEWAY BOLT,MACHINE:SS;II M12 X 35, 18-8 SS. 586",1,36,{"v":207.37111119854424,"d":"R207.37"},{"v":207.37111119854424,"d":"R207.37"},{"v":7465.360003147593,"d":"R7,465.36"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,14,"SAVEWAY WASHER, LOCK:12d=12.5MM A2. 587",1,36,{"v":18.492285319700606,"d":"R18.49"},{"v":18.492285319700606,"d":"R18.49"},{"v":665.7222715092219,"d":"R665.72"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,15,"SAVEWAY NUT, HEX: M12 A2. 588",1,36,{"v":25.66276330080901,"d":"R25.66"},{"v":25.66276330080901,"d":"R25.66"},{"v":923.8594788291244,"d":"R923.86"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,16,"SAVEWAY NUT, CAP: M12 A2. 589",1,36,{"v":113.18452729010406,"d":"R113.18"},{"v":113.18452729010406,"d":"R113.18"},{"v":4074.642982443746,"d":"R4,074.64"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,17,"SPACER: PIECE; 8 X 8 X 1.6MM; BRASS. 593",1,36,{"v":46.22924384558401,"d":"R46.23"},{"v":46.22924384558401,"d":"R46.23"},{"v":1664.2527784410242,"d":"R1,664.25"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,18,"SAVEWAY STUD: CONNECTING; TYPE 2; W/3M WIRE. 1428",1,36,{"v":3918.7956209507815,"d":"R3,918.80"},{"v":3918.7956209507815,"d":"R3,918.80"},{"v":141076.64235422813,"d":"R141,076.64"},"Each(Supplied with Rim Blocks)","Sole supplier (Saveway)"]
[null,19,"SAVEWAY STUD:CONNECTING; TYPE 2; W/5M WIRE. 1315",1,36,{"v":4597.126763520848,"d":"R4,597.13"},{"v":4597.126763520848,"d":"R4,597.13"},{"v":165496.56348675053,"d":"R165,496.56"},"Each(For future emergency use)","Sole supplier (Saveway)"]
[null,20," SAVEWAY MOLD: STYROFOAM. 4555",1,36,{"v":213.51767105848188,"d":"R213.52"},{"v":213.51767105848188,"d":"R213.52"},{"v":7686.636158105348,"d":"R7,686.64"},"Each(Supplied with Rim Blocks)","Sole supplier (Saveway)"]
[null,21,"SAVEWAY NUT, HEX: EXTENDED; RIM BLOCK LUGS. MECH_001",1,36,{"v":18.816683485618846,"d":"R18.82"},{"v":18.816683485618846,"d":"R18.82"},{"v":677.4006054822785,"d":"R677.40"},"Each(Supplied with Rim Blocks)","Sole supplier (Saveway)"]
[null,22,"SAVEWAY SILICONE: CASTING; 310ML TUBE. MECH_002",1,36,{"v":161.64980759479963,"d":"R161.65"},{"v":161.64980759479963,"d":"R161.65"},{"v":5819.393073412786,"d":"R5,819.39"},"Each(Used for Rim Blocks)","Sole supplier (Saveway)"]
[null,23,"SAVEWAY CONE: FOR CONNECTING STUD TYPE II. 594",1,36,{"v":551.0077542041637,"d":"R551.01"},{"v":551.0077542041637,"d":"R551.01"},{"v":19836.279151349892,"d":"R19,836.28"},"Each(Used for Rim Blocks)","Sole supplier (Saveway)"]
[null,24,"SAVEWAY SCREW: M12 X 50MM; HEXAGON HEAD. 595",1,36,{"v":26.540149887047686,"d":"R26.54"},{"v":26.540149887047686,"d":"R26.54"},{"v":955.4453959337167,"d":"R955.45"},"Each(Used for Rim Blocks)","Sole supplier (Saveway)"]
[null,25,"SAVEWAY WASHER, FLAT: M12. 964",1,36,{"v":7.416183727302688,"d":"R7.42"},{"v":7.416183727302688,"d":"R7.42"},{"v":266.9826141828968,"d":"R266.98"},"Each(Used for Rim Blocks)","Sole supplier (Saveway)"]
[null,26,"SAVEWAY TERMINAL BOX, ALUMINUM, ALU UNPAINT. 230x280x110mm.",1,36,{"v":2859.27,"d":"R2,859.27"},{"v":2859.27,"d":"R2,859.27"},{"v":102933.72,"d":"R102,933.72"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,27,"SAVEWAY BLADE Terminal 4mm triple top grey",1,36,{"v":93.53,"d":"R93.53"},{"v":93.53,"d":"R93.53"},{"v":3367.08,"d":"R3,367.08"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,28,"SAVEWAY JUNCTION BOX LID: 163x100x12mm GP03",1,36,{"v":1331.16,"d":"R1,331.16"},{"v":1331.16,"d":"R1,331.16"},{"v":47921.76,"d":"R47,921.76"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,29,"SAVEWAY JUNCTION BOX: 163x100x75mm GP03",1,36,{"v":2515.83,"d":"R2,515.83"},{"v":2515.83,"d":"R2,515.83"},{"v":90569.88,"d":"R90,569.88"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,30,"SAVEWAY JUNCTION BOX LID: 283x183x12mm GP03",1,36,{"v":1684.67,"d":"R1,684.67"},{"v":1684.67,"d":"R1,684.67"},{"v":60648.12,"d":"R60,648.12"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,31,"SAVEWAY JUNCTION BOX: 283x183x75mm GP03",1,36,{"v":6130.59,"d":"R6,130.59"},{"v":6130.59,"d":"R6,130.59"},{"v":220701.24,"d":"R220,701.24"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,32,"SAVEWAY TECHNICIAN. NORMAL HOURS. 865t1",1,36,{"v":650,"d":"R650.00"},{"$f":"F51*9*2","v":{"v":11700,"d":"R11,700.00"}},{"v":421200,"d":"R421,200.00"},"Each(As Hoc)","Sole supplier (Saveway)"]
[null,33,"Earth detector/Spider",2,{"$f":"+D52*36","v":72},{"v":3000,"d":"R3,000.00"},{"v":3000,"d":"R3,000.00"},{"$f":"G52*36","v":{"v":108000,"d":"R108,000.00"}},null,"Sole supplier (Saveway)"]
[null,34,"Copper coil",1,1,{"v":2000000,"d":"R2,000,000.00"},{"v":2000000,"d":"R2,000,000.00"},{"$f":"+G53","v":{"v":2000000,"d":"R2,000,000.00"}},"coil (once-off purchase)","Furnace supliers"]
[null,35,"Thermocouple S-Type",4,{"$f":"+D54*36","v":144},{"v":20000,"d":"R20,000.00"},{"$f":"D54*F54","v":{"v":80000,"d":"R80,000.00"}},{"$f":"G54*36","v":{"v":2880000,"d":"R2,880,000.00"}},"thermocouple","Instrumentation suppliers"]
[null,36,"Thermocouple K-Type",4,144,{"v":10000,"d":"R10,000.00"},{"$f":"D55*F55","v":{"v":40000,"d":"R40,000.00"}},{"$f":"G55*36","v":{"v":1440000,"d":"R1,440,000.00"}},"thermocouple","Instrumentation suppliers"]
[null,37,"Thermocouple S-Type 10 meter extention cables",4,144,{"v":1000,"d":"R1,000.00"},{"v":4000,"d":"R4,000.00"},{"v":144000,"d":"R144,000.00"},"Cables","Instrumentation suppliers"]
[null,38,"Thermocouple K-Type 10 meter extention cables",4,144,{"v":1000,"d":"R1,000.00"},{"v":4000,"d":"R4,000.00"},{"v":144000,"d":"R144,000.00"},"Cables","Instrumentation suppliers"]
[]
["4 ton Furnace Non-Ferrous",1,"Refractory lining material",2125,{"$f":"+D59*36","v":76500},{"v":34.2,"d":"R34.20"},{"$f":"F59*D59","v":{"v":72675,"d":"R72,675.00"}},{"$f":"G59*36","v":{"v":2616300,"d":"R2,616,300.00"}},"Mass in kg -bags","Refractory suppliers"]
[null,2,"Refractory lining material installation (labour)",1,{"$f":"+D60*36","v":36},{"v":24636,"d":"R24,636.00"},{"$f":"F60*D60","v":{"v":24636,"d":"R24,636.00"}},{"$f":"G60*36","v":{"v":886896,"d":"R886,896.00"}},"labour","Refractory suppliers"]
[null,3,"Coil Grout material",500,{"$f":"+D61*36","v":18000},{"v":44.72,"d":"R44.72"},{"$f":"F61*D61","v":{"v":22360,"d":"R22,360.00"}},{"$f":"G61*36","v":{"v":804960,"d":"R804,960.00"}},"Mass in kg - bags","Refractory suppliers"]
[null,4,"Refractory lining installation for 4 ton  ladle (labour)",1,36,{"v":36954,"d":"R36,954.00"},{"$f":"F62*D62","v":{"v":36954,"d":"R36,954.00"}},{"$f":"G63*36","v":{"v":556200,"d":"R556,200.00"}},"LABOUR AND MIXING EQUIPMENT ONLY","Refractory suppliers"]
[null,5,"Refractory lining installation for 1 tons  ladle (labour)",1,36,{"v":15450,"d":"R15,450.00"},{"$f":"F63*D63","v":{"v":15450,"d":"R15,450.00"}},{"$f":"G62*36","v":{"v":1330344,"d":"R1,330,344.00"}},"LABOUR AND MIXING EQUIPMENT ONLY","Refractory suppliers"]
[null,6,"Steel former (made of carbon/mild steel)",1,36,{"v":38912,"d":"R38,912.00"},{"$f":"F64*D64","v":{"v":38912,"d":"R38,912.00"}},{"$f":"G64*36","v":{"v":1400832,"d":"R1,400,832.00"}},"Former  ","Refractory suppliers"]
[null,7,"SAVEWAY ELECTRODE PANEL SET. 4T PILLAR FURNACE. 7 PER SET (7xA-PANELS. H:1400)",1,{"$f":"D65*36","v":36},{"v":44854.4,"d":"R44,854.40"},{"$f":"F65*D65","v":{"v":44854.4,"d":"R44,854.40"}},{"$f":"G65*36","v":{"v":1614758.4000000001,"d":"R1,614,758.40"}},"Set = Each(Use for every reline)","Sole supplier (Saveway)"]
[null,8,"SAVEWAY FOIL:RF 4;25MX1MX0.42MM;PGP0042 25m/1x1000mm",1,{"$f":"D66*36","v":36},{"v":27163.90827130532,"d":"R27,163.91"},{"v":27163.90827130532,"d":"R27,163.91"},{"$f":"G66*36","v":{"v":977900.6977669916,"d":"R977,900.70"}},"Roll = 25m(Minor amount utilised per reline)","Sole supplier (Saveway)"]
[null,9,"SAVEWAY FOIL:RF 4;25MX500MMX0.42MM;PGP0042 25m/2x500mm",1,36,{"v":27571.3668953749,"d":"R27,571.37"},{"v":27571.3668953749,"d":"R27,571.37"},{"v":992569.2082334964,"d":"R992,569.21"},"Roll = 25m(Minor amount utilised per reline)","Sole supplier (Saveway)"]
[null,10,"SAVEWAY FOIL:RF 4;25MX330X0.42MM;PGP0042 25m/3x330mm",1,36,{"v":27978.825519444483,"d":"R27,978.83"},{"v":27978.825519444483,"d":"R27,978.83"},{"$f":"G68*36","v":{"v":1007237.7187000014,"d":"R1,007,237.72"}},"Roll = 25m(Minor amount utilised per reline)","Sole supplier (Saveway)"]
[null,11,"SAVEWAY SILICONE: E-PANEL; 300ML TUBE. 701",1,36,{"v":8717.907383343756,"d":"R8,717.91"},{"v":8717.907383343756,"d":"R8,717.91"},{"$f":"G69*36","v":{"v":313844.6658003752,"d":"R313,844.67"}},"Box = 20 tubes(Use for every reline)","Sole supplier (Saveway)"]
[null,12,"SAVEWAY GREASE:CERAMIC,ANTI-SEIZE;500ML;CAN. 2202",1,36,{"v":3415.8626064546743,"d":"R3,415.86"},{"v":3415.8626064546743,"d":"R3,415.86"},{"v":122971.05383236827,"d":"R122,971.05"},"Each(Minor amount utilised per reline)","Sole supplier (Saveway)"]
[null,13,"SAVEWAY BOLT,MACHINE:SS;II M12 X 35, 18-8 SS. 586",1,36,{"v":207.37111119854424,"d":"R207.37"},{"v":207.37111119854424,"d":"R207.37"},{"v":7465.360003147593,"d":"R7,465.36"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,14,"SAVEWAY WASHER, LOCK:12d=12.5MM A2. 587",1,36,{"v":18.492285319700606,"d":"R18.49"},{"v":18.492285319700606,"d":"R18.49"},{"v":665.7222715092219,"d":"R665.72"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,15,"SAVEWAY NUT, HEX: M12 A2. 588",1,36,{"v":25.66276330080901,"d":"R25.66"},{"v":25.66276330080901,"d":"R25.66"},{"v":923.8594788291244,"d":"R923.86"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,16,"SAVEWAY NUT, CAP: M12 A2. 589",1,36,{"v":113.18452729010406,"d":"R113.18"},{"v":113.18452729010406,"d":"R113.18"},{"v":4074.642982443746,"d":"R4,074.64"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,17,"SPACER: PIECE; 8 X 8 X 1.6MM; BRASS. 593",1,36,{"v":46.22924384558401,"d":"R46.23"},{"v":46.22924384558401,"d":"R46.23"},{"v":1664.2527784410242,"d":"R1,664.25"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,18,"SAVEWAY STUD: CONNECTING; TYPE 2; W/3M WIRE. 1428",1,36,{"v":3918.7956209507815,"d":"R3,918.80"},{"v":3918.7956209507815,"d":"R3,918.80"},{"v":141076.64235422813,"d":"R141,076.64"},"Each(Supplied with Rim Blocks)","Sole supplier (Saveway)"]
[null,19,"SAVEWAY STUD:CONNECTING; TYPE 2; W/5M WIRE. 1315",1,36,{"v":4597.126763520848,"d":"R4,597.13"},{"v":4597.126763520848,"d":"R4,597.13"},{"v":165496.56348675053,"d":"R165,496.56"},"Each(For future emergency use)","Sole supplier (Saveway)"]
[null,20," SAVEWAY MOLD: STYROFOAM. 4555",1,36,{"v":213.51767105848188,"d":"R213.52"},{"v":213.51767105848188,"d":"R213.52"},{"v":7686.636158105348,"d":"R7,686.64"},"Each(Supplied with Rim Blocks)","Sole supplier (Saveway)"]
[null,21,"SAVEWAY NUT, HEX: EXTENDED; RIM BLOCK LUGS. MECH_001",1,36,{"v":18.816683485618846,"d":"R18.82"},{"v":18.816683485618846,"d":"R18.82"},{"v":677.4006054822785,"d":"R677.40"},"Each(Supplied with Rim Blocks)","Sole supplier (Saveway)"]
[null,22,"SAVEWAY SILICONE: CASTING; 310ML TUBE. MECH_002",1,36,{"v":161.64980759479963,"d":"R161.65"},{"v":161.64980759479963,"d":"R161.65"},{"v":5819.393073412786,"d":"R5,819.39"},"Each(Used for Rim Blocks)","Sole supplier (Saveway)"]
[null,23,"SAVEWAY CONE: FOR CONNECTING STUD TYPE II. 594",1,36,{"v":551.0077542041637,"d":"R551.01"},{"v":551.0077542041637,"d":"R551.01"},{"v":19836.279151349892,"d":"R19,836.28"},"Each(Used for Rim Blocks)","Sole supplier (Saveway)"]
[null,24,"SAVEWAY SCREW: M12 X 50MM; HEXAGON HEAD. 595",1,36,{"v":26.540149887047686,"d":"R26.54"},{"v":26.540149887047686,"d":"R26.54"},{"v":955.4453959337167,"d":"R955.45"},"Each(Used for Rim Blocks)","Sole supplier (Saveway)"]
[null,25,"SAVEWAY WASHER, FLAT: M12. 964",1,36,{"v":7.416183727302688,"d":"R7.42"},{"v":7.416183727302688,"d":"R7.42"},{"v":266.9826141828968,"d":"R266.98"},"Each(Used for Rim Blocks)","Sole supplier (Saveway)"]
[null,26,"SAVEWAY TERMINAL BOX, ALUMINUM, ALU UNPAINT. 230x280x110mm.",1,36,{"v":2859.27,"d":"R2,859.27"},{"v":2859.27,"d":"R2,859.27"},{"v":102933.72,"d":"R102,933.72"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,27,"SAVEWAY BLADE Terminal 4mm triple top grey",1,36,{"v":93.53,"d":"R93.53"},{"v":93.53,"d":"R93.53"},{"v":3367.08,"d":"R3,367.08"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,28,"SAVEWAY JUNCTION BOX LID: 163x100x12mm GP03",1,36,{"v":1331.16,"d":"R1,331.16"},{"v":1331.16,"d":"R1,331.16"},{"v":47921.76,"d":"R47,921.76"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,29,"SAVEWAY JUNCTION BOX: 163x100x75mm GP03",1,36,{"v":2515.83,"d":"R2,515.83"},{"v":2515.83,"d":"R2,515.83"},{"v":90569.88,"d":"R90,569.88"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,30,"SAVEWAY JUNCTION BOX LID: 283x183x12mm GP03",1,36,{"v":1684.67,"d":"R1,684.67"},{"v":1684.67,"d":"R1,684.67"},{"v":60648.12,"d":"R60,648.12"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,31,"SAVEWAY JUNCTION BOX: 283x183x75mm GP03",1,36,{"v":6130.59,"d":"R6,130.59"},{"v":6130.59,"d":"R6,130.59"},{"v":220701.24,"d":"R220,701.24"},"Each(Replace when needed)","Sole supplier (Saveway)"]
[null,32,"SAVEWAY TECHNICIAN. NORMAL HOURS. 865t1",1,36,{"v":650,"d":"R650.00"},{"$f":"F90*9*2","v":{"v":11700,"d":"R11,700.00"}},{"v":421200,"d":"R421,200.00"},"Each(As Hoc)","Sole supplier (Saveway)"]
[null,33,"Earth detector/Spider",2,{"$f":"+D91*36","v":72},{"v":3000,"d":"R3,000.00"},{"v":3000,"d":"R3,000.00"},{"$f":"G91*36","v":{"v":108000,"d":"R108,000.00"}},null,"Sole supplier (Saveway)"]
[null,34,"Copper coil",1,1,{"v":2000000,"d":"R2,000,000.00"},{"v":2000000,"d":"R2,000,000.00"},{"$f":"+G92","v":{"v":2000000,"d":"R2,000,000.00"}},"coil (once-off purchase)","Furnace supliers"]
[null,35,"Thermocouple S-Type",4,{"$f":"+D93*36","v":144},{"v":20000,"d":"R20,000.00"},{"$f":"D93*F93","v":{"v":80000,"d":"R80,000.00"}},{"$f":"G93*36","v":{"v":2880000,"d":"R2,880,000.00"}},"thermocouple","Instrumentation suppliers"]
[null,36,"Thermocouple K-Type",4,144,{"v":10000,"d":"R10,000.00"},{"$f":"D94*F94","v":{"v":40000,"d":"R40,000.00"}},{"$f":"G94*36","v":{"v":1440000,"d":"R1,440,000.00"}},"thermocouple","Instrumentation suppliers"]
[null,37,"Thermocouple S-Type 10 meter extention cables",4,144,{"v":1000,"d":"R1,000.00"},{"v":4000,"d":"R4,000.00"},{"v":144000,"d":"R144,000.00"},"Cables","Instrumentation suppliers"]
[null,38,"Thermocouple K-Type 10 meter extention cables",4,144,{"v":1000,"d":"R1,000.00"},{"v":4000,"d":"R4,000.00"},{"v":144000,"d":"R144,000.00"},"Cables","Instrumentation suppliers"]
[null,38,"Copper coil",1,{"$f":"+D97*36","v":36},{"v":2000000,"d":"R2,000,000.00"},{"v":2000000,"d":"R2,000,000.00"},{"$f":"G97*36","v":{"v":72000000,"d":"R72,000,000.00"}},"coil (once of purchase)","Furnace supliers"]
[null,39,"Thermocouple S-Type",2,72,{"v":50000,"d":"R50,000.00"},{"v":50000,"d":"R50,000.00"},null,null,"Instrumentation suppliers"]
[null,40,"Thermocouple K-Type",2,72,{"v":2000,"d":"R2,000.00"},{"v":2000,"d":"R2,000.00"},null,null,"Instrumentation suppliers"]
[null,41,"Thermocouple S-Type 10 meter extention cables",2,72,{"v":20000,"d":"R20,000.00"},{"v":20000,"d":"R20,000.00"},null,null,"Instrumentation suppliers"]
[null,42,"Thermocouple K-Type 10 meter extention cables",2,72,{"v":3000,"d":"R3,000.00"},{"v":3000,"d":"R3,000.00"},null,null,"Instrumentation suppliers"]
[]
["Plasma cutter",1,"NST -Hypertherm 125A cutting shield ",1,{"$f":"+D103*36","v":36},{"v":672,"d":"R672.00"},{"$f":"F103*D103","v":{"v":672,"d":"R672.00"}},{"$f":"G103*36","v":{"v":24192,"d":"R24,192.00"}},"Consumable ","Welding & Engineering suppliers"]
[null,2,"NST-HYPERTHERM 125A Retaining Caps ",1,{"$f":"+D104*E105","v":36},{"v":1460,"d":"R1,460.00"},{"$f":"F104*D104","v":{"v":1460,"d":"R1,460.00"}},{"$f":"G104*36","v":{"v":52560,"d":"R52,560.00"}},"Consumable ","Welding & Engineering suppliers"]
[null,3,"NST-Hypertherm 125A cutting nozzles ",1,{"$f":"+D105*36","v":36},{"v":384,"d":"R384.00"},{"v":384,"d":"R384.00"},{"v":13824,"d":"R13,824.00"},"Consumable ","Welding & Engineering suppliers"]
[null,4,"NST -Hypertherm 125A Electrodes PMX",1,{"$f":"+D106*36","v":36},{"v":384,"d":"R384.00"},{"v":384,"d":"R384.00"},{"v":13824,"d":"R13,824.00"},"Consumable ","Welding & Engineering suppliers"]
[null,5,"NST-Hypertherm 125A Swirl Rings ",1,{"$f":"+D107*36","v":36},{"v":840,"d":"R840.00"},{"v":840,"d":"R840.00"},{"v":30240,"d":"R30,240.00"},"Consumable ","Welding & Engineering suppliers"]