{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["PRICING SCHEDULE","Sheet1"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"PRICING SCHEDULE","index":0,"n_rows":77,"n_cols":21,"rows_kept":77,"merged":[[0,0,0,20],[1,2,1,6],[2,2,2,6],[3,1,6,1],[3,2,3,6],[4,2,4,6],[5,2,5,6],[6,2,6,6],[7,2,7,6],[8,1,11,1],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,1,16,1],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,1,26,1],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,1,31,1],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,1,36,1],[33,2,33,6],[34,2,34,6],[35,2,35,6],[36,2,36,6],[37,2,37,6],[38,1,41,1],[38,2,38,6],[39,2,39,6],[40,2,40,6],[41,2,41,6],[42,1,45,1],[42,2,42,6],[43,2,43,6],[44,2,44,6],[45,2,45,6],[46,2,46,6],[47,2,47,6],[48,2,48,6],[49,2,49,6],[50,2,50,6],[51,2,51,6],[52,2,52,6],[53,2,53,6],[54,2,54,6],[55,2,55,6],[56,2,56,6],[57,2,57,6],[58,2,58,6],[59,2,59,6],[60,2,60,6],[61,2,61,6],[62,2,62,6],[63,2,63,6],[64,2,64,6],[65,2,65,6],[66,2,66,6],[67,2,67,6],[68,2,68,6],[69,2,69,6],[70,2,70,6],[71,2,71,6],[72,2,72,6],[73,2,73,6],[74,2,74,6],[75,2,75,6],[76,2,76,6]]}
["RT74-2024 PRICING SCHEDULE"]
["ITEM CODE","PRODUCT DESCRIPTION","ITEM DESCRIPTION",{"$nulls":4},"BIDDER'S NAME","UNIT OF MEASURE(UNIT)","SPEC DEVIATION (YES/NO)","CONFORM TO SPECIFICATIONS \n( YES/NO)","DELIVERY PERIOD ( DAYS) ","EASTERN CAPE\nPRICE PER UNIT \nINCLUSIVE OF VAT","FREE STATE\nPRICE PER UNIT \nINCLUSIVE OF VAT","GAUTENG\nPRICE PER UNIT \nINCLUSIVE OF VAT","KWAZULU NATAL\nPRICE PER UNIT \nINCLUSIVE OF VAT","LIMPOPO\nPRICE PER UNIT \nINCLUSIVE OF VAT","MPUMALANGA\nPRICE PER UNIT \nINCLUSIVE OF VAT","NORTHERN CAPE\nPRICE PER UNIT \nINCLUSIVE OF VAT","NORTH WEST\nPRICE PER UNIT \nINCLUSIVE OF VAT","WESTERN CAPE\nPRICE PER UNIT \nINCLUSIVE OF VAT"]
["56111906-00100","CLIP TYPE SHELVING","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT. \nSIZE 914mm WIDE X 305mm DEEP. 1mm THICK COLD ROLLED COMMERCIAL QUALITY STEEL\nTHIS ITEM IS ADDITIONAL TO THE BELOW ITEMS: 56111906-00101, 56111906-00102, 56111906-00103, 56111906-00104"]
["56111906-00101","CLIP TYPE SHELVING","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. \nSIZE 1905mm HIGH X 914mm WIDE X 305mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. \nTHE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00102",null,"CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS.\nSIZE 1905mm HIGH X 914mm WIDE X 305mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00103",null,"CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. \nSIZE 2210mm HIGH X 914mm WIDE X 305mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00104",null,"CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS.\n SIZE 2210mm HIGH X 914mm WIDE X 305mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00105","CLIP TYPE SHELVING","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT.\n SIZE 914mm WIDE X 381mm DEEP. 1mm THICK COLD ROLLED COMMERCIAL QUALITY STEEL\nTHIS ITEM IS ADDITIONAL TO THE BELOW ITEMS : 56111906-00106, 56111906-00107, 56111906-00108, 56111906-00109"]
["56111906-00106","CLIP TYPE SHELVING","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. SIZE 1905mm HIGH X 914mm WIDE X 381mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00107",null,"CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. SIZE 1905mm HIGH X 914mm WIDE X 305mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00108",null,"CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. SIZE 2210mm HIGH X 914mm WIDE X 381mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00109",null,"CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. SIZE 2210mm HIGH X 914mm WIDE X 381mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00110","CLIP TYPE SHELVING","ADDITIONAL SHELF FOR CLIP TYPE SHELVING UNIT.\n SIZE 914mm WIDE X 457mm DEEP. 1mm THICK COLD ROLLED COMMERCIAL QUALITY STEEL\nTHIS ITEM IS ADDITIONAL TO THE BELOW ITEMS : 56111906-00111, 56111906-00112, 56111906-00113, 56111906-00114"]
["56111906-00111","CLIP TYPE SHELVING","CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. SIZE 1905mm HIGH X 914mm WIDE X 457mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00112",null,"CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. SIZE 1905mm HIGH X 914mm WIDE X 457mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00113",null,"CLIP TYPE SHELVING UNIT WITH BACK BRACING AND SIDE PANELS. SIZE 2210mm HIGH X 914mm WIDE X 457mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00114",null,"CLIP TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. SIZE 2210mm HIGH X 914mm WIDE X 457mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00166","BEADED TYPE SHELVING","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT.\n SIZE 914mm WIDE X 305mm DEEP. 1mm THICK COLD ROLLED COMMERCIAL QUALITY STEEL\nTHIS ITEM IS ADDITIONAL TO THE BELOW ITEMS : 56111906-00167, 56111906-00119, 56111906-00115, 56111906-00116\n"]
["56111906-00167","BEADED TYPE SHELVING","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. SIZE 1905mm HIGH X 914mm WIDE X 305mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00119","BEADED TYPE SHELVING","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. SIZE 1905mm HIGH X 914mm WIDE X 305mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00115","BEADED TYPE SHELVING","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. SIZE 2210mm HIGH X 914mm WIDE X 305mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00116","BEADED TYPE SHELVING","BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. SIZE 2210mm HIGH X 914mm WIDE X 305mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00117","BEADED TYPE SHELVING","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT.\nSIZE 914mm WIDE X 381mm DEEP. 1mm THICK COLD ROLLED COMMERCIAL QUALITY STEEL\nTHIS ITEM IS ADDITIONAL TO THE BELOW ITEMS : 56111906-00118, 56111906-00119, 56111906-00120, 56111906-00121"]
["56111906-00118","BEADED TYPE SHELVING","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\n SIZE 1905mm HIGH X 914mm WIDE X 381mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00119",null,"BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS.\n SIZE 1905mm HIGH X 914mm WIDE X 305mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00120",null,"BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\n SIZE 2210mm HIGH X 914mm WIDE X 381mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00121",null,"BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS.\n SIZE 2210mm HIGH X 914mm WIDE X 381mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00122","BEADED TYPE SHELVING","ADDITIONAL SHELF FOR BEADED TYPE SHELVING UNIT. SIZE 914mm WIDE X 457mm DEEP. 1mm THICK COLD ROLLED COMMERCIAL QUALITY STEEL\nTHIS ITEM IS ADDITIONAL TO THE BELOW ITEMS : 56111906-00123, 56111906-00124, 56111906-00125, 56111906-00126"]
["56111906-00123","BEADED TYPE SHELVING","BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. SIZE 1905mm HIGH X 914mm WIDE X 457mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00124",null,"BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. SIZE 1905mm HIGH X 914mm WIDE X 457mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00125",null,"BEADED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. SIZE 2210mm HIGH X 914mm WIDE X 457mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00126",null,"BEADED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. SIZE 2210mm HIGH X 914mm WIDE X 457mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00127","BOLTED TYPE SHELVING","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT. \nSIZE 914mm WIDE X 305mm DEEP. 1mm THICK COLD ROLLED COMMERCIAL QUALITY STEEL\nTHIS ITEM IS ADDITIONAL TO THE BELOW ITEMS : 56111906-00128, 56111906-00129, 56111906-00130, 56111906-00131"]
["56111906-00128","BOLTED TYPE SHELVING","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. SIZE 1905mm HIGH X 914mm WIDE X 305mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00129",null,"BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. SIZE 1905mm HIGH X 914mm WIDE X 305mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00130",null,"BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. SIZE 2210mm HIGH X 914mm WIDE X 305mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00131",null,"BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. SIZE 2210mm HIGH X 914mm WIDE X 305mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00132","BOLTED TYPE SHELVING","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSIZE 914mm WIDE X 381mm DEEP. 1mm THICK COLD ROLLED COMMERCIAL QUALITY STEEL\nTHIS ITEM IS ADDITIONAL TO THE BELOW ITEMS : 56111906-00133, 56111906-00134, 56111906-00135, 56111906-00136"]
["56111906-00133","BOLTED TYPE SHELVING","BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. SIZE 1905mm HIGH X 914mm WIDE X 381mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00134",null,"BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS. SIZE 1905mm HIGH X 914mm WIDE X 305mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00135",null,"BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. SIZE 2210mm HIGH X 914mm WIDE X 381mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00136",null,"BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS\nSIZE 2210mm HIGH X 914mm WIDE X 381mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00137","BOLTED TYPE SHELVING","ADDITIONAL SHELF FOR BOLTED TYPE SHELVING UNIT.\nSIZE 914mm WIDE X 457mm DEEP. 1mm THICK COLD ROLLED COMMERCIAL QUALITY STEEL\nTHIS ITEM IS ADDITIONAL TO THE BELOW ITEMS : 56111906-00138, 56111906-00139, 56111906-00140, 56111906-00141"]
["56111906-00138",null,"BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING. \nSIZE 1905mm HIGH X 914mm WIDE X 457mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00139",null,"BOLTED TYPE SHELVING UNIT WITH BACK PANELS AND SIDE PANELS.\n SIZE 1905mm HIGH X 914mm WIDE X 457mm DEEP. 6 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00140",null,"BOLTED TYPE SHELVING UNIT WITH BACK BRACING AND SIDE BRACING.\n SIZE 2210mm HIGH X 914mm WIDE X 457mm DEEP. 7 X SHELVES INCLUDING TOP AND BOTTOM. 1mm THICK COLLED ROLLED COMMERCIAL QUALITY STEEL. UNIFORMLY DISTRIBUTED MASS LOAD OF 170kg PER SHELF. THE UNIT MUST BE FULLY ADJUSTABLE TO ALLOW FOR ADDITIONAL SHELVES. UNIT MUST BE IN ACCORDANCE WITH CKS SPECIFICATIONS 370."]
["56111906-00142","HEAVY DUTY STEEL RACKING","HEAVY DUTY STEEL RACKING WITH NO DECKING. \nSIZE 3353mm HIGH X 2743mm WIDE X 900mm DEEP. 4 X BEAM LEVELS TO THE HEIGHT. UNIFORMLY DISTRIBUTED LOAD OF 3000kg PER BEAM LEVEL. UNIT MUST BE FULLY AJUSTABLE TO ALLOW FOR ADDITIONAL BEAM LEVELS TO BE ADDED. "]
["56111906-00143","HEAVY DUTY STEEL RACKING","HEAVY DUTY STEEL RACKING WITH TIMBER DECKING.\n SIZE 3353mm HIGH X 2743mm WIDE X 900mm DEEP. 4 X BEAM LEVELS TO THE HEIGHT. 25mm THICK TIMBER DECKING. UNIFORMLY DISTRIBUTED LOAD OF 3000kg PER BEAM LEVEL. UNIT MUST BE FULLY AJUSTABLE TO ALLOW FOR ADDITIONAL BEAM LEVELS TO BE ADDED. "]
["56111906-00144","HEAVY DUTY STEEL RACKING","HEAVY DUTY STEEL RACKING WITH STEEL DECKING.\n SIZE 3353mm HIGH X 2743mm WIDE X 900mm DEEP. 4 X BEAM LEVELS TO THE HEIGHT. 1mm THICK STEEL DECKING. UNIFORMLY DISTRIBUTED LOAD OF 3000kg PER BEAM LEVEL. UNIT MUST BE FULLY AJUSTABLE TO ALLOW FOR ADDITIONAL BEAM LEVELS TO BE ADDED. "]
["56111906-00145","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR.\n COMPATIBLE WITH HEAVY DUTY RACKING PLACED ON THE FLOOR. UNIFORMLY DISTRIBUTED LOAD OF 350kg/m². FLOOR TO BE COVERED WITH TIMBER DECKING. PRICE INCLUDES STATNCHIONS , STAIRCASE AND HANDRAILS."]
["56111906-00146","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR","HEAVY DUTY RACK SUPPORTED MEZZANINE FLOOR. \nCOMPATIBLE WITH HEAVY DUTY RACKING PLACED ON THE FLOOR. UNIFORMLY DISTRIBUTED LOAD OF 350kg/m². FLOOR TO BE COVERED WITH STEEL DECKING PRICE INCLUDES STATNCHIONS , STAIRCASE AND HANDRAILS."]
["56111906-00147","SHELVING SUPPORTED MEZZANINE FLOOR","SHELVING SUPPORTED MEZZANINE FLOOR (CATWALK SYSTEM).\n COMPATIBLE WITH SHELVING PLACED ON THE FLOOR. UNIFORMLY DISTRIBUTED LOAD OF 350kg/m². PRICE INCLUDES STATNCHIONS , STAIRCASE AND HANDRAILS."]
["56111906-00148","STRUCTURAL MEZZANINE FLOOR","STRUCTURAL MEZZANINE FLOOR.\n FREE STANDING INDEPENDENT FLOOR. UNIFORMLY DISTRIBUTED LOAD OF 350kg/m². FLOOR TO BE COVERED WITH STEEL DECKING. PRICE INCLUDES STATNCHIONS , STAIRCASE AND HANDRAILS."]
["56111906-00149","STRUCTURAL MEZZANINE FLOOR","STRUCTURAL MEZZANINE FLOOR. \nFREE STANDING INDEPENDENT FLOOR. UNIFORMLY DISTRIBUTED LOAD OF 350kg/m². FLOOR TO BE COVERED WITH TIMBER DECKING. PRICE INCLUDES STATNCHIONS , STAIRCASE AND HANDRAILS."]
["56111906-00150","MOBILE SHELVING (2103H)","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED).\n 2103mm HIGH X 920mm WIDE X 381mm DEEP. 6 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE STATIC BASES , 1 X SINGLE MOVABLE BASE , 1 X SINGLE LOCKABLE BASE AND 1 X 800mm PASSAGE. 1mm THICK COLLED ROLLED STEEL."]
["56111906-00151","MOBILE SHELVING (2103H)","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n 2103mm HIGH X 920mm WIDE X 381mm DEEP. 6 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE MOVABLE BASE. "]
["56111906-00152","MOBILE SHELVING (2103H)","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED).\n 2103mm HIGH X 1840mm WIDE X 381mm DEEP. 6 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE STATIC BASES , 1 X SINGLE MOVABLE BASE , 1 X SINGLE LOCKABLE BASE AND 1 X 800mm PASSAGE. 1mm THICK COLLED ROLLED STEEL."]
["56111906-00153","MOBILE SHELVING (2103H)","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2103mm HIGH X 1840mm WIDE X 381mm DEEP. 6 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE MOVABLE BASE. "]
["56111906-00154","MOBILE SHELVING (2103H)","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm HIGH X 2760mm WIDE X 381mm DEEP. 6 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE STATIC BASES , 1 X SINGLE MOVABLE BASE , 1 X SINGLE LOCKABLE BASE AND 1 X 800mm PASSAGE. 1mm THICK COLLED ROLLED STEEL."]
["56111906-00155","MOBILE SHELVING (2103H)","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED).\n 2103mm HIGH X 2760mm WIDE X 381mm DEEP. 6 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE MOVABLE BASE. "]
["56111906-00156","MOBILE SHELVING (2103H)","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2103mm HIGH X 3680mm WIDE X 381mm DEEP. 6 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE STATIC BASES , 1 X SINGLE MOVABLE BASE , 1 X SINGLE LOCKABLE BASE AND 1 X 800mm PASSAGE. 1mm THICK COLLED ROLLED STEEL."]
["56111906-00157","MOBILE SHELVING (2103H)","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2103mm HIGH X 3680mm WIDE X 381mm DEEP. 6 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE MOVABLE BASE. "]
["56111906-00158","MOBILE SHELVING (2484H)","MOBILE FILING SYSTEM 01 DEEP 03 BASES (HANDLE OPERATED). \n2484mm HIGH X 920mm WIDE X 381mm DEEP. 7 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE STATIC BASES , 1 X SINGLE MOVABLE BASE , 1 X SINGLE LOCKABLE BASE AND 1 X 800mm PASSAGE. 1mm THICK COLLED ROLLED STEEL."]
["56111906-00159","MOBILE SHELVING (2484H)","ADDITIONAL MOBILE FILING SYSTEM 01 DEEP 01 BASE (HANDLE OPERATED).\n 2484mm HIGH X 920mm WIDE X 381mm DEEP. 7 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE MOVABLE BASE. "]
["56111906-00160","MOBILE SHELVING (2484H)","MOBILE FILING SYSTEM 02 DEEP 03 BASES (HANDLE OPERATED). \n2484mm HIGH X 1840mm WIDE X 381mm DEEP. 7 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE STATIC BASES , 1 X SINGLE MOVABLE BASE , 1 X SINGLE LOCKABLE BASE AND 1 X 800mm PASSAGE. 1mm THICK COLLED ROLLED STEEL."]
["56111906-00161","MOBILE SHELVING (2484H)","ADDITIONAL MOBILE FILING SYSTEM 02 DEEP 01 BASE (HANDLE OPERATED). \n2484mm HIGH X 1840mm WIDE X 381mm DEEP. 7 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE MOVABLE BASE. "]
["56111906-00162","MOBILE SHELVING (2484H)","MOBILE FILING SYSTEM 03 DEEP 03 BASES (STEERING WHEEL OPERATED).\n 2484mm HIGH X 2760mm WIDE X 381mm DEEP. 7 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE STATIC BASES , 1 X SINGLE MOVABLE BASE , 1 X SINGLE LOCKABLE BASE AND 1 X 800mm PASSAGE. 1mm THICK COLLED ROLLED STEEL."]
["56111906-00163","MOBILE SHELVING (2484H)","MOBILE FILING SYSTEM 03 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm HIGH X 2760mm WIDE X 381mm DEEP. 7 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE MOVABLE BASE."]
["56111906-00164","MOBILE SHELVING (2484H)","MOBILE FILING SYSTEM 04 DEEP 03 BASES (STEERING WHEEL OPERATED). \n2484mm HIGH X 3680mm WIDE X 381mm DEEP. 7 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE STATIC BASES , 1 X SINGLE MOVABLE BASE , 1 X SINGLE LOCKABLE BASE AND 1 X 800mm PASSAGE. 1mm THICK COLLED ROLLED STEEL."]
["56111906-00165","MOBILE SHELVING (2484H)","MOBILE FILING SYSTEM 04 DEEP 01 BASE (STEERING WHEEL OPERATED). \n2484mm HIGH X 3680mm WIDE X 381mm DEEP. 7 X SHELVES TO THE HEIGHT. UNIT HAS BACK PANELS AND SIDE PANELS. UNIT CONSISTS OF 1 X SINGLE MOVABLE BASE. "]
["30161803-00000","FILING CUPBOARDS","2 Door , 4 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900 mm(w)X 1800(h) \nMaterial  - Mild Steel\nThickness: 0,8mm -1,2 mm"]
["30161803-00001","FILING CUPBOARDS","2 Door, 3 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 1500(h) \nMaterial  - Mild Steel\nThickness: 0,8mm -1,2 mm"]
["30161803-00002","FILING CUPBOARDS","2 Door, 2 Shelf Steel Filing Cupboard, two tone, name tag holder, lockable\nDimensions: 450 mm(d) X 900mm(w)X 900(h) \nMaterial  - Mild Steel\nThickness: 0,8mm -1,2 mm"]
[{"$f":"[1]Sheet1!$C$18","v":"30161803-00003"},"FILING CABINETS","4 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1320(h) \nMaterial  - Mild Steel\nThickness: 0,8mm -1,2 mm"]
[{"$f":"[1]Sheet1!$C$22","v":"30161803-00004"},"FILING CABINETS","3 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 1020(h) \nMaterial  - Mild Steel\nThickness: 0,8mm -1,2 mm"]
[{"$f":"[1]Sheet1!$C$26","v":"30161803-00005"},"FILING CABINETS","2 Drawer Steel Filing Cabinet, two tone, name tag holder, lockable\nDimensions: 630 mm(d) X 470mm(w)X 720(h) \nMaterial  - Mild Steel\nThickness: 0,8mm -1,2 mm"]
["30161803-00006","PARCEL TROLLEY","Overall Size (LxWxH): 1100x650x940mm                                                                                                                              ideal for stock picking and transferring boxed products\nElectro galvanised finish\nRubber castors – 2 x fixed, 2 x swivel\nLoad Capacity: 300kg\nCastors: 160mm\nOverall Size (LxWxH): 1100x650x940mm\nUnit Weight: 36kg"]

{"sheet":"Sheet1","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}