{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["SAP -0198223","SAP-0198223","Deviation Schedules","Test Schedules"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900"}

{"sheet":"SAP -0198223","index":0,"n_rows":43,"n_cols":7,"rows_kept":43,"merged":[[0,1,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[6,2,6,3],[7,2,7,3],[8,3,8,4],[18,3,18,4],[23,3,23,4],[27,2,27,4],[28,2,28,4],[29,3,29,4],[32,3,32,4],[36,1,36,6],[37,1,37,6],[39,0,39,1],[40,5,40,6],[42,2,42,3],[42,5,42,6]]}
[null,"Technical Schedules A and B for"]
[null,"GRIP,STRAIN O/H 35SQ B/NTRL ABC D3060"]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,"1.1","·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No",null,{"v":198223,"d":"0198223"},"xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer's Name",null,"xxxxxxxxxx"]
[null,"1.1.3",null,"Supplier's Name ",null,"xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Product Code",null,"xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's Drawing number & Revision number",null,"xxxxxxxxxx"]
[null,"1.1.6",null,"Manufacturer's Physical identification mark on product",null,"xxxxxxxxxx"]
[null,"1.1.7",null,"Compliance to all dimensions and requirements of Eskom Buyer's Guide drawing","D-DT 3060","YES"]
[null,"1.1.8",null,"Item sample required, upon request from Eskom. (As per the Technical Criteria Document)",null,"YES","xxxxxxxxxx"]
[]
[null,"1.2","·","Mechanical Properties"]
[null,"1.2.1",null,"Material Grade",null,"GRIP/WIRE FORM"]
[null,"1.2.2",null,"Colour coded\n",null,"BLUE /PINK"]
[null,"1.2.3",null,"Minimum Failing Load",null,"10KN"]
[]
[null,"1.3","·","Marking and Packaging"]
[null,"1.3.1",null,"Net weight per container","kg","≤ 30"]
[null,"1.3.2",null,"Labelled and marking of packaging",null,"Yes"]
[]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to be provided in electronic format."]
[null,"2.1","·","General"]
[null,"2.1.1",null,"Outline drawings of item","Sets",1]
[null,"2.1.2",null,"Material grade certification","Certification submitted","YES"]
[null,"2.2","·","Test Reports (where applicable)",null,"Required","Report Number"]
[{"$nulls":3},"Visual examination","Test report submitted","YES"]
[]
[]
[null,"NOTE:  DEVIATION SCHEDULE CONTINUE ON NEXT PAGE.\n             IF NO DEVIATIONS ARE MENTIONED ON THE DEVIATION SCHEDULE IT WILL BE ACCEPTED THAT THE SUPPLIER\n              AND MANUFACTURER FULLY COMPLIES WITH THE REQUIREMENTS OF THE ESKOM SPECIFICATON(S)."]
[null,"SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company Name"]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"SAP-0198223","index":1,"n_rows":55,"n_cols":7,"rows_kept":55,"merged":[[0,1,0,6],[2,1,2,6],[3,1,3,6],[4,1,4,6],[5,1,5,6],[8,2,8,3],[9,2,9,3],[10,3,10,4],[27,3,27,4],[33,3,33,4],[37,2,37,4],[38,2,38,4],[39,3,39,4],[42,3,42,4],[47,1,47,6],[48,1,48,6],[49,1,49,6],[51,0,51,1],[52,5,52,6],[54,2,54,3],[54,5,54,6]]}
[null,"ESKOM TENDER E2719DXLIMOU"]
[]
[null,"Technical Schedules A and B for"]
[null,"GRIP,STRAIN O/H 35SQ B/NTRL ABC D3060"]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,"1.1","·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No",null,{"v":198223,"d":"0198223"},"xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer's ","Manufacturer's Name","xxxxxxxxxx"]
[null,"1.1.3",null,"Supplier's ","Supplier's Name ","xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Product Code","Specify code","xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's Drawing number & Revision number","Specify No and Rev","xxxxxxxxxx"]
[null,"1.1.6",null,"Manufacturer's Physical identification mark on product","240-75883388","xxxxxxxxxx"]
[null,"1.1.7",null,"Compliance to all dimensions and requirements of Eskom Buyer's Guide drawing","D-DT 3060","YES"]
[null,"1.1.8",null,"Item sample required, upon request from Eskom. (As per the Technical Criteria Document)",null,"YES"]
[null,"1.1.9",null,"Compliance to Eskom Buyer's Guide Drawings"]
[null,"1.1.9.1",null,"For use with stay wire as per SAP number","Eskom DDT -3060","70mm SQ Aerial Bundle\nConductor System","xxxxxxxxxx"]
[null,"1.1.9.2",null,"For use on a minimum pole diameter as per SAP\nnumber",null,"Pole Diamater 200m","xxxxxxxxxx"]
[null,"1.1.9.3",null,"Colour code as per SAP number","Eskom DDT-3060,\n240-75883844","BLUE / PINK","xxxxxxxxxx"]
[null,"1.1.9.4",null,"Length of fitting","mm","specify"]
[null,"1.1.9.5",null,"Item sample required, upon request from Eskom\n(As per the Technical Criteria Document)",null,"YES","xxxxxxxxxx"]
[]
[]
[null,"1.2","·","Mechanical Properties"]
[null,"1.2.1",null,"Material Grade",null,"Specify material used and grade"]
[{"$nulls":3},"Grit shall be chemically inert and shall not be\ndamaging to the product or conductor.",null,"YES"]
[null,"1.2.2",null,"Colour coded\n","Eskom DDT-3060,\n240-75883844","BLUE/PINK"]
[null,"1.2.3",null,"Minimum Failing Load","DDT-3060","14KN"]
[{"$nulls":3},"Thimble ","UV stable nylon thimble\nABDE315 THG or\nApproved Equivalent"]
[null,"1.3","·","Marking and Packaging"]
[null,"1.3.1",null,"Net weight per container","kg","≤ 30"]
[null,"1.3.2",null,"Labelled and marking of packaging",null,"Yes"]
[]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to be provided in electronic format."]
[null,"2.1","·","General"]
[null,"2.1.1",null,"Approved Manufacturer Drawings showing\nmarkings and dimensions","1 Sets Submitted",1]
[null,"2.1.2",null,"Material grade certification","Certification submitted","YES"]
[null,"2.2","·","Test Reports ",null,"Required"]
[{"$nulls":3},"Has the relevant signed mandatory test schedule\nbeen submitted.","Signed Test Schedule submitted","YES"]
[]
[]
[]
[null,"ESKOM TENDER E2719DXLIMOU"]
[null,"NOTE:  DEVIATION SCHEDULE CONTINUE ON NEXT PAGE.\n             IF NO DEVIATIONS ARE MENTIONED ON THE DEVIATION SCHEDULE IT WILL BE ACCEPTED THAT THE SUPPLIER\n              AND MANUFACTURER FULLY COMPLIES WITH THE REQUIREMENTS OF THE ESKOM SPECIFICATON(S)."]
[null,"SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company Name"]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Deviation Schedules","index":2,"n_rows":45,"n_cols":5,"rows_kept":45,"merged":[[0,0,0,6],[1,0,1,6],[2,2,2,6],[3,2,3,3],[4,0,4,6],[5,2,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[34,2,34,6],[35,2,35,6],[37,0,37,6],[38,0,38,6],[40,0,40,1],[41,0,41,1],[41,4,41,5],[44,4,44,5]]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation schedule - D-DT 3060 (Insert item description below)"]
["Description :",null,"GRIP,STRAIN O/H 35SQ B/NTRL ABC D3060"]
[null,"SAP:",{"v":198223,"d":"0198223"}]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":31}
["ESKOM TENDER E2719DXLIMOU"]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[null,null,"Name (Print)",null,"Company Name"]
[]
[null,null,"         "]
[null,null,"Sign",null,"Date"]

{"sheet":"Test Schedules","index":3,"n_rows":21,"n_cols":7,"rows_kept":21,"merged":[[0,1,0,6],[1,1,1,6],[2,1,2,3],[3,1,3,3],[6,2,6,3],[12,1,12,6],[13,0,13,6],[15,0,15,1],[16,5,16,6],[20,2,20,3],[20,5,20,6]]}
[null,"ESKOM TENDER E2719DXLIMOU"]
[null,"Test Report Schedule D-DT 3060: "]
[null,"Description:    "]
[null,"GRIP,STRAIN O/H 35SQ B/NTRL ABC D3060",null,null,"SAP:","0198223"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,"Clause No.","Specification","Report Number"]
[null,"2.2.1",null,"Visual examination",4.3,"240-75883388"]
[null,"2.2.2",null,"Dimensional and material verification ",4.3,"240-75883388"]
[null,"2.2.3",null,"Grit Retention test",4.3,"240-75883388"]
[null,"2.2.4",null,"Tensile test",4.3,"240-75883388"]
[]
[null,"ESKOM TENDER E2719DXLIMOU"]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company Name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]