{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["RFP165.2023"],"not_rendered":{"comments":2},"read":"whole","date_system":"1900"}

{"sheet":"RFP165.2023","index":0,"n_rows":43,"n_cols":9,"rows_kept":43,"merged":[[1,3,1,8],[11,3,27,3],[36,3,37,7],[36,8,37,8],[39,3,39,7],[40,3,41,4],[40,5,41,5],[40,6,41,6],[40,7,41,7],[40,8,41,8],[42,3,43,7],[42,8,43,8]]}
[]
[{"$nulls":3},"RFP165/2023: \nTHE SUPPLY, DELIVERY, HIRE, COMMISSIONING & DE – COMMISSIONING OF TOWER CRANE SERVICES FOR PERIOD OF UP TO 14 MONTHS TO DWS CONSTRUCTION NORTH TZANEEN DAM RAISING PROJECT IN THE LIMPOPO PROVINCE"]
[]
[]
[{"$nulls":3},"Item","Description","Unit","Quantity","Rate (Rands)","Total (Rands)"]
[]
[{"$nulls":3},1,"Establishment of cranes on site (Delivery and erecting of cranes on site)","No.",1,null,{"$f":"H7*G7","v":{"v":0,"d":"R0.00"}}]
[]
[{"$nulls":3},2,"Erection of tower crane and testing","No.",1,null,{"$f":"H9*G9","v":{"v":0,"d":"R0.00"}}]
[]
[{"$nulls":3},3,"Commissioning","No.",1,null,{"$f":"H11*G11","v":{"v":0,"d":"R0.00"}}]
[{"$nulls":3},4,"Hiring of the Tower Crane (wet rate)."]
[{"$nulls":4},"a)       number x  01 ","Months",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},"b)       including operator, ","Months",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},"c)        cabling and termination ","Sum",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},"d)        diesel and storage, ","Months",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},"e)       servicing, ","Months",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},"f)       full compliance with legislature, ","Months",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},"g)        Power supply (Generator) and Bunding Wall), ","Months",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},"h)        Flagmen(s) minimum of 2","Months",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},"i)        rigger(s) minimum of 2 certifite","Months",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},"J)        accommodation, ","Months",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},"k)        transport, ","Months",14,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},"l)        safety gear","No",5,null,{"$f":"H24*G24","v":{"v":0,"d":"R0.00"}}]
[{"$nulls":4},"         m)     Lifting equipment as per scope of work","Sum",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},"         n)        safety gear","Sum",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},"         o) Operation and Maintenace Manuals","No.",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":4},"         p) Medical Tests","Sum",1,null,{"v":0,"d":"R0.00"}]
[]
[{"$nulls":3},5,"Design, Construct and Demolition of Tower Crane pad/platform","No",1,null,{"v":0,"d":"R0.00"}]
[]
[]
[{"$nulls":3},6,"Disestablishment of the Tower Cranes from site (Dismantling and collecting cranes from site)","No.",1,null,{"v":0,"d":"R0.00"}]
[{"$nulls":3},7,"Mancage: capacity at maximum 600kg (able to accommodate 5 x people)","No.",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":3},8,"Material cage at minimum capacity of 1 ton  at minimum size of ( width = 2m x Length =12m x Height = 1.6m)","No.",2,null,{"v":0,"d":"R0.00"}]
[{"$nulls":3},9,"Opearational and Maintenace Manuals","No.",3,null,{"v":0,"d":"R0.00"}]
[{"$nulls":3},"SUB TOTAL A",{"$nulls":4},{"$f":"SUM(I7:I36)","v":{"v":0,"d":"R0.00"}}]
[]
[{"$nulls":3},"Contegencies",null,"%",{"v":0.15,"d":"15%"},null,{"$f":"+I37*G39","v":{"v":0,"d":"R0.00"}}]
[{"$nulls":3},"SUB TOTAL B",{"$nulls":4},{"$f":"SUM(I37:I39)","v":{"v":0,"d":"R0.00"}}]
[{"$nulls":3},"VAT @ 15%",null,"%",{"v":0.15,"d":"15%"},null,{"$f":"I40*G41","v":{"v":0,"d":"R0.00"}}]
[]
[{"$nulls":3},"TOTAL",{"$nulls":4},{"$f":"I41+I40","v":{"v":0,"d":"R0.00"}}]