{"text_format":"3","workbook":"xlsx","n_sheets":8,"sheets":["Bill 1","Bill 2","Bill 3","Bill 4","Bill 5","Bill 6","Bill 7","Summary"],"read":"whole","date_system":"1900"}

{"sheet":"Bill 1","index":0,"n_rows":17,"n_cols":6,"rows_kept":17,"merged":[[1,0,1,5],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,4,3,4],[2,5,3,5],[5,0,7,0],[5,1,7,1],[5,2,7,2],[5,3,7,3],[5,4,7,4],[5,5,7,5],[10,0,15,0],[10,1,15,1],[10,2,15,2],[10,3,15,3],[10,4,15,4],[10,5,15,5],[16,0,16,4]]}
[]
["BILL 1"]
["Item nr","Description","Unit","Expected","Rate","Price"]
[{"$nulls":3},"Quantity"]
[1,"Bill no 1 – General Preliminary\n\nALL work to be done by the Appointed Contractor including Safety Compliance Services and emergency response\n\nEskom is an ISO 9001, 18001 registered company and requires from the Contractor to adhere to these"]
[1.1,"To provide Eskom with a Safety File as required and to maintain the fire protection systems throughout the contract period as contemplated","Sum",1]
[]
[]
[1.2,"Provide contract employees with appropriate Personal Protective Equipment including (as a minimum) for the following work categories:"]
["1.2.1","Inspection, Servicing and Testing as per the specification.","Sum",1]
[1.4,"The Contractor shall compile a file, in duplicate and in electronic format (as described) which shall be kept up to-date throughout the contract period and one physical and one electronic copy returned when the contract period has expired.","Sum",1]
[]
[]
[]
[]
[]
["Total Bill 1"]

{"sheet":"Bill 2","index":1,"n_rows":42,"n_cols":7,"rows_kept":42,"merged":[[1,0,1,6],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,4,6],[41,0,41,4]]}
[]
["Bill 2: Monthly Inspect, conduct fault-finding and Restore Faults and Alarms on Station Fire Alarm Systems:"]
["Item nr","Description","Unit","Expected Quantity","Rate","Price for Year 1","Total for 60 months"]
[]
[]
[2,"Monthly Inspection, Fault-finding & Repairing of Faults and Alarm intervals \n\nFor the inspection, fault-finding & Restoring of Faults & Alarms of the Station Fire Alarm System (as per scope) inclusive of all supervision, labour, materials, and traveling costs of:"]
[2.1,"Station Fire Alarm Systems:"]
["2.1.1","Equipment Room Aritech Fire Alarm Panel","Ea",1]
["2.1.2","Equipment Room Aritech Repeater Panel","Ea",1]
["2.1.3","Visitors Center Fire Alarm Panel","Ea",1]
["2.1.4","Outside Store Fire Alarm Panel","Ea",1]
["2.1.5","Headrace Fire Alarm Panel","Ea",1]
["2.1.6","Surface Building Fire Alarm Panel","Ea",1]
[2.2,"Transformer Fire Alarm Systems:"]
["2.2.1","Generator Transformer 1 Fire Alarm Panel","Ea",1]
["2.2.2","Generator Transformer 2 Fire Alarm Panel","Ea",1]
["2.2.3","Generator Transformer 3 Fire Alarm Panel","Ea",1]
["2.2.4","Generator Transformer 4 Fire Alarm Panel","Ea",1]
["2.2.5","Station Transformer 1 Fire Alarm Panel","Ea",1]
["2.2.6","Station Transformer 2 Fire Alarm Panel","Ea",1]
["2.2.7","Service Transformer 1 Fire Alarm Panel","Ea",1]
["2.2.8","Service Transformer 2 Fire Alarm Panel","Ea",1]
[2.3,"Video Fire Alarm & Smoke Detection (VFSD) System:"]
["2.3.1","Control Room Client PC Alarm Monitor","Ea",1]
["2.3.2","Security Room Client PC Alarm Monitor","Ea",1]
["2.3.3","Equipment Rack","Ea",1]
["2.3.4","HUB Enclosures","Ea",5]
["2.3.5","Camera Enclosures","Ea",5]
["2.3.6","Cameras","Ea",5]
["2.3.7","Lights","Ea",5]
[2.4,"Aspiration Units:"]
["2.4.1","Unit 1 Generator Aspiration Unit","Ea",1]
["2.4.2","Unit 2 Generator Aspiration Unit","Ea",1]
["2.4.3","Unit 3 Generator Aspiration Unit","Ea",1]
["2.4.4","Unit 4 Generator Aspiration Unit","Ea",1]
["2.4.5","Lift Shaft Aspiration Unit","Ea",1]
[2.5,"Beam Units:"]
["2.5.1","Unit 1 Spherical Valve Beam Unit","Ea",1]
["2.5.2","Unit 2 Spherical Valve Beam Unit","Ea",1]
["2.5.3","Unit 3 Spherical Valve Beam Unit","Ea",1]
["2.5.4","Unit 4 Spherical Valve Beam Unit","Ea",1]
["Total Bill 2"]

{"sheet":"Bill 3","index":2,"n_rows":42,"n_cols":8,"rows_kept":42,"merged":[[1,0,1,7],[2,0,4,0],[2,1,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,4,6],[2,7,4,7],[5,1,5,2],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,0,41,6]]}
[]
["Bill 3: 3-Monthly inspect and service fire alarm systems:"]
["Item nr","Description",null,"Unit","Expected Quantity","Rate","Price for Year 1","Total for 60 months"]
[]
[]
[3,"3-Monthly Inspection & Servicing intervals\n\nFor the inspection & service of fire alarm system (as per scope) inclusive of all supervision, labour, materials, and traveling costs of:"]
[3.1,"Station Fire Alarm Systems:"]
["3.1.1","Equipment Room Aritech Fire Alarm Panel",null,"Ea",1]
["3.1.2","Equipment Room Aritech Repeater Panel",null,"Ea",1]
["3.1.3","Visitors Center Fire Alarm Panel",null,"Ea",1]
["3.1.4","Outside Store Fire Alarm Panel",null,"Ea",1]
["3.1.5","Headrace Fire Alarm Panel",null,"Ea",1]
["3.1.6","Surface Building Fire Alarm Panel",null,"Ea",1]
[3.2,"Transformer Fire Alarm Systems:"]
["3.2.1","Generator Transformer 1 Fire Alarm Panel",null,"Ea",1]
["3.2.2","Generator Transformer 2 Fire Alarm Panel",null,"Ea",1]
["3.2.3","Generator Transformer 3 Fire Alarm Panel",null,"Ea",1]
["3.2.4","Generator Transformer 4 Fire Alarm Panel",null,"Ea",1]
["3.2.5","Station Transformer 1 Fire Alarm Panel",null,"Ea",1]
["3.2.6","Station Transformer 2 Fire Alarm Panel",null,"Ea",1]
["3.2.7","Service Transformer 1 Fire Alarm Panel",null,"Ea",1]
["3.2.8","Service Transformer 2 Fire Alarm Panel",null,"Ea",1]
[3.3,"Video Fire Alarm & Smoke Detection (VFSD) System:"]
["3.3.1","Control Room Client PC Alarm Monitor",null,"Ea",1]
["3.3.2","Security Room Client PC Alarm Monitor",null,"Ea",1]
["3.3.3","Equipment Rack",null,"Ea",1]
["3.3.4","HUB Enclosures",null,"Ea",17]
["3.3.5","Camera enclosures",null,"Ea",54]
["3.3.6","Cameras",null,"Ea",54]
["3.3.7","Lights",null,"Ea",54]
[3.4,"Aspiration Units:"]
["3.4.1","Unit 1 Generator Aspiration Unit",null,"Ea",1]
["3.4.2","Unit 2 Generator Aspiration Unit",null,"Ea",1]
["3.4.3","Unit 3 Generator Aspiration Unit",null,"Ea",1]
["3.4.4","Unit 4 Generator Aspiration Unit",null,"Ea",1]
["3.4.5","Lift Shaft Aspiration Unit",null,"Ea",1]
[3.5,"Beam Units:"]
["3.5.1","Unit 1 Spherical Valve Beam Unit",null,"Ea",1]
["3.5.2","Unit 2 Spherical Valve Beam Unit",null,"Ea",1]
["3.5.3","Unit 3 Spherical Valve Beam Unit",null,"Ea",1]
["3.5.4","Unit 4 Spherical Valve Beam Unit",null,"Ea",1]
["Total Bill 3"]

{"sheet":"Bill 4","index":3,"n_rows":49,"n_cols":7,"rows_kept":49,"merged":[[1,0,1,6],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,4,4,4],[3,3,4,3],[3,6,4,6],[5,0,7,0],[5,2,7,2],[5,3,7,3],[5,4,7,4],[5,5,7,5],[5,6,7,6],[17,0,18,0],[17,2,18,2],[17,3,18,3],[17,4,18,4],[17,5,18,5],[17,6,18,6],[19,0,20,0],[19,2,20,2],[19,3,20,3],[19,4,20,4],[19,5,20,5],[19,6,20,6],[21,0,22,0],[21,2,22,2],[21,3,22,3],[21,4,22,4],[21,5,22,5],[21,6,22,6],[23,0,24,0],[23,2,24,2],[23,3,24,3],[23,4,24,4],[23,5,24,5],[23,6,24,6],[48,0,48,4]]}
[]
["Bill 4: Yearly service of fire detection systems:"]
["Item nr","Description","Unit","Expected","Rate","Price for","Total for 60"]
[{"$nulls":3},"Quantity",null,null,"months"]
[{"$nulls":5},"Year 1"]
[4,"Yearly Service intervals"]
[]
[null,"For the servicing of fire detection systems inclusive of all supervision, labour, materials, and traveling costs of:"]
[4.1,"Fire Alarm Systems:"]
["4.1.1","Station Fire Alarm Systems:"]
["4.1.1.1","Equipment Room Aritech Fire Alarm Panel","Ea",1]
["4.1.1.2","Equipment Room Aritech Repeater Panel","Ea",1]
["4.1.1.3","Visitors Center Fire Alarm Panel","Ea",1]
["4.1.1.4","Outside Store Fire Alarm Panel","Ea",1]
["4.1.1.5","Headrace Fire Alarm Panel","Ea",1]
["4.1.1.6","Surface Building Fire Alarm Panel","Ea",1]
["4.1.2","Transformer Fire Alarm Systems:"]
["4.1.2.1","Generator Transformer 1 Fire Alarm","Ea",1]
[null,"Panel"]
["4.1.2.2","Generator Transformer 2 Fire Alarm","Ea",1]
[null,"Panel"]
["4.1.2.3","Generator Transformer 3 Fire Alarm","Ea",1]
[null,"Panel"]
["4.1.2.4","Generator Transformer 4 Fire Alarm","Ea",1]
[null,"Panel"]
["4.1.2.5","Station Transformer 1 Fire Alarm Panel","Ea",1]
["4.1.2.6","Station Transformer 2 Fire Alarm Panel","Ea",1]
["4.1.2.7","Service Transformer 1 Fire Alarm Panel","Ea",1]
["4.1.2.8","Service Transformer 2 Fire Alarm Panel","Ea",1]
["4.1.3","Video Fire Alarm & Smoke Detection (VFSD) System:"]
["4.1.3.1","Control Room Client PC Alarm Monitor","Ea",1]
["4.1.3.2","Security Room Client PC Alarm Monitor","Ea",1]
["4.1.3.3","Equipment Rack","Ea",1]
["4.1.3.4","HUB Enclosures","Ea",17]
["4.1.3.5","Camera enclosures","Ea",54]
["4.1.3.6","Cameras","Ea",54]
["4.1.3.7","Lights","Ea",54]
["4.1.4","Aspiration Units:"]
["4.1.4.1","Unit 1 Generator Aspiration Unit","Ea",1]
["4.1.4.2","Unit 2 Generator Aspiration Unit","Ea",1]
["4.1.4.3","Unit 3 Generator Aspiration Unit","Ea",1]
["4.1.4.4","Unit 4 Generator Aspiration Unit","Ea",1]
["4.1.4.5","Lift Shaft Aspiration Unit","Ea",1]
["4.1.5","Beam Units:"]
["4.1.5.1","Unit 1 Spherical Valve Beam Unit","Ea",1]
["4.1.5.2","Unit 2 Spherical Valve Beam Unit","Ea",1]
["4.1.5.3","Unit 3 Spherical Valve Beam Unit","Ea",1]
["4.1.5.4","Unit 4 Spherical Valve Beam Unit","Ea",1]
["Total Bill 4"]

{"sheet":"Bill 5","index":4,"n_rows":8,"n_cols":7,"rows_kept":8,"merged":[[1,0,1,6],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,4,3,4],[7,0,7,4]]}
[]
["Bill 5: Yearly functional test of fire detectors:"]
["Item nr","Description","Unit","Expected","Rate","Price for","Total for 60"]
[{"$nulls":3},"Quantity",null,"Year 1","months"]
[5,"Yearly Functional Test intervals for the functional testing of fire detectors inclusive of all supervision, labour, and traveling costs of:"]
[5.1,"Aritech Fire Detectors","Ea",518]
[5.2,"VFSD Detectors (Cameras)","Ea",54]
["Total Bill 5"]

{"sheet":"Bill 6","index":5,"n_rows":14,"n_cols":6,"rows_kept":14,"merged":[[1,0,1,5],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[13,0,13,3]]}
[]
["Section 6:   Reactive Maintenance"]
["Item nr","Description","Unit","Expected Quantity","Rate","Price"]
[]
[6,"Bill No 12 – Pricing for Reactive maintenance per severity level conformance\n\nSeverity levels are defined in the scope of works and must be priced for availability and responses times indicated.  Response included, personnel with the correct level of expertise, reliable transport with major critical spares at hand","24/7","P/hour"]
[6.1,"Critical Level:\n\nWhen performance failures could result in a life or death situation and/or when performance failures can result in major damage to assets which will directly impact on the availability and performance of Essential Functions required for Power Generation. This level calls for immediate response (≤ 1 hour)","2/h",25]
[6.2,"Level 1: \n\nDuring working hours while turbines are in Generating mode and/or standby support outside of working hours where activities must be performed by highly qualified personnel or being supervised by one and/or when on-site critical spares holding is required to avoid failure. This level calls for a response within 1 to 3 hours","/h",25]
[6.3,"Level 2: \n\nNormal planned repair functions actioned during normal working hours by adequately trained personnel for work which have some degree of built- in redundancy and reserve capacity built in as part of the design, which require maintenance and support only during working hours and which require limited on-site spares holding. This level is requires an approved order, must be planned and must be performed during the planned week.","/h",50]
[6.4,"List of rates for additional resources (Office Hours)"]
["6.4.1","Supervisor of works","/h",5]
["6.4.2","Artisan","/h",5]
["6.4.3","Skilled Worker","/h",5]
["6.4.4","Unskilled Worker","/h",5]
["Total Bill 6"]

{"sheet":"Bill 7","index":6,"n_rows":70,"n_cols":5,"rows_kept":70,"merged":[[1,0,1,4],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[11,0,12,0],[11,2,12,2],[11,3,12,3],[11,4,12,4],[17,2,20,2],[17,3,20,3],[17,4,20,4],[25,0,26,0],[25,2,26,2],[25,3,26,3],[25,4,26,4],[69,0,69,3]]}
[]
["Bill 7: Spares:"]
["Item nr","Description","Unit","Expected Quantity","Total"]
[]
[7,"For the supply of the following spares:","each"]
[7.1,"UV Infrared Explosion Proof Flame Detector and Interface IR3_C3BRS-CC-452-080-C3BRS-CC-452-085","each",6]
[7.2,"Edwards FHSD8015-99 Laser Sense 10 Detector","each",4]
[7.3,"Aritech Panel FP1264C for TRFR and Main surface building","each",4]
[7.4,"Moxa Transio – TFC -142-S Serial to Fibre converter TCF-142-S- ST","each",3]
[7.5,"Long: Fire Resistant Cable, PH 30, 4\nCore x 1.5mm Square, \nOperating Voltage: 300/500V, \nMaximum Operating Temperature: 125 Degree Celsius, \nStranded Plain copper Class 5 Conductor, \nStandard Outer Sheath: Red.","m",300]
[7.6,"Ziton FDR50 – EZ\n\nAddressable loop powered reflective Beam Detector (50M) Brand: Ziton\nPart No.: 1108010\n Categories: Detection","each",4]
[7.7,"Filter Cartridge, Type 9-30755- P/LaserSense Nano/25/100 for LaserSense Smoke Detector, Width","each",30]
[null,"20mm x Height 44mm x Depth 77mm"]
[7.8,"Aritech Panel FP12** Used as repeater","each",1]
[7.9,"950 Series XP95 Optical Detector, DP951","each",100]
[7.1,"Moxa – SFP – 1GLXLC V1.1","each",2]
[7.11,"Aritech Conventional Panel for Head Race 1X-F4-xx","each",3]
[7.12,"Moxa EDS-510E-3GTXSFP V1.0.1","each",3]
[]
[]
[]
[7.13,"Power Supply for Aritech Panel FR1264N03,950 Protocol PS2000","each",9]
[7.14,"Network Card for Aritech Panel FR1264N03,950 Protocol NC2011","each",3]
[7.15,"650 Series Optical Smoke Detector, DP652","each",20]
[7.16,"SigniFire Video Analytic Camera, 2,8mm Lens complete","each",5]
[7.17,"Laser Sense 10 High Sensitivity Smoke Detector FHSD8015-99","each",4]
[null,"English"]
[7.18,"Aritech – 950 Mounting Base","each",6]
[7.19,"Field Server for Aritech Panel FR1264N03, 950 Protocol FS-B2010","each",1]
[7.2,"Conventional Fire Panel Language Kit","each",1]
[7.21,"Apollo Discovery Multi-Sensor (Optical/Heat) DP991T","each",10]
[7.22,"Sounder (KLAXON) TCC-0001","each",6]
[7.23,"Wall Sounder BF430C/CC/DR/65","each",6]
[7.24,"Aritech – Conventional Panel (FRG2064C-99)- global repeater","each",1]
[7.25,"Aritech Host CPU BD (FC2012)","each",4]
[7.26,"Battery CDD28JRY","each",6]
[7.27,"Apollo – Area Sounder Visiual Indicator Red (EN54-3:2001)","each",8]
[7.28,"Discovery Manual Call Point with Isolator (EN4-11:2001)","each",8]
[7.29,"PM86X series27.6 Vdc Switch Mode Power Supply","each",4]
[7.3,"5VDS 24V 5A Boxed PSU","each",4]
[7.31,"Moxa - Gigabit Managed Ethernet Switch; Input: 20; Output: 100; Specification: 20 10/100/1000BASET(X)","each",2]
[7.32,"Synaps Tech Sycall-R6847L","each",5]
[7.33,"Laser sensor","each",6]
[7.34,"Aritech Discovery Optical Smoke Detector DP991","each",30]
[7.35,"TYCO detector base (517.050.041)","each",5]
[7.36,"601P Conventional Optical Smoke Detector","each",5]
[7.37,"Aritech – FEP PCB (FEP2000N) FP2000","each",4]
[7.38,"Aritech – 16 Zone Extension Card (ZE2016)","each",5]
[7.39,"Aritech – SD2000","each",6]
[7.4,"Aritech – Keypad (KP2000) FP/FR1200/2000","each",7]
[7.41,"Aritech – Global RPTR (FRG 2064C-99) 16-642","each",1]
[7.42,"Aritech – LCD display for FP1200, FP12xx (LCD1200)","each",6]
[7.43,"Apollo - Sounder Control Unit XP95, 0956","each",5]
[7.44,"Aritech  -Lead Acid Rechargeable Battery, BS131N","each",20]
[7.45,"Aritech - Lead Acid Rechargeable Battery, BS127N","each",20]
[7.46,"Aritech - Heat Detector, DT992","each",5]
[7.47,"Aritech - 2Loop Ext Card (LC1502), 1200/200","each",15]
[7.48,"Aritech - PSU PCB (PS1200N), FP1200C/FP2000C","each",7]
[7.49,"Aritech - Host CPU BD (FC2012) 1200/2000 SRS","each",7]
[7.5,"Moxa EDS-510E-3GTXSFP V1.0.1","each",3]
[7.51,"Power supply, type: avi 12v 5a dc ups, input: 230 v, output: 12 vdc","each",10]
[7.52,"Apollo Input /Output Unit SA4700-302APO","each",10]
[7.53,"Aritech Panel FP1264C for TRFR and Main surface building","each",4]
[7.54,"Aritech Replacement filter used for HSSD2 and Modulaser","each",30]
[7.55,"Fire Resistant Cable, PH 120, 4\nCore x 1.5mm Square, Operating\nVoltage: 300/500V, Maximum\nOperating Temperature: 125 Degree\nCelsius, Stranded Plain copper Class\n5 Conductor, Standard Outer Sheath: Red.","each",300]
[7.56,"Surge arrestor DG MOD 275","each",10]
[7.57,"Camera Flood light","each",10]
[7.58,"Delivery of spares to Drakensberg","each",1]
[7.59,"Cost plus percentage","percentage"]
["Total Bill 7"]

{"sheet":"Summary","index":7,"n_rows":10,"n_cols":3,"rows_kept":10,"merged":[[0,0,0,2],[9,0,9,1]]}
["SUMMARY"]
["Item Nr","Description","Price"]
[1,"Bill No 1 - Preliminary"]
[2,"Bill No 2 – Monthly inspection, fault-finding & Restoring of Faults & Alarms of the Station Fire Alarm Systems"]
[3,"Bill No 3 – 3-Monthly inspection and servicing of fire alarm systems"]
[4,"Bill No 4 – Annual servicing of fire detection systems"]
[5,"Bill No 5 – Annual functional test of fire detectors"]
[6,"Bill No 6 – Reactive Maintenance"]
[7,"Bill No 7 – Spares"]
["                                               The total of the Prices"]