{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["ACS FULL"],"not_rendered":{"external_links":28,"defined_names":1026},"read":"whole","date_system":"1900"}

{"sheet":"ACS FULL","index":0,"n_rows":66,"n_cols":10,"rows_kept":66,"merged":[[0,0,2,9],[3,0,6,9],[8,1,8,9],[9,1,9,9],[10,4,41,4],[43,1,43,9],[44,4,55,4],[56,1,56,9],[61,0,61,6],[64,0,64,1]]}
["ANNEXURE A"]
[]
[]
[" INSTALLATION  CCTV SYSEM SASSA EC REGION"]
[]
[]
[]
["Item ","Description","Unit","Qty per site","No. of Sites","Total Qty","Supply","Install","Unit Price","Total Price"]
[]
["1","3 x SASSA EC Offices (Regional Office, Idutywa and Qonce local Office)"]
[{"$nulls":4},3]
["1.1","4MP PTZ 25x zoom  Darkfighter H.265/H.264 Camera HD-1520P, Triple Streams, array IR LEDS (150m), 3D Noise Reduction, Wide Dynamic Range Extreme (120dB), Audio in/out, Alarm in/out, SD card slot 128GB, Smart Video Content Analytics, IP66, DC 12V, POE. ","Each",1,null,3,"Supply ","Install"]
[]
["1.2","True Day Night IP H.265 Bullet Panoramic 180 degree Camera, Sony StarVis Starlight/ Equivalent 8.0MP, Triple Streams, 4x 2.8mm lenses internally stitched, array IR LEDS (30m), 3D Noise Reduction, Wide Dynamic Range Extreme (120dB), Audio in/out, Alarm in/out, IP66, DC 12V, POE.","Each",2,null,6,"Supply","Install"]
[]
["1.3","Junction box for panoramic style bullet IP Cameras","Each",2,null,6,"Supply","Install"]
[]
["1.4","CAT6 Network cable and point installation for Controller to main building security network","Meter",8400,null,{"$f":"SUM(D18*E11)","v":25200},"Supply","Install"]
[]
["1.5","9\" Equipment rack. 9U floor standing including 2x 5way power distribution, extraction fans, sides and lockable doors front and back. 600mm deep. Sufficient blanking panels included. 19\" trays for equipment.","Each",1,null,{"$f":"SUM(D20*E11)","v":3},"Supply","Install"]
[]
["1.6","All required equipment including,  trays,  cassettes, SM pig tails, SM patch leads, patch panels,brush panels, labelling and management","LOT",2,null,{"$f":"SUM(D22*E11)","v":6},"Supply"]
[]
["1.7","4 Core single mode fibre optic cable installed, spliced both ends including sleeves and trenching if required. OTDR Test.","Meter",100,null,{"$f":"SUM(D24*E11)","v":300},"Supply","Install"]
[]
["1.8","Layer 2 Managed 24Port 100/1000 PoE Switch with 4x Gigabit uplinks SFP - 400 watt internal power supply","Each",1,null,{"$f":"SUM(D26*E11)","v":3},"Supply","Install"]
[]
["1.9","Gigabit GBIC 1.25G, 1310nm SMF, 20km LX, Duplex LC, DDM","Each",2,null,{"$f":"SUM(D28*E11)","v":6},"Supply","Install "]
[]
["1.10","32 Channel Realtime 4K Network Video Recorder (NVR), H.265/H.264/MJPEG, HDMI, USB Backup, 4 Alarm input/1 Alarm outputs, 1X E-SATA, RS-485, VGA & Smart phone access (FSEYE App), SMART VIDEO ANALYSIS, 8 X SATA HDD, DC 12V, 2U (NO STORAGE INCLUDED), RAID support. Supports 36 channels @ 1.3MP, 2MP, 3MP, 4MP, 5MP & 4K","Each",2,null,2,"Supply","Install"]
[]
["1.11","8TB SATA Surveillance specified hard drives (Installed and tested)","Each",4,null,{"$f":"SUM(D32*E11)","v":12},"Supply","Install"]
[]
["1.12","16 Channel Realtime 4k Network Video Recorder(NVR)H.265/H.264/MPEG/HDMI…","Each",2,null,2,"Supply","Install"]
[]
["1.13","RJ 45 Connectors & boots, cable labelling, cable ties, sprag, PVC Conduit (internal), Bosal conduit (external) and required CAT6 accessories","LOT",1,null,3,"Supply","Install"]
[]
["1.14","Sundries and consumables","LOT",1,null,3,"Supply"]
[]
["1.15","Travelling, transport, delivery, accommodation, meals, subsistence allowances","LOT",1,null,3]
[]
["1.16","Project management, Commissioning and commercial costs","LOT",1,null,3]
["1.17","Installation of existing cameras at 3 Offices","LOT","3",null,84,"N/A","Install"]
["2","Linking of 2 x Sites systems to the IT infrastructure of SASSA including setting up of Admin PC"]
["2.1","27\" LED Displays and Desktop PC mount including cables","Each","1",null,2,"Supply","Install"]
[]
["2.2","Allow for all factors required for the testing, commissioning and handover of the system as specified","LOT",null,null,1]
[]
["2.3","System Commissioning ","Lot",null,null,1]
[]
["2.4","Project Management","Lot",null,null,1]
[]
["2.5","Setup Testing and Commissioning","Lot",null,null,1]
[]
["2.6","Integration testing","Lot",null,null,1]
[]
["3","DOCUMENTATION"]
["3.1","As-built drawings for the systems","Each",null,null,3,"Supply"]
[]
["SUBTOTAL",{"$nulls":6},{"$f":"SUM(H11:H59)","v":0},{"$f":"SUM(I11:I59)","v":0},{"$f":"SUM(J11:J59)","v":0}]
[{"$nulls":7},"VAT"]
[{"$nulls":7},"Grand Total",null,{"$f":"SUM(J60+J61)","v":0}]
[]
["NB: Please note this SASSA Bill of quantities consists of 2 x remote sites with a total of 20 x cameras + 2 NVR installations , Regional office has a total of 64 x cameras and"]
["2 X NVR installations."]
["Atleast 12 months warranty on supplied equipment"]