{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["BOQ","SUMMARY"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"BOQ","index":0,"n_rows":1043,"n_cols":8,"rows_kept":1043,"merged":[[53,1,53,6],[54,1,54,7],[56,1,56,7],[57,1,57,7],[59,1,59,6],[107,1,107,6],[108,1,108,7],[109,1,109,7],[110,1,110,7],[111,1,111,7],[113,1,113,6],[162,1,162,6],[163,1,163,7],[164,1,164,7],[165,1,165,7],[166,1,166,7],[217,1,217,6],[218,1,218,7],[220,1,220,3],[221,1,221,7],[272,1,272,6],[273,1,273,7],[274,1,274,7],[275,1,275,7],[276,1,276,7],[327,1,327,6],[328,1,328,7],[329,1,329,7],[330,1,330,7],[332,1,332,6],[382,1,382,6],[383,1,383,7],[384,1,384,7],[385,1,385,8],[386,1,386,7],[438,1,438,6],[439,1,439,7],[440,1,440,9],[441,1,441,7],[442,1,442,7],[494,1,494,6],[495,1,495,7],[496,1,496,7],[497,1,497,7],[498,1,498,7],[550,1,550,6],[551,1,551,7],[552,1,552,7],[553,1,553,7],[554,1,554,7],[605,1,605,6],[606,1,606,7],[608,1,608,7],[609,1,609,7],[660,1,660,6],[661,1,661,7],[662,1,662,7],[663,1,663,7],[664,1,664,7],[714,1,714,6],[715,1,715,7],[716,1,716,7],[717,1,717,7],[718,1,718,7],[720,1,720,6],[769,1,769,6],[770,1,770,7],[772,1,772,7],[773,1,773,7],[825,1,825,6],[828,1,828,7],[829,1,829,7],[880,1,880,6],[881,1,881,7],[883,1,883,7],[884,1,884,7],[936,1,936,6],[937,1,937,7],[939,1,939,7],[940,1,940,7],[991,1,991,6],[992,1,992,7],[994,1,994,7],[995,1,995,7],[1042,1,1042,6]]}
[null,"SERIES 0: GENERAL"]
[null,"SECTION 001:  GENERAL REQUIREMENTS AND CHARGES"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 0: GENERAL"]
[]
[null,"001",null,"SECTION 001: GENERAL REQUIREMENTS AND CHARGES"]
[]
[null,"B001.01",null,"Preliminary and General "]
[]
[null,"001.01.01",null,"Fixed charges","Lump Sum",1]
[]
[null,"B001.01.02",null,"Time-related charges","Month",18]
[]
[null,"001.02",null,"Locating existing services","Lump Sum",1]
[]
[null,"001.03",null,"Excavate by hand to expose existing services and backfill","m3",40]
[]
[null,"001.04",null,"Compliance with Occupational Health and Safety Act and applicable regulations"]
[]
[null,"B001.04.01",null,"Provision and Implementation of a Health and Safety Plan","Lump Sum",1]
[]
[null,"B001.04.02",null,"Provision of Health and Safety File","Lump Sum",1]
[]
[null,"B001.04.03",null,"Provision of Construction Supervisors","Lump Sum",1]
[]
[null,"001.04.04",null,"Provision of a SACPCMP registered Safety Officer (Full-time)","Month",18]
[]
[null,"B001.04.05",null,"Provision of Health and Safety Training","Lump Sum",1]
[]
[null,"001.04.06",null,"Provision of Personal Protective Clothing and Equipment","Lump Sum",1]
[]
[null,"001.04.07",null,"Provision of Safety Fences, Signs and Barricades","Lump Sum",1]
[]
[null,"001.04.08",null,"Other obligations"]
[]
[null,"001.04.08.01",null,"Medical Entry and Exit for Employees","Lump Sum",1]
[]
[null,"001.04.08.02",null,"Compliance with the Environmental Management Plan.  Allow only for adapting working methods and programmes to comply","Lump Sum",1]
[]
[null,"001.04.08.03",null,"Project Name Boards","No.",2]
{"$rows_empty":12}
[null,"TOTAL SECTION 001 CARRIED FORWARD"]
[]
[]
[null,"SERIES 0: GENERAL"]
[null,"SECTION 001:  GENERAL REQUIREMENTS AND CHARGES"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[null,"BROUGHT FORWARD"]
[]
[null,"001.04.08.05",null,"Provision of accommodation of traffic during pipe jacking","Provisional Sum",1,"-",{"v":250000,"d":"R 250,000.00"}]
[]
[null,"B001.05",null,"Community Liaison Officer (Task Level 5)","Provisional Sum",1,"-",{"v":360000,"d":"R 360,000.00"}]
[]
[null,"B001.05.01",null,"Handling Cost and Charges for the Contractor on Item B001.05","%",{"v":360000,"d":"R 360,000.00"}]
[]
[null,"B001.08",null,"Training of Targeted Labourers ","Provisional Sum",1,"-",{"v":300000,"d":"R 300,000.00"}]
[]
[null,"B001.09",null,"Appointment Of Local (Grade C and D) Security Company For The Duration Of Project","Lump Sum",1]
[]
[null,"B001.10",null,"Dayworks "]
[]
[null,"B001.10.01",null,"Provision of skilled, semi-skilled and unskilled labour."]
[]
[null,"B001.10.01.01",null,"Unskilled labour","hr",1]
[]
[null,"B001.10.01.02",null,"Semi-skilled labour ","hr",1]
[]
[null,"B001.10.01.03",null,"Skilled labour","hr",1]
[]
[null,"B001.10.01.04",null,"Foreman ","hr",1]
[]
[null,"B001.10.02",null,"Construction Plant Hire (use of plant already established on site for dayworks)"]
[]
[null,"B001.10.02.01",null,"Tipper truck (3 – 5 ton)","hr",1]
[]
[null,"B001.10.02.02",null,"Tipper truck (more than 5 ton)","hr",1]
[]
[null,"B001.10.02.03",null,"Loader (0.5m3 bucket)","hr",1]
[]
[null,"B001.10.02.04",null,"Compactor (Roller)","hr",1]
[]
[null,"B001.10.02.05",null,"Water tanker (5 000 Ltr)","hr",1]
[]
[null,"B001.10.02.06",null,"Water tanker (10 000 Ltr)","hr",1]
{"$rows_empty":11}
[null,"TOTAL SECTION 001 CARRIED FORWARD "]
[]
[]
[null,"SERIES 0: GENERAL"]
[null,"SECTION 001:  GENERAL REQUIREMENTS AND CHARGES"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[null,"BROUGHT FORWARD"]
[]
[null,"B001.10.02.07",null,"Flatbed truck (5 ton)","hr",1]
[]
[null,"B001.10.02.08",null,"Light delivery vehicle","hr",1]
[]
[null,"B107.04",null,"Transport of Construction Plant","km",1]
[]
[null,"B001.11",null,"Protection, Removal, Realignment And Replacement Of Services"]
[]
[{"$nulls":3},"a)     Utility services:"]
[]
[{"$nulls":3},"(i)     Relocation Of Services And Payments to Service Owners","Provisional Sum",1,"-",{"v":500000,"d":"R 500,000.00"}]
[]
[{"$nulls":3},"(ii)    Handling cost And Profit in respect of item B001.11 (a) (i)","%",{"v":500000,"d":"R 500,000.00"}]
{"$rows_empty":34}
[null,"TOTAL SECTION 001 CARRIED FORWARD TO SUMMARY"]
[]
[]
[null,"SERIES 0: GENERAL"]
[null,"SECTION 002:  ENGINEER'S ACCOMMODATION"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 0: GENERAL"]
[]
[null,"002",null,"SECTION 002:  ENGINEER'S ACCOMMODATION"]
[]
[null,"002.01",null,"Services And Accommodation:"]
[]
[null,"B002.01.01",null,"Offices and laboratory accommodation","Month",18]
[]
[null,"002.01.02",null,"Services for cooking and ablution facilities on Site for the Engineer's Site staff","Lump Sum",1]
[]
[null,"B002.02","LI","Treatment and maintenance of areas surrounding offices and laboratories","Month",18]
[]
[null,"B002.03",null,"Provision of Survey Equipment and Assistants","Month",18]
{"$rows_empty":35}
[null,"TOTAL SECTION 002 CARRIED FORWARDTO SUMMARY"]
[]
[]
[null,"SERIES 0: GENERAL"]
[null,"SECTION B003:  TRAINING AND DEVELOPMENT"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 0: GENERAL"]
[]
[null,"B003",null,"SECTION B003:  TRAINING AND DEVELOPMENT"]
[]
[null,"B003.05.01",null,"Provision of Accredited Technical Skills Training","Provisional Sum",1,"-",{"v":200000,"d":"R 200,000.00"}]
[]
[{"$nulls":3},"(a)   Handling Cost and Charges for the Contractor on Item B003.05.01","%",{"v":200000,"d":"R 200,000.00"}]
{"$rows_empty":41}
[null,"TOTAL SECTION 003 CARRIED FORWARDTO SUMMARY "]
[]
[]
[null,"SERIES 1: ANCILLARY WORK"]
[null,"SECTION 101: SITE CLEARING AND GRUBBING"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 1: ANCILLARY WORK"]
[]
[null,101,null,"SECTION 101: SITE CLEARING AND GRUBBING"]
[]
[null,"101.01",null,"Clearing and grubbing:"]
[]
[null,"101.01.01","SC","Area","m²",{"v":5720,"d":"5,720"}]
[]
[null,"101.02",null,"Cutting and removing large trees with girth:"]
[]
[null,"101.02.01","SC","Exceeding 1 m and up to and including 2 m","No.",5]
[]
[null,"101.02.02","SC","Exceeding 2 m and up to and including 3 m","No.",1]
[]
[null,"101.02.03","SC","Exceeding 3 m and up to and including 4 m","No.",1]
[]
[null,"101.03",null,"Grubbing and the removal of the stumps and roots of large trees with a girth:"]
[]
[null,"101.03.01","SC","Exceeding 1 m and up to and including 2 m","No.",5]
[]
[null,"101.03.02","SC","Exceeding 2 m and up to and including 3 m","No.",1]
[]
[null,"101.03.03","SC","Exceeding 3 m and up to and including 4 m","No.",1]
[]
[null,"101.04",null,"Re-clearing areas (only on the written instructions of the Engineer)"]
[]
[null,"101.04.01 ","SC","Strips (4 m wide on pipeline route for rising main)","m",250]
[]
[null,"101.04.02 ","SC","Areas not classified as strips (parking area)","m²",300]
[]
[null,"101.05",null,"Removal and disposal of specific elements"]
[]
[null,"101.05.01","SC","Concrete kerbing / kerbing combination","m",880]
{"$rows_empty":15}
[null,"TOTAL SECTION 101 CARRIED FORWARD"]
[]
[null,"SERIES 1: ANCILLARY WORK"]
[null,"SECTION 101: SITE CLEARING AND GRUBBING"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[null,"BROUGHT FORWARD"]
[]
[null,"101.05.02","SC","Concrete or brick elements (reinforced or unreinforced)"]
[]
[null,"101.05.02.01","SC","Foundations and floor slabs of building / valve boxes.","m³",200]
[]
[null,"101.05.02.02 ","SC","Walls of building / valve boxes","m³",200]
[]
[null,"101.05.02.03 ","SC","Asphalt Surfacing","m2",700]
{"$rows_empty":41}
[null,"TOTAL SECTION 101 CARRIED FORWARDTO SUMMARY"]
[]
[]
[null,"SERIES 1: ANCILLARY WORKS"]
[null,"SECTION 104: LANDSCAPING AND GRASSING"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 1: ANCILLARY WORKS"]
[]
[null," 104",null,"SECTION 104: LANDSCAPING AND GRASSING"]
[]
[null,"104.03",null,"Preparing areas for grassing and ground covers"]
[]
[null,"104.03.02",null,"Top soiling on the Site with: "]
[]
[null,"104.03.02.01","LI","Topsoil obtained from the Site","m³",150]
[]
[null,"104.03.02.02",null,"Topsoil provided by the Contractor from other sources","m³",150]
[]
[null,"104.03.05","LI","Stockpiling of topsoil","m³",150]
[]
[null,"104.04",null,"Grassing"]
[]
[null,"104.04.01",null,"Hydroseeding "]
[]
[null,"104.04.04.01",null,"Providing approved seed mixture for hydroseeding","kg",5]
[]
[null,"104.04.04.02",null,"Hydroseeding","ha",1]
[]
[null,"104.07",null,"Trees, shrubs and ground covers"]
[]
[null,"104.07.01","SC","Provision of trees and shrubs","No",30]
[]
[null,"104.07.02","SC","Provision of ground covers","No",10]
[]
[null,"104.07.03","SC","Planting and Establishing of: "]
[]
[null,"104.07.03.01","SC","Trees","No",30]
[]
[null,"104.07.03.03","SC","Ground Covers","No",10]
[]
[null,"104.08",null,"Extra work for landscaping","Provisional Sum"," 1","-",{"v":20000,"d":"R 20,000.00"}]
{"$rows_empty":14}
[null,"TOTAL SECTION 104 CARRIED FORWARDTO SUMMARY"]
[]
[]
[null,"SERIES 1: ANCILLARY WORKS"]
[null,"SECTION 105: FENCING"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 1: ANCILLARY WORKS"]
[]
[null,105,null,"SECTION 105: FENCING"]
[]
[null,"105.01","SC","Supply and Erection of new Fencing Material "]
[]
[null,"B105.01.07",null,"Fencing (Concrete Palisade)","m",100]
[]
[null,"105.06",null,"Provision of Temporary Fencing"]
[]
[null,"105.06.01",null,"Ordinary ","m",160]
{"$rows_empty":38}
[null,"TOTAL SECTION 105 CARRIED FORWARDTO SUMMARY"]
[]
[]
[null,"SERIES 2: EARTHWORKS"]
[null,"SECTION 202: TRENCHING"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 2: EARTHWORKS"]
[]
[null,202,null,"SECTION 202: TRENCHING"]
[]
[null,"202.01",null,"Trench excavations"]
[]
[null,"202.01.01",null,"Up to 1,0 m wide"]
[]
[null,"202.01.01.01",null,"Over 1.5m and up to 2.0m deep","m³","-",null,"Rate Only"]
[]
[null,"202.01.01.02",null,"Over 2.0m and up to 2.5m deep","m³",120]
[]
[null,"202.01.01.03",null,"Over 2.5m and up to 3.0m deep","m³",150]
[]
[null,"202.01.01.04",null,"Over 3.0m and up to 3.5m deep","m³",110]
[]
[null,"202.01.01.05",null,"Over 3.5m and up to 4.0m deep","m³",50]
[]
[null,"202.01.02",null,"Over 1.0m and up to 2.0m wide"]
[]
[null,"202.01.02.01",null,"Over 1.5m and up to 2.0m deep","m³",300]
[]
[null,"202.01.02.02",null,"Over 2.0m and up to 2.5m deep","m³",{"v":2500,"d":"2,500"}]
[]
[null,"202.01.02.03",null,"Over 2.5m and up to 3.0m deep","m³",400]
[]
[null,"202.01.02.04",null,"Over 3.0m and up to 3.5m deep","m³",90]
[]
[null,"202.01.02.05",null,"Over 3.5m and up to 4.0m deep","m³",90]
[]
[null,"202.01.02.06",null,"Over 4.0m and up to 4.5m deep","m³",300]
[]
[null,"202.01.02.07",null,"Over 4.5m and up to 5.0m deep","m³",250]
[]
[null,"202.01.02.08",null,"Over 5.0m and up to 5.5m deep","m³",900]
[]
[null,"202.02",null,"Extra over item 202.01 for excavating in"]
[]
[null,"202.02.01",null,"Intermediate material","m³",900]
{"$rows_empty":10}
[null,"TOTAL SECTION 202 CARRIED FORWARD TO SUMMARY"]
[]
[]
[null,"SERIES 2: EARTHWORKS"]
[null,"SECTION 202: TRENCHING"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 2: EARTHWORKS"]
[]
[null,202,null,"SECTION 202: TRENCHING"]
[]
[null,"202.02.02",null,"Hard material","m³",700]
[]
[null,"202.03",null,"Excavations outside the normal trench profile","m³",950]
[]
[null,"202.04","LI","Hand excavation (extra over item 202.01)","m³",230]
[]
[null,"202.06","LI","The backfilling of trenches (excluding selected backfill around /and the pipe barrel) with material obtained from excavations","m³",{"v":2850,"d":"2,850"}]
[]
[null,"B202.07",null,"Extra over items 202.06 for using backfill material obtained:"]
[]
[null,"B202.07.03",null,"G5 provided by Contractor ","m³",{"v":1700,"d":"1,700"}]
[]
[null,"202.10",null,"Removal of spoil material"]
[]
[null,"202.10.02",null,"To dumping areas to be provided by the Contractor","m³",{"v":1700,"d":"1,700"}]
[]
[null,"B202.11",null,"Timbering And Shoring Left in Excavation","m2",{"v":9600,"d":"9,600"}]
[]
[null,"202.15",null,"Reinstatement of bitumen surfaced roads","m2 ",750]
[]
[null,"B202.16",null,"Cutting and Removal Of Premix"]
[]
[null,"B202.16.01",null,"Premix thickness up to 100mm","m2 ",750]
[]
[null,"B202.17",null,"Hand Excavations For Trenches inside erven trenches 500mm wide and 600mm deep","m3 ",450]
{"$rows_empty":19}
[null,"TOTAL SECTION 203 CARRIED FORWARD TO SUMMARY"]
[]
[]
[null,"SERIES 5: DRAINAGE AND EROSION PROTECTION"]
[null,"SECTION 501: SUBSURFACE DRAINS AND DRAINAGE BLANKETS"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 5: DRAINAGE AND EROSION PROTECTION"]
[]
[null,501,null,"SECTION 501: SUBSURFACE DRAINS AND DRAINAGE BLANKETS"]
[]
[null,"501.01","LI","Crushed stone"]
[]
[null,"501.01.01",null,"19mm graded crushed stone","m³",180]
[]
[null,"501.04","LI","Geotextiles"]
[]
[{"$nulls":3},"(a) Class A6","m²",{"v":1900,"d":"1,900"}]
[]
[null,"501.05",null,"Pipes in subsurface drains"]
[]
[null,"501.05.01",null,"Unplasticized PVC pipes and fittings, normal duty complete with couplings"]
[]
[null,"501.05.01.01",null,"160mm internal diameter, perforated or slotted","m",330]
[]
[null,"501.05.04",null,"PVC UG Junction 160 x 45 deg","No.",4]
[]
[null,"501.07",null,"Concrete outlet structures for subsurface drains including formwork (Concrete class 15/19)","m³",1]
[]
[null,"501.08",null,"Concrete caps for subsurface drainpipes","No.",2]
[]
[null,"B501.09",null,"Complete rodding eye","No.",4]
{"$rows_empty":23}
[null,"TOTAL SECTION 501 CARRIED FORWARD TO SUMMARY"]
[]
[]
[null,"SERIES 5: DRAINAGE AND EROSION PROTECTION"]
[null,"SECTION 502: PREFABRICATED CULVERTS AND STORMWATER DRAINAGE"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 5: DRAINAGE AND EROSION PROTECTION"]
[]
[null,502,null,"PREFABRICATED CULVERTS AND STORMWATER DRAINAGE"]
[]
[null,"502.01","LI","Backfilling with excavated selected material compacted to:"]
[]
[null,"502.01.03",null,"95% Modified AASHTO","m³",{"v":1600,"d":"1,600"}]
[]
[null,"502.02","LI","Supplying and laying of concrete pipe culverts (type SC-pipes)"]
[]
[null,"502.02.01",null,"Class B bedding, Class 50D"]
[]
[null,"502.02.01.01",null,"450mm","m",130]
[]
[null,"502.02.01.02",null,"600mm","m",{"v":1350,"d":"1,350"}]
[]
[null,"502.10",null,"Cast in situ concrete"]
[]
[null,"502.10.03",null,"Inlet and outlet structures, catchpits, manholes and junction boxes excluding form-work, but including class U2 surface finish"]
[]
[null,"502.10.03.01",null,"Class 15/19","m³",18]
[]
[{"$nulls":3},"Class 20/19","m³",10]
[]
[{"$nulls":3},"Class 25/19","m³",10]
[]
[null,"502.16",null,"Manholes, catchpits, precast inlet and outlet structures and junction boxes complete"]
[]
[null,"502.16.01",null,"Manholes for depths up to 2.0m"]
[]
[{"$nulls":3},"(a) 450mm diameter pipe","No",3]
[]
[{"$nulls":3},"(b) 600mm diameter pipe","No",30]
[]
[null,"502.16.03",null,"Precast inlet and outlet structures"]
[]
[{"$nulls":3},"Field inlet "]
[]
[{"$nulls":3},"(a) 600mm diameter pipe","No",1]
{"$rows_empty":8}
[null,"TOTAL SECTION 502 CARRIED FORWARD "]
[]
[]
[null,"SERIES 5: DRAINAGE AND EROSION PROTECTION"]
[null,"SECTION 502: PREFABRICATED CULVERTS AND STORMWATER DRAINAGE"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[null,"BROUGHT FORWARD"]
[]
[{"$nulls":3},"Complete As per Drawing Outlet structure to accommodate; "]
[]
[{"$nulls":3},"(a)  600mm diameter pipe","No",1]
[]
[null,"502.16.05",null,"Junction boxes to accommodate pipe sizes of the following range:"]
[]
[{"$nulls":3},"(a) 450mm diameter pipe","No",1]
[]
[{"$nulls":3},"(b) 600mm diameter pipe","No",6]
[]
[null,"502.16.06",null,"Extra over or under item 502.16.01 for variation in depth of manholes from the standard depth designated for purposes of tendering (Type A)","m",20]
[]
[null,"502.17",null,"Brickwork"]
[]
[null,"502.17.02",null,"230mm thick","m²",120]
[]
[null,"502.17.03",null,"345mm thick","m²",330]
[]
[null,"502.17.04",null,"460mm thick","m²",300]
[]
[null,"502.18",null,"Plaster","m²",50]
[]
[null,"502.22",null,"Extra over items 502.01 for using backfill material obtained"]
[]
[null,"502.22.02",null,"From sources provided by Contractor","m³",{"v":1600,"d":"1,600"}]
[]
[null,"502.23",null,"Cleaning of existing culverts","m³",20]
{"$rows_empty":20}
[null,"TOTAL SECTION 502 CARRIED FORWARDTO SUMMARY"]
[]
[]
[null,"SERIES 5: DRAINAGE AND EROSION PROTECTION"]
[null,"SECTION 503: KERBING AND CHANNELLING"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 5: DRAINAGE AND EROSION PROTECTION"]
[]
[null,503,null,"SECTION 503: KERBING AND CHANNELLING"]
[]
[null,"503.01","SC","Concrete kerbing, class 25 MPa"]
[]
[null,"503.01.01",null,"Fig 8b to SANS 927: 2022","m",20]
[]
[null,"503.01.02",null,"Fig 4 to SANS 927: 2022","m",30]
[]
[null,"503.01.03",null,"Fig 8c to SANS 927: 2022","m",30]
{"$rows_empty":38}
[null,"TOTAL SECTION 503 CARRIED FORWARDTO SUMMARY"]
[]
[]
[null,"SERIES 5: DRAINAGE AND EROSION PROTECTION"]
[null,"SECTION 505: EROSION PROTECTION"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 5: DRAINAGE AND EROSION PROTECTION"]
[]
[null,505,null,"SECTION 505: EROSION PROTECTION"]
[]
[null,"505.01",null,"Foundation trench excavation and backfilling:"]
[]
[null,"505.01.02",null,"In all other classes of material","m³",20]
[]
[null,"505.02","SC","Surface preparation for the bedding of gabions","m²",20]
[]
[null,"505.03","SC","Gabions"]
[]
[null,"505.03.01",null,"Gabion boxes (2 x 1 x 0,5m box from 80 x 100 x 2,7mm Class A galvanized wire mesh)","m³",10]
[]
[null,"505.03.02",null,"Gabion mattresses (2 x 1 x 0,3 mattresses, 80 x 100 2,5mm Class A galvanized wire) ","m³",10]
[]
[null,"505.05","SC","Filter fabric for precast retaining wall blocks, gabions and riprap (non-woven geotextile or similar)","m²"," 30"]
{"$rows_empty":31}
[null,"TOTAL SECTION 505 CARRIED FORWARD TO SUMMARY"]
[]
[]
[null,"SERIES 6: ROADS AND PARKING AREAS"]
[null,"SECTION 601: GRAVEL PAVEMENT LAYERS"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 6: ROADS AND PARKING AREAS"]
[]
[null,601,null,"SECTION 601: GRAVEL PAVEMENT LAYERS"]
[]
[null,"601.01",null,"Preparation and compaction of in situ subgrade material to"]
[]
[null,"601.01.02",null,"93% of modified AASHTO density","m³",120]
[]
[null,"601.03",null,"Gravel layers constructed from material obtained from commercial sources"]
[]
[null,"601.03.01",null,"Subgrade"]
[]
[null,"601.03.01.02",null,"Compacted to 93% of modified AASHTO density","m³",120]
[]
[null,"601.03.02",null,"Subbase"]
[]
[null,"601.03.02.02",null,"Compacted to 95% of modified AASHTO density","m³",120]
[]
[null,"601.03.03",null,"Base "]
[]
[null,"601.03.03.01",null,"Compacted to 98% of modified AASHTO density","m³",120]
{"$rows_empty":28}
[null,"TOTAL SECTION 601 CARRIED FORWARD TO SUMMARY"]
[]
[]
[null,"SERIES 8: SPECIFIC WORKS"]
[null,"SECTION 805: BUILD"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 8: SPECIFIC WORKS"]
[]
[null,804,null,"SECTION 804: PIPE JACKING AND BORING"]
[]
[null,"804.01","SC","Establishment on site for:"]
[]
[null,"804.01.01 ","SC","Pipe jacking","Lump Sum",1]
[]
[null,"804.02","SC","Access to and from the thrust and reception pits","Lump Sum",1]
[]
[null,"804.03","SC","Excavating in soft material for:"]
[]
[null,"804.03.01 ","SC","Thrust and reception pits","Lump Sum",1]
[]
[null," 804.04","SC","Extra over item 804.03 for excavating hard material","m3",20]
[]
[null,"804.05","SC","Backfilling the:"]
[]
[null,"804.05.01","SC","Thrust and reception pits with:"]
[]
[null,"804.05.01.01","SC","Excavated Material","m3",10]
[]
[null,"804.05.01.02","SC","Imported Material","m3",10]
[]
[null,"804.06","SC","Supply of Reinforced concrete pipes Class 100D, SC type joints to SANS 677 to be jacked to the following diameters:"]
[]
[null," 804.06.01"," SC","600 mm Nominal dia","m",45]
[]
[null,"804.06.02","SC","900 mm Nominal dia","m",45]
[]
[null,"804.07","SC","Jacking of pipes through:"]
[]
[null,"804.07.01","SC","Soft Material","m3",40]
[]
[null,"804.07.02","SC","Hard Material","m3",40]
[]
[null,"804.10","SC","The grout of voids pipe jacking:"]
[]
[null,"804.10.01",null,"Unforeseen and exposed during jacking","kg",200]
[]
[null,"804.10.02","SC","Between pipeline and surrounding material after jacking has been completed:"]
[]
[null,"804.10.02.01"," SC","600 mm Nominal dia","m",50]
[]
[null,"804.10.02.02","SC","900 mm Nominal dia","m",50]
[]
[]
[]
[null,"TOTAL SECTION 804 CARRIED FORWARD TO SUMMARY"]
[]
[]
[null,"SERIES 9: QUALITY CONTROL"]
[null,"SECTION 903: TESTING"]
[null,"Item ","LI/SC","Description","Unit","Quantity","Rate"," Amount  "]
[]
[{"$nulls":3},"SERIES 9: QUALITY CONTROL"]
[]
[null,903,null,"SECTION 903: TESTING"]
[]
[null,"903.06",null,"Other special tests requested by the Engineer"]
[]
[null,"903.06.01",null,"Cost of testing","Provisional Sum",1,"-",{"v":100000,"d":"R 100,000.00"}]
[]
[null,"903.06.02",null,"Charge on prime cost sum","%",{"v":100000,"d":"R 100,000.00"}]
{"$rows_empty":35}
[null,"TOTAL SECTION 903 CARRIED FORWARD TO SUMMARY"]

{"sheet":"SUMMARY","index":1,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2]]}
[null,"SECTION","DESCRIPTION","AMOUNT"]
[null,"001","GENERAL REQUIREMENTS AND CHARGES"]
[null,"002","ENGINEER’S ACCOMMODATION"]
[null,"003","TRAINING AND DEVELOPMENT"]
[null,101,"SITE CLEARING AND GRUBBING"]
[null,104,"LANDSCAPING AND GRASSING"]
[null,105,"FENCING"]
[null,202,"TRENCHING"]
[null,501,"SUBSURFACE DRAINS AND DRAINAGE BLANKETS"]
[null,502,"PREFABRICATED CULVERTS AND STORMWATER DRAINAGE"]
[null,503,"KERBING AND CHANNELLING"]
[null,505,"EROSION PROTECTION"]
[null,601,"GRAVEL PAVEMENT LAYERS"]
[null,804,"PIPE JACKING AND BORING"]
[null,903,"TESTING"]
[null,"SUB-TOTAL A"]
[null,"Add 10% for Contingencies on SUB – TOTAL A"]
[null,"SUB-TOTAL B"]
[null,"Add 10% for CPA on SUB – TOTAL B"]
[null,"SUB-TOTAL C "]
[null,"Add 15% VAT on SUB – TOTAL C"]
[null,"TOTAL TENDER PRICE CARRIED TO FORM OF OFFER"]