Reception Renovations (Entrance)

1. Remove the old tiles (from outside reception entrance ,foyer,passage and toilets) – or tile over if more practical (check door clearance)
2. Supply and install tiles ground pearl mat 600X1200 at the reception (non-slip, no-chip, durable, extra box or two need to be supplied) supply to come and confirm measurements
3. Reception wall to be plastered and painted with a light beige colour (washable enamel paint)
4. Reception frames to be re-painted in dark brown colour (all preparations for painting to be done as well, paint fit for use indoors on metal)
5. Supply and install two Bright Star Lighting 3 Light Spotlight - Black (50W) x3
6. Reception wood desk to be restored (to sand and vanished the wood)

Toilets renovation

1. Remove the old toilets suite (taps,basin,soap dispenser,mirrors,old celling, wall tiles and light fittings)
2. Rooms for the removal are Room A29, A26, A6 and A7
3. Supply and install new toilets suite, taps, basins, soap dispensers, mirrors, replace old celling and light fittings) as per the pictures in all rooms A26, A29, A6 and A7
4. Supply a dissability bathroom that comply to standards of OHS officer room A29
5. Supply and install paper towel dispensers in all bathrooms as per picture below
6. Supply and install Lusso pescara basin mixer taps for all x 4 rooms 3 taps for the basins
7. Supply and istall soap dispensers in all bathrooms as per picuture below
8. Supply and install new ceiling boards and paint it white
9. Supply and install movement sensor down lights
10. Supply and install 7x new toilet cleaning brush set as per attached picture
11. Brick walls to be plastered, paintent olive green and put pes plex glass on the wall (artwork pictures will be provided)
12. Supply and install 2 Extraction fans per bathroom
13. Supply and install all bathroom doors (similar to pes plex with different colours for each door) and (doors no gaps from floor and leave a gap at the ceiling)
14. Handles etc to match natural theme
15. Hooks to be installed on the back of doors etc for bags and clothes
16. Supply and install floor tile ground pearl mat 600X1200 Floor tile 1st grade
17. Supply paint remaining walls to be painted with olive green colour
18. Toilet Main Door with Male and female signage accordingly to the toilet
19. All building rubble to remove from the site completely and dumped at a legal site, penalties will be incurred for non-compliance

**Item 2.1 (Concealed cistern for wall hung pan, 3/6litres, 135cm, light green colour as per below picture**)

.

**Item 2.2 (Abella Wall Hung Toilet pan seat) as per above picture**

**Item 2.3 (lockable toilet paper holder) Silver colour**



**Item 2.4 Toilet Brush Holder SENSEA Eden Chrome**

****

**Item 2.5 Toilet 24L SANITARY BIN – STAINLESS STEE**



**Item 2 .6 Toilet wall mosaic tile (mint green) behind the cistern**

**Item 2.7 Toilet wall sides painted Gift of Green colour (plascon) and supply and mosaic tile as per picture on the back of the flashing system.**

****

**Item 12 Doors as per picture below and with no spacing from the floor and vista double robe hook**

****

**Item 2.9 Basin Counter, basin (Benevento basin counter top 560X350X150MM White), Taps( Lusso Pescara basin mixer with its accessories) soap dispenser and mirror, wooden décor, stain steel paper towel as per picture below with 3 basins. Mosaic tiling as per picture below behind the basin sink to cover the whole wall and sides.**

****

**Ground pearl mat tile 600 x 1200**



Caffeteria

1. Supply and install onika duo pvc window blinds on the following windows

* Window 1 (4.5m x 2.0m)
* Window 2 (6.0m x 2.0m)

1. Colour of blinds: cream

NB: All dimensions to be confirmed by the bidder.

All rubble to be removed on site by bidder.

SCM Office Glass wall

1. 3m x 2.5 m glass wall Supply chain office glass wall to be frosted (design to be selected)

**Floor plan at reception**

