{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["A&B Schedules","Deviation Schedule","Test Schedule"],"not_rendered":{"defined_names":3},"read":"whole","date_system":"1900"}

{"sheet":"A&B Schedules","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"merged":[[0,0,0,6],[1,1,1,6],[2,1,2,6],[3,1,3,6],[4,1,4,6],[6,4,6,5],[7,4,7,5],[9,1,9,6],[10,1,10,6],[13,2,13,3],[14,2,14,3],[15,3,15,4],[22,3,22,4],[35,2,35,4],[36,2,36,4],[37,3,37,4],[39,3,39,4],[43,0,43,6],[44,1,45,6],[47,0,47,6],[49,0,49,1],[54,2,54,3]]}
["ESKOM TENDER E2719DXLIMOU"]
[null,"Technical Schedules A and B for"]
[null," D3073- MID-SPAN JOINT"]
[null,"NB. UNIQUE SCHEDULES ARE TO BE COMPLETED PER SAP NUMBER LISTED BELOW "]
[null,"NB. SUPPLIERS TO CONFIRM ADHERENCE TO THE LATEST PUBLISHED REVISION OF ALL APPLICABLE ESKOM DOCUMENTS AND DRAWINGS"]
[]
[{"$nulls":3},"Sap Number","Description",null,"Eskom Standard"]
[{"$nulls":3},"0165848","JOINT,M/SPAN HARE/OAK I/C D3073",null,"240-75883110"]
[]
[null,"Schedule A:  Purchasers specific requirements"]
[null,"Schedule B:  Guarantees and technical particulars of equipment offered"]
[]
[null,1,null,2,null,3,4]
[null,"Item ","Description",null,null,"Schedule A","Schedule B"]
[null,1,"Product Information"]
[null,1.1,"·","Purchasing details"]
[null,"1.1.1",null,"Eskom SAP No","0165848","xxxxxxxxxx"]
[null,"1.1.2",null,"Manufacturer","Manufacturer name","xxxxxxxxxx"]
[null,"1.1.3",null,"Manufacturer's Product Code","Specify Code","xxxxxxxxxx"]
[null,"1.1.4",null,"Manufacturer's Drawing number & Revision number","Specify No and Rev","xxxxxxxxxx"]
[null,"1.1.5",null,"Manufacturer's physical unique identifier indeliby marked on product body as per Eskom D-DT","Specify markings","xxxxxxxxxx"]
[]
[null,1.2,"·","Mechanical Properties"]
[null,"1.2.1",null,"Are the tolerances in compliance with clause 3.1.3 of 240-75883110",null,"Yes"]
[null,"1.2.2",null,"Is the product compliant with the conductor range as per section 3.1.4 of 240-75883110",null,"Yes"]
[null,"1.2.3",null,"For use with hydraulic crimping tool with a force ranging between 48 kN and 55 kN","240-75883110","Yes"]
[null,"1.2.4",null,"Can the product be applied using live line techniques","240-75883110","Yes"]
[null,"1.2.5",null,"Are plugs installed at both ends of the fitting to protect from contamination","240-75883110","Yes"]
[null,"1.2.6",null,"Are the conductive parts of the joint made up of at least 98.5% pure aluminium","240-75883110","Yes"]
[null,"1.2.7",null,"Is an electrical jointing compound compliant with section 3.2 of 240-75883110 supplied with the joint",null,"Yes"]
[null,"1.2.8",null,"Is the joint supplied in two parts (1 part for the steel core of the conductor and 1 part for the outer strands)","240-75883110","Yes"]
[null,"1.2.9",null,"All products shall be cleary and durably marked with the items stipulated in section 5.1 of 240-75883110",null,"Yes"]
[null,"1.2.10",null,"Is the packaging of the supplied joint in compliance with section 5.2 of 240-75883110",null,"Yes"]
[null,"1.2.11",null,"Is product colour code in compliance with Table 1 of 240-75883110",null,"Yes"]
[]
[null,2,"Documentation (to be submitted with tender)"]
[null,null,"Note:  All documentation to also be provided in electronic format."]
[null,2.1,"·","General"]
[null,"2.1.1",null,"Approved Manufacturer Drawings showing markings and dimensions","1 Set submitted","YES"]
[null,2.2,"·","Test Reports (where applicable)",null,"Required"]
[null,"2.2.1",null,"Has the relevant signed mandatory test schedule been submitted.","Signed Test Schedule Submitted ","Yes"]
[]
[]
["ESKOM TENDER E2719DXLIMOU"]
[null,"Deviations to any of the stated requirements are to be captured on the Deviation Schedule."]
[]
[]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[{"$nulls":3},"Name (Print)",null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Deviation Schedule","index":1,"n_rows":46,"n_cols":6,"rows_kept":46,"merged":[[0,0,0,6],[1,0,1,6],[2,0,2,6],[2,7,2,13],[2,14,2,20],[2,21,2,27],[2,28,2,34],[2,35,2,41],[2,42,2,48],[2,49,2,55],[2,56,2,62],[2,63,2,69],[2,70,2,76],[2,77,2,83],[2,84,2,90],[2,91,2,97],[2,98,2,104],[2,105,2,111],[2,112,2,118],[2,119,2,125],[2,126,2,132],[2,133,2,139],[2,140,2,146],[2,147,2,153],[2,154,2,160],[2,161,2,167],[2,168,2,174],[2,175,2,181],[2,182,2,188],[2,189,2,195],[2,196,2,202],[2,203,2,209],[2,210,2,216],[2,217,2,223],[2,224,2,230],[2,231,2,237],[2,238,2,244],[2,245,2,251],[2,252,2,255],[3,0,3,6],[3,7,3,13],[3,14,3,20],[3,21,3,27],[3,28,3,34],[3,35,3,41],[3,42,3,48],[3,49,3,55],[3,56,3,62],[3,63,3,69],[3,70,3,76],[3,77,3,83],[3,84,3,90],[3,91,3,97],[3,98,3,104],[3,105,3,111],[3,112,3,118],[3,119,3,125],[3,126,3,132],[3,133,3,139],[3,140,3,146],[3,147,3,153],[3,154,3,160],[3,161,3,167],[3,168,3,174],[3,175,3,181],[3,182,3,188],[3,189,3,195],[3,196,3,202],[3,203,3,209],[3,210,3,216],[3,217,3,223],[3,224,3,230],[3,231,3,237],[3,238,3,244],[3,245,3,251],[3,252,3,255],[4,0,4,6],[5,2,5,6],[6,2,6,6],[7,2,7,6],[8,2,8,6],[9,2,9,6],[10,2,10,6],[11,2,11,6],[12,2,12,6],[13,2,13,6],[14,2,14,6],[15,2,15,6],[16,2,16,6],[17,2,17,6],[18,2,18,6],[19,2,19,6],[20,2,20,6],[21,2,21,6],[22,2,22,6],[23,2,23,6],[24,2,24,6],[25,2,25,6],[26,2,26,6],[27,2,27,6],[28,2,28,6],[29,2,29,6],[30,2,30,6],[31,2,31,6],[32,2,32,6],[33,2,33,6],[34,2,34,6],[35,2,35,6],[37,0,37,6],[38,0,38,6],[40,0,40,1],[41,2,41,3],[45,2,45,3]]}
["ESKOM TENDER E2719DXLIMOU"]
["Deviation schedule"]
[" D3073- MID-SPAN JOINT"]
["SAP No:. 0165848 - JOINT,M/SPAN HARE/OAK I/C D3073"]
["Any deviations offered to this specification shall be listed below with reasons for deviation.  In addition, evidence shall be provided that the proposed deviation will at least be more cost-effective that that specified by Eskom."]
["Item","Clause","Description of Deviation"]
{"$rows_empty":31}
["ESKOM TENDER E2719DXLIMOU"]
["SUPPLIER SIGNATURES"]
[]
[null,null,"         "]
[null,null,"Name (Print)",null,null,"Company name"]
[]
[]
[]
[null,null,"Sign",null,null,"Date"]

{"sheet":"Test Schedule","index":2,"n_rows":23,"n_cols":6,"rows_kept":23,"merged":[[0,0,0,6],[1,0,1,7],[2,0,2,7],[3,0,3,7],[13,1,13,2],[14,0,14,6],[15,1,15,8],[18,1,18,2],[22,1,22,2]]}
["ESKOM TENDER E2719DXLIMOU"]
["Test Report Schedule"]
[" D3073- MID-SPAN JOINT"]
["SAP No:.  0165848 - JOINT,M/SPAN HARE/OAK I/C D3073"]
[]
[null,1,2,3,4,5]
[null,"Item ","Description","Standard","Clause No.","Report No."]
[null,"2.2.1","Sampling and Visual Inspection Test","240-75883110",4.3]
[null,"2.2.2","Dimension and Material Verification","240-75883110",4.4]
[null,"2.2.3","Mechanical Tension Test","240-75883110",4.5]
[null,"2.2.4","Heat Cycle Test","240-75883110",4.6]
[null,"2.2.5","Corrosion Test","240-75883110",4.7]
[null,"2.2.6","Drift Test","240-75883110",4.8]
[]
["ESKOM TENDER E2719DXLIMOU"]
[null,"SUPPLIER SIGNATURES"]
[]
[]
[null,"Name (Print)",{"$nulls":3},"Company name"]
[]
[]
[]
[null,"Sign",{"$nulls":3},"Date"]