{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["GCINISIZWE-SICGAWU"],"read":"whole","date_system":"1900"}

{"sheet":"GCINISIZWE-SICGAWU","index":0,"n_rows":183,"n_cols":8,"rows_kept":183}
["Client ",null,"Winnie Madikizela Mandela Local Municipality"]
[]
["Contract No",null,"WMM-LM 05/02/26/02 MWC"]
[]
["Contract Name",null," MAINTENANCE OF WARD 9 COMMUNITY HALL "]
[]
["ITEM NO ","PAYMENT",null,"DESCRIPTION","Unit","Quantity","Rate","Amount"]
[null,"SANS 1200 A",null,"SECTION 1:PRELIMINARY AND GENERAL"]
[1,8.3,null,"FIXED-CHANGE ITEMS"]
[1.1,"8.3.1",null,"Contractual Requirements","Sum",1]
[1.2,"8.3.2",null,"Establish Facilities on site :"]
[{"$nulls":3},"b)Facilities for Contractor","Sum ",1]
[1.3]
[1.8,8.4,null,"TIME RELATED ITEMS "]
["1.8.1","8.4.1",null,"Contractual Requirements","Sum",1]
[1.9,"8.2.1",null,"CONTRACTUAL REQUIREMENTS including the provision,maintenance and removal of facilities for the client as"]
[{"$nulls":3},"specified.and for the Contractor "]
["1.9.1","8.2.2",null,"a)Fixed Charges","Sum",1]
[{"$nulls":3},"b)Time-Related Charges","Month/s",1]
[]
["Total Carried Forward to Summary"]
[]
[]
["ITEM NO","PAYMENT",null,"DESCRIPTION ","Unit","Quantity","Rate","Amount"]
[{"$nulls":3},"RENOVATION TO EXISTING BUILDING "]
[2,null,null,"SECTION2:REMOVAL OF EXISTING WORK"]
[]
[{"$nulls":3},"Allow for protecting all existing work liable to suffer damage(I,e.walls ,finishes,floors,windows,etc)from damage during the building "]
[{"$nulls":3},"operations,alterations,etc,and make good all work damaged with new material to match existing to the approval of the director."]
[]
[2.1,null,null,"Carefully taking out and remove all existing roof sheets,windows,wall finishes including skirting."]
[{"$nulls":3},"cornice and timber doors,frames and ceiling boards from hall and ablution facilities"]
["2.1.4",null,null,"Prepair toilet steel windows for painting","No",7]
["2.1.5",null,null,"Taking out and remove single door with frame","No",2]
["2.1.6",null,null,"Taking out and remove double door with frame","No",3]
[]
[2.2,null,null,"Carefully taking out,remove painting and clear surface"]
[]
["2.2.1",null,null,"Remove all painting from the walls","m²",286]
["Total Carried Forward to Summary"]
[]
[]
["ITEM NO","PAYMENT",null,"DESCRIPTION","Unit","Quantity","Rate","Amount"]
[{"$nulls":3},"RENOVATIONS TO EXISTING BUILDING"]
[3,"SABS1200C",null,"SECTION3:EXCAVATION AND CONCRETE"]
[3.1,null,null,"EXCAVATION.ETC"]
[{"$nulls":3},"Excavation in earth and leveling soil to receive  concrete aprons,concrete v-drain and concrete pavers"]
["3.1.1",null,null,"Concrete aprons","m³",2]
[3.2,null,null,"FILLING,ETC"]
[{"$nulls":3},"Earth filling obtained from the excavations and or prescribed stock piles on site compacted to 90%mod AASHTO density"]
["3.2.1",null,null,"Backfilling to sides of aprons","m³",2]
[]
["Total Carried Forward to summary"]
[]
[null,"ITEM","PAYMENT","DESCRIPTION","UNIT","QUALITY","RATE","AMOUNT"]
[null,4,null,"SECTION4:CRACKS AND LINKS"]
[]
[null,4.1,null,"Inspect and fix all cracks in toilet and community hall","Sum",1,5000]
[null,4.2,null,"Inspect and fix all Links on Roof sheeting","Sum",1,10000]
[]
[null,"Total Carried Forward to Summary"]
[]
[]
["ITEM NO ","PAYMENT",null,"DESCRIPTION","Unit","Quantity","Rate","Amount"]
[{"$nulls":3},"RENOVATION TO EXISTING BUILDING"]
[{"$nulls":3},"CARPENTRY AND JOINERY"]
[5,"PS15",null,"SECTION5:WINDOWS,DOORS AND CEILING"]
[]
[5.1,null,null,"STEEL WINDOWS"]
["5.1.1",null,null,"W1-Window type Steel Windows","No",7]
[]
[5.2,null,null,"DOORS(Supply and Install)"]
[{"$nulls":3},"all doors including ,rubber stops, water bar, door cover, door frames"]
[{"$nulls":3},"finishings and locks"]
[]
["5.2.1",null,null,"Standard 2032x813x44mm framed battern meranti door","no",7]
[{"$nulls":3},"including pressed metal frame to still230 wall,including applicable"]
[{"$nulls":3},"pictograms (D1 AND D2)Rate to include 2coats of varnish,"]
[]
[{"$nulls":3},"Check and inspect, to fix the  existing double door ","no",3]
[]
[{"$nulls":3},"Supply and install water bars and door covers in side double doors","no",2]
[]
[]
[5.3,null,null,"Ceiling"]
[]
["5.3.1",null,null,"Supply and install 6.4mm GYPSUM CEILING BOARD to halls","m²",50]
[{"$nulls":3},"including 38x38 brandering and painting"]
[]
["5.3.2",null,null,"trap door size 533x533mm","No",1]
[]
["5.3.3",null,null,"Supply and install 19x50mm PLANED S.A PINE CORNICE:","m",45]
[{"$nulls":3},"Paint as for Ceiling "]
[]
["Total Carried Forward to summary"]
[]
[null,"ITEM NO","PAYMENT ","DESCRIPTION","UNIT","QUANTITY","Rate","Amount"]
[]
[null,6,null,"RENOVATIONS TO EXISTING BUILDING"]
[{"$nulls":3},"SECTION 6: IRONMONONGERY"]
[{"$nulls":3},"PREAMBLE"]
[{"$nulls":3},"For Trade Preamble refer to \"Department of public works : Specification of materials and methods to be used -PW371\""]
[]
[{"$nulls":3},"SUPPLEMENTARY PREAMBLE"]
[{"$nulls":3},"Items material or methods to be specified by trade names or caralogue number only an indication  of the quality"]
[{"$nulls":3},",  item material or methods of similar quality may be used with prio approval from the project leader"]
[null,6.1,null,"HINGES,BOLTS CATCHE, CABIN HOOK ECT"]
[{"$nulls":3},"LOCKS"]
[null,"6.1.1",null,"Three lever mortice locksel(SABS Approved) Single Door","No",6]
[{"$nulls":3},"Three lever mortice locksel(SABS Approved) Double Door","No",3]
[{"$nulls":3},"Door latches for toilet doors in & out","no",14]
[null,6.2,null,"HINGES "]
[null,"6.2.1",null,"100X 75 mm two  bolt bearings bruss butt hinges or similer","No",14]
[]
[null,"Total Carried Forward to summary"]
[]
[null,"ITEM","PAYMENT","DESCRIPTION","UNIT","QUALITY","RATE","AMOUNT"]
[null,7,null,"SECTION7:SECURITY FENCING"]
[]
[null,"7.1.1",null,"Pepair and Fix one panel of fencing","No",1]
[null,"7.1.2",null,"Weatherproof Padlock and chain( to be approved by client)","No",1]
[null,"Total Carried Forward"]
[]
[]
[null,"ITEM NO","PAYMENT","DESCRIPTION","UNIT","QUANTITY","RATE","AMOUNT"]
[{"$nulls":3},"RENOVATION TO EXISTING BUILDING"]
[null,8,"PS10","SECTION8:PAINTWORK"]
[null,null,"PB1"]
[{"$nulls":3},"PREVIOUSLY PAINTED WALLS are to be throughly"]
[{"$nulls":3},"prepared,seal cracks,etc prior to moving new paint."]
[{"$nulls":3},"Colour to be agreed upon on site"]
[null,8.1,null,"High qualityPure Acrylic emusion with a fully Washable"]
[{"$nulls":3},"Medium Sheen Finish with anti-microhial additive"]
[null,"8.1.1",null,"On internal and External walls (Toilets and Internal walls only for Hall)","m²",485]
[]
[null,8.2,null,"ON PREVIUOSLY PAINTED CEILINGS"]
[{"$nulls":3},"Clean and fix Existing Ceiling and prepare for skimming,"]
[{"$nulls":3},"apply 3-6mm coat of Rhinolite as per Manufactures"]
[{"$nulls":3},"instruction Two coats \"plascom Super Acrylic PVA"]
[{"$nulls":3},"(EPL)paint"]
[null,"8.2.1",null,"On Ceilings","m²",160]
[]
[null,8.3,null,"PAINTWORK ON WOOD"]
[]
[{"$nulls":3},"One coat base primer  and two coats internal quality"]
[null,"8.3.1",null,"paint Prepare and apply paint on doors internally","m²",6]
[]
[null,8.4,null,"Scrap down Varnish Repair and make good door and "]
[{"$nulls":3},"frame and prepair to Re-Varnish."]
[null,"8.4.1",null,"Prepair and apply paint on doors externally","m²",2]
[null,"Total Carried Forward"]
[]
[null,"ITEM","PAYMENT","DESCRIPTION","UNIT","QUALITY","RATE","AMOUNT"]
[null,9,null,"SECTION9:BATHROOM FITTINGS"]
[]
[null,"9.1.1",null,"Stainless steel toilet roll holder plugged to wall","No",7]
[null,"9.1.2",null,"Hand Rail for paraplegic","No",1]
[]
[null,"Total Carried Forward to Summary"]
[]
[]
[{"$nulls":3},"GCINILIZWE-SIGCAWU COMMUNITY HALL-RENOVATION",{"$nulls":3},"WARD 9"]
[]
[{"$nulls":3},"SUMMARY PAGE"]
[]
[null,null,1,"SECTON1:PRELIMINARY AND GENERAI"]
[null,null,2,"SECTION2:REMOVAL OF EXISTING WORK"]
[null,null,3,"SECTION3:EXCAVATIONS AND CONCRETE"]
[null,null,4,"SECTION3:CRACKS AND LINKS( Provisional Sums)"]
[null,null,5,"SECTION4:WINDOWS, DOORS AND CEILING"]
[null,null,6,"SECTION5:IRONMONGERY"]
[null,null,7,"SECTION6:SECURITY FENCE"]
[null,null,8,"SECTION7:PAINTWORK"]
[null,null,9,"SECTION11:BATHROOM FITTINGS"]
[]
[{"$nulls":3},"Sub-Total  "]
[{"$nulls":3},"Add Contingencies"]
[{"$nulls":3},"Sub - Total A"]
[]
[{"$nulls":3},"Sub-Total  B"]
[{"$nulls":3},"Vat 15%"]
[]
[{"$nulls":3},"GRAND TOTAL"]