{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"images":3,"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":62,"n_cols":5,"rows_kept":62,"flags":["formulas_cached_only"]}
{"$rows_empty":7}
["Item","Description","Qty","Unit Price","TOTAL"]
[]
[null,"Potchefstroom (80 Walter Sisulu Street) "]
[null,"REFURBISHMENT PROJECT"]
[1,"Paint ceiling on the ground floor with white Dulux ceiling paint","533m²"]
[]
[2,"Prepare the ground floor, supply and install porcelain tiles 600 x 600mm","272m²"]
[3,"Prepare the floor, supply and Install carpet tiles 500 x 500mm  - ( Supplier is Nouwens - Exact Ranger Colour: Green Line) (Similar to Van Dyck's Neon with green stripe.","180m² "]
[4,"Pepare and paint kitchen walls","21.109m²"]
[5,"To build 10 seater dry wall(sound proof) meeting room = 5m x 4.5m and H=3.80m","85,5m²"]
[6,"Prepare the dry walls and paint with first quote and apply two quotes Dulux white interior paint.","85,5m²"]
[7,"Supply and install 4 x LED 4ft light fittings and switch (new boardroom lights)",5]
[8,"Supply and Install 4 x view panels H= 3m x W1200m",4]
[9,"Supply and install 1 x double aluminium door, frame and lock set",3]
[10,"Suppy and install 6 x plug points 3 double and 3 single",6]
[11,"Break the cement stage and remove rubble offsite = 3.5m x 2.6m","9.1m²"]
[12,"Remove wooden and aluminium shopfront  W =10m + 5m x H2.6m, prepare the walls and paint with white interior Dulux paint 2 quotes","78LM"]
[13,"Deep cleaning the ground floor walls","533m²"]
[14,"Washing all the building windows both inside and outside on the  Ground and 1st floors.",30]
[15,"Deep cleaning of the floor on the 1st floor","425m²"]
[16,"Deep cleaning all the toilets on the Ground and 1st floor (basins, toilet bowls and wiping the walls and surfaces)",12]
[17,"Varnish main wooden double doors and repair 1 x damage double wooden door - main entrance.",6]
[18,"Varnish front entrance wooden panel",1]
[19,"Varnish 2 x office walls and match existing wooden varnish paint  ","62m²"]
[20,"Replace 7 x toilet mechenisim",7]
[21,"Supply and install heavy duty door closures - Dorma",4]
[22,"Supply and install 10m copper pipe for 1st floor water supply in the bathrooms.","10m"]
[23,"Replace 7 x toilet seats",7]
[24,"Replace  all PVC waste pipes in the bathrooms and kitchen 110mm"]
[25,"Supply and install 50L geyser for bathrooms on the ground floor only ",1]
[26,"Supply and install non slip floor tiles on the staircase - 13m x 10m","130m²"]
[27,"Supply and install new gate motor Centurion D5, 2 x rail wheels and sensor",2]
[28,"Supply and install 7 'x A/C units, 4 x 36000 btu, 1 x 2400btu and 2 x 12000 btu split units invertor and 7 x Crabtree isolators, Regas and test - Issue COC",7]
[29,"Supply and replace 7 x standard locks set ",7]
[30,"Replace pedestrain gate lock set",1]
[31,"Supply and install plug points 2 x double and 2 x single in the kitchen",4]
[32,"Install 3 x LED spotlights and day night switch",4]
[33,"Supply and install new kitchen cupboards, double kitchen sink unit with  laminated counter tops, tapmixer and  PG bison black slate on the ground floor, (W 4.5m x H = 1m for wall tiles)",1]
[34,"Cleaning of undercover parking garages and remove tremits","186,52m²"]
[35,"Remove old indoor A/C units on the ground floor",11]
[36,"Repair cracked double wooden door ground floor main entrance",1]
[37,"Varnish staircase rails  - 13m x 1m","13m x 1m"]
[39,"Prepare and paint 14 x steal grills on the floor with black paint -1.25m x 1m",14]
[40,"Varnish wooden skirting on the ground floor and match existing paint and replace 2m missing wooden skirting (413 - 15cm - 65)","ground floor"]
[41,"Remove damaged cupboards and clean the boiler room",2]
[42,"Supply And install undercounter geyser-  Kwakot Prisma 10 litres for ground floor kitchen.",1]
[null,"Transport and Installation"]
[null,"NB: All rates must be inclusive of labour, material, transport etc."]
[{"$nulls":4},0]
[]
[null,"Subtotal",null,null,0]
[]
[null,"15% V .A .T",null,null,0]
[]
[null,"Total"]

{"sheet":"Sheet2","index":1,"n_rows":3,"n_cols":1,"rows_kept":3,"flags":["formulas_cached_only"]}
[23]
[4.5]
[103.5]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}