{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Assemblies ","Components "],"read":"whole","date_system":"1900"}

{"sheet":"Assemblies ","index":0,"n_rows":83,"n_cols":9,"rows_kept":83,"merged":[[1,3,1,4],[1,5,1,6]]}
[]
[null,"SAP","Item Description","132kV to 765kV Assemblies",null,"Please indicated with \"X\""]
[null,null,"132kV","Conductor\neg Tern, Wolf, Bear","Configuration\nTwin/Trip\nQuad/Hex","Offered (X)","Not Offered (X)","Estimated Quantities ","Unit Price"]
[null,1,"\"V\" Suspension assembly","Bear","Twin",null,null,3]
[null,2,"Strain Assembly","Bear","Twin",null,null,24]
[null,3,"Vibration damper","Bear","Twin",null,null,120]
[null,4,"Strain Assembly - Single attachment","Chicadee","Single",null,null,0]
[null,5,"\"I\" Suspension Assembly ","Tern","Trip",null,null,102]
[null,6,"\"V\" Suspension assembly","Tern","Trip",null,null,174]
[null,7,"Strain assembly-double attachment","Tern","Trip",null,null,1166]
[null,8,"\"I\" Suspension Assembly ","Zebra","Single",null,null,50]
[null,9,"Cushion Grip Suspension clamp for Suspension assemblies","Zebra","Single",null,null,222]
[null,10,"Strain Assemblies for Phase Conductor (Twr 7618)","Zebra","Single",null,null,20]
[null,11,"Strain Assembly - Single attachment","Zebra","Single",null,null,50]
[null,null,"275kV"]
[null,12,"\"V\" Suspension assembly","Tern","Quad",null,null,27]
[null,13,"Strain assembly-double attachment","Tern","Quad",null,null,120]
[null,14,"\"I\" Suspension Assembly ","Tern","Twin",null,null,96]
[null,15,"\"V\" Suspension assembly","Tern","Twin",null,null,72]
[null,16,"Strain assembly-double attachment","Tern","Twin",null,null,192]
[null,17,"\"V\" Suspension assembly","Zebra","Quad",null,null,18]
[null,18,"Strain assembly-double attachment","Zebra","Quad",null,null,60]
[null,null,"400kV"]
[null,19,"\"I\" Suspension Assembly ","Bersfort","Trip",null,null,603]
[null,20,"\"I\" Suspension Assembly ","Dinosaur","Twin",null,null,6]
[null,21,"\"I\" Suspension Assembly ","IEC315","Trip",null,null,7854]
[null,22,"\"I\" Suspension Assembly ","Tern","Quad",null,null,384]
[null,23,"\"I\" Suspension Assembly ","Tern","Trip",null,null,3678]
[null,24,"\"I\" Suspension Assembly ","Wolf","Quad",null,null,6]
[null,25,"\"V\" Suspension assembly","Bersfort","Trip",null,null,255]
[null,26,"\"V\" Suspension assembly","Dinosaur","Trip",null,null,57]
[null,27,"\"V\" Suspension assembly","Goat","Twin",null,null,84]
[null,28,"\"V\" Suspension assembly","IEC315","Trip",null,null,2814]
[null,29,"\"V\" Suspension assembly","IEC560","Quad",null,null,285]
[null,30,"\"V\" Suspension assembly","Kingbird","Trip",null,null,6]
[null,31,"\"V\" Suspension assembly","Tern","Quad",null,null,617]
[null,32,"\"V\" Suspension assembly","Tern","Trip",null,null,1683]
[null,33,"\"V\" Suspension assembly","Wolf","Quad",null,null,6]
[null,34,"\"V\" Suspension assembly","Zebra","Quad",null,null,3]
[null,35,"Strain assembly-double attachment","Bersfort","Trip",null,null,648]
[null,36,"Strain assembly-double attachment","Dinosaur","Trip",null,null,252]
[null,37,"Strain assembly-double attachment","Goat","Twin",null,null,252]
[null,38,"Strain assembly-double attachment","IEC315","Trip",null,null,4872]
[null,39,"Strain assembly-double attachment","IEC560","Quad",null,null,864]
[null,40,"Strain assembly-double attachment","Kingbird","Trip",null,null,48]
[null,41,"Strain assembly-double attachment","Tern","Quad",null,null,1878]
[null,42,"Strain assembly-double attachment","Tern","Trip",null,null,4020]
[null,43,"Strain assembly-double attachment","Wolf","Quad",null,null,24]
[]
["Apollo",null,"533kV"]
[null,44,"\"V\" Suspension assembly",{"$nulls":4},0]
[null,45,"Strain Assembly",{"$nulls":4},0]
[null,46,"Vibration damper","Oden","Twin",null,null,120]
[null,47,"Vibration damper","Zambezi","Twin",null,null,120]
[null,48,"Strain Assembly - Single attachment",{"$nulls":4},0]
[null,49,"\"I\" Suspension Assembly ",{"$nulls":4},0]
[null,50,"\"V\" Suspension assembly",{"$nulls":4},0]
[null,51,"Strain assembly-double attachment",{"$nulls":4},0]
[null,52,"\"I\" Suspension Assembly ",{"$nulls":4},0]
[null,53,"Cushion Grip Suspension clamp for Suspension assemblies",{"$nulls":4},0]
[null,54,"Strain Assemblies for Phase Conductor (Twr 7618)",{"$nulls":4},0]
[null,55,"Strain Assembly - Single attachment",{"$nulls":4},0]
[null,null,"765kV"]
[null,56,"\"V\" Suspension assembly","Tern","Hex",null,null,18015]
[null,57,"Strain assembly-double attachment","Tern","Hex",null,null,9204]
[null,58,"Bolted slack span assembly","Tern","Hex",null,null,4]
[null,null,"Earthwire"]
[null,59,"EW non-insulated suspension assembly","19/2,70","N/A",null,null,370]
[null,60,"EW insulated strain assembly","19/2,70","N/A",null,null,14]
[null,61,"EW non-insulated strain assembly","19/2,70","N/A",null,null,71]
[null,62,"EW insulated suspension assembly","19/2,70","N/A",null,null,8]
[null,63,"EW insulated suspension assembly","Panther","N/A",null,null,5]
[null,64,"EW non-insulated suspension assembly","Panther","N/A",null,null,3]
[null,65,"EW insulated strain assembly","Panther","N/A",null,null,16]
[null,66,"EW non-insulated strain assembly","Panther","N/A",null,null,5]
[null,67,"EW non-insulated strain assembly","Horse","N/A",null,null,153]
[null,68,"EW insulated suspension assembly","Horse","N/A",null,null,10]
[null,69,"EW non-insulated suspension assembly","Horse","N/A",null,null,162]
[null,70,"EW insulated strain assembly","Horse","N/A",null,null,33]
[null,71,"EW insulated cross rope assembly","Horse","N/A",null,null,15]
[null,72,"EW non-insulated cross rope assembly","Horse","N/A",null,null,249]
[]
[null,"Voltage (kV)","Additional Hardware Assemblies not included but required "]

{"sheet":"Components ","index":1,"n_rows":258,"n_cols":8,"rows_kept":258,"merged":[[0,2,0,3],[0,4,0,5]]}
["SAP","Item Description","Line Hardware Components",null,"Please indicated with \"X\""]
[null,null,"Conductor\neg Tern, Wolf, Bear","Configuration\nTwin/Trip\nQuad/Hex","Offered (X)","Not Offered (X)","Estimated Quantities ","Unit Price"]
[1,"2X 380 mm spacing Spacer Damper for Conductor","Goat","Twin",null,null,630]
[2,"2X 380 mm spacing Spacer Damper for Conductor","Tern","Twin",null,null,621]
[3,"2X 570 mm spacing Spacer Damper for Conductor","Dinosaur","Twin",null,null,70]
[4,"3X 450 mm spacing Spacer Damper for Conductor","Tern","Trip",null,null,19397]
[5,"3X 570 mm spacing Spacer Damper for Conductor","Bersfort","Trip",null,null,3214]
[6,"3X 570 mm spacing Spacer Damper for Conductor","Dinosaur","Trip",null,null,306]
[7,"3X 570 mm spacing Spacer Damper for Conductor","IEC315","Trip",null,null,35432]
[8,"3X 570 mm spacing Spacer Damper for Conductor","Kingbird","Trip",null,null,90]
[9,"4X 380 mm spacing Spacer Damper for Conductor","Tern","Quad",null,null,5136]
[10,"4X 380 mm spacing Spacer Damper for Conductor","Wolf","Quad",null,null,76]
[11,"4X 380 mm spacing Spacer Damper for Conductor","Zebra","Quad",null,null,99]
[12,"4X 570 mm spacing Spacer Damper for Conductor","IEC560","Quad",null,null,2151]
[13,"6X 320 mm spacing Spacer Damper for Conductor","Tern","Hex",null,null,55154]
[14,"Spacer Damper - twin bear","Bear","Twin",null,null,20]
[15,"Midspan Joints for Conductor","Bear","Twin",null,null,26]
[16,"Midspan Joints for Conductor","Bersfort","Trip",null,null,879]
[17,"Midspan Joints for Conductor","Dinosaur","Trip",null,null,76]
[18,"Midspan Joints for Conductor","Goat","Twin",null,null,120]
[19,"Midspan Joints for Conductor","IEC315","Trip",null,null,5770]
[20,"Midspan Joints for Conductor","IEC560","Quad",null,null,424]
[21,"Midspan Joints for Conductor","Kingbird","Trip",null,null,9]
[22,"Midspan Joints for Conductor","Tern","Hex",null,null,25185]
[23,"Midspan Joints for Conductor","Wolf","Quad",null,null,26]
[24,"Midspan Joints for Conductor","Zebra","Quad",null,null,54]
[25,"Vibration damper","Bear","Twin",null,null,120]
[26,"Strain Clamps – Straight type 10-13,5mm",{"$nulls":4},20]
[27,"Midspan Joints -Dino",{"$nulls":4},20]
[28,"Midspan Joints -Zebra",{"$nulls":4},20]
[29,"Midspan Joints - Bersfort",{"$nulls":4},0]
[30,"Midspan Joints –Tern",{"$nulls":4},20]
[31,"Midspan Joints –Goat",{"$nulls":4},0]
[32,"Midspan Joints -Bear",{"$nulls":4},20]
[33,"Midspan Joints -Wolf",{"$nulls":4},20]
[34,"Midspan Joints – Horse",{"$nulls":4},20]
[35,"Midspan Joints - Tiger",{"$nulls":4},20]
[36,"Midspan Joint Compression –Earth wire 13,48mm",{"$nulls":4},20]
[37,"Compression Repair sleeves – Dino (short)",{"$nulls":4},20]
[38,"Compression Repair sleeves- Bersfort",{"$nulls":4},0]
[39,"Compression Repair sleeves - Zebra",{"$nulls":4},20]
[40,"Compression Repair sleeves – Tern",{"$nulls":4},20]
[41,"Compression Repair sleeves – Goat",{"$nulls":4},0]
[42,"Compression Repair sleeves - Bear",{"$nulls":4},0]
[43,"Compression Repair sleeves – Wolf",{"$nulls":4},20]
[44,"Compression Repair sleeves – Horse",{"$nulls":4},20]
[45,"Compression Repair sleeves - Tiger",{"$nulls":4},20]
[46,"Armour Rods/Helical Wraps –Dino - 36mm",{"$nulls":4},20]
[47,"Armour Rods/Helical Wraps - Bersfort",{"$nulls":4},0]
[48,"Armour Rods/Helical Wraps -Zebra",{"$nulls":4},20]
[49,"Armour Rods/Helical Wraps –Tern",{"$nulls":4},20]
[50,"Armour Rods/Helical Wraps –Goat",{"$nulls":4},0]
[51,"Armour Rods/Helical Wraps -Bear",{"$nulls":4},20]
[52,"Armour Rods/Helical Wraps – Wolf",{"$nulls":4},20]
[53,"Armour Rods/Helical Wraps – Horse",{"$nulls":4},20]
[54,"Armour Rods/Helical Wraps - Tiger",{"$nulls":4},20]
[55,"Shackles-210kN",{"$nulls":4},200]
[56,"Shackles-300kN",{"$nulls":4},50]
[57,"Vibration damper - Dinosaur",{"$nulls":4},50]
[58,"Crosby clamps 19/2,70",{"$nulls":4},50]
[59,"Bird Flight Diverters - Black",{"$nulls":4},100]
[60,"Bird Flight Diverters - White",{"$nulls":4},100]
[61,"Aircraft Warning spheres - Red",{"$nulls":4},200]
[62,"Aircraft warning spheres - White",{"$nulls":4},200]
[63,{"$nulls":5},50]
[64,"Suspension Clamps –  16 – 24mm",{"$nulls":4},50]
[65,"Suspension Clamps –  25 – 40mm",{"$nulls":4},50]
[66,"Suspension Clamps – Earth wire type 11-21mm",{"$nulls":4},50]
[67,"Compression Dead-end Clamp-Dino",{"$nulls":4},50]
[68,"Compression Dead-end Clamp Bersfort",{"$nulls":4},50]
[69,"Compression Dead-end Clamp-Zebra",{"$nulls":4},50]
[70,"Compression Dead-end Clamp-Tern",{"$nulls":4},50]
[71,"Compression Dead-end Clamp-Goat",{"$nulls":4},50]
[72,"Compression Dead-end Clamp-Bear",{"$nulls":4},50]
[73,"Compression Dead-end Clamp-Wolf",{"$nulls":4},50]
[74,"Compression Dead-end Clamp - Horse",{"$nulls":4},50]
[75,"Compression Dead-end Clamp - Tiger",{"$nulls":4},50]
[76,"Compression Dead-end Clamp - Chicadee",{"$nulls":4},50]
[77,"Compression Dead-end Clamp-IEC315",{"$nulls":4},50]
[78,"Compression Dead-end Clamp-IEC560",{"$nulls":4},50]
[79,"Strain Clamps – Straight type 10-13,5mm",{"$nulls":4},50]
[80,"Midspan Joints -Dino",{"$nulls":4},50]
[81,"Midspan Joints -Zebra",{"$nulls":4},50]
[82,"Midspan Joints - Bersfort",{"$nulls":4},50]
[83,"Midspan Joints –Tern",{"$nulls":4},50]
[84,"Midspan Joints –Goat",{"$nulls":4},50]
[85,"Midspan Joints -Bear",{"$nulls":4},50]
[86,"Midspan Joints -Wolf",{"$nulls":4},50]
[87,"Midspan Joints – Horse",{"$nulls":4},50]
[88,"Midspan Joints - Tiger",{"$nulls":4},50]
[89,"Midspan Joints - Chicadee",{"$nulls":4},50]
[90,"Midspan Joints –IEC315",{"$nulls":4},50]
[91,"Midspan Joints –IEC560",{"$nulls":4},50]
[92,"Midspan Joint Compression – Earth wire 10.53mm",{"$nulls":4},50]
[93,"Midspan Joint Compression –Earth wire 13,48mm",{"$nulls":4},50]
[94,"Compression Repair sleeves – Dino (short)",{"$nulls":4},50]
[95,"Compression Repair sleeves- Bersfort",{"$nulls":4},75]
[96,"Compression Repair sleeves - Zebra",{"$nulls":4},75]
[97,"Compression Repair sleeves – Tern",{"$nulls":4},75]
[98,"Compression Repair sleeves – Goat",{"$nulls":4},75]
[99,"Compression Repair sleeves - Bear",{"$nulls":4},25]
[100,"Compression Repair sleeves – Wolf",{"$nulls":4},25]
[101,"Compression Repair sleeves – Horse",{"$nulls":4},25]
[102,"Compression Repair sleeves - Tiger",{"$nulls":4},50]
[103,"Compression Repair sleeves – IEC315",{"$nulls":4},50]
[104,"Compression Repair sleeves - IEC560",{"$nulls":4},50]
[105,"Pistol Grip/Cricket Bat Strain Clamps – 7.95 – 10.50mm",{"$nulls":4},50]
[106,"Pistol Grip Strain/Cricket Bat Clamps – 11.50- 13.50mm",{"$nulls":4},50]
[107,"Yoke Plates- triangle, trapezoidal, service, Y and Vee types",{"$nulls":4},45]
[108,"Triangular yoke for I assembly-210kN-with 450mm spacing",{"$nulls":4},25]
[109,"Trapezoidal yoke for V assembly-210kN-450mm spacing",{"$nulls":4},25]
[110,"Rectangular yoke- 450kN with 450mm spacing",{"$nulls":4},25]
[111,"765kv- suspension yoke",{"$nulls":4},25]
[112,"765kv strain yoke-live end",{"$nulls":4},25]
[113,"765kV strain yoke dead end",{"$nulls":4},25]
[114,"I assembly triple yoke -450mm spacing-210kN",{"$nulls":4},25]
[115,"V assembly triple yoke-450mm spacing-210kN",{"$nulls":4},25]
[116,"Strain triple yoke- 600kN- 450mm spacing for 2x 300kN insulators",{"$nulls":4},25]
[117,"Strain V yoke- 600kN- 450mm spacing for 2x 300kN insulators for dead end to connect to tower-single attachment.",{"$nulls":4},25]
[118,"Strain rectangular yoke- 600kN- 450mm spacing for 2x 300kN insulators for dead end to connect to tower-double attachment.",{"$nulls":4},50]
[119,"Armour Rods/Helical Wraps –Dino - 36mm",{"$nulls":4},50]
[120,"Armour Rods/Helical Wraps - Bersfort",{"$nulls":4},100]
[121,"Armour Rods/Helical Wraps -Zebra",{"$nulls":4},100]
[122,"Armour Rods/Helical Wraps –Tern",{"$nulls":4},100]
[123,"Armour Rods/Helical Wraps –Goat",{"$nulls":4},100]
[124,"Armour Rods/Helical Wraps -Bear",{"$nulls":4},0]
[125,"Armour Rods/Helical Wraps – Wolf",{"$nulls":4},50]
[126,"Armour Rods/Helical Wraps – Horse",{"$nulls":4},50]
[127,"Armour Rods/Helical Wraps - Tiger",{"$nulls":4},50]
[128,"Armour Rods/Helical Wraps –IEC315",{"$nulls":4},50]
[129,"Armour Rods/Helical Wraps -IEC560",{"$nulls":4},50]
[130,"Socket Tongues –16mm, 120kN",{"$nulls":4},50]
[131,"Socket Tongues – 20mm, 210kN",{"$nulls":4},50]
[132,"Socket Tongues – 24mm, 300kN",{"$nulls":4},50]
[133,"Socket Tongues – 28mm, 450kN",{"$nulls":4},50]
[134,"Socket Clevis –16mm, 120kN",{"$nulls":4},50]
[135,"Socket Clevis – 20mm, 120kn",{"$nulls":4},50]
[136,"Socket Clevis – 24mm, 300kN",{"$nulls":4},50]
[137,"Socket Clevis – 28mm, 450kN",{"$nulls":4},50]
[138,"Ball Clevis –16mm, 120kN",{"$nulls":4},50]
[139,"Ball Clevis – 20mm, 120kn",{"$nulls":4},50]
[140,"BallClevis – 24mm, 300kN",{"$nulls":4},50]
[141,"Ball Clevis-28mm-450kN",{"$nulls":4},50]
[142,"Ball oval eyes –16mm, 120kN",{"$nulls":4},50]
[143,"Ball oval eyes – 20mm, 120kn",{"$nulls":4},50]
[144,"Balloval eyes – 24mm, 300kN",{"$nulls":4},50]
[145,"Ball oval eyes-28mm-",{"$nulls":4},410]
[146,"Junction Plates – Universal",{"$nulls":4},75]
[147,"Conductor Spacers, 380mm Spacing, Helical Wraps Twin -Dinosaur",{"$nulls":4},75]
[148,"Conductor Spacers, 380mm Spacing, Helical Wraps Twin - Bersfort",{"$nulls":4},75]
[149,"Conductor Spacers, 380mm Spacing, Helical Wraps Twin - Zebra",{"$nulls":4},75]
[150,"Conductor Spacers, 380mm Spacing, Helical Wraps Twin - Tern",{"$nulls":4},75]
[151,"Conductor Spacers, 380mm Spacing, Helical Wraps Twin - Goat",{"$nulls":4},75]
[152,"Conductor Spacers, 380mm Spacing, Helical Wraps Twin - Bear",{"$nulls":4},75]
[153,"Conductor Spacers, 570mm Spacing, Helical Wraps Trip -Dinosaur",{"$nulls":4},5]
[154,"Conductor Spacers, 570mm Spacing, Helical Wraps Trip - Bersfort",{"$nulls":4},5]
[155,"Conductor Spacers, 380mm Spacing, Helical Wraps Trip - Zebra",{"$nulls":4},5]
[156,"Conductor Spacers, 450mm Spacing, Helical Wraps Trip - Tern",{"$nulls":4},5]
[157,"Conductor Spacers, 380mm Spacing, Helical Wraps Trip - IEC315",{"$nulls":4},5]
[158,"Conductor Spacers, 380mm Spacing, Helical Wraps Quad - Bersfort",{"$nulls":4},5]
[159,"Conductor Spacers, 380mm Spacing, Helical Wraps Quad - Zebra",{"$nulls":4},5]
[160,"Conductor Spacers, 380mm Spacing, Helical Wraps Quad - Tern",{"$nulls":4},5]
[161,"Conductor Spacers, 380mm Spacing, Helical Wraps Quad - IEC560",{"$nulls":4},5]
[162,"Conductor Spacers, 320mm Spacing, Helical Wraps Hex - Tern",{"$nulls":4},50]
[163,"Conductor Spacers, Twin Bolted O Ring Type - 380mm Spacing - Dinosaur",{"$nulls":4},0]
[164,"Conductor Spacers, Twin Bolted O Ring Type - 380mm Spacing - Bersfort",{"$nulls":4},50]
[165,"Conductor Spacers, Twin Bolted O Ring Type - 380mm Spacing - Zebra",{"$nulls":4},0]
[166,"Conductor Spacers, Twin Bolted O Ring Type - 380mm Spacing - Tern",{"$nulls":4},50]
[167,"Conductor Spacers, Twin Bolted O Ring Type - 380mm Spacing - Goat",{"$nulls":4},50]
[168,"Conductor Spacers, Twin Bolted O Ring Type - 380mm Spacing - Bear",{"$nulls":4},50]
[169,"Conductor Spacers, Trip Bolted Rigid Type - 380mm Spacing - Dinosaur",{"$nulls":4},50]
[170,"Conductor Spacers, Trip Bolted Rigid Type - 380mm Spacing - Bersfort",{"$nulls":4},50]
[171,"Conductor Spacers, Trip Bolted Rigid Type - 380mm Spacing - Zebra",{"$nulls":4},50]
[172,"Conductor Spacers, Trip Bolted Rigid Type - 380mm Spacing - Tern",{"$nulls":4},50]
[173,"Conductor Spacers, Trip Bolted Rigid Type - 380mm Spacing - IEC315",{"$nulls":4},50]
[174,"Conductor Spacers, Quad Bolted Rigid Type - 380mm Spacing - Bersfort",{"$nulls":4},250]
[175,"Conductor Spacers, Quad Bolted Rigid Type - 380mm Spacing - Zebra",{"$nulls":4},100]
[176,"Conductor Spacers, Quad Bolted Rigid Type - 380mm Spacing - Tern",{"$nulls":4},50]
[177,"Conductor Spacers, Quad Bolted Rigid Type - 380mm Spacing - IEC560",{"$nulls":4},25]
[178,"Conductor Spacers, Hex Bolted Rigid Type - 380mm Spacing - Bull",{"$nulls":4},50]
[179,"Shackles-120kN",{"$nulls":4},50]
[180,"Shackles-210kN",{"$nulls":4},50]
[181,"Shackles-300kN",{"$nulls":4},50]
[182,"Shackles-450kN",{"$nulls":4},0]
[183,"Shackles-600kN",{"$nulls":4},0]
[184,"Shackles-900kN",{"$nulls":4},50]
[185,"Adjustable Extension links-min 300mm-210kN",{"$nulls":4},50]
[186,"Adjustable Extension links-min 300mm-450kN",{"$nulls":4},50]
[187,"Chain links- 120kN",{"$nulls":4},50]
[188,"Chain links- 210kN",{"$nulls":4},100]
[189,"Vibration damper - Dinosaur",{"$nulls":4},100]
[190,"Vibration damper - Bersfort",{"$nulls":4},100]
[191,"Vibration damper - Zebra",{"$nulls":4},100]
[192,"Vibration damper - Tern",{"$nulls":4},100]
[193,"Vibration damper - Goat",{"$nulls":4},100]
[194,"Vibration damper - Bear",{"$nulls":4},100]
[195,"Vibration damper - IEC315",{"$nulls":4},100]
[196,"Vibration damper - IEC560",{"$nulls":4},150]
[197,"Vibration damper - 19/2,70",{"$nulls":4},10]
[198,"Tee off Clamps (Bersfort bolted to Bersfort Compressed)",{"$nulls":4},10]
[199,"Tee off Clamps (Tern bolted to Tern Compressed)",{"$nulls":4},0]
[200,"Parallel groove clamps",{"$nulls":4},10]
[201,"Sag adjuster 210kN",{"$nulls":4},10]
[202,"Sag adjuster 120kN",{"$nulls":4},150]
[203,"Crosby clamps 19/2,70",{"$nulls":4},500]
[204,"Bird Flight Diverters - Black",{"$nulls":4},500]
[205,"Bird Flight Diverters - White",{"$nulls":4},50]
[206,"Aircraft Warning spheres - Red",{"$nulls":4},50]
[207,"Aircraft warning spheres - White",{"$nulls":4},0]
[208,"Earth wire Suspension Assembly",{"$nulls":4},500]
[209,"Earth wire Insulator (Composite types)",{"$nulls":4},100]
[210,"Earth wire Mid-span joints Compression ( Size 17.8)",{"$nulls":4},200]
[211,"Preform repair for steel earth wire",{"$nulls":4},100]
[212,"Earth wire  Full Tension joints ",{"$nulls":4},50]
[213,"Preform Repair Aluminum Zambezi Conductor ()",{"$nulls":4},300]
[214,"Repair Sleeves compression Zambezi conductor (Full Tension)",{"$nulls":4},50]
[215,"Repair Sleeves compression Zambezi conductor (Non-Tension)",{"$nulls":4},50]
[216,"Damper Spacers Quad Zambezi conductor",{"$nulls":4},200]
[217,"Crossing labels",{"$nulls":4},200]
[218,"Vibration Dampers - Shieldwire",{"$nulls":4},100]
[219,"Conductor Vibration Dampers - Zambezi",{"$nulls":4},100]
[220,"Shield Wire Dampers - 533kV  Oden",{"$nulls":4},0]
[221,"Suspension Clamps ",{"$nulls":4},0]
[222,"Compression Dead-end Clamp- Oden",{"$nulls":4},100]
[223,"Compression Dead-end Clamp- Zambezi",{"$nulls":4},0]
[224,"Strain Clamps – Straight type 10-13,5mm",{"$nulls":4},0]
[225,"Midspan Joints -Oden",{"$nulls":4},250]
[226,"Midspan Joints -Zambezi",{"$nulls":4},250]
[227,"Midspan Joint Compression – Earth wire 17.80mm",{"$nulls":4},50]
[228,"Compression Repair sleeves – Oden (short)",{"$nulls":4},50]
[229,"Compression Repair sleeves- Zambezi (Long)",{"$nulls":4},250]
[230,"Yoke Plates- triangle, trapezoidal, service, Y and Vee types",{"$nulls":4},0]
[231,"Armour Rods/Helical Wraps – Oden",{"$nulls":4},500]
[232,"Armour Rods/Helical Wraps - Zambezi",{"$nulls":4},500]
[233,"Socket Tongues –16mm, 120kN",{"$nulls":4},250]
[234,"Ball Clevis –16mm, 120kN",{"$nulls":4},0]
[235,"Junction Plates – Universal",{"$nulls":4},0]
[236,"Conductor Spacers, 380mm Spacing, Helical  Quad - Zambezi",{"$nulls":4},500]
[237,"Conductor Spacers, Twin Bolted O Ring Type - 380mm Spacing - Dinosaur",{"$nulls":4},0]
[238,"Shackles-120kN",{"$nulls":4},0]
[239,"Adjustable Extension links-min 300mm-210kN",{"$nulls":4},0]
[240,"Chain links- 120kN",{"$nulls":4},250]
[241,"Vibration damper - Oden",{"$nulls":4},250]
[242,"Vibration damper - Zambezi",{"$nulls":4},250]
[243,"Tee off Clamps (Bersfort bolted to Bersfort Compressed)",{"$nulls":4},12]
[244,"Parallel groove clamps",{"$nulls":4},20]
[245,"Crosby clamps 19/2,70",{"$nulls":4},20]
[246,"Bird Flight Diverters - Black",{"$nulls":4},100]
[247,"Bird Flight Diverters - White",{"$nulls":4},100]
[248,"Aircraft Warning spheres - Red",{"$nulls":4},20]
[249,"Aircraft warning spheres - White",{"$nulls":4},20]
[250,"4X 450 mm spacing Spacer Damper for Conductor","Zambezi","Quad",null,null,2151]
[251,"Midspan Joints for Conductor","Oden","Solid",null,null,5770]
[252,"Midspan Joints for Conductor","Zambezi","Solid",null,null,34]
[253,"Midspan Joints for Conductor","Oden","Sliding",null,null,5770]
[254,"Midspan Joints for Conductor","Zambezi","Sliding",null,null,34]
[255,"Vibration damper","Zambezi",{"$nulls":3},120]
[null,"Additional Hardware not included but required "]