{"text_format":"3","workbook":"xlsx","n_sheets":18,"sheets":["G1","G2","G3","G4","G5","G6","G7","G8","G9","G10","G11","TEST HOLE 1","TEST HOLE 3","TEST HOLE 3(2)","TEST 2","TEST HOLE 4","TEST HOLE 5","LUGEON METHOD"],"not_rendered":{"defined_names":17},"read":"whole","date_system":"1900"}

{"sheet":"G1","index":0,"n_rows":47,"n_cols":16,"rows_kept":47,"merged":[[0,1,1,12],[2,1,2,12],[2,13,6,13],[3,1,3,12],[4,0,6,0],[4,2,6,2],[4,3,4,6],[4,7,4,8],[4,10,5,10],[5,3,6,3],[5,4,6,4],[5,5,5,6],[5,7,6,7],[5,8,6,8],[5,11,5,12],[7,0,16,0],[7,1,11,1],[7,12,11,12],[7,13,11,13],[12,1,16,1],[12,12,16,12],[12,13,16,13],[17,0,26,0],[17,1,21,1],[17,12,21,12],[17,13,21,13],[22,1,26,1],[22,12,26,12],[22,13,26,13],[27,1,31,1],[27,12,31,12],[27,13,31,13],[32,1,36,1],[32,12,36,12],[32,13,36,13],[39,2,39,12],[40,2,40,12],[41,2,41,12],[42,3,42,13],[43,2,46,2],[43,3,43,13],[44,3,44,13],[45,3,45,13],[46,3,46,13]]}
[null,"G1 - GROUT HOLE "]
[]
[null,"REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
[null,"HOLE DEPTH :  24.1 m"]
["GROUT STAGE NU AND INFO","DATE","WATER TEST STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE Kpa",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
[null,"2024-10-16",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE",{"$nulls":3},300]
[{"$nulls":5},"FROM","TO",null,null,60,"LITRES","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE",null,null,60]
["Stage1 Packer plased on 15m IH Camera 20.1 meter 275 Kg dry mix, Cup Wate = 985g = 1.79q Wet.","2024-10-16","FROM",10,15,"09H00","09H15",100,0.1,650,{"$f":"SUM((J8/$J$7)*E8)","v":162.5},{"$f":"SUM(K8*(H8/I8))","v":162500},null,"A LAMINAR",null,{"$f":"P6/P7","v":5}]
[null,"2024-10-16",16,10,{"$nulls":3},250,null,null,{"$f":"SUM((J9/$J$7)*E9)","v":0},{"$f":"SUM(K9*(H9/I9))","v":{"$error":"#DIV/0!"}}]
[null,"2024-10-16","TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,"2024-10-16",24.1,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"2024-10-16",null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,{"$f":"B8","v":"2024-10-16"},"FROM",10,10,"09H25","09H35",100,1,700,{"$f":"SUM((J13/$J$7)*E13)","v":116.66666666666666},{"v":11666.666666666666,"d":"11667"},null,"B TURBULENT"]
[null,null,12,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,24.1,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[{"$nulls":3},10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null," C DILATION"]
[{"$nulls":3},10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[{"$nulls":3},10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[{"$nulls":3},10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"2024-11-05","FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"D WASH-OUT"]
[null,null,0,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,15.5,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[{"$nulls":3},10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING"]
[{"$nulls":3},10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[{"$nulls":3},10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[{"$nulls":3},10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"*"]
[{"$nulls":3},10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[{"$nulls":3},10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[{"$nulls":3},10,{"$nulls":3},100,null,null,{"$f":"SUM((J37/$J$7)*E38)","v":0},{"$error":"#DIV/0!"}]
[{"$nulls":4},{"$f":"SUM(E8:E36)","v":25}]
[{"$nulls":10},"* PARTING BEYOND PUMP CAPACITY"]
[null,null,"REMARKS :  CRACKS = 15.2m"]
[null,null,"SEVERE CAVITY AT 20.1m"]
[]
[{"$nulls":3},"REMARKS"]
[null,null,"P/B","W/S = 0.5"]
[{"$nulls":3},"GROUT MIX :  CEMENT  50kg"]
[{"$nulls":3},"UCS - 0124 = 250g"]
[{"$nulls":3},"WATER = 25l"]

{"sheet":"G2","index":1,"n_rows":48,"n_cols":13,"rows_kept":48,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[3,0,3,11],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,1,39,11],[40,1,40,11],[41,1,41,11],[42,1,42,11],[43,2,43,12],[44,1,47,1],[44,2,44,12],[45,2,45,12],[46,2,46,12],[47,2,47,12]]}
["G2 - GROUT HOLE "]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
["HOLE DEPTH :  22.7m"]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE Kpa",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-10-16",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
[null,"FROM",10,10,"12H03","12H13",100,1,800,{"$f":"SUM((I8/$I$7)*D8)","v":133.33333333333334},{"$f":"SUM(J8*(G8/H8))","v":{"v":13333.333333333334,"d":"13333"}},null,"A LAMINAR"]
[null,14,10,{"$nulls":3},250,null,null,{"$f":"SUM((I9/$I$7)*D9)","v":0},{"$f":"SUM(J9*(G9/H9))","v":{"$error":"#DIV/0!"}}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,22.7,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,10,"12H20","12H30",100,1,980,163.33333333333331,{"v":16333.333333333332,"d":"16333"},null,"B TURBULENT"]
[null,10,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,22.7,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null," C DILATION"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"D WASH-OUT"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"*"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,"REMARKS"]
[null,"CAVITY :  12.2m"]
[null,"CAVITY :  20.8m"]
[]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"G3","index":2,"n_rows":47,"n_cols":13,"rows_kept":47,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[3,0,3,11],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,1,39,11],[40,1,40,11],[41,1,41,11],[42,2,42,12],[43,1,46,1],[43,2,43,12],[44,2,44,12],[45,2,45,12],[46,2,46,12]]}
["G3 - GROUT HOLE "]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
["HOLE DEPTH :  22.8m"]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE Kpa",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-10-16",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
[null,"FROM",10,10,"13H50","14H00",100,1,650,{"$f":"SUM((I8/$I$7)*D8)","v":108.33333333333334},{"$f":"SUM(J8*(G8/H8))","v":{"v":10833.333333333334,"d":"10833"}},null,"A LAMINAR"]
[null,14,10,{"$nulls":3},250,null,null,{"$f":"SUM((I9/$I$7)*D9)","v":0},{"$f":"SUM(J9*(G9/H9))","v":{"$error":"#DIV/0!"}}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,10,"14H07","14H17",100,1,650,108.33333333333334,{"v":10833.333333333334,"d":"10833"},null,"B TURBULENT"]
[null,10,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null," C DILATION"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"D WASH-OUT"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"*"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,"REMARKS"]
[null,"CAVITY :  13.1m"]
[]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"G4","index":3,"n_rows":47,"n_cols":13,"rows_kept":47,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[3,0,3,11],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,1,39,11],[40,1,40,11],[41,1,41,11],[42,2,42,12],[43,1,46,1],[43,2,43,12],[44,2,44,12],[45,2,45,12],[46,2,46,12]]}
["G4 - GROUT HOLE "]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
["HOLE DEPTH :  23.5m"]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE BARS",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-10-16",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
[null,"FROM",10,10,"14H35","14H45",100,1,650,{"$f":"SUM((I8/$I$7)*D8)","v":108.33333333333334},{"$f":"SUM(J8*(G8/H8))","v":{"v":10833.333333333334,"d":"10833"}},null,"A LAMINAR"]
[null,14,10,{"$nulls":3},250,null,null,{"$f":"SUM((I9/$I$7)*D9)","v":0},{"$f":"SUM(J9*(G9/H9))","v":{"$error":"#DIV/0!"}}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,23.5,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,10,"14H48","14H58",100,1,650,108.33333333333334,{"v":10833.333333333334,"d":"10833"},null,"B TURBULENT"]
[null,9,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,23.5,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null," C DILATION"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"D WASH-OUT"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"*"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,"REMARKS"]
[null,"NO SEVERE CAVITIES"]
[]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"G5","index":4,"n_rows":47,"n_cols":13,"rows_kept":47,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[3,0,3,11],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,1,39,11],[40,1,40,11],[41,1,41,11],[42,2,42,12],[43,1,46,1],[43,2,43,12],[44,2,44,12],[45,2,45,12],[46,2,46,12]]}
["G5 - GROUT HOLE "]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
["HOLE DEPTH :  24m"]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE Kpa",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-10-21",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
[null,"FROM",10,10,"15H22","15H32",100,0.1,650,{"$f":"SUM((I8/$I$7)*D8)","v":108.33333333333334},{"$f":"SUM(J8*(G8/H8))","v":{"v":108333.33333333334,"d":"108333"}},null,"A LAMINAR"]
[null,13,10,{"$nulls":3},250,null,null,{"$f":"SUM((I9/$I$7)*D9)","v":0},{"$f":"SUM(J9*(G9/H9))","v":{"$error":"#DIV/0!"}}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,24,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,10,"15H40","15H55",100,0.9,650,108.33333333333334,{"v":12037.037037037038,"d":"12037"},null,"B TURBULENT"]
[null,9,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,24,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null," C DILATION"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"D WASH-OUT"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"*"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,"REMARKS"]
[null,"SMALL CAVITY :  12.1m"]
[]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"G6","index":5,"n_rows":48,"n_cols":13,"rows_kept":48,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[3,0,3,11],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,1,39,11],[40,1,40,11],[41,1,41,11],[42,1,42,11],[43,2,43,12],[44,1,47,1],[44,2,44,12],[45,2,45,12],[46,2,46,12],[47,2,47,12]]}
["G6 - GROUT HOLE "]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
["HOLE DEPTH :  21.9m"]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE Kpa",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-10-18",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
[null,"FROM",10,15,"09H20","09H35",100,0.1,650,{"$f":"SUM((I8/$I$7)*D8)","v":162.5},{"$f":"SUM(J8*(G8/H8))","v":162500},null,"A LAMINAR"]
[null,10,10,{"$nulls":3},250,null,null,{"$f":"SUM((I9/$I$7)*D9)","v":0},{"$f":"SUM(J9*(G9/H9))","v":{"$error":"#DIV/0!"}}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,21.9,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,0.1,650,{"$f":"SUM((I13/$I$7)*D13)","v":0},0,null,"B TURBULENT"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null," C DILATION"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"D WASH-OUT"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"*"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,"REMARKS"]
[null,"MINOR CAVITY :  10.9m"]
[null,"SEVERE CAVITY :  19.7m"]
[]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"G7","index":6,"n_rows":48,"n_cols":13,"rows_kept":48,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[3,0,3,11],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,1,39,11],[40,1,40,11],[41,1,41,11],[42,1,42,11],[43,2,43,12],[44,1,47,1],[44,2,44,12],[45,2,45,12],[46,2,46,12],[47,2,47,12]]}
["G7 - GROUT HOLE "]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
["HOLE DEPTH :  22.8m"]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE BARS",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-10-18",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
[null,"FROM",10,8,"09H40","09H48",100,0.1,700,{"$f":"SUM((I8/$I$7)*D8)","v":93.33333333333333},{"$f":"SUM(J8*(G8/H8))","v":{"v":93333.33333333333,"d":"93333"}},null,"A LAMINAR"]
[null,11,10,{"$nulls":3},250,null,null,{"$f":"SUM((I9/$I$7)*D9)","v":0},{"$f":"SUM(J9*(G9/H9))","v":{"$error":"#DIV/0!"}}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,22.8,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,12,"09H48","10H00",100,0.1,700,140,140000,null,"B TURBULENT"]
[null,11,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,22.8,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,10,"10H00","10H20",100,2.5,null,0,0,null," C DILATION"]
[null,11,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,22.8,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,10,"10H20","10H30",100,4.5,null,0,0,null,"D WASH-OUT"]
[null,11,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,22.8,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,10,"10H30","10H40",100,2.5,null,0,0,null,"E VOID FILLING"]
[null,11,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,22.8,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"*"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$f":"SUM(D8:D36)","v":50},null,null,100,null,null,0,{"$error":"#DIV/0!"}]
[]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,"REMARKS"]
[null,"MINOR CAVITY :  19.1m"]
[null,"ERRATIC PRESSURE.  DIFFICULT TO KEEP AT ONE PLACE"]
[]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"G8","index":7,"n_rows":47,"n_cols":13,"rows_kept":47,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[3,0,3,11],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,1,39,11],[40,1,40,11],[41,1,41,11],[42,2,42,12],[43,1,46,1],[43,2,43,12],[44,2,44,12],[45,2,45,12],[46,2,46,12]]}
["G8 - GROUT HOLE "]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
["HOLE DEPTH :  25.8m"]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE BARS",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-10-18",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
[null,"FROM",10,15,"10H45","10H50",100,0.1,650,{"$f":"SUM((I8/$I$7)*D8)","v":162.5},{"$f":"SUM(J8*(G8/H8))","v":162500},null,"A LAMINAR"]
[null,12,10,{"$nulls":3},250,null,null,{"$f":"SUM((I9/$I$7)*D9)","v":0},{"$f":"SUM(J9*(G9/H9))","v":{"$error":"#DIV/0!"}}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,25.8,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,0.1,700,0,0,null,"B TURBULENT"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null," C DILATION"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"D WASH-OUT"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"*"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,"REMARKS"]
[null,"SEVERE CAVITY :  21.4m"]
[]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"G9","index":8,"n_rows":47,"n_cols":13,"rows_kept":47,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[3,0,3,11],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,1,39,11],[40,1,40,11],[41,1,41,11],[42,2,42,12],[43,1,46,1],[43,2,43,12],[44,2,44,12],[45,2,45,12],[46,2,46,12]]}
["G9 - GROUT HOLE "]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
["HOLE DEPTH :  23.7m"]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE Kpa",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-10-18",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
[null,"FROM",10,15,"11H05","11H20",100,0.1,650,{"$f":"SUM((I8/$I$7)*D8)","v":162.5},{"$f":"SUM(J8*(G8/H8))","v":162500},null,"A LAMINAR"]
[null,10,10,{"$nulls":3},250,null,null,{"$f":"SUM((I9/$I$7)*D9)","v":0},{"$f":"SUM(J9*(G9/H9))","v":{"$error":"#DIV/0!"}}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,23.7,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,0.1,650,0,0,null,"B TURBULENT"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null," C DILATION"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"D WASH-OUT"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"*"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,"REMARKS"]
[null,"CAVITY :  21.5m"]
[]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"G10","index":9,"n_rows":50,"n_cols":13,"rows_kept":50,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[3,0,3,11],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,1,39,11],[40,1,40,11],[41,1,41,11],[42,1,42,11],[43,1,43,11],[45,2,45,12],[46,1,49,1],[46,2,46,12],[47,2,47,12],[48,2,48,12],[49,2,49,12]]}
["G10 - GROUT HOLE "]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
["HOLE DEPTH :  23.7m"]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE Kpa",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-10-18",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
[null,"FROM",10,15,"13H40","13H55",100,0.1,650,{"$f":"SUM((I8/$I$7)*D8)","v":162.5},{"$f":"SUM(J8*(G8/H8))","v":162500},null,"A LAMINAR"]
[null,11,10,{"$nulls":3},250,null,null,{"$f":"SUM((I9/$I$7)*D9)","v":0},{"$f":"SUM(J9*(G9/H9))","v":{"$error":"#DIV/0!"}}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,23.7,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,650,0,{"$error":"#DIV/0!"},null,"B TURBULENT"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null," C DILATION"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"D WASH-OUT"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"*"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,"REMARKS"]
[null,"SEVERE CAVITY :  16.5m"]
[null,"CAVITY (MINOR) :  4.8m"]
[null,"PACKER :  11.0m FOR GROUTING PRESSURE KPA 250"]
[null,"10 BAGS"]
[]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"G11","index":10,"n_rows":50,"n_cols":13,"rows_kept":50,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[3,0,3,11],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,1,39,11],[40,1,40,11],[41,1,41,11],[42,1,42,11],[43,1,43,11],[45,2,45,12],[46,1,49,1],[46,2,46,12],[47,2,47,12],[48,2,48,12],[49,2,49,12]]}
["G11 - GROUT HOLE "]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
["HOLE DEPTH :  22.7m"]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE BARS",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-10-18",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
[null,"FROM",10,17,"14H18","14H35",100,0.1,650,{"$f":"SUM((I8/$I$7)*D8)","v":184.16666666666669},{"$f":"SUM(J8*(G8/H8))","v":{"v":184166.6666666667,"d":"184167"}},null,"A LAMINAR"]
[null,11,10,{"$nulls":3},250,null,null,{"$f":"SUM((I9/$I$7)*D9)","v":0},{"$f":"SUM(J9*(G9/H9))","v":{"$error":"#DIV/0!"}}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,22.7,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,650,0,{"$error":"#DIV/0!"},null,"B TURBULENT"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null," C DILATION"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"D WASH-OUT"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"*"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,"REMARKS"]
[null,"SEVERE CAVITY :  22.2m"]
[null,"GROUT :   22/10"]
[null,"DENSITY :  960g"]
[null,"PACKER :  11.5m"]
[]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"TEST HOLE 1","index":11,"n_rows":45,"n_cols":13,"rows_kept":45,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,0,42,0],[39,1,39,11],[40,2,40,12],[41,1,44,1],[41,2,41,12],[42,2,42,12],[43,2,43,12],[44,2,44,12]]}
["TEST HOLE 1 :  HERMAN LOMBAARD"]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
[]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE BARS",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-09-13",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES    ","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
["T1","FROM",10,10,"13H00","13H10",100,100,138,{"$f":"SUM((I8/$I$7)*D8)","v":23},{"$f":"SUM(J8*(G8/H8))","v":23},null,"A LAMINAR  "]
[null,"5m",10,11,"13H15","13H26",250,200,350,{"$f":"SUM((I9/$I$7)*D9)","v":64.16666666666666},{"$f":"SUM(J9*(G9/H9))","v":{"v":80.20833333333331,"d":"80"}}]
[null,"TO",10,10,"13H30","13H40410",410,230,650,108.33333333333334,{"v":193.11594202898553,"d":"193"}]
[null,"9.3m",10,9,"13H41","13H50",250,250,355,53.25,{"v":53.25,"d":"53"}]
[null,null,10,8,"13H52","14H00",100,100,135,18,18]
["T2","FROM",10,10,"14H28","14H8",100,100,650,108.33333333333334,{"v":108.33333333333334,"d":"108"},null,"B TURBULENT "]
[null,"1m",10,10,"14H39","14H49",250,135,800,133.33333333333334,{"v":246.9135802469136,"d":"247"}]
[null,"TO",10,11,"14H50","15H01",410,135,830,152.16666666666669,{"v":462.1358024691359,"d":"462"}]
[null,"9.3m",10,10,"15H02","15H12",250,135,950,158.33333333333334,{"v":293.2098765432099,"d":"293"}]
[null,null,10,10,"15H13","15H23",100,100,750,125,125]
["T3","FROM",10,10,"09H09","09H19",100,80,800,133.33333333333334,{"v":166.66666666666669,"d":"167"},null," C DILATION "]
[null,"5.5m",10,10,"09H20","09H30",250,0.1,850,141.66666666666666,{"v":354166.6666666666,"d":"354167"}]
[null,"TO",10,10,"09H30","09H40",410,0.1,850,141.66666666666666,{"v":580833.3333333333,"d":"580833"}]
[null,"9.3m",10,8,"09H41","09H49",250,0.1,850,113.33333333333333,{"v":283333.3333333333,"d":"283333"}]
[null,53,10,6,"09H55","10H01",100,8.5,850,85,{"v":1000.0000000000001,"d":"1000"}]
["T4","FROM",10,10,"10H49","10H59",100,100,50,8.333333333333334,{"v":8.333333333333334,"d":"8"},null,"D WASH-OUT "]
[null,"7.5m",10,10,"11H00","11H10",250,250,65,10.833333333333332,{"v":10.833333333333332,"d":"11"}]
[null,"TO",10,11,"11H12","11H23",410,410,125,22.916666666666668,{"v":22.916666666666668,"d":"23"}]
[null,"9.3m",10,10,"11H25","11H34",250,250,60,10,10]
[null,54,10,10,"11H35","11H45",100,100,60,10,10]
["T5","FROM",10,10,"13H04","13H14",100,0.1,850,141.66666666666666,{"v":141666.66666666666,"d":"141667"},null,"E VOID FILLING"]
[null,"0.9m",10,10,"13H15","13H25",250,0.1,850,141.66666666666666,{"v":354166.6666666666,"d":"354167"}]
[null,"TO",10,11,"13H26","13H37",410,0.1,850,155.83333333333331,{"v":638916.6666666666,"d":"638917"}]
[null,"9.3m",10,3,"13H38","13H41",250,0.1,850,42.5,106250]
[null,null,10,4,"13H42","13H46",100,0.1,850,56.666666666666664,{"v":56666.666666666664,"d":"56667"}]
[null,"FROM",10,{"$nulls":6},0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":6},0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":6},0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":6},0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":6},{"$f":"SUM((I37/$I$7)*D38)","v":0},{"$error":"#DIV/0!"}]
[{"$nulls":3},{"$f":"SUM(D8:D36)","v":232}]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"TEST HOLE 3","index":12,"n_rows":44,"n_cols":13,"rows_kept":44,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[3,0,3,11],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,1,39,11],[40,0,43,0],[40,1,40,11],[41,1,41,11],[42,1,42,11],[43,1,43,11]]}
["TEST HOLE 3 @ 10.3m = 89 = DPT"]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
[]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE Kpa",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-10-09",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
["T HOLE 1","FROM",10,10,"13h58","14h08",100,100,150,{"$f":"SUM((I8/$I$7)*D8)","v":25},{"$f":"SUM(J8*(G8/H8))","v":25},null,"A LAMINAR  - T1"]
[null,5,10,10,"14h09","14h19",250,250,500,{"$f":"SUM((I9/$I$7)*D9)","v":83.33333333333334},{"$f":"SUM(J9*(G9/H9))","v":{"v":83.33333333333334,"d":"83"}}]
[null,"TO",10,7,"14h20","14h27",410,350,650,75.83333333333334,{"v":88.83333333333334,"d":"89"}]
[null,10.3,10,9,"14h28","14h37",250,225,550,82.5,{"v":91.66666666666667,"d":"92"}]
[null,"1st stage",10,9,"14h38","14H47",100,100,150,22.5,{"v":22.5,"d":"23"}]
["T HOLE 1","FROM",10,10,"15H02","15h12",100,100,350,58.33333333333333,{"v":58.33333333333333,"d":"58"},null,"B TURBULENT - T2"]
[null,"1m",10,null,"15H13","15H19",250,250,650,0,0]
[null,"TO",10,{"$nulls":3},410,200,650,0,0]
[null,0.3,10,6,"15H20","15H25",250,150,650,65,{"v":108.33333333333334,"d":"108"}]
[null,"2nd stage",10,7,"15H27","15H37",100,100,450,52.5,{"v":52.5,"d":"53"}]
["2024-10-11","FROM",10,10,"13H06","13H16",100,100,175,29.166666666666664,{"v":29.166666666666664,"d":"29"},null," C DILATION - T3"]
[null,null,10,10,"13H17","13H27",250,250,525,87.5,{"v":87.5,"d":"88"}]
[null,"TO",10,6,"13H28","13H33",410,375,650,65,{"v":71.06666666666666,"d":"71"}]
[null,null,10,6,"13H35","13H41",250,100,550,55,{"v":137.5,"d":"138"}]
[null,null,10,8,"13H42","13H50",100,100,175,23.333333333333332,{"v":23.333333333333332,"d":"23"}]
["2024-10-15","FROM",10,10,"07H20","07h30",100,110,250,41.66666666666667,{"v":37.87878787878788,"d":"38"},null,"D WASH-OUT - T4"]
[null,"1m",10,10,"07H33","07H43",250,250,4.3,0.7166666666666667,{"v":0.7166666666666667,"d":"1"}]
[null,"TO",10,10,"07H45","07H55",410,400,650,108.33333333333334,{"v":111.04166666666667,"d":"111"}]
[null,null,10,10,"08H00","08H10",250,250,500,83.33333333333334,{"v":83.33333333333334,"d":"83"}]
[null,null,10,10,"08H12","08H22",100,100,450,75,75]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING - T5"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"T6"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,{"$f":"SUM((I37/$I$7)*D38)","v":0},{"$error":"#DIV/0!"}]
[{"$nulls":3},{"$f":"SUM(D8:D36)","v":158}]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,"REMARKS"]
["P/B","W/S = 0.5"]
[null,"GROUT MIX :  CEMENT  50kg"]
[null,"UCS - 0124 = 250g"]
[null,"WATER = 25l"]

{"sheet":"TEST HOLE 3(2)","index":13,"n_rows":44,"n_cols":13,"rows_kept":44,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[3,0,3,11],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,0,42,0],[39,2,39,12],[40,1,43,1],[40,2,40,12],[41,2,41,12],[42,2,42,12],[43,2,43,12]]}
["TEST HOLE 3 @ 10.3 - 89 - DPT"]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
[]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE Kpa",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
[null,null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
[null,"FROM",10,10,null,null,100,100,550,{"$f":"SUM((I8/$I$7)*D8)","v":91.66666666666666},{"$f":"SUM(J8*(G8/H8))","v":{"v":91.66666666666666,"d":"92"}},null,"A LAMINAR  "]
[null,2,10,10,null,null,250,200,475,{"$f":"SUM((I9/$I$7)*D9)","v":79.16666666666667},{"$f":"SUM(J9*(G9/H9))","v":{"v":98.95833333333334,"d":"99"}}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,10.3,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,51,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,10,null,null,100,100,550,91.66666666666666,{"v":91.66666666666666,"d":"92"},null,"B TURBULENT "]
[null,"4m",10,10,null,null,250,200,400,66.66666666666667,{"v":83.33333333333334,"d":"83"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,10.3,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,52,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,10,null,null,100,100,550,91.66666666666666,{"v":91.66666666666666,"d":"92"},null," C DILATION "]
[null,6,10,10,null,null,250,200,500,83.33333333333334,{"v":104.16666666666669,"d":"104"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,10.3,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,53,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,10,null,null,100,100,10,1.6666666666666665,{"v":1.6666666666666665,"d":"2"},null,"D WASH-OUT "]
[null,8,10,10,null,null,250,200,30,{"$f":"SUM((I24/$I$7)*D24)","v":5},{"v":6.25,"d":"6"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,10.3,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,54,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,55,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"TEST 2","index":14,"n_rows":44,"n_cols":13,"rows_kept":44,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,0,42,0],[39,2,39,12],[40,1,43,1],[40,2,40,12],[41,2,41,12],[42,2,42,12],[43,2,43,12]]}
["TEST 2"]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
[{"$nulls":9},7.5]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE BARS",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-10-04",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES    ","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
[null,"FROM",10,4.5,"09H48","09H54",100,4.5,250,{"$f":"SUM((I8/$I$7)*D8)","v":18.75},{"$f":"SUM(J8*(G8/H8))","v":{"v":416.66666666666663,"d":"417"}},null,"A LAMINAR  "]
[null,"8m",10,4.5,"09H58","10H04",250,200,104,{"$f":"SUM((I9/$I$7)*D9)","v":7.800000000000001},{"$f":"SUM(J9*(G9/H9))","v":{"v":9.75,"d":"10"}}]
[null,"TO",10,{"$nulls":3},410,450,250,0,0]
[null,"5m",10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,null,"16H03","16H10",100,1.8,800,0,0,null,"B TURBULENT "]
[null,"6m",10,null,"16H15","16H20",250,2,700,0,0]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,"8m",10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,10,"09H32","09H42",100,100,425,70.83333333333333,{"v":70.83333333333333,"d":"71"},null," C DILATION "]
[null,5,10,10,"09H43","09H3",250,85,580,96.66666666666666,{"v":284.3137254901961,"d":"284"}]
[null,"TO",10,5,"09H54","09H59",410,85,650,54.16666666666667,{"v":261.2745098039216,"d":"261"}]
[null,8,10,10,"10H03","10H13",250,85,550,91.66666666666666,{"v":269.6078431372549,"d":"270"}]
[null,53,10,10,"10H14","10H24",100,100,425,70.83333333333333,{"v":70.83333333333333,"d":"71"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"D WASH-OUT "]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,54,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$f":"SUM(D8:D36)","v":54},null,null,100,null,null,0,{"$error":"#DIV/0!"}]
[]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"TEST HOLE 4","index":15,"n_rows":53,"n_cols":13,"rows_kept":53,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,0,42,0],[39,1,39,11],[40,1,40,11],[41,1,41,11],[42,1,42,11],[43,1,43,11],[44,1,44,11],[45,1,45,11],[46,1,46,11],[47,1,47,11],[48,2,48,12],[49,1,52,1],[49,2,49,12],[50,2,50,12],[51,2,51,12],[52,2,52,12]]}
["TEST HOLE 4"]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
[]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE Kpa",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-10-02",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES    ","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
["T1 HERMAN 2024/10/02","FROM",10,null,"11H45",null,100,null,250,{"$f":"SUM((I8/$I$7)*D8)","v":0},{"$f":"SUM(J8*(G8/H8))","v":{"$error":"#DIV/0!"}},null,"A LAMINAR  "]
[null,"5.5m",10,{"$nulls":3},250,null,104,{"$f":"SUM((I9/$I$7)*D9)","v":0},{"$f":"SUM(J9*(G9/H9))","v":{"$error":"#DIV/0!"}}]
[null,"TO",10,{"$nulls":3},410,null,250,0,{"$error":"#DIV/0!"}]
[null,"9.3m",10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
["T2 CPH 2024/10/03","FROM",10,{"$nulls":3},100,null,800,0,{"$error":"#DIV/0!"},null,"B TURBULENT "]
[null,null,10,{"$nulls":3},250,null,700,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
["T3 CPH 2024/10/04","FROM",10,{"$nulls":3},100,null,425,0,{"$error":"#DIV/0!"},null," C DILATION "]
[null,null,10,{"$nulls":3},250,null,580,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,650,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,550,0,{"$error":"#DIV/0!"}]
[null,53,10,{"$nulls":3},100,null,425,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"D WASH-OUT "]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,54,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,"MIX 2"]
[null,"SEMENT 50"]
[null,"UCS-012A 150g"]
[null,"WATER 20 Litres"]
[null,"GROUT MIX"]
[null,"CEMENT 50kg"]
[null,"UCS-012A 150g"]
[null,"WATER 8 Litres"]
[]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"TEST HOLE 5","index":16,"n_rows":44,"n_cols":13,"rows_kept":44,"merged":[[0,0,1,11],[2,0,2,11],[2,12,6,12],[4,1,6,1],[4,2,4,5],[4,6,4,7],[4,9,5,9],[5,2,6,2],[5,3,6,3],[5,4,5,5],[5,6,6,6],[5,7,6,7],[5,10,5,11],[7,0,11,0],[7,11,11,11],[7,12,11,12],[12,0,16,0],[12,11,16,11],[12,12,16,12],[17,0,21,0],[17,11,21,11],[17,12,21,12],[22,0,26,0],[22,11,26,11],[22,12,26,12],[27,0,31,0],[27,11,31,11],[27,12,31,12],[32,0,36,0],[32,11,36,11],[32,12,36,12],[39,2,39,12],[40,1,43,1],[40,2,40,12],[41,2,41,12],[42,2,42,12],[43,2,43,12]]}
["TEST HOLE 5"]
[]
["REPORT FORM & CALCULATIONS",{"$nulls":11},"GROUP"]
[]
["DATE","STAGE","TESTING TIMES",{"$nulls":3},"GAUGE PRESSURE BARS",null,"Liter per Hr","WATER INJECTED INTO HOLE IN TESTING PERIOD TOTAL QUANTITY READ FROM WATER METER)"]
["2024-10-02",null,"REQUIRED MINS.","ACTUAL MINS.","CLOCK TIMES",null,"REQUIRED","ACTUAL",300,null,"LUGEON VALUE"]
[{"$nulls":4},"FROM","TO",null,null,60,"LITRES    ","FOR EACH TEST","REPRESTNTA-TIVE FOR TESTED STAGE"]
["T1 HERMAN 2024/10/02","FROM",10,{"$nulls":3},100,null,250,{"$f":"SUM((I8/$I$7)*D8)","v":0},{"$f":"SUM(J8*(G8/H8))","v":{"$error":"#DIV/0!"}},null,"A LAMINAR  "]
[null,null,10,{"$nulls":3},250,null,104,{"$f":"SUM((I9/$I$7)*D9)","v":0},{"$f":"SUM(J9*(G9/H9))","v":{"$error":"#DIV/0!"}}]
[null,"TO",10,{"$nulls":3},410,null,250,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
["T2 HERMAN","FROM",10,{"$nulls":3},100,null,800,0,{"$error":"#DIV/0!"},null,"B TURBULENT "]
[null,null,10,{"$nulls":3},250,null,700,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
["T3 HERMAN 2024/10/08","FROM",10,{"$nulls":3},100,null,425,0,{"$error":"#DIV/0!"},null," C DILATION "]
[null,null,10,{"$nulls":3},250,null,580,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,650,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,550,0,{"$error":"#DIV/0!"}]
[null,53,10,{"$nulls":3},100,null,425,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"D WASH-OUT "]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,54,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"},null,"E VOID FILLING"]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,"FROM",10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,"TO",10,{"$nulls":3},410,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},250,null,null,0,{"$error":"#DIV/0!"}]
[null,null,10,{"$nulls":3},100,null,null,0,{"$error":"#DIV/0!"}]
[]
[{"$nulls":9},"* PARTING BEYOND PUMP CAPACITY"]
[null,null,"REMARKS"]
[null,"P/B","W/S = 0.5"]
[null,null,"GROUT MIX :  CEMENT  50kg"]
[null,null,"UCS - 0124 = 250g"]
[null,null,"WATER = 25l"]

{"sheet":"LUGEON METHOD","index":17,"n_rows":27,"n_cols":8,"rows_kept":27,"merged":[[0,0,0,9],[1,1,1,9],[9,7,9,8],[10,7,10,8],[12,0,12,9],[13,0,13,9],[14,0,14,9],[15,1,15,9],[16,1,16,9],[17,1,17,9],[18,1,18,9],[19,0,19,9],[20,0,20,9],[21,0,21,9],[22,0,22,9],[23,0,23,9],[24,0,24,9],[25,0,25,9],[26,0,26,9]]}
["THE LUGEON METHOD"]
[1,"Five consecutive water (pump-in) tests are done, each of ten minutes duration;  the"]
[null,"1st 10 minutes is at a low pressure - (pressure \"a\")"]
[null,"2nd 10 minutes run is at a medium pressure - (pressure \"b\")"]
[null,"3rd 10 minutes run is at a peak pressure - (pressure \"c\")"]
[null,"4th 10 minutes run is at a medium pressure - (pressure \"b\" again)"]
[null,"5th 10 minutes run is at a low pressure - (pressure \"a\" again)"]
[]
[]
[2,"Lugeon Value = Water taken in test (litres/metre/min)        X",{"$nulls":5},"10 (bars)"]
[{"$nulls":7},"test pressure (bars)"]
[]
["EXPLANATION OF THE CALCULATION"]
["Lugeon (1933) in his standard test, specified a pressure of 10 bars (150p.s.i.;  1,000kPa)."]
["The \"modified\" test usually uses lower pressure than this because:"]
["(i)","a range of pressures (rather than a single pressure) is desirable, as discussed in this paper."]
["(ii)","use of a pressure as high as 10 bars is not aways advisable, particularly at shallow depths"]
[null,"in the weaker rocks."]
["(iii)","satisfactory results can be readily obtained with lower pressures."]
["When using the \"modified\" test, it is necessary to convert the results into values which would have"]
["been (supposedly) obtained if the \"definition\" pressure (10 bars) has been used."]
["Lugeon values then result from this conversion."]
["Formula (1) carries out this conversion.  However, it presumes direct proportion when relating the"]
["pressures;  this presumption is only valid if flow through open jointing is laminar."]
["Accordingly, when significantly different Lugeon values result from the calculation carried out for five test"]
["runs, it becomes immediately apparent that the flow is not laminar, or that some other factor is exerting"]
["an influence."]