{"text_format":"3","workbook":"xlsx","n_sheets":6,"sheets":["Read Me","Tender Cover Sheet","2.1.0 Preamble","Pricing schedule Transport","Pricing schedule Product","Eskom CPA Proposal"],"not_rendered":{"images":2,"external_links":56,"defined_names":5232,"comments":1},"read":"whole","date_system":"1900"}

{"sheet":"Read Me","index":0,"n_rows":17,"n_cols":3,"rows_kept":17,"merged":[[8,1,8,2],[10,1,10,2]]}
["Enquiry No.",null,{"$f":"'Tender Cover Sheet'!C19","v":0}]
["Package Name:",null,"The “manufacture, supply, delivery, off-loading and commissioning of Liquefied Petroleum Gas (LPG), industrial, medical special gases, and provision of related maintenance refurbishment of relevant gas systems, at various Eskom Generation sites on “an as and when required basis” for a period of five (5) years."]
["Tenderer's Name:",null,{"$f":"'Tender Cover Sheet'!C23","v":0}]
[]
["READ ME"]
[]
[1,"Read these notes BEFORE you commence input or make any changes to this workbook."]
[]
[2,"The Tenderer must provide a clear indication on the Tender Cover Sheet as to whether the offer is \"main\" or \"alternative\" (and if there are several alternatives, to number them). There must be a separate Excel and PDF file for each offer, if applicable."]
[]
[3,"NOTE:  ALL CALCULATIONS ARE THE RESPONSIBILITY OF THE TENDERER, AND MUST BE CHECKED THOROUGHLY.  ANY DISCREPANCY FOUND IN THE CALCULATIONS IN THIS WORKBOOK MUST BE BROUGHT TO THE ATTENTION OF ESKOM, THROUGH THE DESIGNATED BUYER!"]
[]
[4,"This workbook contains the following sheets:"]
[null,"Read Me","This sheet provides an overview to the Tenderer of the content and role of the sheets making up the Price Schedule.  It will not form part of the tender or contract."]
[null,"Tender Cover Sheet","This is the cover sheet for Worksheets 2.1.0 to 2.1.6 and provides the total tendered price which is mandatory be completed.  It is also the source of the package name, tenderer name etc. for the other worksheets.  It will  form part of the tender or contract."]
[null,"2.1.0 Preamble","This sheet provides general guidelines for this section."]
[null,"2.1.1 Pricing","This is the main data entry sheet for the Tenderer to complete. The Tenderer takes responsibility for ensuring correct inputs."]

{"sheet":"Tender Cover Sheet","index":1,"n_rows":51,"n_cols":4,"rows_kept":51,"merged":[[1,1,1,2],[14,1,14,2],[16,1,16,2]]}
[]
[null," "]
{"$rows_empty":12}
[null,"PRICING INFORMATION"]
[]
[null,"REQUEST FOR PROPOSAL"]
[]
[null,"ENQUIRY No."]
[]
[null,"NAME OF PACKAGE:",{"$f":"'[53]Read Me'!C2","v":"The “manufacture, supply, delivery, off-loading and commissioning of Liquefied Petroleum Gas (LPG), industrial, medical special gases, and provision of related maintenance refurbishment of relevant gas systems, at various Eskom Generation sites on “an as and when required basis” for a period of five (5) years."}]
[]
[null,"TENDERER’S NAME:  "]
[]
[]
[null,"THE PRICE:  IN ZAR",{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,"(excluding VAT)"]
[]
[null,"RAND VALUE IN WORDS"]
[]
[]
[null,"VAT"]
[]
[]
[null,"THE PRICE:  IN ZAR",{"$f":"C32+C26","v":{"$error":"#REF!"}}]
[null,"(including VAT)"]
[]
[null,"DATE :"]
[]
[]
[]
[null,"FULL NAMES OF SIGNATORY:"]
[]
[]
[]
[null,"DESIGNATION OF SIGNATORY:"]
[]
[]
[]
[null,"SIGNATURE :"]
[{"$nulls":3}," "]

{"sheet":"2.1.0 Preamble","index":2,"n_rows":13,"n_cols":3,"rows_kept":13,"merged":[[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2]]}
["Enquiry No.",null,{"$f":"'[54]Read Me'!C1","v":0}]
["Package Name:",null,{"$f":"'[53]Read Me'!C2","v":"The “manufacture, supply, delivery, off-loading and commissioning of Liquefied Petroleum Gas (LPG), industrial, medical special gases, and provision of related maintenance refurbishment of relevant gas systems, at various Eskom Generation sites on “an as and when required basis” for a period of five (5) years."}]
["Tenderer's Name:",null,{"$f":"'[54]Read Me'!C3","v":0}]
[]
["2.1.0 PREAMBLE TO PRICE SCHEDULE "]
[]
[1,"The Price Schedule provides the basis of valuation, price adjustment (CPA) formulae and information for general contract progress monitoring. "]
[2,"The Prices are the amounts stated in the price column of the Price Schedule.  Where an estimated quantity is stated for an item in the Price Schedule, the Price is calculated by multiplying the estimated quantity by the rate."]
[3,"If the Supplier has decided not to identify a particular item in the price schedule at the time of tender the cost to the Supplier of doing the work is assumed to be included in, or spread across, the other Prices and rates in the price schedule in order to fulfil the obligation to Provide the Goods and Services for the tendered total of the Prices.  "]
[4,"The total of the prices must include for all direct and indirect costs, overheads, profit on costs, risks, liabilities, obligations, etc. relative to the contract."]
[5,"The Tenderer must allow for all necessary costs to complete the pricing schedule as required in terms of the specifications, technical scope and conditions of contract whether expressly stated or not in the Price Schedules. The Tenderer must provide any breakdown of prices as may be required for specific items not detailed in the Price Schedule prior to or after contract award."]
[6,"The Prices quoted by the supplier should be exclusive and inclusive of VAT."]
[7,"The items on the Pricing Schedule "]

{"sheet":"Pricing schedule Transport","index":3,"n_rows":10,"n_cols":31,"rows_kept":10,"merged":[[9,1,9,29]]}
["Item","Description","Ingula","Sere Wind Farm","Small Hydro","Arnot PS","Ankerlig PS","Gourikwa PS","Potrex ps","Drankensburg PS","Acacia PS","Gariep PS","Palmiet PS","VanderKloof PS","MAJUBA PS","KUSILE PS","KOEBERG ps","Hendrina PS","Grootvlei PS","LETHABO PS","Kriel PS","Medupi PS","Matla PS","Kendal PS","Camden PS","Tutuka PS","Duvha PS","Matimba PS","Total Quantities","Cost","Amount"]
[null,null,"Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)","Distance in km(to be indicated by Tenderer)Distance in km(to be indicated by Tenderer)"]
[40,"1 Ton Delivery Vehicle Rate R/km ",{"$nulls":26},{"$f":"SUM(Table2193[[#This Row],[Ingula]:[Matimba PS]])","v":0},0,{"$f":"AD3*AC3","v":0}]
[580,"4 Ton Delivery Vehicle Rate R/km ",{"$nulls":26},{"$f":"SUM(Table2193[[#This Row],[Ingula]:[Matimba PS]])","v":0},0,{"$f":"AD4*AC4","v":0}]
[540,"6 Ton Delivery Vehicle Rate R/km ",{"$nulls":26},{"$f":"SUM(Table2193[[#This Row],[Ingula]:[Matimba PS]])","v":0},0,0]
[70,"8 Ton Delivery Vehicle Rate R/km ",{"$nulls":26},{"$f":"SUM(Table2193[[#This Row],[Ingula]:[Matimba PS]])","v":0},0,0]
[10,"16 Ton Delivery Vehicle Rate R/km ",{"$nulls":26},{"$f":"SUM(Table2193[[#This Row],[Ingula]:[Matimba PS]])","v":0},0,0]
[310,"144 Cylinder Trailer Rate R/km ",{"$nulls":26},{"$f":"SUM(Table2193[[#This Row],[Ingula]:[Matimba PS]])","v":0},0,0]
[730,"168 Cylinder Trailer Rate R/km ",{"$nulls":26},{"$f":"SUM(Table2193[[#This Row],[Ingula]:[Matimba PS]])","v":0},0,0]
[{"$nulls":30},{"$f":"SUM(AE3:AE9)","v":0}]

{"sheet":"Pricing schedule Product","index":4,"n_rows":186,"n_cols":35,"rows_kept":186,"merged":[[49,1,49,33],[52,1,52,34],[96,1,96,33],[98,1,98,34],[119,1,119,33],[121,1,121,5],[142,1,142,33],[144,1,144,5],[150,1,150,33],[152,1,152,5],[162,1,162,33],[164,1,164,5],[173,1,173,33],[176,1,176,5],[185,1,185,33]]}
["Item","Material","Short text","Description","Cylinder Capacity / KG","Cylinder Type (Tenderer to add additional Cylinder types on Cylinder Type&Size Sheet","Quantities Ingula","Sere Wind Farm","Small Hydro","Arnot PS","Ankerlig PS","Gourikwa PS","Potrex ps","Drankensburg PS","Acacia PS","Gariep PS","Palmiet PS","VanderKloof PS","MAJUBA PS","KUSILE PS","KOEBERG ps","Hendrina PS","Grootvlei PS","LETHABO PS","Kriel PS","Medupi PS","Matla PS","Kendal PS","Camden PS","Tutuka PS","Duvha PS","Matimba PS","Total Quantities","Cost","Amount"]
[null,"MAIN GASES",{"$nulls":8},{"$f":"J2*5","v":{"v":0,"d":"0.00"}},{"$f":"K2*5","v":{"v":0,"d":"0.00"}},{"$f":"L2*5","v":{"v":0,"d":"0.00"}},{"$f":"M2*5","v":{"v":0,"d":"0.00"}},{"$f":"N2*5","v":{"v":0,"d":"0.00"}},{"$f":"O2*5","v":0},{"$f":"P2*5","v":0},{"$f":"Q2*5","v":0},{"$f":"[55]!Table2456789[[#This Row],[Yearly]]*5","v":{"$error":"#REF!"}},{"$f":"[55]!Table245678910[[#This Row],[Yearly]]*5","v":{"$error":"#REF!"}},{"$f":"T2*5","v":{"$error":"#REF!"}},null,null,{"$f":"[55]!Table245678912[[#This Row],[Yearly]]*5","v":{"$error":"#REF!"}}]
[40,"0213051","GAS:HYDROGEN:TECHNICAL GRADE;CYL 0.71 KG",null,0.62,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":1250,"d":"1250.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"v":25,"d":"R25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":100,"d":"100.00"},{"v":1250,"d":"1250.00"},{"v":25,"d":"25.00"},{"v":26550,"d":"26550.00"},{"v":750,"d":"750.00"},{"v":1250,"d":"1250.00"},{"v":1900,"d":"1900.00"},{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":1250,"d":"1250.00"},{"v":1000,"d":"1000.00"},{"v":1250,"d":"1250.00"},{"v":1250,"d":"1250.00"},{"v":1250,"d":"1250.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":39375},0,{"$f":"AH3*AG3","v":0}]
[580,213046,"GAS:HELIUM GASEOUS 5.0;99.999 PCT",null,1.5,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":75,"d":"75.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":150,"d":"150.00"},{"v":75,"d":"75.00"},{"v":50,"d":"50.00"},{"v":25,"d":"25.00"},{"v":75,"d":"75.00"},{"v":500,"d":"500.00"},{"v":75,"d":"75.00"},{"v":295,"d":"295.00"},{"v":75,"d":"75.00"},{"v":75,"d":"75.00"},{"v":150,"d":"150.00"},{"v":75,"d":"75.00"},{"v":75,"d":"75.00"},{"v":50,"d":"50.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":1845},0,{"$f":"AH4*AG4","v":0}]
[540,17693,"GAS ARGON:WELDING;3.5 KG;CYL",null,2.2,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":1935,"d":"1935.00"},{"v":35,"d":"35.00"},{"v":50,"d":"50.00"},{"v":25,"d":"25.00"},{"v":35,"d":"35.00"},{"v":35,"d":"35.00"},{"v":35,"d":"35.00"},{"v":35,"d":"35.00"},{"v":35,"d":"35.00"},{"v":1935,"d":"1,935.00"},{"v":1935,"d":"1935.00"},{"v":1750,"d":"1750.00"},{"v":155,"d":"155.00"},{"v":1935,"d":"1935.00"},{"v":1935,"d":"1935.00"},{"v":1935,"d":"1935.00"},{"v":1770,"d":"1770.00"},{"v":1935,"d":"1935.00"},{"v":1935,"d":"1935.00"},{"v":1750,"d":"1750.00"},{"v":1935,"d":"1935.00"},{"v":1935,"d":"1935.00"},{"v":1995,"d":"1995.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":27055},0,0]
[70,"0624425","GAS:053T;HYDROGEN INDUSTRIAL GRADE 10 PACK",null,6.2,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":250,"d":"250.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":500,"d":"500.00"},{"v":250,"d":"250.00"},{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":100,"d":"100.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":2675},0,0]
[10,"0213039","GAS ACETLN;DISSOLVED ACETYLENE 99 PCT HP",null,8.6,"KG",{"v":30,"d":"30.00"},{"v":10,"d":"10.00"},{"v":20,"d":"20.00"},{"v":500,"d":"500.00"},{"v":50,"d":"50.00"},{"v":100,"d":"100.00"},{"v":50,"d":"50.00"},{"v":75,"d":"75.00"},{"v":75,"d":"75.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":400,"d":"400.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":100,"d":"100.00"},{"v":435,"d":"435.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":100,"d":"100.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":6295},0,0]
[310,"0017718","GAS:NITROGEN:TECH;9.3 KG;PURITY",null,9.3,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":2000,"d":"2000.00"},{"v":25,"d":"25.00"},{"v":125,"d":"125.00"},{"v":25,"d":"25.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":2000,"d":"2,000.00"},{"v":2000,"d":"2000.00"},{"v":2000,"d":"2000.00"},{"v":0,"d":"0.00"},{"v":2000,"d":"2000.00"},{"v":2000,"d":"2000.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":2000,"d":"2000.00"},{"v":2000,"d":"2000.00"},{"v":2000,"d":"2000.00"},{"v":100,"d":"100.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":18750},0,0]
[730,"0017671","GAS MED:340011;COMPRESSED AIR DRY;8.5 KG",null,9.8,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":500,"d":"500.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},null,{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":210,"d":"210.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":6780},0,0]
[90,"0213049","GAS:NITROGEN;HIGH PURITY;11 KG;CYL;HIGH",null,11,"KG",{"v":850,"d":"850.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":660,"d":"660.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":660,"d":"660.00"},{"v":660,"d":"660.00"},{"v":650,"d":"650.00"},{"v":900,"d":"900.00"},{"v":660,"d":"660.00"},{"v":660,"d":"660.00"},{"v":100,"d":"100.00"},{"v":300,"d":"300.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":660,"d":"660.00"},{"v":660,"d":"660.00"},{"v":660,"d":"660.00"},{"v":100,"d":"100.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":8410},0,0]
[50,"0215573","GAS:HYDROGEN;TECHNICAL: 18 PACK",null,12.78,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":250,"d":"250.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":500,"d":"500.00"},{"v":250,"d":"250.00"},{"v":125,"d":"125.00"},{"v":0,"d":"0.00"},{"v":250,"d":"250.00"},{"v":500,"d":"500.00"},{"v":1500,"d":"1500.00"},{"v":1000,"d":"1000.00"},{"v":1500,"d":"1500.00"},{"v":1500,"d":"1500.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":1500,"d":"1500.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":9625},0,0]
[330,"0217601","GAS: OXYGEN:TECHNICAL;99.5;PCT; 13.6KG",null,13.6,"KG",{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":20,"d":"20.00"},{"v":5500,"d":"5500.00"},{"v":70,"d":"70.00"},{"v":70,"d":"70.00"},{"v":70,"d":"70.00"},{"v":70,"d":"70.00"},{"v":75,"d":"75.00"},{"v":70,"d":"70.00"},{"v":50,"d":"50.00"},{"v":70,"d":"70.00"},{"v":5500,"d":"5,500.00"},{"v":5500,"d":"5500.00"},{"v":5500,"d":"5500.00"},{"v":900,"d":"900.00"},{"v":5500,"d":"5500.00"},{"v":5500,"d":"5500.00"},{"v":1100,"d":"1100.00"},{"v":300,"d":"300.00"},{"v":1100,"d":"1100.00"},{"v":1100,"d":"1100.00"},{"v":5500,"d":"5500.00"},{"v":5500,"d":"5500.00"},{"v":5500,"d":"5500.00"},{"v":1100,"d":"1100.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":55690},0,0]
[460,"631500","GAS OXYGEN:MEDICAL;100 PCT;7782-44-7;O2",null,13.6,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":600,"d":"600.00"},{"v":75,"d":"75.00"},{"v":0,"d":"0.00"},{"v":75,"d":"75.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},null,{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"v":0,"d":"0.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":7960},0,0]
[480,213043,"GAS ARGON:16.9 KG;CYL;INDUSTRIAL",null,16.9,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":1100,"d":"1100.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":1100,"d":"1,100.00"},{"v":1100,"d":"1100.00"},{"v":1100,"d":"1100.00"},{"v":155,"d":"155.00"},{"v":1100,"d":"1100.00"},{"v":1100,"d":"1100.00"},{"v":1100,"d":"1100.00"},{"v":1770,"d":"1770.00"},{"v":1100,"d":"1100.00"},{"v":1100,"d":"1100.00"},{"v":1100,"d":"1100.00"},{"v":1100,"d":"1100.00"},{"v":1100,"d":"1100.00"},{"v":1100,"d":"1100.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":16260},0,0]
[590,"0213047","GAS ARGON:16.9 KG;CYL;INSTRUMENTS",null,16.9,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":1935,"d":"1935.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":1500,"d":"1,500.00"},{"v":1935,"d":"1935.00"},{"v":1500,"d":"1500.00"},{"v":155,"d":"155.00"},{"v":1935,"d":"1935.00"},{"v":1935,"d":"1935.00"},{"v":1935,"d":"1935.00"},{"v":1770,"d":"1770.00"},{"v":1500,"d":"1500.00"},{"v":1935,"d":"1935.00"},{"v":1935,"d":"1935.00"},{"v":1935,"d":"1935.00"},{"v":1935,"d":"1935.00"},{"v":1935,"d":"1935.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":25805},0,0]
[490,213044,"GAS:ARGON/CARBON;CYL 17.8 KG;MATERIAL",null,17.8,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":1935,"d":"1935.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":1500,"d":"1,500.00"},{"v":1935,"d":"1935.00"},{"v":1500,"d":"1500.00"},{"v":40,"d":"40.00"},{"v":1000,"d":"1000.00"},{"v":1935,"d":"1935.00"},{"v":1935,"d":"1935.00"},{"v":0,"d":"0.00"},{"v":1500,"d":"1500.00"},{"v":1935,"d":"1935.00"},{"v":1500,"d":"1500.00"},{"v":1935,"d":"1935.00"},{"v":1935,"d":"1935.00"},{"v":1935,"d":"1935.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":22555},0,0]
[290,"0215011","GAS:CARBON DIOXIDE;TECHNICAL GRADE;CYL",null,378,"KG",{"v":0,"d":"0.00"},{"$f":"G17*5","v":{"v":0,"d":"0.00"}},{"v":0,"d":"0.00"},{"v":250,"d":"250.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":0,"d":"0.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":50,"d":"50.00"},{"v":360,"d":"360.00"},{"v":50,"d":"50.00"},{"v":500,"d":"500.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":50,"d":"50.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":3260},0,0]
[800,215572," GAS:CARBON DIOXIDE;99.995 PCT;CYL (dip tube)",null,378,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":500,"d":"500.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},null,{"v":0,"d":"0.00"},null,{"v":500,"d":"500.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},null,{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":1800},0,0]
[410,"16187","GAS:SF6;99.9 PCT;CYL 63 KG;MATERIAL",null,63,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":250,"d":"250.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},null,{"v":100,"d":"100.00"},{"v":250,"d":"250.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":250,"d":"250.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":1750},0,0]
[230,"0636457","GAS:K 153 M;HYDROGEN;99 PCT;CONSIST144",null,102.24,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":250,"d":"250.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},null,{"v":100,"d":"100.00"},{"v":250,"d":"250.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":1600},0,0]
[220,"0636458","GAS:K 153 M;HYDROGEN;99 PCT;CONSIST168",null,119.28,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":150,"d":"150.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":250,"d":"250.00"},{"v":150,"d":"150.00"},{"v":150,"d":"150.00"},null,{"v":150,"d":"150.00"},{"v":150,"d":"150.00"},{"v":150,"d":"150.00"},{"v":0,"d":"0.00"},{"v":150,"d":"150.00"},{"v":150,"d":"150.00"},{"v":200,"d":"200.00"},{"v":150,"d":"150.00"},{"v":150,"d":"150.00"},{"v":150,"d":"150.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":2100},0,0]
[110,"0626803","GAS:OXYGEN:M091 PACK;INDUSTRIAL",null,217.6,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":115,"d":"115.00"},{"v":500,"d":"500.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},null,{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":0,"d":"0.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"v":500,"d":"500.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":6705},0,0]
[100,"0590330","GAS:NITROGEN:PURE;148.8 KG;100 PCT 176 KG M12",null,176,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":120,"d":"120.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":120,"d":"120.00"},{"v":120,"d":"120.00"},{"v":120,"d":"120.00"},{"v":0,"d":"0.00"},{"v":120,"d":"120.00"},{"v":250,"d":"250.00"},{"v":20,"d":"20.00"},{"v":1000,"d":"1000.00"},{"v":20,"d":"20.00"},{"v":20,"d":"20.00"},{"v":120,"d":"120.00"},{"v":120,"d":"120.00"},{"v":120,"d":"120.00"},{"v":20,"d":"20.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":2290},0,0]
[300,"0590329","GAS:NITROGEN;PURE;148.8 KG;100 PCT;GAS M16",null,148.8,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":120,"d":"120.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":120,"d":"120.00"},{"v":120,"d":"120.00"},{"v":120,"d":"120.00"},{"v":0,"d":"0.00"},{"v":120,"d":"120.00"},{"v":250,"d":"250.00"},{"v":20,"d":"20.00"},{"v":750,"d":"750.00"},{"v":20,"d":"20.00"},{"v":20,"d":"20.00"},{"v":120,"d":"120.00"},{"v":120,"d":"120.00"},{"v":120,"d":"120.00"},{"v":20,"d":"20.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":2040},0,0]
[250,"0626803","GAS:OXYGEN:M091:MEGA PACK; INDUSTRIAL",null,217.6,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":250,"d":"250.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":900,"d":"900.00"},{"v":250,"d":"250.00"},{"v":500,"d":"500.00"},{"v":40,"d":"40.00"},{"v":300,"d":"300.00"},{"v":40,"d":"40.00"},{"v":40,"d":"40.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":40,"d":"40.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":3860},0,0]
[30,"0215572","GAS:CARBON DIOXIDE;99.5 PCT;CYL 12 PACK",null,378,"KG (packs)",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":250,"d":"250.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":3400,"d":"3400.00"},{"v":250,"d":"250.00"},{"v":500,"d":"500.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":250,"d":"250.00"},{"v":10,"d":"10.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":5940},0,0]
[340,215008,"GAS:CARBON DIOXIDE DIP/TUBE;TECHNICAL",null,31.5,"KG",{"v":1200,"d":"1200.00"},{"v":1200,"d":"1200.00"},{"v":1200,"d":"1200.00"},{"v":1200,"d":"1200.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"v":1200,"d":"1200.00"},{"v":200,"d":"200.00"},{"v":40,"d":"40.00"},{"v":0,"d":"0.00"},{"v":40,"d":"40.00"},{"v":40,"d":"40.00"},{"v":1200,"d":"1200.00"},{"v":1200,"d":"1200.00"},{"v":1200,"d":"1200.00"},{"v":40,"d":"40.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":10260},0,0]
[350,16194,"GAS OXYGEN:3-GD;PORTAPACK;99.5 PCT;CYL",null,null,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":400,"d":"400.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":400,"d":"400.00"},{"v":400,"d":"400.00"},{"v":400,"d":"400.00"},{"v":75,"d":"75.00"},{"v":400,"d":"400.00"},{"v":400,"d":"400.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":400,"d":"400.00"},{"v":400,"d":"400.00"},{"v":400,"d":"400.00"},{"v":10,"d":"10.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":3740},0,0]
[360,16195,"GAS ACETLN:16-DA;PORTAPACK;CYL;0.94 KG",null,16,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":550,"d":"550.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":550,"d":"550.00"},{"v":550,"d":"550.00"},{"v":550,"d":"550.00"},{"v":400,"d":"400.00"},{"v":550,"d":"550.00"},{"v":550,"d":"550.00"},{"v":10,"d":"10.00"},{"v":435,"d":"435.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":550,"d":"550.00"},{"v":1000,"d":"1000.00"},{"v":550,"d":"550.00"},{"v":10,"d":"10.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":6300},0,0]
[440,"528290","GAS:F0205;TETRAFLUOROETHANE;100 PCT",null,1.84,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},null,{"v":5,"d":"5.00"},{"v":20,"d":"20.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":10,"d":"10.00"},{"v":100,"d":"100.00"},{"v":15,"d":"15.00"},{"v":5,"d":"5.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":225},0,0]
[510,17669,"GAS MED:OXYGEN;1.84 KG;CYL;MIN 99.5 PCT",null,2.75,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":600,"d":"600.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},null,{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"v":0,"d":"0.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"v":600,"d":"600.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":7800},0,0]
[520,17681,"GAS MED:OXYGEN;470 G;PI-CYL",null,0.56,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":900,"d":"900.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":900,"d":"900.00"},{"v":900,"d":"900.00"},{"v":900,"d":"900.00"},null,{"v":900,"d":"900.00"},{"v":900,"d":"900.00"},{"v":900,"d":"900.00"},{"v":0,"d":"0.00"},{"v":900,"d":"900.00"},{"v":900,"d":"900.00"},{"v":900,"d":"900.00"},{"v":900,"d":"900.00"},{"v":900,"d":"900.00"},{"v":900,"d":"900.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":11710},0,0]
[660,635042,"GAS:SULPHUR HEXAFLUORIDE SF6;99.9 PCT",null,50,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},null,{"v":5,"d":"5.00"},{"v":20,"d":"20.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":130},0,0]
[720,17654,"GAS:NITROUS OXIDE;CYL 31.3 KG;MATERIAL",null,31.3,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},null,{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":1400},0,0]
[740,17704,"GAS ARGON:515103-SH-C-P10 (L);P10",null,12.8,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":40,"d":"40.00"},{"v":50,"d":"50.00"},{"v":250,"d":"250.00"},{"v":50,"d":"50.00"},{"v":1770,"d":"1770.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"$f":"SUM(Table219[[#This Row],[Quantities Ingula]:[Matimba PS]])","v":2710},0,0]
[null,"586737","GAS:SF6;99.9 PCT;CYL 9 KG;MATERIAL",null,"9","KG","10",{"$nulls":26},0,0]
[null,"0758348 \n ","Helium Gas HELIUM 5.0; CONTAINER TYPE: GAS CYLINDER; CONTAINER CAPACITY: 130 BAR; HELIUM GAS , HELIUM 5.0 , USED ON GAS GUARD SYSTEM, 50kg bottle",null,50,"KG",5,{"$nulls":26},0,0]
[null,"TDC","GAS: Nitrogen CH 200 Bar, 70kg bottle",null,70,"KG",5,{"$nulls":26},0,0]
[null,"0213049","GAS:NITROGEN;HIGH PURITY;11 KG;CYL;HIGH",null,11,"KG",null,10]
[null,"0213041","GAS LP:CYL:19 KG ",null,19,"KG",null,10]
[null,"0217601","GAS: OXYGEN:TECHNICAL;99.5;PCT; 13.6KG ",null,13.6,"KG",null,10,{"$nulls":3},10,5,null,null,30,5]
[null,"0016195","GAS ACETLN:16-DA;PORTAPACK;CYL;0.94 KG ",null,0.94,"KG",null,10,null,null,10,null,5,null,5]
[null,"0213039","GAS ACETLN;DISSOLVED ACETYLENE 99 PCT HP",null,null,"KG",{"$nulls":4},10]
[null,"213043","GAS ARGON:16.9 KG;CYL;INDUSTRIAL ",null,16.9,"KG",{"$nulls":4},10]
[null,"586737","GAS:SF6;99.9 PCT;CYL 9 KG;MATERIAL",null,9,"KG",{"$nulls":4},10,10,null,50,15,null,30]
[null,"624806","GAS:DIOXIDE/SULPHUR;CYL 5 L",null,null,"KG",{"$nulls":5},10]
[null,"593173","GAS:SF6;146; 054 G/MOL;CYL",null,null,"KG",{"$nulls":5},10]
[null,"0157502","REFRIGERANT:R22;FREON;R22;CYL 65 KG ",null,65,"KG",{"$nulls":10},40]
[null,"213475","GAS ARGON:HIGH PRESSURE;16.9 KG;CYL",null,16.9,"KG",{"$nulls":9},20]
[null,"Sub Total ",{"$nulls":32},{"$f":"SUM(AI3:AI38)","v":0}]
[]
[]
[null,"CALIBRATION GASES"]
[null,"Material","Short text","Description","Tenderer to indicate Cylinder Capacity in Kg","Cylinder Type (Tenderer to add additional Cylinder types on Cylinder Type&Size Sheet","Quantities Ingula","Sere Wind Farm","Small Hydro","Arnot PS","Ankerlig PS","Gourikwa PS","Potrex ps","Drankensburg PS","Acacia PS","Gariep PS","Palmiet PS","VanderKloof PS","MAJUBA PS","KUSILE PS","KOEBERG ps","Hendrina PS","Grootvlei PS","LETHABO PS","Kriel PS","Medupi PS","Matla PS","Kendal PS","Camden PS","Tutuka PS","Duvha PS","Matimba PS","Total Quantities","Cost","Amount"]
[null,157508,"GAS:0XYGEN8PC02;NITROGEN/OXYGEN 10L","GAS: TYPE: NITROGEN/OXYGEN; PURITY: N 92/O2 8 PCT; CONTAINER: CYL AL 10 KG; ANALYSER TEST GAS; BALANCE NITROGEN (N2); PORTAPACK, MATER IAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"Kg",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R25.00 ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"$f":"SUM(G55:AF55)","v":150},0,{"$f":"AH55*AG55","v":0}]
[400,611429,"GAS MIXT:CALIBRATION;10 L;DISPOSABLE","GAS, MIXTURES: TYPE: CALIBRATION; CONTAINER CAPACITY: 1.55 L; CONTAINER TYPE: DISPOSABLE; CONCENTRATION: O2 20/N2 80 PCT; PHYSICAL FORM: GAS; REFERENCE NO: S-CAND 110 20% O2/N2; S-CAND 103/110 20% O2/N2; 16 POINT MATERIAL SAFETY DATA SHEET TO BE SUPPLIED WITH EVERY DELIVERY",null,"KG",{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":25,"d":"25.00"},{"v":15,"d":"15.00"},{"v":15,"d":"15.00"},{"v":25,"d":"25.00"},{"v":15,"d":"15.00"}," R25.00 ",{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"$f":"SUM(G56:AF56)","v":320},0,0]
[630,252736,"GAS,METHCAL 14 (S) 1.4% WITH 21% OXYGEN","GAS: TYPE: ACETYLENE/HYDROGEN/LPG DETECTORS; PURITY: METH CAL 14/CH4 1.4/O2 2.1 PCT; RANGE: SMALL, BALANCE AIR 519114-IH-A W019120 OR W019220",null,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":50,"d":"50.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":25,"d":"25.00"},645,0,0]
[700,683025,"GAS:CALIBRATION COCKTAIL;CYL 1.14 KG","GAS: TYPE: CALIBRATION COCKTAIL; PURITY: CH4: 58%; O2: 15%; CO: 60PPM; H2S: 20PPM; CONTAINER: CYL 1.14 KG; PORTA PAK; DIMENSIONS: DIA 90MM; HEIGHT 364MM",null,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":15,"d":"15.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},150,0,0]
[600,220157,"GAS MIXT:HYDROGEN 3PCT/NITROGEN97PCT;10 L","GAS, MIXTURES: TYPE: HYDROGEN/NITROGEN; CONTAINER CAPACITY: 10 L; CONCENTRATION: HYDROGEN 3 PCT",null,"KG",{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":15,"d":"15.00"},{"v":15,"d":"15.00"},{"v":25,"d":"25.00"},{"v":15,"d":"15.00"}," R25.00 ",{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},515,0,0]
[610,220158,"GAS MIXT:HYDROGEN10PCT/NITROGEN;10 L","GAS, MIXTURES: TYPE: HYDROGEN/NITROGEN; CONTAINER CAPACITY: 10 L; CONCENTRATION: HYDROGEN 10 PCT",null,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":15,"d":"15.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},155,0,0]
[650,634495,"GAS:MIXTURE;11 KG","GAS: TYPE: MIXTURE; PURITY: METHCAL 14-1; 4 PCT METHANE; 20 PCT OXYGEN; BALANCE NITROGEN; CONTAINER: 11 KG",null,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":15,"d":"15.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},155,0,0]
[null,157506,"GAS: Mix Nitrogen/oxygen; 10KG",null,null,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},140,0,0]
[null,157507,"NITROGEN/OXYGEN,N 94.6; O2 5.4 PCT 10L","GAS, MIXTURES: TYPE: NITROGEN/OXYGEN; CONTAINER CAPACITY: 10 KG; CONTAINER TYPE: CYLINDER AL; CONCENTRATION: N 94.6/O2 5.4 PCT; ANALYZER TEST GAS, BALANCE NITROGEN, N2, IN 1370 L CYLINDERS, SHELF LIVE OF 12 MNTHS, PORTAPACK, MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":25,"d":"25.00"},{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"v":20,"d":"20.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},335,0,0]
[930,null,"60%CO and 40%CO2 gas mixture",{"$nulls":3},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," -   ",{"v":15,"d":"15.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},25,0,0]
[null,729183,"GAS: NO & CO2 50L","GAS: TYPE: NO AND CO2; PURITY: 600 TO 1200 PPM NO AND 12% TO 13.5% CO2 PCT; CONTAINER: 50 L; GAS MIX: 600 TO 1200PPM NO AND 12 TO 13.5 % CO2 BALANCE IN N2 IN 50 LITER CYLINDER INCLUDING NMISA CERTIFICATION",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},145,0,0]
[null,729184,"GAS: O2 0.5 PCT 50L","GAS: TYPE: OXYGEN; PURITY: 0.5 PCT; CONTAINER: 50 L; ARNOT: QC TO BE DONE BY C&I BEFORE GASSES ARE BOOKED TO STORES; NMISA CERTIFICATE TO BE PROVIDED WITH EVERY DELIVERY",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":15,"d":"15.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},90,0,0]
[null,729185,"GAS: SO2& CO 50L","GAS: TYPE: SO2 AND CO; PURITY: 1200 TO 1350PPM AND 800 TO 900 PPM CO BALNCE N2 PPM; CONTAINER: 50 L; GAS MIX: 50 LITER CYLINDER INCLUDING NMISA CERTIFICATION",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},75,0,0]
[null,157420,"GAS MIXT:NITROGEN 99PCT/OXYGEN1PCT;1.37 L;CYL","GAS, MIXTURES: TYPE: NITROGEN/OXYGEN; CONTAINER CAPACITY: 1.37 L; CONTAINER TYPE: CYL; CONCENTRATION: N 99/O2 1 PCT; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT; SPECIAL TEST MIXTURE; SMALL",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},140,0,0]
[null,157507,"NITROGEN/OXYGEN,N 94.6; O2 5.4 PCT 10L","GAS, MIXTURES: TYPE: NITROGEN/OXYGEN; CONTAINER CAPACITY: 10 KG; CONTAINER TYPE: CYLINDER AL; CONCENTRATION: N 94.6/O2 5.4 PCT; ANALYZER TEST GAS, BALANCE NITROGEN, N2, IN 1370 L CYLINDERS, SHELF LIVE OF 12 MNTHS, PORTAPACK, MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":20,"d":"20.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},330,0,0]
[null,587437,"GAS,MIXTURES:CO/CO2;50 L;K CYLINDER","GAS, MIXTURES: TYPE: NITROGEN/OXYGEN; CONTAINER CAPACITY: 10 KG; CONTAINER TYPE: CYLINDER AL; CONCENTRATION: N 94.6/O2 5.4 PCT; ANALYZER TEST GAS, BALANCE NITROGEN, N2, IN 1370 L CYLINDERS, SHELF LIVE OF 12 MNTHS, PORTAPACK, MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":15,"d":"15.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":25,"d":"25.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":15,"d":"15.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},315,0,0]
[null,157507,"NITROGEN/OXYGEN,N 94.6; O2 5.4 PCT 10L","GAS, MIXTURES: TYPE: NITROGEN/OXYGEN; CONTAINER CAPACITY: 10 KG; CONTAINER TYPE: CYLINDER AL; CONCENTRATION: N 94.6/O2 5.4 PCT; ANALYZER TEST GAS, BALANCE NITROGEN, N2, IN 1370 L CYLINDERS, SHELF LIVE OF 12 MNTHS, PORTAPACK, MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},75,0,0]
[null,587437,"GAS,MIXTURES:CO/CO2;50 L;K CYLINDER","GAS, MIXTURES: TYPE: CO/CO2; CONTAINER CAPACITY: 50 L; CONTAINER TYPE: CYLINDER K; CONCENTRATION: 60% CO/40% CO2; PHYSICAL FORM: GAS",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},130,0,0]
[370,157506,"GAS MIXT:NITROGEN/OXYGEN;10 KG;CYL","GAS, MIXTURES: TYPE: NITROGEN/OXYGEN; CONTAINER CAPACITY: 10 KG; CONTAINER TYPE: CYL; CONCENTRATION: N 98/O2 2 PCT; TEST GAS, BALANCE NITROGEN, N2; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"KG",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},135,0,0]
[390,611428,"GAS MIXT:CALIBRATION;10 L;DISPOSABLE","GAS, MIXTURES: TYPE: CALIBRATION; CONTAINER CAPACITY: 1.55 L; CONTAINER TYPE: DISPOSABLE; CONCENTRATION: O2 2/N2 98 PCT; PHYSICAL FORM: GAS; REFERENCE NO: S-CAND-103/110 2% O2/N2; S-CAND-110 2% O2/N2; 16 POINT MATERIAL SAFETY DATA SHEET TO BE SUPPLIED WITH EVERY DELIVERY",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},75,0,0]
[null,157452,"GAS:NITROGEN/OXYGEN;N 79.5/O2 20.5 PCT","GAS: TYPE: NITROGEN/OXYGEN; PURITY: N 79.5/O2 20.5 PCT; CONTAINER: CYL; MIX 2 COMPONENT (S), PROOF TEST GAS, TO BE USED FOR CALIBRATION PURPOSES, 340-201, MATERIAL SAFETY DATA SHEET (MSDS) THAT COMPLIES WITH THE OCCUPATIONAL HEALTH AND SAFETY ACT'S REGULATIONS TO BE SUPPLIED, NO SUBSTANCE AND/OR INGREDIENTS THAT FALL UNDER TABLE 1 CATAGORY WILL BE USED, ANY CHEMICAL FALLING UNDER TABLE 3 OF THE SAME REGULATIONS SHALL NOT BE USED, SHALL BE BIODEGRADABLE AND OZONE FRIENDLY, COPY OF MSDS TO BE SENT TO MEDICAL, SMALL",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},60,0,0]
[null,157451,"GAS:NITROGEN/OXYGEN;N 99.5/O2 0.5 PCT","GAS: TYPE: NITROGEN/OXYGEN; PURITY: N 99.5/O2 0.5 PCT; CONTAINER: CYL; SUPPL P/N: 340-202; MIX 2 COMPONENT (S), PROOF TEST GAS, TO BE USED FOR CALIBRATION PURPOSES, MATERIAL SAFETY DATA SHEETS THAT COMPLIES WITH THE OCCUPATIONAL HEALTH AND SAFETY ACT'S REGULATIONS TO BE SUPPLIED, NO SUBSTANCES AND/OR INGREDIENTS THAT FALL UNDER TABLE 1 CATAGORY WILL BE USED, ANY CHEMICAL FALLING UNDER TABLE 3 OF THE SAME REGULATIONS SHALL NOT BE USED, SHALL BE BIODEGRADABLE AND OZONE FRIENDLY, COPY OF MSDS TO BE SENT TO MEDICAL, SMALL",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},140,0,0]
[null,157459,"GAS:OXYGEN BALANCE NITROGEN;20 PCT","GAS: TYPE: OXYGEN BALANCE NITROGEN; PURITY: 20 PCT; CONTAINER: CYL 10 KG; REFERENCE NO: 340201; APPLICATION: USED FOR CALIBRATING O2 BOILER ANALYSER; TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE IN SMALL BOTTLE; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"KG (pack)",{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":25,"d":"25.00"},{"v":15,"d":"15.00"},{"v":15,"d":"15.00"},{"v":25,"d":"25.00"},{"v":10,"d":"10.00"}," R25.00 ",{"v":0,"d":"0.00"},{"v":25,"d":"25.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},280,0,0]
[null,250338,"GAS CRBN:CALIBRATION;50 L;CYLINDER","GAS, CARBON: TYPE: CALIBRATION; CONTAINER CAPACITY: 50 L; CONTAINER TYPE: CYLINDER; CONCENTRATION: CO 850 PPM; CARBON/OXIDE GAS MIX 850PPM CO + RECERTIFICATION BALANCED IN NITROGEN X 50L CYLINDER 850PPM CO IN N2; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},75,0,0]
[null,676383,"GAS MIXT:ANALYZER CALIBRATION;CYLINDER","GAS, MIXTURE: TYPE: ANALYZER CALIBRATION; CONCENTRATION: 2.1% OXYGEN, 150PPM, CARBON MONOXIDE; BALANCE NITROGEN; CONTAINER TYPE: CYLINDER; CONTAINER CAPACITY: 10 KG; GRADE: INSTRUMENT; PHYSICAL FORM: GAS; THE LATEST 16 POINT MATERIAL SAFETY DATA SHEET TOT BE SUPPLIED WITH GAS",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},65,0,0]
[null,611428,"GAS MIXT:CALIBRATION;1.55 L;DISPOSABLE","GAS, MIXTURES: TYPE: CALIBRATION; CONTAINER CAPACITY: 1.55 L; CONTAINER TYPE: DISPOSABLE; CONCENTRATION: O2 2/N2 98 PCT; PHYSICAL FORM: GAS; REFERENCE NO: S-CAND-110 2% O2/N2; S-CAND-103/110 2% O2/N2; 16 POINT MATERIAL SAFETY DATA SHEET TO BE SUPPLIED WITH EVERY DELIVERY",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},65,0,0]
[null,611429,"GAS MIXT:CALIBRATION;1.55 L;DISPOSABLE","GAS, MIXTURES: TYPE: CALIBRATION; CONTAINER CAPACITY: 1.55 L; CONTAINER TYPE: DISPOSABLE; CONCENTRATION: O2 20/N2 80 PCT; PHYSICAL FORM: GAS; REFERENCE NO: S-CAND 103/110 20% O2/N2; S-CAND 110 20% O2/N2; 16 POINT MATERIAL SAFETY DATA SHEET TO BE SUPPLIED WITH EVERY DELIVERY",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},65,0,0]
[null,250337,"GAS OXYGEN:CALIBRATION;0.5 PCT;CYLINDER","GAS, OXYGEN: TYPE: CALIBRATION; CONCENTRATION: 0.5 PCT; CONTAINER TYPE: CYLINDER; CONTAINER CAPACITY: 50 L; GAS MIX: 0.5% OXYGEN + RECERTIFICATION BY NMISA BALANCED IN NITROGEN X 50 L CYLINDER; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT; GAS MIX MUST BE RECERTIFIED BY NMISA BEFORE DELIVERED",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," -   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},20,0,0]
[null," ","GAS:  CALIBRATIOIN; 98 H2 PCT Bal 2PCT N2","98PCT H2 BAL 2 PCT N2 ANALYSER; TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE IN SMALL BOTTLE DISPOSABLE ; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},65,0,0]
[null," ","GAS:  CALIBRATIOIN; 97 H2 PCT Bal 3PCT N2","97PCT H2 BAL 3 PCT N2 ANALYSER; TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE IN SMALL BOTTLE DISPOSABLE; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},65,0,0]
[null," ","GAS:  CALIBRATIOIN; 90 H2 PCT Bal 10PCT N2","90PCT H2 BAL 10 PCT N2 ANALYSER; TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE IN SMALL BOTTLE DISPOSABLE; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},60,0,0]
[null," ","GAS:  CALIBRATIOIN; 99,999 PCT N2 contaminants <10ppm","99,999 PCT N2 contaminants<10ppm ANALYSER; TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE IN SMALL BOTTLE DISPOSABLE; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},55,0,0]
[null," ","GAS:  CALIBRATIOIN; 99,995 PCT CO2","99.995PCT CO2 ANALYSER; TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE IN SMALL BOTTLE DISPOSABLE; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},65,0,0]
[null," ","GAS:  CALIBRATIOIN;5 or 10 ppm O2 Bal N2","5 or 10 ppm O2 Bal N2 ANALYSER; TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE IN SMALL BOTTLE DISPOSABLE; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},65,0,0]
[null," ","GAS:  CALIBRATIOIN 50PCT CO2 Bal 50 PCT N2","50PCT CO2 Bal 50 PCT N2 ANALYSER; TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE IN SMALL BOTTLE DISPOSABLE; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},65,0,0]
[null," ","GAS:  CALIBRATIOIN 99,999PCT H2 contaminants <10ppm","99,999PCT H2 contaminants <10ppm ANALYSER; TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE IN SMALL BOTTLE DISPOSABLE; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},50,0,0]
[null," ","GAS:  CALIBRATIOIN 99,5PCT N2 Bal 0,5 PCT O2","99,5PCT N2 Bal 0,5 PCT O2 ANALYSER; TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE IN SMALL BOTTLE DISPOSABLE; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":10,"d":"10.00"},60,0,0]
[null," ","GAS:  CALIBRATIOIN : Air with CO 250 ppm","Air with CO 250 ppm ANALYSER; TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE IN SMALL BOTTLE DISPOSABLE; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},75,0,0]
[null," ","GAS:  CALIBRATIOIN :99PCT H2 Bal 1PCT O2","99PCT H2 Bal 1PCT O2 ANALYSER; TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE IN SMALL BOTTLE DISPOSABLE; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},75,0,0]
[null,null,"GAS:  CALIBRATIOIN :99PCT O2 Bal 1PCT H2","99PCT O2 Bal 1PCT H2 ANALYSER; TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE IN SMALL BOTTLE; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},95,0,0]
[null,null,"GAS: Calibration Trans former Gas Analyser ","GAS:  CALIBRATIOIN; Acetylene 100PPM, Ethylene 250PPM, Methane 502 PPM, Ethane 501 PPM, Carbon Monaxide 750PPM, Oxygen 1003PPM, Hydrogen 1019 PPM, Carbon Dioxide 3003PPM, Nitrogen Balance, Water 1PPM, Argon 7.9PPM ANALYSER TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE +/- 2% Accurate and 100PPM variance on different Gas element content IN SMALL BOTTLE DISPOSABLE; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":5,"d":"5.00"},95,0,0]
[null," ","GAS:  CALIBRATIOIN 99,999PCT 02 contaminants <10ppm","99,999PCT 02 contaminants <10ppm ANALYSER; TEST GAS, TO BE SUPPLIED WITH SPECIFICATION CERTIFICATE IN SMALL BOTTLE DISPOSABLE; MATERIAL SAFETY DATA SHEETS WITH ENVIRONMENTAL INFORMATION IN THE 16 POINT FORMAT TO BE PROVIDED WITH EVERY DELIVERY AS REQUIRED BY THE OCCUPATIONAL HEALTH AND SAFETY ACT",null,"L",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}," R-   ",{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":10,"d":"10.00"},{"v":5,"d":"5.00"},{"v":5,"d":"5.00"},{"v":0,"d":"0.00"},{"v":10,"d":"10.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},65,0,0]
[null,"Sub Total ",{"$nulls":32},{"$f":"SUM(AI55:AI96)","v":0}]
[]
[null,"RENTAL COSTS"]
[null,"Material","Short text","Description","Tenderer to indicate Cylinder Capacity in Kg","Cylinder Type (Tenderer to add additional Cylinder types on Cylinder Type&Size Sheet","Quantities Ingula","Sere Wind Farm","Small Hydro","Arnot PS","Ankerlig PS","Gourikwa PS","Potrex ps","Drankensburg PS","Acacia PS","Gariep PS","Palmiet PS","VanderKloof PS","MAJUBA PS","KUSILE PS","KOEBERG ps","Hendrina PS","Grootvlei PS","LETHABO PS","Kriel PS","Medupi PS","Matla PS","Kendal PS","Camden PS","Tutuka PS","Duvha PS","Matimba PS","Total Quantities","Cost","Amount"]
[140,"0213052","COSTING:GAS CYLINDER RENTAL (Large)",{"$nulls":3},{"v":535,"d":"535.00"},{"v":55,"d":"55.00"},{"v":55,"d":"55.00"},{"v":100,"d":"100.00"},{"v":25,"d":"25.00"},{"v":160,"d":"160.00"},{"v":25,"d":"25.00"},{"v":535,"d":"535.00"},{"v":85,"d":"85.00"},{"v":25,"d":"25.00"},{"v":100,"d":"100.00"},{"v":25,"d":"25.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},null,{"v":75,"d":"75.00"},{"v":150,"d":"150.00"},null,{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":150,"d":"150.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},{"$f":"SUM(G101:AF101)","v":2900},0,{"$f":"AH101*AG101","v":0}]
[150,"0558587","COSTING:RENTAL MEGA PACKS 18 ",{"$nulls":3},{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":125,"d":"125.00"},{"v":25,"d":"25.00"},{"v":20,"d":"20.00"},{"v":20,"d":"20.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":125,"d":"125.00"},{"v":125,"d":"125.00"},{"v":125,"d":"125.00"},{"v":150,"d":"150.00"},{"v":125,"d":"125.00"},null,{"v":75,"d":"75.00"},{"v":150,"d":"150.00"},null,{"v":125,"d":"125.00"},{"v":150,"d":"150.00"},{"v":150,"d":"150.00"},{"v":125,"d":"125.00"},{"v":0,"d":"0.00"},{"$f":"SUM(G102:AF102)","v":1765},0,0]
[170,"0215063","COSTING:CO2 EQUIPMENT RENTAL;PACKAGE 12",{"$nulls":3},{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":100,"d":"100.00"},{"v":200,"d":"200.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},null,{"v":50,"d":"50.00"},{"v":100,"d":"100.00"},null,{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},1400,0,0]
[160,"0626799","COSTING:053T;H2 10 CYLINDER TROLLEY",{"$nulls":3},{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":50,"d":"50.00"},{"v":25,"d":"25.00"},{"v":20,"d":"20.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"v":25,"d":"25.00"},{"v":100,"d":"100.00"},{"v":150,"d":"150.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":75,"d":"75.00"},null,{"v":75,"d":"75.00"},{"v":100,"d":"100.00"},null,{"v":100,"d":"100.00"},{"v":125,"d":"125.00"},{"v":150,"d":"150.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},1445,0,0]
[850,38891,"PALLET MTRL HNDLG:GAS CYLINDER;STL",{"$nulls":3},{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":45,"d":"45.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},null,{"v":0,"d":"0.00"},{"v":100,"d":"100.00"},null,{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":150,"d":"150.00"},{"v":100,"d":"100.00"},{"v":0,"d":"0.00"},1295,0,0]
[null,null,"COSTING:GAS CYLINDER RENTAL (10l)",{"$nulls":24},{"v":100,"d":"100.00"},{"$nulls":3},{"v":0,"d":"0.00"},100,0,0]
[130,"0636472","COSTING:1527;8 HYDROGEN D/CHAIN 144",{"$nulls":3},{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":50,"d":"50.00"},{"v":200,"d":"200.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":25,"d":"25.00"},null,{"v":25,"d":"25.00"},{"v":100,"d":"100.00"},null,{"v":50,"d":"50.00"},{"v":100,"d":"100.00"},{"v":100,"d":"100.00"},{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},900,0,0]
[120,"0636470","COSTING:1526;8 HYDROGEN DEMOUNT 168",{"$nulls":3},{"v":25,"d":"25.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},{"v":50,"d":"50.00"},{"v":25,"d":"25.00"},{"v":15,"d":"15.00"},{"v":15,"d":"15.00"},{"v":25,"d":"25.00"},{"v":10,"d":"10.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":25,"d":"25.00"},{"v":50,"d":"50.00"},{"v":250,"d":"250.00"},{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"v":0,"d":"0.00"},null,{"v":30,"d":"30.00"},{"v":0,"d":"0.00"},null,{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},{"v":50,"d":"50.00"},{"v":50,"d":"50.00"},{"v":0,"d":"0.00"},770,0,0]
[null,null,"Small",{"$nulls":28},{"v":0,"d":"0.00"},0,0,0]
[null,null,"Disposable 5l",{"$nulls":28},{"v":0,"d":"0.00"},0,0,0]
[null,null,"Disposable 10l",{"$nulls":28},{"v":0,"d":"0.00"},0,0,0]
[null,null,"Multi Cylinder 10",{"$nulls":28},{"v":0,"d":"0.00"},0,0,0]
[null,null,"Multi Cylinder 18",{"$nulls":28},{"v":0,"d":"0.00"},0,0,0]
[null,null,"Multi Cylinder 16",{"$nulls":28},{"v":0,"d":"0.00"},0,0,0]
[null,null,"Multi Cylinder 12",{"$nulls":28},{"v":0,"d":"0.00"},0,0,0]
[null,null,"Bulk Multi Cylinder 144",{"$nulls":28},{"v":0,"d":"0.00"},0,0,0]
[null,null,"Bulk Multi Cylinder 168",{"$nulls":28},{"v":0,"d":"0.00"},0,0,0]
[null,null,"Tune trailer 110kg ",{"$nulls":28},{"v":0,"d":"0.00"},0,0,0]
[null,"Note","Tenderer to quote for the Cylinder Management Tool"]
[null,"Sub Total ",{"$nulls":32},{"$f":"SUM(AI101:AI118)","v":0}]
[]
[null,"Cylinder Cost (Replacement Cost) "]
[null,"Material","Short text","Description","Tenderer to indicate Cylinder Capacity in Kg","Cylinder Type (Tenderer to add additional Cylinder types on Cylinder Type&Size Sheet","Quantities Ingula","Sere Wind Farm","Small Hydro","Arnot PS","Ankerlig PS","Gourikwa PS","Potrex ps","Drankensburg PS","Acacia PS","Gariep PS","Palmiet PS","VanderKloof PS","MAJUBA PS","KUSILE PS","KOEBERG ps","Hendrina PS","Grootvlei PS","LETHABO PS","Kriel PS","Medupi PS","Matla PS","Kendal PS","Camden PS","Tutuka PS","Duvha PS","Matimba PS","Total Quantities","Cost","Amount"]
[{"$nulls":32},{"$f":"SUM(G124:AF124)","v":0},0,{"$f":"AH124*AG124","v":0}]
[null,null,"Large","HP Cylindser",{"$nulls":28},{"$f":"SUM(G125:AF125)","v":0},0,0]
[null,null,"Large","DA Cylinder",{"$nulls":28},0,0,0]
[null,null,"Disposable 5l",{"$nulls":29},0,0,0]
[null,null,"Disposable 10l",{"$nulls":29},0,0,0]
[null,null,"Multi Cylinder 10",{"$nulls":29},0,0,0]
[null,null,"Multi Cylinder 18",{"$nulls":29},0,0,0]
[null,null,"Multi Cylinder 16",{"$nulls":29},0,0,0]
[null,null,"Multi Cylinder 12",{"$nulls":29},0,0,0]
[null,null,"Bulk Multi Cylinder 144",{"$nulls":29},0,0,0]
[null,null,"Bulk Multi Cylinder 168",{"$nulls":29},0,0,0]
[null,null,"Tune trailer 110kg ",{"$nulls":29},0,0,0]
[null,null,"LPG 9kg",{"$nulls":29},0,0,0]
[null,null,"LPG 11kg",{"$nulls":29},0,0,0]
[null,null,"LPG 19kg",{"$nulls":29},0,0,0]
[null,null,"LPG 48kg",{"$nulls":29},0,0,0]
[null,null,"10L",{"$nulls":29},0,0,0]
[null,null,"Portapack",{"$nulls":29},0,0,0]
[null,null,"19kg",{"$nulls":29},0,0,0]
[null,"Sub Total ",{"$nulls":32},{"$f":"SUM(AI124:AI142)","v":0}]
[]
[null,"LPG"]
[null,"Material","Short text","Description","Cylinder Capacity / KG","Cylinder Type (Tenderer to add additional Cylinder types on Cylinder Type&Size Sheet","Quantities Ingula","Sere Wind Farm","Small Hydro","Arnot PS","Ankerlig PS","Gourikwa PS","Potrex ps","Drankensburg PS","Acacia PS","Gariep PS","Palmiet PS","VanderKloof PS","MAJUBA PS","KUSILE PS","KOEBERG ps","Hendrina PS","Grootvlei PS","LETHABO PS","Kriel PS","Medupi PS","Matla PS","Kendal PS","Camden PS","Tutuka PS","Duvha PS","Matimba PS","Total Quantities","Cost","Amount"]
[null,"0016182","GAS:BUTANE/PROPANE:50 PCT:CYL 9 KG",9,"KG",9,{"$nulls":26},{"$f":"SUM(G147:AF147)","v":0},0,{"$f":"AH147*AG147","v":0}]
[null,"0213041","GAS LP:CYL:19 KG",19,"KG",19,0,0,0,1000,{"$nulls":8},500,500,750,1500,1500,1000,1000,500,1000,500,1500,400,500,500,{"$f":"SUM(G148:AF148)","v":12650},0,0]
[null,"0213040","GAS LP:CYL:48 KG",48,"KG",48,10,0,0,500,{"$nulls":8},550,750,500,1000,1000,1000,500,750,500,500,2000,500,500,500,11060,0,0]
[null,"0017666","GAS LP:1122:HANDIGAS;CLEAR LIQUID:BULK",null,"KG",1,0,0,0,250,{"$nulls":8},30,100,100,145,85,1500,100,100,75,100,95,100,0,125,2905,0,0]
[null,"Sub Total ",{"$nulls":32},{"$f":"SUM(AI147:AI150)","v":0}]
[]
[null,"RENTAL LPG"]
[null,"Material","Short text","Description","Cylinder Capacity / KG","Cylinder Type (Tenderer to add additional Cylinder types on Cylinder Type&Size Sheet","Quantities Ingula","Sere Wind Farm","Small Hydro","Arnot PS","Ankerlig PS","Gourikwa PS","Potrex ps","Drankensburg PS","Acacia PS","Gariep PS","Palmiet PS","VanderKloof PS","MAJUBA PS","KUSILE PS","KOEBERG ps","Hendrina PS","Grootvlei PS","LETHABO PS","Kriel PS","Medupi PS","Matla PS","Kendal PS","Camden PS","Tutuka PS","Duvha PS","Matimba PS","Total Quantities","Cost","Amount"]
[null,null,"LPG 9kg",9,"KG",{"$nulls":14},158.85,{"$nulls":3},158.85,158.85,null,158.85,"R158.85",300,0,0,158.85,{"$f":"SUM(G155:AF155)","v":{"v":1094.25,"d":"1094"}},0,{"$f":"AH155*AG155","v":0}]
[null,null,"LPG 11kg",11,"KG",{"$nulls":14},25,{"$nulls":3},25,25,null,25,null,null,0,0,50,{"$f":"SUM(G156:AF156)","v":150},0,0]
[null,null,"LPG 19kg",19,"KG",{"$nulls":14},335.35,{"$nulls":3},335.35,335.35,null,335.35,"R335.35",null,0,0,335.35,{"v":1676.75,"d":"1677"},0,0]
[null,null,"LPG 48kg",48,"KG",{"$nulls":4},2000,{"$nulls":9},847.2,null,null,2000,847.2,847.2,null,847.2,"R847.20",2000,0,0,847.2,10236,0,0]
[null,null,"LPG 9 cub meter",9,"Cub meter",{"$nulls":24},0,0,null,0,0,0]
[null,null,"LPG 4.5 cub meter",4.5,"Cub meter",{"$nulls":24},0,0,null,0,0,0]
[null,null,"LPG 22 cub meter",22,"Cub meter",{"$nulls":24},0,0,null,0,0,0]
[null,"Note","Tenderer to quote for upfront deposit for LPG cylinders"]
[null,"Sub Total ",{"$nulls":32},{"$f":"SUM(AI155:AI161)","v":0}]
[]
[null,"Cylinder Cost (Replacement Cost & LPG bulk) "]
[null,"Material","Short text","Description","Cylinder Capacity / KG","Cylinder Type (Tenderer to add additional Cylinder types on Cylinder Type&Size Sheet","Quantities Ingula","Sere Wind Farm","Small Hydro","Arnot PS","Ankerlig PS","Gourikwa PS","Potrex ps","Drankensburg PS","Acacia PS","Gariep PS","Palmiet PS","VanderKloof PS","MAJUBA PS","KUSILE PS","KOEBERG ps","Hendrina PS","Grootvlei PS","LETHABO PS","Kriel PS","Medupi PS","Matla PS","Kendal PS","Camden PS","Tutuka PS","Duvha PS","Matimba PS","Total Quantities","Cost","Amount"]
[null,null,"LPG 9kg",9,"KG",{"$nulls":4},20,{"$nulls":12},20,{"$nulls":5},20,0,0,0,{"$f":"SUM(G167:AF167)","v":60},0,{"$f":"AH167*AG167","v":0}]
[null,null,"LPG 11kg",11,"KG",{"$nulls":24},0,0,0,{"$f":"SUM(G168:AF168)","v":0},0,0]
[null,null,"LPG 19kg",19,"KG",{"$nulls":24},0,0,0,0,0,0]
[null,null,"LPG 48kg",48,"KG",{"$nulls":24},0,0,0,0,0,0]
[null,null,"LPG 9 cub meter",9,"Cub meter",{"$nulls":24},0,0,0,0,0,0]
[null,null,"LPG 4.5 cub meter",4.5,"Cub meter",{"$nulls":24},0,0,0,0,0,0]
[null,null,"LPG 22 cub meter",22,"Cub meter",{"$nulls":24},0,0,0]
[null,"Sub Total ",{"$nulls":32},{"$f":"SUM(AI167:AI172)","v":0}]
[]
[]
[null,"LPG Bulk Options"]
[null,"Material","Short text","Description","Cylinder Capacity / KG","Cylinder Type (Tenderer to add additional Cylinder types on Cylinder Type&Size Sheet","Quantities Ingula","Sere Wind Farm","Small Hydro","Arnot PS","Ankerlig PS","Gourikwa PS","Potrex ps","Drankensburg PS","Acacia PS","Gariep PS","Palmiet PS","VanderKloof PS","MAJUBA PS","KUSILE PS","KOEBERG ps","Hendrina PS","Grootvlei PS","LETHABO PS","Kriel PS","Medupi PS","Matla PS","Kendal PS","Camden PS","Tutuka PS","Duvha PS","Matimba PS","Total Quantities","Cost","Amount"]
[null,null,"LPG bulk complete facility 9 cub meter (design, manufacture, supply, contruct, install, commission and test including detailed design and data pack)  ",{"$nulls":16},300,{"$nulls":3},300,null,300,300,300,300,300,300,300,{"$f":"SUM(G179:AF179)","v":2700},0,{"$f":"AH179*AG179","v":0}]
[null,null,"LPG bulk complete facility 4,5 cub meter (design, manufacture, supply, contruct, install, commission and test, including detailed design and data pack)  ",{"$nulls":16},0,{"$nulls":3},0,null,0,0,0,0,0,0,0,0,0,0]
[null,null,"LPG bulk complete facility 22 cub meter (design, manufacture, supply, contruct, install, commission and test including detailed design and data pack)  ",{"$nulls":16},0,{"$nulls":3},0,null,0,0,0,0,0,0,0,0,0,0]
[null,null,"LPG bulk complete facility 9 cub meter (take over ownership by Employer including detailed design and data pack)  ",{"$nulls":16},0,{"$nulls":3},0,null,0,0,0,0,0,0,0,0,0,0]
[null,null,"LPG bulk complete facility 4,5 cub meter (take over ownership by Employer including detailed design and data pack) ",{"$nulls":16},0,{"$nulls":3},0,null,0,0,0,0,0,0,0,0,0,0]
[null,null,"LPG bulk complete facility 22 cub meter (take over ownership by Employer including detailed design and data pack) ",{"$nulls":16},0,{"$nulls":3},0,null,0,0,0,0,0,0,0,0,0,0]
[null,null,"LPG Bulk Vessel Maintenance (Deatailed maintenace activities including spares to be indicated under \"Description\" column and priced, manitenace plan documet to be submitted as part of tender submission)",{"$nulls":16},0,{"$nulls":3},0,null,0,0,0,0,0,0,0,0,0,0]
[null,"Sub Total ",{"$nulls":32},{"$f":"SUM(AI179:AI185)","v":0}]

{"sheet":"Eskom CPA Proposal","index":5,"n_rows":41,"n_cols":11,"rows_kept":41,"merged":[[0,0,0,8],[2,0,2,2],[2,3,2,7],[3,0,3,2],[3,3,3,7],[4,0,4,2],[4,3,4,7],[5,0,5,2],[5,3,5,7],[6,0,6,2],[6,3,6,7],[7,0,7,2],[7,3,7,7],[8,0,8,2],[8,3,8,7],[9,0,9,2],[9,3,9,7],[10,0,10,2],[10,3,10,7],[11,0,11,2],[11,3,11,7],[12,0,12,2],[12,3,12,7],[13,0,13,2],[13,3,13,7],[14,0,14,10],[15,0,15,2],[17,2,17,10]]}
["Cost Price Adjustment"]
[]
["Vendor :"]
["Contract Number:"]
["Unit Number:"]
["Base Date of contract (yyyy/mm/dd):",null,null,"2019-03-01"]
["FINAL CPA Cut-off Date (yyyy/mm/dd):"]
["Basic Invoice No.:"]
["Basic End Date of claim (yyyy/mm/dd):"]
["Base Amount as per contract: "]
["CPA Invoice No.:"]
["CPA Amount claimed by Supplier:"]
["Previous CPA Claim"]
["Claimed Amount incl. in Base Invoice"]
[]
["CPA  Formula as per contract:"]
[]
[null,null,"ANNUAL RATE INCREASE CALCULATIONS"]
[null,null,"Components","Weighting %","Table","Months Prior","Final Index Month","Base Index","Ruling Index","Factor","CPA Amount"]
[null,"A",{"$f":"+'[56]CONTRACT DETAIL'!D11","v":"Fixed Portion"},{"v":0.15,"d":"15.00%"}]
[null,"B","Labour",{"v":0.25,"d":"25.00%"},"SEIFSA -Table C3",{"$nulls":4},{"$f":"IF(H21>0,ROUND(((I21-H21)/H21)*$D$21,4),\"\")","v":""},{"$f":"IF(J21<>\"\",ROUND(D10*J21,2),\"\")","v":""}]
[null,"C","Transport",{"v":0.25,"d":"25.00%"},"SEIFSA - L(2) A ",{"$nulls":4},{"$f":"IF(H22>0,ROUND(((I22-H22)/H22)*$D$22,4),\"\")","v":""},{"$f":"IF(J22<>\"\",ROUND(D10*J22,2),\"\")","v":""}]
[null,"D","Material",{"v":0.35,"d":"35.00%"},"SEIFSA - Table UA",{"$nulls":4},{"$f":"IF(H23>0,ROUND(((I23-H23)/H23)*$D$23,4),\"\")","v":""},{"$f":"IF(J23<>\"\",ROUND(D9*J23,2),\"\")","v":""}]
[null,null,"Total",{"$f":"SUM(D20:D23)","v":{"v":1,"d":"100.00%"}},{"$nulls":5},{"$f":"SUM(J20:J23)","v":{"v":0,"d":"0.0000%"}},{"$f":"SUM(K20:K23)","v":{"v":0,"d":"0.00"}}]
[{"$nulls":9},"Base Amount x Factor",{"$f":"ROUND($D$10*J24,2)","v":{"v":0,"d":"0.00"}}]
[{"$nulls":9},"Control =Zero",{"$f":"SUM(K25,-K24)","v":{"v":0,"d":"0.00"}}]
[]
[]
["Total CPA Amount","X",{"$f":"$K$24","v":{"v":0,"d":"0.00"}}]
["Less previous claim",null,{"$f":"+D134","v":{"v":0,"d":"0.00"}}]
["Updated CPA Due",null,{"$f":"+C29-C30","v":{"v":0,"d":"0.00"}}]
["Total Claimed by Supplier","Y",{"v":0,"d":"0.00"}]
["Difference","Z",{"$f":"+C31-C32","v":{"v":0,"d":"0.00"}},{"$f":"IF(C33>-100,\"ACCEPT THEIR CLAIM NO CREDIT NOTE\",\"REQUEST CREDIT NOTE FROM SUPPLIER !!!!!!!!!!\")","v":"ACCEPT THEIR CLAIM NO CREDIT NOTE"}]
[]
[]
["Compiled by:",null,"Kgotso Madisha",{"$nulls":6},"2020-08-31"]
[null,null,"(print name)",null,null,"(signature)",{"$nulls":3},"(yyyy/mm/dd)"]
[]
[]
["Checked by:",null,"Lucky Nemakonde",{"$nulls":6},"2020-08-31"]
[null,null,"(print name)",null,null,"(signature)",{"$nulls":3},"(yyyy/mm/dd)"]